{"text_format":"1","workbook":"xlsx","n_sheets":28,"sheets":["Start","Guidelines","Input Project","Indicators","Input EB","Input Land use","Input RU","Input EQ","Input Bio","Input LW","Output Mass","Uncertainty","Results","Parameters","Data","Lists","Standard Values","IPCC Values","Production feedstock1","Production feedstock2","Transport feedstock1","Transport feedstock2","Conversion feedstock1","Conversion feedstock2","Final conversion","Graph results","MonteCarlo","ID-numbers"],"not_rendered":{"charts":42,"images":36,"macros":1,"external_links":0,"defined_names":89,"comments":12,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Start","index":0,"n_rows":38,"n_cols":13,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,"Welcome"]
[]
[null,null,"You have just opened B-SAT, or the Bio-energy Sustainability Assessment Tool."]
[null,null,"The development of this tool was the main aim of a joint PhD project by VITO (The Flemish Institute for Technological Research)in cooperation with the University of Antwerp and the University of Leuven."]
[]
[null,null,"Why use this tool?"]
[null,null,"Together with the increased production of biofuels as an alternative for fossil fuels, concerns have raised about the sustainability of large scale biomass production for energy."]
[null,null,"This is the first tool that offers the possibility to perform a quick and comprehensive evaluation of the sustainability of a bio-energy system producing electricity and heat without requiring expert skills on this topic."]
[null,null,"Sustainability indicators are assessed throughout the whole life cycle of the bio-energy production system and compared to the corresponding fossil reference system."]
[null,null,"The B-SAT sustainability framework includes, among others, the requirements laid down in the European Renewable Energy Directive (2009/28/EC) and the Commission report COM(2010)11 on the use of solid"]
[null,null,"and gaseous biomass for energy production. "]
[]
[null,null,"Though calculations in this tool follow the rules laid down in the RED and the COM(2010)11, it must be stressed that this tool is not officially acknowledged to perform the RED calculations. Results must thus be seen as indicative."]
[]
[null,null,"On the next page, an overview is given of the various steps required to proceed through the evaluation. "]
[]
[null,null,"Good luck & enjoy!"]
[]
[]
[null,null,"Author: Veerle Buytaert (veerle@buytaert.be)"]
[]
[]
[]
[]
[null,null,"Nathalie Devriendt",null,null,null,null,"Roeland Samson",null,null,null,null,"Bart Muys"]
[null,null,"Unit Transition, Energy & Environment",null,null,null,null,"Department of Bioscience Engineering",null,null,null,null,"Division Forest, Nature and Landscape"]
[null,null,"VITO NV",null,null,null,null,"University of Antwerp",null,null,null,null,"University of Leuven"]
[null,null,"Boeretang 200",null,null,null,null,"Groenenborgerlaan 171 V",null,null,null,null,"Celestijnenlaan 200E, Box 2411"]
[null,null,"BE - 2400 Mol",null,null,null,null,"BE - 2020 Antwerpen",null,null,null,null,"BE - 3001 Leuven"]
[null,null,"nathalie.devriendt@vito.ac.be",null,null,null,null,"roeland.samson@ua.ac.be",null,null,null,null,"bart.muys@ees.kuleuven.be"]

{"sheet":"Guidelines","index":1,"n_rows":82,"n_cols":19,"rows_kept":82,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[null,null,"Guidelines"]
[]
[null,null,null,"User input cells are colored in green and indicated with a red INPUT arrow."]
[null,null,null,"Extra information about a certain section or topic, can be retrieved by clicking on the information icons:"]
[]
[]
[null,null,"The B-SAT sustainability assessment process consists of 5 steps, explained below:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,"* not accessible in the 'limited' B-SAT version"]
[]
[null,null,"1. Project definition"]
[null,null,"In the first step of the assessment process, the entire life cycle of the bio-energy system has to be defined with all the inputs and outputs."]
[null,null,"In the upper part of the sheet, feedstock(s), final conversion technology, final energy and functional unit must be selected from the lists with available options. "]
[null,null,"The calculation structure in this tool offers the possibility to feed up to two different feedstocks (with exception for waste streams as they can also be added in secondary steps) into the bioenergy system."]
[null,null,"The life cycle of one feedstock consequently consists of a biomass production phase, a first transportation/storage phase, a first conversion phase, a second transportation/storage phase, a second conversion"]
[null,null,"phase and a third transportation/storage phase. This life cycle then results in a secondary energy carrier which is used, together with the secondary energy carrier of a possible second feedstock, for the final"]
[null,null,"conversion process into electricity and/or heat. The use of a second feedstock is optional."]
[null,null,"A schematical reproduction of the calculation structure is given below:"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"OPTIONAL"]
[]
[null,null,"An example with two feedstocks is the production of palm oil from fresh palm fruit bunches (feedstock 1: production \" transport 3) and the production of biogas from the fermentation of maize and organic "]
[null,null,"waste (feedstock 2: production \" transport 3), both fed into a dual fuel engine for production of electricity and heat (final conversion)."]
[]
[null,null,"In the second part of the sheet, all data are listed that are needed to calculate the mass balance of the system. For every feedstock option, default data are available in the tool. These are the same data that"]
[null,null,"are used within the calculations of the Renewable Energy Directive. The user is therefore not obliged to fill in data and can directly proceed to the next step if desired. However, it is suggested to use personally "]
[null,null,"derived data as reference data are rather conservative and tend to result in less positive conclusions. Personal data can be inserted in the user input area. In that case the personal data will be used for any further"]
[null,null,"calculation.  A list of standard values used in this tool is available in a separate document, together with the corresponding data sources."]
[]
[null,null,"2. Mass balance"]
[null,null,"After defining the entire life cycle of the system, the result can be viewed and checked in the mass balance sheet. This aids the user to obtain a concise overview of the assessed system and to easily detect poten-"]
[null,null,"tial errors. In case an error is found, the user can go one step back by using the green BACK arrow on at the top or bottom of the sheet and adapt the input value concerned."]
[]
[]
[null,null,"3. Calculation"]
[null,null,"Some general rules apply:"]
[null,null,"• Sustainability impacts of the bio-energy production system are compared to those of the corresponding fossil reference system(s) as laid down in the RED (2009/28/EC) and report COM(2010)11. "]
[null,null,"• Wastes, agricultural crop residues, including straw, bagasse, husks, cobs and nut shells, and residues from processing, including crude glycerine (glycerine that is not refined), are considered to have zero impacts"]
[null,null,"   up to the process of collection of those materials. However, the use of those materials as non-artificial fertiliser for biomass production must be taken into account (see calculation sheet 'Global Warming')."]
[null,null,"• When during the entire bio-energy production process not only the desired final energy carriers are produced, but also other valuable products (co- or by-products), the impacts must be divided between the "]
[null,null,"   final fuel(s) and the co-products in proportion to their energy content. Or, in other words, allocation between final fuel(s) and co-products must be based on the lower heating value of the fuel(s)/products."]
[null,null,"• Waste, including waste heat, and residues leave the system without allocation to it."]
[null,null,"• Allocation takes place directly after a co-product is produced at a process step."]
[null,null,"• For bio-energy installations producing electricity as well as useful heat, impacts are allocated based on the Carnot efficiency of the energy product. "]
[null,null,"• Impacts of the construction of buildings and production of machinery used for both bio-energy production and fossil reference energy production are not included in the calculations."]
[]
[null,null,"Though calculations in this tool follow the rules laid down in the RED and the COM(2010)11, it muss be stressed that this tool is not officially acknowledged to perform the RED calculations. Results must thus be seen as indicative."]
[]
[]
[null,null,"4. Uncertainty analysis"]
[null,null,"As in any other assessment, the use of (default) data is inherently subject to a degree of uncertainty. A method based on Monte Carlo filtering calculates for each quantitative sustainability indicator the variation "]
[null,null,"(uncertainty) in the output. This gives the user better insight in the reliability of the results. "]
[null,null,"In this limited edition the uncertainty analysis is not available."]
[]
[]
[null,null,"5. Results"]
[null,null,"The last sheet gives an overview of the outcomes of the sustainability assessment. For each indicator, overall as well as disaggregated (for each feedstock and for each part of the bioenergy production chain) "]
[null,null,"results are given. For the quantitative indicators, the results of the bio-energy system are set against those of the fossil reference system."]

{"sheet":"Input Project","index":2,"n_rows":354,"n_cols":12,"rows_kept":354,"cut":false,"hidden":false,"merged":[[15,7,15,8],[11,7,11,8],[13,7,13,8]]}
[]
[]
[]
[]
[]
[]
[]
[null,null,"Project definition"]
[]
[null,null,"Feedstock pathway 1"]
[]
[null,null,"Feedstock pathway 2 (optional)"]
[]
[null,null,"Final conversion technology"]
[]
[null,null,"Functional unit",null,null,null,null,null,null,"! if final conversion technology is 'CHP', please choose MJ electricity or MJ heat"]
[null,null,null,null,null,null,null,null,null,"! if final conversion technology is  'no final conversion',"]
[null,null,null,null,null,null,null,null,null,"   please choose MJ gas for biogas or LBM, MJ diesel for biodiesel and MJ heavy oil for bio-oil  production"]
[null,null,"Project input data"]
[]
[null,null,null,null,"Feedstock pathway 1"]
[]
[null,null,null,null,"Feedstock production",null,null,"User input","Default value","Unit"]
[null,null,null,null,"harvested feedstock",null,null,{"$f":"I24","v":"Fresh palm fruit bunches (FFB)"},{"$f":"Parameters!D20","v":"Fresh palm fruit bunches (FFB)"}]
[null,null,null,null,"crop yield",null,null,null,{"$f":"Parameters!D22","v":19000},"kgfm.ha-1.y-1"]
[null,null,null,null,"moisture content of crop",null,null,null,{"$f":"Parameters!D27","v":34},"%"]
[null,null,null,null,"main by-product",null,null,null,{"$f":"Parameters!D29","v":"n.a."}]
[null,null,null,null,"yield of main by-product",null,null,null,{"$f":"Parameters!D31","v":0},"kgfm.ha-1.y-1"]
[null,null,null,null,"moisture content of main by-product",null,null,null,{"$f":"Parameters!D35","v":0},"%"]
[null,null,null,null,"secondary by-product",null,null,null,{"$f":"Parameters!D30","v":"n.a."}]
[null,null,null,null,"yield of secondary by-product",null,null,null,{"$f":"Parameters!D32","v":0},"kgfm.ha-1.y-1"]
[null,null,null,null,"moisture content of secondary by-product",null,null,null,{"$f":"Parameters!D36","v":0},"%"]
[null,null,null,null,"use of seeds",null,null,null,{"$f":"Parameters!D41","v":0},"kg.ha-1.y-1"]
[null,null,null,null,"use of N-fertiliser",null,null,null,{"$f":"Parameters!D42","v":127.908},"kg.ha-1.y-1"]
[null,null,null,null,"use of P2O5-fertiliser",null,null,null,{"$f":"Parameters!D43","v":143.792},"kg.ha-1.y-1"]
[null,null,null,null,"use of K2O-fertiliser",null,null,null,{"$f":"Parameters!D44","v":199.804},"kg.ha-1.y-1"]
[null,null,null,null,"use of CaO-fertiliser",null,null,null,{"$f":"Parameters!D45","v":0},"kg.ha-1.y-1"]
[null,null,null,null,"use of pesticides",null,null,null,{"$f":"Parameters!D46","v":8.36},"kg.ha-1.y-1"]
[null,null,null,null,"type of fuel in farm machinery",null,null,null,{"$f":"Parameters!D54","v":"Diesel"}]
[null,null,null,null,"amount of fuel used",null,null,null,{"$f":"Parameters!D57","v":47.902000000000001},"kg.ha-1.y-1"]
[]
[null,null,null,null,"Feedstock treatment and transport 1",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Drying and storage:",null,null,null,{"$f":"Parameters!D3","v":"No treatment"}]
[null,null,null,null,"heat source",null,null,null,{"$f":"Parameters!D60","v":"n.a."}]
[null,null,null,null,"heat use for drying",null,null,null,{"$f":"Parameters!D59","v":0},"MJ.kgfm-1"]
[null,null,null,null,"electricity source",null,null,null,{"$f":"Parameters!D63","v":"n.a."}]
[null,null,null,null,"electricity use for drying",null,null,null,{"$f":"Parameters!D62","v":0},"MJ.kgfm-1"]
[null,null,null,null,"Feedstock transport:",null,null,null,{"$f":"Parameters!D2","v":"Transport of FFB to the mill"}]
[null,null,null,null,"transport mode 1",null,null,null,{"$f":"Parameters!D462","v":"Truck for FFB transport (Diesel)"}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D480","v":50},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D489","v":"Diesel"}]
[null,null,null,null,"transport mode 2",null,null,null,{"$f":"Parameters!D463","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D481","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D490","v":"n.a."}]
[null,null,null,null,"transport mode 3",null,null,null,{"$f":"Parameters!D464","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D482","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D491","v":"n.a."}]
[]
[null,null,null,null,"Feedstock conversion 1",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Process 1",null,null,{"$f":"I60","v":"Production of Crude Palm Oil (CPO)"},{"$f":"Parameters!D4","v":"Production of Crude Palm Oil (CPO)"}]
[null,null,null,null,"main output flow of process 1",null,null,{"$f":"I61","v":"Crude palm oil"},{"$f":"Parameters!D666","v":"Crude palm oil"}]
[null,null,null,null,"main by-product",null,null,null,{"$f":"Parameters!D668","v":"Palm kernel meal"}]
[null,null,null,null,"moisture content of by-product 1,process 1",null,null,null,{"$f":"Parameters!D669","v":8.1999999999999993},"%"]
[null,null,null,null,"by-product flow 1, process 1",null,null,null,{"$f":"Parameters!D670","v":462.83},"kg.year-1"]
[null,null,null,null,"energy content of by-product 1, process 1",null,null,null,{"$f":"Parameters!D701","v":17},"MJ.kgdm-1"]
[null,null,null,null,"secondary by-product",null,null,null,{"$f":"Parameters!D671","v":"n.a."}]
[null,null,null,null,"moisture content of by-product 2,process 1",null,null,null,{"$f":"Parameters!D672","v":0},"%"]
[null,null,null,null,"by-product flow 2, process 1",null,null,null,{"$f":"Parameters!D673","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 2, process 1",null,null,null,{"$f":"Parameters!D702","v":0},"MJ.kgdm-1"]
[null,null,null,null,"tertiary by-product",null,null,null,{"$f":"Parameters!D674","v":"n.a."}]
[null,null,null,null,"moisture content of by-product 3,process 1",null,null,null,{"$f":"Parameters!D675","v":0},"%"]
[null,null,null,null,"by-product flow 3, process 1",null,null,null,{"$f":"Parameters!D676","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 3, process 1",null,null,null,{"$f":"Parameters!D703","v":0},"MJ.kgdm-1"]
[null,null,null,null,"electricity by-product, process 1",null,null,null,{"$f":"Parameters!D677","v":0},"MWh.year-1"]
[null,null,null,null,"heat by-product, process 1",null,null,null,{"$f":"Parameters!D678","v":0},"MJ.year-1"]
[null,null,null,null,"type 1 of fuel/heat input",null,null,null,{"$f":"Parameters!D761","v":"n.a."}]
[null,null,null,null,"fuel/heat input 1",null,null,null,{"$f":"Parameters!D820","v":0},"MJ.year-1"]
[null,null,null,null,"type 2 of fuel/heat input",null,null,null,{"$f":"Parameters!D762","v":"n.a."}]
[null,null,null,null,"fuel/heat input 2",null,null,null,{"$f":"Parameters!D822","v":0},"MJ.year-1"]
[null,null,null,null,"type 1 of electricity input",null,null,null,{"$f":"Parameters!D805","v":"n.a."}]
[null,null,null,null,"electricity flow 1",null,null,null,{"$f":"Parameters!D798","v":0},"MWh.year-1"]
[null,null,null,null,"type 2 of electricity input",null,null,null,{"$f":"Parameters!D806","v":"n.a."}]
[null,null,null,null,"electricity flow 2",null,null,null,{"$f":"Parameters!D800","v":0},"MWh.year-1"]
[null,null,null,null,"type of main input",null,null,null,{"$f":"Parameters!D719","v":"Fresh palm fruit bunches (FFB)"}]
[null,null,null,null,"main input, process 1",null,null,null,{"$f":"Parameters!D731","v":19000},"kg.year-1"]
[null,null,null,null,"Energy content of main input, process 1",null,null,null,{"$f":"Parameters!D68","v":24},"MJ.kgdm-1"]
[null,null,null,null,"type 1 of material input",null,null,"n.a.",{"$f":"Parameters!D720","v":"n.a."}]
[null,null,null,null,"material input flow 1, process 1",null,null,null,{"$f":"Parameters!D732","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 1, process 1",null,null,null,{"$f":"Parameters!D735","v":0},"%"]
[null,null,null,null,"energy content of input flow 1, process 1",null,null,null,{"$f":"Parameters!D736","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type 2 of material input",null,null,null,{"$f":"Parameters!D721","v":"n.a."}]
[null,null,null,null,"material input flow 2, process 1",null,null,null,{"$f":"Parameters!D737","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 2, process 1",null,null,null,{"$f":"Parameters!D739","v":0},"%"]
[null,null,null,null,"energy content of input flow 2, process 1",null,null,null,{"$f":"Parameters!D740","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type 3 of material input",null,null,null,{"$f":"Parameters!D722","v":"n.a."}]
[null,null,null,null,"material input flow 3, process 1",null,null,null,{"$f":"Parameters!D741","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 3, process 1",null,null,null,{"$f":"Parameters!D743","v":0},"%"]
[null,null,null,null,"energy content of input flow 3, process 1",null,null,null,{"$f":"Parameters!D744","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type of material output",null,null,null,{"$f":"Parameters!D725","v":"n.a."}]
[null,null,null,null,"material output flow, process 1",null,null,null,{"$f":"Parameters!D754","v":4311},"kg.year-1"]
[null,null,null,null,"energy content of material output flow, process 1",null,null,null,{"$f":"Parameters!D715","v":37},"MJ.kgdm-1"]
[null,null,null,null,"type of material output (electricity)",null,null,null,{"$f":"Parameters!D726","v":"n.a."}]
[null,null,null,null,"type of material output (heat)",null,null,null,{"$f":"Parameters!D727","v":"n.a."}]
[]
[null,null,null,null,"Feedstock treatment and transport 2",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Drying and storage:",null,null,null,{"$f":"Parameters!D6","v":"No treatment"}]
[null,null,null,null,"heat source",null,null,null,{"$f":"Parameters!D906","v":"n.a."}]
[null,null,null,null,"heat use for drying",null,null,null,{"$f":"Parameters!D905","v":0},"MJ.MJinput-1"]
[null,null,null,null,"electricity source",null,null,null,{"$f":"Parameters!D908","v":"n.a."}]
[null,null,null,null,"electricity use for drying",null,null,null,{"$f":"Parameters!D907","v":8.4000000000000003E-4},"MJ.MJinput-1"]
[null,null,null,null,"Feedstock transport:",null,null,null,{"$f":"Parameters!D5","v":"Transport of CPO to Belgium"}]
[null,null,null,null,"transport mode 4",null,null,null,{"$f":"Parameters!D465","v":"Truck for liquids (Diesel)"}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D483","v":150},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D492","v":"Diesel"}]
[null,null,null,null,"transport mode 5",null,null,null,{"$f":"Parameters!D466","v":"Ship /product tanker 50kt (HFO maritime)"}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D484","v":10186},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D493","v":"HFO for maritime transport"}]
[null,null,null,null,"transport mode 6",null,null,null,{"$f":"Parameters!D467","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D485","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D494","v":"n.a."}]
[]
[null,null,null,null,"Feedstock conversion 2",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Process 2",null,null,{"$f":"I123","v":"Refinery of Crude Palm Oil"},{"$f":"Parameters!D7","v":"Refinery of Crude Palm Oil"}]
[null,null,null,null,"main output flow of process 2",null,null,{"$f":"I124","v":"Palm stearin"},{"$f":"Parameters!D667","v":"Palm stearin"}]
[null,null,null,null,"main by-product",null,null,null,{"$f":"Parameters!D679","v":"Palm olein"}]
[null,null,null,null,"moisture content of by-product 1,process 2",null,null,null,{"$f":"Parameters!D680","v":0},"%"]
[null,null,null,null,"by-product flow 1, process 2",null,null,null,{"$f":"Parameters!D681","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 1, process 2",null,null,null,{"$f":"Parameters!D704","v":37},"MJ.kgdm-1"]
[null,null,null,null,"secondary by-product",null,null,null,{"$f":"Parameters!D682","v":"n.a."}]
[null,null,null,null,"moisture content of by-product 2,process 2",null,null,null,{"$f":"Parameters!D683","v":0},"%"]
[null,null,null,null,"by-product flow 2, process 2",null,null,null,{"$f":"Parameters!D684","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 2, process 2",null,null,null,{"$f":"Parameters!D705","v":0},"MJ.kgdm-1"]
[null,null,null,null,"electricity by-product, process 2",null,null,null,{"$f":"Parameters!D685","v":0},"MWh.year-1"]
[null,null,null,null,"heat by-product, process 2",null,null,null,{"$f":"Parameters!D686","v":0},"MJ.year-1"]
[null,null,null,null,"type 1 of fuel/heat input",null,null,null,{"$f":"Parameters!D763","v":"Heat from NG boiler"}]
[null,null,null,null,"fuel/heat input 1",null,null,null,{"$f":"Parameters!D824","v":408},"MJ.year-1"]
[null,null,null,null,"type 2 of fuel/heat input",null,null,null,{"$f":"Parameters!D764","v":"n.a."}]
[null,null,null,null,"fuel/heat input 2",null,null,null,{"$f":"Parameters!D826","v":0},"MJ.year-1"]
[null,null,null,null,"type 1 of electricity input",null,null,null,{"$f":"Parameters!D807","v":"Electricity EU mix LV"}]
[null,null,null,null,"electricity flow 1",null,null,null,{"$f":"Parameters!D802","v":8.5000000000000006E-3},"MWh.year-1"]
[null,null,null,null,"type 2 of electricity input",null,null,null,{"$f":"Parameters!D808","v":"n.a."}]
[null,null,null,null,"electricity flow 2",null,null,null,{"$f":"Parameters!D804","v":0},"MWh.year-1"]
[null,null,null,null,"type 1 of material input",null,null,null,{"$f":"Parameters!D723","v":"Fuller's earth"}]
[null,null,null,null,"material input flow 1, process 2",null,null,null,{"$f":"Parameters!D746","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 1, process 2",null,null,null,{"$f":"Parameters!D747","v":0},"%"]
[null,null,null,null,"energy content of input flow 1, process 2",null,null,null,{"$f":"Parameters!D748","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type 2 of material input",null,null,null,{"$f":"Parameters!D724","v":"n.a."}]
[null,null,null,null,"material input flow 2, process 2",null,null,null,{"$f":"Parameters!D750","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 2, process 2",null,null,null,{"$f":"Parameters!D751","v":0},"%"]
[null,null,null,null,"energy content of input flow 2, process 2",null,null,null,{"$f":"Parameters!D752","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type of material output",null,null,null,{"$f":"Parameters!D728","v":"n.a."}]
[null,null,null,null,"material output flow, process 2",null,null,null,{"$f":"Parameters!D758","v":1379},"kg.year-1"]
[null,null,null,null,"energy content of material output, process 2",null,null,null,{"$f":"Parameters!D716","v":37},"MJ.kgdm-1"]
[null,null,null,null,"type of material output (electricity), process 2",null,null,null,{"$f":"Parameters!D729","v":"n.a."}]
[null,null,null,null,"type of material output (heat), process 2",null,null,null,{"$f":"Parameters!D730","v":"n.a."}]
[]
[null,null,null,null,"Feedstock treatment and transport 3",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Drying and storage:",null,null,null,{"$f":"Parameters!D9","v":"No treatment"}]
[null,null,null,null,"heat source",null,null,null,{"$f":"Parameters!D913","v":"n.a."}]
[null,null,null,null,"heat use for drying",null,null,null,{"$f":"Parameters!D912","v":0},"MJ.MJinput-1"]
[null,null,null,null,"electricity source",null,null,null,{"$f":"Parameters!D915","v":"n.a."}]
[null,null,null,null,"electricity use for drying",null,null,null,{"$f":"Parameters!D914","v":8.4000000000000003E-4},"MJ.MJinput-1"]
[null,null,null,null,"Feedstock transport:",null,null,null,{"$f":"Parameters!D8","v":"Transport of PS to the final conversion unit"}]
[null,null,null,null,"transport mode 7",null,null,null,{"$f":"Parameters!D468","v":"Truck for liquids (Diesel)"}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D486","v":100},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D495","v":"Diesel"}]
[null,null,null,null,"transport mode 8",null,null,null,{"$f":"Parameters!D469","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D487","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D496","v":"n.a."}]
[null,null,null,null,"transport mode 9",null,null,null,{"$f":"Parameters!D470","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D488","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D497","v":"n.a."}]
[]
[null,null,null,null,"Feedstock pathway 2 (optional)"]
[]
[null,null,null,null,"Feedstock production",null,null,"User input","Default value","Unit"]
[null,null,null,null,"harvested feedstock",null,null,{"$f":"I177","v":"No crop"},{"$f":"Parameters!D241","v":"No crop"}]
[null,null,null,null,"crop yield",null,null,null,{"$f":"Parameters!D243","v":0},"kgfm.ha-1.y-1"]
[null,null,null,null,"moisture content of crop",null,null,null,{"$f":"Parameters!D248","v":0},"%"]
[null,null,null,null,"main by-product",null,null,null,{"$f":"Parameters!D250","v":"n.a."}]
[null,null,null,null,"yield of main by-product",null,null,null,{"$f":"Parameters!D252","v":0},"kgfm.ha-1.y-1"]
[null,null,null,null,"moisture content of main by-product",null,null,null,{"$f":"Parameters!D256","v":0},"%"]
[null,null,null,null,"secondary by-product",null,null,null,{"$f":"Parameters!D251","v":"n.a."}]
[null,null,null,null,"yield of secondary by-product",null,null,null,{"$f":"Parameters!D253","v":0},"kgfm.ha-1.y-1"]
[null,null,null,null,"moisture content of secondary by-product",null,null,null,{"$f":"Parameters!D257","v":0},"%"]
[null,null,null,null,"use of seeds",null,null,null,{"$f":"Parameters!D262","v":0},"kg.ha-1.y-1"]
[null,null,null,null,"use of N-fertiliser",null,null,null,{"$f":"Parameters!D263","v":0},"kg.ha-1.y-1"]
[null,null,null,null,"use of P2O5-fertiliser",null,null,null,{"$f":"Parameters!D264","v":0},"kg.ha-1.y-1"]
[null,null,null,null,"use of K2O-fertiliser",null,null,null,{"$f":"Parameters!D265","v":0},"kg.ha-1.y-1"]
[null,null,null,null,"use of CaO-fertiliser",null,null,null,{"$f":"Parameters!D266","v":0},"kg.ha-1.y-1"]
[null,null,null,null,"use of pesticides",null,null,null,{"$f":"Parameters!D267","v":0},"kg.ha-1.y-1"]
[null,null,null,null,"type of fuel in farm machinery",null,null,null,{"$f":"Parameters!D275","v":"n.a."}]
[null,null,null,null,"amount of fuel used",null,null,null,{"$f":"Parameters!D278","v":0},"kg.ha-1.y-1"]
[]
[null,null,null,null,"Feedstock treatment and transport 1",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Drying and storage:",null,null,null,{"$f":"Parameters!D11","v":"n.a."}]
[null,null,null,null,"heat source",null,null,null,{"$f":"Parameters!D281","v":"n.a."}]
[null,null,null,null,"heat use for drying",null,null,null,{"$f":"Parameters!D280","v":0},"MJ.kgfm-1"]
[null,null,null,null,"electricity source",null,null,null,{"$f":"Parameters!D284","v":"n.a."}]
[null,null,null,null,"electricity use for drying",null,null,null,{"$f":"Parameters!D283","v":0},"MJ.kgfm-1"]
[null,null,null,null,"Feedstock transport:",null,null,null,{"$f":"Parameters!D10","v":"n.a."}]
[null,null,null,null,"transport mode 1",null,null,null,{"$f":"Parameters!D563","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D581","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D590","v":"n.a."}]
[null,null,null,null,"transport mode 2",null,null,null,{"$f":"Parameters!D564","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D582","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D591","v":"n.a."}]
[null,null,null,null,"transport mode 3",null,null,null,{"$f":"Parameters!D565","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D583","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D592","v":"n.a."}]
[null,null,null,null,null,null,null,null,null,null,null,"data validation!"]
[null,null,null,null,"Feedstock conversion 1",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Process 1",null,null,{"$f":"I213","v":"n.a."},{"$f":"Parameters!D12","v":"n.a."}]
[null,null,null,null,"main output flow of process 1",null,null,{"$f":"I214","v":"n.a."},{"$f":"Parameters!D1037","v":"n.a."}]
[null,null,null,null,"main by-product",null,null,null,{"$f":"Parameters!D1039","v":"n.a."}]
[null,null,null,null,"moisture content of by-product 1,process 1",null,null,null,{"$f":"Parameters!D1040","v":0},"%"]
[null,null,null,null,"by-product flow 1, process 1",null,null,null,{"$f":"Parameters!D1041","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 1, process 1",null,null,null,{"$f":"Parameters!D1071","v":0},"MJ.kgdm-1"]
[null,null,null,null,"secondary by-product",null,null,null,{"$f":"Parameters!D1042","v":"n.a."}]
[null,null,null,null,"moisture content of by-product 2,process 1",null,null,null,{"$f":"Parameters!D1043","v":0},"%"]
[null,null,null,null,"by-product flow 2, process 1",null,null,null,{"$f":"Parameters!D1044","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 2, process 1",null,null,null,{"$f":"Parameters!D1072","v":0},"MJ.kgdm-1"]
[null,null,null,null,"tertiary by-product",null,null,null,{"$f":"Parameters!D1045","v":"n.a."}]
[null,null,null,null,"moisture content of by-product 3,process 1",null,null,null,{"$f":"Parameters!D1046","v":0},"%"]
[null,null,null,null,"by-product flow 3, process 1",null,null,null,{"$f":"Parameters!D1047","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 3, process 1",null,null,null,{"$f":"Parameters!D1073","v":0},"MJ.kgdm-1"]
[null,null,null,null,"electricity by-product, process 1",null,null,null,{"$f":"Parameters!D1048","v":0},"MWh.year-1"]
[null,null,null,null,"heat by-product, process 1",null,null,null,{"$f":"Parameters!D1049","v":0},"MJ.year-1"]
[null,null,null,null,"type 1 of fuel/heat input",null,null,null,{"$f":"Parameters!D1131","v":"n.a."}]
[null,null,null,null,"fuel/heat input 1",null,null,null,{"$f":"Parameters!D1190","v":0},"MJ.year-1"]
[null,null,null,null,"type 2 of fuel/heat input",null,null,null,{"$f":"Parameters!D1132","v":"n.a."}]
[null,null,null,null,"fuel/heat input 2",null,null,null,{"$f":"Parameters!D1192","v":0},"MJ.year-1"]
[null,null,null,null,"type 1 of electricity input",null,null,null,{"$f":"Parameters!D1175","v":"n.a."}]
[null,null,null,null,"electricity flow 1",null,null,null,{"$f":"Parameters!D1168","v":0},"MWh.year-1"]
[null,null,null,null,"type 2 of electricity input",null,null,null,{"$f":"Parameters!D1176","v":"n.a."}]
[null,null,null,null,"electricity flow 2",null,null,null,{"$f":"Parameters!D1170","v":0},"MWh.year-1"]
[null,null,null,null,"type of main input",null,null,null,{"$f":"Parameters!D1089","v":"n.a."}]
[null,null,null,null,"main input, process 1",null,null,null,{"$f":"Parameters!D1101","v":0},"kg.year-1"]
[null,null,null,null,"energy content of main input, process 1",null,null,null,{"$f":"Parameters!D289","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type 1 of material input",null,null,null,{"$f":"Parameters!D1090","v":"n.a."}]
[null,null,null,null,"material input flow 1, process 1",null,null,null,{"$f":"Parameters!D1102","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 1, process 1",null,null,null,{"$f":"Parameters!D1105","v":0},"%"]
[null,null,null,null,"energy content of input flow 1, process 1",null,null,null,{"$f":"Parameters!D1106","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type 2 of material input",null,null,null,{"$f":"Parameters!D1091","v":"n.a."}]
[null,null,null,null,"material input flow 2, process 1",null,null,null,{"$f":"Parameters!D1107","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 2, process 1",null,null,null,{"$f":"Parameters!D1109","v":0},"%"]
[null,null,null,null,"energy content of input flow 2, process 1",null,null,null,{"$f":"Parameters!D1110","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type 3 of material input",null,null,null,{"$f":"Parameters!D1092","v":"n.a."}]
[null,null,null,null,"material input flow 3, process 1",null,null,null,{"$f":"Parameters!D1111","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 3, process 1",null,null,null,{"$f":"Parameters!D1113","v":0},"%"]
[null,null,null,null,"energy content of input flow 3, process 1",null,null,null,{"$f":"Parameters!D1114","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type of material output",null,null,null,{"$f":"Parameters!D1095","v":"n.a."}]
[null,null,null,null,"material output flow, process 1",null,null,null,{"$f":"Parameters!D1124","v":0},"kg.year-1"]
[null,null,null,null,"energy content of material output flow, process 1",null,null,null,{"$f":"Parameters!D1085","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type of material output (electricity), process 1",null,null,null,{"$f":"Parameters!D1096","v":"n.a."}]
[null,null,null,null,"type of material output (heat), process 1",null,null,null,{"$f":"Parameters!D1097","v":"n.a."}]
[]
[null,null,null,null,"Feedstock treatment and transport 2",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Drying and storage:",null,null,null,{"$f":"Parameters!D14","v":"n.a."}]
[null,null,null,null,"heat source",null,null,null,{"$f":"Parameters!D1276","v":"n.a."}]
[null,null,null,null,"heat use for drying",null,null,null,{"$f":"Parameters!D1275","v":0},"MJ.MJinput-1"]
[null,null,null,null,"electricity source",null,null,null,{"$f":"Parameters!D1278","v":"n.a."}]
[null,null,null,null,"electricity use for drying",null,null,null,{"$f":"Parameters!D1277","v":0},"MJ.MJinput-1"]
[null,null,null,null,"Feedstock transport:",null,null,null,{"$f":"Parameters!D13","v":"n.a."}]
[null,null,null,null,"transport mode 4",null,null,null,{"$f":"Parameters!D566","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D584","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D593","v":"n.a."}]
[null,null,null,null,"transport mode 5",null,null,null,{"$f":"Parameters!D567","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D585","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D594","v":"n.a."}]
[null,null,null,null,"transport mode 6",null,null,null,{"$f":"Parameters!D568","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D586","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D595","v":"n.a."}]
[]
[null,null,null,null,"Feedstock conversion 2",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Process 2",null,null,{"$f":"I276","v":"n.a."},{"$f":"Parameters!D15","v":"n.a."}]
[null,null,null,null,"main output flow of process 2",null,null,{"$f":"I277","v":"n.a."},{"$f":"Parameters!D1038","v":"n.a."}]
[null,null,null,null,"main by-product",null,null,null,{"$f":"Parameters!D1050","v":"n.a."}]
[null,null,null,null,"moisture content of by-product 1,process 2",null,null,null,{"$f":"Parameters!D1051","v":0},"%"]
[null,null,null,null,"by-product flow 1, process 2",null,null,null,{"$f":"Parameters!D1052","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 1, process 2",null,null,null,{"$f":"Parameters!D1074","v":0},"MJ.kgdm-1"]
[null,null,null,null,"secondary by-product",null,null,null,{"$f":"Parameters!D1053","v":"n.a."}]
[null,null,null,null,"moisture content of by-product 2,process 2",null,null,null,{"$f":"Parameters!D1054","v":0},"%"]
[null,null,null,null,"by-product flow 2, process 2",null,null,null,{"$f":"Parameters!D1055","v":0},"kg.year-1"]
[null,null,null,null,"energy content of by-product 2, process 2",null,null,null,{"$f":"Parameters!D1075","v":0},"MJ.kgdm-1"]
[null,null,null,null,"electricity by-product, process 2",null,null,null,{"$f":"Parameters!D1056","v":0},"MWh.year-1"]
[null,null,null,null,"heat by-product, process 2",null,null,null,{"$f":"Parameters!D1057","v":0},"MJ.year-1"]
[null,null,null,null,"type 1 of fuel/heat input",null,null,null,{"$f":"Parameters!D1133","v":"n.a."}]
[null,null,null,null,"fuel/heat input 1",null,null,null,{"$f":"Parameters!D1194","v":0},"MJ.year-1"]
[null,null,null,null,"type 2 of fuel/heat input",null,null,null,{"$f":"Parameters!D1134","v":"n.a."}]
[null,null,null,null,"fuel/heat input 2",null,null,null,{"$f":"Parameters!D1196","v":0},"MJ.year-1"]
[null,null,null,null,"type 1 of electricity input",null,null,null,{"$f":"Parameters!D1177","v":"n.a."}]
[null,null,null,null,"electricity flow 1",null,null,null,{"$f":"Parameters!D1172","v":0},"MWh.year-1"]
[null,null,null,null,"type 2 of electricity input",null,null,null,{"$f":"Parameters!D1178","v":"n.a."}]
[null,null,null,null,"electricity flow 2",null,null,null,{"$f":"Parameters!D1174","v":0},"MWh.year-1"]
[null,null,null,null,"type 1 of material input",null,null,null,{"$f":"Parameters!D1093","v":"n.a."}]
[null,null,null,null,"material input flow 1, process 2",null,null,null,{"$f":"Parameters!D1116","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 1, process 2",null,null,null,{"$f":"Parameters!D1117","v":0},"%"]
[null,null,null,null,"energy content of input flow 1, process 2",null,null,null,{"$f":"Parameters!D1118","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type 2 of material input",null,null,null,{"$f":"Parameters!D1094","v":"n.a."}]
[null,null,null,null,"material input flow 2, process 2",null,null,null,{"$f":"Parameters!D1120","v":0},"kg.year-1"]
[null,null,null,null,"moisture content of material input 2, process 2",null,null,null,{"$f":"Parameters!D1121","v":0},"%"]
[null,null,null,null,"energy content of input flow 2, process 2",null,null,null,{"$f":"Parameters!D1122","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type of material output",null,null,null,{"$f":"Parameters!D1098","v":"n.a."}]
[null,null,null,null,"material output flow, process 2",null,null,null,{"$f":"Parameters!D1128","v":0},"kg.year-1"]
[null,null,null,null,"energy content of material output flow, process 2",null,null,null,{"$f":"Parameters!D1086","v":0},"MJ.kgdm-1"]
[null,null,null,null,"type of material output (electricity), process 2",null,null,null,{"$f":"Parameters!D1099","v":"n.a."}]
[null,null,null,null,"type of material output (heat), process 2",null,null,null,{"$f":"Parameters!D1100","v":"n.a."}]
[]
[null,null,null,null,"Feedstock treatment and transport 3",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Drying and storage:",null,null,null,{"$f":"Parameters!D17","v":"n.a."}]
[null,null,null,null,"heat source",null,null,null,{"$f":"Parameters!D1283","v":"n.a."}]
[null,null,null,null,"heat use for drying",null,null,null,{"$f":"Parameters!D1282","v":0},"MJ.MJinput-1"]
[null,null,null,null,"electricity source",null,null,null,{"$f":"Parameters!D1285","v":"n.a."}]
[null,null,null,null,"electricity use for drying",null,null,null,{"$f":"Parameters!D1284","v":0},"MJ.MJinput-1"]
[null,null,null,null,"Feedstock transport:",null,null,null,{"$f":"Parameters!D16","v":"n.a."}]
[null,null,null,null,"transport mode 7",null,null,null,{"$f":"Parameters!D569","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D587","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D596","v":"n.a."}]
[null,null,null,null,"transport mode 8",null,null,null,{"$f":"Parameters!D570","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D588","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D597","v":"n.a."}]
[null,null,null,null,"transport mode 9",null,null,null,{"$f":"Parameters!D571","v":"n.a."}]
[null,null,null,null,"transport distance",null,null,null,{"$f":"Parameters!D589","v":0},"km"]
[null,null,null,null,"type of fuel",null,null,null,{"$f":"Parameters!D598","v":"n.a."}]
[]
[null,null,null,null,"Final conversion"]
[]
[null,null,null,null,"Conversion into final energy source",null,null,"User input","Default value","Unit"]
[null,null,null,null,"Final conversion process",null,null,{"$f":"I330","v":"No final conversion"},{"$f":"Parameters!D18","v":"No final conversion"}]
[null,null,null,null,"input flow from feedstock 1",null,null,{"$f":"Parameters!D666","v":"Crude palm oil"},{"$f":"Parameters!D667","v":"Palm stearin"}]
[null,null,null,null,"input flow from feedstock 2",null,null,{"$f":"I332","v":"n.a."},{"$f":"Parameters!D1038","v":"n.a."}]
[null,null,null,null,"share of input flow 1",null,null,null,{"$f":"Parameters!D1409","v":100},"%"]
[null,null,null,null,"share of input flow 2",null,null,null,{"$f":"Parameters!D1410","v":0},"%"]
[null,null,null,null,"net electrical efficiency of final conversion",null,null,null,{"$f":"Parameters!D1411","v":0},"%"]
[null,null,null,null,"net thermal efficiency of final conversion",null,null,null,{"$f":"Parameters!D1412","v":0},"%"]
[null,null,null,null,"net conversion efficiency, no electricity or heat",null,null,null,{"$f":"Parameters!D1413","v":100},"%"]
[null,null,null,null,"gross electrical efficiency of final conversion",null,null,null,null,"%"]
[null,null,null,null,"gross thermal efficiency of final conversion",null,null,null,null,"%"]
[null,null,null,null,"temperature of useful heat",null,null,null,{"$f":"Parameters!D1482","v":"n.a."},"°C"]
[null,null,null,null,"main by-product",null,null,null,{"$f":"Parameters!D1414","v":"n.a."}]
[null,null,null,null,"yield of main by-product",null,null,null,{"$f":"Parameters!D1418","v":0},"MJbyproduct.MJinput-1"]
[null,null,null,null,"secondary by-product",null,null,null,{"$f":"Parameters!D1415","v":"n.a."}]
[null,null,null,null,"yield of secondary by-product",null,null,null,{"$f":"Parameters!D1419","v":0},"MJbyproduct.MJinput-1"]
[null,null,null,null,"type 1 of fuel/heat input",null,null,null,{"$f":"Parameters!D1426","v":"n.a."}]
[null,null,null,null,"amount of fuel/heat input 1",null,null,null,{"$f":"Parameters!D1428","v":0},"MJ.MJinput-1"]
[null,null,null,null,"type 2 of fuel/heat input",null,null,null,{"$f":"Parameters!D1427","v":"n.a."}]
[null,null,null,null,"amount of fuel/heat input 2",null,null,null,{"$f":"Parameters!D1429","v":0},"MJ.MJinput-1"]
[null,null,null,null,"electricity source",null,null,null,{"$f":"Parameters!D1431","v":"n.a."}]
[null,null,null,null,"net electricity input",null,null,null,{"$f":"Parameters!D1430","v":0},"MJ.MJinput-1"]
[null,null,null,null,"type 1 of material input",null,null,"n.a.",{"$f":"Parameters!D1422","v":"n.a."}]
[null,null,null,null,"amount of material input 1",null,null,null,{"$f":"Parameters!D1424","v":0},"kg.MJinput-1"]
[null,null,null,null,"type 2 of material input",null,null,null,{"$f":"Parameters!D1423","v":"n.a."}]
[null,null,null,null,"amount of material input 2",null,null,null,{"$f":"Parameters!D1425","v":0},"kg.MJinput-1"]

{"sheet":"Indicators","index":3,"n_rows":51,"n_cols":11,"rows_kept":51,"cut":false,"hidden":true,"merged":[]}
[]
[]
[]
[]
[]
[]
[]
[null,"Selection of sustainability indicators"]
[]
[]
[null,null,null,null,null,null,null,null,null,"SELECT","   RED"]
[]
[null,null,null,null,"ECONOMICAL","ENERGY BALANCE",null,"fossil energy requirement"]
[]
[]
[null,null,null,null,"ENVIRONMENTAL","GLOBAL WARMING",null,"greenhouse gas balance",null,null,"þ"]
[null,null,null,null,null,null,null,"carbon debt and repayment time"]
[null,null,null,null,null,"RESOURCE USE",null,"use of water"]
[null,null,null,null,null,null,null,"use of land"]
[null,null,null,null,null,"ENVIRONMENTAL QUALITY",null,"acidification potential"]
[null,null,null,null,null,null,null,"eutrophication potential"]
[null,null,null,null,null,"BIODIVERSITY",null,"biodiversity and high carbon stocks",null,null,"þ"]
[]
[null,null,null,null,"SOCIAL","LOCAL WELL-BEING",null,"human and property rights"]
[null,null,null,null,null,null,null,"working conditions"]
[]
[]
[null,null,"FOSSIL ENERGY REQUIREMENT",null,"The total requirement of fossil energy throughout the whole life cycle, including fossil energy requirement for the production of input materials"]
[null,null,null,null,"It is calculated as the sum of fossil energy requirement throughout the life cycle [MJfossil/MJ]"]
[null,null,"NET ENERGY REQUIREMENT",null,"The total requirement of primary energy throughout the whole life cycle, including fossil energy requirement for the production of input materials"]
[null,null,null,null,"It is calculated as the total energy input over the total energy output [MJin/MJ]"]
[null,null,"GREENHOUSE GAS BALANCE",null,"The sum of greenhouse gas emissions (CO2, CH4, N2O) from the production of biomass fuels throughout the whole life cycle, including direct land use change"]
[null,null,null,null,"It is calculated conform the procedure in the EU Renewable Energy Directive and the report on solid biomass for electricity, heating and cooling [g CO2-eq/MJ]"]
[null,null,"CARBON DEBT",null,"The sum of carbon emissions related to direct land use change necessary to set up the bioenergy system"]
[null,null,null,null,"It is calculated conform the procedure in the EU Renewable Energy Directive and the report on solid biomass for electricity, heating and cooling [t CO2-eq/ha]"]
[null,null,"REPAYMENT TIME",null,"The time it takes to offset this carbon debt through reduced GHG emissions as a result of the use of the bioenergy system instead of the fossil reference system "]
[null,null,null,null,"It is calculated by dividing the total carbon debt by the annual emission reduction of the bioenergy system [years]"]
[null,null,"USE OF WATER",null,"The use of water throughout the life cycle of the bioenergy system, also called the water footprint"]
[null,null,null,null,"It is calculated as the cumulated use of water within each life cyle phase and related to local risk of water shortages [L/MJ]"]
[null,null,"USE OF LAND",null,"The use of land throughout the life cycle of the bioenergy system"]
[null,null,null,null,"It is calculated as the cumulated use of land within each life cyle phase [ha/MJ]"]
[null,null,"ACIDIFICATION POTENTIAL",null,"Atmospheric pollution arising from anthropogenically derived sulphur (S) and nitrogen (N) as NOx or ammonia"]
[null,null,null,null,"It is calculated as the sum of NH3, NOx and SOx emissions to air throughout the life cycle [g SO2-eq/MJ]"]
[null,null,"EUTROPHICATION POTENTIAL",null,"The artificial addition of nutrients, especially phosphates and nitrates, to the water bodies of the ecosystem"]
[null,null,null,null,"It is calculated as the sum of BOD, N and P emissions and flows to water ways and/or ground water [g PO4-eq/MJ]"]
[null,null,"BIODIVERSITY",null,"The impact of bio-energy production on land with high biodiversity and high carbon stock"]
[null,null,null,null,"It is checked conform the procedure in the EU Renewable Energy Directive and the report on solid biomass for electricity, heating and cooling []"]
[null,null,"HUMAN AND PROPERTY RIGHTS",null,"Violation risk of local human and property rights, including child labour"]
[null,null,null,null,"The outcome is a risk factor that gives an indication of the risk that one of the above issues is violated [risk factor]"]
[null,null,"WORKING CONDITIONS",null,"Violation risk of local working conditions, including health and safety at work, fair wages, legal contracts and workers rights"]
[null,null,null,null,"The outcome is a risk factor that gives an indication of the risk that one of the above issues is violated [risk factor]"]

{"sheet":"Input EB","index":4,"n_rows":23,"n_cols":24,"rows_kept":23,"cut":false,"hidden":true,"merged":[[8,1,8,28],[14,1,14,3],[17,1,17,3],[14,5,14,6],[14,8,14,9],[17,5,17,6],[17,8,17,9],[17,11,17,12],[14,11,14,12],[16,23,17,24],[14,14,14,15],[17,14,17,15],[14,17,14,18],[17,17,17,18],[14,20,14,21],[17,20,17,21]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Energy balance"]
[null,"The reduction of fossil energy dependence is a primary goal of the EU renewable energy strategy. It is therefore highly relevant to take this issue into account while evaluating the sustainability of energy systems. The FOSSIL ENERGY REQUIREMENT (FER) is calculated as the sum of all fossil energy requirements throughout the whole bio-energy production pathway, including the production of inputs.  The same calculation rules are adopted as for the greenhouse gas balance (laid down by the European Renewable Energy Directive. The fossil energy reduction is then calculated as the difference between the fossil energy requirements of the bio-energy system en the one of the fossil reference system. "]
[]
[null,"Project overview"]
[]
[]
[]
[null,{"$f":"Parameters!J2","v":"Palm oil (stearin) from palm fruits, refinery"},null,null,null,{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F2","v":"Transport of FFB to the mill"},null,null,{"$f":"Parameters!F4","v":"Production of Crude Palm Oil (CPO)"},null,null,{"$f":"Parameters!F5","v":"Transport of CPO to Belgium"},null,null,{"$f":"Parameters!F7","v":"Refinery of Crude Palm Oil"},null,null,{"$f":"Parameters!F8","v":"Transport of PS to the final conversion unit"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!F18","v":"No final conversion"}]
[null,{"$f":"Parameters!J3","v":"None"},null,null,null,{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F10","v":"n.a."},null,null,{"$f":"Parameters!F12","v":"n.a."},null,null,{"$f":"Parameters!F13","v":"n.a."},null,null,{"$f":"Parameters!F15","v":"n.a."},null,null,{"$f":"Parameters!F16","v":"n.a."}]
[]
[]
[null,"Project input data"]
[]
[null,"No additional project input data are required for this indicator."]

{"sheet":"Input Land use","index":5,"n_rows":209,"n_cols":24,"rows_kept":209,"cut":false,"hidden":false,"merged":[[158,3,159,11],[169,3,170,11],[14,20,14,21],[16,23,17,24],[17,1,17,3],[17,5,17,6],[17,8,17,9],[17,11,17,12],[17,14,17,15],[17,17,17,18],[17,20,17,21],[14,1,14,3],[14,5,14,6],[14,8,14,9],[14,11,14,12],[14,14,14,15],[14,17,14,18],[24,3,24,9],[24,10,24,15],[26,22,26,24],[80,3,80,9],[81,3,81,9],[82,3,82,9],[80,22,80,24],[54,3,54,9],[65,3,65,9],[54,10,54,15],[55,10,55,15],[50,10,50,15],[50,3,50,9],[25,10,25,15],[26,16,26,21],[25,22,25,24],[25,3,25,9],[53,3,53,8],[53,19,53,24],[53,9,53,18],[54,19,54,24],[55,19,55,24],[58,19,58,24],[59,19,59,24],[60,19,60,24],[63,3,64,11],[65,19,65,24],[56,19,56,24],[57,19,57,24],[62,19,62,24],[24,16,24,21],[24,22,24,24],[26,3,26,9],[42,8,42,11],[25,16,25,21],[48,16,48,21],[48,22,48,24],[50,16,50,21],[52,22,52,24],[41,8,41,11],[26,10,26,15],[29,5,29,11],[34,8,34,11],[35,8,35,11],[52,16,52,21],[51,3,51,9],[52,10,52,15],[48,3,48,9],[48,10,48,15],[46,5,47,14],[49,10,49,15],[49,3,49,9],[49,16,49,21],[74,3,75,11],[148,3,148,8],[148,9,148,18],[91,3,91,9],[79,10,79,15],[80,10,80,15],[81,10,81,15],[82,10,82,15],[83,10,83,15],[84,10,84,15],[87,10,87,15],[84,3,84,9],[87,3,87,9],[86,3,86,9],[86,10,86,15],[92,10,92,15],[89,10,89,15],[89,3,89,9],[81,16,81,21],[82,16,82,21],[84,16,84,21],[86,16,86,21],[87,16,87,21],[89,16,89,21],[76,3,76,9],[76,10,76,15],[77,16,77,21],[77,22,77,24],[78,16,78,21],[77,3,77,9],[78,3,78,9],[77,10,77,15],[78,10,78,15],[76,16,76,21],[76,22,76,24],[160,19,160,24],[155,19,155,24],[156,19,156,24],[157,19,157,24],[152,19,152,24],[153,19,153,24],[154,19,154,24],[68,19,68,24],[69,19,69,24],[70,19,70,24],[148,19,148,24],[95,22,95,24],[98,22,98,24],[99,22,99,24],[100,22,100,24],[96,22,96,24],[71,19,71,24],[72,19,72,24],[73,19,73,24],[81,22,81,24],[82,22,82,24],[92,16,92,21],[66,19,66,24],[67,19,67,24],[61,19,61,24],[78,22,78,24],[84,22,84,24],[86,22,86,24],[87,22,87,24],[89,22,89,24],[92,22,92,24],[80,16,80,21],[94,3,94,9],[104,3,104,9],[95,10,95,15],[96,10,96,15],[98,10,98,15],[99,10,99,15],[100,10,100,15],[101,10,101,15],[102,10,102,15],[103,10,103,15],[106,10,106,15],[108,10,108,15],[109,10,109,15],[110,10,110,15],[111,10,111,15],[112,10,112,15],[113,10,113,15],[101,22,101,24],[102,22,102,24],[103,22,103,24],[111,22,111,24],[112,22,112,24],[113,22,113,24],[110,22,110,24],[105,10,105,15],[105,22,105,24],[106,22,106,24],[108,22,108,24],[109,22,109,24],[119,3,119,9],[119,10,119,15],[119,16,119,21],[119,22,119,24],[120,3,120,9],[120,10,120,15],[120,16,120,21],[120,22,120,24],[121,3,121,9],[121,10,121,15],[121,16,121,21],[121,22,121,24],[124,5,124,11],[129,8,129,11],[130,8,130,11],[136,8,136,11],[144,3,144,9],[144,10,144,15],[144,16,144,21],[144,22,144,24],[137,8,137,11],[141,5,142,14],[143,10,143,15],[143,16,143,21],[143,3,143,9],[145,3,145,9],[145,10,145,15],[145,16,145,21],[146,3,146,9],[147,10,147,15],[147,16,147,21],[147,22,147,24],[171,3,171,9],[171,10,171,15],[171,16,171,21],[171,22,171,24],[166,19,166,24],[167,19,167,24],[168,19,168,24],[163,19,163,24],[164,19,164,24],[165,19,165,24],[162,19,162,24],[161,19,161,24],[149,3,149,9],[160,3,160,9],[149,19,149,24],[150,19,150,24],[151,19,151,24],[172,3,172,9],[172,10,172,15],[172,16,172,21],[172,22,172,24],[173,3,173,9],[173,10,173,15],[173,16,173,21],[173,22,173,24],[174,10,174,15],[175,3,175,9],[175,10,175,15],[175,16,175,21],[175,22,175,24],[176,3,176,9],[176,10,176,15],[176,16,176,21],[176,22,176,24],[177,3,177,9],[177,10,177,15],[177,16,177,21],[177,22,177,24],[178,10,178,15],[179,3,179,9],[179,10,179,15],[179,16,179,21],[179,22,179,24],[181,3,181,9],[181,10,181,15],[181,16,181,21],[181,22,181,24],[182,3,182,9],[182,10,182,15],[182,16,182,21],[182,22,182,24],[184,3,184,9],[184,10,184,15],[184,16,184,21],[184,22,184,24],[186,3,186,9],[187,10,187,15],[187,16,187,21],[187,22,187,24],[189,3,189,9],[190,10,190,15],[190,22,190,24],[191,10,191,15],[191,22,191,24],[193,10,193,15],[193,22,193,24],[194,10,194,15],[194,22,194,24],[195,10,195,15],[195,22,195,24],[196,10,196,15],[196,22,196,24],[197,10,197,15],[197,22,197,24],[198,10,198,15],[198,22,198,24],[205,10,205,15],[205,22,205,24],[206,10,206,15],[206,22,206,24],[207,10,207,15],[207,22,207,24],[208,10,208,15],[208,22,208,24],[199,3,199,9],[200,10,200,15],[200,22,200,24],[201,10,201,15],[201,22,201,24],[203,10,203,15],[203,22,203,24],[204,10,204,15],[204,22,204,24]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Land use "]
[]
[]
[null,"Project overview"]
[]
[]
[]
[null,{"$f":"Parameters!J2","v":"Palm oil (stearin) from palm fruits, refinery"},null,null,null,{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F2","v":"Transport of FFB to the mill"},null,null,{"$f":"Parameters!F4","v":"Production of Crude Palm Oil (CPO)"},null,null,{"$f":"Parameters!F5","v":"Transport of CPO to Belgium"},null,null,{"$f":"Parameters!F7","v":"Refinery of Crude Palm Oil"},null,null,{"$f":"Parameters!F8","v":"Transport of PS to the final conversion unit"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!F18","v":"No final conversion"}]
[null,{"$f":"Parameters!J3","v":"None"},null,null,null,{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F10","v":"n.a."},null,null,{"$f":"Parameters!F12","v":"n.a."},null,null,{"$f":"Parameters!F13","v":"n.a."},null,null,{"$f":"Parameters!F15","v":"n.a."},null,null,{"$f":"Parameters!F16","v":"n.a."}]
[]
[]
[null,"Project input data"]
[]
[null,null,null,"Feedstock pathway 1"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"climate",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D103","v":"Tropical Wet"}]
[null,null,null,"soil type",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D104","v":"Low activity clay soils"}]
[null,null,null,null,"search climate and soil type:"]
[null,null,null,null,null,"• search coordinates through location/address:"]
[]
[]
[]
[]
[null,null,null,null,null,"• or insert coordinates manually:"]
[null,null,null,null,null,"longitude"]
[null,null,null,null,null,"latitude"]
[]
[]
[]
[null,null,null,null,null,"(search takes approximately 15 seconds)"]
[]
[null,null,null,null,null,"climate"]
[null,null,null,null,null,"soil type"]
[]
[null,null,null,null,null,"In case the retrieved answer for soil type is \"Other Areas\", see:"]
[null,null,null,null,null,"In case the retrieved answer for soil type is \"Organic\", see: "]
[null,null,null,null,null,"! Do not forget to insert these results in the user input fields above."]
[]
[null,null,null,"Organic soil",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D186=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Soil water saturation",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D183=1,\"yes\",\"no\")","v":"yes"}]
[null,null,null,"Previously degraded land",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D150=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Only for organic soils:"]
[null,null,null,null,"Nutrient level",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D187","v":"n.a."}]
[null,null,null,null,null,null,null,null,null,"User input",null,null,null,null,null,null,null,null,null,"Default value"]
[null,null,null,"Actual land use",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D99","v":"Perennial cropland"}]
[null,null,null,null,"Management type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D152","v":"No till"}]
[null,null,null,null,"Input",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D154","v":"High without manure"}]
[null,null,null,null,"Actual land use - more specific",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D101","v":"Oil palm"}]
[null,null,null,null,"Domain",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D156","v":"n.a."}]
[null,null,null,null,"Climate (specific for IPCC carbon calc.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D105","v":"Tropical wet"}]
[null,null,null,null,"Ecological zone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D158","v":"n.a."}]
[null,null,null,null,"Continent",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D160","v":"n.a."}]
[null,null,null,null,"Type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D162","v":"n.a."}]
[null,null,null,"! If other than default: all parameters must be filled in."]
[]
[null,null,null,"Previous land use (January 1st, 2008)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D100","v":"Perennial cropland"}]
[null,null,null,null,"Management type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D153","v":"No till"}]
[null,null,null,null,"Input",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D155","v":"High without manure"}]
[null,null,null,null,"Previous land use - more specific",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D102","v":"Oil palm"}]
[null,null,null,null,"Domain",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D157","v":"n.a."}]
[null,null,null,null,"Climate (specific for IPCC carbon calc.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D106","v":"Tropical wet"}]
[null,null,null,null,"Ecological zone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D159","v":"n.a."}]
[null,null,null,null,"Continent",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D161","v":"n.a."}]
[null,null,null,null,"Type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D163","v":"n.a."}]
[null,null,null,"! If other than default: all parameters must be filled in."]
[]
[null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Field renewal",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D184","v":1},null,null,null,null,null,"years"]
[null,null,null,"Amount of animal manure N applied to soil",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D189","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,null,"(other than by grazing animals)"]
[null,null,null,"Amount of total sewage N applied to soil",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D190","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,"Amount of total compost N applied to soil",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D191","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,"Amount of N of other organic amendments",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D192","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,null,"applied to soil (used as fertiliser)"]
[null,null,null,"Amount of N-fixing crop residue applied",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D176","v":45},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,null,"to soil"]
[null,null,null,"Fraction of above-ground residues removed",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D204","v":0},null,null,null,null,null,"%"]
[null,null,null,"Ratio of above-ground residues to",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D195","v":0.33333333333333331},null,null,null,null,null,"kgfm.kgfm-1"]
[null,null,null,null,"harvested yield"]
[null,null,null,"Ratio of below-ground residues to",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D200","v":0},null,null,null,null,null,"kgfm.kgfm-1"]
[null,null,null,null,"harvested yield"]
[null,null,null,"Only for oil palm:"]
[null,null,null,null,"Amount of residues returned to field",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D185","v":0.22},null,null,null,null,null,"kgdm.kgfm-1"]
[null,null,null,"This section should only be filled in when data are available for ALL PARAMETERS:"]
[null,null,null,"Actual land use"]
[null,null,null,null,"Weight of below ground living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"OR: Ratio of below ground carbon stock ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tC-1"]
[null,null,null,null,null,"to above ground carbon stock"]
[null,null,null,null,"Weight of above ground living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"Weight of dead wood pool",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"Weight of litter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"C fraction of dry matter in living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,null,"C fraction of dry matter in dead wood",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,null,"C fraction of dry matter in litter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,"Previous land use (January 1st, 2008)"]
[null,null,null,null,"Weight of below ground living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"OR: Ratio of below ground carbon stock ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tC-1"]
[null,null,null,null,null,"to above ground carbon stock"]
[null,null,null,null,"Weight of above ground living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"Weight of dead wood pool",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"Weight of litter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"C fraction of dry matter in living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,null,"C fraction of dry matter in dead wood",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,null,"C fraction of dry matter in litter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[]
[]
[]
[null,null,null,"Feedstock pathway 2"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"climate",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D324","v":"n.a."}]
[null,null,null,"soil type",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D325","v":"n.a."}]
[null,null,null,null,"search climate and soil type:"]
[null,null,null,null,null,"• search coordinates through location/address:"]
[null,null,null,null,null,"belgium"]
[]
[]
[]
[null,null,null,null,null,"• or insert coordinates manually:"]
[null,null,null,null,null,"longitude"]
[null,null,null,null,null,"latitude"]
[]
[]
[]
[null,null,null,null,null,"(search takes approximately 15 seconds)"]
[]
[null,null,null,null,null,"climate"]
[null,null,null,null,null,"soil type"]
[]
[null,null,null,null,null,"In case the retrieved answer for soil type is \"Other Areas\", see:"]
[null,null,null,null,null,"In case the retrieved answer for soil type is \"Organic\", see: "]
[null,null,null,null,null,"! Do not forget to insert these results in the user input fields above."]
[]
[null,null,null,"Organic soil",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D407=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Soil water saturation",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D404=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Previously degraded land",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D371=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Only for organic soils:"]
[null,null,null,null,"Nutrient level",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D408","v":"n.a."}]
[null,null,null,null,null,null,null,null,null,"User input",null,null,null,null,null,null,null,null,null,"Default value"]
[null,null,null,"Actual land use",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D320","v":"n.a."}]
[null,null,null,null,"Management type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D373","v":"n.a."}]
[null,null,null,null,"Input",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D375","v":"n.a."}]
[null,null,null,null,"Actual land use - more specific",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D322","v":"n.a."}]
[null,null,null,null,"Domain",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D377","v":"n.a."}]
[null,null,null,null,"Climate (specific for IPCC carbon calc.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D326","v":"n.a."}]
[null,null,null,null,"Ecological zone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D379","v":"n.a."}]
[null,null,null,null,"Continent",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D381","v":"n.a."}]
[null,null,null,null,"Type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D383","v":"n.a."}]
[null,null,null,"! If other than default: all parameters must be filled in."]
[]
[null,null,null,"Previous land use (January 1st, 2008)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D321","v":"n.a."}]
[null,null,null,null,"Management type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D374","v":"n.a."}]
[null,null,null,null,"Input",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D376","v":"n.a."}]
[null,null,null,null,"Previous land use - more specific",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D323","v":"n.a."}]
[null,null,null,null,"Domain",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D378","v":"n.a."}]
[null,null,null,null,"Climate (specific for IPCC carbon calc.)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D327","v":"n.a."}]
[null,null,null,null,"Ecological zone",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D380","v":"n.a."}]
[null,null,null,null,"Continent",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D382","v":"n.a."}]
[null,null,null,null,"Type",null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D384","v":"n.a."}]
[null,null,null,"! If other than default: all parameters must be filled in."]
[]
[null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Field renewal",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D405","v":0},null,null,null,null,null,"years"]
[null,null,null,"Amount of animal manure N applied to soil",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D410","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,null,"(other than by grazing animals)"]
[null,null,null,"Amount of total sewage N applied to soil",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D411","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,"Amount of total compost N applied to soil",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D412","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,"Amount of N of other organic amendments",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D413","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,null,"applied to soil (used as fertiliser)"]
[null,null,null,"Amount of N-fixing crop residue applied",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D397","v":0},null,null,null,null,null,"kgN.ha-1.y-1"]
[null,null,null,null,"to soil"]
[null,null,null,"Fraction of above-ground residues removed",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D425","v":0},null,null,null,null,null,"%"]
[null,null,null,"Ratio of above-ground residues to",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D416","v":0},null,null,null,null,null,"kgfm.kgfm-1"]
[null,null,null,null,"harvested yield"]
[null,null,null,"Ratio of below-ground residues to",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D421","v":0},null,null,null,null,null,"kgfm.kgfm-1"]
[null,null,null,null,"harvested yield"]
[null,null,null,"Only for oil palm:"]
[null,null,null,null,"Amount of residues returned to field",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D406","v":0},null,null,null,null,null,"kgdm.kgfm-1"]
[null,null,null,"This section should only be filled in when data are available for ALL PARAMETERS:"]
[null,null,null,"Actual land use"]
[null,null,null,null,"Weight of below ground living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"OR: Ratio of below ground carbon stock ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tC-1"]
[null,null,null,null,null,"to above ground carbon stock"]
[null,null,null,null,"Weight of above ground living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"Weight of dead wood pool",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"Weight of litter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"C fraction of dry matter in living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,null,"C fraction of dry matter in dead wood",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,null,"C fraction of dry matter in litter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,"Previous land use (January 1st, 2008)"]
[null,null,null,null,"Weight of below ground living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"OR: Ratio of below ground carbon stock ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tC-1"]
[null,null,null,null,null,"to above ground carbon stock"]
[null,null,null,null,"Weight of above ground living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"Weight of dead wood pool",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"Weight of litter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"t.ha-1.y-1"]
[null,null,null,null,"C fraction of dry matter in living biomass",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,null,"C fraction of dry matter in dead wood",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]
[null,null,null,null,"C fraction of dry matter in litter",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"tC.tdm-1"]

{"sheet":"Input RU","index":6,"n_rows":69,"n_cols":24,"rows_kept":69,"cut":false,"hidden":true,"merged":[[17,20,17,21],[19,23,20,24],[20,1,20,3],[20,5,20,6],[20,8,20,9],[20,11,20,12],[20,14,20,15],[20,17,20,18],[20,20,20,21],[17,1,17,3],[17,5,17,6],[17,8,17,9],[17,11,17,12],[17,14,17,15],[17,17,17,18],[31,3,31,9],[31,10,31,15],[31,16,31,21],[31,22,31,24],[32,3,32,9],[32,10,32,15],[32,16,32,21],[32,22,32,24],[27,3,27,9],[27,10,27,15],[27,16,27,21],[27,22,27,24],[29,3,29,9],[29,10,29,15],[29,16,29,21],[29,22,29,24],[28,3,28,9],[28,10,28,15],[28,16,28,21],[28,22,28,24],[37,3,37,9],[37,10,37,15],[37,16,37,21],[37,22,37,24],[34,3,34,9],[34,10,34,15],[34,16,34,21],[34,22,34,24],[35,3,35,9],[35,10,35,15],[35,16,35,21],[35,22,35,24],[41,3,41,9],[41,10,41,15],[41,16,41,21],[41,22,41,24],[43,3,43,9],[43,10,43,15],[43,16,43,21],[43,22,43,24],[38,3,38,9],[38,10,38,15],[38,16,38,21],[38,22,38,24],[40,3,40,9],[40,10,40,15],[40,16,40,21],[40,22,40,24],[49,3,49,9],[49,10,49,15],[49,16,49,21],[49,22,49,24],[51,3,51,9],[51,10,51,15],[51,16,51,21],[51,22,51,24],[44,3,44,9],[44,10,44,15],[44,16,44,21],[44,22,44,24],[47,3,47,9],[47,10,47,15],[47,16,47,21],[47,22,47,24],[48,3,48,9],[48,10,48,15],[48,16,48,21],[48,22,48,24],[55,3,55,9],[55,10,55,15],[55,16,55,21],[55,22,55,24],[57,3,57,9],[57,10,57,15],[57,16,57,21],[57,22,57,24],[52,3,52,9],[52,10,52,15],[52,16,52,21],[52,22,52,24],[54,3,54,9],[54,10,54,15],[54,16,54,21],[54,22,54,24],[61,3,61,9],[61,10,61,15],[61,16,61,21],[61,22,61,24],[63,3,63,9],[63,10,63,15],[63,16,63,21],[63,22,63,24],[58,3,58,9],[58,10,58,15],[58,16,58,21],[58,22,58,24],[60,3,60,9],[60,10,60,15],[60,16,60,21],[60,22,60,24],[68,3,68,9],[68,10,68,15],[68,16,68,21],[68,22,68,24],[64,3,64,9],[64,10,64,15],[64,16,64,21],[64,22,64,24],[67,3,67,9],[67,10,67,15],[67,16,67,21],[67,22,67,24]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Resource use"]
[null,"Resources are part of the backbone of an economy and unsustainable use of valuable resources can endanger the carrying capacity of the environment and limit access for future generations. The resources that "]
[null,"are considered here are fresh water and land. The use of land is principally related to the cultivation stage of the biomass as the area of land used for storage facilities and infrastructure is very small and thus "]
[null,"negligible. The use of water is related to both the cultivation and the processing of the biomass and is significantly influenced by climatic conditions and agricultural practices."]
[null,"Whether the use of these resources is sustainable or not also depends on its local availability. Resource use must therefore be checked with local situations."]
[]
[null,"Project overview"]
[]
[]
[]
[null,{"$f":"Parameters!J2","v":"Palm oil (stearin) from palm fruits, refinery"},null,null,null,{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F2","v":"Transport of FFB to the mill"},null,null,{"$f":"Parameters!F4","v":"Production of Crude Palm Oil (CPO)"},null,null,{"$f":"Parameters!F5","v":"Transport of CPO to Belgium"},null,null,{"$f":"Parameters!F7","v":"Refinery of Crude Palm Oil"},null,null,{"$f":"Parameters!F8","v":"Transport of PS to the final conversion unit"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!F18","v":"No final conversion"}]
[null,{"$f":"Parameters!J3","v":"None"},null,null,null,{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F10","v":"n.a."},null,null,{"$f":"Parameters!F12","v":"n.a."},null,null,{"$f":"Parameters!F13","v":"n.a."},null,null,{"$f":"Parameters!F15","v":"n.a."},null,null,{"$f":"Parameters!F16","v":"n.a."}]
[]
[]
[null,"Project input data"]
[]
[null,null,null,"Feedstock pathway 1"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Country of production",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D21","v":"Malaysia"},null,null,null,null,null,"-"]
[null,null,null,"Fresh water use for feedstock production",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D165","v":22067.5},null,null,null,null,null,"m³.ha-1"]
[]
[null,null,null,"Feedstock treatment and transport 1",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for storage 1",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D169","v":0},null,null,null,null,null,"m³.kgfm-1"]
[]
[null,null,null,"Feedstock conversion 1",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for conversion 1",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D979","v":0},null,null,null,null,null,"m³.MJoutput-1"]
[]
[null,null,null,"Feedstock treatment and transport 2",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for storage 2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D981","v":0},null,null,null,null,null,"m³.MJinput-1"]
[]
[null,null,null,"Feedstock conversion 2",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for conversion 2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D983","v":0},null,null,null,null,null,"m³.MJoutput-1"]
[]
[null,null,null,"Feedstock treatment and transport 3",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for storage 3",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D985","v":0},null,null,null,null,null,"m³.MJinput-1"]
[]
[null,null,null,"Feedstock pathway 2"]
[null,null,null,"Feedstock production",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Country of production",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D242","v":"n.a."},null,null,null,null,null,"-"]
[null,null,null,"Fresh water use for feedstock production",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D386","v":0},null,null,null,null,null,"m³.ha-1"]
[]
[null,null,null,"Feedstock treatment and transport 1",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for storage 1",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D390","v":0},null,null,null,null,null,"m³.kgfm-1"]
[]
[null,null,null,"Feedstock conversion 1",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for conversion 1",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1349","v":0},null,null,null,null,null,"m³.MJoutput-1"]
[]
[null,null,null,"Feedstock treatment and transport 2",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for storage 2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1351","v":0},null,null,null,null,null,"m³.MJinput-1"]
[]
[null,null,null,"Feedstock conversion 2",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for conversion 2",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1353","v":0},null,null,null,null,null,"m³.MJoutput-1"]
[]
[null,null,null,"Feedstock treatment and transport 3",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for storage 3",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1355","v":0},null,null,null,null,null,"m³.MJinput-1"]
[]
[null,null,null,"Final conversion"]
[null,null,null,"Conversion into final energy source",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Fresh water use for final conversion",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1555","v":0},null,null,null,null,null,"m³.MJinput-1"]

{"sheet":"Input EQ","index":7,"n_rows":75,"n_cols":24,"rows_kept":75,"cut":false,"hidden":true,"merged":[[50,22,50,24],[51,22,51,24],[52,22,52,24],[53,22,53,24],[71,22,71,24],[72,22,72,24],[73,22,73,24],[74,22,74,24],[62,22,62,24],[63,22,63,24],[64,22,64,24],[69,22,69,24],[70,22,70,24],[67,22,67,24],[74,16,74,21],[61,16,61,21],[62,16,62,21],[63,16,63,21],[64,16,64,21],[69,16,69,21],[53,16,53,21],[54,16,54,21],[55,16,55,21],[59,16,59,21],[60,16,60,21],[67,16,67,21],[30,10,30,15],[31,10,31,15],[32,10,32,15],[31,22,31,24],[30,22,30,24],[70,16,70,21],[71,16,71,21],[72,16,72,21],[73,16,73,21],[43,16,43,21],[44,16,44,21],[50,16,50,21],[51,16,51,21],[52,16,52,21],[35,16,35,21],[39,16,39,21],[35,22,35,24],[34,22,34,24],[33,22,33,24],[32,22,32,24],[54,22,54,24],[55,22,55,24],[59,22,59,24],[60,22,60,24],[74,10,74,15],[61,10,61,15],[62,10,62,15],[63,10,63,15],[64,10,64,15],[69,10,69,15],[67,10,67,15],[30,16,30,21],[31,16,31,21],[32,16,32,21],[33,16,33,21],[34,16,34,21],[70,10,70,15],[53,10,53,15],[54,10,54,15],[55,10,55,15],[59,10,59,15],[60,10,60,15],[43,10,43,15],[44,10,44,15],[50,10,50,15],[51,10,51,15],[52,10,52,15],[35,10,35,15],[33,10,33,15],[34,10,34,15],[70,3,70,9],[71,3,71,9],[72,3,72,9],[73,3,73,9],[43,3,43,9],[44,3,44,9],[50,3,50,9],[51,3,51,9],[52,3,52,9],[35,3,35,9],[39,3,39,9],[40,3,40,9],[41,3,41,9],[42,3,42,9],[48,10,48,15],[71,10,71,15],[72,10,72,15],[73,10,73,15],[39,10,39,15],[40,10,40,15],[41,10,41,15],[42,10,42,15],[30,3,30,9],[31,3,31,9],[32,3,32,9],[33,3,33,9],[34,3,34,9],[74,3,74,9],[61,3,61,9],[62,3,62,9],[63,3,63,9],[64,3,64,9],[69,3,69,9],[53,3,53,9],[54,3,54,9],[55,3,55,9],[59,3,59,9],[60,3,60,9],[67,3,67,9],[48,3,48,9],[68,3,68,9],[68,10,68,15],[68,16,68,21],[68,22,68,24],[57,3,57,9],[57,10,57,15],[57,16,57,21],[57,22,57,24],[58,3,58,9],[58,10,58,15],[58,16,58,21],[58,22,58,24],[61,22,61,24],[48,16,48,21],[48,22,48,24],[49,3,49,9],[49,10,49,15],[49,16,49,21],[49,22,49,24],[37,3,37,9],[37,10,37,15],[37,16,37,21],[37,22,37,24],[38,3,38,9],[38,10,38,15],[38,16,38,21],[38,22,38,24],[40,16,40,21],[41,16,41,21],[42,16,42,21],[39,22,39,24],[40,22,40,24],[41,22,41,24],[42,22,42,24],[43,22,43,24],[44,22,44,24],[28,3,28,9],[28,10,28,15],[28,16,28,21],[28,22,28,24],[29,3,29,9],[29,10,29,15],[29,16,29,21],[29,22,29,24],[19,20,19,21],[21,23,22,24],[22,1,22,3],[22,5,22,6],[22,8,22,9],[22,11,22,12],[22,14,22,15],[22,17,22,18],[22,20,22,21],[19,1,19,3],[19,5,19,6],[19,8,19,9],[19,11,19,12],[19,14,19,15],[19,17,19,18]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Environmental quality"]
[null,"The impact of a system on environmental quality is expressed in terms of acidification and eutrophication potential. Acidifying pollutants have a wide variety of impacts on soil, groundwater, surface waters, "]
[null,"biological organisms and ecosystems and can cause species mortality and ecosystem decline. Eutrophication covers all potential impacts of increased environmental levels of macronutrients which can cause"]
[null,"an undesirable alteration in species composition and excessive biomass growth in both aquatic and terrestrial ecosystems."]
[null,"The acidification potential (AP) of a bioenergy production system is defined as the sum of the APs of the ammonia (NH3), nitrogen oxide (NOx) and sulphur oxide (SOx) emissions to air throughout the entire "]
[null,"production chain. The AP is expressed in g SO2 equivalents. In the same way as for global warming, the AP of a certain mass of a substance is expressed against the AP of a similar mass of SO2. The eutrophication "]
[null,"potential (EP) is the sum of COD (chemical oxygen demand), nitrogen (N) and phosphorus (P) emissions and flows to water ways and/or ground water. The EP is expressed in g PO43- equivalents."]
[]
[null,"Project overview"]
[]
[]
[]
[null,{"$f":"Parameters!J2","v":"Palm oil (stearin) from palm fruits, refinery"},null,null,null,{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F2","v":"Transport of FFB to the mill"},null,null,{"$f":"Parameters!F4","v":"Production of Crude Palm Oil (CPO)"},null,null,{"$f":"Parameters!F5","v":"Transport of CPO to Belgium"},null,null,{"$f":"Parameters!F7","v":"Refinery of Crude Palm Oil"},null,null,{"$f":"Parameters!F8","v":"Transport of PS to the final conversion unit"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!F18","v":"No final conversion"}]
[null,{"$f":"Parameters!J3","v":"None"},null,null,null,{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F10","v":"n.a."},null,null,{"$f":"Parameters!F12","v":"n.a."},null,null,{"$f":"Parameters!F13","v":"n.a."},null,null,{"$f":"Parameters!F15","v":"n.a."},null,null,{"$f":"Parameters!F16","v":"n.a."}]
[]
[]
[null,"Project input data"]
[null,null,null,"Feedstock pathway 1"]
[]
[null,null,null,"Feedstock conversion 1",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D773","v":0},null,null,null,null,null,"gNOX . MJoutput-1"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D774","v":0},null,null,null,null,null,"gSOX . MJoutput-1"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D775","v":0},null,null,null,null,null,"gNH3 . MJoutput-1"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D776","v":0},null,null,null,null,null,"gNO3- . MJoutput-1"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D777","v":0},null,null,null,null,null,"gNH4+ . MJoutput-1"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D778","v":0},null,null,null,null,null,"gPO43- . MJoutput-1"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D779","v":20},null,null,null,null,null,"gCOD . MJoutput-1"]
[]
[null,null,null,"Feedstock conversion 2",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D780","v":0},null,null,null,null,null,"gNOX . MJoutput-1"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D781","v":0},null,null,null,null,null,"gSOX . MJoutput-1"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D782","v":0},null,null,null,null,null,"gNH3 . MJoutput-1"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D783","v":0},null,null,null,null,null,"gNO3- . MJoutput-1"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D784","v":0},null,null,null,null,null,"gNH4+ . MJoutput-1"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D785","v":0},null,null,null,null,null,"gPO43- . MJoutput-1"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D786","v":0},null,null,null,null,null,"gCOD . MJoutput-1"]
[]
[null,null,null,"Feedstock pathway 2"]
[]
[null,null,null,"Feedstock conversion 1",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1143","v":0},null,null,null,null,null,"gNOX . MJoutput-1"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1144","v":0},null,null,null,null,null,"gSOX . MJoutput-1"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1145","v":0},null,null,null,null,null,"gNH3 . MJoutput-1"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1146","v":0},null,null,null,null,null,"gNO3- . MJoutput-1"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1147","v":0},null,null,null,null,null,"gNH4+ . MJoutput-1"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1148","v":0},null,null,null,null,null,"gPO43- . MJoutput-1"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1149","v":0},null,null,null,null,null,"gCOD . MJoutput-1"]
[]
[null,null,null,"Feedstock conversion 2",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1150","v":0},null,null,null,null,null,"gNOX . MJoutput-1"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1151","v":0},null,null,null,null,null,"gSOX . MJoutput-1"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1152","v":0},null,null,null,null,null,"gNH3 . MJoutput-1"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1153","v":0},null,null,null,null,null,"gNO3- . MJoutput-1"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1154","v":0},null,null,null,null,null,"gNH4+ . MJoutput-1"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1155","v":0},null,null,null,null,null,"gPO43- . MJoutput-1"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1156","v":0},null,null,null,null,null,"gCOD . MJoutput-1"]
[]
[null,null,null,"Final conversion"]
[null,null,null,"Conversion into final energy source",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1467","v":0},null,null,null,null,null,"gNOX . MJoutput-1"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1468","v":0},null,null,null,null,null,"gSOX . MJoutput-1"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1469","v":0},null,null,null,null,null,"gNH3 . MJoutput-1"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1470","v":0},null,null,null,null,null,"gNO3- . MJoutput-1"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1471","v":0},null,null,null,null,null,"gNH4+ . MJoutput-1"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1472","v":0},null,null,null,null,null,"gPO43- . MJoutput-1"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1473","v":0},null,null,null,null,null,"gCOD . MJoutput-1"]

{"sheet":"Input Bio","index":8,"n_rows":129,"n_cols":24,"rows_kept":129,"cut":false,"hidden":false,"merged":[[44,9,44,10],[123,3,123,9],[127,3,127,9],[127,10,127,11],[72,3,72,9],[85,10,85,15],[86,4,86,24],[89,5,89,11],[94,8,94,11],[95,8,95,11],[97,3,97,9],[62,4,62,24],[82,22,82,24],[80,22,80,24],[59,22,59,24],[79,22,79,24],[56,22,56,24],[58,22,58,24],[99,9,99,10],[130,3,130,9],[111,3,111,9],[111,16,111,21],[111,22,111,24],[113,3,113,9],[113,10,113,15],[113,16,113,21],[113,22,113,24],[114,3,114,9],[114,16,114,21],[114,22,114,24],[115,10,115,15],[115,16,115,21],[117,4,117,24],[34,5,34,11],[39,8,39,11],[40,8,40,11],[42,3,42,9],[46,3,46,9],[51,3,51,9],[82,3,82,9],[82,10,82,15],[82,16,82,21],[58,16,58,21],[59,16,59,21],[60,3,60,9],[72,10,72,11],[80,3,80,15],[80,16,80,21],[56,16,56,21],[60,16,60,21],[79,3,79,9],[79,10,79,15],[79,16,79,21],[64,3,64,9],[68,3,68,9],[75,3,75,9],[60,10,60,15],[24,3,24,9],[24,10,24,15],[24,16,24,21],[9,1,9,25],[14,20,14,21],[16,23,17,24],[17,1,17,3],[17,5,17,6],[17,8,17,9],[17,11,17,12],[17,14,17,15],[17,17,17,18],[17,20,17,21],[14,1,14,3],[14,5,14,6],[14,8,14,9],[14,11,14,12],[14,14,14,15],[14,17,14,18],[25,16,25,21],[27,10,27,15],[28,10,28,15],[29,10,29,15],[25,22,25,24],[25,3,25,15],[27,22,27,24],[28,22,28,24],[29,22,29,24],[27,3,27,9],[28,3,28,9],[29,3,29,9],[27,16,27,21],[28,16,28,21],[29,16,29,21],[8,1,8,28],[111,10,111,15],[119,3,119,9],[114,10,114,15],[115,3,115,9],[83,3,83,9],[83,10,83,15],[83,16,83,21],[83,22,83,24],[84,3,84,9],[84,10,84,15],[84,16,84,21],[84,22,84,24],[101,3,101,9],[106,3,106,9],[30,10,30,15],[56,10,56,15],[58,10,58,15],[59,10,59,15],[56,3,56,9],[58,3,58,9],[59,3,59,9],[31,4,31,24],[24,22,24,24]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Biodiversity and high carbon stocks"]
[null,"The term biodiversity covers every form of life on the planet (plants, animals, fungi and micro-organisms), the diversity of communities that they form and the habitats in which they live (TEEB, 2011). The loss of biodiversity can destabilize ecosystems and ultimately cause changes in the services they provide, involving direct impacts and costs for human society.\nIf land with high carbon stocks in soil or vegetation is converted for the cultivation of biomass for energy, the stored carbon will partially be released into the atmosphere, leading to the formation of CO2.\nTo assess the impact of bio-energy production on biodiversity and high carbon stocks, sustainability requirements of the Renewable Energy Directive (2009/28/EC) are followed. These requirements comprise:\n• biomass should not be obtained from undisturbed forests, highly biodiverse grassland or nature protection areas (LAND WITH HIGH BIODIVERSITY VALUE)\n• biomass should not be obtained from the conversion of wetlands, peatland and continuously forested areas beyond 2008 (LAND WITH HIGH CARBON STOCK)\nThe Renewable Energy Directive provides sustainability requirements but does not offer any means to ascertain them. \nIn first instance the user should try to obtain specific data from the biomass supplier. What kind of land is used for biomass production and what was its status on 1 January 2008?\n"]
[]
[null,"Project overview"]
[]
[]
[]
[null,{"$f":"Parameters!J2","v":"Palm oil (stearin) from palm fruits, refinery"},null,null,null,{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F2","v":"Transport of FFB to the mill"},null,null,{"$f":"Parameters!F4","v":"Production of Crude Palm Oil (CPO)"},null,null,{"$f":"Parameters!F5","v":"Transport of CPO to Belgium"},null,null,{"$f":"Parameters!F7","v":"Refinery of Crude Palm Oil"},null,null,{"$f":"Parameters!F8","v":"Transport of PS to the final conversion unit"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!F18","v":"No final conversion"}]
[null,{"$f":"Parameters!J3","v":"None"},null,null,null,{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F10","v":"n.a."},null,null,{"$f":"Parameters!F12","v":"n.a."},null,null,{"$f":"Parameters!F13","v":"n.a."},null,null,{"$f":"Parameters!F15","v":"n.a."},null,null,{"$f":"Parameters!F16","v":"n.a."}]
[]
[]
[null,"Project input data"]
[]
[null,null,null,"Feedstock pathway 1"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Land with high biodiversity value"]
[null,null,null,"Is the biomass obtained from land that had one of the following statusses in or after January 2008, whether or not the land continues to have that status:"]
[null,null,null,"Undisturbed forest",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D217=1,\"yes\",\"no\")","v":"yes"}]
[null,null,null,"Nature protection area",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D218=1,\"yes\",\"no\")","v":"yes"}]
[null,null,null,"Highly biodiverse grassland",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D219=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Search data:"]
[null,null,null,null,"In case no specific or reliable data can be obtained from the biomass supplier itself, this section offers online or linked databases that can be useful to assess the fulfilment of the particular requirements for land with high biodiversity value."]
[]
[null,null,null,null,null,"• search coordinates through location/address:"]
[]
[]
[]
[]
[null,null,null,null,null,"• or insert coordinates manually:"]
[null,null,null,null,null,"longitude"]
[null,null,null,null,null,"latitude"]
[]
[null,null,null,"Undisturbed forests"]
[null,null,null,null,null,"linked GIS database:"]
[null,null,null,null,null,"response:",null,null,null,false]
[]
[null,null,null,"Nature protection areas"]
[null,null,null,null,null,"online database EU:"]
[null,null,null,null,null,"online databases World:"]
[]
[]
[null,null,null,"Highly biodiverse grasslands"]
[null,null,null,null,null,"since there is not yet an official European definition of highly "]
[null,null,null,null,null,"biodiverse grasslands, no database could be proposed."]
[null,null,null,null,null,"GIS data on grassland in general can be found online (click button) but are not (yet) linked to this tool:"]
[]
[null,null,null,"Land with high carbon stock"]
[null,null,null,"Is the biomass obtained from land that had one of the following statusses in January 2008 and no longer has that status:"]
[null,null,null,"Wetlands",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D220=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Continuously forested areas",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D221=1,\"yes\",\"no\")","v":"yes"}]
[null,null,null,"Peatland",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D222=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Search data:"]
[null,null,null,null,"In case no specific or reliable data can be obtained from the biomass supplier itself, this section offers some online or linked databases that can be useful to assess the fulfilment of the particular requirements for land with high carbon stock."]
[]
[null,null,null,"Wetlands"]
[null,null,null,null,null,"online databases World:"]
[]
[]
[null,null,null,"Continuously forested areas"]
[null,null,null,null,null,"linked GIS database for land use 2005-06:",null,null,null,null,null,null,null,null,null,null,"response:","Rainfed croplands"]
[null,null,null,null,null,"linked GIS database for land use 2009:",null,null,null,null,null,null,null,null,null,null,"response:","Rainfed croplands"]
[]
[null,null,null,"Peatland "]
[null,null,null,null,null,"search soil type:",null,null,null,null,null,null,null,null,null,null,"response:"]
[]
[]
[]
[null,null,null,"Feedstock pathway 2"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,"User input",null,null,null,null,null,"Default value",null,null,null,null,null,"Unit"]
[null,null,null,"Land with high biodiversity value"]
[null,null,null,"Is the biomass obtained from land that had one of the following statusses in or after January 2008, whether or not the land continues to have that status:"]
[null,null,null,"Undisturbed forest",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D438=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Nature protection area",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D439=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Highly biodiverse grassland",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D440=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Search data:"]
[null,null,null,null,"In case no specific or reliable data can be obtained from the biomass supplier itself, this section offers online or linked databases that can be useful to assess the fulfilment of the particular requirements for land with high biodiversity value."]
[]
[null,null,null,null,null,"• search coordinates through location/address:"]
[]
[]
[]
[]
[null,null,null,null,null,"• or insert coordinates manually:"]
[null,null,null,null,null,"longitude"]
[null,null,null,null,null,"latitude"]
[]
[null,null,null,"Undisturbed forests"]
[null,null,null,null,null,"linked GIS database:"]
[null,null,null,null,null,"response:"]
[]
[null,null,null,"Nature protection areas"]
[null,null,null,null,null,"online database EU:"]
[null,null,null,null,null,"online databases World:"]
[]
[]
[null,null,null,"Highly biodiverse grasslands"]
[null,null,null,null,null,"since there is not yet an official European definition of highly "]
[null,null,null,null,null,"biodiverse grasslands, no database could be proposed."]
[null,null,null,null,null,"GIS data on grassland in general can be found online (click button) but are not (yet) linked to this tool:"]
[]
[null,null,null,"Land with high carbon stock"]
[null,null,null,"Is the biomass obtained from land that had one of the following statusses in January 2008 and no longer has that status:"]
[null,null,null,"Wetlands",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D441=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Continuously forested areas",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D442=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Peatland",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(Parameters!D443=1,\"yes\",\"no\")","v":"no"}]
[null,null,null,"Search data:"]
[null,null,null,null,"In case no specific or reliable data can be obtained from the biomass supplier itself, this section offers some online or linked databases that can be useful to assess the fulfilment of the particular requirements for land with high carbon stock."]
[]
[null,null,null,"Wetlands"]
[null,null,null,null,null,"online databases World:"]
[]
[]
[null,null,null,"Continuously forested areas"]
[null,null,null,null,null,"linked GIS database for land use 2005-06:",null,null,null,null,null,null,null,null,null,null,"response:"]
[null,null,null,null,null,"linked GIS database for land use 2009:",null,null,null,null,null,null,null,null,null,null,"response:"]
[]
[null,null,null,"Peatland "]
[null,null,null,null,null,"search soil type:",null,null,null,null,null,null,null,null,null,null,"response:"]

{"sheet":"Input LW","index":9,"n_rows":153,"n_cols":24,"rows_kept":153,"cut":false,"hidden":false,"merged":[[28,3,28,9],[28,10,28,15],[29,3,29,15],[29,16,29,21],[28,23,28,24],[28,19,28,22],[18,20,18,21],[20,23,21,24],[21,1,21,3],[21,5,21,6],[21,8,21,9],[21,11,21,12],[21,14,21,15],[21,17,21,18],[21,20,21,21],[18,1,18,3],[18,5,18,6],[18,8,18,9],[18,11,18,12],[18,14,18,15],[18,17,18,18],[30,23,30,24],[31,23,31,24],[32,23,32,24],[33,23,33,24],[34,23,34,24],[38,22,38,24],[38,3,38,9],[38,10,38,15],[38,16,38,21],[31,20,31,22],[31,3,31,19],[32,3,32,19],[33,3,33,19],[34,3,34,19],[32,20,32,22],[33,20,33,22],[34,20,34,22],[35,3,35,19],[40,3,40,19],[40,20,40,22],[40,23,40,24],[35,20,35,22],[36,20,36,22],[37,20,37,22],[39,3,39,19],[39,20,39,22],[39,23,39,24],[37,3,37,19],[35,23,35,24],[36,23,36,24],[37,23,37,24],[43,3,43,19],[43,20,43,22],[43,23,43,24],[44,20,44,22],[44,23,44,24],[41,3,41,19],[41,20,41,22],[41,23,41,24],[42,3,42,19],[42,20,42,22],[42,23,42,24],[84,3,84,15],[84,16,84,21],[85,23,85,24],[86,3,86,19],[86,20,86,22],[86,23,86,24],[45,3,45,19],[45,20,45,22],[45,23,45,24],[83,3,83,9],[83,10,83,15],[83,19,83,22],[83,23,83,24],[47,3,47,9],[47,10,47,15],[47,19,47,22],[47,23,47,24],[48,3,48,15],[48,16,48,21],[49,23,49,24],[50,3,50,19],[50,20,50,22],[54,20,54,22],[54,23,54,24],[89,3,89,19],[89,20,89,22],[89,23,89,24],[87,3,87,19],[87,20,87,22],[87,23,87,24],[88,3,88,19],[88,20,88,22],[88,23,88,24],[92,3,92,19],[92,20,92,22],[92,23,92,24],[93,3,93,9],[93,10,93,15],[93,16,93,21],[93,22,93,24],[90,3,90,19],[90,20,90,22],[90,23,90,24],[91,20,91,22],[91,23,91,24],[103,3,103,15],[103,16,103,21],[104,23,104,24],[105,3,105,19],[105,20,105,22],[105,23,105,24],[106,3,106,19],[106,20,106,22],[106,23,106,24],[98,20,98,22],[98,23,98,24],[96,3,96,19],[96,20,96,22],[96,23,96,24],[94,3,94,19],[94,20,94,22],[94,23,94,24],[95,3,95,19],[95,20,95,22],[95,23,95,24],[53,3,53,19],[53,20,53,22],[53,23,53,24],[50,23,50,24],[51,3,51,19],[51,20,51,22],[51,23,51,24],[52,3,52,19],[52,20,52,22],[52,23,52,24],[56,3,56,19],[56,20,56,22],[56,23,56,24],[57,3,57,19],[57,20,57,22],[57,23,57,24],[55,3,55,9],[55,10,55,15],[55,16,55,21],[55,22,55,24],[59,3,59,19],[59,20,59,22],[59,23,59,24],[60,3,60,19],[60,20,60,22],[60,23,60,24],[58,3,58,19],[58,20,58,22],[58,23,58,24],[64,3,64,9],[64,10,64,15],[64,19,64,22],[64,23,64,24],[65,3,65,15],[65,16,65,21],[61,20,61,22],[61,23,61,24],[62,3,62,19],[62,20,62,22],[62,23,62,24],[71,23,71,24],[71,20,71,22],[69,3,69,19],[69,20,69,22],[69,23,69,24],[70,3,70,19],[70,20,70,22],[70,23,70,24],[66,23,66,24],[67,3,67,19],[67,20,67,22],[67,23,67,24],[68,3,68,19],[68,20,68,22],[68,23,68,24],[74,3,74,19],[74,20,74,22],[74,23,74,24],[72,3,72,9],[72,10,72,15],[72,16,72,21],[72,22,72,24],[73,3,73,19],[73,20,73,22],[73,23,73,24],[77,3,77,19],[77,20,77,22],[77,23,77,24],[78,20,78,22],[78,23,78,24],[75,3,75,19],[75,20,75,22],[75,23,75,24],[76,3,76,19],[76,20,76,22],[76,23,76,24],[109,23,109,24],[109,20,109,22],[107,3,107,19],[107,20,107,22],[107,23,107,24],[108,3,108,19],[108,20,108,22],[108,23,108,24],[79,3,79,19],[79,20,79,22],[79,23,79,24],[102,3,102,9],[102,10,102,15],[102,19,102,22],[102,23,102,24],[99,20,99,22],[99,23,99,24],[100,3,100,19],[100,20,100,22],[100,23,100,24],[97,3,97,19],[97,20,97,22],[97,23,97,24],[98,3,98,19],[112,3,112,19],[112,20,112,22],[112,23,112,24],[110,3,110,9],[110,10,110,15],[110,16,110,21],[110,22,110,24],[111,3,111,19],[111,20,111,22],[111,23,111,24],[115,3,115,19],[115,20,115,22],[115,23,115,24],[116,20,116,22],[116,23,116,24],[113,3,113,19],[113,20,113,22],[113,23,113,24],[114,3,114,19],[114,20,114,22],[114,23,114,24],[120,3,120,15],[120,16,120,21],[121,23,121,24],[122,3,122,19],[122,20,122,22],[122,23,122,24],[117,3,117,19],[117,20,117,22],[117,23,117,24],[119,3,119,9],[119,10,119,15],[119,19,119,22],[119,23,119,24],[125,3,125,19],[125,20,125,22],[125,23,125,24],[123,3,123,19],[123,20,123,22],[123,23,123,24],[124,3,124,19],[124,20,124,22],[124,23,124,24],[128,3,128,19],[128,20,128,22],[128,23,128,24],[129,3,129,19],[129,20,129,22],[129,23,129,24],[126,20,126,22],[126,23,126,24],[127,3,127,9],[127,10,127,15],[127,16,127,21],[127,22,127,24],[131,3,131,19],[131,20,131,22],[131,23,131,24],[132,3,132,19],[132,20,132,22],[132,23,132,24],[130,3,130,19],[130,20,130,22],[130,23,130,24],[137,3,137,9],[137,10,137,15],[137,19,137,22],[137,23,137,24],[138,3,138,15],[138,16,138,21],[133,20,133,22],[133,23,133,24],[134,3,134,19],[134,20,134,22],[134,23,134,24],[144,23,144,24],[144,20,144,22],[142,3,142,19],[142,20,142,22],[142,23,142,24],[143,3,143,19],[143,20,143,22],[143,23,143,24],[139,23,139,24],[140,3,140,19],[140,20,140,22],[140,23,140,24],[141,3,141,19],[141,20,141,22],[141,23,141,24],[147,3,147,19],[147,20,147,22],[147,23,147,24],[145,3,145,9],[145,10,145,15],[145,16,145,21],[145,22,145,24],[146,3,146,19],[146,20,146,22],[146,23,146,24],[152,3,152,19],[152,20,152,22],[152,23,152,24],[150,3,150,19],[150,20,150,22],[150,23,150,24],[151,20,151,22],[151,23,151,24],[148,3,148,19],[148,20,148,22],[148,23,148,24],[149,3,149,19],[149,20,149,22],[149,23,149,24]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Local Well-being"]
[null,"Although various attempts have been made to integrate social aspects into sustainability assessments, a generally accepted methodology to assess the impact of a product or a process on local well-being is not "]
[null,"yet existing and therefore often omitted in assessment frameworks or tools. Furthermore, most of the social indicators that are used today are qualitative and therefore difficult to integrate. It was chosen to "]
[null,"create for the purpose of this tool a risk factor based on a set of social requirements with respect to human and property rights, and labour rights and conditions. These social requirements are commonly used "]
[null,"in existing certification schemes such as the Roundtable for Sustainable Palm Oil (RSPO) and the Basel criteria. In case the biomass stream used within the bio-energy system is certified, the requirements can be "]
[null,"considered to be fulfilled. Also for biomass cultivated in Western Europe the requirements can be considered to be fulfilled."]
[]
[null,"Project overview"]
[]
[]
[]
[null,{"$f":"Parameters!J2","v":"Palm oil (stearin) from palm fruits, refinery"},null,null,null,{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F2","v":"Transport of FFB to the mill"},null,null,{"$f":"Parameters!F4","v":"Production of Crude Palm Oil (CPO)"},null,null,{"$f":"Parameters!F5","v":"Transport of CPO to Belgium"},null,null,{"$f":"Parameters!F7","v":"Refinery of Crude Palm Oil"},null,null,{"$f":"Parameters!F8","v":"Transport of PS to the final conversion unit"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!F18","v":"No final conversion"}]
[null,{"$f":"Parameters!J3","v":"None"},null,null,null,{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F10","v":"n.a."},null,null,{"$f":"Parameters!F12","v":"n.a."},null,null,{"$f":"Parameters!F13","v":"n.a."},null,null,{"$f":"Parameters!F15","v":"n.a."},null,null,{"$f":"Parameters!F16","v":"n.a."}]
[]
[]
[null,"Project input data"]
[]
[null,null,null,"Feedstock pathway 1"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,"Default value"]
[null,null,null,"Are the following conditions fulfilled?"]
[null,null,null,"Human and property rights"]
[null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D224","v":"Not fulfilled"}]
[null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D225","v":"Not fulfilled"}]
[null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D226","v":"Not fulfilled"}]
[null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D227","v":"Not fulfilled"}]
[null,null,null,"The producer can proof that the land is used legitimately and that traditional land rights have been secured",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D228","v":"Not fulfilled"}]
[null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D229","v":"Not fulfilled"}]
[null,null,null,"The biomass production does not impair food security",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D230","v":"Not fulfilled"}]
[null,null,null,"Labour rights and conditions"]
[null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D231","v":"Not fulfilled"}]
[null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D232","v":"Not fulfilled"}]
[null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D233","v":"Not fulfilled"}]
[null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D234","v":"Not fulfilled"}]
[null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D235","v":"Not fulfilled"}]
[null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D236","v":"Not fulfilled"}]
[null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D237","v":"Not fulfilled"}]
[]
[null,null,null,"Feedstock conversion 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,"Default value"]
[null,null,null,"Are the following conditions fulfilled?"]
[null,null,null,"Human and property rights"]
[null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D987","v":"Not fulfilled"}]
[null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D988","v":"Not fulfilled"}]
[null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D989","v":"Not fulfilled"}]
[null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D990","v":"Not fulfilled"}]
[null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D992","v":"Not fulfilled"}]
[null,null,null,"Labour rights and conditions"]
[null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D994","v":"Not fulfilled"}]
[null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D995","v":"Not fulfilled"}]
[null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D996","v":"Not fulfilled"}]
[null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D997","v":"Not fulfilled"}]
[null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D998","v":"Not fulfilled"}]
[null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D999","v":"Not fulfilled"}]
[null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1000","v":"Not fulfilled"}]
[]
[null,null,null,"Feedstock conversion 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,"Default value"]
[null,null,null,"Are the following conditions fulfilled?"]
[null,null,null,"Human and property rights"]
[null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1001","v":"Not fulfilled"}]
[null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1002","v":"Not fulfilled"}]
[null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1003","v":"Not fulfilled"}]
[null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1004","v":"Not fulfilled"}]
[null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1006","v":"Not fulfilled"}]
[null,null,null,"Labour rights and conditions"]
[null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1008","v":"Not fulfilled"}]
[null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1009","v":"Not fulfilled"}]
[null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1010","v":"Not fulfilled"}]
[null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1011","v":"Not fulfilled"}]
[null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1012","v":"Not fulfilled"}]
[null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1013","v":"Not fulfilled"}]
[null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1014","v":"Not fulfilled"}]
[]
[null,null,null,"Feedstock pathway 2"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,"Default value"]
[null,null,null,"Are the following conditions fulfilled?"]
[null,null,null,"Human and property rights"]
[null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D445","v":"n.a."}]
[null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D446","v":"n.a."}]
[null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D447","v":"n.a."}]
[null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D448","v":"n.a."}]
[null,null,null,"The producer can proof that the land is used legitimately and that traditional land rights have been secured",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D449","v":"n.a."}]
[null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D450","v":"n.a."}]
[null,null,null,"The biomass production does not impair food security",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D451","v":"n.a."}]
[null,null,null,"Labour rights and conditions"]
[null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D452","v":"n.a."}]
[null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D453","v":"n.a."}]
[null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D454","v":"n.a."}]
[null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D455","v":"n.a."}]
[null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D456","v":"n.a."}]
[null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D457","v":"n.a."}]
[null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D458","v":"n.a."}]
[]
[null,null,null,"Feedstock conversion 1",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,"Default value"]
[null,null,null,"Are the following conditions fulfilled?"]
[null,null,null,"Human and property rights"]
[null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1357","v":"n.a."}]
[null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1358","v":"n.a."}]
[null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1359","v":"n.a."}]
[null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1360","v":"n.a."}]
[null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1362","v":"n.a."}]
[null,null,null,"Labour rights and conditions"]
[null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1364","v":"n.a."}]
[null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1365","v":"n.a."}]
[null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1366","v":"n.a."}]
[null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1367","v":"n.a."}]
[null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1368","v":"n.a."}]
[null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1369","v":"n.a."}]
[null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1370","v":"n.a."}]
[]
[null,null,null,"Feedstock conversion 2",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,"Default value"]
[null,null,null,"Are the following conditions fulfilled?"]
[null,null,null,"Human and property rights"]
[null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1371","v":"n.a."}]
[null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1372","v":"n.a."}]
[null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1373","v":"n.a."}]
[null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1374","v":"n.a."}]
[null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1376","v":"n.a."}]
[null,null,null,"Labour rights and conditions"]
[null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1378","v":"n.a."}]
[null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1379","v":"n.a."}]
[null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1380","v":"n.a."}]
[null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1381","v":"n.a."}]
[null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1382","v":"n.a."}]
[null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1383","v":"n.a."}]
[null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1384","v":"n.a."}]
[]
[null,null,null,"Final conversion"]
[null,null,null,"Conversion into final energy source",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,null,"Default value"]
[null,null,null,"Are the following conditions fulfilled?"]
[null,null,null,"Human and property rights"]
[null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1556","v":"Fulfilled"}]
[null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1557","v":"Fulfilled"}]
[null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1558","v":"Fulfilled"}]
[null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1559","v":"Fulfilled"}]
[null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1561","v":"Fulfilled"}]
[null,null,null,"Labour rights and conditions"]
[null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1563","v":"Fulfilled"}]
[null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1564","v":"Fulfilled"}]
[null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1565","v":"Fulfilled"}]
[null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1566","v":"Fulfilled"}]
[null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1567","v":"Fulfilled"}]
[null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1568","v":"Fulfilled"}]
[null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!D1569","v":"Fulfilled"}]

{"sheet":"Output Mass","index":10,"n_rows":73,"n_cols":20,"rows_kept":73,"cut":false,"hidden":false,"merged":[[49,4,49,5],[43,14,43,15],[35,14,35,15],[37,4,37,5],[28,4,28,5],[29,4,29,5],[31,4,31,5],[32,4,32,5],[47,4,47,5],[26,4,26,5],[41,14,41,15],[23,14,23,15],[25,14,25,15],[23,4,23,5],[25,4,25,5],[18,14,18,15],[38,4,38,5],[40,4,40,5],[41,4,41,5],[43,4,43,5],[19,14,19,15],[20,14,20,15],[34,14,34,15],[22,14,22,15],[34,4,34,5],[35,4,35,5],[26,14,26,15],[18,4,18,5],[19,4,19,5],[20,4,20,5],[22,4,22,5],[13,4,13,5],[14,14,14,15],[15,14,15,15],[16,14,16,15],[17,14,17,15],[14,4,14,5],[15,4,15,5],[16,4,16,5],[17,4,17,5],[63,4,63,5],[24,4,24,5],[30,4,30,5],[42,14,42,15],[46,14,46,15],[47,14,47,15],[49,14,49,15],[50,14,50,15],[61,4,61,5],[62,4,62,5],[37,14,37,15],[38,14,38,15],[40,14,40,15],[50,4,50,5],[44,4,44,5],[46,4,46,5],[68,7,69,8],[12,4,12,5],[12,14,12,15],[36,4,36,5],[42,4,42,5],[48,4,48,5],[48,14,48,15],[36,14,36,15],[30,14,30,15],[24,14,24,15],[13,14,13,15],[44,14,44,15],[28,14,28,15],[29,14,29,15],[31,14,31,15],[32,14,32,15]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Mass balance (year)"]
[null,"Feedstock pathway 1:",null,{"$f":"Parameters!J2","v":"Palm oil (stearin) from palm fruits, refinery"}]
[null,"Feedstock pathway 2:",null,{"$f":"Parameters!J3","v":"None"}]
[null,"Final conversion:",null,{"$f":"Parameters!J4","v":"No final conversion, only biofuel production"}]
[]
[null,null,null,null,"FEEDSTOCK 1",null,null,null,null,null,null,null,null,null,"FEEDSTOCK 2"]
[null,"inputs:",null,null,null,null,null,"by-products:",null,null,null,"inputs:",null,null,null,null,null,"by-products:"]
[null,"seeds",{"$f":"Parameters!F41","v":0},"kg/ha",null,null,null,null,null,null,null,"seeds",{"$f":"Parameters!$F262","v":0},"kg/ha"]
[null,"N-fertilizer",{"$f":"Parameters!F42","v":127.908},"kg/ha",null,null,null,null,null,null,null,"N-fertilizer",{"$f":"Parameters!$F263","v":0},"kg/ha"]
[null,"P2O5-fertilizer",{"$f":"Parameters!F43","v":143.792},"kg/ha","Biomass production",null,null,{"$f":"Parameters!F29","v":"n.a."},{"$f":"Parameters!F31","v":0},"kg/ha",null,"P2O5-fertilizer",{"$f":"Parameters!$F264","v":0},"kg/ha","Biomass production",null,null,{"$f":"Parameters!F250","v":"n.a."},{"$f":"Parameters!F252","v":0},"kg/ha"]
[null,"K2O-fertilizer",{"$f":"Parameters!F44","v":199.804},"kg/ha",{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F30","v":"n.a."},{"$f":"Parameters!F32","v":0},"kg/ha",null,"K2O-fertilizer",{"$f":"Parameters!$F265","v":0},"kg/ha",{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F251","v":"n.a."},{"$f":"Parameters!F253","v":0},"kg/ha"]
[null,"CaO-fertilizer",{"$f":"Parameters!F45","v":0},"kg/ha",null,null,null,null,null,null,null,"CaO-fertilizer",{"$f":"Parameters!$F266","v":0},"kg/ha"]
[null,"pesticides",{"$f":"Parameters!F46","v":8.36},"kg/ha",null,null,null,null,null,null,null,"pesticides",{"$f":"Parameters!$F267","v":0},"kg/ha"]
[null,{"$f":"Parameters!F54","v":"Diesel"},{"$f":"Parameters!F57","v":47.902000000000001},"kg/ha",null,null,null,null,null,null,null,{"$f":"Parameters!F275","v":"n.a."},{"$f":"Parameters!$F278","v":0},"MJ/ha"]
[null,null,null,null,null,{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F22","v":19000},"kg/ha",null,null,null,null,null,{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F243","v":0},"kg/ha"]
[null,null,null,null,null,null,null,null,{"$f":"Parameters!F27","v":34},"% moisture",null,null,null,null,null,null,null,null,{"$f":"Parameters!F248","v":0},"% moisture"]
[null,"electricity",{"$f":"Parameters!F62","v":0},"MJ/kgfm","Treatment & transport",null,null,null,{"$f":"Parameters!G23","v":12540},"kgdm/ha",null,"electricity",{"$f":"Parameters!F283","v":0},"MJ/kgfm","Treatment & transport",null,null,null,{"$f":"Parameters!G244","v":0},"kgdm/ha"]
[null,"heat",{"$f":"Parameters!F59","v":0},"MJ/kgfm",{"$f":"Parameters!F2","v":"Transport of FFB to the mill"},null,null,null,null,null,null,"heat",{"$f":"Parameters!F280","v":0},"MJ/kgfm",{"$f":"Parameters!F10","v":"n.a."}]
[null,"transport fuel",{"$f":"Parameters!G471+Parameters!G472+Parameters!G473","v":950},"ton km/ha",{"$f":"Parameters!F3","v":"No treatment"},null,null,"losses",{"$f":"Parameters!F78","v":2},"%",null,"transport fuel",{"$f":"Parameters!G572+Parameters!G573+Parameters!G574","v":0},"ton km/ha",{"$f":"Parameters!F11","v":"n.a."},null,null,"losses",{"$f":"Parameters!F299","v":0},"%"]
[]
[null,null,null,null,null,null,null,null,{"$f":"Parameters!G80","v":12289.2},"kgdm/ha",null,null,null,null,null,null,null,null,{"$f":"Parameters!G301","v":0},"kgdm/ha"]
[null,null,null,null,null,null,null,null,{"$f":"Parameters!G81","v":294940.79999999999},"MJ/ha",null,null,null,null,null,null,null,null,{"$f":"Parameters!G302","v":0},"MJ/ha"]
[null,"electricity",{"$f":"Parameters!F797","v":0},"MJ/MJoutput","Conversion - process 1",null,null,null,null,null,null,"electricity",{"$f":"Parameters!F1167","v":0},"MJ/MJoutput","Conversion - process 1"]
[null,"fuel/heat",{"$f":"Parameters!F819+Parameters!F821","v":0},"MJ/MJoutput",{"$f":"Parameters!F4","v":"Production of Crude Palm Oil (CPO)"},null,null,{"$f":"Parameters!F668","v":"Palm kernel meal"},{"$f":"Parameters!F692","v":2.399961774322297E-2},"MJ/MJinput",null,"fuel/heat",{"$f":"Parameters!F1189+Parameters!F1191","v":0},"MJ/MJoutput",{"$f":"Parameters!F12","v":"n.a."},null,null,{"$f":"Parameters!F1039","v":"n.a."},{"$f":"Parameters!F1062","v":0},"MJ/MJinput"]
[null,{"$f":"Parameters!F720","v":"n.a."},{"$f":"Parameters!F734","v":0},"kg/MJoutput",null,null,null,{"$f":"Parameters!F671","v":"n.a."},{"$f":"Parameters!F693","v":0},"MJ/MJinput",null,{"$f":"Parameters!F1090","v":"n.a."},{"$f":"Parameters!F1104","v":0},"kg/MJoutput",null,null,null,{"$f":"Parameters!F1042","v":"n.a."},{"$f":"Parameters!F1063","v":0},"MJ/MJinput"]
[null,{"$f":"Parameters!F721","v":"n.a."},{"$f":"Parameters!F738","v":0},"kg/MJoutput",null,null,null,null,null,null,null,{"$f":"Parameters!F1091","v":"n.a."},{"$f":"Parameters!F1108","v":0},"kg/MJoutput"]
[null,null,null,null,null,{"$f":"Parameters!F666","v":"Crude palm oil"},null,null,{"$f":"Parameters!G768","v":4224.7799859623219},"kgdm/ha",null,null,null,null,null,{"$f":"Parameters!F1037","v":"n.a."},null,null,{"$f":"Parameters!G1138","v":0},"kgdm/ha"]
[null,null,null,null,null,null,null,null,{"$f":"Parameters!G769","v":156316.8594806059},"MJ/ha",null,null,null,null,null,null,null,null,{"$f":"Parameters!G1139","v":0},"MJ/ha"]
[null,"electricity",{"$f":"Parameters!F907","v":8.4000000000000003E-4},"MJ/MJinput","Treatment & transport",null,null,null,null,null,null,"electricity",{"$f":"Parameters!F1277","v":0},"MJ/MJinput","Treatment & transport"]
[null,"heat",{"$f":"Parameters!F905","v":0},"MJ/MJinput",{"$f":"Parameters!F5","v":"Transport of CPO to Belgium"},null,null,null,null,null,null,"heat",{"$f":"Parameters!F1275","v":0},"MJ/MJinput",{"$f":"Parameters!F13","v":"n.a."}]
[null,"transport fuel",{"$f":"Parameters!G474+Parameters!G475+Parameters!G476","v":43667.325934906563},"ton km/ha",{"$f":"Parameters!F6","v":"No treatment"},null,null,null,null,null,null,"transport fuel",{"$f":"Parameters!G573+Parameters!G574+Parameters!G575","v":0},"ton km/ha",{"$f":"Parameters!F14","v":"n.a."}]
[]
[null,null,null,null,null,{"$f":"Parameters!F666","v":"Crude palm oil"},null,null,{"$f":"Parameters!G768","v":4224.7799859623219},"kgdm/ha",null,null,null,null,null,{"$f":"Parameters!F1037","v":"n.a."},null,null,{"$f":"Parameters!G1138","v":0},"kgdm/ha"]
[null,null,null,null,null,null,null,null,{"$f":"Parameters!G769","v":156316.8594806059},"MJ/ha",null,null,null,null,null,null,null,null,{"$f":"Parameters!G1139","v":0},"MJ/ha"]
[null,"electricity",{"$f":"Parameters!F801","v":5.9972952198558455E-4},"MJ/MJoutput","Conversion - process 2",null,null,null,null,null,null,"electricity",{"$f":"Parameters!F1171","v":0},"MJ/MJoutput","Conversion - process 2"]
[null,"fuel/heat",{"$f":"Parameters!F823+Parameters!F825","v":7.9963936264744601E-3},"MJ/MJoutput",{"$f":"Parameters!D7","v":"Refinery of Crude Palm Oil"},null,null,{"$f":"Parameters!F679","v":"Palm olein"},{"$f":"Parameters!F697","v":0},"MJ/MJinput",null,"fuel/heat",{"$f":"Parameters!F1193+Parameters!F1195","v":0},"MJ/MJoutput",{"$f":"Parameters!F15","v":"n.a."},null,null,{"$f":"Parameters!F1050","v":"n.a."},{"$f":"Parameters!F1067","v":0},"MJ/MJinput"]
[null,{"$f":"Parameters!F723","v":"Fuller's earth"},{"$f":"Parameters!F745","v":0},"kg/MJoutput",null,null,null,{"$f":"Parameters!F682","v":"n.a."},{"$f":"Parameters!F698","v":0},"MJ/MJinput",null,{"$f":"Parameters!F1093","v":"n.a."},{"$f":"Parameters!F1115","v":0},"kg/MJoutput",null,null,null,{"$f":"Parameters!F1053","v":"n.a."},{"$f":"Parameters!F1068","v":0},"MJ/MJinput"]
[null,{"$f":"Parameters!F724","v":"n.a."},{"$f":"Parameters!F749","v":0},"kg/MJoutput",null,null,null,null,null,null,null,{"$f":"Parameters!F1094","v":"n.a."},{"$f":"Parameters!F1119","v":0},"kg/MJoutput"]
[null,null,null,null,null,{"$f":"Parameters!F667","v":"Palm stearin"},null,null,{"$f":"Parameters!G771","v":1351.4199870371556},"kgdm/ha",null,null,null,null,null,{"$f":"Parameters!F1038","v":"n.a."},null,null,{"$f":"Parameters!G1141","v":0},"kgdm/ha"]
[null,null,null,null,null,null,null,null,{"$f":"Parameters!G772","v":50002.539520374754},"MJ/ha",null,null,null,null,null,null,null,null,{"$f":"Parameters!G1142","v":0},"MJ/ha"]
[null,"electricity",{"$f":"Parameters!F914","v":8.4000000000000003E-4},"MJ/MJinput","Treatment & transport",null,null,null,null,null,null,"electricity",{"$f":"Parameters!F1284","v":0},"MJ/MJinput","Treatment & transport"]
[null,"heat",{"$f":"Parameters!F912","v":0},"MJ/MJinput",{"$f":"Parameters!F8","v":"Transport of PS to the final conversion unit"},null,null,null,null,null,null,"heat",{"$f":"Parameters!F1282","v":0},"MJ/MJinput",{"$f":"Parameters!F16","v":"n.a."}]
[null,"transport fuel",{"$f":"Parameters!G477+Parameters!G478+Parameters!G479","v":135.14199870371556},"ton km/ha",{"$f":"Parameters!F9","v":"No treatment"},null,null,null,null,null,null,"transport fuel",{"$f":"Parameters!G576+Parameters!G577+Parameters!G578","v":0},"ton km/ha",{"$f":"Parameters!F17","v":"n.a."}]
[]
[null,null,null,null,null,{"$f":"Parameters!F667","v":"Palm stearin"},null,null,{"$f":"Parameters!G771","v":1351.4199870371556},"kgdm/ha",null,null,null,null,null,{"$f":"Parameters!F1038","v":"n.a."},null,null,{"$f":"Parameters!G1141","v":0},"kgdm/ha"]
[null,null,null,null,null,null,null,null,{"$f":"Parameters!G772","v":50002.539520374754},"MJ/ha",null,null,null,null,null,null,null,null,{"$f":"Parameters!G1142","v":0},"MJ/ha"]
[]
[]
[null,null,{"$f":"Parameters!F667","v":"Palm stearin"},{"$f":"Parameters!F1409","v":100},"%"]
[null,null,null,{"$f":"Parameters!G1478","v":1},"MJ"]
[null,null,{"$f":"Parameters!F1038","v":"n.a."},{"$f":"Parameters!F1410","v":0},"%"]
[null,null,null,{"$f":"Parameters!G1479","v":0},"MJ"]
[]
[null,"inputs:",null,null,null,null,null,"by-products:"]
[]
[null,"electricity",{"$f":"Parameters!F1430","v":0},"MJ/MJFU","Final conversion",null,null,{"$f":"Parameters!F1414","v":"n.a."},{"$f":"Parameters!F1418","v":0},"MJ/MJinput"]
[null,"fuel/heat",{"$f":"Parameters!F1428+Parameters!F1429","v":0},"MJ/MJFU",{"$f":"Parameters!F18","v":"No final conversion"},null,null,{"$f":"Parameters!F1415","v":"n.a."},{"$f":"Parameters!F1419","v":0},"MJ/MJinput"]
[null,{"$f":"Parameters!F1422","v":"n.a."},{"$f":"Parameters!F1424","v":0},"kg/MJFU","ηel (%)",{"$f":"Parameters!F1411","v":0}]
[null,{"$f":"Parameters!F1423","v":"n.a."},{"$f":"Parameters!F1425","v":0},"kg/MJFU","ηh (%)",{"$f":"Parameters!F1412","v":0}]
[]
[]
[null,null,null,null,{"$f":"Parameters!G1476","v":0},"MJh",null,"FINAL OUTPUT"]
[null,null,null,null,{"$f":"Parameters!G1477","v":0},"MJe"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]

{"sheet":"Uncertainty","index":11,"n_rows":230,"n_cols":25,"rows_kept":230,"cut":false,"hidden":true,"merged":[[227,15,227,17],[227,18,227,20],[210,15,210,17],[210,18,210,20],[212,15,212,17],[213,15,213,17],[214,15,214,17],[194,15,194,17],[194,18,194,20],[195,15,195,17],[195,18,195,20],[211,15,211,17],[211,18,211,20],[212,18,212,20],[213,18,213,20],[214,18,214,20],[215,18,215,20],[216,18,216,20],[217,18,217,20],[225,15,225,17],[225,18,225,20],[226,15,226,17],[222,15,222,17],[222,18,222,20],[223,15,223,17],[223,18,223,20],[191,15,191,17],[191,18,191,20],[192,15,192,17],[192,18,192,20],[221,15,221,17],[15,23,16,25],[26,18,26,20],[28,18,28,20],[25,18,25,20],[27,18,27,20],[29,18,29,20],[30,18,30,20],[31,18,31,20],[32,18,32,20],[24,22,24,23],[25,22,25,23],[26,22,26,23],[27,22,27,23],[28,22,28,23],[29,22,29,23],[30,22,30,23],[31,22,31,23],[32,22,32,23],[33,18,33,20],[34,18,34,20],[35,18,35,20],[224,15,224,17],[224,18,224,20],[218,15,218,17],[218,18,218,20],[219,15,219,17],[219,18,219,20],[220,15,220,17],[220,18,220,20],[215,15,215,17],[216,15,216,17],[217,15,217,17],[70,18,70,20],[71,18,71,20],[72,18,72,20],[129,18,129,20],[171,18,171,20],[92,18,92,20],[93,15,93,17],[93,18,93,20],[100,15,100,17],[100,18,100,20],[122,15,122,17],[122,18,122,20],[123,15,123,17],[123,18,123,20],[202,15,202,17],[202,18,202,20],[203,15,203,17],[203,18,203,20],[135,15,135,17],[135,18,135,20],[136,15,136,17],[136,18,136,20],[163,15,163,17],[163,18,163,20],[182,15,182,17],[182,18,182,20],[183,15,183,17],[183,18,183,20],[184,15,184,17],[184,18,184,20],[179,15,179,17],[179,18,179,20],[180,15,180,17],[159,15,159,17],[159,18,159,20],[124,15,124,17],[124,18,124,20],[125,15,125,17],[125,18,125,20],[126,15,126,17],[127,18,127,20],[126,18,126,20],[127,15,127,17],[128,15,128,17],[128,18,128,20],[129,15,129,17],[144,15,144,17],[144,18,144,20],[145,15,145,17],[133,15,133,17],[133,18,133,20],[140,18,140,20],[141,15,141,17],[141,18,141,20],[142,15,142,17],[142,18,142,20],[134,15,134,17],[117,15,117,17],[117,18,117,20],[118,15,118,17],[118,18,118,20],[119,15,119,17],[119,18,119,20],[120,15,120,17],[120,18,120,20],[121,15,121,17],[121,18,121,20],[205,18,205,20],[181,15,181,17],[181,18,181,20],[170,15,170,17],[170,18,170,20],[171,15,171,17],[193,15,193,17],[193,18,193,20],[188,15,188,17],[188,18,188,20],[189,15,189,17],[189,18,189,20],[190,15,190,17],[190,18,190,20],[185,15,185,17],[197,18,197,20],[180,18,180,20],[201,15,201,17],[201,18,201,20],[174,15,174,17],[174,18,174,20],[175,15,175,17],[175,18,175,20],[134,18,134,20],[130,15,130,17],[130,18,130,20],[131,15,131,17],[131,18,131,20],[137,15,137,17],[137,18,137,20],[132,15,132,17],[132,18,132,20],[143,15,143,17],[143,18,143,20],[82,18,82,20],[83,15,83,17],[83,18,83,20],[105,15,105,17],[105,18,105,20],[86,15,86,17],[86,18,86,20],[87,15,87,17],[87,18,87,20],[88,15,88,17],[88,18,88,20],[89,15,89,17],[89,18,89,20],[90,15,90,17],[90,18,90,20],[94,15,94,17],[94,18,94,20],[95,18,95,20],[96,15,96,17],[96,18,96,20],[91,15,91,17],[91,18,91,20],[92,15,92,17],[85,18,85,20],[50,15,50,17],[50,18,50,20],[51,15,51,17],[51,18,51,20],[52,15,52,17],[52,18,52,20],[61,15,61,17],[62,15,62,17],[63,15,63,17],[58,15,58,17],[58,18,58,20],[59,15,59,17],[59,18,59,20],[60,15,60,17],[60,18,60,20],[61,18,61,20],[62,18,62,20],[63,18,63,20],[77,15,77,17],[82,15,82,17],[78,15,78,17],[78,18,78,20],[225,3,225,9],[226,3,226,9],[23,21,23,25],[23,18,23,20],[23,15,23,17],[24,15,24,17],[24,18,24,20],[25,15,25,17],[26,15,26,17],[27,15,27,17],[28,15,28,17],[29,15,29,17],[30,15,30,17],[31,15,31,17],[32,15,32,17],[33,15,33,17],[220,3,220,9],[221,3,221,9],[222,3,222,9],[223,3,223,9],[224,3,224,9],[197,3,197,14],[197,15,197,17],[197,21,197,25],[209,3,209,14],[209,15,209,17],[209,18,209,20],[209,21,209,25],[198,15,198,17],[198,18,198,20],[199,15,199,17],[193,3,193,9],[194,3,194,9],[199,22,199,23],[200,22,200,23],[201,22,201,23],[203,22,203,23],[204,22,204,23],[205,22,205,23],[193,22,193,23],[194,22,194,23],[195,22,195,23],[204,15,204,17],[204,18,204,20],[199,18,199,20],[200,15,200,17],[200,18,200,20],[205,15,205,17],[158,15,158,17],[158,18,158,20],[191,3,191,9],[192,3,192,9],[178,3,178,14],[178,15,178,17],[178,18,178,20],[178,21,178,25],[180,22,180,23],[181,22,181,23],[182,22,182,23],[183,22,183,23],[184,22,184,23],[185,22,185,23],[186,22,186,23],[187,22,187,23],[188,22,188,23],[189,22,189,23],[190,22,190,23],[191,22,191,23],[192,22,192,23],[185,18,185,20],[186,15,186,17],[186,18,186,20],[164,3,164,9],[165,3,165,9],[166,22,166,23],[188,3,188,9],[189,3,189,9],[190,3,190,9],[172,15,172,17],[172,18,172,20],[173,15,173,17],[173,18,173,20],[169,15,169,17],[169,18,169,20],[164,15,164,17],[164,18,164,20],[165,15,165,17],[165,18,165,20],[166,15,166,17],[166,18,166,20],[176,15,176,17],[176,18,176,20],[187,15,187,17],[187,18,187,20],[163,3,163,9],[149,3,149,14],[149,15,149,17],[149,18,149,20],[149,21,149,25],[168,3,168,14],[168,15,168,17],[168,18,168,20],[168,21,168,25],[150,15,150,17],[150,18,150,20],[151,15,151,17],[151,18,151,20],[152,15,152,17],[152,18,152,20],[153,15,153,17],[153,18,153,20],[154,15,154,17],[154,18,154,20],[160,15,160,17],[160,18,160,20],[155,15,155,17],[155,18,155,20],[156,15,156,17],[125,22,125,23],[126,22,126,23],[127,22,127,23],[159,3,159,9],[160,3,160,9],[161,3,161,9],[162,3,162,9],[146,15,146,17],[146,18,146,20],[147,15,147,17],[147,18,147,20],[156,18,156,20],[157,15,157,17],[157,18,157,20],[161,15,161,17],[161,18,161,20],[162,15,162,17],[162,18,162,20],[139,3,139,14],[139,15,139,17],[139,18,139,20],[139,21,139,25],[145,18,145,20],[140,15,140,17],[104,3,104,14],[104,15,104,17],[104,18,104,20],[104,21,104,25],[116,3,116,14],[116,15,116,17],[116,18,116,20],[116,21,116,25],[106,15,106,17],[106,18,106,20],[107,15,107,17],[106,22,106,23],[107,22,107,23],[108,22,108,23],[110,22,110,23],[111,22,111,23],[112,22,112,23],[110,15,110,17],[110,18,110,20],[111,15,111,17],[111,18,111,20],[112,18,112,20],[107,18,107,20],[109,15,109,17],[85,3,85,14],[85,15,85,17],[112,15,112,17],[109,18,109,20],[101,15,101,17],[101,18,101,20],[102,15,102,17],[102,18,102,20],[97,15,97,17],[97,18,97,20],[98,15,98,17],[98,18,98,20],[99,15,99,17],[99,18,99,20],[100,3,100,9],[101,3,101,9],[95,3,95,9],[96,3,96,9],[97,3,97,9],[98,3,98,9],[99,3,99,9],[108,15,108,17],[108,18,108,20],[95,15,95,17],[71,3,71,9],[72,3,72,9],[73,15,73,17],[77,22,77,23],[78,22,78,23],[79,22,79,23],[81,22,81,23],[71,15,71,17],[72,15,72,17],[79,18,79,20],[80,18,80,20],[81,18,81,20],[73,18,73,20],[76,18,76,20],[77,18,77,20],[75,18,75,20],[75,3,75,14],[75,15,75,17],[79,15,79,17],[80,15,80,17],[81,15,81,17],[76,15,76,17],[67,3,67,9],[68,3,68,9],[69,3,69,9],[70,3,70,9],[56,3,56,14],[56,15,56,17],[56,18,56,20],[56,21,56,25],[75,21,75,25],[57,15,57,17],[57,18,57,20],[70,15,70,17],[67,15,67,17],[68,15,68,17],[69,15,69,17],[64,15,64,17],[64,18,64,20],[65,15,65,17],[65,18,65,20],[66,15,66,17],[66,18,66,20],[67,18,67,20],[68,18,68,20],[69,18,69,20],[33,22,33,23],[66,3,66,9],[47,18,47,20],[48,15,48,17],[48,18,48,20],[49,15,49,17],[49,18,49,20],[40,18,40,20],[41,18,41,20],[42,18,42,20],[43,18,43,20],[44,18,44,20],[44,15,44,17],[53,15,53,17],[53,18,53,20],[54,15,54,17],[54,18,54,20],[46,3,46,14],[46,15,46,17],[46,18,46,20],[46,21,46,25],[47,15,47,17],[34,15,34,17],[35,15,35,17],[36,15,36,17],[37,15,37,17],[38,15,38,17],[39,15,39,17],[40,15,40,17],[41,15,41,17],[42,15,42,17],[43,15,43,17],[36,18,36,20],[37,18,37,20],[38,18,38,20],[39,18,39,20],[23,3,23,14],[13,17,13,18],[13,20,13,21],[16,1,16,3],[16,5,16,6],[16,8,16,9],[16,11,16,12],[16,14,16,15],[16,17,16,18],[16,20,16,21],[13,1,13,3],[13,5,13,6],[13,8,13,9],[13,11,13,12],[13,14,13,15],[34,22,34,23],[35,22,35,23],[36,22,36,23],[37,22,37,23],[38,22,38,23],[39,22,39,23],[40,22,40,23],[41,22,41,23],[42,22,42,23],[43,22,43,23],[44,22,44,23],[48,22,48,23],[49,22,49,23],[50,22,50,23],[52,22,52,23],[53,22,53,23],[54,22,54,23],[67,22,67,23],[58,22,58,23],[59,22,59,23],[60,22,60,23],[61,22,61,23],[62,22,62,23],[63,22,63,23],[64,22,64,23],[65,22,65,23],[66,22,66,23],[89,22,89,23],[90,22,90,23],[91,22,91,23],[92,22,92,23],[93,22,93,23],[68,22,68,23],[69,22,69,23],[70,22,70,23],[71,22,71,23],[72,22,72,23],[73,22,73,23],[87,22,87,23],[88,22,88,23],[85,21,85,25],[82,22,82,23],[83,22,83,23],[94,22,94,23],[95,22,95,23],[96,22,96,23],[97,22,97,23],[98,22,98,23],[99,22,99,23],[100,22,100,23],[101,22,101,23],[102,22,102,23],[117,22,117,23],[118,22,118,23],[119,22,119,23],[120,22,120,23],[163,22,163,23],[164,22,164,23],[165,22,165,23],[128,22,128,23],[129,22,129,23],[130,22,130,23],[131,22,131,23],[132,22,132,23],[133,22,133,23],[134,22,134,23],[135,22,135,23],[136,22,136,23],[142,22,142,23],[143,22,143,23],[146,22,146,23],[147,22,147,23],[121,22,121,23],[122,22,122,23],[123,22,123,23],[124,22,124,23],[221,18,221,20],[226,18,226,20],[229,17,232,22],[137,22,137,23],[141,22,141,23],[145,22,145,23],[170,22,170,23],[171,22,171,23],[172,22,172,23],[174,22,174,23],[175,22,175,23],[176,22,176,23],[151,22,151,23],[152,22,152,23],[153,22,153,23],[154,22,154,23],[155,22,155,23],[156,22,156,23],[157,22,157,23],[158,22,158,23],[159,22,159,23],[160,22,160,23],[161,22,161,23],[162,22,162,23],[221,22,221,23],[222,22,222,23],[223,22,223,23],[224,22,224,23],[225,22,225,23],[226,22,226,23],[227,22,227,23],[211,22,211,23],[212,22,212,23],[213,22,213,23],[214,22,214,23],[215,22,215,23],[216,22,216,23],[217,22,217,23],[218,22,218,23],[219,22,219,23],[220,22,220,23]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Uncertainty of data"]
[]
[null,"Project overview"]
[]
[]
[]
[null,{"$f":"Parameters!J2","v":"Palm oil (stearin) from palm fruits, refinery"},null,null,null,{"$f":"Parameters!F20","v":"Fresh palm fruit bunches (FFB)"},null,null,{"$f":"Parameters!F2","v":"Transport of FFB to the mill"},null,null,{"$f":"Parameters!F4","v":"Production of Crude Palm Oil (CPO)"},null,null,{"$f":"Parameters!F5","v":"Transport of CPO to Belgium"},null,null,{"$f":"Parameters!F7","v":"Refinery of Crude Palm Oil"},null,null,{"$f":"Parameters!F8","v":"Transport of PS to the final conversion unit"}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!F18","v":"No final conversion"}]
[null,{"$f":"Parameters!J3","v":"None"},null,null,null,{"$f":"Parameters!F241","v":"No crop"},null,null,{"$f":"Parameters!F10","v":"n.a."},null,null,{"$f":"Parameters!F12","v":"n.a."},null,null,{"$f":"Parameters!F13","v":"n.a."},null,null,{"$f":"Parameters!F15","v":"n.a."},null,null,{"$f":"Parameters!F16","v":"n.a."}]
[]
[]
[null,"Project input data"]
[null,"Only the uncertainty of personal data must be defined by the user (input cells colored in green):"]
[null,null,null,"Feedstock pathway 1"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Crop yield",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C22","v":""},null,null,"kgfm.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Moisture content of crop",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C27","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C31","v":""},null,null,"kgfm.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Moisture content of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C35","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C32","v":""},null,null,"kgfm.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Moisture content of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C36","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of seeds",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C41","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of N-fertiliser",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C42","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of P2O5-fertiliser",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C43","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of K2O-fertiliser",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C44","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of CaO-fertiliser",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C45","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of pesticides",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C46","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel used in farm machinery",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C57","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for feedstock production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C165","v":""},null,null,"m³.ha-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of animal manure N applied to soil",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C189","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of total sewage N applied to soil",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C190","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of total compost N applied to soil",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C191","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of N of other organic amendments applied to soil (used as fertiliser)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C192","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of N-fixing crop residue applied to soil",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C176","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fraction of above-ground residues removed",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C204","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Only for oil palm: Amount of residues returned to field",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C185","v":""},null,null,"kgdm.kgfm-1",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock treatment and transport 1",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Drying and storage:"]
[null,null,null,"Heat use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C59","v":""},null,null,"MJ.kgfm-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Electricity use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C62","v":""},null,null,"MJ.kgfm-2",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for storage 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C169","v":""},null,null,"m³.kgfm-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Feedstock transport:"]
[null,null,null,"Transport distance mode 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C480","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C481","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 3",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C482","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock conversion 1",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Process 1"]
[null,null,null,"Yield (output/input)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C717","v":0},null,null,"MJoutput.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C692","v":0},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C693","v":0},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C819","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C821","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Net electricity input",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C797","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C734","v":0},null,null,"kg.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C738","v":0},null,null,"kg.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C773","v":""},null,null,"gNOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C774","v":""},null,null,"gSOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C775","v":""},null,null,"gNH3 . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C776","v":""},null,null,"gNO3- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C777","v":""},null,null,"gNH4+ . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C778","v":""},null,null,"gPO43- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C779","v":""},null,null,"gCOD . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for conversion 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C979","v":""},null,null,"m³.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock treatment and transport 2",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Drying and storage:"]
[null,null,null,"Heat use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C905","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Electricity use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C907","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for storage 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C981","v":""},null,null,"m³.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Feedstock transport:"]
[null,null,null,"Transport distance mode 4",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C483","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 5",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C484","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 6",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C485","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock conversion 2",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Process 2"]
[null,null,null,"Yield (output/input)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C718","v":0},null,null,"MJoutput.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C697","v":0},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C698","v":0},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C823","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C825","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Net electricity input",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C801","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C745","v":0},null,null,"kg.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C749","v":0},null,null,"kg.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C780","v":""},null,null,"gNOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C781","v":""},null,null,"gSOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C782","v":""},null,null,"gNH3 . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C783","v":""},null,null,"gNO3- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C784","v":""},null,null,"gNH4+ . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C785","v":""},null,null,"gPO43- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C786","v":""},null,null,"gCOD . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for conversion 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C983","v":""},null,null,"m³.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock treatment and transport 3",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Drying and storage:"]
[null,null,null,"Heat use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C912","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Electricity use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C914","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for storage 3",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C985","v":""},null,null,"m³.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Feedstock transport:"]
[null,null,null,"Transport distance mode 7",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C486","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 8",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C487","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 9",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C488","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock pathway 2 (optional)"]
[]
[null,null,null,"Feedstock production",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Crop yield",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C243","v":""},null,null,"kgfm.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Moisture content of crop",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C248","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C252","v":""},null,null,"kgfm.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Moisture content of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C256","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C253","v":""},null,null,"kgfm.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Moisture content of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C257","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of seeds",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C262","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of N-fertiliser",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C263","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of P2O5-fertiliser",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C264","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of K2O-fertiliser",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C265","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of CaO-fertiliser",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C266","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Use of pesticides",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C267","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel used in farm machinery",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C278","v":""},null,null,"kg.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for feedstock production",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C386","v":""},null,null,"m³.ha-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of animal manure N applied to soil",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C410","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of total sewage N applied to soil",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C411","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of total compost N applied to soil",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C412","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of N of other organic amendments applied to soil (used as fertiliser)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C413","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of N-fixing crop residue applied to soil",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C397","v":""},null,null,"kgN.ha-1.y-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fraction of above-ground residues removed",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C425","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Only for oil palm: Amount of residues returned to field",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C406","v":""},null,null,"kgdm.kgfm-1",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock treatment and transport 1",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Drying and storage:"]
[null,null,null,"Heat use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C280","v":""},null,null,"MJ.kgfm-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Electricity use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C283","v":""},null,null,"MJ.kgfm-2",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for storage 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C390","v":""},null,null,"m³.kgfm-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Feedstock transport:"]
[null,null,null,"Transport distance mode 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C581","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C582","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 3",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C583","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock conversion 1",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Process 1"]
[null,null,null,"Yield (output/input)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1087","v":0},null,null,"MJoutput.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1062","v":0},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1063","v":0},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1189","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1191","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Net electricity input",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1167","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1104","v":0},null,null,"kg.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1108","v":0},null,null,"kg.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1143","v":""},null,null,"gNOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1144","v":""},null,null,"gSOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1145","v":""},null,null,"gNH3 . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1146","v":""},null,null,"gNO3- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1147","v":""},null,null,"gNH4+ . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1148","v":""},null,null,"gPO43- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1149","v":""},null,null,"gCOD . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for conversion 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1349","v":""},null,null,"m³.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock treatment and transport 2",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Drying and storage:"]
[null,null,null,"Heat use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1275","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Electricity use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1277","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for storage 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1351","v":""},null,null,"m³.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Feedstock transport:"]
[null,null,null,"Transport distance mode 4",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C584","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 5",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C585","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 6",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C586","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock conversion 2",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Process 2"]
[null,null,null,"Yield (output/input)",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1088","v":0},null,null,"MJoutput.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1067","v":0},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1068","v":0},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1193","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1195","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Net electricity input",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1171","v":0},null,null,"MJ.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1115","v":0},null,null,"kg.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1119","v":0},null,null,"kg.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1150","v":""},null,null,"gNOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1151","v":""},null,null,"gSOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1152","v":""},null,null,"gNH3 . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1153","v":""},null,null,"gNO3- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1154","v":""},null,null,"gNH4+ . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1155","v":""},null,null,"gPO43- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1156","v":""},null,null,"gCOD . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for conversion 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1353","v":""},null,null,"m³.MJoutput-1",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Feedstock treatment and transport 3",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Drying and storage:"]
[null,null,null,"Heat use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1282","v":""},null,null,null,null,null,"Min:",null,null,"Max:"]
[null,null,null,"Electricity use for drying",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1284","v":""},null,null,null,null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for storage 3",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1355","v":""},null,null,null,null,null,"Min:",null,null,"Max:"]
[null,null,null,"Feedstock transport:"]
[null,null,null,"Transport distance mode 7",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C587","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 8",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C588","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Transport distance mode 9",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C589","v":""},null,null,"km",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,"Final conversion"]
[]
[null,null,null,"Conversion into final energy source",null,null,null,null,null,null,null,null,null,null,null,"User input",null,null,"Unit",null,null,"User defined uncertainty"]
[null,null,null,"Final conversion process"]
[null,null,null,"Electrical efficiency of final conversion",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1411","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Thermal efficiency of final conversion",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1412","v":""},null,null,"%",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of main by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1418","v":""},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Yield of secondary by-product",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1419","v":""},null,null,"MJbyproduct.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1428","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of fuel/heat input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1429","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Net electricity input",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1430","v":""},null,null,"MJ.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 1",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1424","v":""},null,null,"kg.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Amount of material input 2",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1425","v":""},null,null,"kg.MJinput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1467","v":""},null,null,"gNOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"SOx emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1468","v":""},null,null,"gSOX . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH3 emissions to air",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1469","v":""},null,null,"gNH3 . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NO3- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1470","v":""},null,null,"gNO3- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"NH4+ emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1471","v":""},null,null,"gNH4+ . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"PO43- emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1472","v":""},null,null,"gPO43- . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"COD emissions to water",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1473","v":""},null,null,"gCOD . MJoutput-1",null,null,"Min:",null,null,"Max:"]
[null,null,null,"Fresh water use for final conversion",null,null,null,null,null,null,null,null,null,null,null,{"$f":"Parameters!C1555","v":""},null,null,"m³.MJinput-1",null,null,"Min:",null,null,"Max:"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"The uncertainty calculation will take approximately 50 seconds.\nA message box will appear when ready."]

{"sheet":"Results","index":12,"n_rows":298,"n_cols":19,"rows_kept":298,"cut":false,"hidden":false,"merged":[[32,6,35,17],[297,5,301,17],[257,5,257,11],[256,5,256,11],[255,5,255,11],[253,5,253,11],[252,5,252,11],[251,5,251,11],[85,6,92,18],[70,6,73,17],[289,12,289,13],[290,12,290,13],[291,12,291,13],[292,12,292,13],[293,12,293,13],[294,12,294,13],[229,7,229,10],[229,11,229,14],[229,16,229,17],[230,7,230,10],[230,11,230,14],[230,16,230,17],[231,7,231,10],[231,11,231,14],[231,16,231,17],[232,6,232,7],[233,16,233,17],[234,16,234,17],[237,6,244,17],[272,12,272,13],[273,12,273,13],[274,12,274,13],[275,12,275,13],[254,12,254,14],[254,16,254,17],[255,12,255,14],[255,16,255,17],[256,12,256,14],[256,16,256,17],[257,12,257,14],[257,16,257,17],[250,12,250,14],[250,16,250,17],[251,12,251,14],[251,16,251,17],[252,12,252,14],[252,16,252,17],[253,12,253,14],[278,5,282,17],[286,12,286,14],[286,15,286,16],[287,12,287,13],[288,12,288,13],[258,12,258,14],[258,16,258,17],[261,5,263,17],[267,12,267,14],[267,15,267,16],[268,12,268,13],[269,12,269,13],[270,12,270,13],[271,12,271,13],[253,16,253,17],[82,17,82,18],[79,7,79,9],[175,5,175,9],[176,5,176,9],[177,5,177,9],[248,12,248,14],[248,16,248,17],[249,12,249,14],[249,16,249,17],[181,17,181,18],[191,14,191,15],[221,5,225,18],[182,14,182,15],[182,17,182,18],[181,5,181,9],[173,14,173,15],[173,17,173,18],[180,14,180,15],[181,14,181,15],[174,14,174,15],[175,14,175,15],[176,14,176,15],[177,14,177,15],[77,17,77,18],[78,17,78,18],[77,7,77,9],[77,14,77,15],[78,7,78,9],[78,14,78,15],[172,14,172,15],[79,14,79,15],[127,6,130,18],[146,6,149,18],[165,6,168,18],[108,6,111,18],[80,6,80,7],[79,17,79,18],[81,17,81,18],[172,17,172,18],[178,14,178,15],[174,17,174,18],[175,17,175,18],[180,17,180,18],[176,17,176,18],[177,17,177,18],[210,16,210,17],[191,16,191,17],[179,5,179,9],[180,5,180,9],[179,14,179,15],[179,17,179,18],[178,17,178,18],[216,12,216,13],[217,12,217,13],[218,12,218,13],[181,11,181,13],[182,11,182,13],[191,11,191,13],[192,11,192,12],[193,11,193,12],[194,11,194,12],[211,12,211,13],[212,12,212,13],[213,12,213,13],[214,12,214,13],[215,12,215,13],[197,13,197,15],[198,13,198,15],[199,13,199,15],[185,5,187,18],[202,5,206,18],[51,6,55,18],[192,13,192,15],[193,13,193,15],[194,13,194,15],[195,13,195,15],[196,13,196,15],[210,12,210,15],[195,11,195,12],[196,11,196,12],[197,11,197,12],[198,11,198,12],[199,11,199,12],[77,10,77,13],[78,10,78,13],[79,10,79,13],[172,11,172,13],[173,11,173,13],[174,11,174,13],[175,11,175,13],[176,11,176,13],[177,11,177,13],[178,11,178,13],[179,11,179,13],[180,11,180,13]]}
[]
[]
[]
[]
[]
[]
[]
[null,"Overview of results"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Energy balance - fossil energy requirement (FER)"]
[]
[null,null,null,null,null,null,"Feedstock pathway 1 ","MJ/MJFS1","MJ/MJFU ",null,"Feedstock pathway 2 ","MJ/MJFS2","MJ/MJFU ",null,null,"Final conversion ",null,null,"MJ/MJFU "]
[null,null,null,null,null,null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP024a\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP025a\",Parameters!$1:$5663,7,FALSE)","v":0},null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP524a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP525a\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"Processing (ep)",null,null,{"$f":"VLOOKUP(\"FC045a\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Processing (ep)",{"$f":"VLOOKUP(\"BC094a\",Parameters!$1:$5663,7,FALSE)","v":1.6357622712156819E-3},{"$f":"VLOOKUP(\"BC095a\",Parameters!$1:$5663,7,FALSE)","v":1.6357622712156819E-3},null,"Processing (ep)",{"$f":"VLOOKUP(\"BC594a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC595a\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,{"$f":"VLOOKUP(\"LC010\",Parameters!$1:$1958,6,FALSE)","v":"No final conversion"},null,null,{"$f":"VLOOKUP(\"FC045a\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC003\",Parameters!$1:$1958,6,FALSE)","v":"Production of Crude Palm Oil (CPO)"},{"$f":"VLOOKUP(\"BC090a\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC091a\",Parameters!$1:$5663,7,FALSE)","v":0},null,{"$f":"VLOOKUP(\"LC503\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC590a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC591a\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,"purification",{"$f":"VLOOKUP(\"BC092a\",Parameters!$1:$5663,7,FALSE)","v":1.6357622712156819E-3},{"$f":"VLOOKUP(\"BC093a\",Parameters!$1:$5663,7,FALSE)","v":1.6357622712156819E-3},null,{"$f":"VLOOKUP(\"LC506\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC592a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC593a\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"TOTAL",null,"MJ/MJFU ",{"$f":"VLOOKUP(\"FC046a\",Parameters!$1:$5663,7,FALSE)","v":0.17800166505611817}]
[null,null,null,null,null,null,"Transport (etd)",{"$f":"VLOOKUP(\"FT026a\",Parameters!$1:$5663,7,FALSE)","v":0.1763659027849025},{"$f":"VLOOKUP(\"FT027a\",Parameters!$1:$5663,7,FALSE)","v":0.1763659027849025},null,"Transport (etd)",{"$f":"VLOOKUP(\"FT526a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT527a\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC001\",Parameters!$1:$1958,6,FALSE)","v":"Transport of FFB to the mill"},{"$f":"VLOOKUP(\"FT020a\",Parameters!$1:$5663,7,FALSE)","v":4.2427297465073593E-2},{"$f":"VLOOKUP(\"FT021a\",Parameters!$1:$5663,7,FALSE)","v":4.2427297465073593E-2},null,{"$f":"VLOOKUP(\"LC501\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT520a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT521a\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC004\",Parameters!$1:$1958,6,FALSE)","v":"Transport of CPO to Belgium"},{"$f":"VLOOKUP(\"FT022a\",Parameters!$1:$5663,7,FALSE)","v":0.1307783891036127},{"$f":"VLOOKUP(\"FT023a\",Parameters!$1:$5663,7,FALSE)","v":0.1307783891036127},null,{"$f":"VLOOKUP(\"LC504\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT522a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT523a\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"REDUCTION COMPARED TO REFERENCE",null,"%",{"$f":"VLOOKUP(\"FC052a\",Parameters!$1:$5663,7,FALSE)","v":84.655028874472578}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC007\",Parameters!$1:$1958,6,FALSE)","v":"Transport of PS to the final conversion unit"},{"$f":"VLOOKUP(\"FT024a\",Parameters!$1:$5663,7,FALSE)","v":3.1602162162162164E-3},{"$f":"VLOOKUP(\"FT025a\",Parameters!$1:$5663,7,FALSE)","v":3.1602162162162164E-3},null,{"$f":"VLOOKUP(\"LC507\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT524a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT525a\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Total feedstock pathway 1",{"$f":"VLOOKUP(\"BC082a\",Parameters!$1:$5663,7,FALSE)","v":0.17800166505611817},{"$f":"VLOOKUP(\"BC083a\",Parameters!$1:$5663,7,FALSE)","v":0.17800166505611817},null,"Total feedstock pathway 2",{"$f":"VLOOKUP(\"BC582a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC583a\",Parameters!$1:$5434,7,FALSE)","v":0}]
[]
[null,null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,null,"The results for the FER indicate how much fossil energy is needed for the production of one MJ functional unit (= electricity and/or heat) and which part(s) of the production chain contribute most. The result for \"reduction\" implies how much fossil fuel can be saved by the use of the particular bio-energy system. When this is a negative result, more fossil energy is needed to produce 1 MJ bio-energy than 1 MJ of the fossil reference energy.\n\n\n"]
[]
[]
[]
[]
[null,"Energy balance - net energy requirement (NER)"]
[]
[null,null,null,null,null,null,"Feedstock pathway 1 ","MJ/MJFS1","MJ/MJFU ",null,"Feedstock pathway 2 ","MJ/MJFS2","MJ/MJFU ",null,null,"Final conversion ",null,null,"MJ/MJFU "]
[null,null,null,null,null,null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP024b\",Parameters!$1:$5663,7,FALSE)","v":0.28755075519938561},{"$f":"VLOOKUP(\"FP025b\",Parameters!$1:$5663,7,FALSE)","v":0.28755075519938561},null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP524b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP525b\",Parameters!$1:$5465,7,FALSE)","v":0},null,null,"Processing (ep)",null,null,{"$f":"VLOOKUP(\"FC045b\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Processing (ep)",{"$f":"VLOOKUP(\"BC094b\",Parameters!$1:$5663,7,FALSE)","v":2.4536434068235229E-3},{"$f":"VLOOKUP(\"BC095b\",Parameters!$1:$5663,7,FALSE)","v":2.4536434068235229E-3},null,"Processing (ep)",{"$f":"VLOOKUP(\"BC594b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC595b\",Parameters!$1:$5465,7,FALSE)","v":0},null,null,{"$f":"VLOOKUP(\"LC010\",Parameters!$1:$1958,6,FALSE)","v":"No final conversion"},null,null,{"$f":"VLOOKUP(\"FC045b\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC003\",Parameters!$1:$1958,6,FALSE)","v":"Production of Crude Palm Oil (CPO)"},{"$f":"VLOOKUP(\"BC090b\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC091b\",Parameters!$1:$5663,7,FALSE)","v":0},null,{"$f":"VLOOKUP(\"LC503\",Parameters!$1:$1760,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC590b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC591b\",Parameters!$1:$5465,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC006\",Parameters!$1:$1958,6,FALSE)","v":"Refinery of Crude Palm Oil"},{"$f":"VLOOKUP(\"BC092b\",Parameters!$1:$5663,7,FALSE)","v":2.4536434068235229E-3},{"$f":"VLOOKUP(\"BC093b\",Parameters!$1:$5663,7,FALSE)","v":2.4536434068235229E-3},null,{"$f":"VLOOKUP(\"LC506\",Parameters!$1:$1760,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC592b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC593b\",Parameters!$1:$5465,7,FALSE)","v":0},null,null,"TOTAL",null,"MJ/MJFU ",{"$f":"VLOOKUP(\"FC046b\",Parameters!$1:$5663,7,FALSE)","v":0.55455325278356304}]
[null,null,null,null,null,null,"Transport (etd)",{"$f":"VLOOKUP(\"FT026b\",Parameters!$1:$5663,7,FALSE)","v":0.26454885417735374},{"$f":"VLOOKUP(\"FT027b\",Parameters!$1:$5663,7,FALSE)","v":0.26454885417735374},null,"Transport (etd)",{"$f":"VLOOKUP(\"FT526b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT527b\",Parameters!$1:$5465,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC001\",Parameters!$1:$1958,6,FALSE)","v":"Transport of FFB to the mill"},{"$f":"VLOOKUP(\"FT020b\",Parameters!$1:$5663,7,FALSE)","v":6.364094619761039E-2},{"$f":"VLOOKUP(\"FT021b\",Parameters!$1:$5663,7,FALSE)","v":6.364094619761039E-2},null,{"$f":"VLOOKUP(\"LC501\",Parameters!$1:$1760,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT520b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT521b\",Parameters!$1:$5465,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC004\",Parameters!$1:$1958,6,FALSE)","v":"Transport of CPO to Belgium"},{"$f":"VLOOKUP(\"FT022b\",Parameters!$1:$5663,7,FALSE)","v":0.19616758365541906},{"$f":"VLOOKUP(\"FT023b\",Parameters!$1:$5663,7,FALSE)","v":0.19616758365541906},null,{"$f":"VLOOKUP(\"LC504\",Parameters!$1:$1760,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT522b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT523b\",Parameters!$1:$5465,7,FALSE)","v":0},null,null,"REDUCTION COMPARED TO REFERENCE",null,"%",{"$f":"VLOOKUP(\"FC052b\",Parameters!$1:$5663,7,FALSE)","v":68.129123403243497}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC007\",Parameters!$1:$1958,6,FALSE)","v":"Transport of PS to the final conversion unit"},{"$f":"VLOOKUP(\"FT024b\",Parameters!$1:$5663,7,FALSE)","v":4.7403243243243241E-3},{"$f":"VLOOKUP(\"FT025b\",Parameters!$1:$5663,7,FALSE)","v":4.7403243243243241E-3},null,{"$f":"VLOOKUP(\"LC507\",Parameters!$1:$1760,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT524b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT525b\",Parameters!$1:$5465,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Total feedstock pathway 1",{"$f":"VLOOKUP(\"BC082b\",Parameters!$1:$5663,7,FALSE)","v":0.55455325278356304},{"$f":"VLOOKUP(\"BC083b\",Parameters!$1:$5663,7,FALSE)","v":0.55455325278356304},null,"Total feedstock pathway 2",{"$f":"VLOOKUP(\"BC582b\",Parameters!$1:$5465,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC583b\",Parameters!$1:$5465,7,FALSE)","v":0}]
[]
[null,null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,null,"Similar as explanation of FER."]
[]
[]
[]
[]
[null,"Global warming - greenhouse gas balance"]
[]
[null,null,null,null,null,null,"Feedstock pathway 1 ","gCO2_eq/MJFS1","gCO2_eq/MJFU",null,"Feedstock pathway 2 ","gCO2_eq/MJFS1","gCO2_eq/MJFU",null,null,"Final conversion ",null,null,"gCO2_eq/MJFU"]
[null,null,null,null,null,null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP061a\",Parameters!$1:$5663,7,FALSE)","v":44.685763325221714},{"$f":"VLOOKUP(\"FP061b\",Parameters!$1:$5663,7,FALSE)","v":44.685763325221714},null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP561a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP561b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"Processing (ep)",null,null,{"$f":"VLOOKUP(\"FC045c\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Processing (ep)",{"$f":"VLOOKUP(\"BC094c\",Parameters!$1:$5663,7,FALSE)","v":0.65300153519651516},{"$f":"VLOOKUP(\"BC095c\",Parameters!$1:$5663,7,FALSE)","v":0.65300153519651516},null,"Processing (ep)",{"$f":"VLOOKUP(\"BC594c\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC595c\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,{"$f":"VLOOKUP(\"LC010\",Parameters!$1:$1958,6,FALSE)","v":"No final conversion"},null,null,{"$f":"VLOOKUP(\"FC045c\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC003\",Parameters!$1:$1958,6,FALSE)","v":"Production of Crude Palm Oil (CPO)"},{"$f":"VLOOKUP(\"BC090c\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC091c\",Parameters!$1:$5663,7,FALSE)","v":0},null,{"$f":"VLOOKUP(\"LC503\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC590c\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC591c\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC006\",Parameters!$1:$1958,6,FALSE)","v":"Refinery of Crude Palm Oil"},{"$f":"VLOOKUP(\"BC092c\",Parameters!$1:$5663,7,FALSE)","v":0.65300153519651516},{"$f":"VLOOKUP(\"BC093c\",Parameters!$1:$5663,7,FALSE)","v":0.65300153519651516},null,{"$f":"VLOOKUP(\"LC506\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC592c\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC593c\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"TOTAL",null,"gCO2_eq/MJFU",{"$f":"VLOOKUP(\"FC046c\",Parameters!$1:$5663,7,FALSE)","v":59.196326779586677}]
[null,null,null,null,null,null,"Transport (etd)",{"$f":"VLOOKUP(\"FT033a\",Parameters!$1:$5663,7,FALSE)","v":13.857561919168443},{"$f":"VLOOKUP(\"FT033b\",Parameters!$1:$5663,7,FALSE)","v":13.857561919168443},null,"Transport (etd)",{"$f":"VLOOKUP(\"FT533a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT533b\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC001\",Parameters!$1:$1958,6,FALSE)","v":"Transport of FFB to the mill"},{"$f":"VLOOKUP(\"FT030a\",Parameters!$1:$5663,7,FALSE)","v":3.2054148348253646},{"$f":"VLOOKUP(\"FT030b\",Parameters!$1:$5663,7,FALSE)","v":3.2054148348253646},null,{"$f":"VLOOKUP(\"LC501\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT530a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT530b\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC004\",Parameters!$1:$1958,6,FALSE)","v":"Transport of CPO to Belgium"},{"$f":"VLOOKUP(\"FT031a\",Parameters!$1:$5663,7,FALSE)","v":10.41339032758632},{"$f":"VLOOKUP(\"FT031b\",Parameters!$1:$5663,7,FALSE)","v":10.41339032758632},null,{"$f":"VLOOKUP(\"LC504\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT531a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT531b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"REDUCTION",null,"%",{"$f":"VLOOKUP(\"FC052c\",Parameters!$1:$5663,7,FALSE)","v":32.454270552611092}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC007\",Parameters!$1:$1958,6,FALSE)","v":"Transport of PS to the final conversion unit"},{"$f":"VLOOKUP(\"FT032a\",Parameters!$1:$5663,7,FALSE)","v":0.23875675675675681},{"$f":"VLOOKUP(\"FT032b\",Parameters!$1:$5663,7,FALSE)","v":0.23875675675675681},null,{"$f":"VLOOKUP(\"LC507\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT532a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT532b\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Total feedstock pathway 1",{"$f":"VLOOKUP(\"BC082c\",Parameters!$1:$5663,7,FALSE)","v":59.196326779586677},{"$f":"VLOOKUP(\"BC083c\",Parameters!$1:$5663,7,FALSE)","v":59.196326779586677},null,"Total feedstock pathway 2",{"$f":"VLOOKUP(\"BC582c\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC583c\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"COMPLIANCE WITH RED REQUIREMENT",null,null,{"$f":"VLOOKUP(\"FC029\",Parameters!$1:$5663,7,FALSE)","v":"no"}]
[null,null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,null,"For bio-energy systems based on energy crops, the cultivation step contributes most to the total emissions of greenhouse gases. This is mainly due to the use of fertilizers and pesticides, and soil carbon emissions in case of land use change prior to cultivation. Therefore, the GHG balance can be positively influenced (i.e. less GHG emissions) by the use of biomass sources without cultivation step (e.g. organic residues). Note that impacts of indirect land use change are not included in this tool as there is not yet an agreement on this topic on EU level. It is highly recommended to include these impacts as soon as possible.\n\n"]
[]
[]
[]
[]
[null,"Global warming - carbon debt and repayment time"]
[]
[null,null,null,null,null,null,null,"Previous land use",null,null,"Actual land use",null,null,null,null,null,null,"Carbon Debt (tCO2_eq/ha)"]
[null,null,null,null,null,null,"Feedstock pathway 1 ",{"$f":"VLOOKUP(\"FP069b\",Parameters!$1:$5663,6,FALSE)","v":"Perennial cropland"},null,null,{"$f":"VLOOKUP(\"FP069a\",Parameters!$1:$5434,6,FALSE)","v":"Perennial cropland"},null,null,null,null,null,null,{"$f":"VLOOKUP(\"FP107a\",Parameters!$1:$5663,7,FALSE)/1000000","v":0}]
[null,null,null,null,null,null,"Feedstock pathway 2 ",{"$f":"VLOOKUP(\"FP569b\",Parameters!$1:$5663,6,FALSE)","v":"Annual cropland"},null,null,{"$f":"VLOOKUP(\"FP569a\",Parameters!$1:$5434,6,FALSE)","v":"n.a."},null,null,null,null,null,null,{"$f":"VLOOKUP(\"FP607a\",Parameters!$1:$5663,7,FALSE)/1000000","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"gCO2_eq/MJFU",null,{"$f":"VLOOKUP(\"FC055\",Parameters!$1:$5288,7,FALSE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"years",null,{"$f":"IF(VLOOKUP(\"FC056\",Parameters!$1:$5663,7,FALSE)<0,0,VLOOKUP(\"FC056\",Parameters!$1:$5663,7,FALSE))","v":0}]
[]
[null,null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,null,"The carbon debt indicates how much carbon was lost during the (direct) conversion of the land prior to cultivation of the biomass feedstock. This includes the carbon stock changes in the soil as well as in above and below ground vegetation. In case no land use change is carried out prior to cultivation, the carbon debt is zero. The risk of carbon debt can therefore be omitted by the use of biomass resources that require no additional land (e.g. organic residues). As is the case for the greenhouse gas balance, the impacts of indirect land use changes are not considered for the calculation of the carbon debt.\nThe repayment time indicates how many years are needed to repay the initial carbon debt by the reduced GHG emissions of the bio-energy system. \"No repayment possible\" means repayment time would be endless, or in other words the bio-energy system does not cause any emission reduction compared to the reference system making repayment impossible."]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Resource use - water"]
[]
[null,null,null,null,null,null,"Feedstock pathway 1 ","m³/GJFS1","m³/GJFU ",null,"Feedstock pathway 2 ","m³/GJFS2","m³/GJFU ",null,null,"Final conversion ",null,null,"m³/GJFU "]
[null,null,null,null,null,null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP102a\",Parameters!$1:$5663,7,FALSE)","v":422.20878511090552},{"$f":"VLOOKUP(\"FP102b\",Parameters!$1:$5663,7,FALSE)","v":422.20878511090552},null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP602a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP602b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"Processing (ep)",null,null,{"$f":"VLOOKUP(\"FC045d\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Processing (ep)",{"$f":"VLOOKUP(\"BC094d\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC095d\",Parameters!$1:$5663,7,FALSE)","v":0},null,"Processing (ep)",{"$f":"VLOOKUP(\"BC594d\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC595d\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,{"$f":"VLOOKUP(\"LC010\",Parameters!$1:$1958,6,FALSE)","v":"No final conversion"},null,null,{"$f":"VLOOKUP(\"FC045d\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC003\",Parameters!$1:$1958,6,FALSE)","v":"Production of Crude Palm Oil (CPO)"},{"$f":"VLOOKUP(\"BC090d\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC091d\",Parameters!$1:$5663,7,FALSE)","v":0},null,{"$f":"VLOOKUP(\"LC503\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC590d\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC591d\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"TOTAL",null,"m³/GJFU ",{"$f":"VLOOKUP(\"FC046d\",Parameters!$1:$5663,7,FALSE)","v":422.20878511090552}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC006\",Parameters!$1:$1958,6,FALSE)","v":"Refinery of Crude Palm Oil"},{"$f":"VLOOKUP(\"BC092d\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC093d\",Parameters!$1:$5663,7,FALSE)","v":0},null,{"$f":"VLOOKUP(\"LC506\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC592d\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC593d\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"electricity",{"$f":"VLOOKUP(\"FC044d\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Transport (etd)",0,0,null,"Transport (etd)",0,0,null,null,null,null,"heat",{"$f":"VLOOKUP(\"FC042d\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC001\",Parameters!$1:$1958,6,FALSE)","v":"Transport of FFB to the mill"},0,0,null,{"$f":"VLOOKUP(\"LC501\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},0,0,null,null,"REDUCTION COMPARED TO REFERENCE",null,"m³/GJFU ",{"$f":"VLOOKUP(\"FC052d\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC004\",Parameters!$1:$1958,6,FALSE)","v":"Transport of CPO to Belgium"},0,0,null,{"$f":"VLOOKUP(\"LC504\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},0,0,null,null,null,null,"electricity",{"$f":"VLOOKUP(\"FC049d\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC007\",Parameters!$1:$1958,6,FALSE)","v":"Transport of PS to the final conversion unit"},0,0,null,{"$f":"VLOOKUP(\"LC507\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},0,0,null,null,null,null,"heat",{"$f":"VLOOKUP(\"FC050d\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Total feedstock pathway 1",{"$f":"VLOOKUP(\"BC082d\",Parameters!$1:$5663,7,FALSE)","v":422.20878511090552},{"$f":"VLOOKUP(\"BC083d\",Parameters!$1:$5663,7,FALSE)","v":422.20878511090552},null,"Total feedstock pathway 2",{"$f":"VLOOKUP(\"BC582d\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC583d\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"WATER AVAILABILITY",null,"m³/capita.yr ","level"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Feedstock 1",{"$f":"VLOOKUP(\"FP002\",Parameters!$1:$5663,6,FALSE)","v":"Malaysia"},{"$f":"VLOOKUP(\"FP104a\",Parameters!$1:$5663,7,FALSE)","v":23320},{"$f":"VLOOKUP(\"FP104b\",Parameters!$1:$5663,7,FALSE)","v":"high"}]
[null,null,null,null,null,null,"Interpretation of results:",null,null,null,null,null,null,null,null,"Feedstock 2",{"$f":"VLOOKUP(\"FP502\",Parameters!$1:$5663,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FP604a\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP604b\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Although fresh water is becoming an increasingly scarce resource worldwide, the impact of the use of water very much depend on local circumstances. The calculation of water use in this tool includes the fresh water used for irrigation and evapotranspiration during the production phase as well as for processing. Some crops have much higher water demands than others. Their cultivation should therefore be avoided in water scarce regions. Although this tool gives an indication of the water condition in the country of cultivation, local circumstances can be very different and should be considered as much as possible."]
[]
[]
[]
[]
[null,"Resource use - land"]
[]
[null,null,null,null,null,null,"Feedstock pathway 1 ","ha/GJFS1","ha/GJFU ",null,"Feedstock pathway 2 ","ha/GJFS2","ha/GJFU ",null,null,"Final conversion ",null,null,"ha/GJFU "]
[null,null,null,null,null,null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP106a\",Parameters!$1:$5663,7,FALSE)","v":1.9132606099961733E-2},{"$f":"VLOOKUP(\"FP106b\",Parameters!$1:$5663,7,FALSE)","v":1.9132606099961733E-2},null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP606a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP606b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"Processing (ep)",null,null,0]
[null,null,null,null,null,null,"Processing (ep)",0,0,null,"Processing (ep)",0,0,null,null,{"$f":"VLOOKUP(\"LC010\",Parameters!$1:$1958,6,FALSE)","v":"No final conversion"},null,null,0]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC003\",Parameters!$1:$1958,6,FALSE)","v":"Production of Crude Palm Oil (CPO)"},0,0,null,{"$f":"VLOOKUP(\"LC503\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},0,0]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC006\",Parameters!$1:$1958,6,FALSE)","v":"Refinery of Crude Palm Oil"},0,0,null,{"$f":"VLOOKUP(\"LC506\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},0,0,null,null,"TOTAL",null,"ha/GJFU ",{"$f":"VLOOKUP(\"FC046e\",Parameters!$1:$5663,7,FALSE)","v":1.9132606099961733E-2}]
[null,null,null,null,null,null,"Transport (etd)",0,0,null,"Transport (etd)",0,0,null,null,null,null,"electricity",{"$f":"VLOOKUP(\"FC044e\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC001\",Parameters!$1:$1958,6,FALSE)","v":"Transport of FFB to the mill"},0,0,null,{"$f":"VLOOKUP(\"LC501\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},0,0,null,null,null,null,"heat",{"$f":"VLOOKUP(\"FC042e\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC004\",Parameters!$1:$1958,6,FALSE)","v":"Transport of CPO to Belgium"},0,0,null,{"$f":"VLOOKUP(\"LC504\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},0,0]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC007\",Parameters!$1:$1958,6,FALSE)","v":"Transport of PS to the final conversion unit"},0,0,null,{"$f":"VLOOKUP(\"LC507\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},0,0]
[null,null,null,null,null,null,"Total feedstock pathway 1",{"$f":"VLOOKUP(\"FP106a\",Parameters!$1:$5663,7,FALSE)","v":1.9132606099961733E-2},{"$f":"VLOOKUP(\"FP106b\",Parameters!$1:$5663,7,FALSE)","v":1.9132606099961733E-2},null,"Total feedstock pathway 2",{"$f":"VLOOKUP(\"FP606a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP606b\",Parameters!$1:$5434,7,FALSE)","v":0}]
[]
[null,null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,null,"Increasing amounts of land are needed to feed the growing world population and it does not seem as this will change soon. Although various reasons lay behind the latest trends of increasing food prices, the impact of bio-energy production on food security due to land use competition cannot be denied. As with water use,  the impact of the use of land depends on local circumstances. Yet, it can be generally stated that risks can be minimised by the use of biomass feestocks that require the smallest amount of land for its production."]
[]
[]
[]
[]
[null,"Environmental quality - acidification potential"]
[]
[null,null,null,null,null,null,"Feedstock pathway 1 ","gSO2_eq/MJFS1","gSO2_eq/MJFU",null,"Feedstock pathway 2 ","gSO2_eq/MJFS1","gSO2_eq/MJFU",null,null,"Final conversion ",null,null,"gSO2_eq/MJFU"]
[null,null,null,null,null,null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP115a\",Parameters!$1:$5663,7,FALSE)","v":0.78450695493120459},{"$f":"VLOOKUP(\"FP115b\",Parameters!$1:$5663,7,FALSE)","v":0.78450695493120459},null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP615a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP615b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"Processing (ep)",null,null,{"$f":"VLOOKUP(\"FC045f\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Processing (ep)",{"$f":"VLOOKUP(\"BC094f\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC095f\",Parameters!$1:$5663,7,FALSE)","v":0},null,"Processing (ep)",{"$f":"VLOOKUP(\"BC594f\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC595f\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,{"$f":"VLOOKUP(\"LC010\",Parameters!$1:$1958,6,FALSE)","v":"No final conversion"},null,null,{"$f":"VLOOKUP(\"FC045f\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC003\",Parameters!$1:$1958,6,FALSE)","v":"Production of Crude Palm Oil (CPO)"},{"$f":"VLOOKUP(\"BC090f\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC091f\",Parameters!$1:$5663,7,FALSE)","v":0},null,{"$f":"VLOOKUP(\"LC503\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC590f\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC591f\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC006\",Parameters!$1:$1958,6,FALSE)","v":"Refinery of Crude Palm Oil"},{"$f":"VLOOKUP(\"BC092f\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC093f\",Parameters!$1:$5663,7,FALSE)","v":0},null,{"$f":"VLOOKUP(\"LC506\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC592f\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC593f\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"TOTAL",null,"gSO2_eq/MJFU",{"$f":"VLOOKUP(\"FC046f\",Parameters!$1:$5663,7,FALSE)","v":0.93786277735394152}]
[null,null,null,null,null,null,"Transport (etd)",{"$f":"VLOOKUP(\"FT043a\",Parameters!$1:$5663,7,FALSE)","v":0.15335582242273696},{"$f":"VLOOKUP(\"FT043b\",Parameters!$1:$5663,7,FALSE)","v":0.15335582242273696},null,"Transport (etd)",{"$f":"VLOOKUP(\"FT543a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT543b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"electricity",{"$f":"VLOOKUP(\"FC044f\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC001\",Parameters!$1:$1958,6,FALSE)","v":"Transport of FFB to the mill"},{"$f":"VLOOKUP(\"FT040a\",Parameters!$1:$5663,7,FALSE)","v":3.5353642870465642E-2},{"$f":"VLOOKUP(\"FT040b\",Parameters!$1:$5663,7,FALSE)","v":3.5353642870465642E-2},null,{"$f":"VLOOKUP(\"LC501\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT540a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT540b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"heat",{"$f":"VLOOKUP(\"FC042f\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC004\",Parameters!$1:$1958,6,FALSE)","v":"Transport of CPO to Belgium"},{"$f":"VLOOKUP(\"FT041a\",Parameters!$1:$5663,7,FALSE)","v":0.11536884766037943},{"$f":"VLOOKUP(\"FT041b\",Parameters!$1:$5663,7,FALSE)","v":0.11536884766037943},null,{"$f":"VLOOKUP(\"LC504\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT541a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT541b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"REDUCTION COMPARED TO REFERENCE",null,"%",{"$f":"VLOOKUP(\"FC052f\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC007\",Parameters!$1:$1958,6,FALSE)","v":"Transport of PS to the final conversion unit"},{"$f":"VLOOKUP(\"FT042a\",Parameters!$1:$5663,7,FALSE)","v":2.633331891891892E-3},{"$f":"VLOOKUP(\"FT042b\",Parameters!$1:$5663,7,FALSE)","v":2.633331891891892E-3},null,{"$f":"VLOOKUP(\"LC507\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT542a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT542b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"electricity",{"$f":"VLOOKUP(\"FC049f\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Total feedstock pathway 1",{"$f":"VLOOKUP(\"BC082f\",Parameters!$1:$5663,7,FALSE)","v":0.93786277735394152},{"$f":"VLOOKUP(\"BC083f\",Parameters!$1:$5663,7,FALSE)","v":0.93786277735394152},null,"Total feedstock pathway 2",{"$f":"VLOOKUP(\"BC582f\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC583f\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"heat",{"$f":"VLOOKUP(\"FC050f\",Parameters!$1:$5663,7,FALSE)","v":0}]
[]
[null,null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,null,"The acidification potential as it is calculated in this tool gives an indication of the risk of reduced environmental quality caused by a variety of air polutants. Main causes of acidification within a bio-energy production system are NH3 volatilization due to N fertilizer application during cultivation, and NOX and SOX emissions from fuel use during transport and processing."]
[]
[]
[]
[]
[null,"Environmental quality - eutrophication potential"]
[]
[null,null,null,null,null,null,"Feedstock pathway 1 ","gPO4_eq/MJFS1","gPO4_eq/MJFU",null,"Feedstock pathway 2 ","gPO4_eq/MJFS1","gPO4_eq/MJFU",null,null,"Final conversion ",null,null,"gPO4_eq/MJFU"]
[null,null,null,null,null,null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP125a\",Parameters!$1:$5663,7,FALSE)","v":1.9914646988440075},{"$f":"VLOOKUP(\"FP125b\",Parameters!$1:$5663,7,FALSE)","v":1.9914646988440075},null,"Cultivation (eec)",{"$f":"VLOOKUP(\"FP625a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FP625b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"Processing (ep)",null,null,{"$f":"VLOOKUP(\"FC045g\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Processing (ep)",{"$f":"VLOOKUP(\"BC094g\",Parameters!$1:$5663,7,FALSE)","v":1.3159295156592201},{"$f":"VLOOKUP(\"BC095g\",Parameters!$1:$5663,7,FALSE)","v":1.3159295156592201},null,"Processing (ep)",{"$f":"VLOOKUP(\"BC594g\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC595g\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,{"$f":"VLOOKUP(\"LC010\",Parameters!$1:$1958,6,FALSE)","v":"No final conversion"},null,null,{"$f":"VLOOKUP(\"FC045g\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC003\",Parameters!$1:$1958,6,FALSE)","v":"Production of Crude Palm Oil (CPO)"},{"$f":"VLOOKUP(\"BC090g\",Parameters!$1:$5663,7,FALSE)","v":1.3159295156592201},{"$f":"VLOOKUP(\"BC091g\",Parameters!$1:$5663,7,FALSE)","v":1.3159295156592201},null,{"$f":"VLOOKUP(\"LC503\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC590g\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC591g\",Parameters!$1:$5434,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC006\",Parameters!$1:$1958,6,FALSE)","v":"Refinery of Crude Palm Oil"},{"$f":"VLOOKUP(\"BC092g\",Parameters!$1:$5663,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC093g\",Parameters!$1:$5663,7,FALSE)","v":0},null,{"$f":"VLOOKUP(\"LC506\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"BC592g\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC593g\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"TOTAL",null,"gPO4_eq/MJFU",{"$f":"VLOOKUP(\"FC046g\",Parameters!$1:$5663,7,FALSE)","v":3.3257093356913932}]
[null,null,null,null,null,null,"Transport (etd)",{"$f":"VLOOKUP(\"FT047a\",Parameters!$1:$5663,7,FALSE)","v":1.8315121188165487E-2},{"$f":"VLOOKUP(\"FT047b\",Parameters!$1:$5663,7,FALSE)","v":1.8315121188165487E-2},null,"Transport (etd)",{"$f":"VLOOKUP(\"FT547a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT547b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"electricity",{"$f":"VLOOKUP(\"FC044g\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC001\",Parameters!$1:$1958,6,FALSE)","v":"Transport of FFB to the mill"},{"$f":"VLOOKUP(\"FT044a\",Parameters!$1:$5663,7,FALSE)","v":4.2222476029035319E-3},{"$f":"VLOOKUP(\"FT044b\",Parameters!$1:$5663,7,FALSE)","v":4.2222476029035319E-3},null,{"$f":"VLOOKUP(\"LC501\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT544a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT544b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"heat",{"$f":"VLOOKUP(\"FC042g\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC004\",Parameters!$1:$1958,6,FALSE)","v":"Transport of CPO to Belgium"},{"$f":"VLOOKUP(\"FT045a\",Parameters!$1:$5663,7,FALSE)","v":1.3778377585261953E-2},{"$f":"VLOOKUP(\"FT045b\",Parameters!$1:$5663,7,FALSE)","v":1.3778377585261953E-2},null,{"$f":"VLOOKUP(\"LC504\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT545a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT545b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,"REDUCTION COMPARED TO REFERENCE",null,"%",{"$f":"VLOOKUP(\"FC052g\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,{"$f":"VLOOKUP(\"LC007\",Parameters!$1:$1958,6,FALSE)","v":"Transport of PS to the final conversion unit"},{"$f":"VLOOKUP(\"FT046a\",Parameters!$1:$5663,7,FALSE)","v":3.1449600000000005E-4},{"$f":"VLOOKUP(\"FT046b\",Parameters!$1:$5663,7,FALSE)","v":3.144960000000001E-4},null,{"$f":"VLOOKUP(\"LC507\",Parameters!$1:$1729,6,FALSE)","v":"n.a."},{"$f":"VLOOKUP(\"FT546a\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"FT546b\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"electricity",{"$f":"VLOOKUP(\"FC049g\",Parameters!$1:$5663,7,FALSE)","v":0}]
[null,null,null,null,null,null,"Total feedstock pathway 1",{"$f":"VLOOKUP(\"BC082g\",Parameters!$1:$5663,7,FALSE)","v":3.3257093356913932},{"$f":"VLOOKUP(\"BC083g\",Parameters!$1:$5663,7,FALSE)","v":3.3257093356913932},null,"Total feedstock pathway 2",{"$f":"VLOOKUP(\"BC582g\",Parameters!$1:$5434,7,FALSE)","v":0},{"$f":"VLOOKUP(\"BC583g\",Parameters!$1:$5434,7,FALSE)","v":0},null,null,null,null,"heat",{"$f":"VLOOKUP(\"FC050g\",Parameters!$1:$5663,7,FALSE)","v":0}]
[]
[null,null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,null,"The eutrophication potential as it is calculated in this tool gives an indication of the risk of reduced environmental quality caused by a variety of air and water polutants. Main causes of eutrophication within a bio-energy production system are leaching and  volatilization of N due to fertilizer application during cultivation, NOX emissions from fuel use during transport and processing, and leaching of untreated wastewater (typically in palm oil production)."]
[]
[]
[]
[]
[null,"Biodiversity - biodiversity & high carbon stocks"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Feedstock pathway 1 ",null,null,null,null,null,"Feedstock pathway 2"]
[null,null,null,null,null,null,null,null,null,null,null,"Cultivation",null,null,null,null,null,"Cultivation"]
[null,null,null,null,null,"Land with high biodiversity value"]
[null,null,null,null,1,"Undisturbed forest",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP161\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP661\",Parameters!$1:$5296,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,2,"Nature protection area",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP162\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP662\",Parameters!$1:$5296,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,3,"Highly biodiverse grassland",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP163\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"},null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP663\",Parameters!$1:$5296,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Land with high carbon stock"]
[null,null,null,null,4,"Wetlands",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP164\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"},null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP664\",Parameters!$1:$5296,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,5,"Continuously forested areas",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP165\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP665\",Parameters!$1:$5296,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,6,"Peatland",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP166\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"},null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP666\",Parameters!$1:$5296,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Compliance with RED requirements",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP167\",Parameters!$1:$5067,7,FALSE)=1,\"√\",\"x\")","v":"√"},null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP667\",Parameters!$1:$5296,7,FALSE)=1,\"√\",\"x\")","v":"√"}]
[]
[null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,"As could be noticed in the biodiversity calculation sheet, the impacts of bio-energy production on biodiversity/carbon stocks are not easily measurable. The sustainability requirements in this tool are adopted from and restricted to those laid down in the Renewable Energy Directive. Reliable data on biodiversity are still scarce and possible impacts depend on many different factors. The results must therefore be seen as an indication and a more profound assessment of this topic is highly recommended."]
[]
[]
[]
[null,"Local Well-being - human and property rights"]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Feedstock pathway 1 ",null,null,null,null,"Feedstock pathway 2",null,"Final conv."]
[null,null,null,null,null,null,null,null,null,null,null,"Cultivation",null,"Processing",null,null,"Cultivation","Processing","Processing"]
[null,null,null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,{"$f":"IF(VLOOKUP(\"FP670a\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654a\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080a\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,{"$f":"IF(VLOOKUP(\"FP670b\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654b\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080b\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,{"$f":"IF(VLOOKUP(\"FP670c\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654c\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080c\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,{"$f":"IF(VLOOKUP(\"FP670d\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654d\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080d\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"The producer can proof that the land is used legitimately and that traditional land rights have been secured",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170e\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,"√",null,null,{"$f":"IF(VLOOKUP(\"FP670e\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},"√","√"]
[null,null,null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,{"$f":"IF(VLOOKUP(\"FP670f\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654f\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080f\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"The biomass production does not impair food security",null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170g\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,"√",null,null,{"$f":"IF(VLOOKUP(\"FP670g\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},"√","√"]
[]
[null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,"In many sustainability assessments, social criteria are omitted due to a lack of qualitative indicators and widespread accessible data. Moreover, socio-economic and cultural differences throughout the world complicate the use of a defined set of indicators and standards. Therefore, the approach adopted in this tool rather aims at giving the user an idea of which issues play an important role in the social dimension of the sustainability of bio-energy systems, than providing a straight forward answer. The reporting requirements on social issues in the RED and the development of certification systems such as RSPO, RSB and FSC among others can bring more clarity on these topics. The criteria in this tool on human and property rights are the same that can be found in these systems."]
[]
[]
[]
[]
[]
[null,"Local Well-being - working conditions"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Feedstock pathway 1 ",null,null,null,"Feedstock pathway 2",null,"Final conv."]
[null,null,null,null,null,null,null,null,null,null,null,null,"Cultivation",null,"Processing","Processing","Cultivation","Processing","Processing"]
[null,null,null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"BC155a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP671a\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655a\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081a\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"BC155b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP671b\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655b\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081b\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"BC155c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP671c\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655c\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081c\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"BC155d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP671d\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655d\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081d\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171e\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,"√","√",{"$f":"IF(VLOOKUP(\"FP671e\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},"√","√"]
[null,null,null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"BC155f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP670f\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655f\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081f\",Parameters!$1:$5296,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171g\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,"√","√",{"$f":"IF(VLOOKUP(\"FP671g\",Parameters!$1:$5296,7,FALSE)=0,\"√\",\"x\")","v":"√"},"√","√"]
[]
[null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,"Same as explanation of human and property rights."]
[]
[]
[]
[]
[]
[null,"Global warming - carbon debt and repayment time"]
[]
[null,null,null,null,null,null,null,"Previous land use",null,null,null,"Actual land use",null,null,null,null,"Carbon Debt (tCO2_eq/ha)"]
[null,null,null,null,null,null,"Feedstock pathway 1 ",{"$f":"VLOOKUP(\"FP069b\",Parameters!$1:$5434,6,FALSE)","v":"Perennial cropland"},null,null,null,{"$f":"VLOOKUP(\"FP069a\",Parameters!$1:$5434,6,FALSE)","v":"Perennial cropland"},null,null,null,null,{"$f":"VLOOKUP(\"FP107a\",Parameters!$1:$5434,7,FALSE)/1000000","v":0}]
[null,null,null,null,null,null,"Feedstock pathway 2 ",{"$f":"VLOOKUP(\"FP569b\",Parameters!$1:$5434,6,FALSE)","v":"Annual cropland"},null,null,null,{"$f":"VLOOKUP(\"FP569a\",Parameters!$1:$5434,6,FALSE)","v":"n.a."},null,null,null,null,{"$f":"VLOOKUP(\"FP607a\",Parameters!$1:$5434,7,FALSE)/1000000","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,"TOTAL CARBON DEBT DUE TO LAND USE CHANGE",null,null,null,"gCO2_eq/MJFU",null,{"$f":"VLOOKUP(\"FC055\",Parameters!$1:$5059,7,FALSE)","v":0}]
[null,null,null,null,null,null,null,null,null,null,"REPAYMENT TIME",null,null,null,"years",null,{"$f":"IF(VLOOKUP(\"FC056\",Parameters!$1:$5434,7,FALSE)<0,0,VLOOKUP(\"FC056\",Parameters!$1:$5434,7,FALSE))","v":0}]
[]
[null,null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,null,"The carbon debt indicates how much carbon was lost during the (direct) conversion of the land prior to cultivation of the biomass feedstock. This includes the carbon stock changes in the soil as well as in above and below ground vegetation. In case no land use change is carried out prior to cultivation, the carbon debt is zero. The risk of carbon debt can therefore be omitted by the use of biomass resources that require no additional land (e.g. organic residues). As is the case for the greenhouse gas balance, the impacts of indirect land use changes are not considered for the calculation of the carbon debt.\nThe repayment time indicates how many years are needed to repay the initial carbon debt by the reduced GHG emissions of the bio-energy system. \"No repayment possible\" means repayment time would be endless, or in other words the bio-energy system does not cause any emission reduction compared to the reference system making repayment impossible."]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Biodiversity - biodiversity & high carbon stocks"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Feedstock pathway 1 ",null,null,null,"Feedstock pathway 2"]
[null,null,null,null,null,null,null,null,null,null,null,null,"Cultivation",null,null,null,"Cultivation"]
[null,null,null,null,null,"Land with high biodiversity value"]
[null,null,null,null,1,"Undisturbed forest",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP161\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,null,{"$f":"IF(VLOOKUP(\"FP661\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,2,"Nature protection area",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP162\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,null,{"$f":"IF(VLOOKUP(\"FP662\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,3,"Highly biodiverse grassland",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP163\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"},null,null,null,{"$f":"IF(VLOOKUP(\"FP663\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Land with high carbon stock"]
[null,null,null,null,4,"Wetlands",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP164\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"},null,null,null,{"$f":"IF(VLOOKUP(\"FP664\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,5,"Continuously forested areas",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP165\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"x"},null,null,null,{"$f":"IF(VLOOKUP(\"FP665\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,6,"Peatland",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP166\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"},null,null,null,{"$f":"IF(VLOOKUP(\"FP666\",Parameters!$1:$5067,6,FALSE)=0,\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Compliance with RED requirements",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP167\",Parameters!$1:$5067,7,FALSE)=1,\"√\",\"x\")","v":"√"},null,null,null,{"$f":"IF(VLOOKUP(\"FP667\",Parameters!$1:$5067,7,FALSE)=1,\"√\",\"x\")","v":"√"}]
[]
[null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,"As could be noticed in the biodiversity calculation sheet, the impacts of bio-energy production on biodiversity/carbon stocks are not easily measurable. The sustainability requirements in this tool are adopted from and restricted to those laid down in the Renewable Energy Directive. Reliable data on biodiversity are still scarce and possible impacts depend on many different factors. The results must therefore be seen as an indication and a more profound assessment of this topic is highly recommended."]
[]
[]
[]
[null,"Local Well-being - human and property rights"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Feedstock pathway 1 ",null,null,"Feedstock pathway 2",null,"Final conv."]
[null,null,null,null,null,null,null,null,null,null,null,null,"Cultivation",null,"Processing","Cultivation","Processing","Processing"]
[null,null,null,null,null,"There is no forced labour at the farm/factory",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP670a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080a\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"There is no child labour at the farm/factory",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP670b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080b\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"A self-declaration on good social practices regarding human rights has been communicated",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP670c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080c\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"There is no discrimination practiced that denies or impairs equality of opportunity, conditions or treatment",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP670d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080d\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"The producer can proof that the land is used legitimately and that traditional land rights have been secured",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170e\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,"√",{"$f":"IF(VLOOKUP(\"FP670e\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},"√","√"]
[null,null,null,null,null,"There is open and transparent communication with local communities and stakeholders",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC154f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP670f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC654f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC080f\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"The biomass production does not impair food security",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP170g\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,"√",{"$f":"IF(VLOOKUP(\"FP670g\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},"√","√"]
[]
[null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,"In many sustainability assessments, social criteria are omitted due to a lack of qualitative indicators and widespread accessible data. Moreover, socio-economic and cultural differences throughout the world complicate the use of a defined set of indicators and standards. Therefore, the approach adopted in this tool rather aims at giving the user an idea of which issues play an important role in the social dimension of the sustainability of bio-energy systems, than providing a straight forward answer. The reporting requirements on social issues in the RED and the development of certification systems such as RSPO, RSB and FSC among others can bring more clarity on these topics. The criteria in this tool on human and property rights are the same that can be found in these systems."]
[]
[]
[]
[]
[]
[null,"Local Well-being - working conditions"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"Feedstock pathway 1 ",null,null,"Feedstock pathway 2",null,"Final conv."]
[null,null,null,null,null,null,null,null,null,null,null,null,"Cultivation",null,"Processing","Cultivation","Processing","Processing"]
[null,null,null,null,null,"Employees are provided with fair legal contracts",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP671a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655a\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081a\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Workers are informed about their rights",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP671b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655b\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081b\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Workers have the freedom to join labour organizations or organize themselves",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP671c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655c\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081c\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"Payslips document the conformity of payment with at least legal regulations and/or collective agreements",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP671d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655d\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081d\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"The farm/factory has a written health, safety and hygiene policy and corresponding procedures",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171e\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,"√",{"$f":"IF(VLOOKUP(\"FP671e\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},"√","√"]
[null,null,null,null,null,"The farm/factory has a written risk assessment for safe and healthy working conditions",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,{"$f":"IF(VLOOKUP(\"BC155f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},{"$f":"IF(VLOOKUP(\"FP670f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"BC655f\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},{"$f":"IF(VLOOKUP(\"FC081f\",Parameters!$1:$5067,6,FALSE)=\"Fulfilled\",\"√\",\"x\")","v":"√"}]
[null,null,null,null,null,"All workers received adequate health and safety training and are instructed according to the risk assessment",null,null,null,null,null,null,{"$f":"IF(VLOOKUP(\"FP171g\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"x"},null,"√",{"$f":"IF(VLOOKUP(\"FP671g\",Parameters!$1:$5067,7,FALSE)=0,\"√\",\"x\")","v":"√"},"√","√"]
[]
[null,null,null,null,null,"Interpretation of results:"]
[null,null,null,null,null,"Same as explanation of human and property rights."]

{"sheet":"Parameters","index":13,"n_rows":1650,"n_cols":16,"rows_kept":1650,"cut":false,"hidden":true,"merged":[[17,12,17,13],[17,14,17,15],[17,7,17,10],[1,9,1,11],[2,9,2,11],[3,9,3,11],[4,9,4,11]]}
["ID-nr","Description","Manual Input","Auto Input","Monte Carlo Input","Final Input","Output"]
[{"$f":"'ID-numbers'!$A11","v":"LC001"},{"$f":"VLOOKUP(A2,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description transport 1 (mode 1-2-3)"},{"$f":"IF('Input Project'!H48=\"\",\"\",'Input Project'!H48)","v":""},{"$f":"VLOOKUP($A2,list_database1,$I$8,FALSE)","v":"Transport of FFB to the mill"},null,{"$f":"IF($C2=\"\",$D2,$C2)","v":"Transport of FFB to the mill"},null,"Selected feedstock pathway 1",1,{"$f":"INDEX(list_pathways_I,I2)","v":"Palm oil (stearin) from palm fruits, refinery"},null,null,"Energy balance",true]
[{"$f":"'ID-numbers'!$A12","v":"LC002"},{"$f":"VLOOKUP(A3,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description treatment 1"},{"$f":"IF('Input Project'!H43=\"\",\"\",'Input Project'!H43)","v":""},"No treatment",null,"No treatment",null,"Selected feedstock pathway 2",9,{"$f":"INDEX(list_pathways_II,I3)","v":"None"},null,null,"Global warming",true]
[{"$f":"'ID-numbers'!$A13","v":"LC003"},{"$f":"VLOOKUP(A4,'ID-numbers'!$1:$1048576,2,FALSE)","v":"BC_Process description conversion process 1"},{"$f":"IF('Input Project'!H60=\"\",\"\",'Input Project'!H60)","v":"Production of Crude Palm Oil (CPO)"},{"$f":"VLOOKUP($A4,list_database1,$I$8,FALSE)","v":"Production of Crude Palm Oil (CPO)"},null,"Production of Crude Palm Oil (CPO)",null,"Selected final conversion",4,{"$f":"INDEX(lijst_conversion,I4)","v":"No final conversion, only biofuel production"},null,null,"Resource use",true]
[{"$f":"'ID-numbers'!$A14","v":"LC004"},{"$f":"VLOOKUP(A5,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description transport 2 (mode 4-5-6)"},{"$f":"IF('Input Project'!H111=\"\",\"\",'Input Project'!H111)","v":""},"Transport of CPO to Belgium",null,"Transport of CPO to Belgium",null,"Selected functional unit",4,{"$f":"INDEX(list_functionalunit,I5)","v":"MJ diesel"},null,null,"Environmental quality",true]
[{"$f":"'ID-numbers'!$A15","v":"LC005"},{"$f":"VLOOKUP(A6,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description treatment 2"},{"$f":"IF('Input Project'!H106=\"\",\"\",'Input Project'!H106)","v":""},"No treatment",null,"No treatment",null,null,null,null,null,null,"Biodiversity",true]
[{"$f":"'ID-numbers'!$A16","v":"LC006"},{"$f":"VLOOKUP(A7,'ID-numbers'!$1:$1048576,2,FALSE)","v":"BC_Process description conversion process 2"},{"$f":"IF('Input Project'!H123=\"\",\"\",'Input Project'!H123)","v":"Refinery of Crude Palm Oil"},"Refinery of Crude Palm Oil",null,"Refinery of Crude Palm Oil",null,null,null,null,null,null,"Local well-being",true]
[{"$f":"'ID-numbers'!$A17","v":"LC007"},{"$f":"VLOOKUP(A8,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description transport 3 (mode 7-8-9)"},{"$f":"IF('Input Project'!H163=\"\",\"\",'Input Project'!H163)","v":""},"Transport of PS to the final conversion unit",null,"Transport of PS to the final conversion unit",null,"Column nr for 'Data' feedstock 1:",{"$f":"MATCH(J2,list_databasesystems,0)","v":6},{"$f":"I8-1","v":5}]
[{"$f":"'ID-numbers'!$A18","v":"LC008"},{"$f":"VLOOKUP(A9,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description treatment 3"},{"$f":"IF('Input Project'!H158=\"\",\"\",'Input Project'!H158)","v":""},"No treatment",null,"No treatment",null,"Column nr for 'Data' feedstock 2:",{"$f":"MATCH(J3,list_databasesystems,0)-1","v":30},{"$f":"I9-1","v":29}]
[{"$f":"'ID-numbers'!$A19","v":"LC501"},{"$f":"VLOOKUP(A10,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description transport 1 (mode 1-2-3)"},{"$f":"IF('Input Project'!H201=\"\",\"\",'Input Project'!H201)","v":""},{"$f":"VLOOKUP($A10,list_database2,$I$9,FALSE)","v":"n.a."},null,"n.a.",null,"Column nr for 'Data' final conversion:",{"$f":"MATCH(J4,list_databasesystems,0)","v":56},{"$f":"I10-1","v":55}]
[{"$f":"'ID-numbers'!$A20","v":"LC502"},{"$f":"VLOOKUP(A11,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description treatment 1"},{"$f":"IF('Input Project'!H196=\"\",\"\",'Input Project'!H196)","v":""},{"$f":"VLOOKUP($A11,list_database2,$I$9,FALSE)","v":"n.a."},null,"n.a."]
[{"$f":"'ID-numbers'!$A21","v":"LC503"},{"$f":"VLOOKUP(A12,'ID-numbers'!$1:$1048576,2,FALSE)","v":"BC_Process description conversion process 1"},{"$f":"IF('Input Project'!H213=\"\",\"\",'Input Project'!H213)","v":"n.a."},"n.a.",null,"n.a.",null,"Monte Carlo ",0]
[{"$f":"'ID-numbers'!$A22","v":"LC504"},{"$f":"VLOOKUP(A13,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description transport 2 (mode 4-5-6)"},{"$f":"IF('Input Project'!H264=\"\",\"\",'Input Project'!H264)","v":""},"n.a.",null,"n.a."]
[{"$f":"'ID-numbers'!$A23","v":"LC505"},{"$f":"VLOOKUP(A14,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description treatment 2"},{"$f":"IF('Input Project'!H259=\"\",\"\",'Input Project'!H259)","v":""},"n.a.",null,"n.a."]
[{"$f":"'ID-numbers'!$A24","v":"LC506"},{"$f":"VLOOKUP(A15,'ID-numbers'!$1:$1048576,2,FALSE)","v":"BC_Process description conversion process 2"},{"$f":"IF('Input Project'!H276=\"\",\"\",'Input Project'!H276)","v":"n.a."},"n.a.",null,"n.a."]
[{"$f":"'ID-numbers'!$A25","v":"LC507"},{"$f":"VLOOKUP(A16,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description transport 3 (mode 7-8-9)"},{"$f":"IF('Input Project'!H316=\"\",\"\",'Input Project'!H316)","v":""},"n.a.",null,"n.a."]
[{"$f":"'ID-numbers'!$A26","v":"LC508"},{"$f":"VLOOKUP(A17,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FT_Process description treatment 3"},{"$f":"IF('Input Project'!H311=\"\",\"\",'Input Project'!H311)","v":""},"n.a.",null,"n.a."]
[{"$f":"'ID-numbers'!$A27","v":"LC010"},{"$f":"VLOOKUP(A18,'ID-numbers'!$1:$1048576,2,FALSE)","v":"FC_Process description final conversion"},{"$f":"IF('Input Project'!H330=\"\",\"\",'Input Project'!H330)","v":"No final conversion"},{"$f":"VLOOKUP($A18,list_database1,$I$10,FALSE)","v":"No final conversion"},null,"No final conversion",null,"Uncertainty:",null,null,null,null,"Manual input",null,"Auto input"]
[null,null,null,null,null,null,null,"Mean","Min","Max","σ","Input parameter","Min","Max","Min","Max"]
[{"$f":"'ID-numbers'!$A30","v":"FP001"},{"$f":"VLOOKUP(A20,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Feedstock type 1"},null,{"$f":"VLOOKUP($A20,list_database1,$I$8,FALSE)","v":"Fresh palm fruit bunches (FFB)"},{"$f":"IF(MonteCarlo=1,IF($L20=1,IF($H20=\"n.a.\",0,IF($H20<0.009,0,MIN(MAX(NORMINV(RAND(),$H20,$K20),$I20),$J20))),\"\"),\"\")","v":""},{"$f":"IF($L20=1,IF(MonteCarlo=1,$E20,IF($C20=\"\",$D20,$C20)),IF($C20=\"\",$D20,$C20))","v":"Fresh palm fruit bunches (FFB)"},null,{"$f":"IF($L20=1,IF($C20=\"\",$D20,$C20),\"\")","v":""},{"$f":"IF($L20=1,IF($M20=\"\",$O20,$M20),\"\")","v":""},{"$f":"IF($L20=1,IF($N20=\"\",$P20,$N20),\"\")","v":""},{"$f":"IF($L20=1,($J20-$I20)/6,\"\")","v":""},0,null,null,{"$f":"IF($L20=1,VLOOKUP($A20,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L20=1,VLOOKUP($A20,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A31","v":"FP002"},{"$f":"VLOOKUP(A21,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Origin of the feedstock"},{"$f":"IF('Input RU'!K29=\"\",\"\",'Input RU'!K29)","v":""},{"$f":"VLOOKUP($A21,list_database1,$I$8,FALSE)","v":"Malaysia"},"",{"$f":"IF($L21=1,IF(MonteCarlo=1,$E21,IF($C21=\"\",$D21,$C21)),IF($C21=\"\",$D21,$C21))","v":"Malaysia"},null,"",{"$f":"IF($L21=1,IF($M21=\"\",$O21,$M21),\"\")","v":""},{"$f":"IF($L21=1,IF($N21=\"\",$P21,$N21),\"\")","v":""},{"$f":"IF($L21=1,($J21-$I21)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A32","v":"FP003a"},{"$f":"VLOOKUP(A22,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 1 per ha"},{"$f":"IF('Input Project'!H25=\"\",\"\",'Input Project'!H25)","v":""},{"$f":"VLOOKUP($A22,list_database1,$I$8,FALSE)","v":19000},"",{"$f":"IF($L22=1,IF(MonteCarlo=1,$E22,IF($C22=\"\",$D22,$C22)),IF($C22=\"\",$D22,$C22))","v":19000},null,19000,11450,21000,1591.6666666666667,1,{"$f":"IF(Uncertainty!W25=\"\",\"\",Uncertainty!W25)","v":""},{"$f":"IF(Uncertainty!Z25=\"\",\"\",Uncertainty!Z25)","v":""},11450,21000]
[{"$f":"'ID-numbers'!$A33","v":"FP003b"},{"$f":"VLOOKUP(A23,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of feedstock 1 per ha"},null,null,"",null,{"$f":"VLOOKUP(A23,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":12540},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A34","v":"FP003c"},{"$f":"VLOOKUP(A24,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of feedstock 1 per ha"},null,null,"",null,{"$f":"VLOOKUP(A24,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":300960},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A35","v":"FP005"},{"$f":"VLOOKUP(A25,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Number of harvests per year"},null,{"$f":"VLOOKUP($A25,list_database1,$I$8,FALSE)","v":1},"",{"$f":"IF($L25=1,IF(MonteCarlo=1,$E25,IF($C25=\"\",$D25,$C25)),IF($C25=\"\",$D25,$C25))","v":1},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A36","v":"FP006"},{"$f":"VLOOKUP(A26,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Rotation system"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A37","v":"FP009"},{"$f":"VLOOKUP(A27,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of the harvested crop"},{"$f":"IF('Input Project'!H26=\"\",\"\",'Input Project'!H26)","v":""},{"$f":"VLOOKUP($A27,list_database1,$I$8,FALSE)","v":34},"",{"$f":"IF($L27=1,IF(MonteCarlo=1,$E27,IF($C27=\"\",$D27,$C27)),IF($C27=\"\",$D27,$C27))","v":34},null,34,30,36,1,1,{"$f":"IF(Uncertainty!W26=\"\",\"\",Uncertainty!W26)","v":""},{"$f":"IF(Uncertainty!Z26=\"\",\"\",Uncertainty!Z26)","v":""},30,36]
[{"$f":"'ID-numbers'!$A38","v":"FP010"},{"$f":"VLOOKUP(A28,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of the dry energy crop (LHV)"},null,null,"",null,{"$f":"VLOOKUP(A28,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":24},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A39","v":"FP016a"},{"$f":"VLOOKUP(A29,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 1"},{"$f":"IF('Input Project'!H27=\"\",\"\",'Input Project'!H27)","v":""},{"$f":"VLOOKUP($A29,list_database1,$I$8,FALSE)","v":"n.a."},"",{"$f":"IF($L29=1,IF(MonteCarlo=1,$E29,IF($C29=\"\",$D29,$C29)),IF($C29=\"\",$D29,$C29))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A40","v":"FP016b"},{"$f":"VLOOKUP(A30,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 2"},{"$f":"IF('Input Project'!H30=\"\",\"\",'Input Project'!H30)","v":""},{"$f":"VLOOKUP($A30,list_database1,$I$8,FALSE)","v":"n.a."},"",{"$f":"IF($L30=1,IF(MonteCarlo=1,$E30,IF($C30=\"\",$D30,$C30)),IF($C30=\"\",$D30,$C30))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A41","v":"FP017a"},{"$f":"VLOOKUP(A31,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of by-product 1 per ha"},{"$f":"IF('Input Project'!H28=\"\",\"\",'Input Project'!H28)","v":""},{"$f":"VLOOKUP($A31,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L31=1,IF(MonteCarlo=1,$E31,IF($C31=\"\",$D31,$C31)),IF($C31=\"\",$D31,$C31))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W27=\"\",\"\",Uncertainty!W27)","v":""},{"$f":"IF(Uncertainty!Z27=\"\",\"\",Uncertainty!Z27)","v":""},0,0]
[{"$f":"'ID-numbers'!$A42","v":"FP017b"},{"$f":"VLOOKUP(A32,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of by-product 2 per ha"},{"$f":"IF('Input Project'!H31=\"\",\"\",'Input Project'!H31)","v":""},{"$f":"VLOOKUP($A32,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L32=1,IF(MonteCarlo=1,$E32,IF($C32=\"\",$D32,$C32)),IF($C32=\"\",$D32,$C32))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W29=\"\",\"\",Uncertainty!W29)","v":""},{"$f":"IF(Uncertainty!Z29=\"\",\"\",Uncertainty!Z29)","v":""},0,0]
[{"$f":"'ID-numbers'!$A43","v":"FP018a"},{"$f":"VLOOKUP(A33,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of by-product 1 per ha"},null,null,"",null,{"$f":"VLOOKUP(A33,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A44","v":"FP018b"},{"$f":"VLOOKUP(A34,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of by-product 2 per ha"},null,null,"",null,{"$f":"VLOOKUP(A34,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A45","v":"FP019a"},{"$f":"VLOOKUP(A35,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 1"},{"$f":"IF('Input Project'!H29=\"\",\"\",'Input Project'!H29)","v":""},{"$f":"VLOOKUP($A35,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L35=1,IF(MonteCarlo=1,$E35,IF($C35=\"\",$D35,$C35)),IF($C35=\"\",$D35,$C35))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W28=\"\",\"\",Uncertainty!W28)","v":""},{"$f":"IF(Uncertainty!Z28=\"\",\"\",Uncertainty!Z28)","v":""},0,0]
[{"$f":"'ID-numbers'!$A46","v":"FP019b"},{"$f":"VLOOKUP(A36,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 2"},{"$f":"IF('Input Project'!H32=\"\",\"\",'Input Project'!H32)","v":""},{"$f":"VLOOKUP($A36,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L36=1,IF(MonteCarlo=1,$E36,IF($C36=\"\",$D36,$C36)),IF($C36=\"\",$D36,$C36))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W30=\"\",\"\",Uncertainty!W30)","v":""},{"$f":"IF(Uncertainty!Z30=\"\",\"\",Uncertainty!Z30)","v":""},0,0]
[{"$f":"'ID-numbers'!$A47","v":"FP020a"},{"$f":"VLOOKUP(A37,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of the dry by-product 1 (LHV)"},null,null,"",null,{"$f":"VLOOKUP(A37,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A48","v":"FP020b"},{"$f":"VLOOKUP(A38,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of the dry by-product 2 (LHV)"},null,null,"",null,{"$f":"VLOOKUP(A38,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A49","v":"FP021a"},{"$f":"VLOOKUP(A39,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A50","v":"FP021b"},{"$f":"VLOOKUP(A40,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A51","v":"FP022"},{"$f":"VLOOKUP(A41,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of seeds"},{"$f":"IF('Input Project'!H33=\"\",\"\",'Input Project'!H33)","v":""},{"$f":"VLOOKUP($A41,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L41=1,IF(MonteCarlo=1,$E41,IF($C41=\"\",$D41,$C41)),IF($C41=\"\",$D41,$C41))","v":0},null,0,0,200,33.333333333333336,1,{"$f":"IF(Uncertainty!W31=\"\",\"\",Uncertainty!W31)","v":""},{"$f":"IF(Uncertainty!Z31=\"\",\"\",Uncertainty!Z31)","v":""},0,200]
[{"$f":"'ID-numbers'!$A52","v":"FP023a"},{"$f":"VLOOKUP(A42,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of N fertiliser (synthetic)"},{"$f":"IF('Input Project'!H34=\"\",\"\",'Input Project'!H34)","v":""},127.908,"",127.908,null,127.908,0,185,30.833333333333332,1,{"$f":"IF(Uncertainty!W32=\"\",\"\",Uncertainty!W32)","v":""},{"$f":"IF(Uncertainty!Z32=\"\",\"\",Uncertainty!Z32)","v":""},0,185]
[{"$f":"'ID-numbers'!$A53","v":"FP023b"},{"$f":"VLOOKUP(A43,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of P2O5 fertiliser"},{"$f":"IF('Input Project'!H35=\"\",\"\",'Input Project'!H35)","v":""},143.792,"",143.792,null,143.792,0,160,26.666666666666668,1,{"$f":"IF(Uncertainty!W33=\"\",\"\",Uncertainty!W33)","v":""},{"$f":"IF(Uncertainty!Z33=\"\",\"\",Uncertainty!Z33)","v":""},0,160]
[{"$f":"'ID-numbers'!$A54","v":"FP023c"},{"$f":"VLOOKUP(A44,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of K2O fertiliser"},{"$f":"IF('Input Project'!H36=\"\",\"\",'Input Project'!H36)","v":""},199.804,"",199.804,null,199.804,0,250,41.666666666666664,1,{"$f":"IF(Uncertainty!W34=\"\",\"\",Uncertainty!W34)","v":""},{"$f":"IF(Uncertainty!Z34=\"\",\"\",Uncertainty!Z34)","v":""},0,250]
[{"$f":"'ID-numbers'!$A55","v":"FP023d"},{"$f":"VLOOKUP(A45,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of CaO fertiliser"},{"$f":"IF('Input Project'!H37=\"\",\"\",'Input Project'!H37)","v":""},0,"",0,null,0,0,100,16.666666666666668,1,{"$f":"IF(Uncertainty!W35=\"\",\"\",Uncertainty!W35)","v":""},{"$f":"IF(Uncertainty!Z35=\"\",\"\",Uncertainty!Z35)","v":""},0,100]
[{"$f":"'ID-numbers'!$A56","v":"FP023e"},{"$f":"VLOOKUP(A46,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of pesticides"},{"$f":"IF('Input Project'!H38=\"\",\"\",'Input Project'!H38)","v":""},8.36,"",8.36,null,8.36,0,15,2.5,1,{"$f":"IF(Uncertainty!W36=\"\",\"\",Uncertainty!W36)","v":""},{"$f":"IF(Uncertainty!Z36=\"\",\"\",Uncertainty!Z36)","v":""},0,15]
[{"$f":"'ID-numbers'!$A57","v":"FP024a"},{"$f":"VLOOKUP(A47,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A47,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A58","v":"FP024b"},{"$f":"VLOOKUP(A48,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A48,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0.28755075519938561},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A59","v":"FP025a"},{"$f":"VLOOKUP(A49,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A49,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A60","v":"FP025b"},{"$f":"VLOOKUP(A50,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A50,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0.28755075519938561},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A63","v":"FP029a"},{"$f":"VLOOKUP(A51,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy used for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A51,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1.1985132664625198},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A65","v":"FP030"},{"$f":"VLOOKUP(A52,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to energy crop"},null,null,"",null,{"$f":"VLOOKUP(A52,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":100},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A66","v":"FP031"},{"$f":"VLOOKUP(A53,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-products"},null,null,"",null,{"$f":"VLOOKUP(A53,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A71","v":"FP034"},{"$f":"VLOOKUP(A54,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for agricultural machinery"},{"$f":"IF('Input Project'!H39=\"\",\"\",'Input Project'!H39)","v":""},{"$f":"VLOOKUP($A54,list_database1,$I$8,FALSE)","v":"Diesel"},"",{"$f":"IF($L54=1,IF(MonteCarlo=1,$E54,IF($C54=\"\",$D54,$C54)),IF($C54=\"\",$D54,$C54))","v":"Diesel"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A72","v":"FP035a"},{"$f":"VLOOKUP(A55,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to agrifuel use"},null,null,"",null,{"$f":"VLOOKUP(A55,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":2394.9083919999998},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A74","v":"FP036"},{"$f":"VLOOKUP(A56,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of fuel used in agricultural machinery"},null,null,"",null,{"$f":"VLOOKUP(A56,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":49.995999999999995},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A75","v":"FP037"},{"$f":"VLOOKUP(A57,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel used in agricultural machinery"},{"$f":"IF('Input Project'!H40=\"\",\"\",'Input Project'!H40)","v":""},{"$f":"VLOOKUP($A57,list_database1,$I$8,FALSE)","v":47.902000000000001},"",{"$f":"IF($L57=1,IF(MonteCarlo=1,$E57,IF($C57=\"\",$D57,$C57)),IF($C57=\"\",$D57,$C57))","v":47.902000000000001},null,47.902000000000001,40,75,5.833333333333333,1,{"$f":"IF(Uncertainty!W37=\"\",\"\",Uncertainty!W37)","v":""},{"$f":"IF(Uncertainty!Z37=\"\",\"\",Uncertainty!Z37)","v":""},40,75]
[{"$f":"'ID-numbers'!$A78","v":"FP039a"},{"$f":"VLOOKUP(A58,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy used for heat and electricity for drying and storage per MJ endfuel"},null,null,"",null,{"$f":"VLOOKUP(A58,'Production feedstock1'!$D$10:$G$659,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A80","v":"FP040"},{"$f":"VLOOKUP(A59,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat energy use for drying and storage of the crop"},{"$f":"IF('Input Project'!H45=\"\",\"\",'Input Project'!H45)","v":""},{"$f":"VLOOKUP($A59,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L59=1,IF(MonteCarlo=1,$E59,IF($C59=\"\",$D59,$C59)),IF($C59=\"\",$D59,$C59))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W49=\"\",\"\",Uncertainty!W49)","v":""},{"$f":"IF(Uncertainty!Z49=\"\",\"\",Uncertainty!Z49)","v":""},0,0]
[{"$f":"'ID-numbers'!$A81","v":"FP041"},{"$f":"VLOOKUP(A60,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat source"},{"$f":"IF('Input Project'!H44=\"\",\"\",'Input Project'!H44)","v":""},{"$f":"VLOOKUP($A60,list_database1,$I$8,FALSE)","v":"n.a."},"",{"$f":"IF($L60=1,IF(MonteCarlo=1,$E60,IF($C60=\"\",$D60,$C60)),IF($C60=\"\",$D60,$C60))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A82","v":"FP042a"},{"$f":"VLOOKUP(A61,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of heat production for crop drying and storage"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A87","v":"FP043"},{"$f":"VLOOKUP(A62,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity energy use for drying and storage of the crop"},{"$f":"IF('Input Project'!H47=\"\",\"\",'Input Project'!H47)","v":""},{"$f":"VLOOKUP($A62,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L62=1,IF(MonteCarlo=1,$E62,IF($C62=\"\",$D62,$C62)),IF($C62=\"\",$D62,$C62))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W50=\"\",\"\",Uncertainty!W50)","v":""},{"$f":"IF(Uncertainty!Z50=\"\",\"\",Uncertainty!Z50)","v":""},0,0]
[{"$f":"'ID-numbers'!$A88","v":"FP044"},{"$f":"VLOOKUP(A63,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity source"},{"$f":"IF('Input Project'!H46=\"\",\"\",'Input Project'!H46)","v":""},{"$f":"VLOOKUP($A63,list_database1,$I$8,FALSE)","v":"n.a."},"",{"$f":"IF($L63=1,IF(MonteCarlo=1,$E63,IF($C63=\"\",$D63,$C63)),IF($C63=\"\",$D63,$C63))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A89","v":"FP045a"},{"$f":"VLOOKUP(A64,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of electricity for crop drying and storage"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A94","v":"FP046a"},{"$f":"VLOOKUP(A65,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use of seeds, fertilisers and pesticides"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A96","v":"FP047"},{"$f":"VLOOKUP(A66,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Pretreated feedstock"},null,{"$f":"VLOOKUP($A66,list_database1,$I$8,FALSE)","v":"Fresh palm fruit bunches (FFB)"},null,{"$f":"IF($L66=1,IF(MonteCarlo=1,$E66,IF($C66=\"\",$D66,$C66)),IF($C66=\"\",$D66,$C66))","v":"Fresh palm fruit bunches (FFB)"}]
[{"$f":"'ID-numbers'!$A97","v":"FP048"},{"$f":"VLOOKUP(A67,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content pretreated feedstock"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A98","v":"FP049"},{"$f":"VLOOKUP(A68,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content pretreated feedstock (LHV)"},{"$f":"IF('Input Project'!H86=\"\",\"\",'Input Project'!H86)","v":""},{"$f":"VLOOKUP($A68,list_database1,$I$8,FALSE)","v":24},"",{"$f":"IF($L68=1,IF(MonteCarlo=1,$E68,IF($C68=\"\",$D68,$C68)),IF($C68=\"\",$D68,$C68))","v":24},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A99","v":"FP050a"},{"$f":"VLOOKUP(A69,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of N fertiliser"},null,null,"",null,{"$f":"VLOOKUP(A69,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":48.990600000000001},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A100","v":"FP050b"},{"$f":"VLOOKUP(A70,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of P fertiliser"},null,null,"",null,{"$f":"VLOOKUP(A70,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":15.2334},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A101","v":"FP050c"},{"$f":"VLOOKUP(A71,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of K fertiliser"},null,null,"",null,{"$f":"VLOOKUP(A71,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":9.67896},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A102","v":"FP050d"},{"$f":"VLOOKUP(A72,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of Ca fertiliser"},null,null,"",null,{"$f":"VLOOKUP(A72,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1.9735200000000002},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A103","v":"FP050e"},{"$f":"VLOOKUP(A73,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of pesticides"},null,null,"",null,{"$f":"VLOOKUP(A73,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":268.39980000000003},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A104","v":"FP050f"},{"$f":"VLOOKUP(A74,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of seeds"},null,null,"",null,{"$f":"VLOOKUP(A74,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A105","v":"FP051"},{"$f":"VLOOKUP(A75,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of pretreated feedstock 1 per ha"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A106","v":"FP052"},{"$f":"VLOOKUP(A76,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of pretreated feedstock 1 per ha"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A107","v":"FP053"},{"$f":"VLOOKUP(A77,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of pretreated feedstock 1 per ha"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A108","v":"FP054"},{"$f":"VLOOKUP(A78,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield loss through treatment and transport of feedstock 1"},null,{"$f":"VLOOKUP($A78,list_database1,$I$8,FALSE)","v":2},"",{"$f":"IF($L78=1,IF(MonteCarlo=1,$E78,IF($C78=\"\",$D78,$C78)),IF($C78=\"\",$D78,$C78))","v":2},null,2,0,5,0.83333333333333337,1,null,null,0,5]
[{"$f":"'ID-numbers'!$A109","v":"FP055a"},{"$f":"VLOOKUP(A79,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of pretreated feedstock 1 before conversion"},null,null,"",null,{"$f":"VLOOKUP(A79,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":18620},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A110","v":"FP055b"},{"$f":"VLOOKUP(A80,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of pretreated feedstock 1 before conversion"},null,null,"",null,{"$f":"VLOOKUP(A80,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":12289.2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A111","v":"FP055c"},{"$f":"VLOOKUP(A81,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of pretreated feedstock 1 before conversion"},null,null,"",null,{"$f":"VLOOKUP(A81,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":294940.79999999999},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A112","v":"FP056a"},{"$f":"VLOOKUP(A82,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with inputs for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A82,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":102.49380483244373},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A114","v":"FP057"},{"$f":"VLOOKUP(A83,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated GHG emissions from feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A83,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":46.709260201046042},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A115","v":"FP058"},{"$f":"VLOOKUP(A84,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with fuel used in agricultural machinery"},null,null,"",null,{"$f":"VLOOKUP(A84,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":180937.16419444449},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A116","v":"FP059"},{"$f":"VLOOKUP(A85,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions of the fuel used in agricultural machinery"},null,null,{"$f":"IF(MonteCarlo=1,IF($L85=1,IF($H85=\"n.a.\",0,IF($H85<0.009,0,MIN(MAX(NORMINV(RAND(),$H85,$K85),$I85),$J85))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A85,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":3777.2361111111118},{"$f":"IF($L85=1,IF($C85=\"\",$D85,$C85),\"\")","v":""},"","","",0,null,null,{"$f":"IF($L85=1,VLOOKUP($A85,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L85=1,VLOOKUP($A85,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A117","v":"FP061a"},{"$f":"VLOOKUP(A86,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A86,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":44.685763325221714},"",{"$f":"IF($L86=1,IF($M86=\"\",$O86,$M86),\"\")","v":""},{"$f":"IF($L86=1,IF($N86=\"\",$P86,$N86),\"\")","v":""},{"$f":"IF($L86=1,($J86-$I86)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A118","v":"FP061b"},{"$f":"VLOOKUP(A87,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A87,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":44.685763325221714},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A119","v":"FP062a"},{"$f":"VLOOKUP(A88,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with heat and electricity for drying and storage per kg"},null,null,"",null,{"$f":"VLOOKUP(A88,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A120","v":"FP062b"},{"$f":"VLOOKUP(A89,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with heat and electricity for drying and storage per MJ endfuel"},null,null,"",null,{"$f":"VLOOKUP(A89,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A121","v":"FP064"},{"$f":"VLOOKUP(A90,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with production of seeds, fertilisers and pesticides"},null,null,"",null,{"$f":"VLOOKUP(A90,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1104335.1484043999},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A122","v":"FP067a"},{"$f":"VLOOKUP(A91,'ID-numbers'!$1:$1048576,2,FALSE)","v":"N: specific GHG emissions"},null,null,"",null,{"$f":"VLOOKUP(A91,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":5880.5900999999994},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A123","v":"FP067b"},{"$f":"VLOOKUP(A92,'ID-numbers'!$1:$1048576,2,FALSE)","v":"P2O5: specific GHG emissions"},null,null,"",null,{"$f":"VLOOKUP(A92,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1010.7434999999999},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A124","v":"FP067c"},{"$f":"VLOOKUP(A93,'ID-numbers'!$1:$1048576,2,FALSE)","v":"K2O: specific GHG emissions"},null,null,"",null,{"$f":"VLOOKUP(A93,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":576.08240000000001},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A125","v":"FP067d"},{"$f":"VLOOKUP(A94,'ID-numbers'!$1:$1048576,2,FALSE)","v":"CaO: specific GHG emissions"},null,null,"",null,{"$f":"VLOOKUP(A94,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":129.49850000000001},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A126","v":"FP067e"},{"$f":"VLOOKUP(A95,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Pesticides: specific GHG emissions"},null,null,"",null,{"$f":"VLOOKUP(A95,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":10971.3197},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A127","v":"FP067f"},{"$f":"VLOOKUP(A96,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Seeds: specific GHG emissions"},null,null,"",null,{"$f":"VLOOKUP(A96,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A128","v":"FP068a"},{"$f":"VLOOKUP(A97,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with land use change (carbon stock changes) per MJ"},null,null,"",null,{"$f":"VLOOKUP(A97,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A129","v":"FP068b"},{"$f":"VLOOKUP(A98,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with land use change (carbon stock changes) per ha"},null,null,"",null,{"$f":"VLOOKUP(A98,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A130","v":"FP069a"},{"$f":"VLOOKUP(A99,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Actual land use"},null,{"$f":"VLOOKUP($A99,list_database1,$I$8,FALSE)","v":"Perennial cropland"},"",{"$f":"IF($L99=1,IF(MonteCarlo=1,$E99,IF($C99=\"\",$D99,$C99)),IF($C99=\"\",$D99,$C99))","v":"Perennial cropland"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A131","v":"FP069b"},{"$f":"VLOOKUP(A100,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Previous land use (January 1st, 2008)"},null,"Perennial cropland","","Perennial cropland",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A132","v":"FP069c"},{"$f":"VLOOKUP(A101,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Actual land use_specific for carbon stock veg"},null,"Oil palm","","Oil palm",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A133","v":"FP069d"},{"$f":"VLOOKUP(A102,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Previous land use (January 1st, 2008)_specific for carbon stock veg"},null,"Oil palm","","Oil palm",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A134","v":"FP070a"},{"$f":"VLOOKUP(A103,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Climate region"},{"$f":"IF('Input Land use'!K26=\"\",\"\",'Input Land use'!K26)","v":""},"Tropical Wet","","Tropical Wet",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A135","v":"FP070b"},{"$f":"VLOOKUP(A104,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Soil type"},{"$f":"IF('Input Land use'!K27=\"\",\"\",'Input Land use'!K27)","v":""},"Low activity clay soils","","Low activity clay soils",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A136","v":"FP070c"},{"$f":"VLOOKUP(A105,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Climate region_specific for carbon stock_actual land use"},null,"Tropical wet","","Tropical wet",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A137","v":"FP070d"},{"$f":"VLOOKUP(A106,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Climate region_specific for carbon stock_previous land use"},null,"Tropical wet","","Tropical wet",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A138","v":"FP071"},{"$f":"VLOOKUP(A107,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A139","v":"FP072"},{"$f":"VLOOKUP(A108,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A140","v":"FP073a"},{"$f":"VLOOKUP(A109,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Soil organic carbon actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A141","v":"FP073b"},{"$f":"VLOOKUP(A110,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Soil organic carbon previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A142","v":"FP074"},{"$f":"VLOOKUP(A111,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard soil organic carbon_feedstock 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A143","v":"FP075a"},{"$f":"VLOOKUP(A112,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use factor actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A144","v":"FP075b"},{"$f":"VLOOKUP(A113,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use factor previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A145","v":"FP076a"},{"$f":"VLOOKUP(A114,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Management factor actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A146","v":"FP076b"},{"$f":"VLOOKUP(A115,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Management factor previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A147","v":"FP077a"},{"$f":"VLOOKUP(A116,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input factor actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A148","v":"FP077b"},{"$f":"VLOOKUP(A117,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input factor previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A149","v":"FP078a"},{"$f":"VLOOKUP(A118,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A150","v":"FP078b"},{"$f":"VLOOKUP(A119,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A151","v":"FP079a"},{"$f":"VLOOKUP(A120,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock in living biomass actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A152","v":"FP079b"},{"$f":"VLOOKUP(A121,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock in living biomass previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A153","v":"FP080a"},{"$f":"VLOOKUP(A122,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above ground vegetation carbon stock in living biomass actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A154","v":"FP080b"},{"$f":"VLOOKUP(A123,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above ground vegetation carbon stock in living biomass previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A155","v":"FP081a"},{"$f":"VLOOKUP(A124,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of above ground living biomass actual land use"},{"$f":"IF('Input Land use'!K99=\"\",\"\",'Input Land use'!K99)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A156","v":"FP081b"},{"$f":"VLOOKUP(A125,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of above ground living biomass previous land use"},{"$f":"IF('Input Land use'!K109=\"\",\"\",'Input Land use'!K109)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A157","v":"FP082aa"},{"$f":"VLOOKUP(A126,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in living biomass actual land use"},{"$f":"IF('Input Land use'!K102=\"\",\"\",'Input Land use'!K102)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A158","v":"FP082ab"},{"$f":"VLOOKUP(A127,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in living biomass previous land use"},{"$f":"IF('Input Land use'!K112=\"\",\"\",'Input Land use'!K112)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A159","v":"FP082ba"},{"$f":"VLOOKUP(A128,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in dead wood actual land use"},{"$f":"IF('Input Land use'!K103=\"\",\"\",'Input Land use'!K103)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A160","v":"FP082bb"},{"$f":"VLOOKUP(A129,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in dead wood previous land use"},{"$f":"IF('Input Land use'!K113=\"\",\"\",'Input Land use'!K113)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A161","v":"FP082ca"},{"$f":"VLOOKUP(A130,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in litter actual land use"},{"$f":"IF('Input Land use'!K104=\"\",\"\",'Input Land use'!K104)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A162","v":"FP082cb"},{"$f":"VLOOKUP(A131,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in litter previous land use"},{"$f":"IF('Input Land use'!K114=\"\",\"\",'Input Land use'!K114)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A163","v":"FP083a"},{"$f":"VLOOKUP(A132,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below ground carbon stock to above ground carbon stock in living biomass actual land use"},{"$f":"IF('Input Land use'!K97=\"\",\"\",'Input Land use'!K97)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A164","v":"FP083b"},{"$f":"VLOOKUP(A133,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below ground carbon stock to above ground carbon stock in living biomass previous land use"},{"$f":"IF('Input Land use'!K107=\"\",\"\",'Input Land use'!K107)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A165","v":"FP084a"},{"$f":"VLOOKUP(A134,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Below ground vegetation carbon stock in living biomass actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A166","v":"FP084b"},{"$f":"VLOOKUP(A135,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Below ground vegetation carbon stock in living biomass previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A167","v":"FP085a"},{"$f":"VLOOKUP(A136,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of below ground living biomass actual land use"},{"$f":"IF('Input Land use'!K96=\"\",\"\",'Input Land use'!K96)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A168","v":"FP085b"},{"$f":"VLOOKUP(A137,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of below ground living biomass previous land use"},{"$f":"IF('Input Land use'!K106=\"\",\"\",'Input Land use'!K106)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A169","v":"FP086a"},{"$f":"VLOOKUP(A138,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock in dead organic matter actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A170","v":"FP086b"},{"$f":"VLOOKUP(A139,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock in dead organic matter previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A171","v":"FP087a"},{"$f":"VLOOKUP(A140,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock in dead wood pool actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A172","v":"FP087b"},{"$f":"VLOOKUP(A141,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock in dead wood pool previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A173","v":"FP088a"},{"$f":"VLOOKUP(A142,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of dead wood pool actual land use"},{"$f":"IF('Input Land use'!K100=\"\",\"\",'Input Land use'!K100)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A174","v":"FP088b"},{"$f":"VLOOKUP(A143,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of dead wood pool previous land use"},{"$f":"IF('Input Land use'!K110=\"\",\"\",'Input Land use'!K110)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A175","v":"FP089a"},{"$f":"VLOOKUP(A144,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock in litter actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A176","v":"FP089b"},{"$f":"VLOOKUP(A145,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock in litter previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A177","v":"FP090a"},{"$f":"VLOOKUP(A146,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of litter actual land use"},{"$f":"IF('Input Land use'!K101=\"\",\"\",'Input Land use'!K101)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A178","v":"FP090b"},{"$f":"VLOOKUP(A147,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of litter previous land use"},{"$f":"IF('Input Land use'!K111=\"\",\"\",'Input Land use'!K111)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A179","v":"FP091a"},{"$f":"VLOOKUP(A148,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Peatland"},null,{"$f":"VLOOKUP($A148,list_database1,$I$8,FALSE)","v":{"$error":"#N/A"}},"",{"$f":"IF($L148=1,IF(MonteCarlo=1,$E148,IF($C148=\"\",$D148,$C148)),IF($C148=\"\",$D148,$C148))","v":{"$error":"#N/A"}},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A180","v":"FP091b"},{"$f":"VLOOKUP(A149,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Emission factor soil organic carbon_peatland"},null,null,{"$f":"IF(MonteCarlo=1,IF($L149=1,IF($H149=\"n.a.\",0,IF($H149<0.009,0,MIN(MAX(NORMINV(RAND(),$H149,$K149),$I149),$J149))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A149,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":20},{"$f":"IF($L149=1,IF($C149=\"\",$D149,$C149),\"\")","v":""},"","","",0,null,null,{"$f":"IF($L149=1,VLOOKUP($A149,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L149=1,VLOOKUP($A149,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A181","v":"FP092a"},{"$f":"VLOOKUP(A150,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Previously degraded land"},null,{"$f":"VLOOKUP($A150,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L150=1,IF(MonteCarlo=1,$E150,IF($C150=\"\",$D150,$C150)),IF($C150=\"\",$D150,$C150))","v":0},null,"",{"$f":"IF($L150=1,IF($M150=\"\",$O150,$M150),\"\")","v":""},{"$f":"IF($L150=1,IF($N150=\"\",$P150,$N150),\"\")","v":""},{"$f":"IF($L150=1,($J150-$I150)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A182","v":"FP092b"},{"$f":"VLOOKUP(A151,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Bonus restored degraded land"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A183","v":"FP093a"},{"$f":"VLOOKUP(A152,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land management actual land use"},null,{"$f":"VLOOKUP($A152,list_database1,$I$8,FALSE)","v":"No till"},"",{"$f":"IF($L152=1,IF(MonteCarlo=1,$E152,IF($C152=\"\",$D152,$C152)),IF($C152=\"\",$D152,$C152))","v":"No till"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A184","v":"FP093b"},{"$f":"VLOOKUP(A153,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land management previous land use"},null,"No till","","No till",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A185","v":"FP094a"},{"$f":"VLOOKUP(A154,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input actual land use"},"","High without manure","","High without manure",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A186","v":"FP094b"},{"$f":"VLOOKUP(A155,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input previous land use"},null,"High without manure","","High without manure",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A187","v":"FP095a"},{"$f":"VLOOKUP(A156,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Domain actual land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A188","v":"FP095b"},{"$f":"VLOOKUP(A157,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Domain previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A189","v":"FP096a"},{"$f":"VLOOKUP(A158,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ecological zone actual land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A190","v":"FP096b"},{"$f":"VLOOKUP(A159,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ecological zone previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A191","v":"FP097a"},{"$f":"VLOOKUP(A160,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Continent actual land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A192","v":"FP097b"},{"$f":"VLOOKUP(A161,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Continent previous land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A193","v":"FP098a"},{"$f":"VLOOKUP(A162,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type actual land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A194","v":"FP098b"},{"$f":"VLOOKUP(A163,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type previous land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A195","v":"FP099"},{"$f":"VLOOKUP(A164,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with indirect land use change (soil carbon release)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A196","v":"FP100"},{"$f":"VLOOKUP(A165,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock production"},{"$f":"IF('Input RU'!K30=\"\",\"\",'Input RU'!K30)","v":""},22067.5,"",{"$f":"IF($L165=1,IF(MonteCarlo=1,$E165,IF($C165=\"\",$D165,$C165)),IF($C165=\"\",$D165,$C165))","v":22067.5},null,22067.5,6858.8,37276.25,5069.5749999999998,1,{"$f":"IF(Uncertainty!W38=\"\",\"\",Uncertainty!W38)","v":""},{"$f":"IF(Uncertainty!Z38=\"\",\"\",Uncertainty!Z38)","v":""},6858.8,37276.25]
[{"$f":"'ID-numbers'!$A197","v":"FP101"},{"$f":"VLOOKUP(A166,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated water use for feedstock production"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A198","v":"FP102a"},{"$f":"VLOOKUP(A167,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A167,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":422.20878511090552},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A199","v":"FP102b"},{"$f":"VLOOKUP(A168,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A168,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":422.20878511090552},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A200","v":"FP103a"},{"$f":"VLOOKUP(A169,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},{"$f":"IF('Input RU'!K33=\"\",\"\",'Input RU'!K33)","v":""},{"$f":"VLOOKUP($A169,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L169=1,IF(MonteCarlo=1,$E169,IF($C169=\"\",$D169,$C169)),IF($C169=\"\",$D169,$C169))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W51=\"\",\"\",Uncertainty!W51)","v":""},{"$f":"IF(Uncertainty!Z51=\"\",\"\",Uncertainty!Z51)","v":""},0,0]
[{"$f":"'ID-numbers'!$A201","v":"FP103b"},{"$f":"VLOOKUP(A170,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A202","v":"FP104a"},{"$f":"VLOOKUP(A171,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Country freshwater availability"},null,null,null,null,{"$f":"VLOOKUP(A171,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":23320}]
[{"$f":"'ID-numbers'!$A203","v":"FP104b"},{"$f":"VLOOKUP(A172,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Country freshwater level"},null,null,null,null,{"$f":"VLOOKUP(A172,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":"high"}]
[{"$f":"'ID-numbers'!$A205","v":"FP106a"},{"$f":"VLOOKUP(A173,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated land use for feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A173,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1.9132606099961733E-2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A206","v":"FP106b"},{"$f":"VLOOKUP(A174,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated land use for feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A174,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1.9132606099961733E-2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A207","v":"FP107a"},{"$f":"VLOOKUP(A175,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon debt due to land use change"},null,null,null,null,{"$f":"VLOOKUP(A175,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A211","v":"FP109"},{"$f":"VLOOKUP(A176,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input of N-fixing crop residue to the soil"},{"$f":"IF('Input Land use'!K85=\"\",\"\",'Input Land use'!K85)","v":""},{"$f":"VLOOKUP($A176,list_database1,$I$8,FALSE)","v":45},"",{"$f":"IF($L176=1,IF(MonteCarlo=1,$E176,IF($C176=\"\",$D176,$C176)),IF($C176=\"\",$D176,$C176))","v":45},null,45,0,45,7.5,1,{"$f":"IF(Uncertainty!W43=\"\",\"\",Uncertainty!W43)","v":""},{"$f":"IF(Uncertainty!Z43=\"\",\"\",Uncertainty!Z43)","v":""},0,45]
[{"$f":"'ID-numbers'!$A220","v":"FP115a"},{"$f":"VLOOKUP(A177,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A177,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0.78450695493120459},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A221","v":"FP115b"},{"$f":"VLOOKUP(A178,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A178,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0.78450695493120459},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A238","v":"FP125a"},{"$f":"VLOOKUP(A179,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A179,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1.9914646988440075},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A239","v":"FP125b"},{"$f":"VLOOKUP(A180,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A180,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1.9914646988440075},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A242","v":"FP130a"},{"$f":"VLOOKUP(A181,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total (direct + indirect) N2O emissions from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A243","v":"FP130b"},{"$f":"VLOOKUP(A182,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total (direct + indirect) N2O emissions from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A244","v":"FP131"},{"$f":"VLOOKUP(A183,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Soil water saturation (yes=1,no=0)"},{"$f":"IF('Input Land use'!K50=\"yes\",\"1\",IF('Input Land use'!K50=\"no\",\"0\",\"\"))","v":""},1,"",{"$f":"IF($L183=1,IF(MonteCarlo=1,$E183,IF($C183=\"\",$D183,$C183)),IF($C183=\"\",$D183,$C183))","v":1},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A245","v":"FP132"},{"$f":"VLOOKUP(A184,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Field renewal (annual crops = 1)"},{"$f":"IF('Input Land use'!K78=\"\",\"\",'Input Land use'!K78)","v":""},1,"",{"$f":"IF($L184=1,IF(MonteCarlo=1,$E184,IF($C184=\"\",$D184,$C184)),IF($C184=\"\",$D184,$C184))","v":1},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A246","v":"FP133"},{"$f":"VLOOKUP(A185,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of crop residue returned to the field (only for palm)"},{"$f":"IF('Input Land use'!K93=\"\",\"\",'Input Land use'!K93)","v":""},0.22,"",{"$f":"IF($L185=1,IF(MonteCarlo=1,$E185,IF($C185=\"\",$D185,$C185)),IF($C185=\"\",$D185,$C185))","v":0.22},null,0.22,0,0.5,8.3333333333333329E-2,1,{"$f":"IF(Uncertainty!W45=\"\",\"\",Uncertainty!W45)","v":""},{"$f":"IF(Uncertainty!Z45=\"\",\"\",Uncertainty!Z45)","v":""},0,0.5]
[{"$f":"'ID-numbers'!$A247","v":"FP134"},{"$f":"VLOOKUP(A186,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Organic soil (yes=1,no=0)"},{"$f":"IF('Input Land use'!K49=\"yes\",\"1\",IF('Input Land use'!K49=\"no\",\"0\",\"\"))","v":""},0,"",{"$f":"IF($L186=1,IF(MonteCarlo=1,$E186,IF($C186=\"\",$D186,$C186)),IF($C186=\"\",$D186,$C186))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A248","v":"FP135"},{"$f":"VLOOKUP(A187,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Nutrient level (only for ORGANIC soils + temperate/boreal climate + forest (native and managed))"},{"$f":"IF('Input Land use'!K53=\"\",\"\",'Input Land use'!K53)","v":""},"n.a.","",{"$f":"IF($L187=1,IF(MonteCarlo=1,$E187,IF($C187=\"\",$D187,$C187)),IF($C187=\"\",$D187,$C187))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A257","v":"FP140"},{"$f":"VLOOKUP(A188,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total amount of organic N fertiliser applied to soil (other than by grazing animals)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A258","v":"FP141a"},{"$f":"VLOOKUP(A189,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of animal manure N applied to soil (other than by grazing animals)"},{"$f":"IF('Input Land use'!K79=\"\",\"\",'Input Land use'!K79)","v":""},{"$f":"VLOOKUP($A189,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L189=1,IF(MonteCarlo=1,$E189,IF($C189=\"\",$D189,$C189)),IF($C189=\"\",$D189,$C189))","v":0},null,0,0,185,30.833333333333332,1,{"$f":"IF(Uncertainty!W39=\"\",\"\",Uncertainty!W39)","v":""},{"$f":"IF(Uncertainty!Z39=\"\",\"\",Uncertainty!Z39)","v":""},0,185]
[{"$f":"'ID-numbers'!$A259","v":"FP141b"},{"$f":"VLOOKUP(A190,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of total sewage N applied to soil"},{"$f":"IF('Input Land use'!K81=\"\",\"\",'Input Land use'!K81)","v":""},{"$f":"VLOOKUP($A190,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L190=1,IF(MonteCarlo=1,$E190,IF($C190=\"\",$D190,$C190)),IF($C190=\"\",$D190,$C190))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W40=\"\",\"\",Uncertainty!W40)","v":""},{"$f":"IF(Uncertainty!Z40=\"\",\"\",Uncertainty!Z40)","v":""},0,0]
[{"$f":"'ID-numbers'!$A260","v":"FP141c"},{"$f":"VLOOKUP(A191,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of total compost N applied to soil"},{"$f":"IF('Input Land use'!K82=\"\",\"\",'Input Land use'!K82)","v":""},{"$f":"VLOOKUP($A191,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L191=1,IF(MonteCarlo=1,$E191,IF($C191=\"\",$D191,$C191)),IF($C191=\"\",$D191,$C191))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W41=\"\",\"\",Uncertainty!W41)","v":""},{"$f":"IF(Uncertainty!Z41=\"\",\"\",Uncertainty!Z41)","v":""},0,0]
[{"$f":"'ID-numbers'!$A261","v":"FP141d"},{"$f":"VLOOKUP(A192,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of N of other organic amendments applied to soil (used as fertiliser)"},{"$f":"IF('Input Land use'!K83=\"\",\"\",'Input Land use'!K83)","v":""},{"$f":"VLOOKUP($A192,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L192=1,IF(MonteCarlo=1,$E192,IF($C192=\"\",$D192,$C192)),IF($C192=\"\",$D192,$C192))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W42=\"\",\"\",Uncertainty!W42)","v":""},{"$f":"IF(Uncertainty!Z42=\"\",\"\",Uncertainty!Z42)","v":""},0,0]
[{"$f":"'ID-numbers'!$A262","v":"FP142"},{"$f":"VLOOKUP(A193,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total amount of N in crop residues (including N-fixing crops and renewal) returned to soil"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A263","v":"FP143a"},{"$f":"VLOOKUP(A194,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of above-ground residues to harvested yield_calculated"},null,null,"",null,{"$f":"VLOOKUP(A194,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0.33333333333333331},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A264","v":"FP143b"},{"$f":"VLOOKUP(A195,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of above-ground residues to harvested yield_final"},{"$f":"IF('Input Land use'!K88=\"\",\"\",'Input Land use'!K88)","v":""},{"$f":"G194","v":0.33333333333333331},"",{"$f":"IF($L195=1,IF(MonteCarlo=1,$E195,IF($C195=\"\",$D195,$C195)),IF($C195=\"\",$D195,$C195))","v":0.33333333333333331},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A265","v":"FP144"},{"$f":"VLOOKUP(A196,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above-ground residue (dry) (=AGDM(T))"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A266","v":"FP145a"},{"$f":"VLOOKUP(A197,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Slope to calculate above-ground residue"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A267","v":"FP145b"},{"$f":"VLOOKUP(A198,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Intercept to calculate above-ground residue"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A268","v":"FP146a"},{"$f":"VLOOKUP(A199,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below-ground residues to harvested yield_calculated"},null,null,"",null,{"$f":"VLOOKUP(A199,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A269","v":"FP146b"},{"$f":"VLOOKUP(A200,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below-ground residues to harvested yield_final"},{"$f":"IF('Input Land use'!K90=\"\",\"\",'Input Land use'!K90)","v":""},{"$f":"G199","v":0},"",{"$f":"IF($L200=1,IF(MonteCarlo=1,$E200,IF($C200=\"\",$D200,$C200)),IF($C200=\"\",$D200,$C200))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A270","v":"FP147"},{"$f":"VLOOKUP(A201,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below-ground residues to above-ground biomass"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A271","v":"FP148a"},{"$f":"VLOOKUP(A202,'ID-numbers'!$1:$1048576,2,FALSE)","v":"N content of above-ground residues"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A272","v":"FP148b"},{"$f":"VLOOKUP(A203,'ID-numbers'!$1:$1048576,2,FALSE)","v":"N content of below-ground residues"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A273","v":"FP149"},{"$f":"VLOOKUP(A204,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fraction of above-ground residues removed"},{"$f":"IF('Input Land use'!K87=\"\",\"\",'Input Land use'!K87)","v":""},{"$f":"VLOOKUP($A204,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L204=1,IF(MonteCarlo=1,$E204,IF($C204=\"\",$D204,$C204)),IF($C204=\"\",$D204,$C204))","v":0},null,0,0,5,0.83333333333333337,1,{"$f":"IF(Uncertainty!W44=\"\",\"\",Uncertainty!W44)","v":""},{"$f":"IF(Uncertainty!Z44=\"\",\"\",Uncertainty!Z44)","v":""},0,5]
[{"$f":"'ID-numbers'!$A274","v":"FP150"},{"$f":"VLOOKUP(A205,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total amount of N mineralised in mineral soil due to carbon loss through land use change"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A275","v":"FP151"},{"$f":"VLOOKUP(A206,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Average annual loss of soil carbon"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A276","v":"FP152"},{"$f":"VLOOKUP(A207,'ID-numbers'!$1:$1048576,2,FALSE)","v":"C:N ratio of the soil organic matter"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A277","v":"FP153"},{"$f":"VLOOKUP(A208,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Previous land use is cropland (yes=1,no=0)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A278","v":"FP154"},{"$f":"VLOOKUP(A209,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Direct N2O_N emissions from managed organic soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A279","v":"FP155a"},{"$f":"VLOOKUP(A210,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Indirect N2O_N emissions from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A280","v":"FP155b"},{"$f":"VLOOKUP(A211,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Indirect N2O emissions from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A281","v":"FP156"},{"$f":"VLOOKUP(A212,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Indirect N2O_N emissions from atmospheric deposition of N volatilized from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A282","v":"FP157"},{"$f":"VLOOKUP(A213,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fraction of synthetic fertiliser N that volatilises as NH3 and NOx"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A283","v":"FP158"},{"$f":"VLOOKUP(A214,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fraction of organic fertiliser N that volatilises as NH3 and NOx"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A284","v":"FP159"},{"$f":"VLOOKUP(A215,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Indirect N2O_N emissions from N leaching/runoff from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A285","v":"FP160"},{"$f":"VLOOKUP(A216,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fraction of all N added to managed soils that is lost through leaching and runoff"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A286","v":"FP161"},{"$f":"VLOOKUP(A217,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in or after January 2008 = undisturbed forest (yes=1,no=0)"},{"$f":"IF('Input Bio'!K28=\"yes\",1,IF('Input Bio'!K28=\"no\",0,\"\"))","v":""},{"$f":"VLOOKUP($A217,list_database1,$I$8,FALSE)","v":1},"",{"$f":"IF($L217=1,IF(MonteCarlo=1,$E217,IF($C217=\"\",$D217,$C217)),IF($C217=\"\",$D217,$C217))","v":1},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A287","v":"FP162"},{"$f":"VLOOKUP(A218,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in or after January 2008 = nature protection area"},{"$f":"IF('Input Bio'!K29=\"yes\",1,IF('Input Bio'!K29=\"no\",0,\"\"))","v":""},1,"",{"$f":"IF($L218=1,IF(MonteCarlo=1,$E218,IF($C218=\"\",$D218,$C218)),IF($C218=\"\",$D218,$C218))","v":1},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A288","v":"FP163"},{"$f":"VLOOKUP(A219,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in or after January 2008 = highly biodiverse grassland"},{"$f":"IF('Input Bio'!K30=\"yes\",1,IF('Input Bio'!K30=\"no\",0,\"\"))","v":""},0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A289","v":"FP164"},{"$f":"VLOOKUP(A220,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in January 2008 and not longer now = wetland"},{"$f":"IF('Input Bio'!K59=\"yes\",1,IF('Input Bio'!K59=\"no\",0,\"\"))","v":""},0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A290","v":"FP165"},{"$f":"VLOOKUP(A221,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in January 2008 and not longer now = continuously forested area"},{"$f":"IF('Input Bio'!K60=\"yes\",1,IF('Input Bio'!K60=\"no\",0,\"\"))","v":""},1,"",1,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A291","v":"FP166"},{"$f":"VLOOKUP(A222,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in January 2008 and not longer now = peatland"},{"$f":"IF('Input Bio'!K61=\"yes\",1,IF('Input Bio'!K61=\"no\",0,\"\"))","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L222=1,IF($H222=\"n.a.\",0,IF($H222<0.009,0,MIN(MAX(NORMINV(RAND(),$H222,$K222),$I222),$J222))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L222=1,IF($C222=\"\",$D222,$C222),\"\")","v":""},"","","",0,null,null,{"$f":"IF($L222=1,VLOOKUP($A222,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L222=1,VLOOKUP($A222,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A292","v":"FP167"},{"$f":"VLOOKUP(A223,'ID-numbers'!$1:$1048576,2,FALSE)","v":"The requirements of the RED concerning biodiversity & high carbon stocks are met"},null,null,"",null,{"$f":"VLOOKUP(A223,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"",{"$f":"IF($L223=1,IF($M223=\"\",$O223,$M223),\"\")","v":""},{"$f":"IF($L223=1,IF($N223=\"\",$P223,$N223),\"\")","v":""},{"$f":"IF($L223=1,($J223-$I223)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A293","v":"FP170a"},{"$f":"VLOOKUP(A224,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour"},{"$f":"IF('Input LW'!U32=\"\",\"\",'Input LW'!U32)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A224,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A294","v":"FP170b"},{"$f":"VLOOKUP(A225,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour "},{"$f":"IF('Input LW'!U33=\"\",\"\",'Input LW'!U33)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A225,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A295","v":"FP170c"},{"$f":"VLOOKUP(A226,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights"},{"$f":"IF('Input LW'!U34=\"\",\"\",'Input LW'!U34)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A226,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A296","v":"FP170d"},{"$f":"VLOOKUP(A227,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination"},{"$f":"IF('Input LW'!U35=\"\",\"\",'Input LW'!U35)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A227,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A297","v":"FP170e"},{"$f":"VLOOKUP(A228,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured"},{"$f":"IF('Input LW'!U36=\"\",\"\",'Input LW'!U36)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A228,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A298","v":"FP170f"},{"$f":"VLOOKUP(A229,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders"},{"$f":"IF('Input LW'!U37=\"\",\"\",'Input LW'!U37)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A229,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A299","v":"FP170g"},{"$f":"VLOOKUP(A230,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security"},{"$f":"IF('Input LW'!U38=\"\",\"\",'Input LW'!U38)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A230,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A300","v":"FP171a"},{"$f":"VLOOKUP(A231,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts"},{"$f":"IF('Input LW'!U40=\"\",\"\",'Input LW'!U40)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A231,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A301","v":"FP171b"},{"$f":"VLOOKUP(A232,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights"},{"$f":"IF('Input LW'!U41=\"\",\"\",'Input LW'!U41)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A232,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A302","v":"FP171c"},{"$f":"VLOOKUP(A233,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves"},{"$f":"IF('Input LW'!U42=\"\",\"\",'Input LW'!U42)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A233,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A303","v":"FP171d"},{"$f":"VLOOKUP(A234,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules"},{"$f":"IF('Input LW'!U43=\"\",\"\",'Input LW'!U43)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A234,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A304","v":"FP171e"},{"$f":"VLOOKUP(A235,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy"},{"$f":"IF('Input LW'!U44=\"\",\"\",'Input LW'!U44)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A235,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A305","v":"FP171f"},{"$f":"VLOOKUP(A236,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions"},{"$f":"IF('Input LW'!U45=\"\",\"\",'Input LW'!U45)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A236,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A306","v":"FP171g"},{"$f":"VLOOKUP(A237,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training"},{"$f":"IF('Input LW'!U46=\"\",\"\",'Input LW'!U46)","v":""},"Not fulfilled","","Not fulfilled",{"$f":"VLOOKUP(A237,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A307","v":"FP172"},{"$f":"VLOOKUP(A238,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights_score"},null,null,"",null,{"$f":"VLOOKUP(A238,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":7},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A308","v":"FP173"},{"$f":"VLOOKUP(A239,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions_score"},null,null,"",null,{"$f":"VLOOKUP(A239,'Production feedstock1'!$D$9:$G$5037,4,FALSE)","v":7},"","","","",0,null,null,"",""]
[null,null,null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A311","v":"FP501"},{"$f":"VLOOKUP(A241,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Feedstock type 2"},{"$f":"IF('Input Project'!H177=\"\",\"\",'Input Project'!H177)","v":"No crop"},{"$f":"VLOOKUP($A241,list_database2,$I$9,FALSE)","v":"No crop"},"",{"$f":"IF($L241=1,IF(MonteCarlo=1,$E241,IF($C241=\"\",$D241,$C241)),IF($C241=\"\",$D241,$C241))","v":"No crop"},null,"","","","",0,null,null,{"$f":"IF($L241=1,VLOOKUP($A241,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L241=1,VLOOKUP($A241,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A312","v":"FP502"},{"$f":"VLOOKUP(A242,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Origin of the feedstock"},{"$f":"IF('Input RU'!K49=\"\",\"\",'Input RU'!K49)","v":""},{"$f":"VLOOKUP($A242,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L242=1,IF(MonteCarlo=1,$E242,IF($C242=\"\",$D242,$C242)),IF($C242=\"\",$D242,$C242))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A313","v":"FP503a"},{"$f":"VLOOKUP(A243,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 2 per ha"},{"$f":"IF('Input Project'!H178=\"\",\"\",'Input Project'!H178)","v":""},{"$f":"VLOOKUP($A243,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L243=1,IF(MonteCarlo=1,$E243,IF($C243=\"\",$D243,$C243)),IF($C243=\"\",$D243,$C243))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W118=\"\",\"\",Uncertainty!W118)","v":""},{"$f":"IF(Uncertainty!Z118=\"\",\"\",Uncertainty!Z118)","v":""},0,0]
[{"$f":"'ID-numbers'!$A314","v":"FP503b"},{"$f":"VLOOKUP(A244,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of feedstock 2 per ha"},null,null,"",null,{"$f":"VLOOKUP(A244,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A315","v":"FP503c"},{"$f":"VLOOKUP(A245,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of feedstock 2 per ha"},null,null,"",null,{"$f":"VLOOKUP(A245,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A316","v":"FP505"},{"$f":"VLOOKUP(A246,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Number of harvests per year"},null,{"$f":"VLOOKUP($A246,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L246=1,IF(MonteCarlo=1,$E246,IF($C246=\"\",$D246,$C246)),IF($C246=\"\",$D246,$C246))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A317","v":"FP506"},{"$f":"VLOOKUP(A247,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Rotation system"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A318","v":"FP509"},{"$f":"VLOOKUP(A248,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of the harvested crop"},{"$f":"IF('Input Project'!H179=\"\",\"\",'Input Project'!H179)","v":""},{"$f":"VLOOKUP($A248,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L248=1,IF(MonteCarlo=1,$E248,IF($C248=\"\",$D248,$C248)),IF($C248=\"\",$D248,$C248))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W119=\"\",\"\",Uncertainty!W119)","v":""},{"$f":"IF(Uncertainty!Z119=\"\",\"\",Uncertainty!Z119)","v":""},0,0]
[{"$f":"'ID-numbers'!$A319","v":"FP510"},{"$f":"VLOOKUP(A249,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of the dry energy crop (LHV)"},null,null,"",null,{"$f":"VLOOKUP(A249,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A320","v":"FP516a"},{"$f":"VLOOKUP(A250,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 1"},{"$f":"IF('Input Project'!H180=\"\",\"\",'Input Project'!H180)","v":""},{"$f":"VLOOKUP($A250,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L250=1,IF(MonteCarlo=1,$E250,IF($C250=\"\",$D250,$C250)),IF($C250=\"\",$D250,$C250))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A321","v":"FP516b"},{"$f":"VLOOKUP(A251,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 2"},{"$f":"IF('Input Project'!H183=\"\",\"\",'Input Project'!H183)","v":""},{"$f":"VLOOKUP($A251,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L251=1,IF(MonteCarlo=1,$E251,IF($C251=\"\",$D251,$C251)),IF($C251=\"\",$D251,$C251))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A322","v":"FP517a"},{"$f":"VLOOKUP(A252,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of by-product 1 per ha"},{"$f":"IF('Input Project'!H181=\"\",\"\",'Input Project'!H181)","v":""},{"$f":"VLOOKUP($A252,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L252=1,IF(MonteCarlo=1,$E252,IF($C252=\"\",$D252,$C252)),IF($C252=\"\",$D252,$C252))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W120=\"\",\"\",Uncertainty!W120)","v":""},{"$f":"IF(Uncertainty!Z120=\"\",\"\",Uncertainty!Z120)","v":""},0,0]
[{"$f":"'ID-numbers'!$A323","v":"FP517b"},{"$f":"VLOOKUP(A253,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of by-product 2 per ha"},{"$f":"IF('Input Project'!H184=\"\",\"\",'Input Project'!H184)","v":""},{"$f":"VLOOKUP($A253,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L253=1,IF(MonteCarlo=1,$E253,IF($C253=\"\",$D253,$C253)),IF($C253=\"\",$D253,$C253))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W122=\"\",\"\",Uncertainty!W122)","v":""},{"$f":"IF(Uncertainty!Z122=\"\",\"\",Uncertainty!Z122)","v":""},0,0]
[{"$f":"'ID-numbers'!$A324","v":"FP518a"},{"$f":"VLOOKUP(A254,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of by-product 1 per ha"},null,null,"",null,{"$f":"VLOOKUP(A254,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A325","v":"FP518b"},{"$f":"VLOOKUP(A255,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of by-product 2 per ha"},null,null,"",null,{"$f":"VLOOKUP(A255,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A326","v":"FP519a"},{"$f":"VLOOKUP(A256,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 1"},{"$f":"IF('Input Project'!H182=\"\",\"\",'Input Project'!H182)","v":""},{"$f":"VLOOKUP($A256,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L256=1,IF(MonteCarlo=1,$E256,IF($C256=\"\",$D256,$C256)),IF($C256=\"\",$D256,$C256))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W121=\"\",\"\",Uncertainty!W121)","v":""},{"$f":"IF(Uncertainty!Z121=\"\",\"\",Uncertainty!Z121)","v":""},0,0]
[{"$f":"'ID-numbers'!$A327","v":"FP519b"},{"$f":"VLOOKUP(A257,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 2"},{"$f":"IF('Input Project'!H185=\"\",\"\",'Input Project'!H185)","v":""},{"$f":"VLOOKUP($A257,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L257=1,IF(MonteCarlo=1,$E257,IF($C257=\"\",$D257,$C257)),IF($C257=\"\",$D257,$C257))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W123=\"\",\"\",Uncertainty!W123)","v":""},{"$f":"IF(Uncertainty!Z123=\"\",\"\",Uncertainty!Z123)","v":""},0,0]
[{"$f":"'ID-numbers'!$A328","v":"FP520a"},{"$f":"VLOOKUP(A258,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of the dry by-product 1 (LHV)"},null,null,"",null,{"$f":"VLOOKUP(A258,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A329","v":"FP520b"},{"$f":"VLOOKUP(A259,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of the dry by-product 2 (LHV)"},null,null,"",null,{"$f":"VLOOKUP(A259,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A330","v":"FP521a"},{"$f":"VLOOKUP(A260,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A331","v":"FP521b"},{"$f":"VLOOKUP(A261,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A332","v":"FP522"},{"$f":"VLOOKUP(A262,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of seeds"},{"$f":"IF('Input Project'!H186=\"\",\"\",'Input Project'!H186)","v":""},{"$f":"VLOOKUP($A262,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L262=1,IF(MonteCarlo=1,$E262,IF($C262=\"\",$D262,$C262)),IF($C262=\"\",$D262,$C262))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W124=\"\",\"\",Uncertainty!W124)","v":""},{"$f":"IF(Uncertainty!Z124=\"\",\"\",Uncertainty!Z124)","v":""},0,0]
[{"$f":"'ID-numbers'!$A333","v":"FP523a"},{"$f":"VLOOKUP(A263,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of N-fertiliser (synthetic)"},{"$f":"IF('Input Project'!H187=\"\",\"\",'Input Project'!H187)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W125=\"\",\"\",Uncertainty!W125)","v":""},{"$f":"IF(Uncertainty!Z125=\"\",\"\",Uncertainty!Z125)","v":""},0,0]
[{"$f":"'ID-numbers'!$A334","v":"FP523b"},{"$f":"VLOOKUP(A264,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of P2O5-fertiliser"},{"$f":"IF('Input Project'!H188=\"\",\"\",'Input Project'!H188)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W126=\"\",\"\",Uncertainty!W126)","v":""},{"$f":"IF(Uncertainty!Z126=\"\",\"\",Uncertainty!Z126)","v":""},0,0]
[{"$f":"'ID-numbers'!$A335","v":"FP523c"},{"$f":"VLOOKUP(A265,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of K2O-fertiliser"},{"$f":"IF('Input Project'!H189=\"\",\"\",'Input Project'!H189)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W127=\"\",\"\",Uncertainty!W127)","v":""},{"$f":"IF(Uncertainty!Z127=\"\",\"\",Uncertainty!Z127)","v":""},0,0]
[{"$f":"'ID-numbers'!$A336","v":"FP523d"},{"$f":"VLOOKUP(A266,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of CaO-fertiliser"},{"$f":"IF('Input Project'!H190=\"\",\"\",'Input Project'!H190)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W128=\"\",\"\",Uncertainty!W128)","v":""},{"$f":"IF(Uncertainty!Z128=\"\",\"\",Uncertainty!Z128)","v":""},0,0]
[{"$f":"'ID-numbers'!$A337","v":"FP523e"},{"$f":"VLOOKUP(A267,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Use of pesticides"},{"$f":"IF('Input Project'!H191=\"\",\"\",'Input Project'!H191)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W129=\"\",\"\",Uncertainty!W129)","v":""},{"$f":"IF(Uncertainty!Z129=\"\",\"\",Uncertainty!Z129)","v":""},0,0]
[{"$f":"'ID-numbers'!$A338","v":"FP524a"},{"$f":"VLOOKUP(A268,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A268,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A339","v":"FP524b"},{"$f":"VLOOKUP(A269,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A269,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A340","v":"FP525a"},{"$f":"VLOOKUP(A270,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A270,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A341","v":"FP525b"},{"$f":"VLOOKUP(A271,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A271,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A344","v":"FP529a"},{"$f":"VLOOKUP(A272,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy used for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A272,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A346","v":"FP530"},{"$f":"VLOOKUP(A273,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to energy crop"},null,null,"",null,{"$f":"VLOOKUP(A273,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":100},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A347","v":"FP531"},{"$f":"VLOOKUP(A274,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-products"},null,null,"",null,{"$f":"VLOOKUP(A274,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A352","v":"FP534"},{"$f":"VLOOKUP(A275,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for agricultural machinery"},{"$f":"IF('Input Project'!H192=\"\",\"\",'Input Project'!H192)","v":""},{"$f":"VLOOKUP($A275,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L275=1,IF(MonteCarlo=1,$E275,IF($C275=\"\",$D275,$C275)),IF($C275=\"\",$D275,$C275))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A353","v":"FP535a"},{"$f":"VLOOKUP(A276,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to agrifuel use"},null,null,"",null,{"$f":"VLOOKUP(A276,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A355","v":"FP536"},{"$f":"VLOOKUP(A277,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of fuel used in agricultural machinery"},null,null,"",null,{"$f":"VLOOKUP(A277,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A356","v":"FP537"},{"$f":"VLOOKUP(A278,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel used in agricultural machinery"},{"$f":"IF('Input Project'!H193=\"\",\"\",'Input Project'!H193)","v":""},{"$f":"VLOOKUP($A278,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L278=1,IF(MonteCarlo=1,$E278,IF($C278=\"\",$D278,$C278)),IF($C278=\"\",$D278,$C278))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W130=\"\",\"\",Uncertainty!W130)","v":""},{"$f":"IF(Uncertainty!Z130=\"\",\"\",Uncertainty!Z130)","v":""},0,0]
[{"$f":"'ID-numbers'!$A360","v":"FP539b"},{"$f":"VLOOKUP(A279,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy used for heat and electricity for drying and storage per MJ endfuel"},null,null,"",null,{"$f":"VLOOKUP(A279,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A361","v":"FP540"},{"$f":"VLOOKUP(A280,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat energy use for drying and storage of the crop"},{"$f":"IF('Input Project'!H198=\"\",\"\",'Input Project'!H198)","v":""},{"$f":"VLOOKUP($A280,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L280=1,IF(MonteCarlo=1,$E280,IF($C280=\"\",$D280,$C280)),IF($C280=\"\",$D280,$C280))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W142=\"\",\"\",Uncertainty!W142)","v":""},{"$f":"IF(Uncertainty!Z142=\"\",\"\",Uncertainty!Z142)","v":""},0,0]
[{"$f":"'ID-numbers'!$A362","v":"FP541"},{"$f":"VLOOKUP(A281,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat source"},{"$f":"IF('Input Project'!H197=\"\",\"\",'Input Project'!H197)","v":""},{"$f":"VLOOKUP($A281,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L281=1,IF(MonteCarlo=1,$E281,IF($C281=\"\",$D281,$C281)),IF($C281=\"\",$D281,$C281))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A363","v":"FP542a"},{"$f":"VLOOKUP(A282,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of heat production for crop drying and storage"},null,null,"",null,{"$f":"VLOOKUP(A282,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A368","v":"FP543"},{"$f":"VLOOKUP(A283,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity energy use for drying and storage of the crop"},{"$f":"IF('Input Project'!H200=\"\",\"\",'Input Project'!H200)","v":""},{"$f":"VLOOKUP($A283,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L283=1,IF(MonteCarlo=1,$E283,IF($C283=\"\",$D283,$C283)),IF($C283=\"\",$D283,$C283))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W143=\"\",\"\",Uncertainty!W143)","v":""},{"$f":"IF(Uncertainty!Z143=\"\",\"\",Uncertainty!Z143)","v":""},0,0]
[{"$f":"'ID-numbers'!$A369","v":"FP544"},{"$f":"VLOOKUP(A284,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity source"},{"$f":"IF('Input Project'!H199=\"\",\"\",'Input Project'!H199)","v":""},{"$f":"VLOOKUP($A284,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L284=1,IF(MonteCarlo=1,$E284,IF($C284=\"\",$D284,$C284)),IF($C284=\"\",$D284,$C284))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A370","v":"FP545a"},{"$f":"VLOOKUP(A285,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of electricity for crop drying and storage"},null,null,"",null,{"$f":"VLOOKUP(A285,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A375","v":"FP546a"},{"$f":"VLOOKUP(A286,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use of seeds, fertilisers and pesticides"},null,null,{"$f":"IF(MonteCarlo=1,IF($L286=1,IF($H286=\"n.a.\",0,IF($H286<0.009,0,MIN(MAX(NORMINV(RAND(),$H286,$K286),$I286),$J286))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A286,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},{"$f":"IF($L286=1,IF($C286=\"\",$D286,$C286),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A377","v":"FP547"},{"$f":"VLOOKUP(A287,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Pretreated feedstock"},null,{"$f":"VLOOKUP($A287,list_database2,$I$9,FALSE)","v":"No crop"},null,{"$f":"IF($L287=1,IF(MonteCarlo=1,$E287,IF($C287=\"\",$D287,$C287)),IF($C287=\"\",$D287,$C287))","v":"No crop"}]
[{"$f":"'ID-numbers'!$A378","v":"FP548"},{"$f":"VLOOKUP(A288,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content pretreated feedstock"},null,null,"",null,null,"",{"$f":"IF($L288=1,IF($M288=\"\",$O288,$M288),\"\")","v":""},{"$f":"IF($L288=1,IF($N288=\"\",$P288,$N288),\"\")","v":""},{"$f":"IF($L288=1,($J288-$I288)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A379","v":"FP549"},{"$f":"VLOOKUP(A289,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content pretreated feedstock"},{"$f":"IF('Input Project'!H239=\"\",\"\",'Input Project'!H239)","v":""},{"$f":"VLOOKUP($A289,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L289=1,IF(MonteCarlo=1,$E289,IF($C289=\"\",$D289,$C289)),IF($C289=\"\",$D289,$C289))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A380","v":"FP550a"},{"$f":"VLOOKUP(A290,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of N fertiliser"},null,null,"",null,{"$f":"VLOOKUP(A290,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":48.990600000000001},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A381","v":"FP550b"},{"$f":"VLOOKUP(A291,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of P fertiliser"},null,null,"",null,{"$f":"VLOOKUP(A291,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":15.2334},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A382","v":"FP550c"},{"$f":"VLOOKUP(A292,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of K fertiliser"},null,null,"",null,{"$f":"VLOOKUP(A292,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":9.67896},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A383","v":"FP550d"},{"$f":"VLOOKUP(A293,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of Ca fertiliser"},null,null,"",null,{"$f":"VLOOKUP(A293,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":1.9735200000000002},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A384","v":"FP550e"},{"$f":"VLOOKUP(A294,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of pesticides"},null,null,"",null,{"$f":"VLOOKUP(A294,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":268.39980000000003},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A385","v":"FP550f"},{"$f":"VLOOKUP(A295,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy coefficient of seeds"},null,null,"",null,{"$f":"VLOOKUP(A295,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A386","v":"FP551"},{"$f":"VLOOKUP(A296,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of pretreated feedstock 2 per ha"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A387","v":"FP552"},{"$f":"VLOOKUP(A297,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of pretreated feedstock 2 per ha"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A388","v":"FP553"},{"$f":"VLOOKUP(A298,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of pretreated feedstock 2 per ha"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A389","v":"FP554"},{"$f":"VLOOKUP(A299,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield loss through treatment and transport of feedstock 2"},null,{"$f":"VLOOKUP($A299,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L299=1,IF(MonteCarlo=1,$E299,IF($C299=\"\",$D299,$C299)),IF($C299=\"\",$D299,$C299))","v":0},null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A390","v":"FP555a"},{"$f":"VLOOKUP(A300,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of pretreated feedstock 2 before conversion"},null,null,"",null,{"$f":"VLOOKUP(A300,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A391","v":"FP555b"},{"$f":"VLOOKUP(A301,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of pretreated feedstock 2 before conversion"},null,null,"",null,{"$f":"VLOOKUP(A301,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A392","v":"FP555c"},{"$f":"VLOOKUP(A302,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of pretreated feedstock 2 before conversion"},null,null,"",null,{"$f":"VLOOKUP(A302,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A393","v":"FP556a"},{"$f":"VLOOKUP(A303,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with inputs for feedstock production"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A395","v":"FP557"},{"$f":"VLOOKUP(A304,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated GHG emissions from feedstock production"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A396","v":"FP558"},{"$f":"VLOOKUP(A305,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with fuel used in agricultural machinery"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A397","v":"FP559"},{"$f":"VLOOKUP(A306,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions of the fuel used in agricultural machinery"},null,null,"",null,null,"","","","",0,null,null,{"$f":"IF($L306=1,VLOOKUP($A306,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L306=1,VLOOKUP($A306,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A398","v":"FP561a"},{"$f":"VLOOKUP(A307,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A307,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A399","v":"FP561b"},{"$f":"VLOOKUP(A308,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A308,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A400","v":"FP562a"},{"$f":"VLOOKUP(A309,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with heat and electricity for drying and storage per kg"},null,null,"",null,{"$f":"VLOOKUP(A309,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A401","v":"FP562b"},{"$f":"VLOOKUP(A310,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with heat and electricity for drying and storage per MJ endfuel"},null,null,"",null,{"$f":"VLOOKUP(A310,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A402","v":"FP564"},{"$f":"VLOOKUP(A311,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with production of seeds, fertilisers and pesticides"},null,null,"",null,{"$f":"VLOOKUP(A311,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A403","v":"FP567a"},{"$f":"VLOOKUP(A312,'ID-numbers'!$1:$1048576,2,FALSE)","v":"N: specific GHG emissions"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A404","v":"FP567b"},{"$f":"VLOOKUP(A313,'ID-numbers'!$1:$1048576,2,FALSE)","v":"P2O5: specific GHG emissions"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A405","v":"FP567c"},{"$f":"VLOOKUP(A314,'ID-numbers'!$1:$1048576,2,FALSE)","v":"K2O: specific GHG emissions"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A406","v":"FP567d"},{"$f":"VLOOKUP(A315,'ID-numbers'!$1:$1048576,2,FALSE)","v":"CaO: specific GHG emissions"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A407","v":"FP567e"},{"$f":"VLOOKUP(A316,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Pesticides: specific GHG emissions"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A408","v":"FP567f"},{"$f":"VLOOKUP(A317,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Seeds: specific GHG emissions"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A409","v":"FP568a"},{"$f":"VLOOKUP(A318,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with land use change (carbon stock changes) per MJ"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A410","v":"FP568b"},{"$f":"VLOOKUP(A319,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with land use change (carbon stock changes) per ha"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A411","v":"FP569a"},{"$f":"VLOOKUP(A320,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Actual land use"},"",{"$f":"VLOOKUP($A320,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L320=1,IF(MonteCarlo=1,$E320,IF($C320=\"\",$D320,$C320)),IF($C320=\"\",$D320,$C320))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A412","v":"FP569b"},{"$f":"VLOOKUP(A321,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Previous land use (January 1st, 2008)"},"Annual cropland","n.a.","","Annual cropland",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A413","v":"FP569c"},{"$f":"VLOOKUP(A322,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Actual land use_specific for carbon stock veg"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A414","v":"FP569d"},{"$f":"VLOOKUP(A323,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Previous land use (January 1st, 2008)_specific for carbon stock veg"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A415","v":"FP570a"},{"$f":"VLOOKUP(A324,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Climate region"},{"$f":"IF('Input Land use'!K121=\"\",\"\",'Input Land use'!K121)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A416","v":"FP570b"},{"$f":"VLOOKUP(A325,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Soil type"},{"$f":"IF('Input Land use'!K122=\"\",\"\",'Input Land use'!K122)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A417","v":"FP570c"},{"$f":"VLOOKUP(A326,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Climate region_specific for carbon stock_actual land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A418","v":"FP570d"},{"$f":"VLOOKUP(A327,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Climate region_specific for carbon stock_previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A419","v":"FP571"},{"$f":"VLOOKUP(A328,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A420","v":"FP572"},{"$f":"VLOOKUP(A329,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A421","v":"FP573a"},{"$f":"VLOOKUP(A330,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Soil organic carbon actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A422","v":"FP573b"},{"$f":"VLOOKUP(A331,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Soil organic carbon previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A423","v":"FP574"},{"$f":"VLOOKUP(A332,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard soil organic carbon_feedstock 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A424","v":"FP575a"},{"$f":"VLOOKUP(A333,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use factor actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A425","v":"FP575b"},{"$f":"VLOOKUP(A334,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use factor previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A426","v":"FP576a"},{"$f":"VLOOKUP(A335,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Management factor actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A427","v":"FP576b"},{"$f":"VLOOKUP(A336,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Management factor previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A428","v":"FP577a"},{"$f":"VLOOKUP(A337,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input factor actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A429","v":"FP577b"},{"$f":"VLOOKUP(A338,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input factor previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A430","v":"FP578a"},{"$f":"VLOOKUP(A339,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A431","v":"FP578b"},{"$f":"VLOOKUP(A340,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A432","v":"FP579a"},{"$f":"VLOOKUP(A341,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock in living biomass actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A433","v":"FP579b"},{"$f":"VLOOKUP(A342,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock in living biomass previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A434","v":"FP580a"},{"$f":"VLOOKUP(A343,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above ground vegetation carbon stock in living biomass actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A435","v":"FP580b"},{"$f":"VLOOKUP(A344,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above ground vegetation carbon stock in living biomass previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A436","v":"FP581a"},{"$f":"VLOOKUP(A345,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of above ground living biomass actual land use"},{"$f":"IF('Input Land use'!K194=\"\",\"\",'Input Land use'!K194)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A437","v":"FP581b"},{"$f":"VLOOKUP(A346,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of above ground living biomass previous land use"},{"$f":"IF('Input Land use'!K204=\"\",\"\",'Input Land use'!K204)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A438","v":"FP582aa"},{"$f":"VLOOKUP(A347,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in living biomass actual land use"},{"$f":"IF('Input Land use'!K197=\"\",\"\",'Input Land use'!K197)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A439","v":"FP582ab"},{"$f":"VLOOKUP(A348,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in living biomass previous land use"},{"$f":"IF('Input Land use'!K207=\"\",\"\",'Input Land use'!K207)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A440","v":"FP582ba"},{"$f":"VLOOKUP(A349,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in dead wood actual land use"},{"$f":"IF('Input Land use'!K198=\"\",\"\",'Input Land use'!K198)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A441","v":"FP582bb"},{"$f":"VLOOKUP(A350,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in dead wood previous land use"},{"$f":"IF('Input Land use'!K208=\"\",\"\",'Input Land use'!K208)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A442","v":"FP582ca"},{"$f":"VLOOKUP(A351,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in litter actual land use"},{"$f":"IF('Input Land use'!K199=\"\",\"\",'Input Land use'!K199)","v":""},null,{"$f":"IF(MonteCarlo=1,IF($L351=1,IF($H351=\"n.a.\",0,IF($H351<0.009,0,MIN(MAX(NORMINV(RAND(),$H351,$K351),$I351),$J351))),\"\"),\"\")","v":""},null,null,{"$f":"IF($L351=1,IF($C351=\"\",$D351,$C351),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A443","v":"FP582cb"},{"$f":"VLOOKUP(A352,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon fraction of dry matter in litter previous land use"},{"$f":"IF('Input Land use'!K209=\"\",\"\",'Input Land use'!K209)","v":""},null,"",null,null,"",{"$f":"IF($L352=1,IF($M352=\"\",$O352,$M352),\"\")","v":""},{"$f":"IF($L352=1,IF($N352=\"\",$P352,$N352),\"\")","v":""},{"$f":"IF($L352=1,($J352-$I352)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A444","v":"FP583a"},{"$f":"VLOOKUP(A353,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below ground carbon stock to above ground carbon stock in living biomass actual land use"},{"$f":"IF('Input Land use'!K192=\"\",\"\",'Input Land use'!K192)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A445","v":"FP583b"},{"$f":"VLOOKUP(A354,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below ground carbon stock to above ground carbon stock in living biomass previous land use"},{"$f":"IF('Input Land use'!K202=\"\",\"\",'Input Land use'!K202)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A446","v":"FP584a"},{"$f":"VLOOKUP(A355,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Below ground vegetation carbon stock in living biomass actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A447","v":"FP584b"},{"$f":"VLOOKUP(A356,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Below ground vegetation carbon stock in living biomass previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A448","v":"FP585a"},{"$f":"VLOOKUP(A357,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of below ground living biomass actual land use"},{"$f":"IF('Input Land use'!K191=\"\",\"\",'Input Land use'!K191)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A449","v":"FP585b"},{"$f":"VLOOKUP(A358,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of below ground living biomass previous land use"},{"$f":"IF('Input Land use'!K201=\"\",\"\",'Input Land use'!K201)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A450","v":"FP586a"},{"$f":"VLOOKUP(A359,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock in dead organic matter actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A451","v":"FP586b"},{"$f":"VLOOKUP(A360,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above and below vegetation carbon stock in dead organic matter previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A452","v":"FP587a"},{"$f":"VLOOKUP(A361,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock in dead wood pool actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A453","v":"FP587b"},{"$f":"VLOOKUP(A362,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock in dead wood pool previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A454","v":"FP588a"},{"$f":"VLOOKUP(A363,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of dead wood pool actual land use"},{"$f":"IF('Input Land use'!K195=\"\",\"\",'Input Land use'!K195)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A455","v":"FP588b"},{"$f":"VLOOKUP(A364,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of dead wood pool previous land use"},{"$f":"IF('Input Land use'!K205=\"\",\"\",'Input Land use'!K205)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A456","v":"FP589a"},{"$f":"VLOOKUP(A365,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock in litter actual land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A457","v":"FP589b"},{"$f":"VLOOKUP(A366,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon stock in litter previous land use"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A458","v":"FP590a"},{"$f":"VLOOKUP(A367,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of litter actual land use"},{"$f":"IF('Input Land use'!K196=\"\",\"\",'Input Land use'!K196)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A459","v":"FP590b"},{"$f":"VLOOKUP(A368,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Weight of litter previous land use"},{"$f":"IF('Input Land use'!K206=\"\",\"\",'Input Land use'!K206)","v":""},null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A460","v":"FP591a"},{"$f":"VLOOKUP(A369,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Peatland"},null,{"$f":"VLOOKUP($A369,list_database2,$I$9,FALSE)","v":{"$error":"#N/A"}},"",{"$f":"IF($L369=1,IF(MonteCarlo=1,$E369,IF($C369=\"\",$D369,$C369)),IF($C369=\"\",$D369,$C369))","v":{"$error":"#N/A"}},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A461","v":"FP591b"},{"$f":"VLOOKUP(A370,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Emission factor soil organic carbon_peatland"},null,null,"",null,null,"","","","",0,null,null,{"$f":"IF($L370=1,VLOOKUP($A370,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L370=1,VLOOKUP($A370,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A462","v":"FP592a"},{"$f":"VLOOKUP(A371,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Previously degraded land"},{"$f":"IF('Input Land use'!K146=\"yes\",\"1\",IF('Input Land use'!K146=\"no\",\"0\",\"\"))","v":""},{"$f":"VLOOKUP($A371,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L371=1,IF(MonteCarlo=1,$E371,IF($C371=\"\",$D371,$C371)),IF($C371=\"\",$D371,$C371))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A463","v":"FP592b"},{"$f":"VLOOKUP(A372,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Bonus restored degraded land"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A464","v":"FP593a"},{"$f":"VLOOKUP(A373,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land management actual land use"},"",{"$f":"VLOOKUP($A373,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L373=1,IF(MonteCarlo=1,$E373,IF($C373=\"\",$D373,$C373)),IF($C373=\"\",$D373,$C373))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A465","v":"FP593b"},{"$f":"VLOOKUP(A374,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land management previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A466","v":"FP594a"},{"$f":"VLOOKUP(A375,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input actual land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A467","v":"FP594b"},{"$f":"VLOOKUP(A376,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A468","v":"FP595a"},{"$f":"VLOOKUP(A377,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Domain actual land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A469","v":"FP595b"},{"$f":"VLOOKUP(A378,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Domain previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A470","v":"FP596a"},{"$f":"VLOOKUP(A379,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ecological zone actual land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A471","v":"FP596b"},{"$f":"VLOOKUP(A380,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ecological zone previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A472","v":"FP597a"},{"$f":"VLOOKUP(A381,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Continent actual land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A473","v":"FP597b"},{"$f":"VLOOKUP(A382,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Continent previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A474","v":"FP598a"},{"$f":"VLOOKUP(A383,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type actual land use"},"","n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A475","v":"FP598b"},{"$f":"VLOOKUP(A384,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type previous land use"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A476","v":"FP599"},{"$f":"VLOOKUP(A385,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with indirect land use change (soil carbon release)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A477","v":"FP600"},{"$f":"VLOOKUP(A386,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock production"},{"$f":"IF('Input RU'!K50=\"\",\"\",'Input RU'!K50)","v":""},0,"",{"$f":"IF($L386=1,IF(MonteCarlo=1,$E386,IF($C386=\"\",$D386,$C386)),IF($C386=\"\",$D386,$C386))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W131=\"\",\"\",Uncertainty!W131)","v":""},{"$f":"IF(Uncertainty!Z131=\"\",\"\",Uncertainty!Z131)","v":""},0,0]
[{"$f":"'ID-numbers'!$A478","v":"FP601"},{"$f":"VLOOKUP(A387,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated water use for feedstock production"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A479","v":"FP602a"},{"$f":"VLOOKUP(A388,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A388,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A480","v":"FP602b"},{"$f":"VLOOKUP(A389,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use for feedstock production"},null,null,"",null,{"$f":"VLOOKUP(A389,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A481","v":"FP603a"},{"$f":"VLOOKUP(A390,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},{"$f":"IF('Input RU'!K53=\"\",\"\",'Input RU'!K53)","v":""},{"$f":"VLOOKUP($A390,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L390=1,IF(MonteCarlo=1,$E390,IF($C390=\"\",$D390,$C390)),IF($C390=\"\",$D390,$C390))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W144=\"\",\"\",Uncertainty!W144)","v":""},{"$f":"IF(Uncertainty!Z144=\"\",\"\",Uncertainty!Z144)","v":""},0,0]
[{"$f":"'ID-numbers'!$A482","v":"FP603b"},{"$f":"VLOOKUP(A391,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A483","v":"FP604a"},{"$f":"VLOOKUP(A392,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Country freshwater availability"},null,null,null,null,{"$f":"VLOOKUP(A392,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A484","v":"FP604b"},{"$f":"VLOOKUP(A393,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Country freshwater level"},null,null,null,null,{"$f":"VLOOKUP(A393,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A486","v":"FP606a"},{"$f":"VLOOKUP(A394,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated land use for feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A394,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A487","v":"FP606b"},{"$f":"VLOOKUP(A395,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated land use for feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A395,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A488","v":"FP607a"},{"$f":"VLOOKUP(A396,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Carbon debt due to land use change"},null,null,null,null,{"$f":"VLOOKUP(A396,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A492","v":"FP609"},{"$f":"VLOOKUP(A397,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input of N-fixing crop residue to the soil"},{"$f":"IF('Input Land use'!K180=\"\",\"\",'Input Land use'!K180)","v":""},0,"",{"$f":"IF($L397=1,IF(MonteCarlo=1,$E397,IF($C397=\"\",$D397,$C397)),IF($C397=\"\",$D397,$C397))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W136=\"\",\"\",Uncertainty!W136)","v":""},{"$f":"IF(Uncertainty!Z136=\"\",\"\",Uncertainty!Z136)","v":""},0,0]
[{"$f":"'ID-numbers'!$A501","v":"FP615a"},{"$f":"VLOOKUP(A398,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A398,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A502","v":"FP615b"},{"$f":"VLOOKUP(A399,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A399,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A519","v":"FP625a"},{"$f":"VLOOKUP(A400,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A400,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A520","v":"FP625b"},{"$f":"VLOOKUP(A401,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from feedstock production"},null,null,null,null,{"$f":"VLOOKUP(A401,'Production feedstock2'!$D$9:$G$5048,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A523","v":"FP630a"},{"$f":"VLOOKUP(A402,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total (direct + indirect) N2O emissions from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A524","v":"FP630b"},{"$f":"VLOOKUP(A403,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total (direct + indirect) N2O emissions from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A525","v":"FP631"},{"$f":"VLOOKUP(A404,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Soil water saturation (yes=1,no=0)"},{"$f":"IF('Input Land use'!K145=\"yes\",\"1\",IF('Input Land use'!K145=\"no\",\"0\",\"\"))","v":""},"n.a.","",{"$f":"IF($L404=1,IF(MonteCarlo=1,$E404,IF($C404=\"\",$D404,$C404)),IF($C404=\"\",$D404,$C404))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A526","v":"FP632"},{"$f":"VLOOKUP(A405,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Field renewal (annual crops = 1)"},{"$f":"IF('Input Land use'!K173=\"\",\"\",'Input Land use'!K173)","v":""},0,"",{"$f":"IF($L405=1,IF(MonteCarlo=1,$E405,IF($C405=\"\",$D405,$C405)),IF($C405=\"\",$D405,$C405))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A527","v":"FP633"},{"$f":"VLOOKUP(A406,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of crop residue returned to the field (only for palm)"},{"$f":"IF('Input Land use'!K188=\"\",\"\",'Input Land use'!K188)","v":""},0,"",{"$f":"IF($L406=1,IF(MonteCarlo=1,$E406,IF($C406=\"\",$D406,$C406)),IF($C406=\"\",$D406,$C406))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W138=\"\",\"\",Uncertainty!W138)","v":""},{"$f":"IF(Uncertainty!Z138=\"\",\"\",Uncertainty!Z138)","v":""},0,0]
[{"$f":"'ID-numbers'!$A528","v":"FP634"},{"$f":"VLOOKUP(A407,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Organic soil (yes=1,no=0)"},{"$f":"IF('Input Land use'!K144=\"yes\",\"1\",IF('Input Land use'!K144=\"no\",\"0\",\"\"))","v":""},"n.a.","",{"$f":"IF($L407=1,IF(MonteCarlo=1,$E407,IF($C407=\"\",$D407,$C407)),IF($C407=\"\",$D407,$C407))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A529","v":"FP635"},{"$f":"VLOOKUP(A408,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Nutrient level (only for ORGANIC soils + temperate/boreal climate + forest (native and managed))"},{"$f":"IF('Input Land use'!K148=\"\",\"\",'Input Land use'!K148)","v":""},"n.a.","",{"$f":"IF($L408=1,IF(MonteCarlo=1,$E408,IF($C408=\"\",$D408,$C408)),IF($C408=\"\",$D408,$C408))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A538","v":"FP640"},{"$f":"VLOOKUP(A409,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total amount of organic N fertiliser applied to soil (other than by grazing animals)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A539","v":"FP641a"},{"$f":"VLOOKUP(A410,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of animal manure N applied to soil (other than by grazing animals)"},{"$f":"IF('Input Land use'!K174=\"\",\"\",'Input Land use'!K174)","v":""},{"$f":"VLOOKUP($A410,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L410=1,IF(MonteCarlo=1,$E410,IF($C410=\"\",$D410,$C410)),IF($C410=\"\",$D410,$C410))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W132=\"\",\"\",Uncertainty!W132)","v":""},{"$f":"IF(Uncertainty!Z132=\"\",\"\",Uncertainty!Z132)","v":""},0,0]
[{"$f":"'ID-numbers'!$A540","v":"FP641b"},{"$f":"VLOOKUP(A411,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of total sewage N applied to soil"},{"$f":"IF('Input Land use'!K176=\"\",\"\",'Input Land use'!K176)","v":""},{"$f":"VLOOKUP($A411,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L411=1,IF(MonteCarlo=1,$E411,IF($C411=\"\",$D411,$C411)),IF($C411=\"\",$D411,$C411))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W133=\"\",\"\",Uncertainty!W133)","v":""},{"$f":"IF(Uncertainty!Z133=\"\",\"\",Uncertainty!Z133)","v":""},0,0]
[{"$f":"'ID-numbers'!$A541","v":"FP641c"},{"$f":"VLOOKUP(A412,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of total compost N applied to soil"},{"$f":"IF('Input Land use'!K177=\"\",\"\",'Input Land use'!K177)","v":""},{"$f":"VLOOKUP($A412,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L412=1,IF(MonteCarlo=1,$E412,IF($C412=\"\",$D412,$C412)),IF($C412=\"\",$D412,$C412))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W134=\"\",\"\",Uncertainty!W134)","v":""},{"$f":"IF(Uncertainty!Z134=\"\",\"\",Uncertainty!Z134)","v":""},0,0]
[{"$f":"'ID-numbers'!$A542","v":"FP641d"},{"$f":"VLOOKUP(A413,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of N of other organic amendments applied to soil (used as fertiliser)"},{"$f":"IF('Input Land use'!K178=\"\",\"\",'Input Land use'!K178)","v":""},{"$f":"VLOOKUP($A413,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L413=1,IF(MonteCarlo=1,$E413,IF($C413=\"\",$D413,$C413)),IF($C413=\"\",$D413,$C413))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W135=\"\",\"\",Uncertainty!W135)","v":""},{"$f":"IF(Uncertainty!Z135=\"\",\"\",Uncertainty!Z135)","v":""},0,0]
[{"$f":"'ID-numbers'!$A543","v":"FP642"},{"$f":"VLOOKUP(A414,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total amount of N in crop residues (including N-fixing crops and renewal) returned to soil"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A544","v":"FP643a"},{"$f":"VLOOKUP(A415,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of above-ground residues to harvested yield_calculated"},null,null,"",null,{"$f":"VLOOKUP(A415,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A545","v":"FP643b"},{"$f":"VLOOKUP(A416,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of above-ground residues to harvested yield_final"},{"$f":"IF('Input Land use'!K183=\"\",\"\",'Input Land use'!K183)","v":""},{"$f":"G415","v":0},"",{"$f":"IF($L416=1,IF(MonteCarlo=1,$E416,IF($C416=\"\",$D416,$C416)),IF($C416=\"\",$D416,$C416))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A546","v":"FP644"},{"$f":"VLOOKUP(A417,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Above-ground residue (dry) (=AGDM(T))"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A547","v":"FP645a"},{"$f":"VLOOKUP(A418,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Slope to calculate above-ground residue"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A548","v":"FP645b"},{"$f":"VLOOKUP(A419,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Intercept to calculate above-ground residue"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A549","v":"FP646a"},{"$f":"VLOOKUP(A420,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below-ground residues to harvested yield_calculated"},null,null,"",null,{"$f":"VLOOKUP(A420,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A550","v":"FP646b"},{"$f":"VLOOKUP(A421,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below-ground residues to harvested yield_final"},{"$f":"IF('Input Land use'!K185=\"\",\"\",'Input Land use'!K185)","v":""},{"$f":"G420","v":0},"",{"$f":"IF($L421=1,IF(MonteCarlo=1,$E421,IF($C421=\"\",$D421,$C421)),IF($C421=\"\",$D421,$C421))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A551","v":"FP647"},{"$f":"VLOOKUP(A422,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Ratio of below-ground residues to above-ground biomass"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A552","v":"FP648a"},{"$f":"VLOOKUP(A423,'ID-numbers'!$1:$1048576,2,FALSE)","v":"N content of above-ground residues"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A553","v":"FP648b"},{"$f":"VLOOKUP(A424,'ID-numbers'!$1:$1048576,2,FALSE)","v":"N content of below-ground residues"},null,null,{"$f":"IF(MonteCarlo=1,IF($L424=1,IF($H424=\"n.a.\",0,IF($H424<0.009,0,MIN(MAX(NORMINV(RAND(),$H424,$K424),$I424),$J424))),\"\"),\"\")","v":""},null,null,{"$f":"IF($L424=1,IF($C424=\"\",$D424,$C424),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A554","v":"FP649"},{"$f":"VLOOKUP(A425,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fraction of above-ground residues removed"},{"$f":"IF('Input Land use'!K182=\"\",\"\",'Input Land use'!K182)","v":""},{"$f":"VLOOKUP($A425,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L425=1,IF(MonteCarlo=1,$E425,IF($C425=\"\",$D425,$C425)),IF($C425=\"\",$D425,$C425))","v":0},null,0,{"$f":"IF($L425=1,IF($M425=\"\",$O425,$M425),\"\")","v":0},{"$f":"IF($L425=1,IF($N425=\"\",$P425,$N425),\"\")","v":0},{"$f":"IF($L425=1,($J425-$I425)/6,\"\")","v":0},1,{"$f":"IF(Uncertainty!W137=\"\",\"\",Uncertainty!W137)","v":""},{"$f":"IF(Uncertainty!Z137=\"\",\"\",Uncertainty!Z137)","v":""},0,0]
[{"$f":"'ID-numbers'!$A555","v":"FP650"},{"$f":"VLOOKUP(A426,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total amount of N mineralised in mineral soil due to carbon loss through land use change"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A556","v":"FP651"},{"$f":"VLOOKUP(A427,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Average annual loss of soil carbon"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A557","v":"FP652"},{"$f":"VLOOKUP(A428,'ID-numbers'!$1:$1048576,2,FALSE)","v":"C:N ratio of the soil organic matter"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A558","v":"FP653"},{"$f":"VLOOKUP(A429,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Previous land use is cropland (yes=1,no=0)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A559","v":"FP654"},{"$f":"VLOOKUP(A430,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Direct N2O_N emissions from managed organic soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A560","v":"FP655a"},{"$f":"VLOOKUP(A431,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Indirect N2O_N emissions from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A561","v":"FP655b"},{"$f":"VLOOKUP(A432,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Indirect N2O emissions from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A562","v":"FP656"},{"$f":"VLOOKUP(A433,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Indirect N2O_N emissions from atmospheric deposition of N volatilized from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A563","v":"FP657"},{"$f":"VLOOKUP(A434,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fraction of synthetic fertiliser N that volatilises as NH3 and NOx"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A564","v":"FP658"},{"$f":"VLOOKUP(A435,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fraction of organic fertiliser N that volatilises as NH3 and NOx"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A565","v":"FP659"},{"$f":"VLOOKUP(A436,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Indirect N2O_N emissions from N leaching/runoff from managed soils"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A566","v":"FP660"},{"$f":"VLOOKUP(A437,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fraction of all N added to managed soils that is lost through leaching and runoff"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A567","v":"FP661"},{"$f":"VLOOKUP(A438,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in or after January 2008 = undisturbed forest (yes=1,no=0)"},{"$f":"IF('Input Bio'!K83=\"yes\",1,IF('Input Bio'!K83=\"no\",0,\"\"))","v":""},{"$f":"VLOOKUP($A438,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L438=1,IF(MonteCarlo=1,$E438,IF($C438=\"\",$D438,$C438)),IF($C438=\"\",$D438,$C438))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A568","v":"FP662"},{"$f":"VLOOKUP(A439,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in or after January 2008 = nature protection area"},{"$f":"IF('Input Bio'!K84=\"yes\",1,IF('Input Bio'!K84=\"no\",0,\"\"))","v":""},0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A569","v":"FP663"},{"$f":"VLOOKUP(A440,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in or after January 2008 = highly biodiverse grassland"},{"$f":"IF('Input Bio'!K85=\"yes\",1,IF('Input Bio'!K85=\"no\",0,\"\"))","v":""},0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A570","v":"FP664"},{"$f":"VLOOKUP(A441,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in January 2008 and not longer now = wetland"},{"$f":"IF('Input Bio'!K114=\"yes\",1,IF('Input Bio'!K114=\"no\",0,\"\"))","v":""},0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A571","v":"FP665"},{"$f":"VLOOKUP(A442,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in January 2008 and not longer now = continuously forested area"},{"$f":"IF('Input Bio'!K115=\"yes\",1,IF('Input Bio'!K115=\"no\",0,\"\"))","v":""},0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A572","v":"FP666"},{"$f":"VLOOKUP(A443,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land status in January 2008 and not longer now = peatland"},{"$f":"IF('Input Bio'!K116=\"yes\",1,IF('Input Bio'!K116=\"no\",0,\"\"))","v":""},0,"",0,null,"","","","",0,null,null,{"$f":"IF($L443=1,VLOOKUP($A443,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L443=1,VLOOKUP($A443,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A573","v":"FP667"},{"$f":"VLOOKUP(A444,'ID-numbers'!$1:$1048576,2,FALSE)","v":"The requirements of the RED concerning biodiversity & high carbon stocks are met"},null,null,"",null,{"$f":"VLOOKUP(A444,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A574","v":"FP670a"},{"$f":"VLOOKUP(A445,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour"},{"$f":"IF('Input LW'!U87=\"\",\"\",'Input LW'!U87)","v":""},{"$f":"VLOOKUP($A445,list_database2,$I$9,FALSE)","v":"n.a."},"","n.a.",{"$f":"VLOOKUP(A445,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A575","v":"FP670b"},{"$f":"VLOOKUP(A446,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour "},{"$f":"IF('Input LW'!U88=\"\",\"\",'Input LW'!U88)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A446,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A576","v":"FP670c"},{"$f":"VLOOKUP(A447,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights"},{"$f":"IF('Input LW'!U89=\"\",\"\",'Input LW'!U89)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A447,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A577","v":"FP670d"},{"$f":"VLOOKUP(A448,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination"},{"$f":"IF('Input LW'!U90=\"\",\"\",'Input LW'!U90)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A448,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A578","v":"FP670e"},{"$f":"VLOOKUP(A449,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured"},{"$f":"IF('Input LW'!U91=\"\",\"\",'Input LW'!U91)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A449,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A579","v":"FP670f"},{"$f":"VLOOKUP(A450,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders"},{"$f":"IF('Input LW'!U92=\"\",\"\",'Input LW'!U92)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A450,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A580","v":"FP670g"},{"$f":"VLOOKUP(A451,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security"},{"$f":"IF('Input LW'!U93=\"\",\"\",'Input LW'!U93)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A451,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A581","v":"FP671a"},{"$f":"VLOOKUP(A452,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts"},{"$f":"IF('Input LW'!U95=\"\",\"\",'Input LW'!U95)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A452,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A582","v":"FP671b"},{"$f":"VLOOKUP(A453,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights"},{"$f":"IF('Input LW'!U96=\"\",\"\",'Input LW'!U96)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A453,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A583","v":"FP671c"},{"$f":"VLOOKUP(A454,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves"},{"$f":"IF('Input LW'!U97=\"\",\"\",'Input LW'!U97)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A454,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A584","v":"FP671d"},{"$f":"VLOOKUP(A455,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules"},{"$f":"IF('Input LW'!U98=\"\",\"\",'Input LW'!U98)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A455,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A585","v":"FP671e"},{"$f":"VLOOKUP(A456,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy"},{"$f":"IF('Input LW'!U99=\"\",\"\",'Input LW'!U99)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A456,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A586","v":"FP671f"},{"$f":"VLOOKUP(A457,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions"},{"$f":"IF('Input LW'!U100=\"\",\"\",'Input LW'!U100)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A457,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A587","v":"FP671g"},{"$f":"VLOOKUP(A458,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training"},{"$f":"IF('Input LW'!U101=\"\",\"\",'Input LW'!U101)","v":""},"n.a.","","n.a.",{"$f":"VLOOKUP(A458,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A588","v":"FP672"},{"$f":"VLOOKUP(A459,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights_score"},null,null,"",null,{"$f":"VLOOKUP(A459,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A589","v":"FP673"},{"$f":"VLOOKUP(A460,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions_score"},null,null,"",null,{"$f":"VLOOKUP(A460,'Production feedstock2'!$D$9:$G$5042,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[null,null,null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A592","v":"FT001a"},{"$f":"VLOOKUP(A462,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 1"},{"$f":"IF('Input Project'!H49=\"\",\"\",'Input Project'!H49)","v":""},{"$f":"VLOOKUP($A462,list_database1,$I$8,FALSE)","v":"Truck for FFB transport (Diesel)"},"",{"$f":"IF($L462=1,IF(MonteCarlo=1,$E462,IF($C462=\"\",$D462,$C462)),IF($C462=\"\",$D462,$C462))","v":"Truck for FFB transport (Diesel)"},null,"","","","",0,null,null,{"$f":"IF($L462=1,VLOOKUP($A462,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L462=1,VLOOKUP($A462,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A593","v":"FT001b"},{"$f":"VLOOKUP(A463,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 2"},{"$f":"IF('Input Project'!H52=\"\",\"\",'Input Project'!H52)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A594","v":"FT001c"},{"$f":"VLOOKUP(A464,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 3"},{"$f":"IF('Input Project'!H55=\"\",\"\",'Input Project'!H55)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A595","v":"FT001d"},{"$f":"VLOOKUP(A465,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 4"},{"$f":"IF('Input Project'!H112=\"\",\"\",'Input Project'!H112)","v":""},"Truck for liquids (Diesel)","","Truck for liquids (Diesel)",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A596","v":"FT001e"},{"$f":"VLOOKUP(A466,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 5"},{"$f":"IF('Input Project'!H115=\"\",\"\",'Input Project'!H115)","v":""},"Ship /product tanker 50kt (HFO maritime)","","Ship /product tanker 50kt (HFO maritime)",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A597","v":"FT001f"},{"$f":"VLOOKUP(A467,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 6"},{"$f":"IF('Input Project'!H118=\"\",\"\",'Input Project'!H118)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A598","v":"FT001g"},{"$f":"VLOOKUP(A468,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 7"},{"$f":"IF('Input Project'!H164=\"\",\"\",'Input Project'!H164)","v":""},"Truck for liquids (Diesel)","","Truck for liquids (Diesel)",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A599","v":"FT001h"},{"$f":"VLOOKUP(A469,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 8"},{"$f":"IF('Input Project'!H167=\"\",\"\",'Input Project'!H167)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A600","v":"FT001i"},{"$f":"VLOOKUP(A470,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 9"},{"$f":"IF('Input Project'!H170=\"\",\"\",'Input Project'!H170)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A601","v":"FT002a"},{"$f":"VLOOKUP(A471,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 1"},null,null,"",null,{"$f":"VLOOKUP(A471,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":950},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A602","v":"FT002b"},{"$f":"VLOOKUP(A472,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 2"},null,null,"",null,{"$f":"VLOOKUP(A472,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A603","v":"FT002c"},{"$f":"VLOOKUP(A473,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 3"},null,null,"",null,{"$f":"VLOOKUP(A473,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A604","v":"FT002d"},{"$f":"VLOOKUP(A474,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 4"},null,null,"",null,{"$f":"VLOOKUP(A474,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":633.71699789434831},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A605","v":"FT002e"},{"$f":"VLOOKUP(A475,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 5"},null,null,"",null,{"$f":"VLOOKUP(A475,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":43033.608937012214},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A606","v":"FT002f"},{"$f":"VLOOKUP(A476,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 6"},null,null,"",null,{"$f":"VLOOKUP(A476,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A607","v":"FT002g"},{"$f":"VLOOKUP(A477,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 7"},null,null,"",null,{"$f":"VLOOKUP(A477,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":135.14199870371556},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A608","v":"FT002h"},{"$f":"VLOOKUP(A478,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 8"},null,null,"",null,{"$f":"VLOOKUP(A478,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A609","v":"FT002i"},{"$f":"VLOOKUP(A479,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 9"},null,null,"",null,{"$f":"VLOOKUP(A479,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A610","v":"FT003a"},{"$f":"VLOOKUP(A480,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 1"},{"$f":"IF('Input Project'!H50=\"\",\"\",'Input Project'!H50)","v":""},{"$f":"VLOOKUP($A480,list_database1,$I$8,FALSE)","v":50},"",{"$f":"IF($L480=1,IF(MonteCarlo=1,$E480,IF($C480=\"\",$D480,$C480)),IF($C480=\"\",$D480,$C480))","v":50},null,50,20,100,13.333333333333334,1,{"$f":"IF(Uncertainty!W53=\"\",\"\",Uncertainty!W53)","v":""},{"$f":"IF(Uncertainty!Z53=\"\",\"\",Uncertainty!Z53)","v":""},20,100]
[{"$f":"'ID-numbers'!$A611","v":"FT003b"},{"$f":"VLOOKUP(A481,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 2"},{"$f":"IF('Input Project'!H53=\"\",\"\",'Input Project'!H53)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W54=\"\",\"\",Uncertainty!W54)","v":""},{"$f":"IF(Uncertainty!Z54=\"\",\"\",Uncertainty!Z54)","v":""},0,0]
[{"$f":"'ID-numbers'!$A612","v":"FT003c"},{"$f":"VLOOKUP(A482,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 3"},{"$f":"IF('Input Project'!H56=\"\",\"\",'Input Project'!H56)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W55=\"\",\"\",Uncertainty!W55)","v":""},{"$f":"IF(Uncertainty!Z55=\"\",\"\",Uncertainty!Z55)","v":""},0,0]
[{"$f":"'ID-numbers'!$A613","v":"FT003d"},{"$f":"VLOOKUP(A483,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 4"},{"$f":"IF('Input Project'!H113=\"\",\"\",'Input Project'!H113)","v":""},150,"",150,null,150,100,200,16.666666666666668,1,{"$f":"IF(Uncertainty!W82=\"\",\"\",Uncertainty!W82)","v":""},{"$f":"IF(Uncertainty!Z82=\"\",\"\",Uncertainty!Z82)","v":""},100,200]
[{"$f":"'ID-numbers'!$A614","v":"FT003e"},{"$f":"VLOOKUP(A484,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 5"},{"$f":"IF('Input Project'!H116=\"\",\"\",'Input Project'!H116)","v":""},10186,"",10186,null,10186,10000,11000,166.66666666666666,1,{"$f":"IF(Uncertainty!W83=\"\",\"\",Uncertainty!W83)","v":""},{"$f":"IF(Uncertainty!Z83=\"\",\"\",Uncertainty!Z83)","v":""},10000,11000]
[{"$f":"'ID-numbers'!$A615","v":"FT003f"},{"$f":"VLOOKUP(A485,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 6"},{"$f":"IF('Input Project'!H119=\"\",\"\",'Input Project'!H119)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W84=\"\",\"\",Uncertainty!W84)","v":""},{"$f":"IF(Uncertainty!Z84=\"\",\"\",Uncertainty!Z84)","v":""},0,0]
[{"$f":"'ID-numbers'!$A616","v":"FT003g"},{"$f":"VLOOKUP(A486,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 7"},{"$f":"IF('Input Project'!H165=\"\",\"\",'Input Project'!H165)","v":""},100,"",100,null,100,20,200,30,1,{"$f":"IF(Uncertainty!W111=\"\",\"\",Uncertainty!W111)","v":""},{"$f":"IF(Uncertainty!Z111=\"\",\"\",Uncertainty!Z111)","v":""},20,200]
[{"$f":"'ID-numbers'!$A617","v":"FT003h"},{"$f":"VLOOKUP(A487,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 8"},{"$f":"IF('Input Project'!H168=\"\",\"\",'Input Project'!H168)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W112=\"\",\"\",Uncertainty!W112)","v":""},{"$f":"IF(Uncertainty!Z112=\"\",\"\",Uncertainty!Z112)","v":""},0,0]
[{"$f":"'ID-numbers'!$A618","v":"FT003i"},{"$f":"VLOOKUP(A488,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 9"},{"$f":"IF('Input Project'!H171=\"\",\"\",'Input Project'!H171)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L488=1,IF($H488=\"n.a.\",0,IF($H488<0.009,0,MIN(MAX(NORMINV(RAND(),$H488,$K488),$I488),$J488))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L488=1,IF($C488=\"\",$D488,$C488),\"\")","v":0},0,0,0,1,{"$f":"IF(Uncertainty!W113=\"\",\"\",Uncertainty!W113)","v":""},{"$f":"IF(Uncertainty!Z113=\"\",\"\",Uncertainty!Z113)","v":""},0,0]
[{"$f":"'ID-numbers'!$A619","v":"FT004a"},{"$f":"VLOOKUP(A489,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 1"},{"$f":"IF('Input Project'!H51=\"\",\"\",'Input Project'!H51)","v":""},"Diesel","","Diesel",null,"",{"$f":"IF($L489=1,IF($M489=\"\",$O489,$M489),\"\")","v":""},{"$f":"IF($L489=1,IF($N489=\"\",$P489,$N489),\"\")","v":""},{"$f":"IF($L489=1,($J489-$I489)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A620","v":"FT004b"},{"$f":"VLOOKUP(A490,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 2"},{"$f":"IF('Input Project'!H54=\"\",\"\",'Input Project'!H54)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A621","v":"FT004c"},{"$f":"VLOOKUP(A491,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 3"},{"$f":"IF('Input Project'!H57=\"\",\"\",'Input Project'!H57)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A622","v":"FT004d"},{"$f":"VLOOKUP(A492,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 4"},{"$f":"IF('Input Project'!H114=\"\",\"\",'Input Project'!H114)","v":""},"Diesel","","Diesel",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A623","v":"FT004e"},{"$f":"VLOOKUP(A493,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 5"},{"$f":"IF('Input Project'!H117=\"\",\"\",'Input Project'!H117)","v":""},"HFO for maritime transport","","HFO for maritime transport",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A624","v":"FT004f"},{"$f":"VLOOKUP(A494,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 6"},{"$f":"IF('Input Project'!H120=\"\",\"\",'Input Project'!H120)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,{"$f":"IF($L494=1,VLOOKUP($A494,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L494=1,VLOOKUP($A494,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A625","v":"FT004g"},{"$f":"VLOOKUP(A495,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 7"},{"$f":"IF('Input Project'!H166=\"\",\"\",'Input Project'!H166)","v":""},"Diesel","","Diesel",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A626","v":"FT004h"},{"$f":"VLOOKUP(A496,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 8"},{"$f":"IF('Input Project'!H169=\"\",\"\",'Input Project'!H169)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A627","v":"FT004i"},{"$f":"VLOOKUP(A497,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 9"},{"$f":"IF('Input Project'!H172=\"\",\"\",'Input Project'!H172)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A664","v":"FT009a"},{"$f":"VLOOKUP(A498,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 1"},null,null,"",null,{"$f":"VLOOKUP(A498,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":2217.5388571428571},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A665","v":"FT009b"},{"$f":"VLOOKUP(A499,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 2"},null,null,"",null,{"$f":"VLOOKUP(A499,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A666","v":"FT009c"},{"$f":"VLOOKUP(A500,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 3"},null,null,"",null,{"$f":"VLOOKUP(A500,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A667","v":"FT009d"},{"$f":"VLOOKUP(A501,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 4"},null,null,"",null,{"$f":"VLOOKUP(A501,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":740.99261129790364},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A668","v":"FT009e"},{"$f":"VLOOKUP(A502,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 5"},null,null,"",null,{"$f":"VLOOKUP(A502,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":5798.2589582664377},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A669","v":"FT009f"},{"$f":"VLOOKUP(A503,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 6"},null,null,"",null,{"$f":"VLOOKUP(A503,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A670","v":"FT009g"},{"$f":"VLOOKUP(A504,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 7"},null,null,"",null,{"$f":"VLOOKUP(A504,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":158.01883624428052},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A671","v":"FT009h"},{"$f":"VLOOKUP(A505,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 8"},null,null,"",null,{"$f":"VLOOKUP(A505,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A672","v":"FT009i"},{"$f":"VLOOKUP(A506,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 9"},null,null,"",null,{"$f":"VLOOKUP(A506,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A673","v":"FT010a"},{"$f":"VLOOKUP(A507,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 1"},null,null,"",null,{"$f":"VLOOKUP(A507,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3326.3082857142858},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A674","v":"FT010b"},{"$f":"VLOOKUP(A508,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 2"},null,null,"",null,{"$f":"VLOOKUP(A508,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A675","v":"FT010c"},{"$f":"VLOOKUP(A509,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 3"},null,null,"",null,{"$f":"VLOOKUP(A509,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A676","v":"FT010d"},{"$f":"VLOOKUP(A510,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 4"},null,null,"",null,{"$f":"VLOOKUP(A510,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":1111.4889169468554},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A677","v":"FT010e"},{"$f":"VLOOKUP(A511,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 5"},null,null,"",null,{"$f":"VLOOKUP(A511,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":8697.3884373996571},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A678","v":"FT010f"},{"$f":"VLOOKUP(A512,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 6"},null,null,"",null,{"$f":"VLOOKUP(A512,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A679","v":"FT010g"},{"$f":"VLOOKUP(A513,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 7"},null,null,"",null,{"$f":"VLOOKUP(A513,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":237.02825436642075},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A680","v":"FT010h"},{"$f":"VLOOKUP(A514,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 8"},null,null,"",null,{"$f":"VLOOKUP(A514,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A681","v":"FT010i"},{"$f":"VLOOKUP(A515,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 9"},null,null,"",null,{"$f":"VLOOKUP(A515,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A691","v":"FT012a"},{"$f":"VLOOKUP(A516,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport 1 (mode 1-2-3)"},null,null,"",null,{"$f":"VLOOKUP(A516,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":4.4348524663217689E-2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A692","v":"FT012b"},{"$f":"VLOOKUP(A517,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport 1 (mode 1-2-3)"},null,null,"",null,{"$f":"VLOOKUP(A517,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":6.6522786994826541E-2},"","","","",0,null,null,{"$f":"IF($L517=1,VLOOKUP($A517,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L517=1,VLOOKUP($A517,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A693","v":"FT013a"},{"$f":"VLOOKUP(A518,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport 2 (mode 4-5-6)"},null,null,"",null,{"$f":"VLOOKUP(A518,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.1307783891036127},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A694","v":"FT013b"},{"$f":"VLOOKUP(A519,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport 2 (mode 4-5-6)"},null,null,"",null,{"$f":"VLOOKUP(A519,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.19616758365541906},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A695","v":"FT014a"},{"$f":"VLOOKUP(A520,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport 3 (mode 7-8-9)"},null,null,"",null,{"$f":"VLOOKUP(A520,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.1602162162162164E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A696","v":"FT014b"},{"$f":"VLOOKUP(A521,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport 3 (mode 7-8-9)"},null,null,"",null,{"$f":"VLOOKUP(A521,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":4.7403243243243241E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A706","v":"FT020a"},{"$f":"VLOOKUP(A522,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 1"},null,null,"",null,{"$f":"VLOOKUP(A522,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":4.2427297465073593E-2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A707","v":"FT020b"},{"$f":"VLOOKUP(A523,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 1"},null,null,"",null,{"$f":"VLOOKUP(A523,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":6.364094619761039E-2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A708","v":"FT021a"},{"$f":"VLOOKUP(A524,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 1"},null,null,"",null,{"$f":"VLOOKUP(A524,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":4.2427297465073593E-2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A709","v":"FT021b"},{"$f":"VLOOKUP(A525,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 1"},null,null,"",null,{"$f":"VLOOKUP(A525,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":6.364094619761039E-2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A710","v":"FT022a"},{"$f":"VLOOKUP(A526,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 2"},null,null,"",null,{"$f":"VLOOKUP(A526,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.1307783891036127},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A711","v":"FT022b"},{"$f":"VLOOKUP(A527,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 2"},null,null,"",null,{"$f":"VLOOKUP(A527,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.19616758365541906},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A712","v":"FT023a"},{"$f":"VLOOKUP(A528,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 2"},null,null,"",null,{"$f":"VLOOKUP(A528,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.1307783891036127},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A713","v":"FT023b"},{"$f":"VLOOKUP(A529,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 2"},null,null,"",null,{"$f":"VLOOKUP(A529,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.19616758365541906},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A714","v":"FT024a"},{"$f":"VLOOKUP(A530,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 3"},null,null,"",null,{"$f":"VLOOKUP(A530,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.1602162162162164E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A715","v":"FT024b"},{"$f":"VLOOKUP(A531,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 3"},null,null,"",null,{"$f":"VLOOKUP(A531,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":4.7403243243243241E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A716","v":"FT025a"},{"$f":"VLOOKUP(A532,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 3"},null,null,"",null,{"$f":"VLOOKUP(A532,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.1602162162162164E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A717","v":"FT025b"},{"$f":"VLOOKUP(A533,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 3"},null,null,"",null,{"$f":"VLOOKUP(A533,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":4.7403243243243241E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A718","v":"FT026a"},{"$f":"VLOOKUP(A534,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A534,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.1763659027849025},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A719","v":"FT026b"},{"$f":"VLOOKUP(A535,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A535,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.26454885417735374},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A720","v":"FT027a"},{"$f":"VLOOKUP(A536,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A536,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.1763659027849025},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A721","v":"FT027b"},{"$f":"VLOOKUP(A537,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A537,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.26454885417735374},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A722","v":"FT030a"},{"$f":"VLOOKUP(A538,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 1"},null,null,"",null,{"$f":"VLOOKUP(A538,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.2054148348253646},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A723","v":"FT030b"},{"$f":"VLOOKUP(A539,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 1"},null,null,"",null,{"$f":"VLOOKUP(A539,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.2054148348253646},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A724","v":"FT031a"},{"$f":"VLOOKUP(A540,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 2"},null,null,"",null,{"$f":"VLOOKUP(A540,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":10.41339032758632},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A725","v":"FT031b"},{"$f":"VLOOKUP(A541,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 2"},null,null,"",null,{"$f":"VLOOKUP(A541,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":10.41339032758632},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A726","v":"FT032a"},{"$f":"VLOOKUP(A542,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 3"},null,null,"",null,{"$f":"VLOOKUP(A542,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.23875675675675681},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A727","v":"FT032b"},{"$f":"VLOOKUP(A543,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 3"},null,null,{"$f":"IF(MonteCarlo=1,IF($L543=1,IF($H543=\"n.a.\",0,IF($H543<0.009,0,MIN(MAX(NORMINV(RAND(),$H543,$K543),$I543),$J543))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A543,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.23875675675675681},{"$f":"IF($L543=1,IF($C543=\"\",$D543,$C543),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A728","v":"FT033a"},{"$f":"VLOOKUP(A544,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A544,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":13.857561919168443},"",{"$f":"IF($L544=1,IF($M544=\"\",$O544,$M544),\"\")","v":""},{"$f":"IF($L544=1,IF($N544=\"\",$P544,$N544),\"\")","v":""},{"$f":"IF($L544=1,($J544-$I544)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A729","v":"FT033b"},{"$f":"VLOOKUP(A545,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A545,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":13.857561919168443},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A766","v":"FT040a"},{"$f":"VLOOKUP(A546,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 1"},null,null,null,null,{"$f":"VLOOKUP(A546,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.5353642870465642E-2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A767","v":"FT040b"},{"$f":"VLOOKUP(A547,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 1"},null,null,null,null,{"$f":"VLOOKUP(A547,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.5353642870465642E-2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A768","v":"FT041a"},{"$f":"VLOOKUP(A548,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 2"},null,null,null,null,{"$f":"VLOOKUP(A548,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.11536884766037943},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A769","v":"FT041b"},{"$f":"VLOOKUP(A549,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 2"},null,null,null,null,{"$f":"VLOOKUP(A549,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.11536884766037943},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A770","v":"FT042a"},{"$f":"VLOOKUP(A550,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 3"},null,null,null,null,{"$f":"VLOOKUP(A550,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":2.633331891891892E-3},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A771","v":"FT042b"},{"$f":"VLOOKUP(A551,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 3"},null,null,null,null,{"$f":"VLOOKUP(A551,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":2.633331891891892E-3},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A772","v":"FT043a"},{"$f":"VLOOKUP(A552,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from total transport (1-3)"},null,null,null,null,{"$f":"VLOOKUP(A552,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.15335582242273696},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A773","v":"FT043b"},{"$f":"VLOOKUP(A553,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from total transport (1-3)"},null,null,null,null,{"$f":"VLOOKUP(A553,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":0.15335582242273696},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A774","v":"FT044a"},{"$f":"VLOOKUP(A554,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 1"},null,null,null,null,{"$f":"VLOOKUP(A554,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":4.2222476029035319E-3},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A775","v":"FT044b"},{"$f":"VLOOKUP(A555,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 1"},null,null,null,null,{"$f":"VLOOKUP(A555,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":4.2222476029035319E-3},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A776","v":"FT045a"},{"$f":"VLOOKUP(A556,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 2"},null,null,null,null,{"$f":"VLOOKUP(A556,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":1.3778377585261953E-2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A777","v":"FT045b"},{"$f":"VLOOKUP(A557,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 2"},null,null,null,null,{"$f":"VLOOKUP(A557,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":1.3778377585261953E-2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A778","v":"FT046a"},{"$f":"VLOOKUP(A558,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 3"},null,null,null,null,{"$f":"VLOOKUP(A558,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.1449600000000005E-4},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A779","v":"FT046b"},{"$f":"VLOOKUP(A559,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 3"},null,null,null,null,{"$f":"VLOOKUP(A559,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":3.144960000000001E-4},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A780","v":"FT047a"},{"$f":"VLOOKUP(A560,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from total transport (1-3)"},null,null,null,null,{"$f":"VLOOKUP(A560,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":1.8315121188165487E-2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A781","v":"FT047b"},{"$f":"VLOOKUP(A561,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from total transport (1-3)"},null,null,null,null,{"$f":"VLOOKUP(A561,'Transport feedstock1'!$D$9:$G$5019,4,FALSE)","v":1.8315121188165487E-2},null,null,null,null,0]
[null,null,null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A784","v":"FT501a"},{"$f":"VLOOKUP(A563,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 1"},{"$f":"IF('Input Project'!H202=\"\",\"\",'Input Project'!H202)","v":""},{"$f":"VLOOKUP($A563,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L563=1,IF(MonteCarlo=1,$E563,IF($C563=\"\",$D563,$C563)),IF($C563=\"\",$D563,$C563))","v":"n.a."},null,"","","","",0,null,null,{"$f":"IF($L563=1,VLOOKUP($A563,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L563=1,VLOOKUP($A563,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A785","v":"FT501b"},{"$f":"VLOOKUP(A564,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 2"},{"$f":"IF('Input Project'!H205=\"\",\"\",'Input Project'!H205)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A786","v":"FT501c"},{"$f":"VLOOKUP(A565,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 3"},{"$f":"IF('Input Project'!H208=\"\",\"\",'Input Project'!H208)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A787","v":"FT501d"},{"$f":"VLOOKUP(A566,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 4"},{"$f":"IF('Input Project'!H265=\"\",\"\",'Input Project'!H265)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A788","v":"FT501e"},{"$f":"VLOOKUP(A567,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 5"},{"$f":"IF('Input Project'!H268=\"\",\"\",'Input Project'!H268)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A789","v":"FT501f"},{"$f":"VLOOKUP(A568,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 6"},{"$f":"IF('Input Project'!H271=\"\",\"\",'Input Project'!H271)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A790","v":"FT501g"},{"$f":"VLOOKUP(A569,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 7"},{"$f":"IF('Input Project'!H317=\"\",\"\",'Input Project'!H317)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A791","v":"FT501h"},{"$f":"VLOOKUP(A570,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 8"},{"$f":"IF('Input Project'!H320=\"\",\"\",'Input Project'!H320)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A792","v":"FT501i"},{"$f":"VLOOKUP(A571,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Transport mode 9"},{"$f":"IF('Input Project'!H323=\"\",\"\",'Input Project'!H323)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A793","v":"FT502a"},{"$f":"VLOOKUP(A572,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 1"},null,null,"",null,{"$f":"VLOOKUP(A572,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A794","v":"FT502b"},{"$f":"VLOOKUP(A573,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 2"},null,null,"",null,{"$f":"VLOOKUP(A573,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A795","v":"FT502c"},{"$f":"VLOOKUP(A574,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 3"},null,null,"",null,{"$f":"VLOOKUP(A574,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A796","v":"FT502d"},{"$f":"VLOOKUP(A575,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 4"},null,null,"",null,{"$f":"VLOOKUP(A575,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A797","v":"FT502e"},{"$f":"VLOOKUP(A576,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 5"},null,null,"",null,{"$f":"VLOOKUP(A576,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A798","v":"FT502f"},{"$f":"VLOOKUP(A577,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 6"},null,null,"",null,{"$f":"VLOOKUP(A577,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A799","v":"FT502g"},{"$f":"VLOOKUP(A578,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 7"},null,null,"",null,{"$f":"VLOOKUP(A578,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A800","v":"FT502h"},{"$f":"VLOOKUP(A579,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 8"},null,null,"",null,{"$f":"VLOOKUP(A579,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A801","v":"FT502i"},{"$f":"VLOOKUP(A580,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of transport mode 9"},null,null,"",null,{"$f":"VLOOKUP(A580,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A802","v":"FT503a"},{"$f":"VLOOKUP(A581,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 1"},{"$f":"IF('Input Project'!H203=\"\",\"\",'Input Project'!H203)","v":""},{"$f":"VLOOKUP($A581,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L581=1,IF(MonteCarlo=1,$E581,IF($C581=\"\",$D581,$C581)),IF($C581=\"\",$D581,$C581))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W146=\"\",\"\",Uncertainty!W146)","v":""},{"$f":"IF(Uncertainty!Z146=\"\",\"\",Uncertainty!Z146)","v":""},0,0]
[{"$f":"'ID-numbers'!$A803","v":"FT503b"},{"$f":"VLOOKUP(A582,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 2"},{"$f":"IF('Input Project'!H206=\"\",\"\",'Input Project'!H206)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W147=\"\",\"\",Uncertainty!W147)","v":""},{"$f":"IF(Uncertainty!Z147=\"\",\"\",Uncertainty!Z147)","v":""},0,0]
[{"$f":"'ID-numbers'!$A804","v":"FT503c"},{"$f":"VLOOKUP(A583,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 3"},{"$f":"IF('Input Project'!H209=\"\",\"\",'Input Project'!H209)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W148=\"\",\"\",Uncertainty!W148)","v":""},{"$f":"IF(Uncertainty!Z148=\"\",\"\",Uncertainty!Z148)","v":""},0,0]
[{"$f":"'ID-numbers'!$A805","v":"FT503d"},{"$f":"VLOOKUP(A584,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 4"},{"$f":"IF('Input Project'!H266=\"\",\"\",'Input Project'!H266)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W175=\"\",\"\",Uncertainty!W175)","v":""},{"$f":"IF(Uncertainty!Z175=\"\",\"\",Uncertainty!Z175)","v":""},0,0]
[{"$f":"'ID-numbers'!$A806","v":"FT503e"},{"$f":"VLOOKUP(A585,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 5"},{"$f":"IF('Input Project'!H269=\"\",\"\",'Input Project'!H269)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W176=\"\",\"\",Uncertainty!W176)","v":""},{"$f":"IF(Uncertainty!Z176=\"\",\"\",Uncertainty!Z176)","v":""},0,0]
[{"$f":"'ID-numbers'!$A807","v":"FT503f"},{"$f":"VLOOKUP(A586,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 6"},{"$f":"IF('Input Project'!H272=\"\",\"\",'Input Project'!H272)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W177=\"\",\"\",Uncertainty!W177)","v":""},{"$f":"IF(Uncertainty!Z177=\"\",\"\",Uncertainty!Z177)","v":""},0,0]
[{"$f":"'ID-numbers'!$A808","v":"FT503g"},{"$f":"VLOOKUP(A587,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 7"},{"$f":"IF('Input Project'!H318=\"\",\"\",'Input Project'!H318)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W204=\"\",\"\",Uncertainty!W204)","v":""},{"$f":"IF(Uncertainty!Z204=\"\",\"\",Uncertainty!Z204)","v":""},0,0]
[{"$f":"'ID-numbers'!$A809","v":"FT503h"},{"$f":"VLOOKUP(A588,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 8"},{"$f":"IF('Input Project'!H321=\"\",\"\",'Input Project'!H321)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W205=\"\",\"\",Uncertainty!W205)","v":""},{"$f":"IF(Uncertainty!Z205=\"\",\"\",Uncertainty!Z205)","v":""},0,0]
[{"$f":"'ID-numbers'!$A810","v":"FT503i"},{"$f":"VLOOKUP(A589,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Distance of transport mode 9"},{"$f":"IF('Input Project'!H324=\"\",\"\",'Input Project'!H324)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W206=\"\",\"\",Uncertainty!W206)","v":""},{"$f":"IF(Uncertainty!Z206=\"\",\"\",Uncertainty!Z206)","v":""},0,0]
[{"$f":"'ID-numbers'!$A811","v":"FT504a"},{"$f":"VLOOKUP(A590,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 1"},{"$f":"IF('Input Project'!H204=\"\",\"\",'Input Project'!H204)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A812","v":"FT504b"},{"$f":"VLOOKUP(A591,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 2"},{"$f":"IF('Input Project'!H207=\"\",\"\",'Input Project'!H207)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A813","v":"FT504c"},{"$f":"VLOOKUP(A592,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 3"},{"$f":"IF('Input Project'!H210=\"\",\"\",'Input Project'!H210)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A814","v":"FT504d"},{"$f":"VLOOKUP(A593,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 4"},{"$f":"IF('Input Project'!H267=\"\",\"\",'Input Project'!H267)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A815","v":"FT504e"},{"$f":"VLOOKUP(A594,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 5"},{"$f":"IF('Input Project'!H270=\"\",\"\",'Input Project'!H270)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A816","v":"FT504f"},{"$f":"VLOOKUP(A595,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 6"},{"$f":"IF('Input Project'!H273=\"\",\"\",'Input Project'!H273)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,{"$f":"IF($L595=1,VLOOKUP($A595,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L595=1,VLOOKUP($A595,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A817","v":"FT504g"},{"$f":"VLOOKUP(A596,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 7"},{"$f":"IF('Input Project'!H319=\"\",\"\",'Input Project'!H319)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A818","v":"FT504h"},{"$f":"VLOOKUP(A597,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 8"},{"$f":"IF('Input Project'!H322=\"\",\"\",'Input Project'!H322)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A819","v":"FT504i"},{"$f":"VLOOKUP(A598,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel used for transport mode 9"},{"$f":"IF('Input Project'!H325=\"\",\"\",'Input Project'!H325)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A856","v":"FT509a"},{"$f":"VLOOKUP(A599,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 1"},null,null,"",null,{"$f":"VLOOKUP(A599,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A857","v":"FT509b"},{"$f":"VLOOKUP(A600,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 2"},null,null,"",null,{"$f":"VLOOKUP(A600,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A858","v":"FT509c"},{"$f":"VLOOKUP(A601,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 3"},null,null,"",null,{"$f":"VLOOKUP(A601,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A859","v":"FT509d"},{"$f":"VLOOKUP(A602,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 4"},null,null,"",null,{"$f":"VLOOKUP(A602,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A860","v":"FT509e"},{"$f":"VLOOKUP(A603,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 5"},null,null,"",null,{"$f":"VLOOKUP(A603,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A861","v":"FT509f"},{"$f":"VLOOKUP(A604,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 6"},null,null,"",null,{"$f":"VLOOKUP(A604,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A862","v":"FT509g"},{"$f":"VLOOKUP(A605,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 7"},null,null,"",null,{"$f":"VLOOKUP(A605,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A863","v":"FT509h"},{"$f":"VLOOKUP(A606,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 8"},null,null,"",null,{"$f":"VLOOKUP(A606,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A864","v":"FT509i"},{"$f":"VLOOKUP(A607,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport mode 9"},null,null,"",null,{"$f":"VLOOKUP(A607,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A865","v":"FT510a"},{"$f":"VLOOKUP(A608,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 1"},null,null,"",null,{"$f":"VLOOKUP(A608,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A866","v":"FT510b"},{"$f":"VLOOKUP(A609,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 2"},null,null,"",null,{"$f":"VLOOKUP(A609,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A867","v":"FT510c"},{"$f":"VLOOKUP(A610,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 3"},null,null,"",null,{"$f":"VLOOKUP(A610,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A868","v":"FT510d"},{"$f":"VLOOKUP(A611,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 4"},null,null,"",null,{"$f":"VLOOKUP(A611,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A869","v":"FT510e"},{"$f":"VLOOKUP(A612,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 5"},null,null,"",null,{"$f":"VLOOKUP(A612,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A870","v":"FT510f"},{"$f":"VLOOKUP(A613,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 6"},null,null,"",null,{"$f":"VLOOKUP(A613,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A871","v":"FT510g"},{"$f":"VLOOKUP(A614,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 7"},null,null,"",null,{"$f":"VLOOKUP(A614,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A872","v":"FT510h"},{"$f":"VLOOKUP(A615,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 8"},null,null,"",null,{"$f":"VLOOKUP(A615,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A873","v":"FT510i"},{"$f":"VLOOKUP(A616,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport mode 9"},null,null,"",null,{"$f":"VLOOKUP(A616,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A883","v":"FT512a"},{"$f":"VLOOKUP(A617,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport 1 (mode 1-2-3)"},null,null,{"$f":"IF(MonteCarlo=1,IF($L617=1,IF($H617=\"n.a.\",0,IF($H617<0.009,0,MIN(MAX(NORMINV(RAND(),$H617,$K617),$I617),$J617))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A617,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},{"$f":"IF($L617=1,IF($C617=\"\",$D617,$C617),\"\")","v":""},{"$f":"IF($L617=1,IF($M617=\"\",$O617,$M617),\"\")","v":""},{"$f":"IF($L617=1,IF($N617=\"\",$P617,$N617),\"\")","v":""},{"$f":"IF($L617=1,($J617-$I617)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A884","v":"FT512b"},{"$f":"VLOOKUP(A618,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport 1 (mode 1-2-3)"},null,null,"",null,{"$f":"VLOOKUP(A618,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,{"$f":"IF($L618=1,VLOOKUP($A618,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L618=1,VLOOKUP($A618,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A885","v":"FT513a"},{"$f":"VLOOKUP(A619,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport 2 (mode 4-5-6)"},null,null,"",null,{"$f":"VLOOKUP(A619,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A886","v":"FT513b"},{"$f":"VLOOKUP(A620,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport 2 (mode 4-5-6)"},null,null,"",null,{"$f":"VLOOKUP(A620,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A887","v":"FT514a"},{"$f":"VLOOKUP(A621,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for transport 3 (mode 7-8-9)"},null,null,"",null,{"$f":"VLOOKUP(A621,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A888","v":"FT514b"},{"$f":"VLOOKUP(A622,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for transport 3 (mode 7-8-9)"},null,null,"",null,{"$f":"VLOOKUP(A622,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A898","v":"FT520a"},{"$f":"VLOOKUP(A623,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 1"},null,null,"",null,{"$f":"VLOOKUP(A623,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A899","v":"FT520b"},{"$f":"VLOOKUP(A624,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 1"},null,null,"",null,{"$f":"VLOOKUP(A624,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A900","v":"FT521a"},{"$f":"VLOOKUP(A625,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 1"},null,null,"",null,{"$f":"VLOOKUP(A625,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A901","v":"FT521b"},{"$f":"VLOOKUP(A626,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 1"},null,null,"",null,{"$f":"VLOOKUP(A626,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A902","v":"FT522a"},{"$f":"VLOOKUP(A627,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 2"},null,null,"",null,{"$f":"VLOOKUP(A627,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A903","v":"FT522b"},{"$f":"VLOOKUP(A628,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 2"},null,null,"",null,{"$f":"VLOOKUP(A628,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A904","v":"FT523a"},{"$f":"VLOOKUP(A629,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 2"},null,null,"",null,{"$f":"VLOOKUP(A629,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A905","v":"FT523b"},{"$f":"VLOOKUP(A630,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 2"},null,null,"",null,{"$f":"VLOOKUP(A630,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A906","v":"FT524a"},{"$f":"VLOOKUP(A631,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 3"},null,null,"",null,{"$f":"VLOOKUP(A631,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A907","v":"FT524b"},{"$f":"VLOOKUP(A632,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 3"},null,null,"",null,{"$f":"VLOOKUP(A632,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A908","v":"FT525a"},{"$f":"VLOOKUP(A633,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 3"},null,null,"",null,{"$f":"VLOOKUP(A633,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A909","v":"FT525b"},{"$f":"VLOOKUP(A634,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in transport 3"},null,null,"",null,{"$f":"VLOOKUP(A634,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A910","v":"FT526a"},{"$f":"VLOOKUP(A635,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A635,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A911","v":"FT526b"},{"$f":"VLOOKUP(A636,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A636,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A912","v":"FT527a"},{"$f":"VLOOKUP(A637,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A637,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A913","v":"FT527b"},{"$f":"VLOOKUP(A638,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A638,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A914","v":"FT530a"},{"$f":"VLOOKUP(A639,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 1"},null,null,"",null,{"$f":"VLOOKUP(A639,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A915","v":"FT530b"},{"$f":"VLOOKUP(A640,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 1"},null,null,"",null,{"$f":"VLOOKUP(A640,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A916","v":"FT531a"},{"$f":"VLOOKUP(A641,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 2"},null,null,"",null,{"$f":"VLOOKUP(A641,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A917","v":"FT531b"},{"$f":"VLOOKUP(A642,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 2"},null,null,"",null,{"$f":"VLOOKUP(A642,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A918","v":"FT532a"},{"$f":"VLOOKUP(A643,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 3"},null,null,"",null,{"$f":"VLOOKUP(A643,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A919","v":"FT532b"},{"$f":"VLOOKUP(A644,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from transport 3"},null,null,"",null,{"$f":"VLOOKUP(A644,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A920","v":"FT533a"},{"$f":"VLOOKUP(A645,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A645,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A921","v":"FT533b"},{"$f":"VLOOKUP(A646,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from total transport (1-3)"},null,null,"",null,{"$f":"VLOOKUP(A646,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A958","v":"FT540a"},{"$f":"VLOOKUP(A647,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 1"},null,null,null,null,{"$f":"VLOOKUP(A647,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A959","v":"FT540b"},{"$f":"VLOOKUP(A648,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 1"},null,null,null,null,{"$f":"VLOOKUP(A648,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A960","v":"FT541a"},{"$f":"VLOOKUP(A649,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 2"},null,null,null,null,{"$f":"VLOOKUP(A649,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A961","v":"FT541b"},{"$f":"VLOOKUP(A650,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 2"},null,null,null,null,{"$f":"VLOOKUP(A650,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A962","v":"FT542a"},{"$f":"VLOOKUP(A651,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 3"},null,null,null,null,{"$f":"VLOOKUP(A651,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A963","v":"FT542b"},{"$f":"VLOOKUP(A652,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from transport 3"},null,null,null,null,{"$f":"VLOOKUP(A652,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A964","v":"FT543a"},{"$f":"VLOOKUP(A653,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from total transport (1-3)"},null,null,null,null,{"$f":"VLOOKUP(A653,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A965","v":"FT543b"},{"$f":"VLOOKUP(A654,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from total transport (1-3)"},null,null,null,null,{"$f":"VLOOKUP(A654,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A966","v":"FT544a"},{"$f":"VLOOKUP(A655,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 1"},null,null,null,null,{"$f":"VLOOKUP(A655,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A967","v":"FT544b"},{"$f":"VLOOKUP(A656,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 1"},null,null,null,null,{"$f":"VLOOKUP(A656,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A968","v":"FT545a"},{"$f":"VLOOKUP(A657,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 2"},null,null,null,null,{"$f":"VLOOKUP(A657,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A969","v":"FT545b"},{"$f":"VLOOKUP(A658,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 2"},null,null,null,null,{"$f":"VLOOKUP(A658,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A970","v":"FT546a"},{"$f":"VLOOKUP(A659,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 3"},null,null,null,null,{"$f":"VLOOKUP(A659,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A971","v":"FT546b"},{"$f":"VLOOKUP(A660,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from transport 3"},null,null,null,null,{"$f":"VLOOKUP(A660,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A972","v":"FT547a"},{"$f":"VLOOKUP(A661,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from total transport (1-3)"},null,null,null,null,{"$f":"VLOOKUP(A661,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A973","v":"FT547b"},{"$f":"VLOOKUP(A662,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from total transport (1-3)"},null,null,null,null,{"$f":"VLOOKUP(A662,'Transport feedstock2'!$D$9:$G$5077,4,FALSE)","v":0},null,null,null,null,0]
[null,null,null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A976","v":"BC000a"},{"$f":"'ID-numbers'!$A976","v":"BC000a"},null,{"$f":"VLOOKUP($A664,list_database1,$I$8,FALSE)","v":"Oil extraction"},"",{"$f":"IF($L664=1,IF(MonteCarlo=1,$E664,IF($C664=\"\",$D664,$C664)),IF($C664=\"\",$D664,$C664))","v":"Oil extraction"},null,"","","","",0,null,null,{"$f":"IF($L664=1,VLOOKUP($A664,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L664=1,VLOOKUP($A664,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A977","v":"BC000b"},{"$f":"VLOOKUP(A665,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Process 2 description "},null,"Refining","","Refining",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A978","v":"BC001a"},{"$f":"VLOOKUP(A666,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of main output flow, process 1"},{"$f":"IF('Input Project'!H61=\"\",\"\",'Input Project'!H61)","v":"Crude palm oil"},"Crude palm oil","","Crude palm oil",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A979","v":"BC001b"},{"$f":"VLOOKUP(A667,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of main output flow, process 2"},{"$f":"IF('Input Project'!H124=\"\",\"\",'Input Project'!H124)","v":"Palm stearin"},"Palm stearin","","Palm stearin",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A980","v":"BC002a1"},{"$f":"VLOOKUP(A668,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 1, process 1"},{"$f":"IF('Input Project'!H62=\"\",\"\",'Input Project'!H62)","v":""},"Palm kernel meal","","Palm kernel meal",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A981","v":"BC002a10"},{"$f":"VLOOKUP(A669,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 1, process 1"},{"$f":"IF('Input Project'!H63=\"\",\"\",'Input Project'!H63)","v":""},8.1999999999999993,null,8.1999999999999993,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A982","v":"BC002a11"},{"$f":"VLOOKUP(A670,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 1, process 1"},{"$f":"IF('Input Project'!H64=\"\",\"\",'Input Project'!H64)","v":""},462.83,{"$f":"IF(MonteCarlo=1,IF($L670=1,IF($H670=\"n.a.\",0,IF($H670<0.009,0,MIN(MAX(NORMINV(RAND(),$H670,$K670),$I670),$J670))),\"\"),\"\")","v":""},462.83,null,{"$f":"IF($L670=1,IF($C670=\"\",$D670,$C670),\"\")","v":462.83},{"$f":"IF($L670=1,IF($M670=\"\",$O670,$M670),\"\")","v":0},{"$f":"IF($L670=1,IF($N670=\"\",$P670,$N670),\"\")","v":0},{"$f":"IF($L670=1,($J670-$I670)/6,\"\")","v":0},1,null,null,0,0]
[{"$f":"'ID-numbers'!$A983","v":"BC002a2"},{"$f":"VLOOKUP(A671,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 2, process 1"},{"$f":"IF('Input Project'!H66=\"\",\"\",'Input Project'!H66)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A984","v":"BC002a20"},{"$f":"VLOOKUP(A672,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 2, process 1"},{"$f":"IF('Input Project'!H67=\"\",\"\",'Input Project'!H67)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A985","v":"BC002a21"},{"$f":"VLOOKUP(A673,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 2, process 1"},{"$f":"IF('Input Project'!H68=\"\",\"\",'Input Project'!H68)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L673=1,IF($H673=\"n.a.\",0,IF($H673<0.009,0,MIN(MAX(NORMINV(RAND(),$H673,$K673),$I673),$J673))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L673=1,IF($C673=\"\",$D673,$C673),\"\")","v":0},{"$f":"IF($L673=1,IF($M673=\"\",$O673,$M673),\"\")","v":0},{"$f":"IF($L673=1,IF($N673=\"\",$P673,$N673),\"\")","v":0},{"$f":"IF($L673=1,($J673-$I673)/6,\"\")","v":0},1,null,null,0,0]
[{"$f":"'ID-numbers'!$A986","v":"BC002a3"},{"$f":"VLOOKUP(A674,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 3, process 1"},{"$f":"IF('Input Project'!H70=\"\",\"\",'Input Project'!H70)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A987","v":"BC002a30"},{"$f":"VLOOKUP(A675,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 3, process 1"},{"$f":"IF('Input Project'!H71=\"\",\"\",'Input Project'!H71)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A988","v":"BC002a31"},{"$f":"VLOOKUP(A676,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 3, process 1"},{"$f":"IF('Input Project'!H72=\"\",\"\",'Input Project'!H72)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L676=1,IF($H676=\"n.a.\",0,IF($H676<0.009,0,MIN(MAX(NORMINV(RAND(),$H676,$K676),$I676),$J676))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L676=1,IF($C676=\"\",$D676,$C676),\"\")","v":0},{"$f":"IF($L676=1,IF($M676=\"\",$O676,$M676),\"\")","v":0},{"$f":"IF($L676=1,IF($N676=\"\",$P676,$N676),\"\")","v":0},{"$f":"IF($L676=1,($J676-$I676)/6,\"\")","v":0},1,null,null,0,0]
[{"$f":"'ID-numbers'!$A989","v":"BC002a41"},{"$f":"VLOOKUP(A677,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity by-product, process 1"},{"$f":"IF('Input Project'!H74=\"\",\"\",'Input Project'!H74)","v":""},0,"",0,null,{"$f":"IF($L677=1,IF($C677=\"\",$D677,$C677),\"\")","v":0},0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A990","v":"BC002a51"},{"$f":"VLOOKUP(A678,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat by-product, process 1"},{"$f":"IF('Input Project'!H75=\"\",\"\",'Input Project'!H75)","v":""},0,"",0,null,{"$f":"IF($L678=1,IF($C678=\"\",$D678,$C678),\"\")","v":0},0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A991","v":"BC002b1"},{"$f":"VLOOKUP(A679,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 1, process 2"},{"$f":"IF('Input Project'!H125=\"\",\"\",'Input Project'!H125)","v":""},"Palm olein","","Palm olein",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A992","v":"BC002b10"},{"$f":"VLOOKUP(A680,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 1, process 2"},{"$f":"IF('Input Project'!H126=\"\",\"\",'Input Project'!H126)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A993","v":"BC002b11"},{"$f":"VLOOKUP(A681,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 1, process 2"},{"$f":"IF('Input Project'!H127=\"\",\"\",'Input Project'!H127)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L681=1,IF($H681=\"n.a.\",0,IF($H681<0.009,0,MIN(MAX(NORMINV(RAND(),$H681,$K681),$I681),$J681))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L681=1,IF($C681=\"\",$D681,$C681),\"\")","v":0},{"$f":"IF($L681=1,IF($M681=\"\",$O681,$M681),\"\")","v":0},{"$f":"IF($L681=1,IF($N681=\"\",$P681,$N681),\"\")","v":0},{"$f":"IF($L681=1,($J681-$I681)/6,\"\")","v":0},1,null,null,0,0]
[{"$f":"'ID-numbers'!$A994","v":"BC002b2"},{"$f":"VLOOKUP(A682,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 2, process 2"},{"$f":"IF('Input Project'!H129=\"\",\"\",'Input Project'!H129)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A995","v":"BC002b20"},{"$f":"VLOOKUP(A683,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 2, process 2"},{"$f":"IF('Input Project'!H130=\"\",\"\",'Input Project'!H130)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A996","v":"BC002b21"},{"$f":"VLOOKUP(A684,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 2, process 2"},{"$f":"IF('Input Project'!H131=\"\",\"\",'Input Project'!H131)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L684=1,IF($H684=\"n.a.\",0,IF($H684<0.009,0,MIN(MAX(NORMINV(RAND(),$H684,$K684),$I684),$J684))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L684=1,IF($C684=\"\",$D684,$C684),\"\")","v":0},{"$f":"IF($L684=1,IF($M684=\"\",$O684,$M684),\"\")","v":0},{"$f":"IF($L684=1,IF($N684=\"\",$P684,$N684),\"\")","v":0},{"$f":"IF($L684=1,($J684-$I684)/6,\"\")","v":0},1,null,null,0,0]
[{"$f":"'ID-numbers'!$A997","v":"BC002b41"},{"$f":"VLOOKUP(A685,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity by-product, process 2"},{"$f":"IF('Input Project'!H133=\"\",\"\",'Input Project'!H133)","v":""},0,"",0,null,{"$f":"IF($L685=1,IF($C685=\"\",$D685,$C685),\"\")","v":0},0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A998","v":"BC002b51"},{"$f":"VLOOKUP(A686,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat by-product, process 2"},{"$f":"IF('Input Project'!H134=\"\",\"\",'Input Project'!H134)","v":""},0,"",0,null,{"$f":"IF($L686=1,IF($C686=\"\",$D686,$C686),\"\")","v":0},0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A999","v":"BC003a1"},{"$f":"VLOOKUP(A687,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (kg)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1000","v":"BC003a2"},{"$f":"VLOOKUP(A688,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (kg)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1001","v":"BC003a3"},{"$f":"VLOOKUP(A689,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (kg)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1002","v":"BC003b1"},{"$f":"VLOOKUP(A690,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (kg)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1003","v":"BC003b2"},{"$f":"VLOOKUP(A691,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (kg)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1004","v":"BC004a1"},{"$f":"VLOOKUP(A692,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (MJ)"},null,2.399961774322297E-2,"",{"$f":"IF($L692=1,IF(MonteCarlo=1,$E692,IF($C692=\"\",$D692,$C692)),IF($C692=\"\",$D692,$C692))","v":2.399961774322297E-2},null,2.399961774322297E-2,1.7999999999999999E-2,2.1999999999999999E-2,6.6666666666666664E-4,1,{"$f":"IF(Uncertainty!W60=\"\",\"\",Uncertainty!W60)","v":""},{"$f":"IF(Uncertainty!Z60=\"\",\"\",Uncertainty!Z60)","v":""},1.7999999999999999E-2,2.1999999999999999E-2]
[{"$f":"'ID-numbers'!$A1005","v":"BC004a2"},{"$f":"VLOOKUP(A693,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (MJ)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W61=\"\",\"\",Uncertainty!W61)","v":""},{"$f":"IF(Uncertainty!Z61=\"\",\"\",Uncertainty!Z61)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1006","v":"BC004a3"},{"$f":"VLOOKUP(A694,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (MJ)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W62=\"\",\"\",Uncertainty!W62)","v":""},{"$f":"IF(Uncertainty!Z62=\"\",\"\",Uncertainty!Z62)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1007","v":"BC004a4"},{"$f":"VLOOKUP(A695,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of electricity by-product, process 1 (MJ)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W63=\"\",\"\",Uncertainty!W63)","v":""},{"$f":"IF(Uncertainty!Z63=\"\",\"\",Uncertainty!Z63)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1008","v":"BC004a5"},{"$f":"VLOOKUP(A696,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of heat by-product, process 1 (MJ)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W64=\"\",\"\",Uncertainty!W64)","v":""},{"$f":"IF(Uncertainty!Z64=\"\",\"\",Uncertainty!Z64)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1009","v":"BC004b1"},{"$f":"VLOOKUP(A697,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (MJ)"},null,0,"",0,null,0,0.6,0.7,1.6666666666666663E-2,1,{"$f":"IF(Uncertainty!W89=\"\",\"\",Uncertainty!W89)","v":""},{"$f":"IF(Uncertainty!Z89=\"\",\"\",Uncertainty!Z89)","v":""},0.6,0.7]
[{"$f":"'ID-numbers'!$A1010","v":"BC004b2"},{"$f":"VLOOKUP(A698,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (MJ)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W90=\"\",\"\",Uncertainty!W90)","v":""},{"$f":"IF(Uncertainty!Z90=\"\",\"\",Uncertainty!Z90)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1011","v":"BC004b4"},{"$f":"VLOOKUP(A699,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of electricity by-product, process 2 (MJ)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W91=\"\",\"\",Uncertainty!W91)","v":""},{"$f":"IF(Uncertainty!Z91=\"\",\"\",Uncertainty!Z91)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1012","v":"BC004b5"},{"$f":"VLOOKUP(A700,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of heat by-product, process 2 (MJ)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W92=\"\",\"\",Uncertainty!W92)","v":""},{"$f":"IF(Uncertainty!Z92=\"\",\"\",Uncertainty!Z92)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1013","v":"BC005a1"},{"$f":"VLOOKUP(A701,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 1, process 1 (LHV)"},{"$f":"IF('Input Project'!H65=\"\",\"\",'Input Project'!H65)","v":""},17,"",17,null,"","","","",0,{"$f":"IF(Uncertainty!W91=\"\",\"\",Uncertainty!W91)","v":""},{"$f":"IF(Uncertainty!Z91=\"\",\"\",Uncertainty!Z91)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1014","v":"BC005a2"},{"$f":"VLOOKUP(A702,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 2, process 1 (LHV)"},{"$f":"IF('Input Project'!H69=\"\",\"\",'Input Project'!H69)","v":""},0,"",0,null,"","","","",0,{"$f":"IF(Uncertainty!W92=\"\",\"\",Uncertainty!W92)","v":""},{"$f":"IF(Uncertainty!Z92=\"\",\"\",Uncertainty!Z92)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1015","v":"BC005a3"},{"$f":"VLOOKUP(A703,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 3, process 1 (LHV)"},{"$f":"IF('Input Project'!H73=\"\",\"\",'Input Project'!H73)","v":""},0,"",0,null,"","","","",0,{"$f":"IF(Uncertainty!W93=\"\",\"\",Uncertainty!W93)","v":""},{"$f":"IF(Uncertainty!Z93=\"\",\"\",Uncertainty!Z93)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1016","v":"BC005b1"},{"$f":"VLOOKUP(A704,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 1, process 2 (LHV)"},{"$f":"IF('Input Project'!H128=\"\",\"\",'Input Project'!H128)","v":""},37,"",37,null,"","","","",0,{"$f":"IF(Uncertainty!W94=\"\",\"\",Uncertainty!W94)","v":""},{"$f":"IF(Uncertainty!Z94=\"\",\"\",Uncertainty!Z94)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1017","v":"BC005b2"},{"$f":"VLOOKUP(A705,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 2, process 2 (LHV)"},{"$f":"IF('Input Project'!H132=\"\",\"\",'Input Project'!H132)","v":""},0,"",0,null,"","","","",0,{"$f":"IF(Uncertainty!W95=\"\",\"\",Uncertainty!W95)","v":""},{"$f":"IF(Uncertainty!Z95=\"\",\"\",Uncertainty!Z95)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1018","v":"BC006a1"},{"$f":"VLOOKUP(A706,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 1, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1019","v":"BC006a2"},{"$f":"VLOOKUP(A707,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 2, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1020","v":"BC006a3"},{"$f":"VLOOKUP(A708,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 3, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1021","v":"BC006a4"},{"$f":"VLOOKUP(A709,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of electricity by-product, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1022","v":"BC006a5"},{"$f":"VLOOKUP(A710,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of heat by-product, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1023","v":"BC006b1"},{"$f":"VLOOKUP(A711,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 1, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1024","v":"BC006b2"},{"$f":"VLOOKUP(A712,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 2, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1025","v":"BC006b4"},{"$f":"VLOOKUP(A713,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of electricity by-product, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1026","v":"BC006b5"},{"$f":"VLOOKUP(A714,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of heat by-product, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1027","v":"BC007a"},{"$f":"VLOOKUP(A715,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of main output flow, process 1 (LHV)"},{"$f":"IF('Input Project'!H73=\"\",\"\",'Input Project'!H73)","v":""},{"$f":"VLOOKUP($A715,list_database1,$I$8,FALSE)","v":37},"",{"$f":"IF($L715=1,IF(MonteCarlo=1,$E715,IF($C715=\"\",$D715,$C715)),IF($C715=\"\",$D715,$C715))","v":37},null,{"$f":"IF($L715=1,IF($C715=\"\",$D715,$C715),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1028","v":"BC007b"},{"$f":"VLOOKUP(A716,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of main output flow, process 2 (LHV)"},{"$f":"IF('Input Project'!H153=\"\",\"\",'Input Project'!H153)","v":""},{"$f":"VLOOKUP($A716,list_database1,$I$8,FALSE)","v":37},{"$f":"IF(MonteCarlo=1,IF($L716=1,IF($H716=\"n.a.\",0,IF($H716<0.009,0,MIN(MAX(NORMINV(RAND(),$H716,$K716),$I716),$J716))),\"\"),\"\")","v":""},{"$f":"IF($L716=1,IF(MonteCarlo=1,$E716,IF($C716=\"\",$D716,$C716)),IF($C716=\"\",$D716,$C716))","v":37},null,"","","","",0,null,null,{"$f":"IF($L716=1,VLOOKUP($A716,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L716=1,VLOOKUP($A716,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1029","v":"BC008a"},{"$f":"VLOOKUP(A717,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate (output/input), process 1"},null,0.52999401737774465,"",0.52999401737774465,null,0.52999401737774465,0.51,0.55000000000000004,6.6666666666666723E-3,1,{"$f":"IF(Uncertainty!W59=\"\",\"\",Uncertainty!W59)","v":""},{"$f":"IF(Uncertainty!Z59=\"\",\"\",Uncertainty!Z59)","v":""},0.51,0.55000000000000004]
[{"$f":"'ID-numbers'!$A1030","v":"BC008b"},{"$f":"VLOOKUP(A718,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate (output/input), process 2"},null,0.31987937632906788,"",0.31987937632906788,null,0.31987937632906788,0.3,0.34,6.6666666666666723E-3,1,{"$f":"IF(Uncertainty!W88=\"\",\"\",Uncertainty!W88)","v":""},{"$f":"IF(Uncertainty!Z88=\"\",\"\",Uncertainty!Z88)","v":""},0.3,0.34]
[{"$f":"'ID-numbers'!$A1031","v":"BC009a0"},{"$f":"VLOOKUP(A719,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of main input, process 1"},{"$f":"IF('Input Project'!H84=\"\",\"\",'Input Project'!H84)","v":""},"Fresh palm fruit bunches (FFB)","","Fresh palm fruit bunches (FFB)",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1032","v":"BC009a1"},{"$f":"VLOOKUP(A720,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 1, process 1"},{"$f":"IF('Input Project'!H87=\"\",\"\",'Input Project'!H87)","v":"n.a."},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1033","v":"BC009a2"},{"$f":"VLOOKUP(A721,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 2, process 1"},{"$f":"IF('Input Project'!H91=\"\",\"\",'Input Project'!H91)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1034","v":"BC009a3"},{"$f":"VLOOKUP(A722,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 3, process 1"},{"$f":"IF('Input Project'!H95=\"\",\"\",'Input Project'!H95)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1035","v":"BC009b1"},{"$f":"VLOOKUP(A723,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 1, process 2"},{"$f":"IF('Input Project'!H143=\"\",\"\",'Input Project'!H143)","v":""},"Fuller's earth",{"$f":"IF(MonteCarlo=1,IF($L723=1,IF($H723=\"n.a.\",0,IF($H723<0.009,0,MIN(MAX(NORMINV(RAND(),$H723,$K723),$I723),$J723))),\"\"),\"\")","v":""},"Fuller's earth",null,{"$f":"IF($L723=1,IF($C723=\"\",$D723,$C723),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1036","v":"BC009b2"},{"$f":"VLOOKUP(A724,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 2, process 2"},{"$f":"IF('Input Project'!H147=\"\",\"\",'Input Project'!H147)","v":""},"n.a.","","n.a.",null,"",{"$f":"IF($L724=1,IF($M724=\"\",$O724,$M724),\"\")","v":""},{"$f":"IF($L724=1,IF($N724=\"\",$P724,$N724),\"\")","v":""},{"$f":"IF($L724=1,($J724-$I724)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1037","v":"BC009c"},{"$f":"VLOOKUP(A725,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material output flow, process 1"},{"$f":"IF('Input Project'!H99=\"\",\"\",'Input Project'!H99)","v":""},"n.a.","","n.a.",null,{"$f":"IF($L725=1,IF($C725=\"\",$D725,$C725),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1038","v":"BC009c1"},{"$f":"VLOOKUP(A726,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of output flow, process 1 (electricity)"},{"$f":"IF('Input Project'!H102=\"\",\"\",'Input Project'!H102)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1039","v":"BC009c2"},{"$f":"VLOOKUP(A727,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of output flow, process 1 (heat)"},{"$f":"IF('Input Project'!H103=\"\",\"\",'Input Project'!H103)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1040","v":"BC009d"},{"$f":"VLOOKUP(A728,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material output flow, process 2"},{"$f":"IF('Input Project'!H151=\"\",\"\",'Input Project'!H151)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1041","v":"BC009d1"},{"$f":"VLOOKUP(A729,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of output flow, process 2 (electricity)"},{"$f":"IF('Input Project'!H154=\"\",\"\",'Input Project'!H154)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1042","v":"BC009d2"},{"$f":"VLOOKUP(A730,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of output flow, process 2 (heat)"},{"$f":"IF('Input Project'!H155=\"\",\"\",'Input Project'!H155)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1043","v":"BC010a0"},{"$f":"VLOOKUP(A731,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Main input, process 1"},{"$f":"IF('Input Project'!H85=\"\",\"\",'Input Project'!H85)","v":""},19000,"",19000,null,19000,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1044","v":"BC010a01"},{"$f":"VLOOKUP(A732,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 1, process 1"},{"$f":"IF('Input Project'!H88=\"\",\"\",'Input Project'!H88)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1045","v":"BC010a"},{"$f":"VLOOKUP(A733,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of main input, process 1"},null,7.8617238875928711E-2,"",7.8617238875928711E-2,null,7.8617238875928711E-2,0,0,0,1,{"$f":"IF(Uncertainty!W64=\"\",\"\",Uncertainty!W64)","v":""},{"$f":"IF(Uncertainty!Z64=\"\",\"\",Uncertainty!Z64)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1046","v":"BC010a1"},{"$f":"VLOOKUP(A734,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 1, process 1"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W65=\"\",\"\",Uncertainty!W65)","v":""},{"$f":"IF(Uncertainty!Z65=\"\",\"\",Uncertainty!Z65)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1047","v":"BC010a10"},{"$f":"VLOOKUP(A735,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 1, process 1"},{"$f":"IF('Input Project'!H89=\"\",\"\",'Input Project'!H89)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1048","v":"BC010a11"},{"$f":"VLOOKUP(A736,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 1, process 1"},{"$f":"IF('Input Project'!H90=\"\",\"\",'Input Project'!H90)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L736=1,IF($H736=\"n.a.\",0,IF($H736<0.009,0,MIN(MAX(NORMINV(RAND(),$H736,$K736),$I736),$J736))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L736=1,IF($C736=\"\",$D736,$C736),\"\")","v":""},{"$f":"IF($L736=1,IF($M736=\"\",$O736,$M736),\"\")","v":""},{"$f":"IF($L736=1,IF($N736=\"\",$P736,$N736),\"\")","v":""},{"$f":"IF($L736=1,($J736-$I736)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1049","v":"BC010a02"},{"$f":"VLOOKUP(A737,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 2, process 1"},{"$f":"IF('Input Project'!H92=\"\",\"\",'Input Project'!H92)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1050","v":"BC010a2"},{"$f":"VLOOKUP(A738,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 2, process 1"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W66=\"\",\"\",Uncertainty!W66)","v":""},{"$f":"IF(Uncertainty!Z66=\"\",\"\",Uncertainty!Z66)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1051","v":"BC010a20"},{"$f":"VLOOKUP(A739,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 2, process 1"},{"$f":"IF('Input Project'!H93=\"\",\"\",'Input Project'!H93)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1052","v":"BC010a21"},{"$f":"VLOOKUP(A740,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 2, process 1"},{"$f":"IF('Input Project'!H94=\"\",\"\",'Input Project'!H94)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L740=1,IF($H740=\"n.a.\",0,IF($H740<0.009,0,MIN(MAX(NORMINV(RAND(),$H740,$K740),$I740),$J740))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L740=1,IF($C740=\"\",$D740,$C740),\"\")","v":""},{"$f":"IF($L740=1,IF($M740=\"\",$O740,$M740),\"\")","v":""},{"$f":"IF($L740=1,IF($N740=\"\",$P740,$N740),\"\")","v":""},{"$f":"IF($L740=1,($J740-$I740)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1053","v":"BC010a03"},{"$f":"VLOOKUP(A741,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 3, process 1"},{"$f":"IF('Input Project'!H96=\"\",\"\",'Input Project'!H96)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1054","v":"BC010a3"},{"$f":"VLOOKUP(A742,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 3, process 1"},null,0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1055","v":"BC010a30"},{"$f":"VLOOKUP(A743,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 3, process 1"},{"$f":"IF('Input Project'!H97=\"\",\"\",'Input Project'!H97)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1056","v":"BC010a31"},{"$f":"VLOOKUP(A744,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 3, process 1"},{"$f":"IF('Input Project'!H98=\"\",\"\",'Input Project'!H98)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L744=1,IF($H744=\"n.a.\",0,IF($H744<0.009,0,MIN(MAX(NORMINV(RAND(),$H744,$K744),$I744),$J744))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L744=1,IF($C744=\"\",$D744,$C744),\"\")","v":""},{"$f":"IF($L744=1,IF($M744=\"\",$O744,$M744),\"\")","v":""},{"$f":"IF($L744=1,IF($N744=\"\",$P744,$N744),\"\")","v":""},{"$f":"IF($L744=1,($J744-$I744)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1057","v":"BC010b1"},{"$f":"VLOOKUP(A745,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 1, process 2"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W94=\"\",\"\",Uncertainty!W94)","v":""},{"$f":"IF(Uncertainty!Z94=\"\",\"\",Uncertainty!Z94)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1058","v":"BC010b10"},{"$f":"VLOOKUP(A746,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 1, process 2"},{"$f":"IF('Input Project'!H144=\"\",\"\",'Input Project'!H144)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1059","v":"BC010b11"},{"$f":"VLOOKUP(A747,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 1, process 2"},{"$f":"IF('Input Project'!H145=\"\",\"\",'Input Project'!H145)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1060","v":"BC010b12"},{"$f":"VLOOKUP(A748,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 1, process 2"},{"$f":"IF('Input Project'!H146=\"\",\"\",'Input Project'!H146)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L748=1,IF($H748=\"n.a.\",0,IF($H748<0.009,0,MIN(MAX(NORMINV(RAND(),$H748,$K748),$I748),$J748))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L748=1,IF($C748=\"\",$D748,$C748),\"\")","v":""},{"$f":"IF($L748=1,IF($M748=\"\",$O748,$M748),\"\")","v":""},{"$f":"IF($L748=1,IF($N748=\"\",$P748,$N748),\"\")","v":""},{"$f":"IF($L748=1,($J748-$I748)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1061","v":"BC010b2"},{"$f":"VLOOKUP(A749,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 2, process 2"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W95=\"\",\"\",Uncertainty!W95)","v":""},{"$f":"IF(Uncertainty!Z95=\"\",\"\",Uncertainty!Z95)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1062","v":"BC010b20"},{"$f":"VLOOKUP(A750,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 2, process 2"},{"$f":"IF('Input Project'!H148=\"\",\"\",'Input Project'!H148)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1063","v":"BC010b21"},{"$f":"VLOOKUP(A751,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 2, process 2"},{"$f":"IF('Input Project'!H149=\"\",\"\",'Input Project'!H149)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1064","v":"BC010b22"},{"$f":"VLOOKUP(A752,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 2, process 2"},{"$f":"IF('Input Project'!H150=\"\",\"\",'Input Project'!H150)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L752=1,IF($H752=\"n.a.\",0,IF($H752<0.009,0,MIN(MAX(NORMINV(RAND(),$H752,$K752),$I752),$J752))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L752=1,IF($C752=\"\",$D752,$C752),\"\")","v":""},{"$f":"IF($L752=1,IF($M752=\"\",$O752,$M752),\"\")","v":""},{"$f":"IF($L752=1,IF($N752=\"\",$P752,$N752),\"\")","v":""},{"$f":"IF($L752=1,($J752-$I752)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1065","v":"BC010c"},{"$f":"VLOOKUP(A753,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 1"},null,2.6636946173917474E-3,"",2.6636946173917474E-3,null,2.6636946173917474E-3,0,0,0,1,{"$f":"IF(Uncertainty!W96=\"\",\"\",Uncertainty!W96)","v":""},{"$f":"IF(Uncertainty!Z96=\"\",\"\",Uncertainty!Z96)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1066","v":"BC010c0"},{"$f":"VLOOKUP(A754,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material output flow, process 1"},{"$f":"IF('Input Project'!H100=\"\",\"\",'Input Project'!H100)","v":""},4311,"",4311,null,4311,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1067","v":"BC010c1"},{"$f":"VLOOKUP(A755,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 1 (Electricity)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W98=\"\",\"\",Uncertainty!W98)","v":""},{"$f":"IF(Uncertainty!Z98=\"\",\"\",Uncertainty!Z98)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1068","v":"BC010c2"},{"$f":"VLOOKUP(A756,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 1 (Heat)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W99=\"\",\"\",Uncertainty!W99)","v":""},{"$f":"IF(Uncertainty!Z99=\"\",\"\",Uncertainty!Z99)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1069","v":"BC010d"},{"$f":"VLOOKUP(A757,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 2"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W97=\"\",\"\",Uncertainty!W97)","v":""},{"$f":"IF(Uncertainty!Z97=\"\",\"\",Uncertainty!Z97)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1070","v":"BC010d0"},{"$f":"VLOOKUP(A758,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material output flow, process 2"},{"$f":"IF('Input Project'!H152=\"\",\"\",'Input Project'!H152)","v":""},1379,"",1379,null,1379,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1071","v":"BC010d1"},{"$f":"VLOOKUP(A759,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 2 (Electricity)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W99=\"\",\"\",Uncertainty!W99)","v":""},{"$f":"IF(Uncertainty!Z99=\"\",\"\",Uncertainty!Z99)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1072","v":"BC010d2"},{"$f":"VLOOKUP(A760,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 2 (Heat)"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W100=\"\",\"\",Uncertainty!W100)","v":""},{"$f":"IF(Uncertainty!Z100=\"\",\"\",Uncertainty!Z100)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1073","v":"BC011a1"},{"$f":"VLOOKUP(A761,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 1, process 1"},{"$f":"IF('Input Project'!H76=\"\",\"\",'Input Project'!H76)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1074","v":"BC011a2"},{"$f":"VLOOKUP(A762,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 2, process 1"},{"$f":"IF('Input Project'!H78=\"\",\"\",'Input Project'!H78)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1075","v":"BC011b1"},{"$f":"VLOOKUP(A763,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 1, process 2"},{"$f":"IF('Input Project'!H135=\"\",\"\",'Input Project'!H135)","v":""},"Heat from NG boiler","","Heat from NG boiler",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1076","v":"BC011b2"},{"$f":"VLOOKUP(A764,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 2, process 2"},{"$f":"IF('Input Project'!H137=\"\",\"\",'Input Project'!H137)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1077","v":"BC012a"},{"$f":"VLOOKUP(A765,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of main output flow, process 1"},null,0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1078","v":"BC012b"},{"$f":"VLOOKUP(A766,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of main output flow, process 2"},null,0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1079","v":"BC014a"},{"$f":"VLOOKUP(A767,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 1 per ha after conversion process 1"},null,null,"",null,{"$f":"VLOOKUP(A767,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":4224.7799859623219},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1080","v":"BC014b"},{"$f":"VLOOKUP(A768,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of feedstock 1 per ha after conversion process 1"},null,null,"",null,{"$f":"VLOOKUP(A768,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":4224.7799859623219},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1081","v":"BC014c"},{"$f":"VLOOKUP(A769,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of feedstock 1 per ha after conversion process 1"},null,null,"",null,{"$f":"VLOOKUP(A769,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":156316.8594806059},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1082","v":"BC015a"},{"$f":"VLOOKUP(A770,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 1 per ha after conversion process 2"},null,null,"",null,{"$f":"VLOOKUP(A770,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1351.4199870371556},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1083","v":"BC015b"},{"$f":"VLOOKUP(A771,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of feedstock 1 per ha after conversion process 2"},null,null,"",null,{"$f":"VLOOKUP(A771,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1351.4199870371556},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1084","v":"BC015c"},{"$f":"VLOOKUP(A772,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of feedstock 1 per ha after conversion process 2"},null,null,"",null,{"$f":"VLOOKUP(A772,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":50002.539520374754},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1085","v":"BC016a"},{"$f":"VLOOKUP(A773,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K30=\"\",\"\",'Input EQ'!K30)","v":""},{"$f":"VLOOKUP($A773,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L773=1,IF(MonteCarlo=1,$E773,IF($C773=\"\",$D773,$C773)),IF($C773=\"\",$D773,$C773))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W67=\"\",\"\",Uncertainty!W67)","v":""},{"$f":"IF(Uncertainty!Z67=\"\",\"\",Uncertainty!Z67)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1086","v":"BC016b"},{"$f":"VLOOKUP(A774,'ID-numbers'!$1:$1048576,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K31=\"\",\"\",'Input EQ'!K31)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W68=\"\",\"\",Uncertainty!W68)","v":""},{"$f":"IF(Uncertainty!Z68=\"\",\"\",Uncertainty!Z68)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1087","v":"BC016c"},{"$f":"VLOOKUP(A775,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K32=\"\",\"\",'Input EQ'!K32)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W69=\"\",\"\",Uncertainty!W69)","v":""},{"$f":"IF(Uncertainty!Z69=\"\",\"\",Uncertainty!Z69)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1088","v":"BC016d"},{"$f":"VLOOKUP(A776,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K33=\"\",\"\",'Input EQ'!K33)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W70=\"\",\"\",Uncertainty!W70)","v":""},{"$f":"IF(Uncertainty!Z70=\"\",\"\",Uncertainty!Z70)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1089","v":"BC016e"},{"$f":"VLOOKUP(A777,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K34=\"\",\"\",'Input EQ'!K34)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W71=\"\",\"\",Uncertainty!W71)","v":""},{"$f":"IF(Uncertainty!Z71=\"\",\"\",Uncertainty!Z71)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1090","v":"BC016f"},{"$f":"VLOOKUP(A778,'ID-numbers'!$1:$1048576,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K35=\"\",\"\",'Input EQ'!K35)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W72=\"\",\"\",Uncertainty!W72)","v":""},{"$f":"IF(Uncertainty!Z72=\"\",\"\",Uncertainty!Z72)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1091","v":"BC016g"},{"$f":"VLOOKUP(A779,'ID-numbers'!$1:$1048576,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K36=\"\",\"\",'Input EQ'!K36)","v":""},20,"",20,null,20,15,25,1.6666666666666667,1,{"$f":"IF(Uncertainty!W73=\"\",\"\",Uncertainty!W73)","v":""},{"$f":"IF(Uncertainty!Z73=\"\",\"\",Uncertainty!Z73)","v":""},15,25]
[{"$f":"'ID-numbers'!$A1092","v":"BC017a"},{"$f":"VLOOKUP(A780,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K39=\"\",\"\",'Input EQ'!K39)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W96=\"\",\"\",Uncertainty!W96)","v":""},{"$f":"IF(Uncertainty!Z96=\"\",\"\",Uncertainty!Z96)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1093","v":"BC017b"},{"$f":"VLOOKUP(A781,'ID-numbers'!$1:$1048576,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K40=\"\",\"\",'Input EQ'!K40)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W97=\"\",\"\",Uncertainty!W97)","v":""},{"$f":"IF(Uncertainty!Z97=\"\",\"\",Uncertainty!Z97)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1094","v":"BC017c"},{"$f":"VLOOKUP(A782,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K41=\"\",\"\",'Input EQ'!K41)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W98=\"\",\"\",Uncertainty!W98)","v":""},{"$f":"IF(Uncertainty!Z98=\"\",\"\",Uncertainty!Z98)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1095","v":"BC017d"},{"$f":"VLOOKUP(A783,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K42=\"\",\"\",'Input EQ'!K42)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W99=\"\",\"\",Uncertainty!W99)","v":""},{"$f":"IF(Uncertainty!Z99=\"\",\"\",Uncertainty!Z99)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1096","v":"BC017e"},{"$f":"VLOOKUP(A784,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K43=\"\",\"\",'Input EQ'!K43)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W100=\"\",\"\",Uncertainty!W100)","v":""},{"$f":"IF(Uncertainty!Z100=\"\",\"\",Uncertainty!Z100)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1097","v":"BC017f"},{"$f":"VLOOKUP(A785,'ID-numbers'!$1:$1048576,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K44=\"\",\"\",'Input EQ'!K44)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W101=\"\",\"\",Uncertainty!W101)","v":""},{"$f":"IF(Uncertainty!Z101=\"\",\"\",Uncertainty!Z101)","v":""},{"$f":"IF($L785=1,VLOOKUP($A785,list_database1,$I$8+1,FALSE),\"\")","v":0},{"$f":"IF($L785=1,VLOOKUP($A785,list_database1,$I$8+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1098","v":"BC017g"},{"$f":"VLOOKUP(A786,'ID-numbers'!$1:$1048576,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K45=\"\",\"\",'Input EQ'!K45)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W102=\"\",\"\",Uncertainty!W102)","v":""},{"$f":"IF(Uncertainty!Z102=\"\",\"\",Uncertainty!Z102)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1101","v":"BC020a"},{"$f":"VLOOKUP(A787,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use in process 1"},null,null,"",null,{"$f":"VLOOKUP(A787,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1102","v":"BC020b"},{"$f":"VLOOKUP(A788,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use in process 2"},null,null,"",null,{"$f":"VLOOKUP(A788,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.6357622712156819E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1103","v":"BC021a"},{"$f":"VLOOKUP(A789,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use in process 1"},null,null,"",null,{"$f":"VLOOKUP(A789,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1104","v":"BC021b"},{"$f":"VLOOKUP(A790,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use in process 2"},null,null,"",null,{"$f":"VLOOKUP(A790,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2.4536434068235229E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1105","v":"BC022a"},{"$f":"VLOOKUP(A791,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-products, process 1"},null,null,"",null,{"$f":"VLOOKUP(A791,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":4.3321107358900459},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1106","v":"BC022b"},{"$f":"VLOOKUP(A792,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-products, process 2"},null,null,"",null,{"$f":"VLOOKUP(A792,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1107","v":"BC024a"},{"$f":"VLOOKUP(A793,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to electricity input, process 1"},null,null,"",null,{"$f":"VLOOKUP(A793,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1108","v":"BC024b"},{"$f":"VLOOKUP(A794,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to electricity input, process 2"},null,null,"",null,{"$f":"VLOOKUP(A794,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.6357622712156819E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1109","v":"BC025a"},{"$f":"VLOOKUP(A795,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to electricity input, process 1"},null,null,"",null,{"$f":"VLOOKUP(A795,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1110","v":"BC025b"},{"$f":"VLOOKUP(A796,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to electricity input, process 2"},null,null,"",null,{"$f":"VLOOKUP(A796,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2.4536434068235229E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1111","v":"BC026a"},{"$f":"VLOOKUP(A797,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of electricity input 1, process 1"},null,{"$f":"VLOOKUP($A797,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L797=1,IF(MonteCarlo=1,$E797,IF($C797=\"\",$D797,$C797)),IF($C797=\"\",$D797,$C797))","v":0},null,0,{"$f":"IF($L797=1,IF($M797=\"\",$O797,$M797),\"\")","v":0},0,0,1,{"$f":"IF(Uncertainty!W64=\"\",\"\",Uncertainty!W64)","v":""},{"$f":"IF(Uncertainty!Z64=\"\",\"\",Uncertainty!Z64)","v":""},0,{"$f":"IF($L797=1,VLOOKUP($A797,list_database1,$I$8+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1112","v":"BC026a0"},{"$f":"VLOOKUP(A798,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity flow 1, process 1"},{"$f":"IF('Input Project'!H81=\"\",\"\",'Input Project'!H81)","v":""},0,"",0,null,0,{"$f":"IF($L798=1,IF($M798=\"\",$O798,$M798),\"\")","v":0},0,0,1,{"$f":"IF(Uncertainty!W65=\"\",\"\",Uncertainty!W65)","v":""},{"$f":"IF(Uncertainty!Z65=\"\",\"\",Uncertainty!Z65)","v":""},0,{"$f":"IF($L798=1,VLOOKUP($A798,list_database1,$I$8+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1113","v":"BC026a1"},{"$f":"VLOOKUP(A799,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of electricity input 2, process 1"},null,0,"",0,null,0,{"$f":"IF($L799=1,IF($M799=\"\",$O799,$M799),\"\")","v":0},0,0,1,{"$f":"IF(Uncertainty!W65=\"\",\"\",Uncertainty!W65)","v":""},{"$f":"IF(Uncertainty!Z65=\"\",\"\",Uncertainty!Z65)","v":""},0,{"$f":"IF($L799=1,VLOOKUP($A799,list_database1,$I$8+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1114","v":"BC026a10"},{"$f":"VLOOKUP(A800,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity flow 2, process 1"},{"$f":"IF('Input Project'!H83=\"\",\"\",'Input Project'!H83)","v":""},0,"",0,null,0,{"$f":"IF($L800=1,IF($M800=\"\",$O800,$M800),\"\")","v":0},0,0,1,{"$f":"IF(Uncertainty!W67=\"\",\"\",Uncertainty!W67)","v":""},{"$f":"IF(Uncertainty!Z67=\"\",\"\",Uncertainty!Z67)","v":""},0,{"$f":"IF($L800=1,VLOOKUP($A800,list_database1,$I$8+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1115","v":"BC026b"},{"$f":"VLOOKUP(A801,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of electricity input 1, process 2"},null,5.9972952198558455E-4,"",5.9972952198558455E-4,null,5.9972952198558455E-4,0,0,0,1,{"$f":"IF(Uncertainty!W93=\"\",\"\",Uncertainty!W93)","v":""},{"$f":"IF(Uncertainty!Z93=\"\",\"\",Uncertainty!Z93)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1116","v":"BC026b0"},{"$f":"VLOOKUP(A802,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity flow 1, process 2"},{"$f":"IF('Input Project'!H140=\"\",\"\",'Input Project'!H140)","v":""},8.5000000000000006E-3,"",8.5000000000000006E-3,null,8.5000000000000006E-3,{"$f":"IF($L802=1,IF($M802=\"\",$O802,$M802),\"\")","v":0},0,0,1,{"$f":"IF(Uncertainty!W69=\"\",\"\",Uncertainty!W69)","v":""},{"$f":"IF(Uncertainty!Z69=\"\",\"\",Uncertainty!Z69)","v":""},0,{"$f":"IF($L802=1,VLOOKUP($A802,list_database1,$I$8+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1117","v":"BC026b1"},{"$f":"VLOOKUP(A803,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of electricity input 2, process 2"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W94=\"\",\"\",Uncertainty!W94)","v":""},{"$f":"IF(Uncertainty!Z94=\"\",\"\",Uncertainty!Z94)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1118","v":"BC026b10"},{"$f":"VLOOKUP(A804,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity flow 2, process 2"},{"$f":"IF('Input Project'!H142=\"\",\"\",'Input Project'!H142)","v":""},0,"",0,null,0,{"$f":"IF($L804=1,IF($M804=\"\",$O804,$M804),\"\")","v":0},0,0,1,{"$f":"IF(Uncertainty!W71=\"\",\"\",Uncertainty!W71)","v":""},{"$f":"IF(Uncertainty!Z71=\"\",\"\",Uncertainty!Z71)","v":""},0,{"$f":"IF($L804=1,VLOOKUP($A804,list_database1,$I$8+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1119","v":"BC027a"},{"$f":"VLOOKUP(A805,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of electricity flow 1, process 1"},{"$f":"IF('Input Project'!H80=\"\",\"\",'Input Project'!H80)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1120","v":"BC027a1"},{"$f":"VLOOKUP(A806,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of electricity flow 2, process 1"},{"$f":"IF('Input Project'!H82=\"\",\"\",'Input Project'!H82)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1121","v":"BC027b"},{"$f":"VLOOKUP(A807,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of electricity flow 1, process 2"},{"$f":"IF('Input Project'!H139=\"\",\"\",'Input Project'!H139)","v":""},"Electricity EU mix LV","","Electricity EU mix LV",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1122","v":"BC027b1"},{"$f":"VLOOKUP(A808,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of electricity flow 2, process 2"},{"$f":"IF('Input Project'!H141=\"\",\"\",'Input Project'!H141)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1123","v":"BC028a"},{"$f":"VLOOKUP(A809,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A809,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1124","v":"BC028a1"},{"$f":"VLOOKUP(A810,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A810,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1125","v":"BC028b"},{"$f":"VLOOKUP(A811,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A811,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2.7275},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1126","v":"BC028b1"},{"$f":"VLOOKUP(A812,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A812,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1127","v":"BC029a"},{"$f":"VLOOKUP(A813,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A813,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1128","v":"BC029a1"},{"$f":"VLOOKUP(A814,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A814,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1129","v":"BC029b"},{"$f":"VLOOKUP(A815,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A815,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":4.0912500000000005},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1130","v":"BC029b1"},{"$f":"VLOOKUP(A816,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A816,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1131","v":"BC030a"},{"$f":"VLOOKUP(A817,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A817,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1132","v":"BC030b"},{"$f":"VLOOKUP(A818,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A818,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1133","v":"BC031a1"},{"$f":"VLOOKUP(A819,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat input 1, process 1"},null,{"$f":"VLOOKUP($A819,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L819=1,IF(MonteCarlo=1,$E819,IF($C819=\"\",$D819,$C819)),IF($C819=\"\",$D819,$C819))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W62=\"\",\"\",Uncertainty!W62)","v":""},{"$f":"IF(Uncertainty!Z62=\"\",\"\",Uncertainty!Z62)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1134","v":"BC031a10"},{"$f":"VLOOKUP(A820,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fuel/heat flow 1, process 1"},{"$f":"IF('Input Project'!H77=\"\",\"\",'Input Project'!H77)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W63=\"\",\"\",Uncertainty!W63)","v":""},{"$f":"IF(Uncertainty!Z63=\"\",\"\",Uncertainty!Z63)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1135","v":"BC031a2"},{"$f":"VLOOKUP(A821,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat input 2, process 1"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W63=\"\",\"\",Uncertainty!W63)","v":""},{"$f":"IF(Uncertainty!Z63=\"\",\"\",Uncertainty!Z63)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1136","v":"BC031a20"},{"$f":"VLOOKUP(A822,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fuel/heat flow 2, process 1"},{"$f":"IF('Input Project'!H79=\"\",\"\",'Input Project'!H79)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W65=\"\",\"\",Uncertainty!W65)","v":""},{"$f":"IF(Uncertainty!Z65=\"\",\"\",Uncertainty!Z65)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1137","v":"BC031b1"},{"$f":"VLOOKUP(A823,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat input 1, process 2"},null,7.9963936264744601E-3,"",7.9963936264744601E-3,null,{"$f":"IF($L823=1,IF($C823=\"\",$D823,$C823),\"\")","v":7.9963936264744601E-3},0,{"$f":"IF($L823=1,IF($N823=\"\",$P823,$N823),\"\")","v":0.02},3.3333333333333335E-3,1,{"$f":"IF(Uncertainty!W91=\"\",\"\",Uncertainty!W91)","v":""},{"$f":"IF(Uncertainty!Z91=\"\",\"\",Uncertainty!Z91)","v":""},0,0.02]
[{"$f":"'ID-numbers'!$A1138","v":"BC031b10"},{"$f":"VLOOKUP(A824,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fuel/heat flow 1, process 2"},{"$f":"IF('Input Project'!H136=\"\",\"\",'Input Project'!H136)","v":""},408,"",408,null,408,0,0,0,1,{"$f":"IF(Uncertainty!W67=\"\",\"\",Uncertainty!W67)","v":""},{"$f":"IF(Uncertainty!Z67=\"\",\"\",Uncertainty!Z67)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1139","v":"BC031b2"},{"$f":"VLOOKUP(A825,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat input 2, process 2"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W92=\"\",\"\",Uncertainty!W92)","v":""},{"$f":"IF(Uncertainty!Z92=\"\",\"\",Uncertainty!Z92)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1140","v":"BC031b20"},{"$f":"VLOOKUP(A826,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fuel/heat flow 2, process 2"},{"$f":"IF('Input Project'!H138=\"\",\"\",'Input Project'!H138)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W69=\"\",\"\",Uncertainty!W69)","v":""},{"$f":"IF(Uncertainty!Z69=\"\",\"\",Uncertainty!Z69)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1141","v":"BC032a1"},{"$f":"VLOOKUP(A827,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A827,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1142","v":"BC032a2"},{"$f":"VLOOKUP(A828,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A828,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1143","v":"BC032b1"},{"$f":"VLOOKUP(A829,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A829,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1144","v":"BC032b2"},{"$f":"VLOOKUP(A830,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A830,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1145","v":"BC033a1"},{"$f":"VLOOKUP(A831,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, process 1"},null,null,{"$f":"IF(MonteCarlo=1,IF($L831=1,IF($H831=\"n.a.\",0,IF($H831<0.009,0,MIN(MAX(NORMINV(RAND(),$H831,$K831),$I831),$J831))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A831,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},{"$f":"IF($L831=1,IF($C831=\"\",$D831,$C831),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1146","v":"BC033a2"},{"$f":"VLOOKUP(A832,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A832,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"",{"$f":"IF($L832=1,IF($M832=\"\",$O832,$M832),\"\")","v":""},{"$f":"IF($L832=1,IF($N832=\"\",$P832,$N832),\"\")","v":""},{"$f":"IF($L832=1,($J832-$I832)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1147","v":"BC033b1"},{"$f":"VLOOKUP(A833,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A833,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1148","v":"BC033b2"},{"$f":"VLOOKUP(A834,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A834,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1149","v":"BC034a"},{"$f":"VLOOKUP(A835,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to fuel/heat input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A835,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1150","v":"BC034b"},{"$f":"VLOOKUP(A836,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to fuel/heat input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A836,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1151","v":"BC035a"},{"$f":"VLOOKUP(A837,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to material input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A837,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1152","v":"BC035a1"},{"$f":"VLOOKUP(A838,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A838,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1153","v":"BC035a2"},{"$f":"VLOOKUP(A839,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A839,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1154","v":"BC035a3"},{"$f":"VLOOKUP(A840,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 3, process 1"},null,null,"",null,{"$f":"VLOOKUP(A840,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1155","v":"BC035b"},{"$f":"VLOOKUP(A841,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to material input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A841,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1156","v":"BC035b1"},{"$f":"VLOOKUP(A842,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A842,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2.5405200000000003},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1157","v":"BC035b2"},{"$f":"VLOOKUP(A843,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A843,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1158","v":"BC035c"},{"$f":"VLOOKUP(A844,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material output flow, process 1"}]
[{"$f":"'ID-numbers'!$A1159","v":"BC035c1"},{"$f":"VLOOKUP(A845,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for  output flow, process 1 (electricity)"}]
[{"$f":"'ID-numbers'!$A1160","v":"BC035c2"},{"$f":"VLOOKUP(A846,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for  output flow, process 1 (heat)"}]
[{"$f":"'ID-numbers'!$A1161","v":"BC035d"},{"$f":"VLOOKUP(A847,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material output flow, process 2"}]
[{"$f":"'ID-numbers'!$A1162","v":"BC035d1"},{"$f":"VLOOKUP(A848,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for  output flow, process 2 (electricity)"}]
[{"$f":"'ID-numbers'!$A1163","v":"BC035d2"},{"$f":"VLOOKUP(A849,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for  output flow, process 2 (heat)"}]
[{"$f":"'ID-numbers'!$A1164","v":"BC036a"},{"$f":"VLOOKUP(A850,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to material input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A850,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1165","v":"BC036a0"},{"$f":"VLOOKUP(A851,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for main input, process 1"},null,null,"",null,{"$f":"VLOOKUP(A851,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1166","v":"BC036a1"},{"$f":"VLOOKUP(A852,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A852,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1167","v":"BC036a2"},{"$f":"VLOOKUP(A853,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A853,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1168","v":"BC036a3"},{"$f":"VLOOKUP(A854,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 3, process 1"},null,null,"",null,{"$f":"VLOOKUP(A854,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1169","v":"BC036b"},{"$f":"VLOOKUP(A855,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to material input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A855,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1170","v":"BC036b1"},{"$f":"VLOOKUP(A856,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A856,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":3.8107800000000003},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1171","v":"BC036b2"},{"$f":"VLOOKUP(A857,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A857,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1172","v":"BC036c"},{"$f":"VLOOKUP(A858,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material output flow, process 1"}]
[{"$f":"'ID-numbers'!$A1173","v":"BC036c1"},{"$f":"VLOOKUP(A859,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for  output flow, process 1 (electricity)"}]
[{"$f":"'ID-numbers'!$A1174","v":"BC036c2"},{"$f":"VLOOKUP(A860,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for  output flow, process 1 (heat)"}]
[{"$f":"'ID-numbers'!$A1175","v":"BC036d"},{"$f":"VLOOKUP(A861,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material output flow, process 2"}]
[{"$f":"'ID-numbers'!$A1176","v":"BC036d1"},{"$f":"VLOOKUP(A862,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for output flow, process 2 (electricity)"}]
[{"$f":"'ID-numbers'!$A1177","v":"BC036d2"},{"$f":"VLOOKUP(A863,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for output flow, process 2 (heat)"}]
[{"$f":"'ID-numbers'!$A1178","v":"BC037a"},{"$f":"VLOOKUP(A864,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to process 1"},null,null,"",null,{"$f":"VLOOKUP(A864,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1179","v":"BC037b"},{"$f":"VLOOKUP(A865,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to process 2"},null,null,"",null,{"$f":"VLOOKUP(A865,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.65300153519651516},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1180","v":"BC041a"},{"$f":"VLOOKUP(A866,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to electricity input, process 1"},null,null,"",null,{"$f":"VLOOKUP(A866,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1181","v":"BC041b"},{"$f":"VLOOKUP(A867,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to electricity input, process 2"},null,null,"",null,{"$f":"VLOOKUP(A867,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":7.7478873694630399E-2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1182","v":"BC042a"},{"$f":"VLOOKUP(A868,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A868,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1183","v":"BC042a1"},{"$f":"VLOOKUP(A869,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A869,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1184","v":"BC042b"},{"$f":"VLOOKUP(A870,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A870,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":129.18969444444446},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1185","v":"BC042b1"},{"$f":"VLOOKUP(A871,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A871,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1186","v":"BC043a"},{"$f":"VLOOKUP(A872,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to fuel/heat input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A872,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1187","v":"BC043a1"},{"$f":"VLOOKUP(A873,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A873,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1188","v":"BC043a2"},{"$f":"VLOOKUP(A874,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A874,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1189","v":"BC043b"},{"$f":"VLOOKUP(A875,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to fuel/heat input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A875,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.5755226615018848},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1190","v":"BC043b1"},{"$f":"VLOOKUP(A876,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A876,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":71.972777777777765},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1191","v":"BC043b2"},{"$f":"VLOOKUP(A877,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A877,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1192","v":"BC047a"},{"$f":"VLOOKUP(A878,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to material input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A878,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1193","v":"BC047a1"},{"$f":"VLOOKUP(A879,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A879,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1194","v":"BC047a2"},{"$f":"VLOOKUP(A880,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A880,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1195","v":"BC047a3"},{"$f":"VLOOKUP(A881,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 3, process 1"},null,null,"",null,{"$f":"VLOOKUP(A881,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1196","v":"BC047b"},{"$f":"VLOOKUP(A882,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to material input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A882,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1197","v":"BC047b1"},{"$f":"VLOOKUP(A883,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A883,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":199.7227},"","","","",0,null,null,{"$f":"IF($L883=1,VLOOKUP($A883,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L883=1,VLOOKUP($A883,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1198","v":"BC047b2"},{"$f":"VLOOKUP(A884,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A884,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1199","v":"BC047c"},{"$f":"VLOOKUP(A885,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material output flow, process 1"}]
[{"$f":"'ID-numbers'!$A1200","v":"BC047c1"},{"$f":"VLOOKUP(A886,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to  output flow, process 1 (electricity)"}]
[{"$f":"'ID-numbers'!$A1201","v":"BC047c2"},{"$f":"VLOOKUP(A887,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to  output flow, process 1 (heat)"}]
[{"$f":"'ID-numbers'!$A1202","v":"BC047d"},{"$f":"VLOOKUP(A888,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material output flow, process 2"}]
[{"$f":"'ID-numbers'!$A1203","v":"BC047d1"},{"$f":"VLOOKUP(A889,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to  output flow, process 2 (electricity)"}]
[{"$f":"'ID-numbers'!$A1204","v":"BC047d2"},{"$f":"VLOOKUP(A890,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to  output flow, process 2 (heat)"}]
[{"$f":"'ID-numbers'!$A1205","v":"BC050a"},{"$f":"VLOOKUP(A891,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to energy crop, process 1"},null,null,"",null,{"$f":"VLOOKUP(A891,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":95.667889264109959},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1206","v":"BC050b"},{"$f":"VLOOKUP(A892,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to energy crop, process 2"},null,null,"",null,{"$f":"VLOOKUP(A892,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":100},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1207","v":"BC051a1"},{"$f":"VLOOKUP(A893,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A893,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":4.3321107358900459},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1208","v":"BC051a2"},{"$f":"VLOOKUP(A894,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A894,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1209","v":"BC051a3"},{"$f":"VLOOKUP(A895,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 3, process 1"},null,null,"",null,{"$f":"VLOOKUP(A895,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1210","v":"BC051a4"},{"$f":"VLOOKUP(A896,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to electricity by-product, process 1"},null,null,"",null,{"$f":"VLOOKUP(A896,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1211","v":"BC051a5"},{"$f":"VLOOKUP(A897,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to heat by-product, process 1"},null,null,"",null,{"$f":"VLOOKUP(A897,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1212","v":"BC051b1"},{"$f":"VLOOKUP(A898,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A898,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1213","v":"BC051b2"},{"$f":"VLOOKUP(A899,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A899,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1214","v":"BC051b4"},{"$f":"VLOOKUP(A900,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to electricity by-product, process 2"},null,null,"",null,{"$f":"VLOOKUP(A900,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1215","v":"BC051b5"},{"$f":"VLOOKUP(A901,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to heat by-product, process 2"},null,null,"",null,{"$f":"VLOOKUP(A901,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1216","v":"BC059a"},{"$f":"VLOOKUP(A902,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for treatment 2 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A902,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1217","v":"BC059b"},{"$f":"VLOOKUP(A903,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for treatment 2 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A903,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1218","v":"BC059c"},{"$f":"VLOOKUP(A904,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with treatment 2 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A904,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1221","v":"BC060"},{"$f":"VLOOKUP(A905,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat energy use for treatment 2 (storage)"},{"$f":"IF('Input Project'!H108=\"\",\"\",'Input Project'!H108)","v":""},{"$f":"VLOOKUP($A905,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L905=1,IF(MonteCarlo=1,$E905,IF($C905=\"\",$D905,$C905)),IF($C905=\"\",$D905,$C905))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W78=\"\",\"\",Uncertainty!W78)","v":""},{"$f":"IF(Uncertainty!Z78=\"\",\"\",Uncertainty!Z78)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1222","v":"BC061"},{"$f":"VLOOKUP(A906,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat source for treatment 2 (storage)"},{"$f":"IF('Input Project'!H107=\"\",\"\",'Input Project'!H107)","v":""},{"$f":"VLOOKUP($A906,list_database1,$I$8,FALSE)","v":"n.a."},"",{"$f":"IF($L906=1,IF(MonteCarlo=1,$E906,IF($C906=\"\",$D906,$C906)),IF($C906=\"\",$D906,$C906))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1228","v":"BC065"},{"$f":"VLOOKUP(A907,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity energy use for treatment 2 (storage)"},{"$f":"IF('Input Project'!H110=\"\",\"\",'Input Project'!H110)","v":""},{"$f":"VLOOKUP($A907,list_database1,$I$8,FALSE)","v":8.4000000000000003E-4},"",{"$f":"IF($L907=1,IF(MonteCarlo=1,$E907,IF($C907=\"\",$D907,$C907)),IF($C907=\"\",$D907,$C907))","v":8.4000000000000003E-4},null,8.4000000000000003E-4,0,1E-3,1.6666666666666666E-4,1,{"$f":"IF(Uncertainty!W79=\"\",\"\",Uncertainty!W79)","v":""},{"$f":"IF(Uncertainty!Z79=\"\",\"\",Uncertainty!Z79)","v":""},0,1E-3]
[{"$f":"'ID-numbers'!$A1229","v":"BC066"},{"$f":"VLOOKUP(A908,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity source for treatment 2 (storage)"},{"$f":"IF('Input Project'!H109=\"\",\"\",'Input Project'!H109)","v":""},{"$f":"VLOOKUP($A908,list_database1,$I$8,FALSE)","v":"n.a."},"",{"$f":"IF($L908=1,IF(MonteCarlo=1,$E908,IF($C908=\"\",$D908,$C908)),IF($C908=\"\",$D908,$C908))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1235","v":"BC069a"},{"$f":"VLOOKUP(A909,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A909,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1236","v":"BC069b"},{"$f":"VLOOKUP(A910,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A910,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1237","v":"BC069c"},{"$f":"VLOOKUP(A911,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A911,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1240","v":"BC070"},{"$f":"VLOOKUP(A912,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat energy use for treatment 3 (storage)"},{"$f":"IF('Input Project'!H160=\"\",\"\",'Input Project'!H160)","v":""},{"$f":"VLOOKUP($A912,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L912=1,IF(MonteCarlo=1,$E912,IF($C912=\"\",$D912,$C912)),IF($C912=\"\",$D912,$C912))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W107=\"\",\"\",Uncertainty!W107)","v":""},{"$f":"IF(Uncertainty!Z107=\"\",\"\",Uncertainty!Z107)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1241","v":"BC071"},{"$f":"VLOOKUP(A913,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat source for treatment 3 (storage)"},{"$f":"IF('Input Project'!H159=\"\",\"\",'Input Project'!H159)","v":""},{"$f":"VLOOKUP($A913,list_database1,$I$8,FALSE)","v":"n.a."},"",{"$f":"IF($L913=1,IF(MonteCarlo=1,$E913,IF($C913=\"\",$D913,$C913)),IF($C913=\"\",$D913,$C913))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1247","v":"BC075"},{"$f":"VLOOKUP(A914,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity energy use for treatment 3 (storage)"},{"$f":"IF('Input Project'!H162=\"\",\"\",'Input Project'!H162)","v":""},{"$f":"VLOOKUP($A914,list_database1,$I$8,FALSE)","v":8.4000000000000003E-4},"",{"$f":"IF($L914=1,IF(MonteCarlo=1,$E914,IF($C914=\"\",$D914,$C914)),IF($C914=\"\",$D914,$C914))","v":8.4000000000000003E-4},null,8.4000000000000003E-4,0,1E-3,1.6666666666666666E-4,1,{"$f":"IF(Uncertainty!W108=\"\",\"\",Uncertainty!W108)","v":""},{"$f":"IF(Uncertainty!Z108=\"\",\"\",Uncertainty!Z108)","v":""},0,1E-3]
[{"$f":"'ID-numbers'!$A1248","v":"BC076"},{"$f":"VLOOKUP(A915,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity source for treatment 3 (storage)"},{"$f":"IF('Input Project'!H161=\"\",\"\",'Input Project'!H161)","v":""},{"$f":"VLOOKUP($A915,list_database1,$I$8,FALSE)","v":"n.a."},"",{"$f":"IF($L915=1,IF(MonteCarlo=1,$E915,IF($C915=\"\",$D915,$C915)),IF($C915=\"\",$D915,$C915))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1249","v":"BC077a"},{"$f":"VLOOKUP(A916,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy use for electricity production for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A916,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1250","v":"BC077b"},{"$f":"VLOOKUP(A917,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy use for electricity production for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A917,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1251","v":"BC077c"},{"$f":"VLOOKUP(A918,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to electricity production for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A918,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1254","v":"BC080a"},{"$f":"VLOOKUP(A919,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated fossil energy use after conversion 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A919,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":4.2427297465073593E-2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1255","v":"BC080b"},{"$f":"VLOOKUP(A920,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated primary energy use after conversion 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A920,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.35119170139699607},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1256","v":"BC080c"},{"$f":"VLOOKUP(A921,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated GHG emissions after conversion 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A921,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":47.891178160047083},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1257","v":"BC080d"},{"$f":"VLOOKUP(A922,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated water use after conversion 1 (per GJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A922,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":422.20878511090552},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1258","v":"BC080f"},{"$f":"VLOOKUP(A923,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated acidification potential after conversion 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A923,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.8198605978016702},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1259","v":"BC080g"},{"$f":"VLOOKUP(A924,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated eutrophication potential after conversion 1 (per MJ feedstock 1 fuel)"},null,null,{"$f":"IF(MonteCarlo=1,IF($L924=1,IF($H924=\"n.a.\",0,IF($H924<0.009,0,MIN(MAX(NORMINV(RAND(),$H924,$K924),$I924),$J924))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A924,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":3.3116164621061315},{"$f":"IF($L924=1,IF($C924=\"\",$D924,$C924),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1260","v":"BC081a"},{"$f":"VLOOKUP(A925,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated fossil energy use after conversion 2 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A925,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.17484144883990196},"",{"$f":"IF($L925=1,IF($M925=\"\",$O925,$M925),\"\")","v":""},{"$f":"IF($L925=1,IF($N925=\"\",$P925,$N925),\"\")","v":""},{"$f":"IF($L925=1,($J925-$I925)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1261","v":"BC081b"},{"$f":"VLOOKUP(A926,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated primary energy use after conversion 2 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A926,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.54981292845923868},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1262","v":"BC081c"},{"$f":"VLOOKUP(A927,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated GHG emissions after conversion 2 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A927,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":58.95757002282992},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1263","v":"BC081d"},{"$f":"VLOOKUP(A928,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated water use after conversion 2 (per GJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A928,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":422.20878511090552},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1264","v":"BC081f"},{"$f":"VLOOKUP(A929,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated acidification potential after conversion 2 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A929,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.93522944546204967},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1265","v":"BC081g"},{"$f":"VLOOKUP(A930,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated eutrophication potential after conversion 2 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A930,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":3.325394839691393},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1266","v":"BC082a"},{"$f":"VLOOKUP(A931,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use feedstock 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A931,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.17800166505611817},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1267","v":"BC082b"},{"$f":"VLOOKUP(A932,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use feedstock 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A932,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.55455325278356304},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1268","v":"BC082c"},{"$f":"VLOOKUP(A933,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions feedstock 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A933,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":59.196326779586677},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1269","v":"BC082d"},{"$f":"VLOOKUP(A934,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total water use feedstock 1 (per GJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A934,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":422.20878511090552},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1270","v":"BC082f"},{"$f":"VLOOKUP(A935,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total acidification potential feedstock 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A935,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.93786277735394152},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1271","v":"BC082g"},{"$f":"VLOOKUP(A936,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total eutrophication potential feedstock 1 (per MJ feedstock 1 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A936,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":3.3257093356913932},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1272","v":"BC083a"},{"$f":"VLOOKUP(A937,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use feedstock 1 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A937,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.17800166505611817},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1273","v":"BC083b"},{"$f":"VLOOKUP(A938,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use feedstock 1 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A938,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.55455325278356304},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1274","v":"BC083c"},{"$f":"VLOOKUP(A939,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions feedstock 1 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A939,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":59.196326779586677},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1275","v":"BC083d"},{"$f":"VLOOKUP(A940,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total water use feedstock 1 (per GJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A940,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":422.20878511090552},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1276","v":"BC083f"},{"$f":"VLOOKUP(A941,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total acidification potential feedstock 1 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A941,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.93786277735394152},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1277","v":"BC083g"},{"$f":"VLOOKUP(A942,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total eutrophication potential feedstock 1 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A942,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":3.3257093356913932},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1279","v":"BC090a"},{"$f":"VLOOKUP(A943,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in process 1"},null,null,"",null,{"$f":"VLOOKUP(A943,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1280","v":"BC090b"},{"$f":"VLOOKUP(A944,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in process 1"},null,null,"",null,{"$f":"VLOOKUP(A944,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1281","v":"BC090c"},{"$f":"VLOOKUP(A945,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions in process 1"},null,null,"",null,{"$f":"VLOOKUP(A945,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1282","v":"BC090d"},{"$f":"VLOOKUP(A946,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use in process 1"},null,null,"",null,{"$f":"VLOOKUP(A946,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1283","v":"BC090f"},{"$f":"VLOOKUP(A947,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from process 1"},null,null,"",null,{"$f":"VLOOKUP(A947,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1284","v":"BC090g"},{"$f":"VLOOKUP(A948,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from process 1"},null,null,"",null,{"$f":"VLOOKUP(A948,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.3159295156592201},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1285","v":"BC091a"},{"$f":"VLOOKUP(A949,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in process 1"},null,null,"",null,{"$f":"VLOOKUP(A949,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1286","v":"BC091b"},{"$f":"VLOOKUP(A950,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in process 1"},null,null,"",null,{"$f":"VLOOKUP(A950,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1287","v":"BC091c"},{"$f":"VLOOKUP(A951,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions in process 1"},null,null,"",null,{"$f":"VLOOKUP(A951,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1288","v":"BC091d"},{"$f":"VLOOKUP(A952,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use in process 1"},null,null,"",null,{"$f":"VLOOKUP(A952,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1289","v":"BC091f"},{"$f":"VLOOKUP(A953,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from process 1"},null,null,"",null,{"$f":"VLOOKUP(A953,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1290","v":"BC091g"},{"$f":"VLOOKUP(A954,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from process 1"},null,null,"",null,{"$f":"VLOOKUP(A954,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.3159295156592201},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1291","v":"BC092a"},{"$f":"VLOOKUP(A955,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in process 2"},null,null,"",null,{"$f":"VLOOKUP(A955,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.6357622712156819E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1292","v":"BC092b"},{"$f":"VLOOKUP(A956,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in process 2"},null,null,"",null,{"$f":"VLOOKUP(A956,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2.4536434068235229E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1293","v":"BC092c"},{"$f":"VLOOKUP(A957,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions in process 2"},null,null,"",null,{"$f":"VLOOKUP(A957,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.65300153519651516},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1294","v":"BC092d"},{"$f":"VLOOKUP(A958,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use in process 2"},null,null,"",null,{"$f":"VLOOKUP(A958,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,{"$f":"IF($L958=1,VLOOKUP($A958,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L958=1,VLOOKUP($A958,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1295","v":"BC092f"},{"$f":"VLOOKUP(A959,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from process 2"},null,null,"",null,{"$f":"VLOOKUP(A959,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1296","v":"BC092g"},{"$f":"VLOOKUP(A960,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from process 2"},null,null,"",null,{"$f":"VLOOKUP(A960,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1297","v":"BC093a"},{"$f":"VLOOKUP(A961,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in process 2"},null,null,"",null,{"$f":"VLOOKUP(A961,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.6357622712156819E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1298","v":"BC093b"},{"$f":"VLOOKUP(A962,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in process 2"},null,null,"",null,{"$f":"VLOOKUP(A962,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2.4536434068235229E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1299","v":"BC093c"},{"$f":"VLOOKUP(A963,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions in process 2"},null,null,"",null,{"$f":"VLOOKUP(A963,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.65300153519651516},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1300","v":"BC093d"},{"$f":"VLOOKUP(A964,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use in process 2"},null,null,"",null,{"$f":"VLOOKUP(A964,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1301","v":"BC093f"},{"$f":"VLOOKUP(A965,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from process 2"},null,null,"",null,{"$f":"VLOOKUP(A965,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1302","v":"BC093g"},{"$f":"VLOOKUP(A966,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from process 2"},null,null,"",null,{"$f":"VLOOKUP(A966,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1303","v":"BC094a"},{"$f":"VLOOKUP(A967,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A967,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.6357622712156819E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1304","v":"BC094b"},{"$f":"VLOOKUP(A968,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A968,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2.4536434068235229E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1305","v":"BC094c"},{"$f":"VLOOKUP(A969,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A969,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.65300153519651516},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1306","v":"BC094d"},{"$f":"VLOOKUP(A970,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A970,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1307","v":"BC094f"},{"$f":"VLOOKUP(A971,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A971,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1308","v":"BC094g"},{"$f":"VLOOKUP(A972,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A972,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.3159295156592201},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1309","v":"BC095a"},{"$f":"VLOOKUP(A973,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A973,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.6357622712156819E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1310","v":"BC095b"},{"$f":"VLOOKUP(A974,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A974,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2.4536434068235229E-3},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1311","v":"BC095c"},{"$f":"VLOOKUP(A975,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A975,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0.65300153519651516},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1312","v":"BC095d"},{"$f":"VLOOKUP(A976,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A976,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1313","v":"BC095f"},{"$f":"VLOOKUP(A977,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A977,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1314","v":"BC095g"},{"$f":"VLOOKUP(A978,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A978,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":1.3159295156592201},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1315","v":"BC100a"},{"$f":"VLOOKUP(A979,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for conversion process 1"},{"$f":"IF('Input RU'!K36=\"\",\"\",'Input RU'!K36)","v":""},{"$f":"VLOOKUP($A979,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L979=1,IF(MonteCarlo=1,$E979,IF($C979=\"\",$D979,$C979)),IF($C979=\"\",$D979,$C979))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W74=\"\",\"\",Uncertainty!W74)","v":""},{"$f":"IF(Uncertainty!Z74=\"\",\"\",Uncertainty!Z74)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1316","v":"BC100b"},{"$f":"VLOOKUP(A980,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for conversion process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1317","v":"BC101a"},{"$f":"VLOOKUP(A981,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},{"$f":"IF('Input RU'!K39=\"\",\"\",'Input RU'!K39)","v":""},{"$f":"VLOOKUP($A981,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L981=1,IF(MonteCarlo=1,$E981,IF($C981=\"\",$D981,$C981)),IF($C981=\"\",$D981,$C981))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W80=\"\",\"\",Uncertainty!W80)","v":""},{"$f":"IF(Uncertainty!Z80=\"\",\"\",Uncertainty!Z80)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1318","v":"BC101b"},{"$f":"VLOOKUP(A982,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1319","v":"BC102a"},{"$f":"VLOOKUP(A983,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for conversion process 2"},{"$f":"IF('Input RU'!K42=\"\",\"\",'Input RU'!K42)","v":""},{"$f":"VLOOKUP($A983,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L983=1,IF(MonteCarlo=1,$E983,IF($C983=\"\",$D983,$C983)),IF($C983=\"\",$D983,$C983))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W103=\"\",\"\",Uncertainty!W103)","v":""},{"$f":"IF(Uncertainty!Z103=\"\",\"\",Uncertainty!Z103)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1320","v":"BC102b"},{"$f":"VLOOKUP(A984,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for conversion process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1321","v":"BC103a"},{"$f":"VLOOKUP(A985,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},{"$f":"IF('Input RU'!K45=\"\",\"\",'Input RU'!K45)","v":""},{"$f":"VLOOKUP($A985,list_database1,$I$8,FALSE)","v":0},"",{"$f":"IF($L985=1,IF(MonteCarlo=1,$E985,IF($C985=\"\",$D985,$C985)),IF($C985=\"\",$D985,$C985))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W109=\"\",\"\",Uncertainty!W109)","v":""},{"$f":"IF(Uncertainty!Z109=\"\",\"\",Uncertainty!Z109)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1322","v":"BC103b"},{"$f":"VLOOKUP(A986,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1381","v":"BC150a"},{"$f":"VLOOKUP(A987,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour, process 1"},{"$f":"IF('Input LW'!U51=\"\",\"\",'Input LW'!U51)","v":""},{"$f":"VLOOKUP($A987,list_database1,$I$8,FALSE)","v":"Not fulfilled"},"",{"$f":"IF($L987=1,IF(MonteCarlo=1,$E987,IF($C987=\"\",$D987,$C987)),IF($C987=\"\",$D987,$C987))","v":"Not fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1382","v":"BC150b"},{"$f":"VLOOKUP(A988,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour, process 1"},{"$f":"IF('Input LW'!U52=\"\",\"\",'Input LW'!U52)","v":""},{"$f":"VLOOKUP($A988,list_database1,$I$8,FALSE)","v":"Not fulfilled"},{"$f":"IF(MonteCarlo=1,IF($L988=1,IF($H988=\"n.a.\",0,IF($H988<0.009,0,MIN(MAX(NORMINV(RAND(),$H988,$K988),$I988),$J988))),\"\"),\"\")","v":""},{"$f":"IF($L988=1,IF(MonteCarlo=1,$E988,IF($C988=\"\",$D988,$C988)),IF($C988=\"\",$D988,$C988))","v":"Not fulfilled"},null,{"$f":"IF($L988=1,IF($C988=\"\",$D988,$C988),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1383","v":"BC150c"},{"$f":"VLOOKUP(A989,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights, process 1"},{"$f":"IF('Input LW'!U53=\"\",\"\",'Input LW'!U53)","v":""},{"$f":"VLOOKUP($A989,list_database1,$I$8,FALSE)","v":"Not fulfilled"},"",{"$f":"IF($L989=1,IF(MonteCarlo=1,$E989,IF($C989=\"\",$D989,$C989)),IF($C989=\"\",$D989,$C989))","v":"Not fulfilled"},null,"",{"$f":"IF($L989=1,IF($M989=\"\",$O989,$M989),\"\")","v":""},{"$f":"IF($L989=1,IF($N989=\"\",$P989,$N989),\"\")","v":""},{"$f":"IF($L989=1,($J989-$I989)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1384","v":"BC150d"},{"$f":"VLOOKUP(A990,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination, process 1"},{"$f":"IF('Input LW'!U54=\"\",\"\",'Input LW'!U54)","v":""},{"$f":"VLOOKUP($A990,list_database1,$I$8,FALSE)","v":"Not fulfilled"},"",{"$f":"IF($L990=1,IF(MonteCarlo=1,$E990,IF($C990=\"\",$D990,$C990)),IF($C990=\"\",$D990,$C990))","v":"Not fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1385","v":"BC150e"},{"$f":"VLOOKUP(A991,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1386","v":"BC150f"},{"$f":"VLOOKUP(A992,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 1"},{"$f":"IF('Input LW'!U55=\"\",\"\",'Input LW'!U55)","v":""},{"$f":"VLOOKUP($A992,list_database1,$I$8,FALSE)","v":"Not fulfilled"},"",{"$f":"IF($L992=1,IF(MonteCarlo=1,$E992,IF($C992=\"\",$D992,$C992)),IF($C992=\"\",$D992,$C992))","v":"Not fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1387","v":"BC150g"},{"$f":"VLOOKUP(A993,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1388","v":"BC151a"},{"$f":"VLOOKUP(A994,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts, process 1"},{"$f":"IF('Input LW'!U57=\"\",\"\",'Input LW'!U57)","v":""},{"$f":"VLOOKUP($A994,list_database1,$I$8,FALSE)","v":"Not fulfilled"},"",{"$f":"IF($L994=1,IF(MonteCarlo=1,$E994,IF($C994=\"\",$D994,$C994)),IF($C994=\"\",$D994,$C994))","v":"Not fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1389","v":"BC151b"},{"$f":"VLOOKUP(A995,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights, process 1"},{"$f":"IF('Input LW'!U58=\"\",\"\",'Input LW'!U58)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1390","v":"BC151c"},{"$f":"VLOOKUP(A996,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 1"},{"$f":"IF('Input LW'!U59=\"\",\"\",'Input LW'!U59)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1391","v":"BC151d"},{"$f":"VLOOKUP(A997,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules, process 1"},{"$f":"IF('Input LW'!U60=\"\",\"\",'Input LW'!U60)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1392","v":"BC151e"},{"$f":"VLOOKUP(A998,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy, process 1"},{"$f":"IF('Input LW'!U61=\"\",\"\",'Input LW'!U61)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1393","v":"BC151f"},{"$f":"VLOOKUP(A999,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 1"},{"$f":"IF('Input LW'!U62=\"\",\"\",'Input LW'!U62)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1394","v":"BC151g"},{"$f":"VLOOKUP(A1000,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training, process 1"},{"$f":"IF('Input LW'!U63=\"\",\"\",'Input LW'!U63)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1395","v":"BC152a"},{"$f":"VLOOKUP(A1001,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour, process 2"},{"$f":"IF('Input LW'!U68=\"\",\"\",'Input LW'!U68)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1396","v":"BC152b"},{"$f":"VLOOKUP(A1002,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour, process 2"},{"$f":"IF('Input LW'!U69=\"\",\"\",'Input LW'!U69)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1397","v":"BC152c"},{"$f":"VLOOKUP(A1003,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights, process 2"},{"$f":"IF('Input LW'!U70=\"\",\"\",'Input LW'!U70)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1398","v":"BC152d"},{"$f":"VLOOKUP(A1004,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination, process 2"},{"$f":"IF('Input LW'!U71=\"\",\"\",'Input LW'!U71)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1399","v":"BC152e"},{"$f":"VLOOKUP(A1005,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1400","v":"BC152f"},{"$f":"VLOOKUP(A1006,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 2"},{"$f":"IF('Input LW'!U72=\"\",\"\",'Input LW'!U72)","v":""},{"$f":"VLOOKUP($A1006,list_database1,$I$8,FALSE)","v":"Not fulfilled"},"",{"$f":"IF($L1006=1,IF(MonteCarlo=1,$E1006,IF($C1006=\"\",$D1006,$C1006)),IF($C1006=\"\",$D1006,$C1006))","v":"Not fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1401","v":"BC152g"},{"$f":"VLOOKUP(A1007,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1402","v":"BC153a"},{"$f":"VLOOKUP(A1008,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts, process 2"},{"$f":"IF('Input LW'!U74=\"\",\"\",'Input LW'!U74)","v":""},{"$f":"VLOOKUP($A1008,list_database1,$I$8,FALSE)","v":"Not fulfilled"},"",{"$f":"IF($L1008=1,IF(MonteCarlo=1,$E1008,IF($C1008=\"\",$D1008,$C1008)),IF($C1008=\"\",$D1008,$C1008))","v":"Not fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1403","v":"BC153b"},{"$f":"VLOOKUP(A1009,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights, process 2"},{"$f":"IF('Input LW'!U75=\"\",\"\",'Input LW'!U75)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1404","v":"BC153c"},{"$f":"VLOOKUP(A1010,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 2"},{"$f":"IF('Input LW'!U76=\"\",\"\",'Input LW'!U76)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1405","v":"BC153d"},{"$f":"VLOOKUP(A1011,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules, process 2"},{"$f":"IF('Input LW'!U77=\"\",\"\",'Input LW'!U77)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1406","v":"BC153e"},{"$f":"VLOOKUP(A1012,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy, process 2"},{"$f":"IF('Input LW'!U78=\"\",\"\",'Input LW'!U78)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1407","v":"BC153f"},{"$f":"VLOOKUP(A1013,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 2"},{"$f":"IF('Input LW'!U79=\"\",\"\",'Input LW'!U79)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1408","v":"BC153g"},{"$f":"VLOOKUP(A1014,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training, process 2"},{"$f":"IF('Input LW'!U80=\"\",\"\",'Input LW'!U80)","v":""},"Not fulfilled","","Not fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1409","v":"BC154a"},{"$f":"VLOOKUP(A1015,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour, processing FS1"},null,null,"",null,{"$f":"VLOOKUP(A1015,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1410","v":"BC154b"},{"$f":"VLOOKUP(A1016,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour, processing FS1"},null,null,"",null,{"$f":"VLOOKUP(A1016,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1411","v":"BC154c"},{"$f":"VLOOKUP(A1017,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1017,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1412","v":"BC154d"},{"$f":"VLOOKUP(A1018,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1018,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1413","v":"BC154e"},{"$f":"VLOOKUP(A1019,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1019,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1414","v":"BC154f"},{"$f":"VLOOKUP(A1020,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1020,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1415","v":"BC154g"},{"$f":"VLOOKUP(A1021,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1021,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1416","v":"BC155a"},{"$f":"VLOOKUP(A1022,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1022,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1417","v":"BC155b"},{"$f":"VLOOKUP(A1023,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1023,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1418","v":"BC155c"},{"$f":"VLOOKUP(A1024,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1024,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1419","v":"BC155d"},{"$f":"VLOOKUP(A1025,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1025,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1420","v":"BC155e"},{"$f":"VLOOKUP(A1026,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1026,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1421","v":"BC155f"},{"$f":"VLOOKUP(A1027,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1027,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1422","v":"BC155g"},{"$f":"VLOOKUP(A1028,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training, processing FS1"},null,null,null,null,{"$f":"VLOOKUP(A1028,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1423","v":"BC156"},{"$f":"VLOOKUP(A1029,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights, process 1_score"},null,null,null,null,{"$f":"VLOOKUP(A1029,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":5},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1424","v":"BC157"},{"$f":"VLOOKUP(A1030,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions, process 1_score"},null,null,null,null,{"$f":"VLOOKUP(A1030,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":7},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1425","v":"BC158"},{"$f":"VLOOKUP(A1031,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights, process 2_score"},null,null,"",null,{"$f":"VLOOKUP(A1031,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":5},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1426","v":"BC159"},{"$f":"VLOOKUP(A1032,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions, process 2_score"},null,null,"",null,{"$f":"VLOOKUP(A1032,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":7},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1427","v":"BC160"},{"$f":"VLOOKUP(A1033,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights, processing overall_score"},null,null,null,null,{"$f":"VLOOKUP(A1033,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":10},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1428","v":"BC161"},{"$f":"VLOOKUP(A1034,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions, processing overall_score"},null,null,null,null,{"$f":"VLOOKUP(A1034,'Conversion feedstock1'!$D$9:$G$5197,4,FALSE)","v":14},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1430","v":"BC500a"},{"$f":"VLOOKUP(A1035,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Process 1 description "},null,{"$f":"VLOOKUP($A1035,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1035=1,IF(MonteCarlo=1,$E1035,IF($C1035=\"\",$D1035,$C1035)),IF($C1035=\"\",$D1035,$C1035))","v":"n.a."},null,"","","","",0,null,null,{"$f":"IF($L1035=1,VLOOKUP($A1035,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L1035=1,VLOOKUP($A1035,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1431","v":"BC500b"},{"$f":"VLOOKUP(A1036,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Process 2 description "},null,"n.a.","",{"$f":"IF($L1036=1,IF(MonteCarlo=1,$E1036,IF($C1036=\"\",$D1036,$C1036)),IF($C1036=\"\",$D1036,$C1036))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1432","v":"BC501a"},{"$f":"VLOOKUP(A1037,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of main output flow, process 1"},{"$f":"IF('Input Project'!H214=\"\",\"\",'Input Project'!H214)","v":"n.a."},"n.a.","",{"$f":"IF($L1037=1,IF(MonteCarlo=1,$E1037,IF($C1037=\"\",$D1037,$C1037)),IF($C1037=\"\",$D1037,$C1037))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1433","v":"BC501b"},{"$f":"VLOOKUP(A1038,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of main output flow, process 2"},{"$f":"IF('Input Project'!H277=\"\",\"\",'Input Project'!H277)","v":"n.a."},"n.a.","",{"$f":"IF($L1038=1,IF(MonteCarlo=1,$E1038,IF($C1038=\"\",$D1038,$C1038)),IF($C1038=\"\",$D1038,$C1038))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1434","v":"BC502a1"},{"$f":"VLOOKUP(A1039,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 1, process 1"},{"$f":"IF('Input Project'!H215=\"\",\"\",'Input Project'!H215)","v":""},"n.a.","",{"$f":"IF($L1039=1,IF(MonteCarlo=1,$E1039,IF($C1039=\"\",$D1039,$C1039)),IF($C1039=\"\",$D1039,$C1039))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1435","v":"BC502a10"},{"$f":"VLOOKUP(A1040,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 1, process 1"},{"$f":"IF('Input Project'!H216=\"\",\"\",'Input Project'!H216)","v":""},0,null,{"$f":"IF($L1040=1,IF(MonteCarlo=1,$E1040,IF($C1040=\"\",$D1040,$C1040)),IF($C1040=\"\",$D1040,$C1040))","v":0},null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1436","v":"BC502a11"},{"$f":"VLOOKUP(A1041,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 1, process 1"},{"$f":"IF('Input Project'!H217=\"\",\"\",'Input Project'!H217)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1041=1,IF($H1041=\"n.a.\",0,IF($H1041<0.009,0,MIN(MAX(NORMINV(RAND(),$H1041,$K1041),$I1041),$J1041))),\"\"),\"\")","v":""},{"$f":"IF($L1041=1,IF(MonteCarlo=1,$E1041,IF($C1041=\"\",$D1041,$C1041)),IF($C1041=\"\",$D1041,$C1041))","v":0},null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1437","v":"BC502a2"},{"$f":"VLOOKUP(A1042,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 2, process 1"},{"$f":"IF('Input Project'!H219=\"\",\"\",'Input Project'!H219)","v":""},"n.a.","",{"$f":"IF($L1042=1,IF(MonteCarlo=1,$E1042,IF($C1050=\"\",$D1042,$C1050)),IF($C1050=\"\",$D1042,$C1050))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1438","v":"BC502a20"},{"$f":"VLOOKUP(A1043,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 2, process 1"},{"$f":"IF('Input Project'!H220=\"\",\"\",'Input Project'!H220)","v":""},0,null,{"$f":"IF($L1043=1,IF(MonteCarlo=1,$E1043,IF($C1043=\"\",$D1043,$C1043)),IF($C1043=\"\",$D1043,$C1043))","v":0},null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1439","v":"BC502a21"},{"$f":"VLOOKUP(A1044,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 2, process 1"},{"$f":"IF('Input Project'!H221=\"\",\"\",'Input Project'!H221)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1044=1,IF($H1044=\"n.a.\",0,IF($H1044<0.009,0,MIN(MAX(NORMINV(RAND(),$H1044,$K1044),$I1044),$J1044))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1440","v":"BC502a3"},{"$f":"VLOOKUP(A1045,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 3, process 1"},{"$f":"IF('Input Project'!H223=\"\",\"\",'Input Project'!H223)","v":""},"n.a.","",{"$f":"IF($L1045=1,IF(MonteCarlo=1,$E1045,IF($C1053=\"\",$D1045,$C1053)),IF($C1053=\"\",$D1045,$C1053))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1441","v":"BC502a30"},{"$f":"VLOOKUP(A1046,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 3, process 1"},{"$f":"IF('Input Project'!H224=\"\",\"\",'Input Project'!H224)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1442","v":"BC502a31"},{"$f":"VLOOKUP(A1047,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 3, process 1"},{"$f":"IF('Input Project'!H225=\"\",\"\",'Input Project'!H225)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1047=1,IF($H1047=\"n.a.\",0,IF($H1047<0.009,0,MIN(MAX(NORMINV(RAND(),$H1047,$K1047),$I1047),$J1047))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1443","v":"BC502a41"},{"$f":"VLOOKUP(A1048,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity by-product, process 1"},{"$f":"IF('Input Project'!H227=\"\",\"\",'Input Project'!H227)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1048=1,IF($H1048=\"n.a.\",0,IF($H1048<0.009,0,MIN(MAX(NORMINV(RAND(),$H1048,$K1048),$I1048),$J1048))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1444","v":"BC502a51"},{"$f":"VLOOKUP(A1049,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat by-product, process 1"},{"$f":"IF('Input Project'!H228=\"\",\"\",'Input Project'!H228)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1049=1,IF($H1049=\"n.a.\",0,IF($H1049<0.009,0,MIN(MAX(NORMINV(RAND(),$H1049,$K1049),$I1049),$J1049))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1445","v":"BC502b1"},{"$f":"VLOOKUP(A1050,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 1, process 2"},{"$f":"IF('Input Project'!H278=\"\",\"\",'Input Project'!H278)","v":""},"n.a.","",{"$f":"IF($L1050=1,IF(MonteCarlo=1,$E1050,IF($C1053=\"\",$D1050,$C1053)),IF($C1053=\"\",$D1050,$C1053))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1446","v":"BC502b10"},{"$f":"VLOOKUP(A1051,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 1, process 2"},{"$f":"IF('Input Project'!H279=\"\",\"\",'Input Project'!H279)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1447","v":"BC502b11"},{"$f":"VLOOKUP(A1052,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 1, process 2"},{"$f":"IF('Input Project'!H280=\"\",\"\",'Input Project'!H280)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1052=1,IF($H1052=\"n.a.\",0,IF($H1052<0.009,0,MIN(MAX(NORMINV(RAND(),$H1052,$K1052),$I1052),$J1052))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1448","v":"BC502b2"},{"$f":"VLOOKUP(A1053,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 2, process 2"},{"$f":"IF('Input Project'!H282=\"\",\"\",'Input Project'!H282)","v":""},"n.a.","",{"$f":"IF($L1053=1,IF(MonteCarlo=1,$E1053,IF($C1058=\"\",$D1053,$C1058)),IF($C1058=\"\",$D1053,$C1058))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1449","v":"BC502b20"},{"$f":"VLOOKUP(A1054,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 2, process 2"},{"$f":"IF('Input Project'!H283=\"\",\"\",'Input Project'!H283)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1450","v":"BC502b21"},{"$f":"VLOOKUP(A1055,'ID-numbers'!$1:$1048576,2,FALSE)","v":"By-product flow 2, process 2"},{"$f":"IF('Input Project'!H284=\"\",\"\",'Input Project'!H284)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1055=1,IF($H1055=\"n.a.\",0,IF($H1055<0.009,0,MIN(MAX(NORMINV(RAND(),$H1055,$K1055),$I1055),$J1055))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1451","v":"BC502b41"},{"$f":"VLOOKUP(A1056,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity by-product, process 2"},{"$f":"IF('Input Project'!H286=\"\",\"\",'Input Project'!H286)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1056=1,IF($H1056=\"n.a.\",0,IF($H1056<0.009,0,MIN(MAX(NORMINV(RAND(),$H1056,$K1056),$I1056),$J1056))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1452","v":"BC502b51"},{"$f":"VLOOKUP(A1057,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat by-product, process 2"},{"$f":"IF('Input Project'!H287=\"\",\"\",'Input Project'!H287)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1057=1,IF($H1057=\"n.a.\",0,IF($H1057<0.009,0,MIN(MAX(NORMINV(RAND(),$H1057,$K1057),$I1057),$J1057))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1453","v":"BC503a1"},{"$f":"VLOOKUP(A1058,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (kg)"},null,null,"",null,{"$f":"VLOOKUP(A1058,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1454","v":"BC503a2"},{"$f":"VLOOKUP(A1059,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (kg)"},null,null,"",null,{"$f":"VLOOKUP(A1059,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1456","v":"BC503b1"},{"$f":"VLOOKUP(A1060,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (kg)"},null,null,"",null,{"$f":"VLOOKUP(A1060,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1457","v":"BC503b2"},{"$f":"VLOOKUP(A1061,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (kg)"},null,null,"",null,{"$f":"VLOOKUP(A1061,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1458","v":"BC504a1"},{"$f":"VLOOKUP(A1062,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (MJ)"},null,{"$f":"VLOOKUP($A1062,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1062=1,IF(MonteCarlo=1,$E1062,IF($C1063=\"\",$D1062,$C1063)),IF($C1063=\"\",$D1062,$C1063))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W153=\"\",\"\",Uncertainty!W153)","v":""},{"$f":"IF(Uncertainty!Z153=\"\",\"\",Uncertainty!Z153)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1459","v":"BC504a2"},{"$f":"VLOOKUP(A1063,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (MJ)"},null,0,"",{"$f":"IF($L1063=1,IF(MonteCarlo=1,$E1063,IF($C1067=\"\",$D1063,$C1067)),IF($C1067=\"\",$D1063,$C1067))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W154=\"\",\"\",Uncertainty!W154)","v":""},{"$f":"IF(Uncertainty!Z154=\"\",\"\",Uncertainty!Z154)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1460","v":"BC504a3"},{"$f":"VLOOKUP(A1064,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (MJ)"},null,0,"",{"$f":"IF($L1064=1,IF(MonteCarlo=1,$E1064,IF($C1068=\"\",$D1064,$C1068)),IF($C1068=\"\",$D1064,$C1068))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W155=\"\",\"\",Uncertainty!W155)","v":""},{"$f":"IF(Uncertainty!Z155=\"\",\"\",Uncertainty!Z155)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1461","v":"BC504a4"},{"$f":"VLOOKUP(A1065,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of electricity by-product, process 1 (MJ)"},null,0,"",{"$f":"IF($L1065=1,IF(MonteCarlo=1,$E1065,IF($C1069=\"\",$D1065,$C1069)),IF($C1069=\"\",$D1065,$C1069))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W156=\"\",\"\",Uncertainty!W156)","v":""},{"$f":"IF(Uncertainty!Z156=\"\",\"\",Uncertainty!Z156)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1462","v":"BC504a5"},{"$f":"VLOOKUP(A1066,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of heat by-product, process 1 (MJ)"},null,0,"",{"$f":"IF($L1066=1,IF(MonteCarlo=1,$E1066,IF($C1070=\"\",$D1066,$C1070)),IF($C1070=\"\",$D1066,$C1070))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W157=\"\",\"\",Uncertainty!W157)","v":""},{"$f":"IF(Uncertainty!Z157=\"\",\"\",Uncertainty!Z157)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1463","v":"BC504b1"},{"$f":"VLOOKUP(A1067,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (MJ)"},null,0,"",{"$f":"IF($L1067=1,IF(MonteCarlo=1,$E1067,IF($C1068=\"\",$D1067,$C1068)),IF($C1068=\"\",$D1067,$C1068))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W182=\"\",\"\",Uncertainty!W182)","v":""},{"$f":"IF(Uncertainty!Z182=\"\",\"\",Uncertainty!Z182)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1464","v":"BC504b2"},{"$f":"VLOOKUP(A1068,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (MJ)"},null,0,"",{"$f":"IF($L1068=1,IF(MonteCarlo=1,$E1068,IF($C1071=\"\",$D1068,$C1071)),IF($C1071=\"\",$D1068,$C1071))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W183=\"\",\"\",Uncertainty!W183)","v":""},{"$f":"IF(Uncertainty!Z183=\"\",\"\",Uncertainty!Z183)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1465","v":"BC504b4"},{"$f":"VLOOKUP(A1069,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of electricity by-product, process 2 (MJ)"},null,0,"",{"$f":"IF($L1069=1,IF(MonteCarlo=1,$E1069,IF($C1072=\"\",$D1069,$C1072)),IF($C1072=\"\",$D1069,$C1072))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W184=\"\",\"\",Uncertainty!W184)","v":""},{"$f":"IF(Uncertainty!Z184=\"\",\"\",Uncertainty!Z184)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1466","v":"BC504b5"},{"$f":"VLOOKUP(A1070,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of heat by-product, process 2 (MJ)"},null,0,"",{"$f":"IF($L1070=1,IF(MonteCarlo=1,$E1070,IF($C1073=\"\",$D1070,$C1073)),IF($C1073=\"\",$D1070,$C1073))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W185=\"\",\"\",Uncertainty!W185)","v":""},{"$f":"IF(Uncertainty!Z185=\"\",\"\",Uncertainty!Z185)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1467","v":"BC505a1"},{"$f":"VLOOKUP(A1071,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 1, process 1 (LHV)"},{"$f":"IF('Input Project'!H218=\"\",\"\",'Input Project'!H218)","v":""},0,"",{"$f":"IF($L1071=1,IF(MonteCarlo=1,$E1071,IF($C1071=\"\",$D1071,$C1071)),IF($C1071=\"\",$D1071,$C1071))","v":0},null,"","","","",0,{"$f":"IF(Uncertainty!W422=\"\",\"\",Uncertainty!W422)","v":""},{"$f":"IF(Uncertainty!Z422=\"\",\"\",Uncertainty!Z422)","v":""},{"$f":"IF($L1071=1,VLOOKUP($A1071,list_database1,$I$8+1,FALSE),\"\")","v":""},{"$f":"IF($L1071=1,VLOOKUP($A1071,list_database1,$I$8+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1468","v":"BC505a2"},{"$f":"VLOOKUP(A1072,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 2, process 1 (LHV)"},{"$f":"IF('Input Project'!H222=\"\",\"\",'Input Project'!H222)","v":""},0,"",{"$f":"IF($L1072=1,IF(MonteCarlo=1,$E1072,IF($C1072=\"\",$D1072,$C1072)),IF($C1072=\"\",$D1072,$C1072))","v":0},null,"","","","",0,{"$f":"IF(Uncertainty!W423=\"\",\"\",Uncertainty!W423)","v":""},{"$f":"IF(Uncertainty!Z423=\"\",\"\",Uncertainty!Z423)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1469","v":"BC505a3"},{"$f":"VLOOKUP(A1073,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 3, process 1 (LHV)"},{"$f":"IF('Input Project'!H226=\"\",\"\",'Input Project'!H226)","v":""},0,"",{"$f":"IF($L1073=1,IF(MonteCarlo=1,$E1073,IF($C1073=\"\",$D1073,$C1073)),IF($C1073=\"\",$D1073,$C1073))","v":0},null,"","","","",0,{"$f":"IF(Uncertainty!W424=\"\",\"\",Uncertainty!W424)","v":""},{"$f":"IF(Uncertainty!Z424=\"\",\"\",Uncertainty!Z424)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1470","v":"BC505b1"},{"$f":"VLOOKUP(A1074,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 1, process 2 (LHV)"},{"$f":"IF('Input Project'!H281=\"\",\"\",'Input Project'!H281)","v":""},0,"",{"$f":"IF($L1074=1,IF(MonteCarlo=1,$E1074,IF($C1074=\"\",$D1074,$C1074)),IF($C1074=\"\",$D1074,$C1074))","v":0},null,"","","","",0,{"$f":"IF(Uncertainty!W425=\"\",\"\",Uncertainty!W425)","v":""},{"$f":"IF(Uncertainty!Z425=\"\",\"\",Uncertainty!Z425)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1471","v":"BC505b2"},{"$f":"VLOOKUP(A1075,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of by-product 2, process 2 (LHV)"},{"$f":"IF('Input Project'!H285=\"\",\"\",'Input Project'!H285)","v":""},0,"",{"$f":"IF($L1075=1,IF(MonteCarlo=1,$E1075,IF($C1075=\"\",$D1075,$C1075)),IF($C1075=\"\",$D1075,$C1075))","v":0},null,"","","","",0,{"$f":"IF(Uncertainty!W426=\"\",\"\",Uncertainty!W426)","v":""},{"$f":"IF(Uncertainty!Z426=\"\",\"\",Uncertainty!Z426)","v":""},"",""]
[{"$f":"'ID-numbers'!$A1472","v":"BC506a1"},{"$f":"VLOOKUP(A1076,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 1, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1473","v":"BC506a2"},{"$f":"VLOOKUP(A1077,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 2, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1474","v":"BC506a3"},{"$f":"VLOOKUP(A1078,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 3, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1475","v":"BC506a4"},{"$f":"VLOOKUP(A1079,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of electricity by-product, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1476","v":"BC506a5"},{"$f":"VLOOKUP(A1080,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of heat by-product, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1477","v":"BC506b1"},{"$f":"VLOOKUP(A1081,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 1, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1478","v":"BC506b2"},{"$f":"VLOOKUP(A1082,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 2, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1479","v":"BC506b4"},{"$f":"VLOOKUP(A1083,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of electricity by-product, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1480","v":"BC506b5"},{"$f":"VLOOKUP(A1084,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of heat by-product, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1481","v":"BC507a"},{"$f":"VLOOKUP(A1085,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of main output flow, process 1 (LHV)"},{"$f":"IF('Input Project'!H254=\"\",\"\",'Input Project'!H254)","v":""},{"$f":"VLOOKUP($A1085,list_database2,$I$9,FALSE)","v":0},{"$f":"IF(MonteCarlo=1,IF($L1085=1,IF($H1085=\"n.a.\",0,IF($H1085<0.009,0,MIN(MAX(NORMINV(RAND(),$H1085,$K1085),$I1085),$J1085))),\"\"),\"\")","v":""},{"$f":"IF($L1085=1,IF(MonteCarlo=1,$E1085,IF($C1085=\"\",$D1085,$C1085)),IF($C1085=\"\",$D1085,$C1085))","v":0},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1482","v":"BC507b"},{"$f":"VLOOKUP(A1086,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of main output flow, process 2 (LHV)"},{"$f":"IF('Input Project'!H306=\"\",\"\",'Input Project'!H306)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1086=1,IF($H1086=\"n.a.\",0,IF($H1086<0.009,0,MIN(MAX(NORMINV(RAND(),$H1086,$K1086),$I1086),$J1086))),\"\"),\"\")","v":""},0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1483","v":"BC508a"},{"$f":"VLOOKUP(A1087,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate (output/input), process 1"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W152=\"\",\"\",Uncertainty!W152)","v":""},{"$f":"IF(Uncertainty!Z152=\"\",\"\",Uncertainty!Z152)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1484","v":"BC508b"},{"$f":"VLOOKUP(A1088,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate (output/input), process 2"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W181=\"\",\"\",Uncertainty!W181)","v":""},{"$f":"IF(Uncertainty!Z181=\"\",\"\",Uncertainty!Z181)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1485","v":"BC509a0"},{"$f":"VLOOKUP(A1089,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of main input,process 1"},{"$f":"IF('Input Project'!H237=\"\",\"\",'Input Project'!H237)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1486","v":"BC509a1"},{"$f":"VLOOKUP(A1090,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 1, process 1"},{"$f":"IF('Input Project'!H240=\"\",\"\",'Input Project'!H240)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1487","v":"BC509a2"},{"$f":"VLOOKUP(A1091,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 2, process 1"},{"$f":"IF('Input Project'!H244=\"\",\"\",'Input Project'!H244)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1488","v":"BC509a3"},{"$f":"VLOOKUP(A1092,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 3, process 1"},{"$f":"IF('Input Project'!H248=\"\",\"\",'Input Project'!H248)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1489","v":"BC509b1"},{"$f":"VLOOKUP(A1093,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 1, process 2"},{"$f":"IF('Input Project'!H296=\"\",\"\",'Input Project'!H296)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1490","v":"BC509b2"},{"$f":"VLOOKUP(A1094,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 2, process 2"},{"$f":"IF('Input Project'!H300=\"\",\"\",'Input Project'!H300)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1491","v":"BC509c"},{"$f":"VLOOKUP(A1095,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material output flow, process 1"},{"$f":"IF('Input Project'!H252=\"\",\"\",'Input Project'!H252)","v":""},"n.a.","","n.a."]
[{"$f":"'ID-numbers'!$A1492","v":"BC509c1"},{"$f":"VLOOKUP(A1096,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of output flow, process 1 (electricity)"},{"$f":"IF('Input Project'!H255=\"\",\"\",'Input Project'!H255)","v":""},"n.a.","","n.a."]
[{"$f":"'ID-numbers'!$A1493","v":"BC509c2"},{"$f":"VLOOKUP(A1097,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of output flow, process 1 (heat)"},{"$f":"IF('Input Project'!H256=\"\",\"\",'Input Project'!H256)","v":""},"n.a.","","n.a."]
[{"$f":"'ID-numbers'!$A1494","v":"BC509d"},{"$f":"VLOOKUP(A1098,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material output flow, process 2"},{"$f":"IF('Input Project'!H304=\"\",\"\",'Input Project'!H304)","v":""},"n.a.",{"$f":"IF(MonteCarlo=1,IF($L1098=1,IF($H1098=\"n.a.\",0,IF($H1098<0.009,0,MIN(MAX(NORMINV(RAND(),$H1098,$K1098),$I1098),$J1098))),\"\"),\"\")","v":""},"n.a."]
[{"$f":"'ID-numbers'!$A1495","v":"BC509d1"},{"$f":"VLOOKUP(A1099,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of output flow, process 2 (electricity)"},{"$f":"IF('Input Project'!H307=\"\",\"\",'Input Project'!H307)","v":""},"n.a.",{"$f":"IF(MonteCarlo=1,IF($L1099=1,IF($H1099=\"n.a.\",0,IF($H1099<0.009,0,MIN(MAX(NORMINV(RAND(),$H1099,$K1099),$I1099),$J1099))),\"\"),\"\")","v":""},"n.a."]
[{"$f":"'ID-numbers'!$A1496","v":"BC509d2"},{"$f":"VLOOKUP(A1100,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of output flow, process 2 (heat)"},{"$f":"IF('Input Project'!H308=\"\",\"\",'Input Project'!H308)","v":""},"n.a.",{"$f":"IF(MonteCarlo=1,IF($L1100=1,IF($H1100=\"n.a.\",0,IF($H1100<0.009,0,MIN(MAX(NORMINV(RAND(),$H1100,$K1100),$I1100),$J1100))),\"\"),\"\")","v":""},"n.a."]
[{"$f":"'ID-numbers'!$A1497","v":"BC510a0"},{"$f":"VLOOKUP(A1101,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Main input, process 1"},{"$f":"IF('Input Project'!H238=\"\",\"\",'Input Project'!H238)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1101=1,IF($H1101=\"n.a.\",0,IF($H1101<0.009,0,MIN(MAX(NORMINV(RAND(),$H1101,$K1101),$I1101),$J1101))),\"\"),\"\")","v":""},0,null,{"$f":"IF($L1101=1,IF($C1101=\"\",$D1101,$C1101),\"\")","v":0},0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1499","v":"BC510a01"},{"$f":"VLOOKUP(A1102,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 1, process 1"},{"$f":"IF('Input Project'!H241=\"\",\"\",'Input Project'!H241)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1102=1,IF($H1102=\"n.a.\",0,IF($H1102<0.009,0,MIN(MAX(NORMINV(RAND(),$H1102,$K1102),$I1102),$J1102))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1498","v":"BC510a"},{"$f":"VLOOKUP(A1103,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of main input, process 1"},null,0,{"$f":"IF(MonteCarlo=1,IF($L1103=1,IF($H1103=\"n.a.\",0,IF($H1103<0.009,0,MIN(MAX(NORMINV(RAND(),$H1103,$K1103),$I1103),$J1103))),\"\"),\"\")","v":""},0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W157=\"\",\"\",Uncertainty!W157)","v":""},{"$f":"IF(Uncertainty!Z157=\"\",\"\",Uncertainty!Z157)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1500","v":"BC510a1"},{"$f":"VLOOKUP(A1104,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 1, process 1"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W158=\"\",\"\",Uncertainty!W158)","v":""},{"$f":"IF(Uncertainty!Z158=\"\",\"\",Uncertainty!Z158)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1501","v":"BC510a10"},{"$f":"VLOOKUP(A1105,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 1, process 1"},{"$f":"IF('Input Project'!H242=\"\",\"\",'Input Project'!H242)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1502","v":"BC510a11"},{"$f":"VLOOKUP(A1106,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 1, process 1"},{"$f":"IF('Input Project'!H243=\"\",\"\",'Input Project'!H243)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1106=1,IF($H1106=\"n.a.\",0,IF($H1106<0.009,0,MIN(MAX(NORMINV(RAND(),$H1106,$K1106),$I1106),$J1106))),\"\"),\"\")","v":""},0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1503","v":"BC510a02"},{"$f":"VLOOKUP(A1107,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 2, process 1"},{"$f":"IF('Input Project'!H245=\"\",\"\",'Input Project'!H245)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1504","v":"BC510a2"},{"$f":"VLOOKUP(A1108,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 2, process 1"},null,0,"",0,null,0,{"$f":"IF($L1108=1,IF($M1108=\"\",$O1108,$M1108),\"\")","v":0},{"$f":"IF($L1108=1,IF($N1108=\"\",$P1108,$N1108),\"\")","v":0},{"$f":"IF($L1108=1,($J1108-$I1108)/6,\"\")","v":0},1,{"$f":"IF(Uncertainty!W159=\"\",\"\",Uncertainty!W159)","v":""},{"$f":"IF(Uncertainty!Z159=\"\",\"\",Uncertainty!Z159)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1505","v":"BC510a20"},{"$f":"VLOOKUP(A1109,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 2, process 1"},{"$f":"IF('Input Project'!H246=\"\",\"\",'Input Project'!H246)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1506","v":"BC510a21"},{"$f":"VLOOKUP(A1110,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 2, process 1"},{"$f":"IF('Input Project'!H247=\"\",\"\",'Input Project'!H247)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1110=1,IF($H1110=\"n.a.\",0,IF($H1110<0.009,0,MIN(MAX(NORMINV(RAND(),$H1110,$K1110),$I1110),$J1110))),\"\"),\"\")","v":""},0,null,"",{"$f":"IF($L1110=1,IF($M1110=\"\",$O1110,$M1110),\"\")","v":""},{"$f":"IF($L1110=1,IF($N1110=\"\",$P1110,$N1110),\"\")","v":""},{"$f":"IF($L1110=1,($J1110-$I1110)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1507","v":"BC510a03"},{"$f":"VLOOKUP(A1111,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 3, process 1"},{"$f":"IF('Input Project'!H249=\"\",\"\",'Input Project'!H249)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1508","v":"BC510a3"},{"$f":"VLOOKUP(A1112,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 3, process 1"},null,0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1509","v":"BC510a30"},{"$f":"VLOOKUP(A1113,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 3, process 1"},{"$f":"IF('Input Project'!H250=\"\",\"\",'Input Project'!H250)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1510","v":"BC510a31"},{"$f":"VLOOKUP(A1114,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 3, process 1"},{"$f":"IF('Input Project'!H251=\"\",\"\",'Input Project'!H251)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1114=1,IF($H1114=\"n.a.\",0,IF($H1114<0.009,0,MIN(MAX(NORMINV(RAND(),$H1114,$K1114),$I1114),$J1114))),\"\"),\"\")","v":""},0,null,"",{"$f":"IF($L1114=1,IF($M1114=\"\",$O1114,$M1114),\"\")","v":""},{"$f":"IF($L1114=1,IF($N1114=\"\",$P1114,$N1114),\"\")","v":""},{"$f":"IF($L1114=1,($J1114-$I1114)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1511","v":"BC510b1"},{"$f":"VLOOKUP(A1115,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 1, process 2"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W187=\"\",\"\",Uncertainty!W187)","v":""},{"$f":"IF(Uncertainty!Z187=\"\",\"\",Uncertainty!Z187)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1512","v":"BC510b10"},{"$f":"VLOOKUP(A1116,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 1, process 2"},{"$f":"IF('Input Project'!H297=\"\",\"\",'Input Project'!H297)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1513","v":"BC510b11"},{"$f":"VLOOKUP(A1117,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 1, process 2"},{"$f":"IF('Input Project'!H298=\"\",\"\",'Input Project'!H298)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1514","v":"BC510b12"},{"$f":"VLOOKUP(A1118,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 1, process 2"},{"$f":"IF('Input Project'!H299=\"\",\"\",'Input Project'!H299)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1118=1,IF($H1118=\"n.a.\",0,IF($H1118<0.009,0,MIN(MAX(NORMINV(RAND(),$H1118,$K1118),$I1118),$J1118))),\"\"),\"\")","v":""},0,null,"",{"$f":"IF($L1118=1,IF($M1118=\"\",$O1118,$M1118),\"\")","v":""},{"$f":"IF($L1118=1,IF($N1118=\"\",$P1118,$N1118),\"\")","v":""},{"$f":"IF($L1118=1,($J1118-$I1118)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1515","v":"BC510b2"},{"$f":"VLOOKUP(A1119,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 2, process 2"},null,0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W188=\"\",\"\",Uncertainty!W188)","v":""},{"$f":"IF(Uncertainty!Z188=\"\",\"\",Uncertainty!Z188)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1516","v":"BC510b20"},{"$f":"VLOOKUP(A1120,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material input flow 2, process 2"},{"$f":"IF('Input Project'!H301=\"\",\"\",'Input Project'!H301)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1517","v":"BC510b21"},{"$f":"VLOOKUP(A1121,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of material input flow 2, process 2"},{"$f":"IF('Input Project'!H302=\"\",\"\",'Input Project'!H302)","v":""},0,null,0,null,"",null,null,null,0]
[{"$f":"'ID-numbers'!$A1518","v":"BC510b22"},{"$f":"VLOOKUP(A1122,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Energy content of input flow 2, process 2"},{"$f":"IF('Input Project'!H303=\"\",\"\",'Input Project'!H303)","v":""},0,{"$f":"IF(MonteCarlo=1,IF($L1122=1,IF($H1122=\"n.a.\",0,IF($H1122<0.009,0,MIN(MAX(NORMINV(RAND(),$H1122,$K1122),$I1122),$J1122))),\"\"),\"\")","v":""},0,null,"",{"$f":"IF($L1122=1,IF($M1122=\"\",$O1122,$M1122),\"\")","v":""},{"$f":"IF($L1122=1,IF($N1122=\"\",$P1122,$N1122),\"\")","v":""},{"$f":"IF($L1122=1,($J1122-$I1122)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1519","v":"BC510c"},{"$f":"VLOOKUP(A1123,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 1"},null,0,"",0]
[{"$f":"'ID-numbers'!$A1520","v":"BC510c0"},{"$f":"VLOOKUP(A1124,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material output flow, process 1"},{"$f":"IF('Input Project'!H253=\"\",\"\",'Input Project'!H253)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1521","v":"BC510c1"},{"$f":"VLOOKUP(A1125,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 1 (electricity)"},null,0,"",0]
[{"$f":"'ID-numbers'!$A1522","v":"BC510c2"},{"$f":"VLOOKUP(A1126,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 1 (heat)"},null,0,"",0]
[{"$f":"'ID-numbers'!$A1523","v":"BC510d"},{"$f":"VLOOKUP(A1127,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 2"},null,0,"",0]
[{"$f":"'ID-numbers'!$A1524","v":"BC510d0"},{"$f":"VLOOKUP(A1128,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Material output flow, process 2"},{"$f":"IF('Input Project'!H305=\"\",\"\",'Input Project'!H305)","v":""},0,"",0,null,0,0,0,0,1,null,null,0,0]
[{"$f":"'ID-numbers'!$A1525","v":"BC510d1"},{"$f":"VLOOKUP(A1129,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 2 (electricity)"},null,0,"",0]
[{"$f":"'ID-numbers'!$A1526","v":"BC510d2"},{"$f":"VLOOKUP(A1130,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material output flow, process 2 (heat)"},null,0,"",0]
[{"$f":"'ID-numbers'!$A1527","v":"BC511a1"},{"$f":"VLOOKUP(A1131,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 1, process 1"},{"$f":"IF('Input Project'!H229=\"\",\"\",'Input Project'!H229)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1528","v":"BC511a2"},{"$f":"VLOOKUP(A1132,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 2, process 1"},{"$f":"IF('Input Project'!H231=\"\",\"\",'Input Project'!H231)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1529","v":"BC511b1"},{"$f":"VLOOKUP(A1133,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 1, process 2"},{"$f":"IF('Input Project'!H288=\"\",\"\",'Input Project'!H288)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1530","v":"BC511b2"},{"$f":"VLOOKUP(A1134,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 2, process 2"},{"$f":"IF('Input Project'!H290=\"\",\"\",'Input Project'!H290)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1531","v":"BC512a"},{"$f":"VLOOKUP(A1135,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of main output flow, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1532","v":"BC512b"},{"$f":"VLOOKUP(A1136,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of main output flow, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1533","v":"BC514a"},{"$f":"VLOOKUP(A1137,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 2 per ha after conversion process 1"},null,null,"",null,{"$f":"VLOOKUP(A1137,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1534","v":"BC514b"},{"$f":"VLOOKUP(A1138,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of feedstock 2 per ha after conversion process 1"},null,null,"",null,{"$f":"VLOOKUP(A1138,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1535","v":"BC514c"},{"$f":"VLOOKUP(A1139,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of feedstock 2 per ha after conversion process 1"},null,null,"",null,{"$f":"VLOOKUP(A1139,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1536","v":"BC515a"},{"$f":"VLOOKUP(A1140,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 2 per ha after conversion process 2"},null,null,"",null,{"$f":"VLOOKUP(A1140,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1537","v":"BC515b"},{"$f":"VLOOKUP(A1141,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (dry) of feedstock 2 per ha after conversion process 2"},null,null,"",null,{"$f":"VLOOKUP(A1141,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1538","v":"BC515c"},{"$f":"VLOOKUP(A1142,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Yield rate (energy) of feedstock 2 per ha after conversion process 2"},null,null,"",null,{"$f":"VLOOKUP(A1142,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1539","v":"BC516a"},{"$f":"VLOOKUP(A1143,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K50=\"\",\"\",'Input EQ'!K50)","v":""},{"$f":"VLOOKUP($A1143,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1143=1,IF(MonteCarlo=1,$E1143,IF($C1143=\"\",$D1143,$C1143)),IF($C1143=\"\",$D1143,$C1143))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W160=\"\",\"\",Uncertainty!W160)","v":""},{"$f":"IF(Uncertainty!Z160=\"\",\"\",Uncertainty!Z160)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1540","v":"BC516b"},{"$f":"VLOOKUP(A1144,'ID-numbers'!$1:$1048576,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K51=\"\",\"\",'Input EQ'!K51)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W161=\"\",\"\",Uncertainty!W161)","v":""},{"$f":"IF(Uncertainty!Z161=\"\",\"\",Uncertainty!Z161)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1541","v":"BC516c"},{"$f":"VLOOKUP(A1145,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K52=\"\",\"\",'Input EQ'!K52)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W162=\"\",\"\",Uncertainty!W162)","v":""},{"$f":"IF(Uncertainty!Z162=\"\",\"\",Uncertainty!Z162)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1542","v":"BC516d"},{"$f":"VLOOKUP(A1146,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K53=\"\",\"\",'Input EQ'!K53)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W163=\"\",\"\",Uncertainty!W163)","v":""},{"$f":"IF(Uncertainty!Z163=\"\",\"\",Uncertainty!Z163)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1543","v":"BC516e"},{"$f":"VLOOKUP(A1147,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K54=\"\",\"\",'Input EQ'!K54)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W164=\"\",\"\",Uncertainty!W164)","v":""},{"$f":"IF(Uncertainty!Z164=\"\",\"\",Uncertainty!Z164)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1544","v":"BC516f"},{"$f":"VLOOKUP(A1148,'ID-numbers'!$1:$1048576,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K55=\"\",\"\",'Input EQ'!K55)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W165=\"\",\"\",Uncertainty!W165)","v":""},{"$f":"IF(Uncertainty!Z165=\"\",\"\",Uncertainty!Z165)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1545","v":"BC516g"},{"$f":"VLOOKUP(A1149,'ID-numbers'!$1:$1048576,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 1"},{"$f":"IF('Input EQ'!K56=\"\",\"\",'Input EQ'!K56)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W166=\"\",\"\",Uncertainty!W166)","v":""},{"$f":"IF(Uncertainty!Z166=\"\",\"\",Uncertainty!Z166)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1546","v":"BC517a"},{"$f":"VLOOKUP(A1150,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K59=\"\",\"\",'Input EQ'!K59)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W189=\"\",\"\",Uncertainty!W189)","v":""},{"$f":"IF(Uncertainty!Z189=\"\",\"\",Uncertainty!Z189)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1547","v":"BC517b"},{"$f":"VLOOKUP(A1151,'ID-numbers'!$1:$1048576,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K60=\"\",\"\",'Input EQ'!K60)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W190=\"\",\"\",Uncertainty!W190)","v":""},{"$f":"IF(Uncertainty!Z190=\"\",\"\",Uncertainty!Z190)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1548","v":"BC517c"},{"$f":"VLOOKUP(A1152,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K61=\"\",\"\",'Input EQ'!K61)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W191=\"\",\"\",Uncertainty!W191)","v":""},{"$f":"IF(Uncertainty!Z191=\"\",\"\",Uncertainty!Z191)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1549","v":"BC517d"},{"$f":"VLOOKUP(A1153,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K62=\"\",\"\",'Input EQ'!K62)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W192=\"\",\"\",Uncertainty!W192)","v":""},{"$f":"IF(Uncertainty!Z192=\"\",\"\",Uncertainty!Z192)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1550","v":"BC517e"},{"$f":"VLOOKUP(A1154,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K63=\"\",\"\",'Input EQ'!K63)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W193=\"\",\"\",Uncertainty!W193)","v":""},{"$f":"IF(Uncertainty!Z193=\"\",\"\",Uncertainty!Z193)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1551","v":"BC517f"},{"$f":"VLOOKUP(A1155,'ID-numbers'!$1:$1048576,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K64=\"\",\"\",'Input EQ'!K64)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W194=\"\",\"\",Uncertainty!W194)","v":""},{"$f":"IF(Uncertainty!Z194=\"\",\"\",Uncertainty!Z194)","v":""},{"$f":"IF($L1155=1,VLOOKUP($A1155,list_database2,$I$9+1,FALSE),\"\")","v":0},{"$f":"IF($L1155=1,VLOOKUP($A1155,list_database2,$I$9+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1552","v":"BC517g"},{"$f":"VLOOKUP(A1156,'ID-numbers'!$1:$1048576,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 2"},{"$f":"IF('Input EQ'!K65=\"\",\"\",'Input EQ'!K65)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W195=\"\",\"\",Uncertainty!W195)","v":""},{"$f":"IF(Uncertainty!Z195=\"\",\"\",Uncertainty!Z195)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1555","v":"BC520a"},{"$f":"VLOOKUP(A1157,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1157,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1556","v":"BC520b"},{"$f":"VLOOKUP(A1158,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1158,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1557","v":"BC521a"},{"$f":"VLOOKUP(A1159,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1159,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1558","v":"BC521b"},{"$f":"VLOOKUP(A1160,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1160,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1559","v":"BC522a"},{"$f":"VLOOKUP(A1161,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-products, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1161,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1560","v":"BC522b"},{"$f":"VLOOKUP(A1162,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-products, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1162,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1561","v":"BC524a"},{"$f":"VLOOKUP(A1163,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to electricity input, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1163,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1562","v":"BC524b"},{"$f":"VLOOKUP(A1164,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to electricity input, process 2"},null,null,"",{"$f":"IF($L1164=1,IF(MonteCarlo=1,$E1164,IF($C1166=\"\",$D1164,$C1166)),IF($C1166=\"\",$D1164,$C1166))","v":0},{"$f":"VLOOKUP(A1164,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1563","v":"BC525a"},{"$f":"VLOOKUP(A1165,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to electricity input, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1165,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1564","v":"BC525b"},{"$f":"VLOOKUP(A1166,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to electricity input, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1166,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1565","v":"BC526a"},{"$f":"VLOOKUP(A1167,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of electricity input 1, process 1"},null,{"$f":"VLOOKUP($A1167,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1167=1,IF(MonteCarlo=1,$E1167,IF($C1171=\"\",$D1167,$C1171)),IF($C1171=\"\",$D1167,$C1171))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W157=\"\",\"\",Uncertainty!W157)","v":""},{"$f":"IF(Uncertainty!Z157=\"\",\"\",Uncertainty!Z157)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1566","v":"BC526a0"},{"$f":"VLOOKUP(A1168,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity flow 1, process 1"},{"$f":"IF('Input Project'!H234=\"\",\"\",'Input Project'!H234)","v":""},0,"",{"$f":"IF($L1168=1,IF(MonteCarlo=1,$E1168,IF($C1172=\"\",$D1168,$C1172)),IF($C1172=\"\",$D1168,$C1172))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W158=\"\",\"\",Uncertainty!W158)","v":""},{"$f":"IF(Uncertainty!Z158=\"\",\"\",Uncertainty!Z158)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1567","v":"BC526a1"},{"$f":"VLOOKUP(A1169,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of electricity input 2, process 1"},null,0,"",{"$f":"IF($L1169=1,IF(MonteCarlo=1,$E1169,IF($C1175=\"\",$D1169,$C1175)),IF($C1175=\"\",$D1169,$C1175))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W158=\"\",\"\",Uncertainty!W158)","v":""},{"$f":"IF(Uncertainty!Z158=\"\",\"\",Uncertainty!Z158)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1568","v":"BC526a10"},{"$f":"VLOOKUP(A1170,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity flow 2, process 1"},{"$f":"IF('Input Project'!H236=\"\",\"\",'Input Project'!H236)","v":""},0,"",{"$f":"IF($L1170=1,IF(MonteCarlo=1,$E1170,IF($C1174=\"\",$D1170,$C1174)),IF($C1174=\"\",$D1170,$C1174))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W160=\"\",\"\",Uncertainty!W160)","v":""},{"$f":"IF(Uncertainty!Z160=\"\",\"\",Uncertainty!Z160)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1569","v":"BC526b"},{"$f":"VLOOKUP(A1171,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of electricity input 1, process 2"},null,0,"",{"$f":"IF($L1171=1,IF(MonteCarlo=1,$E1171,IF($C1177=\"\",$D1171,$C1177)),IF($C1177=\"\",$D1171,$C1177))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W186=\"\",\"\",Uncertainty!W186)","v":""},{"$f":"IF(Uncertainty!Z186=\"\",\"\",Uncertainty!Z186)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1570","v":"BC526b0"},{"$f":"VLOOKUP(A1172,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity flow 1, process 2"},{"$f":"IF('Input Project'!H293=\"\",\"\",'Input Project'!H293)","v":""},0,"",{"$f":"IF($L1172=1,IF(MonteCarlo=1,$E1172,IF($C1176=\"\",$D1172,$C1176)),IF($C1176=\"\",$D1172,$C1176))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W162=\"\",\"\",Uncertainty!W162)","v":""},{"$f":"IF(Uncertainty!Z162=\"\",\"\",Uncertainty!Z162)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1571","v":"BC526b1"},{"$f":"VLOOKUP(A1173,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of electricity input 2, process 2"},null,0,"",{"$f":"IF($L1173=1,IF(MonteCarlo=1,$E1173,IF($C1179=\"\",$D1173,$C1179)),IF($C1179=\"\",$D1173,$C1179))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W187=\"\",\"\",Uncertainty!W187)","v":""},{"$f":"IF(Uncertainty!Z187=\"\",\"\",Uncertainty!Z187)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1572","v":"BC526b10"},{"$f":"VLOOKUP(A1174,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity flow 2, process 2"},{"$f":"IF('Input Project'!H295=\"\",\"\",'Input Project'!H295)","v":""},0,"",{"$f":"IF($L1174=1,IF(MonteCarlo=1,$E1174,IF($C1178=\"\",$D1174,$C1178)),IF($C1178=\"\",$D1174,$C1178))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W164=\"\",\"\",Uncertainty!W164)","v":""},{"$f":"IF(Uncertainty!Z164=\"\",\"\",Uncertainty!Z164)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1573","v":"BC527a"},{"$f":"VLOOKUP(A1175,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of electricity flow 1, process 1"},{"$f":"IF('Input Project'!H233=\"\",\"\",'Input Project'!H233)","v":""},"n.a.","",{"$f":"IF($L1175=1,IF(MonteCarlo=1,$E1175,IF($C1179=\"\",$D1175,$C1179)),IF($C1179=\"\",$D1175,$C1179))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1574","v":"BC527a1"},{"$f":"VLOOKUP(A1176,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of electricity flow 2, process 1"},{"$f":"IF('Input Project'!H235=\"\",\"\",'Input Project'!H235)","v":""},"n.a.","",{"$f":"IF($L1176=1,IF(MonteCarlo=1,$E1176,IF($C1181=\"\",$D1176,$C1181)),IF($C1181=\"\",$D1176,$C1181))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1575","v":"BC527b"},{"$f":"VLOOKUP(A1177,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of electricity flow 1, process 2"},{"$f":"IF('Input Project'!H292=\"\",\"\",'Input Project'!H292)","v":""},"n.a.","",{"$f":"IF($L1177=1,IF(MonteCarlo=1,$E1177,IF($C1181=\"\",$D1177,$C1181)),IF($C1181=\"\",$D1177,$C1181))","v":"n.a."},null,"",{"$f":"IF($L1177=1,IF($M1177=\"\",$O1177,$M1177),\"\")","v":""},"","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1576","v":"BC527b1"},{"$f":"VLOOKUP(A1178,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of electricity flow 2, process 2"},{"$f":"IF('Input Project'!H294=\"\",\"\",'Input Project'!H294)","v":""},"n.a.","",{"$f":"IF($L1178=1,IF(MonteCarlo=1,$E1178,IF($C1183=\"\",$D1178,$C1183)),IF($C1183=\"\",$D1178,$C1183))","v":"n.a."},null,"",{"$f":"IF($L1178=1,IF($M1178=\"\",$O1178,$M1178),\"\")","v":""},"","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1577","v":"BC528a"},{"$f":"VLOOKUP(A1179,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1179,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1578","v":"BC528a1"},{"$f":"VLOOKUP(A1180,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1180,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1579","v":"BC528b"},{"$f":"VLOOKUP(A1181,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1181,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1580","v":"BC528b1"},{"$f":"VLOOKUP(A1182,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1182,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1581","v":"BC529a"},{"$f":"VLOOKUP(A1183,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1183,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1582","v":"BC529a1"},{"$f":"VLOOKUP(A1184,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1184,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1583","v":"BC529b"},{"$f":"VLOOKUP(A1185,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1185,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1584","v":"BC529b1"},{"$f":"VLOOKUP(A1186,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1186,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1585","v":"BC530a"},{"$f":"VLOOKUP(A1187,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1187,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1586","v":"BC530b"},{"$f":"VLOOKUP(A1188,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1188,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1587","v":"BC531a1"},{"$f":"VLOOKUP(A1189,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat input 1, process 1"},null,{"$f":"VLOOKUP($A1189,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1189=1,IF(MonteCarlo=1,$E1189,IF($C1191=\"\",$D1189,$C1191)),IF($C1191=\"\",$D1189,$C1191))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W155=\"\",\"\",Uncertainty!W155)","v":""},{"$f":"IF(Uncertainty!Z155=\"\",\"\",Uncertainty!Z155)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1588","v":"BC531a10"},{"$f":"VLOOKUP(A1190,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fuel/heat flow 1, process 1"},{"$f":"IF('Input Project'!H230=\"\",\"\",'Input Project'!H230)","v":""},0,"",{"$f":"IF($L1190=1,IF(MonteCarlo=1,$E1190,IF($C1192=\"\",$D1190,$C1192)),IF($C1192=\"\",$D1190,$C1192))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W156=\"\",\"\",Uncertainty!W156)","v":""},{"$f":"IF(Uncertainty!Z156=\"\",\"\",Uncertainty!Z156)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1589","v":"BC531a2"},{"$f":"VLOOKUP(A1191,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat input 2, process 1"},null,0,"",{"$f":"IF($L1191=1,IF(MonteCarlo=1,$E1191,IF($C1195=\"\",$D1191,$C1195)),IF($C1195=\"\",$D1191,$C1195))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W156=\"\",\"\",Uncertainty!W156)","v":""},{"$f":"IF(Uncertainty!Z156=\"\",\"\",Uncertainty!Z156)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1590","v":"BC531a20"},{"$f":"VLOOKUP(A1192,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fuel/heat flow 2, process 1"},{"$f":"IF('Input Project'!H232=\"\",\"\",'Input Project'!H232)","v":""},0,"",{"$f":"IF($L1192=1,IF(MonteCarlo=1,$E1192,IF($C1194=\"\",$D1192,$C1194)),IF($C1194=\"\",$D1192,$C1194))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W158=\"\",\"\",Uncertainty!W158)","v":""},{"$f":"IF(Uncertainty!Z158=\"\",\"\",Uncertainty!Z158)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1591","v":"BC531b1"},{"$f":"VLOOKUP(A1193,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat input 1, process 2"},null,0,"",{"$f":"IF($L1193=1,IF(MonteCarlo=1,$E1193,IF($C1197=\"\",$D1193,$C1197)),IF($C1197=\"\",$D1193,$C1197))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W184=\"\",\"\",Uncertainty!W184)","v":""},{"$f":"IF(Uncertainty!Z184=\"\",\"\",Uncertainty!Z184)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1592","v":"BC531b10"},{"$f":"VLOOKUP(A1194,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fuel/heat flow 1, process 2"},{"$f":"IF('Input Project'!H289=\"\",\"\",'Input Project'!H289)","v":""},0,"",{"$f":"IF($L1194=1,IF(MonteCarlo=1,$E1194,IF($C1196=\"\",$D1194,$C1196)),IF($C1196=\"\",$D1194,$C1196))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W160=\"\",\"\",Uncertainty!W160)","v":""},{"$f":"IF(Uncertainty!Z160=\"\",\"\",Uncertainty!Z160)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1593","v":"BC531b2"},{"$f":"VLOOKUP(A1195,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat input 2, process 2"},null,0,"",{"$f":"IF($L1195=1,IF(MonteCarlo=1,$E1195,IF($C1198=\"\",$D1195,$C1198)),IF($C1198=\"\",$D1195,$C1198))","v":0},null,0,0,{"$f":"IF($L1195=1,IF($N1195=\"\",$P1195,$N1195),\"\")","v":0},0,1,{"$f":"IF(Uncertainty!W185=\"\",\"\",Uncertainty!W185)","v":""},{"$f":"IF(Uncertainty!Z185=\"\",\"\",Uncertainty!Z185)","v":""},{"$f":"IF($L1195=1,VLOOKUP($A1195,list_database2,$I$9+1,FALSE),\"\")","v":0},0]
[{"$f":"'ID-numbers'!$A1594","v":"BC531b20"},{"$f":"VLOOKUP(A1196,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fuel/heat flow 2, process 2"},{"$f":"IF('Input Project'!H291=\"\",\"\",'Input Project'!H291)","v":""},0,"",{"$f":"IF($L1196=1,IF(MonteCarlo=1,$E1196,IF($C1198=\"\",$D1196,$C1198)),IF($C1198=\"\",$D1196,$C1198))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W162=\"\",\"\",Uncertainty!W162)","v":""},{"$f":"IF(Uncertainty!Z162=\"\",\"\",Uncertainty!Z162)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1595","v":"BC532a1"},{"$f":"VLOOKUP(A1197,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1197,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1596","v":"BC532a2"},{"$f":"VLOOKUP(A1198,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1198,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1597","v":"BC532b1"},{"$f":"VLOOKUP(A1199,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1199,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1598","v":"BC532b2"},{"$f":"VLOOKUP(A1200,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1200,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1599","v":"BC533a1"},{"$f":"VLOOKUP(A1201,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1201,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1600","v":"BC533a2"},{"$f":"VLOOKUP(A1202,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1202,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1601","v":"BC533b1"},{"$f":"VLOOKUP(A1203,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, process 2"},null,null,{"$f":"IF(MonteCarlo=1,IF($L1203=1,IF($H1203=\"n.a.\",0,IF($H1203<0.009,0,MIN(MAX(NORMINV(RAND(),$H1203,$K1203),$I1203),$J1203))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A1203,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},{"$f":"IF($L1203=1,IF($C1203=\"\",$D1203,$C1203),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1602","v":"BC533b2"},{"$f":"VLOOKUP(A1204,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1204,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"",{"$f":"IF($L1204=1,IF($M1204=\"\",$O1204,$M1204),\"\")","v":""},{"$f":"IF($L1204=1,IF($N1204=\"\",$P1204,$N1204),\"\")","v":""},{"$f":"IF($L1204=1,($J1204-$I1204)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1603","v":"BC534a"},{"$f":"VLOOKUP(A1205,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to fuel/heat input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1205,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1604","v":"BC534b"},{"$f":"VLOOKUP(A1206,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to fuel/heat input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1206,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1605","v":"BC535a"},{"$f":"VLOOKUP(A1207,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to material input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1207,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1606","v":"BC535a1"},{"$f":"VLOOKUP(A1208,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1208,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1607","v":"BC535a2"},{"$f":"VLOOKUP(A1209,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1209,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1608","v":"BC535a3"},{"$f":"VLOOKUP(A1210,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 3, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1210,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1609","v":"BC535b"},{"$f":"VLOOKUP(A1211,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to material input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1211,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1610","v":"BC535b1"},{"$f":"VLOOKUP(A1212,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1212,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1611","v":"BC535b2"},{"$f":"VLOOKUP(A1213,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1213,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1612","v":"BC535c"},{"$f":"VLOOKUP(A1214,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material output flow, process 1"}]
[{"$f":"'ID-numbers'!$A1613","v":"BC535c1"},{"$f":"VLOOKUP(A1215,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for output flow, process 1 (electricity)"}]
[{"$f":"'ID-numbers'!$A1614","v":"BC535c2"},{"$f":"VLOOKUP(A1216,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for output flow, process 1 (heat)"}]
[{"$f":"'ID-numbers'!$A1615","v":"BC535d"},{"$f":"VLOOKUP(A1217,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material output flow, process 2"}]
[{"$f":"'ID-numbers'!$A1616","v":"BC535d1"},{"$f":"VLOOKUP(A1218,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for output flow, process 2 (electricity)"}]
[{"$f":"'ID-numbers'!$A1617","v":"BC535d2"},{"$f":"VLOOKUP(A1219,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for output flow, process 2 (heat)"}]
[{"$f":"'ID-numbers'!$A1618","v":"BC536a"},{"$f":"VLOOKUP(A1220,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to material input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1220,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1619","v":"BC536a0"},{"$f":"VLOOKUP(A1221,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for main input, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1221,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1620","v":"BC536a1"},{"$f":"VLOOKUP(A1222,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1222,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1621","v":"BC536a2"},{"$f":"VLOOKUP(A1223,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1223,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1622","v":"BC536a3"},{"$f":"VLOOKUP(A1224,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 3, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1224,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1623","v":"BC536b"},{"$f":"VLOOKUP(A1225,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to material input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1225,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1624","v":"BC536b1"},{"$f":"VLOOKUP(A1226,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1226,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1625","v":"BC536b2"},{"$f":"VLOOKUP(A1227,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1227,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1626","v":"BC536c"},{"$f":"VLOOKUP(A1228,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material output flow, process 1"}]
[{"$f":"'ID-numbers'!$A1627","v":"BC536c1"},{"$f":"VLOOKUP(A1229,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for  output flow, process 1 (electricity)"}]
[{"$f":"'ID-numbers'!$A1628","v":"BC536c2"},{"$f":"VLOOKUP(A1230,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for output flow, process 1 (heat)"}]
[{"$f":"'ID-numbers'!$A1629","v":"BC536d"},{"$f":"VLOOKUP(A1231,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material output flow, process 2"}]
[{"$f":"'ID-numbers'!$A1630","v":"BC536d1"},{"$f":"VLOOKUP(A1232,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for output flow, process 2 (electricity)"}]
[{"$f":"'ID-numbers'!$A1631","v":"BC536d2"},{"$f":"VLOOKUP(A1233,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for output flow, process 2 (heat)"}]
[{"$f":"'ID-numbers'!$A1632","v":"BC537a"},{"$f":"VLOOKUP(A1234,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to process 1"},null,null,"",null,{"$f":"VLOOKUP(A1234,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1633","v":"BC537b"},{"$f":"VLOOKUP(A1235,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to process 2"},null,null,"",null,{"$f":"VLOOKUP(A1235,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1634","v":"BC541a"},{"$f":"VLOOKUP(A1236,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to electricity input, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1236,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1635","v":"BC541b"},{"$f":"VLOOKUP(A1237,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to electricity input, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1237,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1636","v":"BC542a"},{"$f":"VLOOKUP(A1238,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1238,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1637","v":"BC542a1"},{"$f":"VLOOKUP(A1239,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1239,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1638","v":"BC542b"},{"$f":"VLOOKUP(A1240,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1240,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1639","v":"BC542b1"},{"$f":"VLOOKUP(A1241,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1241,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1640","v":"BC543a"},{"$f":"VLOOKUP(A1242,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to fuel/heat input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1242,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1641","v":"BC543a1"},{"$f":"VLOOKUP(A1243,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1243,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1642","v":"BC543a2"},{"$f":"VLOOKUP(A1244,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1244,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1643","v":"BC543b"},{"$f":"VLOOKUP(A1245,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to fuel/heat input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1245,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1644","v":"BC543b1"},{"$f":"VLOOKUP(A1246,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1246,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1645","v":"BC543b2"},{"$f":"VLOOKUP(A1247,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1247,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1646","v":"BC547a"},{"$f":"VLOOKUP(A1248,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to material input flows, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1248,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1647","v":"BC547a1"},{"$f":"VLOOKUP(A1249,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1249,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1648","v":"BC547a2"},{"$f":"VLOOKUP(A1250,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1250,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1649","v":"BC547a3"},{"$f":"VLOOKUP(A1251,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 3, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1251,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1650","v":"BC547b"},{"$f":"VLOOKUP(A1252,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to material input flows, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1252,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1651","v":"BC547b1"},{"$f":"VLOOKUP(A1253,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1253,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,{"$f":"IF($L1253=1,VLOOKUP($A1253,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L1253=1,VLOOKUP($A1253,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1652","v":"BC547b2"},{"$f":"VLOOKUP(A1254,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1254,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1653","v":"BC547c"},{"$f":"VLOOKUP(A1255,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material output flow, process 1"}]
[{"$f":"'ID-numbers'!$A1654","v":"BC547c1"},{"$f":"VLOOKUP(A1256,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to output flow, process 1 (electricity)"}]
[{"$f":"'ID-numbers'!$A1655","v":"BC547c2"},{"$f":"VLOOKUP(A1257,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to output flow, process 1 (heat)"}]
[{"$f":"'ID-numbers'!$A1656","v":"BC547d"},{"$f":"VLOOKUP(A1258,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material output flow, process 2"}]
[{"$f":"'ID-numbers'!$A1657","v":"BC547d1"},{"$f":"VLOOKUP(A1259,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to output flow, process 2 (electricity)"}]
[{"$f":"'ID-numbers'!$A1658","v":"BC547d2"},{"$f":"VLOOKUP(A1260,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to output flow, process 2 (heat)"}]
[{"$f":"'ID-numbers'!$A1659","v":"BC550a"},{"$f":"VLOOKUP(A1261,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to energy crop, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1261,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":100},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1660","v":"BC550b"},{"$f":"VLOOKUP(A1262,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to energy crop, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1262,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":100},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1661","v":"BC551a1"},{"$f":"VLOOKUP(A1263,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 1, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1263,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1662","v":"BC551a2"},{"$f":"VLOOKUP(A1264,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 2, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1264,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1663","v":"BC551a3"},{"$f":"VLOOKUP(A1265,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 3, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1265,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1664","v":"BC551a4"},{"$f":"VLOOKUP(A1266,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to electricity by-product, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1266,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1665","v":"BC551a5"},{"$f":"VLOOKUP(A1267,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to heat by-product, process 1"},null,null,"",null,{"$f":"VLOOKUP(A1267,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1666","v":"BC551b1"},{"$f":"VLOOKUP(A1268,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 1, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1268,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1667","v":"BC551b2"},{"$f":"VLOOKUP(A1269,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 2, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1269,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1668","v":"BC551b4"},{"$f":"VLOOKUP(A1270,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to electricity by-product, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1270,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1669","v":"BC551b5"},{"$f":"VLOOKUP(A1271,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to heat by-product, process 2"},null,null,"",null,{"$f":"VLOOKUP(A1271,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1670","v":"BC559a"},{"$f":"VLOOKUP(A1272,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for treatment 2 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1272,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1671","v":"BC559b"},{"$f":"VLOOKUP(A1273,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for treatment 2 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1273,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1672","v":"BC559c"},{"$f":"VLOOKUP(A1274,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with treatment 2 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1274,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1675","v":"BC560"},{"$f":"VLOOKUP(A1275,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat energy use for treatment 2 (storage)"},{"$f":"IF('Input Project'!H261=\"\",\"\",'Input Project'!H261)","v":""},{"$f":"VLOOKUP($A1275,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1275=1,IF(MonteCarlo=1,$E1275,IF($C1275=\"\",$D1275,$C1275)),IF($C1275=\"\",$D1275,$C1275))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W171=\"\",\"\",Uncertainty!W171)","v":""},{"$f":"IF(Uncertainty!Z171=\"\",\"\",Uncertainty!Z171)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1676","v":"BC561"},{"$f":"VLOOKUP(A1276,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat source for treatment 2 (storage)"},{"$f":"IF('Input Project'!H260=\"\",\"\",'Input Project'!H260)","v":""},{"$f":"VLOOKUP($A1276,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1276=1,IF(MonteCarlo=1,$E1276,IF($C1276=\"\",$D1276,$C1276)),IF($C1276=\"\",$D1276,$C1276))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1682","v":"BC565"},{"$f":"VLOOKUP(A1277,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity energy use for treatment 2 (storage)"},{"$f":"IF('Input Project'!H263=\"\",\"\",'Input Project'!H263)","v":""},{"$f":"VLOOKUP($A1277,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1277=1,IF(MonteCarlo=1,$E1277,IF($C1277=\"\",$D1277,$C1277)),IF($C1277=\"\",$D1277,$C1277))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W172=\"\",\"\",Uncertainty!W172)","v":""},{"$f":"IF(Uncertainty!Z172=\"\",\"\",Uncertainty!Z172)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1683","v":"BC566"},{"$f":"VLOOKUP(A1278,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity source for treatment 2 (storage)"},{"$f":"IF('Input Project'!H262=\"\",\"\",'Input Project'!H262)","v":""},{"$f":"VLOOKUP($A1278,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1278=1,IF(MonteCarlo=1,$E1278,IF($C1278=\"\",$D1278,$C1278)),IF($C1278=\"\",$D1278,$C1278))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1689","v":"BC569a"},{"$f":"VLOOKUP(A1279,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1279,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1690","v":"BC569b"},{"$f":"VLOOKUP(A1280,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1280,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1691","v":"BC569c"},{"$f":"VLOOKUP(A1281,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions associated with treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1281,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1694","v":"BC570"},{"$f":"VLOOKUP(A1282,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat energy use for treatment 3 (storage)"},{"$f":"IF('Input Project'!H313=\"\",\"\",'Input Project'!H313)","v":""},{"$f":"VLOOKUP($A1282,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1282=1,IF(MonteCarlo=1,$E1282,IF($C1282=\"\",$D1282,$C1282)),IF($C1282=\"\",$D1282,$C1282))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W200=\"\",\"\",Uncertainty!W200)","v":""},{"$f":"IF(Uncertainty!Z200=\"\",\"\",Uncertainty!Z200)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1695","v":"BC571"},{"$f":"VLOOKUP(A1283,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Heat source for treatment 3 (storage)"},{"$f":"IF('Input Project'!H312=\"\",\"\",'Input Project'!H312)","v":""},{"$f":"VLOOKUP($A1283,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1283=1,IF(MonteCarlo=1,$E1283,IF($C1283=\"\",$D1283,$C1283)),IF($C1283=\"\",$D1283,$C1283))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1701","v":"BC575"},{"$f":"VLOOKUP(A1284,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity energy use for treatment 3 (storage)"},{"$f":"IF('Input Project'!H315=\"\",\"\",'Input Project'!H315)","v":""},{"$f":"VLOOKUP($A1284,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1284=1,IF(MonteCarlo=1,$E1284,IF($C1284=\"\",$D1284,$C1284)),IF($C1284=\"\",$D1284,$C1284))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W201=\"\",\"\",Uncertainty!W201)","v":""},{"$f":"IF(Uncertainty!Z201=\"\",\"\",Uncertainty!Z201)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1702","v":"BC576"},{"$f":"VLOOKUP(A1285,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity source for treatment 3 (storage)"},{"$f":"IF('Input Project'!H314=\"\",\"\",'Input Project'!H314)","v":""},{"$f":"VLOOKUP($A1285,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1285=1,IF(MonteCarlo=1,$E1285,IF($C1285=\"\",$D1285,$C1285)),IF($C1285=\"\",$D1285,$C1285))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1703","v":"BC577a"},{"$f":"VLOOKUP(A1286,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy use for electricity production for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1286,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1704","v":"BC577b"},{"$f":"VLOOKUP(A1287,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy use for electricity production for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1287,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1705","v":"BC577c"},{"$f":"VLOOKUP(A1288,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to electricity production for treatment 3 (storage)"},null,null,"",null,{"$f":"VLOOKUP(A1288,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1708","v":"BC580a"},{"$f":"VLOOKUP(A1289,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated fossil energy use after conversion 1 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1289,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1709","v":"BC580b"},{"$f":"VLOOKUP(A1290,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated primary energy use after conversion 1 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1290,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1710","v":"BC580c"},{"$f":"VLOOKUP(A1291,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated GHG emissions after conversion 1 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1291,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1711","v":"BC580d"},{"$f":"VLOOKUP(A1292,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated water use after conversion 1 (per GJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1292,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1712","v":"BC580f"},{"$f":"VLOOKUP(A1293,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated acidification potential after conversion 1 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1293,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1713","v":"BC580g"},{"$f":"VLOOKUP(A1294,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated eutrophication potential after conversion 1 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1294,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1714","v":"BC581a"},{"$f":"VLOOKUP(A1295,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated fossil energy use after conversion 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1295,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1715","v":"BC581b"},{"$f":"VLOOKUP(A1296,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated primary energy use after conversion 2 (per MJ feedstock 2 fuel)"},null,null,{"$f":"IF(MonteCarlo=1,IF($L1296=1,IF($H1296=\"n.a.\",0,IF($H1296<0.009,0,MIN(MAX(NORMINV(RAND(),$H1296,$K1296),$I1296),$J1296))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A1296,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},{"$f":"IF($L1296=1,IF($C1296=\"\",$D1296,$C1296),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1716","v":"BC581c"},{"$f":"VLOOKUP(A1297,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated GHG emissions after conversion 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1297,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"",{"$f":"IF($L1297=1,IF($M1297=\"\",$O1297,$M1297),\"\")","v":""},{"$f":"IF($L1297=1,IF($N1297=\"\",$P1297,$N1297),\"\")","v":""},{"$f":"IF($L1297=1,($J1297-$I1297)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1717","v":"BC581d"},{"$f":"VLOOKUP(A1298,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated water use after conversion 2 (per GJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1298,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1718","v":"BC581f"},{"$f":"VLOOKUP(A1299,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated acidification potential after conversion 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1299,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1719","v":"BC581g"},{"$f":"VLOOKUP(A1300,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocated eutrophication potential after conversion 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1300,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1720","v":"BC582a"},{"$f":"VLOOKUP(A1301,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use feedstock 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1301,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1721","v":"BC582b"},{"$f":"VLOOKUP(A1302,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use feedstock 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1302,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1722","v":"BC582c"},{"$f":"VLOOKUP(A1303,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions feedstock 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1303,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1723","v":"BC582d"},{"$f":"VLOOKUP(A1304,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total water use feedstock 2 (per GJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1304,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1724","v":"BC582f"},{"$f":"VLOOKUP(A1305,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total acidification potential feedstock 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1305,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1725","v":"BC582g"},{"$f":"VLOOKUP(A1306,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total eutrophication potential feedstock 2 (per MJ feedstock 2 fuel)"},null,null,"",null,{"$f":"VLOOKUP(A1306,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1726","v":"BC583a"},{"$f":"VLOOKUP(A1307,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use feedstock 2 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A1307,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1727","v":"BC583b"},{"$f":"VLOOKUP(A1308,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use feedstock 2 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A1308,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1728","v":"BC583c"},{"$f":"VLOOKUP(A1309,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions feedstock 2 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A1309,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1729","v":"BC583d"},{"$f":"VLOOKUP(A1310,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total water use feedstock 2 (per GJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A1310,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1730","v":"BC583f"},{"$f":"VLOOKUP(A1311,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total acidification potential feedstock 2 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A1311,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1731","v":"BC583g"},{"$f":"VLOOKUP(A1312,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total eutrophication potential feedstock 2 (per MJ functional unit)"},null,null,"",null,{"$f":"VLOOKUP(A1312,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1733","v":"BC590a"},{"$f":"VLOOKUP(A1313,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1313,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1734","v":"BC590b"},{"$f":"VLOOKUP(A1314,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1314,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1735","v":"BC590c"},{"$f":"VLOOKUP(A1315,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1315,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1736","v":"BC590d"},{"$f":"VLOOKUP(A1316,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1316,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1737","v":"BC590f"},{"$f":"VLOOKUP(A1317,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from process 1"},null,null,"",null,{"$f":"VLOOKUP(A1317,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1738","v":"BC590g"},{"$f":"VLOOKUP(A1318,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from process 1"},null,null,"",null,{"$f":"VLOOKUP(A1318,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1739","v":"BC591a"},{"$f":"VLOOKUP(A1319,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1319,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1740","v":"BC591b"},{"$f":"VLOOKUP(A1320,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1320,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1741","v":"BC591c"},{"$f":"VLOOKUP(A1321,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1321,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1742","v":"BC591d"},{"$f":"VLOOKUP(A1322,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use in process 1"},null,null,"",null,{"$f":"VLOOKUP(A1322,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1743","v":"BC591f"},{"$f":"VLOOKUP(A1323,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from process 1"},null,null,"",null,{"$f":"VLOOKUP(A1323,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1744","v":"BC591g"},{"$f":"VLOOKUP(A1324,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from process 1"},null,null,"",null,{"$f":"VLOOKUP(A1324,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1745","v":"BC592a"},{"$f":"VLOOKUP(A1325,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1325,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1746","v":"BC592b"},{"$f":"VLOOKUP(A1326,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1326,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1747","v":"BC592c"},{"$f":"VLOOKUP(A1327,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1327,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1748","v":"BC592d"},{"$f":"VLOOKUP(A1328,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1328,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,{"$f":"IF($L1328=1,VLOOKUP($A1328,list_database2,$I$9+1,FALSE),\"\")","v":""},{"$f":"IF($L1328=1,VLOOKUP($A1328,list_database2,$I$9+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1749","v":"BC592f"},{"$f":"VLOOKUP(A1329,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from process 2"},null,null,"",null,{"$f":"VLOOKUP(A1329,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1750","v":"BC592g"},{"$f":"VLOOKUP(A1330,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from process 2"},null,null,"",null,{"$f":"VLOOKUP(A1330,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1751","v":"BC593a"},{"$f":"VLOOKUP(A1331,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1331,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1752","v":"BC593b"},{"$f":"VLOOKUP(A1332,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1332,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1753","v":"BC593c"},{"$f":"VLOOKUP(A1333,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1333,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1754","v":"BC593d"},{"$f":"VLOOKUP(A1334,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use in process 2"},null,null,"",null,{"$f":"VLOOKUP(A1334,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1755","v":"BC593f"},{"$f":"VLOOKUP(A1335,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from process 2"},null,null,"",null,{"$f":"VLOOKUP(A1335,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1756","v":"BC593g"},{"$f":"VLOOKUP(A1336,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from process 2"},null,null,"",null,{"$f":"VLOOKUP(A1336,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1757","v":"BC594a"},{"$f":"VLOOKUP(A1337,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1337,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1758","v":"BC594b"},{"$f":"VLOOKUP(A1338,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1338,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1759","v":"BC594c"},{"$f":"VLOOKUP(A1339,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1339,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1760","v":"BC594d"},{"$f":"VLOOKUP(A1340,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1340,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1761","v":"BC594f"},{"$f":"VLOOKUP(A1341,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1341,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1762","v":"BC594g"},{"$f":"VLOOKUP(A1342,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1342,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1763","v":"BC595a"},{"$f":"VLOOKUP(A1343,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1343,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1764","v":"BC595b"},{"$f":"VLOOKUP(A1344,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1344,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1765","v":"BC595c"},{"$f":"VLOOKUP(A1345,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1345,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1766","v":"BC595d"},{"$f":"VLOOKUP(A1346,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use for conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1346,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1767","v":"BC595f"},{"$f":"VLOOKUP(A1347,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1347,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1768","v":"BC595g"},{"$f":"VLOOKUP(A1348,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from conversion (process 1 + 2)"},null,null,"",null,{"$f":"VLOOKUP(A1348,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1769","v":"BC600a"},{"$f":"VLOOKUP(A1349,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for conversion process 1"},{"$f":"IF('Input RU'!K56=\"\",\"\",'Input RU'!K56)","v":""},{"$f":"VLOOKUP($A1349,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1349=1,IF(MonteCarlo=1,$E1349,IF($C1349=\"\",$D1349,$C1349)),IF($C1349=\"\",$D1349,$C1349))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W167=\"\",\"\",Uncertainty!W167)","v":""},{"$f":"IF(Uncertainty!Z167=\"\",\"\",Uncertainty!Z167)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1770","v":"BC600b"},{"$f":"VLOOKUP(A1350,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for conversion process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1771","v":"BC601a"},{"$f":"VLOOKUP(A1351,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},{"$f":"IF('Input RU'!K59=\"\",\"\",'Input RU'!K59)","v":""},{"$f":"VLOOKUP($A1351,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1351=1,IF(MonteCarlo=1,$E1351,IF($C1351=\"\",$D1351,$C1351)),IF($C1351=\"\",$D1351,$C1351))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W173=\"\",\"\",Uncertainty!W173)","v":""},{"$f":"IF(Uncertainty!Z173=\"\",\"\",Uncertainty!Z173)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1772","v":"BC601b"},{"$f":"VLOOKUP(A1352,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1773","v":"BC602a"},{"$f":"VLOOKUP(A1353,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for conversion process 2"},{"$f":"IF('Input RU'!K62=\"\",\"\",'Input RU'!K62)","v":""},{"$f":"VLOOKUP($A1353,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1353=1,IF(MonteCarlo=1,$E1353,IF($C1353=\"\",$D1353,$C1353)),IF($C1353=\"\",$D1353,$C1353))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W196=\"\",\"\",Uncertainty!W196)","v":""},{"$f":"IF(Uncertainty!Z196=\"\",\"\",Uncertainty!Z196)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1774","v":"BC602b"},{"$f":"VLOOKUP(A1354,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for conversion process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1775","v":"BC603a"},{"$f":"VLOOKUP(A1355,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},{"$f":"IF('Input RU'!K65=\"\",\"\",'Input RU'!K65)","v":""},{"$f":"VLOOKUP($A1355,list_database2,$I$9,FALSE)","v":0},"",{"$f":"IF($L1355=1,IF(MonteCarlo=1,$E1355,IF($C1355=\"\",$D1355,$C1355)),IF($C1355=\"\",$D1355,$C1355))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W202=\"\",\"\",Uncertainty!W202)","v":""},{"$f":"IF(Uncertainty!Z202=\"\",\"\",Uncertainty!Z202)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1776","v":"BC603b"},{"$f":"VLOOKUP(A1356,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1835","v":"BC650a"},{"$f":"VLOOKUP(A1357,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour, process 1"},{"$f":"IF('Input LW'!U106=\"\",\"\",'Input LW'!U106)","v":""},{"$f":"VLOOKUP($A1357,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1357=1,IF(MonteCarlo=1,$E1357,IF($C1357=\"\",$D1357,$C1357)),IF($C1357=\"\",$D1357,$C1357))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1836","v":"BC650b"},{"$f":"VLOOKUP(A1358,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour, process 1"},{"$f":"IF('Input LW'!U107=\"\",\"\",'Input LW'!U107)","v":""},{"$f":"VLOOKUP($A1358,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1358=1,IF(MonteCarlo=1,$E1358,IF($C1358=\"\",$D1358,$C1358)),IF($C1358=\"\",$D1358,$C1358))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1837","v":"BC650c"},{"$f":"VLOOKUP(A1359,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights, process 1"},{"$f":"IF('Input LW'!U108=\"\",\"\",'Input LW'!U108)","v":""},{"$f":"VLOOKUP($A1359,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1359=1,IF(MonteCarlo=1,$E1359,IF($C1359=\"\",$D1359,$C1359)),IF($C1359=\"\",$D1359,$C1359))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1838","v":"BC650d"},{"$f":"VLOOKUP(A1360,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination, process 1"},{"$f":"IF('Input LW'!U109=\"\",\"\",'Input LW'!U109)","v":""},{"$f":"VLOOKUP($A1360,list_database2,$I$9,FALSE)","v":"n.a."},{"$f":"IF(MonteCarlo=1,IF($L1360=1,IF($H1360=\"n.a.\",0,IF($H1360<0.009,0,MIN(MAX(NORMINV(RAND(),$H1360,$K1360),$I1360),$J1360))),\"\"),\"\")","v":""},{"$f":"IF($L1360=1,IF(MonteCarlo=1,$E1360,IF($C1360=\"\",$D1360,$C1360)),IF($C1360=\"\",$D1360,$C1360))","v":"n.a."},null,{"$f":"IF($L1360=1,IF($C1360=\"\",$D1360,$C1360),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1839","v":"BC650e"},{"$f":"VLOOKUP(A1361,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured, process 1"},null,null,"",null,null,"",{"$f":"IF($L1361=1,IF($M1361=\"\",$O1361,$M1361),\"\")","v":""},{"$f":"IF($L1361=1,IF($N1361=\"\",$P1361,$N1361),\"\")","v":""},{"$f":"IF($L1361=1,($J1361-$I1361)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1840","v":"BC650f"},{"$f":"VLOOKUP(A1362,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 1"},{"$f":"IF('Input LW'!U110=\"\",\"\",'Input LW'!U110)","v":""},{"$f":"VLOOKUP($A1362,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1362=1,IF(MonteCarlo=1,$E1362,IF($C1362=\"\",$D1362,$C1362)),IF($C1362=\"\",$D1362,$C1362))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1841","v":"BC650g"},{"$f":"VLOOKUP(A1363,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security, process 1"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1842","v":"BC651a"},{"$f":"VLOOKUP(A1364,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts, process 1"},{"$f":"IF('Input LW'!U112=\"\",\"\",'Input LW'!U112)","v":""},{"$f":"VLOOKUP($A1364,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1364=1,IF(MonteCarlo=1,$E1364,IF($C1364=\"\",$D1364,$C1364)),IF($C1364=\"\",$D1364,$C1364))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1843","v":"BC651b"},{"$f":"VLOOKUP(A1365,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights, process 1"},{"$f":"IF('Input LW'!U113=\"\",\"\",'Input LW'!U113)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1844","v":"BC651c"},{"$f":"VLOOKUP(A1366,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 1"},{"$f":"IF('Input LW'!U114=\"\",\"\",'Input LW'!U114)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1845","v":"BC651d"},{"$f":"VLOOKUP(A1367,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules, process 1"},{"$f":"IF('Input LW'!U115=\"\",\"\",'Input LW'!U115)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1846","v":"BC651e"},{"$f":"VLOOKUP(A1368,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy, process 1"},{"$f":"IF('Input LW'!U116=\"\",\"\",'Input LW'!U116)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1847","v":"BC651f"},{"$f":"VLOOKUP(A1369,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 1"},{"$f":"IF('Input LW'!U117=\"\",\"\",'Input LW'!U117)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1848","v":"BC651g"},{"$f":"VLOOKUP(A1370,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training, process 1"},{"$f":"IF('Input LW'!U118=\"\",\"\",'Input LW'!U118)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1849","v":"BC652a"},{"$f":"VLOOKUP(A1371,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour, process 2"},{"$f":"IF('Input LW'!U123=\"\",\"\",'Input LW'!U123)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1850","v":"BC652b"},{"$f":"VLOOKUP(A1372,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour, process 2"},{"$f":"IF('Input LW'!U124=\"\",\"\",'Input LW'!U124)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1851","v":"BC652c"},{"$f":"VLOOKUP(A1373,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights, process 2"},{"$f":"IF('Input LW'!U125=\"\",\"\",'Input LW'!U125)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1852","v":"BC652d"},{"$f":"VLOOKUP(A1374,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination, process 2"},{"$f":"IF('Input LW'!U126=\"\",\"\",'Input LW'!U126)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1853","v":"BC652e"},{"$f":"VLOOKUP(A1375,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1854","v":"BC652f"},{"$f":"VLOOKUP(A1376,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 2"},{"$f":"IF('Input LW'!U127=\"\",\"\",'Input LW'!U127)","v":""},{"$f":"VLOOKUP($A1376,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1376=1,IF(MonteCarlo=1,$E1376,IF($C1376=\"\",$D1376,$C1376)),IF($C1376=\"\",$D1376,$C1376))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1855","v":"BC652g"},{"$f":"VLOOKUP(A1377,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security, process 2"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1856","v":"BC653a"},{"$f":"VLOOKUP(A1378,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts, process 2"},{"$f":"IF('Input LW'!U129=\"\",\"\",'Input LW'!U129)","v":""},{"$f":"VLOOKUP($A1378,list_database2,$I$9,FALSE)","v":"n.a."},"",{"$f":"IF($L1378=1,IF(MonteCarlo=1,$E1378,IF($C1378=\"\",$D1378,$C1378)),IF($C1378=\"\",$D1378,$C1378))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1857","v":"BC653b"},{"$f":"VLOOKUP(A1379,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights, process 2"},{"$f":"IF('Input LW'!U130=\"\",\"\",'Input LW'!U130)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1858","v":"BC653c"},{"$f":"VLOOKUP(A1380,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 2"},{"$f":"IF('Input LW'!U131=\"\",\"\",'Input LW'!U131)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1859","v":"BC653d"},{"$f":"VLOOKUP(A1381,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules, process 2"},{"$f":"IF('Input LW'!U132=\"\",\"\",'Input LW'!U132)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1860","v":"BC653e"},{"$f":"VLOOKUP(A1382,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy, process 2"},{"$f":"IF('Input LW'!U133=\"\",\"\",'Input LW'!U133)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1861","v":"BC653f"},{"$f":"VLOOKUP(A1383,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 2"},{"$f":"IF('Input LW'!U134=\"\",\"\",'Input LW'!U134)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1862","v":"BC653g"},{"$f":"VLOOKUP(A1384,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training, process 2"},{"$f":"IF('Input LW'!U135=\"\",\"\",'Input LW'!U135)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1863","v":"BC654a"},{"$f":"VLOOKUP(A1385,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour, processing FS2"},null,null,"",null,{"$f":"VLOOKUP(A1385,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1864","v":"BC654b"},{"$f":"VLOOKUP(A1386,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour, processing FS2"},null,null,"",null,{"$f":"VLOOKUP(A1386,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1865","v":"BC654c"},{"$f":"VLOOKUP(A1387,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights, processing FS2"},null,null,"",null,{"$f":"VLOOKUP(A1387,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1866","v":"BC654d"},{"$f":"VLOOKUP(A1388,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination, processing FS2"},null,null,"",null,{"$f":"VLOOKUP(A1388,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1867","v":"BC654e"},{"$f":"VLOOKUP(A1389,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1389,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1868","v":"BC654f"},{"$f":"VLOOKUP(A1390,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1390,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1869","v":"BC654g"},{"$f":"VLOOKUP(A1391,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1391,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1870","v":"BC655a"},{"$f":"VLOOKUP(A1392,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1392,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1871","v":"BC655b"},{"$f":"VLOOKUP(A1393,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1393,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1872","v":"BC655c"},{"$f":"VLOOKUP(A1394,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1394,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1873","v":"BC655d"},{"$f":"VLOOKUP(A1395,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1395,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1874","v":"BC655e"},{"$f":"VLOOKUP(A1396,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1396,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1875","v":"BC655f"},{"$f":"VLOOKUP(A1397,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1397,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1876","v":"BC655g"},{"$f":"VLOOKUP(A1398,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training, processing FS2"},null,null,null,null,{"$f":"VLOOKUP(A1398,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1877","v":"BC656"},{"$f":"VLOOKUP(A1399,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights, process 1_score"},null,null,null,null,{"$f":"VLOOKUP(A1399,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1878","v":"BC657"},{"$f":"VLOOKUP(A1400,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions, process 1_score"},null,null,null,null,{"$f":"VLOOKUP(A1400,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1879","v":"BC658"},{"$f":"VLOOKUP(A1401,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights, process 2_score"},null,null,null,null,{"$f":"VLOOKUP(A1401,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1880","v":"BC659"},{"$f":"VLOOKUP(A1402,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions, process 2_score"},null,null,null,null,{"$f":"VLOOKUP(A1402,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1881","v":"BC660"},{"$f":"VLOOKUP(A1403,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights, processing overall_score"},null,null,null,null,{"$f":"VLOOKUP(A1403,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1882","v":"BC661"},{"$f":"VLOOKUP(A1404,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions, processing overall_score"},null,null,null,null,{"$f":"VLOOKUP(A1404,'Conversion feedstock2'!$D$9:$G$5178,4,FALSE)","v":0},null,null,null,null,0]
[null,null,null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1885","v":"FC000"},{"$f":"VLOOKUP(A1406,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Final conversion process"},null,{"$f":"VLOOKUP($A1406,list_database1,$I$10,FALSE)","v":"No final conversion"},"",{"$f":"IF($L1406=1,IF(MonteCarlo=1,$E1406,IF($C1406=\"\",$D1406,$C1406)),IF($C1406=\"\",$D1406,$C1406))","v":"No final conversion"},null,"","","","",0,null,null,{"$f":"IF($L1406=1,VLOOKUP($A1406,list_database1,$I$10+1,FALSE),\"\")","v":""},{"$f":"IF($L1406=1,VLOOKUP($A1406,list_database1,$I$10+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1886","v":"FC001a"},{"$f":"VLOOKUP(A1407,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of input flow, feedstock 1"},null,"Liquid biomethane (LBM)","","Liquid biomethane (LBM)",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1887","v":"FC001b"},{"$f":"VLOOKUP(A1408,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of input flow, feedstock 2"},null,"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1888","v":"FC002a"},{"$f":"VLOOKUP(A1409,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Share of input flow 1 (caloric)"},{"$f":"IF('Input Project'!H333=\"\",\"\",'Input Project'!H333)","v":""},100,"",100,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1889","v":"FC002b"},{"$f":"VLOOKUP(A1410,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Share of input flow 2 (caloric)"},{"$f":"IF('Input Project'!H334=\"\",\"\",'Input Project'!H334)","v":""},0,"",0,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1890","v":"FC003a"},{"$f":"VLOOKUP(A1411,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Net electrical efficiency, final conversion"},{"$f":"IF('Input Project'!H335=\"\",\"\",'Input Project'!H335)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W212=\"\",\"\",Uncertainty!W212)","v":""},{"$f":"IF(Uncertainty!Z212=\"\",\"\",Uncertainty!Z212)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1891","v":"FC003b"},{"$f":"VLOOKUP(A1412,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Net thermal efficiency, final conversion"},{"$f":"IF('Input Project'!H336=\"\",\"\",'Input Project'!H336)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W213=\"\",\"\",Uncertainty!W213)","v":""},{"$f":"IF(Uncertainty!Z213=\"\",\"\",Uncertainty!Z213)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1892","v":"FC003c"},{"$f":"VLOOKUP(A1413,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Net conversion efficiency, final conversion - other than electricity or heat"},{"$f":"IF('Input Project'!H337=\"\",\"\",'Input Project'!H337)","v":""},100,"",100]
[{"$f":"'ID-numbers'!$A1893","v":"FC004a"},{"$f":"VLOOKUP(A1414,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 1, final conversion"},{"$f":"IF('Input Project'!H341=\"\",\"\",'Input Project'!H341)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1894","v":"FC004b"},{"$f":"VLOOKUP(A1415,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of by-product 2, final conversion"},{"$f":"IF('Input Project'!H343=\"\",\"\",'Input Project'!H343)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1895","v":"FC005a"},{"$f":"VLOOKUP(A1416,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, final conversion (kg)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1896","v":"FC005b"},{"$f":"VLOOKUP(A1417,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, final conversion (kg)"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1897","v":"FC006a"},{"$f":"VLOOKUP(A1418,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 1, final conversion (MJ)"},{"$f":"IF('Input Project'!H342=\"\",\"\",'Input Project'!H342)","v":""},0,"",{"$f":"IF($L1418=1,IF(MonteCarlo=1,$E1418,IF($C1418=\"\",$D1418,$C1418)),IF($C1418=\"\",$D1418,$C1418))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W214=\"\",\"\",Uncertainty!W214)","v":""},{"$f":"IF(Uncertainty!Z214=\"\",\"\",Uncertainty!Z214)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1898","v":"FC006b"},{"$f":"VLOOKUP(A1419,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Extraction rate of by-product 2, final conversion (MJ)"},{"$f":"IF('Input Project'!H344=\"\",\"\",'Input Project'!H344)","v":""},0,"",{"$f":"IF($L1419=1,IF(MonteCarlo=1,$E1419,IF($C1419=\"\",$D1419,$C1419)),IF($C1419=\"\",$D1419,$C1419))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W215=\"\",\"\",Uncertainty!W215)","v":""},{"$f":"IF(Uncertainty!Z215=\"\",\"\",Uncertainty!Z215)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1901","v":"FC008a"},{"$f":"VLOOKUP(A1420,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 1, final conversion"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1902","v":"FC008b"},{"$f":"VLOOKUP(A1421,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Valorisation of by-product 2, final conversion"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1903","v":"FC009a"},{"$f":"VLOOKUP(A1422,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 1, final conversion"},{"$f":"IF('Input Project'!H351=\"\",\"\",'Input Project'!H351)","v":"n.a."},"n.a.","",{"$f":"IF($L1422=1,IF(MonteCarlo=1,$E1422,IF($C1422=\"\",$D1422,$C1422)),IF($C1422=\"\",$D1422,$C1422))","v":"n.a."},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1904","v":"FC009b"},{"$f":"VLOOKUP(A1423,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of material input flow 2, final conversion"},{"$f":"IF('Input Project'!H353=\"\",\"\",'Input Project'!H353)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1905","v":"FC010a"},{"$f":"VLOOKUP(A1424,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 1, final conversion"},{"$f":"IF('Input Project'!H352=\"\",\"\",'Input Project'!H352)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W219=\"\",\"\",Uncertainty!W219)","v":""},{"$f":"IF(Uncertainty!Z219=\"\",\"\",Uncertainty!Z219)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1906","v":"FC010b"},{"$f":"VLOOKUP(A1425,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of material input flow 2, final conversion"},{"$f":"IF('Input Project'!H354=\"\",\"\",'Input Project'!H354)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W220=\"\",\"\",Uncertainty!W220)","v":""},{"$f":"IF(Uncertainty!Z220=\"\",\"\",Uncertainty!Z220)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1907","v":"FC011a"},{"$f":"VLOOKUP(A1426,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 1, final conversion"},{"$f":"IF('Input Project'!H345=\"\",\"\",'Input Project'!H345)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1908","v":"FC011b"},{"$f":"VLOOKUP(A1427,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Type of fuel/heat flow 2, final conversion"},{"$f":"IF('Input Project'!H347=\"\",\"\",'Input Project'!H347)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1909","v":"FC012a"},{"$f":"VLOOKUP(A1428,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat flow 1, final conversion"},{"$f":"IF('Input Project'!H346=\"\",\"\",'Input Project'!H346)","v":""},{"$f":"VLOOKUP($A1428,list_database1,$I$10,FALSE)","v":0},"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W216=\"\",\"\",Uncertainty!W216)","v":""},{"$f":"IF(Uncertainty!Z216=\"\",\"\",Uncertainty!Z216)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1910","v":"FC012b"},{"$f":"VLOOKUP(A1429,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Amount of fuel/heat flow 2, final conversion"},{"$f":"IF('Input Project'!H348=\"\",\"\",'Input Project'!H348)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W217=\"\",\"\",Uncertainty!W217)","v":""},{"$f":"IF(Uncertainty!Z217=\"\",\"\",Uncertainty!Z217)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1911","v":"FC013"},{"$f":"VLOOKUP(A1430,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Net amount of electricity input, final conversion"},{"$f":"IF('Input Project'!H350=\"\",\"\",'Input Project'!H350)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W218=\"\",\"\",Uncertainty!W218)","v":""},{"$f":"IF(Uncertainty!Z218=\"\",\"\",Uncertainty!Z218)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1912","v":"FC014"},{"$f":"VLOOKUP(A1431,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Electricity source, final conversion"},{"$f":"IF('Input Project'!H349=\"\",\"\",'Input Project'!H349)","v":""},"n.a.","","n.a.",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1913","v":"FC015a"},{"$f":"VLOOKUP(A1432,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 1, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1432,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1914","v":"FC015b"},{"$f":"VLOOKUP(A1433,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for material input flow 2, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1433,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1915","v":"FC015c"},{"$f":"VLOOKUP(A1434,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1434,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1916","v":"FC015d"},{"$f":"VLOOKUP(A1435,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1435,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1917","v":"FC015e"},{"$f":"VLOOKUP(A1436,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific fossil energy used for external electricity production, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1436,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1918","v":"FC016a"},{"$f":"VLOOKUP(A1437,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 1, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1437,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1919","v":"FC016b"},{"$f":"VLOOKUP(A1438,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for material input flow 2, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1438,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1920","v":"FC016c"},{"$f":"VLOOKUP(A1439,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1439,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,{"$f":"IF($L1439=1,VLOOKUP($A1439,list_database1,$I$10+1,FALSE),\"\")","v":""},{"$f":"IF($L1439=1,VLOOKUP($A1439,list_database1,$I$10+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A1921","v":"FC016d"},{"$f":"VLOOKUP(A1440,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1440,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1922","v":"FC016e"},{"$f":"VLOOKUP(A1441,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific primary energy used for external electricity production, final conversion"},null,null,{"$f":"IF(MonteCarlo=1,IF($L1441=1,IF($H1441=\"n.a.\",0,IF($H1441<0.009,0,MIN(MAX(NORMINV(RAND(),$H1441,$K1441),$I1441),$J1441))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A1441,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},{"$f":"IF($L1441=1,IF($C1441=\"\",$D1441,$C1441),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1923","v":"FC017a"},{"$f":"VLOOKUP(A1442,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1442,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"",{"$f":"IF($L1442=1,IF($M1442=\"\",$O1442,$M1442),\"\")","v":""},{"$f":"IF($L1442=1,IF($N1442=\"\",$P1442,$N1442),\"\")","v":""},{"$f":"IF($L1442=1,($J1442-$I1442)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1924","v":"FC017b"},{"$f":"VLOOKUP(A1443,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1443,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1925","v":"FC017c"},{"$f":"VLOOKUP(A1444,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1444,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1926","v":"FC017d"},{"$f":"VLOOKUP(A1445,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1445,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1927","v":"FC017e"},{"$f":"VLOOKUP(A1446,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Specific GHG emissions related to external electricity production, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1446,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1928","v":"FC018a"},{"$f":"VLOOKUP(A1447,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to electricity input, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1447,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1929","v":"FC018b"},{"$f":"VLOOKUP(A1448,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1448,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1930","v":"FC018c"},{"$f":"VLOOKUP(A1449,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use related to material input flows, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1449,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1931","v":"FC019"},{"$f":"VLOOKUP(A1450,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy use in final conversion process"},null,null,"",null,{"$f":"VLOOKUP(A1450,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1932","v":"FC020a"},{"$f":"VLOOKUP(A1451,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to electricity input, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1451,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1933","v":"FC020b"},{"$f":"VLOOKUP(A1452,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to fuel/heat flows, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1452,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1934","v":"FC020c"},{"$f":"VLOOKUP(A1453,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use related to material input flows, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1453,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1935","v":"FC021"},{"$f":"VLOOKUP(A1454,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy use in final conversion process"},null,null,"",null,{"$f":"VLOOKUP(A1454,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1936","v":"FC022a"},{"$f":"VLOOKUP(A1455,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to electricity use, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1455,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1937","v":"FC022b"},{"$f":"VLOOKUP(A1456,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to fuel/heat flows, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1456,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1938","v":"FC022c"},{"$f":"VLOOKUP(A1457,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to material input flows, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1457,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1939","v":"FC023"},{"$f":"VLOOKUP(A1458,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions related to final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1458,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1940","v":"FC024a"},{"$f":"VLOOKUP(A1459,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 1, final conversion"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1941","v":"FC024b"},{"$f":"VLOOKUP(A1460,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Moisture content of by-product 2, final conversion"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1942","v":"FC025a"},{"$f":"VLOOKUP(A1461,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to heat, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1461,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":100},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1943","v":"FC025b"},{"$f":"VLOOKUP(A1462,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to electricity, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1462,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":100},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1944","v":"FC025c"},{"$f":"VLOOKUP(A1463,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to energy products, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1463,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":100},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1945","v":"FC026"},{"$f":"VLOOKUP(A1464,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-products, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1464,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1946","v":"FC027a"},{"$f":"VLOOKUP(A1465,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 1, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1465,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1947","v":"FC027b"},{"$f":"VLOOKUP(A1466,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Allocation to by-product 2, final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1466,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1948","v":"FC028a"},{"$f":"VLOOKUP(A1467,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NOX emissions to air (not from material/energy input), final conversion"},{"$f":"IF('Input EQ'!K69=\"\",\"\",'Input EQ'!K69)","v":""},{"$f":"VLOOKUP($A1467,list_database1,$I$10,FALSE)","v":0},"",{"$f":"IF($L1467=1,IF(MonteCarlo=1,$E1467,IF($C1467=\"\",$D1467,$C1467)),IF($C1467=\"\",$D1467,$C1467))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W221=\"\",\"\",Uncertainty!W221)","v":""},{"$f":"IF(Uncertainty!Z221=\"\",\"\",Uncertainty!Z221)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1949","v":"FC028b"},{"$f":"VLOOKUP(A1468,'ID-numbers'!$1:$1048576,2,FALSE)","v":"SOX emissions to air (not from material/energy input), final conversion"},{"$f":"IF('Input EQ'!K70=\"\",\"\",'Input EQ'!K70)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W222=\"\",\"\",Uncertainty!W222)","v":""},{"$f":"IF(Uncertainty!Z222=\"\",\"\",Uncertainty!Z222)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1950","v":"FC028c"},{"$f":"VLOOKUP(A1469,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), final conversion"},{"$f":"IF('Input EQ'!K71=\"\",\"\",'Input EQ'!K71)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W223=\"\",\"\",Uncertainty!W223)","v":""},{"$f":"IF(Uncertainty!Z223=\"\",\"\",Uncertainty!Z223)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1951","v":"FC028d"},{"$f":"VLOOKUP(A1470,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), final conversion"},{"$f":"IF('Input EQ'!K72=\"\",\"\",'Input EQ'!K72)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W224=\"\",\"\",Uncertainty!W224)","v":""},{"$f":"IF(Uncertainty!Z224=\"\",\"\",Uncertainty!Z224)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1952","v":"FC028e"},{"$f":"VLOOKUP(A1471,'ID-numbers'!$1:$1048576,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), final conversion"},{"$f":"IF('Input EQ'!K73=\"\",\"\",'Input EQ'!K73)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W225=\"\",\"\",Uncertainty!W225)","v":""},{"$f":"IF(Uncertainty!Z225=\"\",\"\",Uncertainty!Z225)","v":""},{"$f":"IF($L1471=1,VLOOKUP($A1471,list_database1,$I$10+1,FALSE),\"\")","v":0},{"$f":"IF($L1471=1,VLOOKUP($A1471,list_database1,$I$10+2,FALSE),\"\")","v":0}]
[{"$f":"'ID-numbers'!$A1953","v":"FC028f"},{"$f":"VLOOKUP(A1472,'ID-numbers'!$1:$1048576,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), final conversion"},{"$f":"IF('Input EQ'!K74=\"\",\"\",'Input EQ'!K74)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W226=\"\",\"\",Uncertainty!W226)","v":""},{"$f":"IF(Uncertainty!Z226=\"\",\"\",Uncertainty!Z226)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1954","v":"FC028g"},{"$f":"VLOOKUP(A1473,'ID-numbers'!$1:$1048576,2,FALSE)","v":"COD emissions to water (not from material/energy input), final conversion"},{"$f":"IF('Input EQ'!K75=\"\",\"\",'Input EQ'!K75)","v":""},0,"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W227=\"\",\"\",Uncertainty!W227)","v":""},{"$f":"IF(Uncertainty!Z227=\"\",\"\",Uncertainty!Z227)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1955","v":"FC029"},{"$f":"VLOOKUP(A1474,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Compliance with RED requirements on GHG savings"},null,null,null,null,{"$f":"VLOOKUP(A1474,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":"no"},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1956","v":"FC030"},{"$f":"VLOOKUP(A1475,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Functional unit"},{"$f":"J5","v":"MJ diesel"},{"$f":"VLOOKUP($A1475,list_database1,$I$10,FALSE)","v":"MJ biogas"},"","MJ diesel",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1957","v":"FC031"},{"$f":"VLOOKUP(A1476,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Output heat per MJ functional unit"},null,null,"",null,{"$f":"VLOOKUP(A1476,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1958","v":"FC032"},{"$f":"VLOOKUP(A1477,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Output electricity per MJ functional unit"},null,null,"",null,{"$f":"VLOOKUP(A1477,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1959","v":"FC033"},{"$f":"VLOOKUP(A1478,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input feedstock 1 per MJ functional unit"},null,null,"",null,{"$f":"VLOOKUP(A1478,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":1},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1960","v":"FC034"},{"$f":"VLOOKUP(A1479,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Input feedstock 2 per MJ functional unit"},null,null,"",null,{"$f":"VLOOKUP(A1479,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1971","v":"FC037a"},{"$f":"VLOOKUP(A1480,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Gross electrical efficiency, final conversion"},{"$f":"IF('Input Project'!H338=\"\",\"\",'Input Project'!H338)","v":""},{"$f":"VLOOKUP($A1480,list_database1,$I$10,FALSE)","v":0},"",{"$f":"IF($L1480=1,IF(MonteCarlo=1,$E1480,IF($C1480=\"\",$D1480,$C1480)),IF($C1480=\"\",$D1480,$C1480))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W234=\"\",\"\",Uncertainty!W234)","v":""},{"$f":"IF(Uncertainty!Z234=\"\",\"\",Uncertainty!Z234)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1972","v":"FC037b"},{"$f":"VLOOKUP(A1481,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Gross thermal efficiency, final conversion"},{"$f":"IF('Input Project'!H339=\"\",\"\",'Input Project'!H339)","v":""},{"$f":"VLOOKUP($A1481,list_database1,$I$10,FALSE)","v":0},"",0,null,0,0,0,0,1,{"$f":"IF(Uncertainty!W235=\"\",\"\",Uncertainty!W235)","v":""},{"$f":"IF(Uncertainty!Z235=\"\",\"\",Uncertainty!Z235)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1973","v":"FC038"},{"$f":"VLOOKUP(A1482,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Temperature of useful heat"},{"$f":"IF('Input Project'!H340=\"\",\"\",'Input Project'!H340)","v":""},{"$f":"VLOOKUP($A1482,list_database1,$I$10,FALSE)","v":"n.a."},"","n.a.",null,"n.a.",0,0,0,1,{"$f":"IF(Uncertainty!W236=\"\",\"\",Uncertainty!W236)","v":""},{"$f":"IF(Uncertainty!Z236=\"\",\"\",Uncertainty!Z236)","v":""},0,0]
[{"$f":"'ID-numbers'!$A1976","v":"FC040a"},{"$f":"VLOOKUP(A1483,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use before allocation 4"},null,null,"",null,{"$f":"VLOOKUP(A1483,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0.17800166505611817},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1977","v":"FC040b"},{"$f":"VLOOKUP(A1484,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use before allocation 4"},null,null,"",null,{"$f":"VLOOKUP(A1484,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0.55455325278356304},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1978","v":"FC040c"},{"$f":"VLOOKUP(A1485,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions before allocation 4"},null,null,"",null,{"$f":"VLOOKUP(A1485,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":59.196326779586677},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1983","v":"FC041a"},{"$f":"VLOOKUP(A1486,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use allocated to heat production"},null,null,"",null,{"$f":"VLOOKUP(A1486,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1984","v":"FC041b"},{"$f":"VLOOKUP(A1487,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use allocated to heat production"},null,null,"",null,{"$f":"VLOOKUP(A1487,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1985","v":"FC041c"},{"$f":"VLOOKUP(A1488,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions allocated to heat production"},null,null,"",null,{"$f":"VLOOKUP(A1488,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1990","v":"FC042a"},{"$f":"VLOOKUP(A1489,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use allocated to heat production"},null,null,"",null,{"$f":"VLOOKUP(A1489,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1991","v":"FC042b"},{"$f":"VLOOKUP(A1490,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use allocated to heat production"},null,null,"",null,{"$f":"VLOOKUP(A1490,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1992","v":"FC042c"},{"$f":"VLOOKUP(A1491,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions allocated to heat production"},null,null,"",null,{"$f":"VLOOKUP(A1491,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1993","v":"FC042d"},{"$f":"VLOOKUP(A1492,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total water use allocated to heat production"},null,null,null,null,{"$f":"VLOOKUP(A1492,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1994","v":"FC042e"},{"$f":"VLOOKUP(A1493,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total land use allocated to heat production"},null,null,null,null,{"$f":"VLOOKUP(A1493,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1995","v":"FC042f"},{"$f":"VLOOKUP(A1494,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total acidification potential allocated to heat production"},null,null,null,null,{"$f":"VLOOKUP(A1494,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1996","v":"FC042g"},{"$f":"VLOOKUP(A1495,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total eutrophication potential allocated to heat production"},null,null,null,null,{"$f":"VLOOKUP(A1495,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A1997","v":"FC043a"},{"$f":"VLOOKUP(A1496,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use allocated to electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1496,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1998","v":"FC043b"},{"$f":"VLOOKUP(A1497,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use allocated to electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1497,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A1999","v":"FC043c"},{"$f":"VLOOKUP(A1498,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions allocated to electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1498,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2004","v":"FC044a"},{"$f":"VLOOKUP(A1499,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use allocated to electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1499,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2005","v":"FC044b"},{"$f":"VLOOKUP(A1500,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use allocated to electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1500,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2006","v":"FC044c"},{"$f":"VLOOKUP(A1501,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions allocated to electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1501,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2007","v":"FC044d"},{"$f":"VLOOKUP(A1502,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total water use allocated to electricity production"},null,null,null,null,{"$f":"VLOOKUP(A1502,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2008","v":"FC044e"},{"$f":"VLOOKUP(A1503,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total land use allocated to electricity production"},null,null,null,null,{"$f":"VLOOKUP(A1503,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2009","v":"FC044f"},{"$f":"VLOOKUP(A1504,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total acidification potential allocated to electricity production"},null,null,null,null,{"$f":"VLOOKUP(A1504,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2010","v":"FC044g"},{"$f":"VLOOKUP(A1505,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total eutrophication potential allocated to electricity production"},null,null,null,null,{"$f":"VLOOKUP(A1505,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2011","v":"FC045a"},{"$f":"VLOOKUP(A1506,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated fossil energy requirement for final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1506,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2012","v":"FC045b"},{"$f":"VLOOKUP(A1507,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated primary energy requirement for final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1507,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2013","v":"FC045c"},{"$f":"VLOOKUP(A1508,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated GHG emissions from final conversion"},null,null,"",null,{"$f":"VLOOKUP(A1508,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2014","v":"FC045d"},{"$f":"VLOOKUP(A1509,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated water use from final conversion"},null,null,null,null,{"$f":"VLOOKUP(A1509,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2015","v":"FC045f"},{"$f":"VLOOKUP(A1510,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated acidification potential from final conversion"},null,null,null,null,{"$f":"VLOOKUP(A1510,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2016","v":"FC045g"},{"$f":"VLOOKUP(A1511,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Totally allocated eutrophication potential from final conversion"},null,null,null,null,{"$f":"VLOOKUP(A1511,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2017","v":"FC046a"},{"$f":"VLOOKUP(A1512,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total fossil energy use allocated to energy production"},null,null,"",null,{"$f":"VLOOKUP(A1512,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0.17800166505611817},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2018","v":"FC046b"},{"$f":"VLOOKUP(A1513,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total primary energy use allocated to energy production"},null,null,"",null,{"$f":"VLOOKUP(A1513,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0.55455325278356304},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2019","v":"FC046c"},{"$f":"VLOOKUP(A1514,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total GHG emissions allocated to energy production"},null,null,"",null,{"$f":"VLOOKUP(A1514,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":59.196326779586677},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2020","v":"FC046d"},{"$f":"VLOOKUP(A1515,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total water use allocated to energy production"},null,null,null,null,{"$f":"VLOOKUP(A1515,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":422.20878511090552},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2021","v":"FC046e"},{"$f":"VLOOKUP(A1516,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total land use allocated to energy production"},null,null,null,null,{"$f":"VLOOKUP(A1516,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":1.9132606099961733E-2},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2022","v":"FC046f"},{"$f":"VLOOKUP(A1517,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total acidification potential allocated to energy production"},null,null,null,null,{"$f":"VLOOKUP(A1517,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0.93786277735394152},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2023","v":"FC046g"},{"$f":"VLOOKUP(A1518,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total eutrophication potential allocated to energy production"},null,null,null,null,{"$f":"VLOOKUP(A1518,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":3.3257093356913932},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2024","v":"FC047a"},{"$f":"VLOOKUP(A1519,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy requirement of reference system for heat"},null,null,"",null,{"$f":"VLOOKUP(A1519,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":1.43},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2025","v":"FC047b"},{"$f":"VLOOKUP(A1520,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy requirement of reference system for heat"},null,null,"",null,{"$f":"VLOOKUP(A1520,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":2.145},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2026","v":"FC047c"},{"$f":"VLOOKUP(A1521,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions of reference system for heat"},null,null,"",null,{"$f":"VLOOKUP(A1521,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":85.18},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2031","v":"FC048a"},{"$f":"VLOOKUP(A1522,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy requirement of reference system for electricity"},null,null,"",null,{"$f":"VLOOKUP(A1522,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":2.7275},"","","","",0,null,null,{"$f":"IF($L1522=1,VLOOKUP($A1522,list_database1,$I$10+1,FALSE),\"\")","v":""},{"$f":"IF($L1522=1,VLOOKUP($A1522,list_database1,$I$10+2,FALSE),\"\")","v":""}]
[{"$f":"'ID-numbers'!$A2032","v":"FC048b"},{"$f":"VLOOKUP(A1523,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy requirement of reference system for electricity"},null,null,"",null,{"$f":"VLOOKUP(A1523,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":4.0912500000000005},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2033","v":"FC048c"},{"$f":"VLOOKUP(A1524,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions of reference system for electricity"},null,null,{"$f":"IF(MonteCarlo=1,IF($L1524=1,IF($H1524=\"n.a.\",0,IF($H1524<0.009,0,MIN(MAX(NORMINV(RAND(),$H1524,$K1524),$I1524),$J1524))),\"\"),\"\")","v":""},null,{"$f":"VLOOKUP(A1524,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":129.19},{"$f":"IF($L1524=1,IF($C1524=\"\",$D1524,$C1524),\"\")","v":""},"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2038","v":"FC049a"},{"$f":"VLOOKUP(A1525,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy reduction of heat production"},null,null,"",null,{"$f":"VLOOKUP(A1525,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"",{"$f":"IF($L1525=1,IF($M1525=\"\",$O1525,$M1525),\"\")","v":""},{"$f":"IF($L1525=1,IF($N1525=\"\",$P1525,$N1525),\"\")","v":""},{"$f":"IF($L1525=1,($J1525-$I1525)/6,\"\")","v":""},0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2039","v":"FC049b"},{"$f":"VLOOKUP(A1526,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy reduction of heat production"},null,null,"",null,{"$f":"VLOOKUP(A1526,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2040","v":"FC049c"},{"$f":"VLOOKUP(A1527,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emission reduction of heat production"},null,null,"",null,{"$f":"VLOOKUP(A1527,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2041","v":"FC049d"},{"$f":"VLOOKUP(A1528,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use reduction of heat production"},null,null,null,null,{"$f":"VLOOKUP(A1528,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2042","v":"FC049e"},{"$f":"VLOOKUP(A1529,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use reduction of heat production"},null,null,null,null,{"$f":"VLOOKUP(A1529,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2043","v":"FC049f"},{"$f":"VLOOKUP(A1530,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Acidification potential reduction of heat production"},null,null,null,null,{"$f":"VLOOKUP(A1530,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2044","v":"FC049g"},{"$f":"VLOOKUP(A1531,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Eutrophication potential reduction of heat production"},null,null,null,null,{"$f":"VLOOKUP(A1531,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2045","v":"FC050a"},{"$f":"VLOOKUP(A1532,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy reduction of electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1532,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2046","v":"FC050b"},{"$f":"VLOOKUP(A1533,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy reduction of electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1533,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2047","v":"FC050c"},{"$f":"VLOOKUP(A1534,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emission reduction of electricity production"},null,null,"",null,{"$f":"VLOOKUP(A1534,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2048","v":"FC050d"},{"$f":"VLOOKUP(A1535,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use reduction of electricity production"},null,null,null,null,{"$f":"VLOOKUP(A1535,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2049","v":"FC050e"},{"$f":"VLOOKUP(A1536,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use reduction of electricity production"},null,null,null,null,{"$f":"VLOOKUP(A1536,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2050","v":"FC050f"},{"$f":"VLOOKUP(A1537,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Acidification potential reduction of electricity production"},null,null,null,null,{"$f":"VLOOKUP(A1537,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2051","v":"FC050g"},{"$f":"VLOOKUP(A1538,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Eutrophication potential reduction of electricity production"},null,null,null,null,{"$f":"VLOOKUP(A1538,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2052","v":"FC051a"},{"$f":"VLOOKUP(A1539,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy requirement of total reference system"},null,null,"",null,{"$f":"VLOOKUP(A1539,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":1.1599999999999999},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2053","v":"FC051b"},{"$f":"VLOOKUP(A1540,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy requirement of total reference system"},null,null,"",null,{"$f":"VLOOKUP(A1540,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":1.7399999999999998},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2054","v":"FC051c"},{"$f":"VLOOKUP(A1541,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions of total reference system"},null,null,"",null,{"$f":"VLOOKUP(A1541,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":87.6388888888889},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2055","v":"FC051d"},{"$f":"VLOOKUP(A1542,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use of total reference system"},null,null,null,null,{"$f":"VLOOKUP(A1542,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2056","v":"FC051e"},{"$f":"VLOOKUP(A1543,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use of total reference system"},null,null,null,null,{"$f":"VLOOKUP(A1543,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2057","v":"FC051f"},{"$f":"VLOOKUP(A1544,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Acidification potential of total reference system"},null,null,null,null,{"$f":"VLOOKUP(A1544,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2058","v":"FC051g"},{"$f":"VLOOKUP(A1545,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Eutrophication potential of total reference system"},null,null,null,null,{"$f":"VLOOKUP(A1545,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2059","v":"FC052a"},{"$f":"VLOOKUP(A1546,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy reduction of total energy production"},null,null,"",null,{"$f":"VLOOKUP(A1546,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":84.655028874472578},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2060","v":"FC052b"},{"$f":"VLOOKUP(A1547,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy reduction of total energy production"},null,null,"",null,{"$f":"VLOOKUP(A1547,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":68.129123403243497},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2061","v":"FC052c"},{"$f":"VLOOKUP(A1548,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emission reduction of total energy production"},null,null,"",null,{"$f":"VLOOKUP(A1548,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":32.454270552611092},"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2062","v":"FC052d"},{"$f":"VLOOKUP(A1549,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use reduction of total energy production"},null,null,null,null,{"$f":"VLOOKUP(A1549,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2063","v":"FC052e"},{"$f":"VLOOKUP(A1550,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use reduction of total energy production"},null,null,null,null,{"$f":"VLOOKUP(A1550,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2064","v":"FC052f"},{"$f":"VLOOKUP(A1551,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Acidification potential reduction of total energy production"},null,null,null,null,{"$f":"VLOOKUP(A1551,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2065","v":"FC052g"},{"$f":"VLOOKUP(A1552,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Eutrophication potential reduction of total energy production"},null,null,null,null,{"$f":"VLOOKUP(A1552,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2068","v":"FC055"},{"$f":"VLOOKUP(A1553,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Total carbon debt due to land use change"},null,null,null,null,{"$f":"VLOOKUP(A1553,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2069","v":"FC056"},{"$f":"VLOOKUP(A1554,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Repayment time"},null,null,null,null,{"$f":"VLOOKUP(A1554,'Final conversion'!$D$9:$G$5074,4,FALSE)","v":0},null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2072","v":"FC058a"},{"$f":"VLOOKUP(A1555,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use for final conversion process"},{"$f":"IF('Input RU'!K69=\"\",\"\",'Input RU'!K69)","v":""},{"$f":"VLOOKUP($A1555,list_database1,$I$10,FALSE)","v":0},"",{"$f":"IF($L1555=1,IF(MonteCarlo=1,$E1555,IF($C1555=\"\",$D1555,$C1555)),IF($C1555=\"\",$D1555,$C1555))","v":0},null,0,0,0,0,1,{"$f":"IF(Uncertainty!W228=\"\",\"\",Uncertainty!W228)","v":""},{"$f":"IF(Uncertainty!Z228=\"\",\"\",Uncertainty!Z228)","v":""},0,0]
[{"$f":"'ID-numbers'!$A2084","v":"FC080a"},{"$f":"VLOOKUP(A1556,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No forced labour, final conversion"},{"$f":"IF('Input LW'!U141=\"\",\"\",'Input LW'!U141)","v":""},{"$f":"VLOOKUP($A1556,list_database1,$I$10,FALSE)","v":"Fulfilled"},"",{"$f":"IF($L1556=1,IF(MonteCarlo=1,$E1556,IF($C1556=\"\",$D1556,$C1556)),IF($C1556=\"\",$D1556,$C1556))","v":"Fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2085","v":"FC080b"},{"$f":"VLOOKUP(A1557,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No child labour, final conversion"},{"$f":"IF('Input LW'!U142=\"\",\"\",'Input LW'!U142)","v":""},{"$f":"VLOOKUP($A1557,list_database1,$I$10,FALSE)","v":"Fulfilled"},"",{"$f":"IF($L1557=1,IF(MonteCarlo=1,$E1557,IF($C1557=\"\",$D1557,$C1557)),IF($C1557=\"\",$D1557,$C1557))","v":"Fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2086","v":"FC080c"},{"$f":"VLOOKUP(A1558,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Good social practices regarding human rights, final conversion"},{"$f":"IF('Input LW'!U143=\"\",\"\",'Input LW'!U143)","v":""},{"$f":"VLOOKUP($A1558,list_database1,$I$10,FALSE)","v":"Fulfilled"},"",{"$f":"IF($L1558=1,IF(MonteCarlo=1,$E1558,IF($C1558=\"\",$D1558,$C1558)),IF($C1558=\"\",$D1558,$C1558))","v":"Fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2087","v":"FC080d"},{"$f":"VLOOKUP(A1559,'ID-numbers'!$1:$1048576,2,FALSE)","v":"No discrimination, final conversion"},{"$f":"IF('Input LW'!U144=\"\",\"\",'Input LW'!U144)","v":""},{"$f":"VLOOKUP($A1559,list_database1,$I$10,FALSE)","v":"Fulfilled"},"",{"$f":"IF($L1559=1,IF(MonteCarlo=1,$E1559,IF($C1559=\"\",$D1559,$C1559)),IF($C1559=\"\",$D1559,$C1559))","v":"Fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2088","v":"FC080e"},{"$f":"VLOOKUP(A1560,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land is used legitimately / land rights have been secured, final conversion"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2089","v":"FC080f"},{"$f":"VLOOKUP(A1561,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, final conversion"},{"$f":"IF('Input LW'!U145=\"\",\"\",'Input LW'!U145)","v":""},{"$f":"VLOOKUP($A1561,list_database1,$I$10,FALSE)","v":"Fulfilled"},"",{"$f":"IF($L1561=1,IF(MonteCarlo=1,$E1561,IF($C1561=\"\",$D1561,$C1561)),IF($C1561=\"\",$D1561,$C1561))","v":"Fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2090","v":"FC080g"},{"$f":"VLOOKUP(A1562,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Food security, final conversion"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2091","v":"FC081a"},{"$f":"VLOOKUP(A1563,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair legal contracts, final conversion"},{"$f":"IF('Input LW'!U147=\"\",\"\",'Input LW'!U147)","v":""},{"$f":"VLOOKUP($A1563,list_database1,$I$10,FALSE)","v":"Fulfilled"},"",{"$f":"IF($L1563=1,IF(MonteCarlo=1,$E1563,IF($C1563=\"\",$D1563,$C1563)),IF($C1563=\"\",$D1563,$C1563))","v":"Fulfilled"},null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2092","v":"FC081b"},{"$f":"VLOOKUP(A1564,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Workers rights, final conversion"},{"$f":"IF('Input LW'!U148=\"\",\"\",'Input LW'!U148)","v":""},"Fulfilled","","Fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2093","v":"FC081c"},{"$f":"VLOOKUP(A1565,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, final conversion"},{"$f":"IF('Input LW'!U149=\"\",\"\",'Input LW'!U149)","v":""},"Fulfilled","","Fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2094","v":"FC081d"},{"$f":"VLOOKUP(A1566,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fair wages and compensation rules, final conversion"},{"$f":"IF('Input LW'!U150=\"\",\"\",'Input LW'!U150)","v":""},"Fulfilled","","Fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2095","v":"FC081e"},{"$f":"VLOOKUP(A1567,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health, safety and hygiene policy, final conversion"},{"$f":"IF('Input LW'!U151=\"\",\"\",'Input LW'!U151)","v":""},"Fulfilled","","Fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2096","v":"FC081f"},{"$f":"VLOOKUP(A1568,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, final conversion"},{"$f":"IF('Input LW'!U152=\"\",\"\",'Input LW'!U152)","v":""},"Fulfilled","","Fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2097","v":"FC081g"},{"$f":"VLOOKUP(A1569,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Health and safety training, final conversion"},{"$f":"IF('Input LW'!U153=\"\",\"\",'Input LW'!U153)","v":""},"Fulfilled","","Fulfilled",null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2098","v":"FC082"},{"$f":"VLOOKUP(A1570,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Human and property rights, final conversion_score"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2099","v":"FC083"},{"$f":"VLOOKUP(A1571,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Labour rights and conditions, final conversion_score"},null,null,"",null,null,"","","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2100","v":"FC100a"},{"$f":"VLOOKUP(A1572,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC082a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2101","v":"FC100b"},{"$f":"VLOOKUP(A1573,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC082b"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2102","v":"FC100c"},{"$f":"VLOOKUP(A1574,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC082c"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2103","v":"FC100d"},{"$f":"VLOOKUP(A1575,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC082d"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2104","v":"FC100e"},{"$f":"VLOOKUP(A1576,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FP106a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2105","v":"FC100f"},{"$f":"VLOOKUP(A1577,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC082f"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2106","v":"FC100g"},{"$f":"VLOOKUP(A1578,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC082g"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2107","v":"FC100h"},{"$f":"VLOOKUP(A1579,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FP107a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2108","v":"FC101a"},{"$f":"VLOOKUP(A1580,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC582a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2109","v":"FC101b"},{"$f":"VLOOKUP(A1581,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC582b"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2110","v":"FC101c"},{"$f":"VLOOKUP(A1582,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC582c"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2111","v":"FC101d"},{"$f":"VLOOKUP(A1583,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC582d"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2112","v":"FC101e"},{"$f":"VLOOKUP(A1584,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FP606a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2113","v":"FC101f"},{"$f":"VLOOKUP(A1585,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC582f"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2114","v":"FC101g"},{"$f":"VLOOKUP(A1586,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of BC582g"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2115","v":"FC101h"},{"$f":"VLOOKUP(A1587,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FP607a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2116","v":"FC102a"},{"$f":"VLOOKUP(A1588,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FC046a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2117","v":"FC102b"},{"$f":"VLOOKUP(A1589,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FC046b"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2118","v":"FC102c"},{"$f":"VLOOKUP(A1590,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FC046c"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2119","v":"FC102d"},{"$f":"VLOOKUP(A1591,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FC046d"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2120","v":"FC102e"},{"$f":"VLOOKUP(A1592,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FC046e"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2121","v":"FC102f"},{"$f":"VLOOKUP(A1593,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FC046f"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2122","v":"FC102g"},{"$f":"VLOOKUP(A1594,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FC046g"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2123","v":"FC102h"},{"$f":"VLOOKUP(A1595,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Mean of FC055"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2124","v":"FC103a"},{"$f":"VLOOKUP(A1596,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC082a"},null,null,null,null,null,null,"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2125","v":"FC103b"},{"$f":"VLOOKUP(A1597,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC082b"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2126","v":"FC103c"},{"$f":"VLOOKUP(A1598,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC082c"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2127","v":"FC103d"},{"$f":"VLOOKUP(A1599,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC082d"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2128","v":"FC103e"},{"$f":"VLOOKUP(A1600,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FP106a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2129","v":"FC103f"},{"$f":"VLOOKUP(A1601,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC082f"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2130","v":"FC103g"},{"$f":"VLOOKUP(A1602,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC082g"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2131","v":"FC103h"},{"$f":"VLOOKUP(A1603,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FP107a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2132","v":"FC104a"},{"$f":"VLOOKUP(A1604,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC582a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2133","v":"FC104b"},{"$f":"VLOOKUP(A1605,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC582b"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2134","v":"FC104c"},{"$f":"VLOOKUP(A1606,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC582c"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2135","v":"FC104d"},{"$f":"VLOOKUP(A1607,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC582d"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2136","v":"FC104e"},{"$f":"VLOOKUP(A1608,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FP606a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2137","v":"FC104f"},{"$f":"VLOOKUP(A1609,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC582f"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2138","v":"FC104g"},{"$f":"VLOOKUP(A1610,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of BC582g"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2139","v":"FC104h"},{"$f":"VLOOKUP(A1611,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FP607a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2140","v":"FC105a"},{"$f":"VLOOKUP(A1612,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FC046a"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2141","v":"FC105b"},{"$f":"VLOOKUP(A1613,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FC046b"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2142","v":"FC105c"},{"$f":"VLOOKUP(A1614,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FC046c"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2143","v":"FC105d"},{"$f":"VLOOKUP(A1615,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FC046d"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2144","v":"FC105e"},{"$f":"VLOOKUP(A1616,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FC046e"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2145","v":"FC105f"},{"$f":"VLOOKUP(A1617,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FC046f"},null,null,null,null,null,null,"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2146","v":"FC105g"},{"$f":"VLOOKUP(A1618,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FC046g"},null,null,null,null,null,null,"","","",0,null,null,"",""]
[{"$f":"'ID-numbers'!$A2147","v":"FC105h"},{"$f":"VLOOKUP(A1619,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Standard deviation of FC055"},null,null,null,null,null,null,null,null,null,0]
[{"$f":"'ID-numbers'!$A2148","v":"FC110a"},{"$f":"VLOOKUP(A1620,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy requirement of reference system for biogas"}]
[{"$f":"'ID-numbers'!$A2149","v":"FC110b"},{"$f":"VLOOKUP(A1621,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy requirement of reference system for biogas"}]
[{"$f":"'ID-numbers'!$A2150","v":"FC110c"},{"$f":"VLOOKUP(A1622,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions of reference system for biogas"}]
[{"$f":"'ID-numbers'!$A2151","v":"FC110d"},{"$f":"VLOOKUP(A1623,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use of reference system for biogas"}]
[{"$f":"'ID-numbers'!$A2152","v":"FC110e"},{"$f":"VLOOKUP(A1624,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use of reference system for biogas"}]
[{"$f":"'ID-numbers'!$A2153","v":"FC110f"},{"$f":"VLOOKUP(A1625,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Acidification potential of reference system for biogas"}]
[{"$f":"'ID-numbers'!$A2154","v":"FC110g"},{"$f":"VLOOKUP(A1626,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Eutrophication potential of reference system for biogas"}]
[{"$f":"'ID-numbers'!$A2155","v":"FC111a"},{"$f":"VLOOKUP(A1627,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy requirement of reference system for diesel"}]
[{"$f":"'ID-numbers'!$A2156","v":"FC111b"},{"$f":"VLOOKUP(A1628,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy requirement of reference system for diesel"}]
[{"$f":"'ID-numbers'!$A2157","v":"FC111c"},{"$f":"VLOOKUP(A1629,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions of reference system for diesel"}]
[{"$f":"'ID-numbers'!$A2158","v":"FC111d"},{"$f":"VLOOKUP(A1630,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use of reference system for diesel"}]
[{"$f":"'ID-numbers'!$A2159","v":"FC111e"},{"$f":"VLOOKUP(A1631,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use of reference system for diesel"}]
[{"$f":"'ID-numbers'!$A2160","v":"FC111f"},{"$f":"VLOOKUP(A1632,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Acidification potential of reference system for diesel"}]
[{"$f":"'ID-numbers'!$A2161","v":"FC111g"},{"$f":"VLOOKUP(A1633,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Eutrophication potential of reference system for diesel"}]
[{"$f":"'ID-numbers'!$A2162","v":"FC112a"},{"$f":"VLOOKUP(A1634,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy requirement of reference system for gasoline"}]
[{"$f":"'ID-numbers'!$A2163","v":"FC112b"},{"$f":"VLOOKUP(A1635,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy requirement of reference system for gasoline"}]
[{"$f":"'ID-numbers'!$A2164","v":"FC112c"},{"$f":"VLOOKUP(A1636,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions of reference system for gasoline"}]
[{"$f":"'ID-numbers'!$A2165","v":"FC112d"},{"$f":"VLOOKUP(A1637,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use of reference system for gasoline"}]
[{"$f":"'ID-numbers'!$A2166","v":"FC112e"},{"$f":"VLOOKUP(A1638,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use of reference system for gasoline"}]
[{"$f":"'ID-numbers'!$A2167","v":"FC112f"},{"$f":"VLOOKUP(A1639,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Acidification potential of reference system for gasoline"}]
[{"$f":"'ID-numbers'!$A2168","v":"FC112g"},{"$f":"VLOOKUP(A1640,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Eutrophication potential of reference system for gasoline"}]
[{"$f":"'ID-numbers'!$A2169","v":"FC113a"},{"$f":"VLOOKUP(A1641,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Fossil energy requirement of reference system for heavy fuel oil"}]
[{"$f":"'ID-numbers'!$A2170","v":"FC113b"},{"$f":"VLOOKUP(A1642,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Primary energy requirement of reference system for heavy fuel oil"}]
[{"$f":"'ID-numbers'!$A2171","v":"FC113c"},{"$f":"VLOOKUP(A1643,'ID-numbers'!$1:$1048576,2,FALSE)","v":"GHG emissions of reference system for heavy fuel oil"}]
[{"$f":"'ID-numbers'!$A2172","v":"FC113d"},{"$f":"VLOOKUP(A1644,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Water use of reference system for heavy fuel oil"}]
[{"$f":"'ID-numbers'!$A2173","v":"FC113e"},{"$f":"VLOOKUP(A1645,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Land use of reference system for heavy fuel oil"}]
[{"$f":"'ID-numbers'!$A2174","v":"FC113f"},{"$f":"VLOOKUP(A1646,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Acidification potential of reference system for heavy fuel oil"}]
[{"$f":"'ID-numbers'!$A2175","v":"FC113g"},{"$f":"VLOOKUP(A1647,'ID-numbers'!$1:$1048576,2,FALSE)","v":"Eutrophication potential of reference system for heavy fuel oil"}]
[]
[]
[null,null,null,null,null,null,null,null,"","","",null,null,null,"",""]

{"sheet":"Data","index":14,"n_rows":351,"n_cols":100,"rows_kept":351,"cut":false,"hidden":true,"merged":[[2,86,2,89],[2,91,2,94],[2,71,2,74],[2,76,2,79],[2,96,2,99],[2,81,2,84],[2,21,2,24],[1,0,1,2],[2,6,2,9],[2,11,2,14],[2,16,2,19],[2,56,2,59],[2,26,2,29],[2,36,2,39],[2,41,2,44],[2,46,2,49],[2,51,2,54],[2,31,2,34]]}
["Database variables (feedstocks & conversion)"]
["ID-numbers",null,null,"Description","Unit","Palm oil (stearin) from palm fruits, refinery",null,null,null,null,"Palm oil (olein) from palm fruits, refinery",null,null,null,null,null,null,null,null,null,"Biogas from organic residues, anaerobic digestion",null,null,null,null,"Biogas from maize + organic residues, anaerobic digestion + purification",null,null,null,null,"None",null,null,null,null,"CHP - gas",null,null,null,null,"CHP - pure plant oil",null,null,null,null,"CHP - dual fuel (gas + ppo)",null,null,null,null,"LBM from GFT, anaerobic digestion + upgrading",null,null,null,null,"No final conversion, only biofuel production",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"LBM from harvested grass, anaerobic digestion + upgrading",null,null,null,null,"Biodiesel from fatty residues, esterification",null,null,null,null,"Bio-oil from wood waste, fast pyrolysis",null,null,null,null,"LBM from GFT, anaerobic digestion + upgrading"]
["Data Source",null,null,null,null,"DS003 (Column AA), DS002","Uncertainty",null,null,null,"DS003 (Column AA), DS002","Uncertainty",null,null,null,null,null,null,null,null,"DS001, DS005, DS006","Uncertainty",null,null,null,"DS001, DS005, DS006","Uncertainty",null,null,null,null,"Uncertainty",null,null,null,"DS005","Uncertainty",null,null,null,"DS005","Uncertainty",null,null,null,"DS005","Uncertainty",null,null,null,"DS001, DS005, DS006","Uncertainty",null,null,null,null,"Uncertainty",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DS001, DS005, DS006","Uncertainty",null,null,null,"DS001, DS005, DS006","Uncertainty",null,null,null,"DS001, DS005, DS006","Uncertainty",null,null,null,"DS001, DS005, DS006","Uncertainty"]
["Remarks",null,null,null,null,"FP - FT - BC","Min","Max","σ","distr.","FP - FT - BC","Min","Max","σ","distr.",null,null,null,null,null,"FP - FT - BC","Min","Max","σ","distr.","FP - FT - BC","Min","Max","σ","distr.","FP - FT - BC","Min","Max","σ","distr.","FC","Min","Max","σ","distr.","FC","Min","Max","σ","distr.","FC","Min","Max","σ","distr.","FP - FT - BC","Min","Max","σ","distr.","FC","Min","Max","σ","distr.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FP - FT - BC","Min","Max","σ","distr.","FP - FT - BC","Min","Max","σ","distr.","FP - FT - BC","Min","Max","σ","distr.","FP - FT - BC","Min","Max","σ","distr."]
["LC001","LC501",null,{"$f":"VLOOKUP(Data!A5,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"FT_Process description transport 1 (mode 1-2-3)"},null,"Transport of FFB to the mill",null,null,null,null,"Transport of FFB to the mill",null,null,null,null,null,null,null,null,null,"No transport",null,null,null,null,"Transport to the conversion plant",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Transport",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Transport",null,null,null,null,"Transport",null,null,null,null,"Transport",null,null,null,null,"Transport"]
["LC002","LC502",null,{"$f":"VLOOKUP(Data!A6,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"FT_Process description treatment 1"},null,"No treatment",null,null,null,null,"No treatment",null,null,null,null,null,null,null,null,null,"Storage in cellar/silage",null,null,null,null,"Storage in cellar/silage",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Storage in cellar/silage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Storage in cellar/silage",null,null,null,null,"Storage in cellar/silage",null,null,null,null,"Storage in cellar/silage",null,null,null,null,"Storage in cellar/silage"]
["LC003","LC503",null,{"$f":"VLOOKUP(Data!A7,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"BC_Process description conversion process 1"},null,"Production of Crude Palm Oil (CPO)",null,null,null,null,"Production of Crude Palm Oil (CPO)",null,null,null,null,null,null,null,null,null,"Anaerobic co-digestion",null,null,null,null,"Anaerobic co-digestion",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anaerobic digestion+post-composting",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anaerobic digestion+post-composting",null,null,null,null,"Esterification",null,null,null,null,"Pyrolysis",null,null,null,null,"Anaerobic digestion+post-composting"]
["LC004","LC504",null,{"$f":"VLOOKUP(Data!A8,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"FT_Process description transport 2 (mode 4-5-6)"},null,"Transport of CPO to Belgium",null,null,null,null,"Transport of CPO to Belgium",null,null,null,null,null,null,null,null,null,"No transport",null,null,null,null,"No transport",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No transport",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No transport",null,null,null,null,"No transport",null,null,null,null,"No transport",null,null,null,null,"No transport"]
["LC005","LC505",null,{"$f":"VLOOKUP(Data!A9,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"FT_Process description treatment 2"},null,"No treatment",null,null,null,null,"No treatment",null,null,null,null,null,null,null,null,null,"Biogas storage",null,null,null,null,"Biogas storage",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biogas storage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biogas storage",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biogas storage"]
["LC006","LC506",null,{"$f":"VLOOKUP(Data!A10,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"BC_Process description conversion process 2"},null,"Refinery of Crude Palm Oil",null,null,null,null,"Refinery of Crude Palm Oil",null,null,null,null,null,null,null,null,null,"Composting",null,null,null,null,"Biogas purification",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Purification",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Purification",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Purification"]
["LC007","LC507",null,{"$f":"VLOOKUP(Data!A11,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"FT_Process description transport 3 (mode 7-8-9)"},null,"Transport of PS to the final conversion unit",null,null,null,null,"Transport of PS to the final conversion unit",null,null,null,null,null,null,null,null,null,"No transport",null,null,null,null,"No transport",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No transport",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No transport",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No transport"]
["LC008","LC508",null,{"$f":"VLOOKUP(Data!A12,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"FT_Process description treatment 3"},null,"No treatment",null,null,null,null,"No treatment",null,null,null,null,null,null,null,null,null,"No treatment",null,null,null,null,"No treatment",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No treatment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No treatment"]
["LC010",null,null,{"$f":"VLOOKUP(Data!A13,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"FC_Process description final conversion"},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Combustion at CHP plant",null,null,null,null,"Combustion at CHP plant",null,null,null,null,"Combustion at CHP plant",null,null,null,null,null,null,null,null,null,"No final conversion"]
[]
["FP001","FP501",null,{"$f":"VLOOKUP(Data!A15,'ID-numbers'!A$2:B$2373,2,FALSE)","v":"Feedstock type 1"},{"$f":"VLOOKUP(Data!A15,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Fresh palm fruit bunches (FFB)",null,null,"n.a.","n.a.","Fresh palm fruit bunches (FFB)",null,null,"n.a.","n.a.",null,null,null,null,null,"No crop",null,null,"n.a.","n.a.","Maize (corn)",null,null,"n.a.","n.a.","No crop",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","No crop",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No crop",null,null,"n.a.","n.a.","No crop",null,null,"n.a.","n.a.","No crop",null,null,"n.a.","n.a.","No crop",null,null,"n.a.","n.a."]
["FP002","FP502",null,{"$f":"VLOOKUP(Data!A16,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Origin of the feedstock"},{"$f":"VLOOKUP(Data!A16,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Malaysia",null,null,"n.a.","n.a.","Malaysia",null,null,"n.a.","n.a.",null,null,null,null,null,"Netherlands",null,null,"n.a.","n.a.","Belgium",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Netherlands",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Netherlands",null,null,"n.a.","n.a.","Netherlands",null,null,"n.a.","n.a.","Netherlands",null,null,"n.a.","n.a.","Belgium",null,null,"n.a.","n.a."]
["FP003a","FP503a",null,{"$f":"VLOOKUP(Data!A17,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 1 per ha"},{"$f":"VLOOKUP(Data!A17,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},19000,11450,21000,{"$f":"(H17-G17)/6","v":1591.6666666666667},"normal",19000,11450,21000,{"$f":"(M17-L17)/6","v":1591.6666666666667},"normal",null,null,null,null,null,32000000,400000,600000,{"$f":"(W17-V17)/6","v":33333.333333333336},"normal",44000,41000,47000,{"$f":"(AB17-AA17)/6","v":1000},"normal",0,0,0,{"$f":"(AG17-AF17)/6","v":0},"normal",null,null,null,{"$f":"(AL17-AK17)/6","v":0},"normal",null,null,null,{"$f":"(AQ17-AP17)/6","v":0},"normal",null,null,null,{"$f":"(AV17-AU17)/6","v":0},"normal",32000000,null,null,{"$f":"(BA17-AZ17)/6","v":0},"normal",null,null,null,{"$f":"(BF17-BE17)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,7770000,null,null,{"$f":"(CE17-CD17)/6","v":0},"normal",8000000,null,null,{"$f":"(CJ17-CI17)/6","v":0},"normal",44737000,null,null,{"$f":"(CO17-CN17)/6","v":0},"normal",32000000,null,null,{"$f":"(CT17-CS17)/6","v":0},"normal"]
["FP005","FP505",null,{"$f":"VLOOKUP(Data!A18,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Number of harvests per year"},{"$f":"VLOOKUP(Data!A18,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"1/yr"},1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP009","FP509",null,{"$f":"VLOOKUP(Data!A19,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of the harvested crop"},{"$f":"VLOOKUP(Data!A19,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},34,30,36,{"$f":"(H19-G19)/6","v":1},"normal",34,30,36,{"$f":"(M19-L19)/6","v":1},"normal",null,null,null,null,null,55,40,60,{"$f":"(W19-V19)/6","v":3.3333333333333335},"normal",70,65,73,{"$f":"(AB19-AA19)/6","v":1.3333333333333333},"normal",0,0,0,{"$f":"(AG19-AF19)/6","v":0},"normal",null,null,null,{"$f":"(AL19-AK19)/6","v":0},"normal",null,null,null,{"$f":"(AQ19-AP19)/6","v":0},"normal",null,null,null,{"$f":"(AV19-AU19)/6","v":0},"normal",55,null,null,{"$f":"(BA19-AZ19)/6","v":0},"normal",null,null,null,{"$f":"(BF19-BE19)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,62,null,null,{"$f":"(CE19-CD19)/6","v":0},"normal",1.21,null,null,{"$f":"(CJ19-CI19)/6","v":0},"normal",5,null,null,{"$f":"(CO19-CN19)/6","v":0},"normal",55,null,null,{"$f":"(CT19-CS19)/6","v":0},"normal"]
["FP016a","FP516a",null,{"$f":"VLOOKUP(Data!A20,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of by-product 1"},{"$f":"VLOOKUP(Data!A20,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP016b","FP516b",null,{"$f":"VLOOKUP(Data!A21,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of by-product 2"},{"$f":"VLOOKUP(Data!A21,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP017a","FP517a",null,{"$f":"VLOOKUP(Data!A22,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Yield rate (moist/wet) of by-product 1 per ha"},{"$f":"VLOOKUP(Data!A22,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},0,0,0,{"$f":"(H22-G22)/6","v":0},"normal",0,0,0,{"$f":"(M22-L22)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W22-V22)/6","v":0},"normal",0,0,0,{"$f":"(AB22-AA22)/6","v":0},"normal",0,0,0,{"$f":"(AG22-AF22)/6","v":0},"normal",null,null,null,{"$f":"(AL22-AK22)/6","v":0},"normal",null,null,null,{"$f":"(AQ22-AP22)/6","v":0},"normal",null,null,null,{"$f":"(AV22-AU22)/6","v":0},"normal",0,null,null,{"$f":"(BA22-AZ22)/6","v":0},"normal",null,null,null,{"$f":"(BF22-BE22)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE22-CD22)/6","v":0},"normal",0,null,null,{"$f":"(CJ22-CI22)/6","v":0},"normal",0,null,null,{"$f":"(CO22-CN22)/6","v":0},"normal",0,null,null,{"$f":"(CT22-CS22)/6","v":0},"normal"]
["FP017b","FP517b",null,{"$f":"VLOOKUP(Data!A23,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Yield rate (moist/wet) of by-product 2 per ha"},{"$f":"VLOOKUP(Data!A23,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},0,0,0,{"$f":"(H23-G23)/6","v":0},"normal",0,0,0,{"$f":"(M23-L23)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W23-V23)/6","v":0},"normal",0,0,0,{"$f":"(AB23-AA23)/6","v":0},"normal",0,0,0,{"$f":"(AG23-AF23)/6","v":0},"normal",null,null,null,{"$f":"(AL23-AK23)/6","v":0},"normal",null,null,null,{"$f":"(AQ23-AP23)/6","v":0},"normal",null,null,null,{"$f":"(AV23-AU23)/6","v":0},"normal",0,null,null,{"$f":"(BA23-AZ23)/6","v":0},"normal",null,null,null,{"$f":"(BF23-BE23)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE23-CD23)/6","v":0},"normal",0,null,null,{"$f":"(CJ23-CI23)/6","v":0},"normal",0,null,null,{"$f":"(CO23-CN23)/6","v":0},"normal",0,null,null,{"$f":"(CT23-CS23)/6","v":0},"normal"]
["FP019a","FP519a",null,{"$f":"VLOOKUP(Data!A24,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of by-product 1"},{"$f":"VLOOKUP(Data!A24,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP019b","FP519b",null,{"$f":"VLOOKUP(Data!A25,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of by-product 2"},{"$f":"VLOOKUP(Data!A25,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP021a","FP521a",null,{"$f":"VLOOKUP(Data!A26,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of by-product 1"},{"$f":"VLOOKUP(Data!A26,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP021b","FP521b",null,{"$f":"VLOOKUP(Data!A27,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of by-product 2"},{"$f":"VLOOKUP(Data!A27,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP022","FP522",null,{"$f":"VLOOKUP(Data!A28,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Use of seeds"},{"$f":"VLOOKUP(Data!A28,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},0,0,200,{"$f":"(H28-G28)/6","v":33.333333333333336},"normal",0,0,200,{"$f":"(M28-L28)/6","v":33.333333333333336},"normal",null,null,null,null,null,0,0,0,{"$f":"(W28-V28)/6","v":0},"normal",0,0,0,{"$f":"(AB28-AA28)/6","v":0},"normal",0,0,0,{"$f":"(AG28-AF28)/6","v":0},"normal",null,null,null,{"$f":"(AL28-AK28)/6","v":0},"normal",null,null,null,{"$f":"(AQ28-AP28)/6","v":0},"normal",null,null,null,{"$f":"(AV28-AU28)/6","v":0},"normal",0,null,null,{"$f":"(BA28-AZ28)/6","v":0},"normal",null,null,null,{"$f":"(BF28-BE28)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE28-CD28)/6","v":0},"normal",0,null,null,{"$f":"(CJ28-CI28)/6","v":0},"normal",0,null,null,{"$f":"(CO28-CN28)/6","v":0},"normal",0,null,null,{"$f":"(CT28-CS28)/6","v":0},"normal"]
["FP023a","FP523a",null,{"$f":"VLOOKUP(Data!A29,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Use of N fertiliser (synthetic)"},{"$f":"VLOOKUP(Data!A29,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},127.908,0,185,30.833333333333332,"normal",127.908,0,185,30.833333333333332,"normal",null,null,null,null,null,0,0,0,0,"normal",185,0,250,41.666666666666664,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP023b","FP523b",null,{"$f":"VLOOKUP(Data!A30,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Use of P2O5 fertiliser"},{"$f":"VLOOKUP(Data!A30,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},143.792,0,160,26.666666666666668,"normal",143.792,0,160,26.666666666666668,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP023c","FP523c",null,{"$f":"VLOOKUP(Data!A31,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Use of K2O fertiliser"},{"$f":"VLOOKUP(Data!A31,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},199.804,0,250,41.666666666666664,"normal",199.804,0,250,41.666666666666664,"normal",null,null,null,null,null,0,0,0,0,"normal",150,0,180,30,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP023d","FP523d",null,{"$f":"VLOOKUP(Data!A32,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Use of CaO fertiliser"},{"$f":"VLOOKUP(Data!A32,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},0,0,100,16.666666666666668,"normal",0,0,100,16.666666666666668,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP023e","FP523e",null,{"$f":"VLOOKUP(Data!A33,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Use of pesticides"},{"$f":"VLOOKUP(Data!A33,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},8.36,0,15,2.5,"normal",8.36,0,15,2.5,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP034","FP534",null,{"$f":"VLOOKUP(Data!A34,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for agricultural machinery"},{"$f":"VLOOKUP(Data!A34,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP037","FP537",null,{"$f":"VLOOKUP(Data!A35,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of fuel used in agricultural machinery"},{"$f":"VLOOKUP(Data!A35,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},47.902000000000001,40,75,5.833333333333333,"normal",47.902000000000001,40,75,{"$f":"(M35-L35)/6","v":5.833333333333333},"normal",null,null,null,null,null,0,0,0,{"$f":"(W35-V35)/6","v":0},"normal",41.6,35,55,{"$f":"(AB35-AA35)/6","v":3.3333333333333335},"normal",0,0,0,{"$f":"(AG35-AF35)/6","v":0},"normal",null,null,null,{"$f":"(AL35-AK35)/6","v":0},"normal",null,null,null,{"$f":"(AQ35-AP35)/6","v":0},"normal",null,null,null,{"$f":"(AV35-AU35)/6","v":0},"normal",0,null,null,{"$f":"(BA35-AZ35)/6","v":0},"normal",null,null,null,{"$f":"(BF35-BE35)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE35-CD35)/6","v":0},"normal",0,null,null,{"$f":"(CJ35-CI35)/6","v":0},"normal",0,null,null,{"$f":"(CO35-CN35)/6","v":0},"normal",0,null,null,{"$f":"(CT35-CS35)/6","v":0},"normal"]
["FP040","FP540",null,{"$f":"VLOOKUP(Data!A36,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Heat energy use for drying and storage of the crop"},{"$f":"VLOOKUP(Data!A36,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJheat/kgfm"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP041","FP541",null,{"$f":"VLOOKUP(Data!A37,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Heat source"},{"$f":"VLOOKUP(Data!A37,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP043","FP543",null,{"$f":"VLOOKUP(Data!A38,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity energy use for drying and storage of the crop"},{"$f":"VLOOKUP(Data!A38,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/kgfm"},0,0,0,0,"normal",0,0,0,{"$f":"(M38-L38)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W38-V38)/6","v":0},"normal",0,0,0,{"$f":"(AB38-AA38)/6","v":0},"normal",0,0,0,{"$f":"(AG38-AF38)/6","v":0},"normal",null,null,null,{"$f":"(AL38-AK38)/6","v":0},"normal",null,null,null,{"$f":"(AQ38-AP38)/6","v":0},"normal",null,null,null,{"$f":"(AV38-AU38)/6","v":0},"normal",0,null,null,{"$f":"(BA38-AZ38)/6","v":0},"normal",null,null,null,{"$f":"(BF38-BE38)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE38-CD38)/6","v":0},"normal",0,null,null,{"$f":"(CJ38-CI38)/6","v":0},"normal",0,null,null,{"$f":"(CO38-CN38)/6","v":0},"normal",0,null,null,{"$f":"(CT38-CS38)/6","v":0},"normal"]
["FP044","FP544",null,{"$f":"VLOOKUP(Data!A39,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity source"},{"$f":"VLOOKUP(Data!A39,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP047","FP547",null,{"$f":"VLOOKUP(Data!A40,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Pretreated feedstock"},{"$f":"VLOOKUP(Data!A40,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Fresh palm fruit bunches (FFB)",null,null,"n.a.","n.a.","Fresh palm fruit bunches (FFB)",null,null,"n.a.","n.a.",null,null,null,null,null,"Organic domestical waste",null,null,"n.a.","n.a.","Maize (corn)",null,null,"n.a.","n.a.","No crop",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Organic domestical waste",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Harvested grass",null,null,"n.a.","n.a.","Fatty residues",null,null,"n.a.","n.a.","Wood waste",null,null,"n.a.","n.a.","Organic domestical waste",null,null,"n.a.","n.a."]
["FP049","FP549",null,{"$f":"VLOOKUP(Data!A41,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content pretreated feedstock (LHV)"},{"$f":"VLOOKUP(Data!A41,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"VLOOKUP(F40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":24},null,null,null,null,{"$f":"VLOOKUP(K40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":24},null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(U40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":10.1},null,null,null,null,{"$f":"VLOOKUP(Z40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":18.5},null,null,null,null,{"$f":"VLOOKUP(AE40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(AY40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":10.1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"VLOOKUP(CC40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":17.2},null,null,null,null,{"$f":"VLOOKUP(CH40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":38.799999999999997},null,null,null,null,{"$f":"VLOOKUP(CM40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":17.73},null,null,null,null,{"$f":"VLOOKUP(CR40,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":10.1}]
["FP054","FP554",null,{"$f":"VLOOKUP(Data!A42,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Yield loss through treatment and transport of feedstock 1"},{"$f":"VLOOKUP(Data!A42,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},2,0,5,0.83333333333333337,"normal",2,0,5,{"$f":"(M42-L42)/6","v":0.83333333333333337},"normal",null,null,null,null,null,0,0,5,{"$f":"(W42-V42)/6","v":0.83333333333333337},"normal",0,0,5,{"$f":"(AB42-AA42)/6","v":0.83333333333333337},"normal",0,0,0,{"$f":"(AG42-AF42)/6","v":0},"normal",null,null,null,{"$f":"(AL42-AK42)/6","v":0},"normal",null,null,null,{"$f":"(AQ42-AP42)/6","v":0},"normal",null,null,null,{"$f":"(AV42-AU42)/6","v":0},"normal",0,null,null,{"$f":"(BA42-AZ42)/6","v":0},"normal",null,null,null,{"$f":"(BF42-BE42)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE42-CD42)/6","v":0},"normal",0,null,null,{"$f":"(CJ42-CI42)/6","v":0},"normal",0,null,null,{"$f":"(CO42-CN42)/6","v":0},"normal",0,null,null,{"$f":"(CT42-CS42)/6","v":0},"normal"]
["FP070a","FP570a",null,{"$f":"VLOOKUP(Data!A43,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Climate region"},{"$f":"VLOOKUP(Data!A43,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Tropical Wet",null,null,"n.a.","n.a.","Tropical Wet",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Cool temperate moist",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP070b","FP570b",null,{"$f":"VLOOKUP(Data!A44,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Soil type"},{"$f":"VLOOKUP(Data!A44,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Low activity clay soils",null,null,"n.a.","n.a.","Low activity clay soils",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","High activity clay soils",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP069a","FP569a",null,{"$f":"VLOOKUP(Data!A45,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Actual land use"},{"$f":"VLOOKUP(Data!A45,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Perennial cropland",null,null,"n.a.","n.a.","Perennial cropland",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Annual cropland",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP069c","FP569c",null,{"$f":"VLOOKUP(Data!A46,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Actual land use_specific for carbon stock veg"},{"$f":"VLOOKUP(Data!A46,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Oil palm",null,null,"n.a.","n.a.","Oil palm",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","All other annual crops",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP070c","FP570c",null,{"$f":"VLOOKUP(Data!A47,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Climate region_specific for carbon stock_actual land use"},{"$f":"VLOOKUP(Data!A47,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Tropical wet",null,null,"n.a.","n.a.","Tropical wet",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Cool temperate moist",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP093a","FP593a",null,{"$f":"VLOOKUP(Data!A48,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land management actual land use"},{"$f":"VLOOKUP(Data!A48,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"No till",null,null,"n.a.","n.a.","No till",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Reduced tillage",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP094a","FP594a",null,{"$f":"VLOOKUP(Data!A49,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Input actual land use"},{"$f":"VLOOKUP(Data!A49,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"High without manure",null,null,"n.a.","n.a.","High without manure",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Medium",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP095a","FP595a",null,{"$f":"VLOOKUP(Data!A50,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Domain actual land use"},{"$f":"VLOOKUP(Data!A50,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP096a","FP596a",null,{"$f":"VLOOKUP(Data!A51,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Ecological zone actual land use"},{"$f":"VLOOKUP(Data!A51,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP097a","FP597a",null,{"$f":"VLOOKUP(Data!A52,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Continent actual land use"},{"$f":"VLOOKUP(Data!A52,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP098a","FP598a",null,{"$f":"VLOOKUP(Data!A53,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type actual land use"},{"$f":"VLOOKUP(Data!A53,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP069b","FP569b",null,{"$f":"VLOOKUP(Data!A54,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Previous land use (January 1st, 2008)"},{"$f":"VLOOKUP(Data!A54,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Perennial cropland",null,null,"n.a.","n.a.","Perennial cropland",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Grassland and savannah",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP069d","FP569d",null,{"$f":"VLOOKUP(Data!A55,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Previous land use (January 1st, 2008)_specific for carbon stock veg"},{"$f":"VLOOKUP(Data!A55,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Oil palm",null,null,"n.a.","n.a.","Oil palm",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Grassland and savannah",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP070d","FP570d",null,{"$f":"VLOOKUP(Data!A56,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Climate region_specific for carbon stock_previous land use"},{"$f":"VLOOKUP(Data!A56,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Tropical wet",null,null,"n.a.","n.a.","Tropical wet",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Cool temperate moist",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP093b","FP593b",null,{"$f":"VLOOKUP(Data!A57,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land management previous land use"},{"$f":"VLOOKUP(Data!A57,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"No till",null,null,"n.a.","n.a.","No till",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Nominally managed",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP094b","FP594b",null,{"$f":"VLOOKUP(Data!A58,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Input previous land use"},{"$f":"VLOOKUP(Data!A58,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"High without manure",null,null,"n.a.","n.a.","High without manure",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Medium",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP095b","FP595b",null,{"$f":"VLOOKUP(Data!A59,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Domain previous land use"},{"$f":"VLOOKUP(Data!A59,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP096b","FP596b",null,{"$f":"VLOOKUP(Data!A60,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Ecological zone previous land use"},{"$f":"VLOOKUP(Data!A60,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP097b","FP597b",null,{"$f":"VLOOKUP(Data!A61,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Continent previous land use"},{"$f":"VLOOKUP(Data!A61,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP098b","FP598b",null,{"$f":"VLOOKUP(Data!A62,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type previous land use"},{"$f":"VLOOKUP(Data!A62,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP092a","FP592a",null,{"$f":"VLOOKUP(Data!A63,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Previously degraded land"},{"$f":"VLOOKUP(Data!A63,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP100","FP600",null,{"$f":"VLOOKUP(Data!A64,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Water use for feedstock production"},{"$f":"VLOOKUP(Data!A64,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"m³/ha"},22067.5,6858.8,37276.25,{"$f":"(H64-G64)/6","v":5069.5749999999998},"normal",22067.5,6858.8,37276.25,{"$f":"(M64-L64)/6","v":5069.5749999999998},"normal",null,null,null,null,null,0,0,0,{"$f":"(W64-V64)/6","v":0},"normal",2019.6,0,2500,{"$f":"(AB64-AA64)/6","v":416.66666666666669},"normal",0,0,0,{"$f":"(AG64-AF64)/6","v":0},"normal",null,null,null,{"$f":"(AL64-AK64)/6","v":0},"normal",null,null,null,{"$f":"(AQ64-AP64)/6","v":0},"normal",null,null,null,{"$f":"(AV64-AU64)/6","v":0},"normal",0,null,null,{"$f":"(BA64-AZ64)/6","v":0},"normal",null,null,null,{"$f":"(BF64-BE64)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE64-CD64)/6","v":0},"normal",0,null,null,{"$f":"(CJ64-CI64)/6","v":0},"normal",0,null,null,{"$f":"(CO64-CN64)/6","v":0},"normal",0,null,null,{"$f":"(CT64-CS64)/6","v":0},"normal"]
["FP103a","FP603a",null,{"$f":"VLOOKUP(Data!A65,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},{"$f":"VLOOKUP(Data!A65,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"m³/kgfm"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP109","FP609",null,{"$f":"VLOOKUP(Data!A66,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Input of N-fixing crop residue to the soil"},{"$f":"VLOOKUP(Data!A66,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/ha"},45,0,45,7.5,"normal",45,0,45,7.5,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,60,10,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP131","FP631",null,{"$f":"VLOOKUP(Data!A67,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Soil water saturation (yes=1,no=0)"},{"$f":"VLOOKUP(Data!A67,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP132","FP632",null,{"$f":"VLOOKUP(Data!A68,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Field renewal (annual crops = 1)"},{"$f":"VLOOKUP(Data!A68,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"years"},1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP133","FP633",null,{"$f":"VLOOKUP(Data!A69,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of crop residue returned to the field (only for palm)"},{"$f":"VLOOKUP(Data!A69,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgdm/kgfm"},0.22,0,0.5,{"$f":"(H69-G69)/6","v":8.3333333333333329E-2},"normal",0.22,0,0.5,{"$f":"(M69-L69)/6","v":8.3333333333333329E-2},"normal",null,null,null,null,null,0,0,0,{"$f":"(W69-V69)/6","v":0},"normal",0,0,0,{"$f":"(AB69-AA69)/6","v":0},"normal",0,0,0,{"$f":"(AG69-AF69)/6","v":0},"normal",null,null,null,{"$f":"(AL69-AK69)/6","v":0},"normal",null,null,null,{"$f":"(AQ69-AP69)/6","v":0},"normal",null,null,null,{"$f":"(AV69-AU69)/6","v":0},"normal",0,null,null,{"$f":"(BA69-AZ69)/6","v":0},"normal",null,null,null,{"$f":"(BF69-BE69)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE69-CD69)/6","v":0},"normal",0,null,null,{"$f":"(CJ69-CI69)/6","v":0},"normal",0,null,null,{"$f":"(CO69-CN69)/6","v":0},"normal",0,null,null,{"$f":"(CT69-CS69)/6","v":0},"normal"]
["FP134","FP634","FP136",{"$f":"VLOOKUP(Data!A70,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Organic soil (yes=1,no=0)"},{"$f":"VLOOKUP(Data!A70,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP135","FP635",null,{"$f":"VLOOKUP(Data!A71,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Nutrient level (only for ORGANIC soils + temperate/boreal climate + forest (native and managed))"},{"$f":"VLOOKUP(Data!A71,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FP141a","FP641a",null,{"$f":"VLOOKUP(Data!A72,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of animal manure N applied to soil (other than by grazing animals)"},{"$f":"VLOOKUP(Data!A72,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgN/ha"},0,0,185,{"$f":"(H72-G72)/6","v":30.833333333333332},"normal",0,0,185,{"$f":"(M72-L72)/6","v":30.833333333333332},"normal",null,null,null,null,null,0,0,0,{"$f":"(W72-V72)/6","v":0},"normal",185,0,250,{"$f":"(AB72-AA72)/6","v":41.666666666666664},"normal",0,0,0,{"$f":"(AG72-AF72)/6","v":0},"normal",null,null,null,{"$f":"(AL72-AK72)/6","v":0},"normal",null,null,null,{"$f":"(AQ72-AP72)/6","v":0},"normal",null,null,null,{"$f":"(AV72-AU72)/6","v":0},"normal",0,null,null,{"$f":"(BA72-AZ72)/6","v":0},"normal",null,null,null,{"$f":"(BF72-BE72)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE72-CD72)/6","v":0},"normal",0,null,null,{"$f":"(CJ72-CI72)/6","v":0},"normal",0,null,null,{"$f":"(CO72-CN72)/6","v":0},"normal",0,null,null,{"$f":"(CT72-CS72)/6","v":0},"normal"]
["FP141b","FP641b",null,{"$f":"VLOOKUP(Data!A73,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of total sewage N applied to soil"},{"$f":"VLOOKUP(Data!A73,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgN/ha"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP141c","FP641c",null,{"$f":"VLOOKUP(Data!A74,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of total compost N applied to soil"},{"$f":"VLOOKUP(Data!A74,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgN/ha"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP141d","FP641d",null,{"$f":"VLOOKUP(Data!A75,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of N of other organic amendments applied to soil (used as fertiliser)"},{"$f":"VLOOKUP(Data!A75,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgN/ha"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP149","FP649",null,{"$f":"VLOOKUP(Data!A76,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fraction of above-ground residues removed"},{"$f":"VLOOKUP(Data!A76,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,0,5,0.83333333333333337,"normal",0,0,5,0.83333333333333337,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,50,8.3333333333333339,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FP161","FP661",null,{"$f":"VLOOKUP(Data!A77,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land status in or after January 2008 = undisturbed forest (yes=1,no=0)"},{"$f":"VLOOKUP(Data!A77,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP162","FP662",null,{"$f":"VLOOKUP(Data!A78,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land status in or after January 2008 = nature protection area"},{"$f":"VLOOKUP(Data!A78,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP163","FP663",null,{"$f":"VLOOKUP(Data!A79,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land status in or after January 2008 = highly biodiverse grassland"},{"$f":"VLOOKUP(Data!A79,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP164","FP664",null,{"$f":"VLOOKUP(Data!A80,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land status in January 2008 and not longer now = wetland"},{"$f":"VLOOKUP(Data!A80,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP165","FP665",null,{"$f":"VLOOKUP(Data!A81,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land status in January 2008 and not longer now = continuously forested area"},{"$f":"VLOOKUP(Data!A81,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP166","FP666",null,{"$f":"VLOOKUP(Data!A82,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land status in January 2008 and not longer now = peatland"},{"$f":"VLOOKUP(Data!A82,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["FP170a","FP670a",null,{"$f":"VLOOKUP(Data!A83,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No forced labour"},{"$f":"VLOOKUP(Data!A83,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP170b","FP670b",null,{"$f":"VLOOKUP(Data!A84,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No child labour "},{"$f":"VLOOKUP(Data!A84,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP170c","FP670c",null,{"$f":"VLOOKUP(Data!A85,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Good social practices regarding human rights"},{"$f":"VLOOKUP(Data!A85,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP170d","FP670d",null,{"$f":"VLOOKUP(Data!A86,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No discrimination"},{"$f":"VLOOKUP(Data!A86,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP170e","FP670e",null,{"$f":"VLOOKUP(Data!A87,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Land is used legitimately / land rights have been secured"},{"$f":"VLOOKUP(Data!A87,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP170f","FP670f",null,{"$f":"VLOOKUP(Data!A88,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders"},{"$f":"VLOOKUP(Data!A88,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP170g","FP670g",null,{"$f":"VLOOKUP(Data!A89,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Food security"},{"$f":"VLOOKUP(Data!A89,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP171a","FP671a",null,{"$f":"VLOOKUP(Data!A90,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fair legal contracts"},{"$f":"VLOOKUP(Data!A90,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP171b","FP671b",null,{"$f":"VLOOKUP(Data!A91,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Workers rights"},{"$f":"VLOOKUP(Data!A91,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP171c","FP671c",null,{"$f":"VLOOKUP(Data!A92,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Freedom to join labour organizations or organize themselves"},{"$f":"VLOOKUP(Data!A92,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP171d","FP671d",null,{"$f":"VLOOKUP(Data!A93,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fair wages and compensation rules"},{"$f":"VLOOKUP(Data!A93,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP171e","FP671e",null,{"$f":"VLOOKUP(Data!A94,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Health, safety and hygiene policy"},{"$f":"VLOOKUP(Data!A94,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP171f","FP671f",null,{"$f":"VLOOKUP(Data!A95,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Risk assessment for safe and healthy working conditions"},{"$f":"VLOOKUP(Data!A95,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["FP171g","FP671g",null,{"$f":"VLOOKUP(Data!A96,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Health and safety training"},{"$f":"VLOOKUP(Data!A96,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
[]
["FT001a","FT501a",null,{"$f":"VLOOKUP(Data!A98,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 1"},{"$f":"VLOOKUP(Data!A98,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Truck for FFB transport (Diesel)",null,null,"n.a.","n.a.","Truck for FFB transport (Diesel)",null,null,"n.a.","n.a.",null,null,null,null,null,"Truck for dry product (diesel)",null,null,"n.a.","n.a.","Truck for dry product (diesel)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Truck for dry product (diesel)",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Truck for dry product (diesel)",null,null,"n.a.","n.a.","Truck for liquids (diesel)",null,null,"n.a.","n.a.","Truck for dry product (diesel)",null,null,"n.a.","n.a.","Truck for dry product (diesel)",null,null,"n.a.","n.a."]
["FT001b","FT501b",null,{"$f":"VLOOKUP(Data!A99,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 2"},{"$f":"VLOOKUP(Data!A99,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"Truck for dry product (diesel)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Truck for dry product (diesel)",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Truck for dry product (diesel)",null,null,"n.a.","n.a.","Truck for liquids (diesel)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Truck for dry product (diesel)",null,null,"n.a.","n.a."]
["FT001c","FT501c",null,{"$f":"VLOOKUP(Data!A100,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 3"},{"$f":"VLOOKUP(Data!A100,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Truck for dry product (diesel)",null,null,"n.a.","n.a.","Truck for liquids (diesel)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Truck for dry product (diesel)",null,null,"n.a.","n.a."]
["FT001d","FT501d",null,{"$f":"VLOOKUP(Data!A101,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 4"},{"$f":"VLOOKUP(Data!A101,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Truck for liquids (Diesel)",null,null,"n.a.","n.a.","Truck for liquids (Diesel)",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT001e","FT501e",null,{"$f":"VLOOKUP(Data!A102,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 5"},{"$f":"VLOOKUP(Data!A102,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Ship /product tanker 50kt (HFO maritime)",null,null,"n.a.","n.a.","Ship /product tanker 50kt (HFO maritime)",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT001f","FT501f",null,{"$f":"VLOOKUP(Data!A103,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 6"},{"$f":"VLOOKUP(Data!A103,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT001g","FT501g",null,{"$f":"VLOOKUP(Data!A104,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 7"},{"$f":"VLOOKUP(Data!A104,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Truck for liquids (Diesel)",null,null,"n.a.","n.a.","Truck for liquids (Diesel)",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT001h","FT501h",null,{"$f":"VLOOKUP(Data!A105,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 8"},{"$f":"VLOOKUP(Data!A105,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT001i","FT501i",null,{"$f":"VLOOKUP(Data!A106,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Transport mode 9"},{"$f":"VLOOKUP(Data!A106,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT003a","FT503a",null,{"$f":"VLOOKUP(Data!A107,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 1"},{"$f":"VLOOKUP(Data!A107,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},50,20,100,{"$f":"(H107-G107)/6","v":13.333333333333334},"normal",50,20,100,{"$f":"(M107-L107)/6","v":13.333333333333334},"normal",null,null,null,null,null,40,0,0,{"$f":"(W107-V107)/6","v":0},"normal",20,10,50,5,"normal",0,0,0,{"$f":"(AG107-AF107)/6","v":0},"normal",null,null,null,{"$f":"(AL107-AK107)/6","v":0},"normal",null,null,null,{"$f":"(AQ107-AP107)/6","v":0},"normal",null,null,null,{"$f":"(AV107-AU107)/6","v":0},"normal",40,null,null,{"$f":"(BA107-AZ107)/6","v":0},"normal",null,null,null,{"$f":"(BF107-BE107)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,null,null,{"$f":"(CE107-CD107)/6","v":0},"normal",40,null,null,{"$f":"(CJ107-CI107)/6","v":0},"normal",40,null,null,{"$f":"(CO107-CN107)/6","v":0},"normal",40,null,null,{"$f":"(CT107-CS107)/6","v":0},"normal"]
["FT003b","FT503b",null,{"$f":"VLOOKUP(Data!A108,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 2"},{"$f":"VLOOKUP(Data!A108,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,40,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",40,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,null,null,0,"normal",40,null,null,0,"normal",0,null,null,0,"normal",40,null,null,0,"normal"]
["FT003c","FT503c",null,{"$f":"VLOOKUP(Data!A109,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 3"},{"$f":"VLOOKUP(Data!A109,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,40,null,null,0,"normal",40,null,null,0,"normal",0,null,null,0,"normal",40,null,null,0,"normal"]
["FT003d","FT503d",null,{"$f":"VLOOKUP(Data!A110,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 4"},{"$f":"VLOOKUP(Data!A110,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},150,100,200,16.666666666666668,"normal",150,100,200,16.666666666666668,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FT003e","FT503e",null,{"$f":"VLOOKUP(Data!A111,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 5"},{"$f":"VLOOKUP(Data!A111,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},10186,10000,11000,166.66666666666666,"normal",10186,10000,11000,166.66666666666666,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FT003f","FT503f",null,{"$f":"VLOOKUP(Data!A112,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 6"},{"$f":"VLOOKUP(Data!A112,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FT003g","FT503g",null,{"$f":"VLOOKUP(Data!A113,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 7"},{"$f":"VLOOKUP(Data!A113,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},100,20,200,30,"normal",100,20,200,30,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FT003h","FT503h",null,{"$f":"VLOOKUP(Data!A114,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 8"},{"$f":"VLOOKUP(Data!A114,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FT003i","FT503i",null,{"$f":"VLOOKUP(Data!A115,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Distance of transport mode 9"},{"$f":"VLOOKUP(Data!A115,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"km"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["FT004a","FT504a",null,{"$f":"VLOOKUP(Data!A116,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 1"},{"$f":"VLOOKUP(Data!A116,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.",null,null,null,null,null,"Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a."]
["FT004b","FT504b",null,{"$f":"VLOOKUP(Data!A117,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 2"},{"$f":"VLOOKUP(Data!A117,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"Diesel",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a."]
["FT004c","FT504c",null,{"$f":"VLOOKUP(Data!A118,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 3"},{"$f":"VLOOKUP(Data!A118,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a."]
["FT004d","FT504d",null,{"$f":"VLOOKUP(Data!A119,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 4"},{"$f":"VLOOKUP(Data!A119,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT004e","FT504e",null,{"$f":"VLOOKUP(Data!A120,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 5"},{"$f":"VLOOKUP(Data!A120,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"HFO for maritime transport",null,null,"n.a.","n.a.","HFO for maritime transport",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT004f","FT504f",null,{"$f":"VLOOKUP(Data!A121,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 6"},{"$f":"VLOOKUP(Data!A121,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT004g","FT504g",null,{"$f":"VLOOKUP(Data!A122,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 7"},{"$f":"VLOOKUP(Data!A122,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Diesel",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT004h","FT504h",null,{"$f":"VLOOKUP(Data!A123,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 8"},{"$f":"VLOOKUP(Data!A123,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT004i","FT504i",null,{"$f":"VLOOKUP(Data!A124,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel used for transport mode 9"},{"$f":"VLOOKUP(Data!A124,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["FT025a","FT525a",null,"Source of additional GHG emissions",{"$f":"VLOOKUP(Data!A125,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJfossil/MJFU"},"Depot",null,null,"n.a.","n.a.","Depot",null,null,"n.a.","n.a.",null,null,null,null,null,"Depot",null,null,"n.a.","n.a.","Depot",null,null,"n.a.","n.a.","Depot",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Depot",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Depot",null,null,"n.a.","n.a.","Depot",null,null,"n.a.","n.a.","Depot",null,null,"n.a.","n.a.","Depot",null,null,"n.a.","n.a."]
["FT025b","FT525b",null,"Amount of additional GHG emissions",{"$f":"VLOOKUP(Data!A126,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJprim/MJFU"},0.2,0,0.5,{"$f":"(H126-G126)/6","v":8.3333333333333329E-2},"normal",0.2,0,0.5,{"$f":"(M126-L126)/6","v":8.3333333333333329E-2},"normal",null,null,null,null,null,0,null,null,{"$f":"(W126-V126)/6","v":0},"normal",0,null,null,0,"normal",0,null,null,{"$f":"(AG126-AF126)/6","v":0},"normal",null,null,null,{"$f":"(AL126-AK126)/6","v":0},"normal",null,null,null,{"$f":"(AQ126-AP126)/6","v":0},"normal",null,null,null,{"$f":"(AV126-AU126)/6","v":0},"normal",0,null,null,{"$f":"(BA126-AZ126)/6","v":0},"normal",null,null,null,{"$f":"(BF126-BE126)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE126-CD126)/6","v":0},"normal",0,null,null,{"$f":"(CJ126-CI126)/6","v":0},"normal",0,null,null,{"$f":"(CO126-CN126)/6","v":0},"normal",0,null,null,{"$f":"(CT126-CS126)/6","v":0},"normal"]
[]
["BC000a","BC500a",null,{"$f":"VLOOKUP(Data!A128,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Process 1 description "},{"$f":"VLOOKUP(Data!A128,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Oil extraction",null,null,"n.a.","n.a.","Oil extraction",null,null,"n.a.","n.a.",null,null,null,null,null,"Anaerobic digestion+post-composting",null,null,"n.a.","n.a.","Anaerobic digestion",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Anaerobic digestion+post-composting",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Anaerobic digestion",null,null,"n.a.","n.a.","Esterification",null,null,"n.a.","n.a.","Pyrolysis",null,null,"n.a.","n.a.","Anaerobic digestion+post-composting",null,null,"n.a.","n.a."]
["BC000b","BC500b",null,{"$f":"VLOOKUP(Data!A129,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Process 2 description "},{"$f":"VLOOKUP(Data!A129,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Refining",null,null,"n.a.","n.a.","Refining",null,null,"n.a.","n.a.",null,null,null,null,null,"Purification",null,null,"n.a.","n.a.","Purification",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Purification",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Purification",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Purification",null,null,"n.a.","n.a."]
["BC001a","BC501a",null,{"$f":"VLOOKUP(Data!A130,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of main output flow, process 1"},{"$f":"VLOOKUP(Data!A130,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Crude palm oil",null,null,"n.a.","n.a.","Crude palm oil",null,null,"n.a.","n.a.",null,null,null,null,null,"Biogas (55% CH4)",null,null,"n.a.","n.a.","Biogas (55% CH4)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Biogas (55% CH4)",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biogas (55% CH4)",null,null,"n.a.","n.a.","Biodiesel",null,null,"n.a.","n.a.","Fast pyrolysis bio-oil",null,null,"n.a.","n.a.","Biogas (55% CH4)",null,null,"n.a.","n.a."]
["BC001b","BC501b",null,{"$f":"VLOOKUP(Data!A131,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of main output flow, process 2"},{"$f":"VLOOKUP(Data!A131,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Palm stearin",null,null,"n.a.","n.a.","Palm olein",null,null,"n.a.","n.a.",null,null,null,null,null,"Purified biogas (55% CH4)",null,null,"n.a.","n.a.","Purified biogas (55% CH4)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Liquid biomethane (LBM)",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Liquid biomethane (LBM)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Liquid biomethane (LBM)",null,null,"n.a.","n.a."]
["BC012a","BC512a",null,{"$f":"VLOOKUP(Data!A132,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of main output flow, process 1"},{"$f":"VLOOKUP(Data!A132,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,0,0,{"$f":"(H132-G132)/6","v":0},"normal",0,0,0,{"$f":"(M132-L132)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W132-V132)/6","v":0},"normal",0,0,0,{"$f":"(AB132-AA132)/6","v":0},"normal",0,0,0,{"$f":"(AG132-AF132)/6","v":0},"normal",null,null,null,{"$f":"(AL132-AK132)/6","v":0},"normal",null,null,null,{"$f":"(AQ132-AP132)/6","v":0},"normal",null,null,null,{"$f":"(AV132-AU132)/6","v":0},"normal",0,null,null,{"$f":"(BA132-AZ132)/6","v":0},"normal",null,null,null,{"$f":"(BF132-BE132)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE132-CD132)/6","v":0},"normal",0,null,null,{"$f":"(CJ132-CI132)/6","v":0},"normal",0,null,null,{"$f":"(CO132-CN132)/6","v":0},"normal",0,null,null,{"$f":"(CT132-CS132)/6","v":0},"normal"]
["BC012b","BC512b",null,{"$f":"VLOOKUP(Data!A133,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of main output flow, process 2"},{"$f":"VLOOKUP(Data!A133,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC002a1","BC502a1",null,{"$f":"VLOOKUP(Data!A134,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of by-product 1, process 1"},{"$f":"VLOOKUP(Data!A134,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Palm kernel meal",null,null,"n.a.","n.a.","Palm kernel meal",null,null,"n.a.","n.a.",null,null,null,null,null,"Compost Breda - tunnel",null,null,"n.a.","n.a.","Digestate breda",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Compost Breda - tunnel",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Digestate moerdijk",null,null,"n.a.","n.a.","Glycerol",null,null,"n.a.","n.a.","Wood ash",null,null,"n.a.","n.a.","Compost Breda - tunnel",null,null,"n.a.","n.a."]
["BC002a10","BC502a10",null,{"$f":"VLOOKUP(Data!A135,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of by-product 1, process 1"},{"$f":"VLOOKUP(Data!A135,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},8.1999999999999993,null,null,null,null,8.1999999999999993,null,null,null,null,null,null,null,null,null,49.2,null,null,null,null,65.7,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,49.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,67.3,null,null,null,null,15,null,null,null,null,0,null,null,null,null,49.2]
["BC002a11","BC502a11",null,{"$f":"VLOOKUP(Data!A136,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"By-product flow 1, process 1"},{"$f":"VLOOKUP(Data!A136,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},462.83,null,null,"n.a.","n.a.",462.83,null,null,"n.a.","n.a.",null,null,null,null,null,17920000,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17920000,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,90274000,null,null,"n.a.","n.a.",1000000,null,null,"n.a.","n.a.",9012000,null,null,"n.a.","n.a.",17920000,null,null,"n.a.","n.a."]
["BC002a2","BC502a2",null,{"$f":"VLOOKUP(Data!A137,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of by-product 2, process 1"},{"$f":"VLOOKUP(Data!A137,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC002a20","BC502a20",null,{"$f":"VLOOKUP(Data!A138,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of by-product 2, process 1"},{"$f":"VLOOKUP(Data!A138,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002a21","BC502a21",null,{"$f":"VLOOKUP(Data!A139,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"By-product flow 2, process 1"},{"$f":"VLOOKUP(Data!A139,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002a3","BC502a3",null,{"$f":"VLOOKUP(Data!A140,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of by-product 3, process 1"},{"$f":"VLOOKUP(Data!A140,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a."]
["BC002a30","BC502a30",null,{"$f":"VLOOKUP(Data!A141,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of by-product 3, process 1"},{"$f":"VLOOKUP(Data!A141,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002a31","BC502a31",null,{"$f":"VLOOKUP(Data!A142,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"By-product flow 3, process 1"},{"$f":"VLOOKUP(Data!A142,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002a41","BC502a41",null,{"$f":"VLOOKUP(Data!A143,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity by-product, process 1"},{"$f":"VLOOKUP(Data!A143,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MWh/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,15108,null,null,null,null,0]
["BC002a51","BC502a51",null,{"$f":"VLOOKUP(Data!A144,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Heat by-product, process 1"},{"$f":"VLOOKUP(Data!A144,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,333719000,null,null,null,null,0]
["BC002b1","BC502b1",null,{"$f":"VLOOKUP(Data!A145,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of by-product 1, process 2"},{"$f":"VLOOKUP(Data!A145,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Palm olein",null,null,"n.a.","n.a.","Palm olein",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC002b10","BC502b10",null,{"$f":"VLOOKUP(Data!A146,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of by-product 1, process 2"},{"$f":"VLOOKUP(Data!A146,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002b11","BC502b11",null,{"$f":"VLOOKUP(Data!A147,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"By-product flow 1, process 2"},{"$f":"VLOOKUP(Data!A147,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002b2","BC502b2",null,{"$f":"VLOOKUP(Data!A148,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of by-product 2, process 2"},{"$f":"VLOOKUP(Data!A148,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC002b20","BC502b20",null,{"$f":"VLOOKUP(Data!A149,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of by-product 2, process 2"},{"$f":"VLOOKUP(Data!A149,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002b21","BC502b21",null,{"$f":"VLOOKUP(Data!A150,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"By-product flow 2, process 2"},{"$f":"VLOOKUP(Data!A150,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002b41","BC502b41",null,{"$f":"VLOOKUP(Data!A151,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity by-product, process 2"},{"$f":"VLOOKUP(Data!A151,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MWh/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC002b51","BC502b51",null,{"$f":"VLOOKUP(Data!A152,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Heat by-product, process 2"},{"$f":"VLOOKUP(Data!A152,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC003a1","BC503a1",null,{"$f":"VLOOKUP(Data!A153,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (kg)"},{"$f":"VLOOKUP(Data!A153,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgbyproduct /kginput"},{"$f":"IF(F136=\"n.a.\",0,F136/((F197+F198+F203+F207)+0.001))","v":2.4359472402133032E-2},null,null,"n.a.","n.a.",{"$f":"IF(K136=\"n.a.\",0,K136/((K197+K198+K203+K207)+0.001))","v":2.4359472402133032E-2},null,null,"n.a.","n.a.",null,null,null,null,null,{"$f":"IF(U136=\"n.a.\",0,U136/((U197+U198+U203+U207)+0.001))","v":0.55999999998250005},null,null,"n.a.","n.a.",{"$f":"IF(Z136=\"n.a.\",0,Z136/((Z197+Z198+Z203+Z207)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(AE136=\"n.a.\",0,AE136/((AE197+AE198+AE203+AE207)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",{"$f":"IF(AY136=\"n.a.\",0,AY136/((AY197+AY198+AY203+AY207)+0.001))","v":0.44799999998879997},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC136=\"n.a.\",0,CC136/((CC197+CC198+CC203+CC207)+0.001))","v":0.89815045118546077},null,null,"n.a.","n.a.",{"$f":"IF(CH136=\"n.a.\",0,CH136/((CH197+CH198+CH203+CH207)+0.001))","v":8.3724045538871056E-2},null,null,"n.a.","n.a.",{"$f":"IF(CM136=\"n.a.\",0,CM136/((CM197+CM198+CM203+CM207)+0.001))","v":0.11886672997627326},null,null,"n.a.","n.a.",{"$f":"IF(CR136=\"n.a.\",0,CR136/((CR197+CR198+CR203+CR207)+0.001))","v":0.44799999998879997},null,null,"n.a.","n.a."]
["BC003a2","BC503a2",null,{"$f":"VLOOKUP(Data!A154,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (kg)"},{"$f":"VLOOKUP(Data!A154,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgbyproduct /kginput"},{"$f":"IF(F139=\"n.a.\",0,F139/((F197+F198+F203+F207)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(K139=\"n.a.\",0,K139/((K197+K198+K203+K207)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,null,null,{"$f":"IF(U139=\"n.a.\",0,U139/((U197+U198+U203+U207)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(Z139=\"n.a.\",0,Z139/((Z197+Z198+Z203+Z207)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(AE139=\"n.a.\",0,AE139/((AE197+AE198+AE203+AE207)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",{"$f":"IF(AY139=\"n.a.\",0,AY139/((AY197+AY198+AY203+AY207)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC139=\"n.a.\",0,CC139/((CC197+CC198+CC203+CC207)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CH139=\"n.a.\",0,CH139/((CH197+CH198+CH203+CH207)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CM139=\"n.a.\",0,CM139/((CM197+CM198+CM203+CM207)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CR139=\"n.a.\",0,CR139/((CR197+CR198+CR203+CR207)+0.001))","v":0},null,null,"n.a.","n.a."]
["BC003a3","BC503a3",null,{"$f":"VLOOKUP(Data!A155,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (kg)"},{"$f":"VLOOKUP(Data!A155,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgbyproduct /kginput"},{"$f":"IF(F142=\"n.a.\",0,F142/((F197+F198+F203+F207)+0.001))","v":0},null,null,null,null,{"$f":"IF(K142=\"n.a.\",0,K142/((K197+K198+K203+K207)+0.001))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U142=\"n.a.\",0,U142/((U197+U198+U203+U207)+0.001))","v":0},null,null,null,null,{"$f":"IF(Z142=\"n.a.\",0,Z142/((Z197+Z198+Z203+Z207)+0.001))","v":0},null,null,null,null,{"$f":"IF(AE142=\"n.a.\",0,AE142/((AE197+AE198+AE203+AE207)+0.001))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY142=\"n.a.\",0,AY142/((AY197+AY198+AY203+AY207)+0.001))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC142=\"n.a.\",0,CC142/((CC197+CC198+CC203+CC207)+0.001))","v":0},null,null,null,null,{"$f":"IF(CH142=\"n.a.\",0,CH142/((CH197+CH198+CH203+CH207)+0.001))","v":0},null,null,null,null,{"$f":"IF(CM142=\"n.a.\",0,CM142/((CM197+CM198+CM203+CM207)+0.001))","v":0},null,null,null,null,{"$f":"IF(CR142=\"n.a.\",0,CR142/((CR197+CR198+CR203+CR207)+0.001))","v":0}]
["BC003b1","BC503b1",null,{"$f":"VLOOKUP(Data!A156,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (kg)"},{"$f":"VLOOKUP(Data!A156,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgbyproduct /kginput"},{"$f":"IF(F147=\"n.a.\",0,F147/((F212+F216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(K147=\"n.a.\",0,K147/((K212+K216)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,null,null,{"$f":"IF(U147=\"n.a.\",0,U147/((U212+U216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(Z147=\"n.a.\",0,Z147/((Z212+Z216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(AE147=\"n.a.\",0,AE147/((AE212+AE216)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",{"$f":"IF(AY147=\"n.a.\",0,AY147/((AY212+AY216)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC147=\"n.a.\",0,CC147/((CC212+CC216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CH147=\"0\",0,CH147/((CH212+CH216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CM147=\"0\",0,CM147/((CM212+CM216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CR147=\"0\",0,CR147/((CR212+CR216)+0.001))","v":0},null,null,"n.a.","n.a."]
["BC003b2","BC503b2",null,{"$f":"VLOOKUP(Data!A157,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (kg)"},{"$f":"VLOOKUP(Data!A157,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgbyproduct /kginput"},{"$f":"IF(F150=\"n.a.\",0,F150/((F212+F216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(K150=\"n.a.\",0,K150/((K212+K216)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,null,null,{"$f":"IF(U150=\"n.a.\",0,U150/((U212+U216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(Z150=\"n.a.\",0,Z150/((Z212+Z216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(AE150=\"n.a.\",0,AE150/((AE212+AE216)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",{"$f":"IF(AY150=\"n.a.\",0,AY150/((AY212+AY216)+0.001))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC150=\"n.a.\",0,CC150/((CC212+CC216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CH150=\"n.a.\",0,CH150/((CH212+CH216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CM150=\"n.a.\",0,CM150/((CM212+CM216)+0.001))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CR150=\"n.a.\",0,CR150/((CR212+CR216)+0.001))","v":0},null,null,"n.a.","n.a."]
["BC004a1","BC504a1",null,{"$f":"VLOOKUP(Data!A158,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (MJ)"},{"$f":"VLOOKUP(Data!A158,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F136*(1-F135/100)*F167)/((F197*(1-F19/100)*F41+F198*(1-F201/100)*F202+F203*(1-F205/100)*F206+F207*(1-F209/100)*F210)+0.001)","v":2.399961774322297E-2},1.7999999999999999E-2,2.1999999999999999E-2,{"$f":"(H158-G158)/6","v":6.6666666666666664E-4},"normal",{"$f":"(K136*(1-K135/100)*K167)/((K197*(1-K19/100)*K41+K198*(1-K201/100)*K202+K203*(1-K205/100)*K206+K207*(1-K209/100)*K210)+0.001)","v":2.399961774322297E-2},1.7999999999999999E-2,2.1999999999999999E-2,{"$f":"(M158-L158)/6","v":6.6666666666666664E-4},"normal",null,null,null,null,null,{"$f":"(U136*(1-U135/100)*U167)/((U197*(1-U19/100)*U41+U198*(1-U201/100)*U202+U203*(1-U205/100)*U206+U207*(1-U209/100)*U210)+0.001)","v":0.92010033002667724},0,0,{"$f":"(W158-V158)/6","v":0},"normal",{"$f":"(Z136*(1-Z135/100)*Z167)/((Z197*(1-Z19/100)*Z41+Z198*(1-Z201/100)*Z202+Z203*(1-Z205/100)*Z206+Z207*(1-Z209/100)*Z210)+0.001)","v":0},0,0,{"$f":"(AB158-AA158)/6","v":0},"normal",{"$f":"(AE136*(1-AE135/100)*AE167)/((AE197*(1-AE19/100)*AE41+AE198*(1-AE201/100)*AE202+AE203*(1-AE205/100)*AE206+AE207*(1-AE209/100)*AE210)+0.001)","v":0},0,0,{"$f":"(AG158-AF158)/6","v":0},"normal",null,null,null,{"$f":"(AL158-AK158)/6","v":0},"normal",null,null,null,{"$f":"(AQ158-AP158)/6","v":0},"normal",null,null,null,{"$f":"(AV158-AU158)/6","v":0},"normal",{"$f":"(AY136*(1-AY135/100)*AY167)/((AY197*(1-AY19/100)*AY41+AY198*(1-AY201/100)*AY202+AY203*(1-AY205/100)*AY206+AY207*(1-AY209/100)*AY210)+0.001)","v":0.79669575156698502},null,null,{"$f":"(BA158-AZ158)/6","v":0},"normal",null,null,null,{"$f":"(BF158-BE158)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC136*(1-CC135/100)*CC167)/((CC197*(1-CC19/100)*CC41+CC198*(1-CC201/100)*CC202+CC203*(1-CC205/100)*CC206+CC207*(1-CC209/100)*CC210)+0.001)","v":0.62030416885341033},null,null,{"$f":"(CE158-CD158)/6","v":0},"normal",{"$f":"(CH136*(1-CH135/100)*CH167)/((CH197*(1-CH19/100)*CH41+CH198*(1-CH201/100)*CH202+CH203*(1-CH205/100)*CH206+CH207*(1-CH209/100)*CH210)+0.001)","v":4.4351081070500897E-2},null,null,{"$f":"(CJ158-CI158)/6","v":0},"normal",{"$f":"(CM136*(1-CM135/100)*CM167)/((CM197*(1-CM19/100)*CM41+CM198*(1-CM201/100)*CM202+CM203*(1-CM205/100)*CM206+CM207*(1-CM209/100)*CM210)+0.001)","v":0.14268117583571391},null,null,{"$f":"(CO158-CN158)/6","v":0},"normal",{"$f":"(CR136*(1-CR135/100)*CR167)/((CR197*(1-CR19/100)*CR41+CR198*(1-CR201/100)*CR202+CR203*(1-CR205/100)*CR206+CR207*(1-CR209/100)*CR210)+0.001)","v":0.79669575156698502},null,null,{"$f":"(CT158-CS158)/6","v":0},"normal"]
["BC004a2","BC504a2",null,{"$f":"VLOOKUP(Data!A159,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (MJ)"},{"$f":"VLOOKUP(Data!A159,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F139*(1-F138/100)*F168)/((F197*(1-F19/100)*F41+F198*(1-F201/100)*F202+F203*(1-F205/100)*F206+F207*(1-F209/100)*F210)+0.001)","v":0},0,0,0,"normal",{"$f":"(K139*(1-K138/100)*K168)/((K197*(1-K19/100)*K41+K198*(1-K201/100)*K202+K203*(1-K205/100)*K206+K207*(1-K209/100)*K210)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"(U139*(1-U138/100)*U168)/((U197*(1-U19/100)*U41+U198*(1-U201/100)*U202+U203*(1-U205/100)*U206+U207*(1-U209/100)*U210)+0.001)","v":0},0,0,0,"normal",{"$f":"(Z139*(1-Z138/100)*Z168)/((Z197*(1-Z19/100)*Z41+Z198*(1-Z201/100)*Z202+Z203*(1-Z205/100)*Z206+Z207*(1-Z209/100)*Z210)+0.001)","v":0},0,0,0,"normal",{"$f":"(AE139*(1-AE138/100)*AE168)/((AE197*(1-AE19/100)*AE41+AE198*(1-AE201/100)*AE202+AE203*(1-AE205/100)*AE206+AE207*(1-AE209/100)*AE210)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"(AY139*(1-AY138/100)*AY168)/((AY197*(1-AY19/100)*AY41+AY198*(1-AY201/100)*AY202+AY203*(1-AY205/100)*AY206+AY207*(1-AY209/100)*AY210)+0.001)","v":0},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC139*(1-CC138/100)*CC168)/((CC197*(1-CC19/100)*CC41+CC198*(1-CC201/100)*CC202+CC203*(1-CC205/100)*CC206+CC207*(1-CC209/100)*CC210)+0.001)","v":0},null,null,0,"normal",{"$f":"(CH139*(1-CH138/100)*CH168)/((CH197*(1-CH19/100)*CH41+CH198*(1-CH201/100)*CH202+CH203*(1-CH205/100)*CH206+CH207*(1-CH209/100)*CH210)+0.001)","v":0},null,null,0,"normal",{"$f":"(CM139*(1-CM138/100)*CM168)/((CM197*(1-CM19/100)*CM41+CM198*(1-CM201/100)*CM202+CM203*(1-CM205/100)*CM206+CM207*(1-CM209/100)*CM210)+0.001)","v":0},null,null,0,"normal",{"$f":"(CR139*(1-CR138/100)*CR168)/((CR197*(1-CR19/100)*CR41+CR198*(1-CR201/100)*CR202+CR203*(1-CR205/100)*CR206+CR207*(1-CR209/100)*CR210)+0.001)","v":0},null,null,0,"normal"]
["BC004a3","BC504a3",null,{"$f":"VLOOKUP(Data!A160,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (MJ)"},{"$f":"VLOOKUP(Data!A160,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F142*(1-F141/100)*F169)/((F197*(1-F19/100)*F41+F198*(1-F201/100)*F202+F203*(1-F205/100)*F206+F207*(1-F209/100)*F210)+0.001)","v":0},0,0,0,"normal",{"$f":"(K142*(1-K141/100)*K169)/((K197*(1-K19/100)*K41+K198*(1-K201/100)*K202+K203*(1-K205/100)*K206+K207*(1-K209/100)*K210)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"(U142*(1-U141/100)*U169)/((U197*(1-U19/100)*U41+U198*(1-U201/100)*U202+U203*(1-U205/100)*U206+U207*(1-U209/100)*U210)+0.001)","v":0},0,0,0,"normal",{"$f":"(Z142*(1-Z141/100)*Z169)/((Z197*(1-Z19/100)*Z41+Z198*(1-Z201/100)*Z202+Z203*(1-Z205/100)*Z206+Z207*(1-Z209/100)*Z210)+0.001)","v":0},0,0,0,"normal",{"$f":"(AE142*(1-AE141/100)*AE169)/((AE197*(1-AE19/100)*AE41+AE198*(1-AE201/100)*AE202+AE203*(1-AE205/100)*AE206+AE207*(1-AE209/100)*AE210)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"(AY142*(1-AY141/100)*AY169)/((AY197*(1-AY19/100)*AY41+AY198*(1-AY201/100)*AY202+AY203*(1-AY205/100)*AY206+AY207*(1-AY209/100)*AY210)+0.001)","v":0},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC142*(1-CC141/100)*CC169)/((CC197*(1-CC19/100)*CC41+CC198*(1-CC201/100)*CC202+CC203*(1-CC205/100)*CC206+CC207*(1-CC209/100)*CC210)+0.001)","v":0},null,null,0,"normal",{"$f":"(CH142*(1-CH141/100)*CH169)/((CH197*(1-CH19/100)*CH41+CH198*(1-CH201/100)*CH202+CH203*(1-CH205/100)*CH206+CH207*(1-CH209/100)*CH210)+0.001)","v":0},null,null,0,"normal",{"$f":"(CM142*(1-CM141/100)*CM169)/((CM197*(1-CM19/100)*CM41+CM198*(1-CM201/100)*CM202+CM203*(1-CM205/100)*CM206+CM207*(1-CM209/100)*CM210)+0.001)","v":0},null,null,0,"normal",{"$f":"(CR142*(1-CR141/100)*CR169)/((CR197*(1-CR19/100)*CR41+CR198*(1-CR201/100)*CR202+CR203*(1-CR205/100)*CR206+CR207*(1-CR209/100)*CR210)+0.001)","v":0},null,null,0,"normal"]
["BC004a4","BC504a4",null,{"$f":"VLOOKUP(Data!A161,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of electricity by-product, process 1 (MJ)"},{"$f":"VLOOKUP(Data!A161,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F143*3600)/((F197*(1-F19/100)*F41+F198*(1-F201/100)*F202+F203*(1-F205/100)*F206+F207*(1-F209/100)*F210)+0.001)","v":0},0,0,{"$f":"(H161-G161)/6","v":0},"normal",{"$f":"(K143*3600)/((K197*(1-K19/100)*K41+K198*(1-K201/100)*K202+K203*(1-K205/100)*K206+K207*(1-K209/100)*K210)+0.001)","v":0},0,0,{"$f":"(M161-L161)/6","v":0},"normal",null,null,null,null,null,{"$f":"(U143*3600)/((U197*(1-U19/100)*U41+U198*(1-U201/100)*U202+U203*(1-U205/100)*U206+U207*(1-U209/100)*U210)+0.001)","v":0},0,0,{"$f":"(W161-V161)/6","v":0},"normal",{"$f":"(Z143*3600)/((Z197*(1-Z19/100)*Z41+Z198*(1-Z201/100)*Z202+Z203*(1-Z205/100)*Z206+Z207*(1-Z209/100)*Z210)+0.001)","v":0},0,0,{"$f":"(AB161-AA161)/6","v":0},"normal",{"$f":"(AE143*3600)/((AE197*(1-AE19/100)*AE41+AE198*(1-AE201/100)*AE202+AE203*(1-AE205/100)*AE206+AE207*(1-AE209/100)*AE210)+0.001)","v":0},0,0,{"$f":"(AG161-AF161)/6","v":0},"normal",null,null,null,{"$f":"(AL161-AK161)/6","v":0},"normal",null,null,null,{"$f":"(AQ161-AP161)/6","v":0},"normal",null,null,null,{"$f":"(AV161-AU161)/6","v":0},"normal",{"$f":"(AY143*3600)/((AY197*(1-AY19/100)*AY41+AY198*(1-AY201/100)*AY202+AY203*(1-AY205/100)*AY206+AY207*(1-AY209/100)*AY210)+0.001)","v":0},null,null,{"$f":"(BA161-AZ161)/6","v":0},"normal",null,null,null,{"$f":"(BF161-BE161)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC143*3600)/((CC197*(1-CC19/100)*CC41+CC198*(1-CC201/100)*CC202+CC203*(1-CC205/100)*CC206+CC207*(1-CC209/100)*CC210)+0.001)","v":0},null,null,{"$f":"(CE161-CD161)/6","v":0},"normal",{"$f":"(CH143*3600)/((CH197*(1-CH19/100)*CH41+CH198*(1-CH201/100)*CH202+CH203*(1-CH205/100)*CH206+CH207*(1-CH209/100)*CH210)+0.001)","v":0},null,null,{"$f":"(CJ161-CI161)/6","v":0},"normal",{"$f":"(CM143*3600)/((CM197*(1-CM19/100)*CM41+CM198*(1-CM201/100)*CM202+CM203*(1-CM205/100)*CM206+CM207*(1-CM209/100)*CM210)+0.001)","v":4.8322264018927974E-2},null,null,{"$f":"(CO161-CN161)/6","v":0},"normal",{"$f":"(CR143*3600)/((CR197*(1-CR19/100)*CR41+CR198*(1-CR201/100)*CR202+CR203*(1-CR205/100)*CR206+CR207*(1-CR209/100)*CR210)+0.001)","v":0},null,null,{"$f":"(CT161-CS161)/6","v":0},"normal"]
["BC004a5","BC504a5",null,{"$f":"VLOOKUP(Data!A162,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of heat by-product, process 1 (MJ)"},{"$f":"VLOOKUP(Data!A162,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F144)/((F197*(1-F19/100)*F41+F198*(1-F201/100)*F202+F203*(1-F205/100)*F206+F207*(1-F209/100)*F210)+0.001)","v":0},0,0,0,"normal",{"$f":"(K144)/((K197*(1-K19/100)*K41+K198*(1-K201/100)*K202+K203*(1-K205/100)*K206+K207*(1-K209/100)*K210)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"(U144)/((U197*(1-U19/100)*U41+U198*(1-U201/100)*U202+U203*(1-U205/100)*U206+U207*(1-U209/100)*U210)+0.001)","v":0},0,0,0,"normal",{"$f":"(Z144)/((Z197*(1-Z19/100)*Z41+Z198*(1-Z201/100)*Z202+Z203*(1-Z205/100)*Z206+Z207*(1-Z209/100)*Z210)+0.001)","v":0},0,0,0,"normal",{"$f":"(AE144)/((AE197*(1-AE19/100)*AE41+AE198*(1-AE201/100)*AE202+AE203*(1-AE205/100)*AE206+AE207*(1-AE209/100)*AE210)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"(AY144)/((AY197*(1-AY19/100)*AY41+AY198*(1-AY201/100)*AY202+AY203*(1-AY205/100)*AY206+AY207*(1-AY209/100)*AY210)+0.001)","v":0},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC144)/((CC197*(1-CC19/100)*CC41+CC198*(1-CC201/100)*CC202+CC203*(1-CC205/100)*CC206+CC207*(1-CC209/100)*CC210)+0.001)","v":0},null,null,0,"normal",{"$f":"(CH144)/((CH197*(1-CH19/100)*CH41+CH198*(1-CH201/100)*CH202+CH203*(1-CH205/100)*CH206+CH207*(1-CH209/100)*CH210)+0.001)","v":0},null,null,0,"normal",{"$f":"(CM144)/((CM197*(1-CM19/100)*CM41+CM198*(1-CM201/100)*CM202+CM203*(1-CM205/100)*CM206+CM207*(1-CM209/100)*CM210)+0.001)","v":0.29649592611222575},null,null,0,"normal",{"$f":"(CR144)/((CR197*(1-CR19/100)*CR41+CR198*(1-CR201/100)*CR202+CR203*(1-CR205/100)*CR206+CR207*(1-CR209/100)*CR210)+0.001)","v":0},null,null,0,"normal"]
["BC004b1","BC504b1",null,{"$f":"VLOOKUP(Data!A163,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (MJ)"},{"$f":"VLOOKUP(Data!A163,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F147*(1-F146/100)*F170)/((F212*(1-F213/100)*F214+F216*(1-F217/100)*F218)+0.001)","v":0},0.6,0.7,1.6666666666666663E-2,"normal",{"$f":"(K147*(1-K146/100)*K170)/((K212*(1-K213/100)*K214+K216*(1-K217/100)*K218)+0.001)","v":0},0.6,0.7,1.6666666666666663E-2,"normal",null,null,null,null,null,{"$f":"(U147*(1-U146/100)*U170)/((U212*(1-U213/100)*U214+U216*(1-U217/100)*U218)+0.001)","v":0},0,0,0,"normal",{"$f":"(Z147*(1-Z146/100)*Z170)/((Z212*(1-Z213/100)*Z214+Z216*(1-Z217/100)*Z218)+0.001)","v":0},0,0,0,"normal",{"$f":"(AE147*(1-AE146/100)*AE170)/((AE212*(1-AE213/100)*AE214+AE216*(1-AE217/100)*AE218)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"(AY147*(1-AY146/100)*AY170)/((AY212*(1-AY213/100)*AY214+AY216*(1-AY217/100)*AY218)+0.001)","v":0},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC147*(1-CC146/100)*CC170)/((CC212*(1-CC213/100)*CC214+CC216*(1-CC217/100)*CC218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CH147*(1-CH146/100)*CH170)/((CH212*(1-CH213/100)*CH214+CH216*(1-CH217/100)*CH218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CM147*(1-CM146/100)*CM170)/((CM212*(1-CM213/100)*CM214+CM216*(1-CM217/100)*CM218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CR147*(1-CR146/100)*CR170)/((CR212*(1-CR213/100)*CR214+CR216*(1-CR217/100)*CR218)+0.001)","v":0},null,null,{"$f":"(CT163-CS163)/6","v":0},"normal"]
["BC004b2","BC504b2",null,{"$f":"VLOOKUP(Data!A164,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (MJ)"},{"$f":"VLOOKUP(Data!A164,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F150*(1-F149/100)*F171)/((F212*(1-F213/100)*F214+F216*(1-F217/100)*F218)+0.001)","v":0},0,0,0,"normal",{"$f":"(K150*(1-K149/100)*K171)/((K212*(1-K213/100)*K214+K216*(1-K217/100)*K218)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"(U150*(1-U149/100)*U171)/((U212*(1-U213/100)*U214+U216*(1-U217/100)*U218)+0.001)","v":0},0,0,0,"normal",{"$f":"(Z150*(1-Z149/100)*Z171)/((Z212*(1-Z213/100)*Z214+Z216*(1-Z217/100)*Z218)+0.001)","v":0},0,0,0,"normal",{"$f":"(AE150*(1-AE149/100)*AE171)/((AE212*(1-AE213/100)*AE214+AE216*(1-AE217/100)*AE218)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"(AY150*(1-AY149/100)*AY171)/((AY212*(1-AY213/100)*AY214+AY216*(1-AY217/100)*AY218)+0.001)","v":0},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC150*(1-CC149/100)*CC171)/((CC212*(1-CC213/100)*CC214+CC216*(1-CC217/100)*CC218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CH150*(1-CH149/100)*CH171)/((CH212*(1-CH213/100)*CH214+CH216*(1-CH217/100)*CH218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CM150*(1-CM149/100)*CM171)/((CM212*(1-CM213/100)*CM214+CM216*(1-CM217/100)*CM218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CR150*(1-CR149/100)*CR171)/((CR212*(1-CR213/100)*CR214+CR216*(1-CR217/100)*CR218)+0.001)","v":0},null,null,0,"normal"]
["BC004b4","BC504b4",null,{"$f":"VLOOKUP(Data!A165,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of electricity by-product, process 2 (MJ)"},{"$f":"VLOOKUP(Data!A165,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F151*3600)/((F212*(1-F213/100)*F214+F216*(1-F217/100)*F218)+0.001)","v":0},0,0,0,"normal",{"$f":"(K151*3600)/((K212*(1-K213/100)*K214+K216*(1-K217/100)*K218)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"(U151*3600)/((U212*(1-U213/100)*U214+U216*(1-U217/100)*U218)+0.001)","v":0},0,0,{"$f":"(W165-V165)/6","v":0},"normal",{"$f":"(Z151*3600)/((Z212*(1-Z213/100)*Z214+Z216*(1-Z217/100)*Z218)+0.001)","v":0},0,0,{"$f":"(AB165-AA165)/6","v":0},"normal",{"$f":"(AE151*3600)/((AE212*(1-AE213/100)*AE214+AE216*(1-AE217/100)*AE218)+0.001)","v":0},0,0,{"$f":"(AG165-AF165)/6","v":0},"normal",null,null,null,{"$f":"(AL165-AK165)/6","v":0},"normal",null,null,null,{"$f":"(AQ165-AP165)/6","v":0},"normal",null,null,null,{"$f":"(AV165-AU165)/6","v":0},"normal",{"$f":"(AY151*3600)/((AY212*(1-AY213/100)*AY214+AY216*(1-AY217/100)*AY218)+0.001)","v":0},null,null,{"$f":"(BA165-AZ165)/6","v":0},"normal",null,null,null,{"$f":"(BF165-BE165)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC151*3600)/((CC212*(1-CC213/100)*CC214+CC216*(1-CC217/100)*CC218)+0.001)","v":0},null,null,{"$f":"(CE165-CD165)/6","v":0},"normal",{"$f":"(CH151*3600)/((CH212*(1-CH213/100)*CH214+CH216*(1-CH217/100)*CH218)+0.001)","v":0},null,null,{"$f":"(CJ165-CI165)/6","v":0},"normal",{"$f":"(CM151*3600)/((CM212*(1-CM213/100)*CM214+CM216*(1-CM217/100)*CM218)+0.001)","v":0},null,null,{"$f":"(CO165-CN165)/6","v":0},"normal",{"$f":"(CR151*3600)/((CR212*(1-CR213/100)*CR214+CR216*(1-CR217/100)*CR218)+0.001)","v":0},null,null,{"$f":"(CT165-CS165)/6","v":0},"normal"]
["BC004b5","BC504b5",null,{"$f":"VLOOKUP(Data!A166,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate of heat by-product, process 2 (MJ)"},{"$f":"VLOOKUP(Data!A166,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJbyproduct /MJinput"},{"$f":"(F152)/((F212*(1-F213/100)*F214+F216*(1-F217/100)*F218)+0.001)","v":0},0,0,{"$f":"(H166-G166)/6","v":0},"normal",{"$f":"(K152)/((K212*(1-K213/100)*K214+K216*(1-K217/100)*K218)+0.001)","v":0},0,0,{"$f":"(M166-L166)/6","v":0},"normal",null,null,null,null,null,{"$f":"(U152)/((U212*(1-U213/100)*U214+U216*(1-U217/100)*U218)+0.001)","v":0},0,0,0,"normal",{"$f":"(Z152)/((Z212*(1-Z213/100)*Z214+Z216*(1-Z217/100)*Z218)+0.001)","v":0},0,0,0,"normal",{"$f":"(AE152)/((AE212*(1-AE213/100)*AE214+AE216*(1-AE217/100)*AE218)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"(AY152)/((AY212*(1-AY213/100)*AY214+AY216*(1-AY217/100)*AY218)+0.001)","v":0},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC152)/((CC212*(1-CC213/100)*CC214+CC216*(1-CC217/100)*CC218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CH152)/((CH212*(1-CH213/100)*CH214+CH216*(1-CH217/100)*CH218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CM152)/((CM212*(1-CM213/100)*CM214+CM216*(1-CM217/100)*CM218)+0.001)","v":0},null,null,0,"normal",{"$f":"(CR152)/((CR212*(1-CR213/100)*CR214+CR216*(1-CR217/100)*CR218)+0.001)","v":0},null,null,0,"normal"]
["BC005a1","BC505a1",null,{"$f":"VLOOKUP(Data!A167,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of by-product 1, process 1 (LHV)"},{"$f":"VLOOKUP(Data!A167,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F134=\"n.a.\",0,VLOOKUP(F134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":17},null,null,null,null,{"$f":"IF(K134=\"n.a.\",0,VLOOKUP(K134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":17},null,null,null,null,null,null,null,null,null,{"$f":"IF(U134=\"n.a.\",0,VLOOKUP(U134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":14.7},null,null,null,null,{"$f":"IF(Z134=\"n.a.\",0,VLOOKUP(Z134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":8.5500000000000007},null,null,null,null,{"$f":"IF(AE134=\"n.a.\",0,VLOOKUP(AE134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY134=\"n.a.\",0,VLOOKUP(AY134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":14.7},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC134=\"n.a.\",0,VLOOKUP(CC134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":12.6},null,null,null,null,{"$f":"IF(CH134=\"n.a.\",0,VLOOKUP(CH134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":16},null,null,null,null,{"$f":"IF(CM134=\"n.a.\",0,VLOOKUP(CM134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":17.82},null,null,null,null,{"$f":"IF(CR134=\"n.a.\",0,VLOOKUP(CR134,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":14.7}]
["BC005a2","BC505a2",null,{"$f":"VLOOKUP(Data!A168,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of by-product 2, process 1 (LHV)"},{"$f":"VLOOKUP(Data!A168,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F137=\"n.a.\",0,VLOOKUP(F137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(K137=\"n.a.\",0,VLOOKUP(K137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U137=\"n.a.\",0,VLOOKUP(U137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z137=\"n.a.\",0,VLOOKUP(Z137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(AE137=\"n.a.\",0,VLOOKUP(AE137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY137=\"n.a.\",0,VLOOKUP(AY137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC137=\"n.a.\",0,VLOOKUP(CC137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CH137=\"n.a.\",0,VLOOKUP(CH137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CM137=\"n.a.\",0,VLOOKUP(CM137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CR137=\"n.a.\",0,VLOOKUP(CR137,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0}]
["BC005a3","BC505a3",null,{"$f":"VLOOKUP(Data!A169,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of by-product 3, process 1 (LHV)"},{"$f":"VLOOKUP(Data!A169,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F140=\"n.a.\",0,VLOOKUP(F140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(K140=\"n.a.\",0,VLOOKUP(K140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U140=\"n.a.\",0,VLOOKUP(U140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z140=\"n.a.\",0,VLOOKUP(Z140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(AE140=\"n.a.\",0,VLOOKUP(AE140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY140=\"n.a.\",0,VLOOKUP(AY140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC140=\"n.a.\",0,VLOOKUP(CC140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CH140=\"n.a.\",0,VLOOKUP(CH140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CM140=\"n.a.\",0,VLOOKUP(CM140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CR140=\"n.a.\",0,VLOOKUP(CR140,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0}]
["BC005b1","BC505b1",null,{"$f":"VLOOKUP(Data!A170,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of by-product 1, process 2 (LHV)"},{"$f":"VLOOKUP(Data!A170,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F145=\"n.a.\",0,VLOOKUP(F145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},null,null,null,null,{"$f":"IF(K145=\"n.a.\",0,VLOOKUP(K145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},null,null,null,null,null,null,null,null,null,{"$f":"IF(U145=\"n.a.\",0,VLOOKUP(U145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z145=\"n.a.\",0,VLOOKUP(Z145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(AE145=\"n.a.\",0,VLOOKUP(AE145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY145=\"n.a.\",0,VLOOKUP(AY145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC145=\"n.a.\",0,VLOOKUP(CC145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CH145=\"n.a.\",0,VLOOKUP(CH145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CM145=\"n.a.\",0,VLOOKUP(CM145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CR145=\"n.a.\",0,VLOOKUP(CR145,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0}]
["BC005b2","BC505b2",null,{"$f":"VLOOKUP(Data!A171,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of by-product 2, process 2 (LHV)"},{"$f":"VLOOKUP(Data!A171,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F148=\"n.a.\",0,VLOOKUP(F148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(K148=\"n.a.\",0,VLOOKUP(K148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U148=\"n.a.\",0,VLOOKUP(U148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z148=\"n.a.\",0,VLOOKUP(Z148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(AE148=\"n.a.\",0,VLOOKUP(AE148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY148=\"n.a.\",0,VLOOKUP(AY148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC148=\"n.a.\",0,VLOOKUP(CC148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CH148=\"n.a.\",0,VLOOKUP(CH148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CM148=\"n.a.\",0,VLOOKUP(CM148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CR148=\"n.a.\",0,VLOOKUP(CR148,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0}]
["BC006a1","BC506a1",null,{"$f":"VLOOKUP(Data!A172,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of by-product 1, process 1"},{"$f":"VLOOKUP(Data!A172,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,null,null,1,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a."]
["BC006a2","BC506a2",null,{"$f":"VLOOKUP(Data!A173,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of by-product 2, process 1"},{"$f":"VLOOKUP(Data!A173,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["BC006a3","BC506a3",null,{"$f":"VLOOKUP(Data!A174,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of by-product 3, process 1"},{"$f":"VLOOKUP(Data!A174,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["BC006a4","BC506a4",null,{"$f":"VLOOKUP(Data!A175,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of electricity by-product, process 1"},"binary",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["BC006a5","BC506a5",null,{"$f":"VLOOKUP(Data!A176,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of heat by-product, process 1"},"binary",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["BC006b1","BC506b1",null,{"$f":"VLOOKUP(Data!A177,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of by-product 1, process 2"},{"$f":"VLOOKUP(Data!A177,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},1,null,null,"n.a.","n.a.",1,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["BC006b2","BC506b2",null,{"$f":"VLOOKUP(Data!A178,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of by-product 2, process 2"},{"$f":"VLOOKUP(Data!A178,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"binary"},0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["BC006b4","BC506b4",null,{"$f":"VLOOKUP(Data!A179,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of electricity by-product, process 2"},"binary",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["BC006b5","BC506b5",null,{"$f":"VLOOKUP(Data!A180,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Valorisation of heat by-product, process 2"},"binary",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a."]
["BC007a","BC507a",null,{"$f":"VLOOKUP(Data!A181,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of main output flow, process 1 (LHV)"},{"$f":"VLOOKUP(Data!A181,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F130=\"n.a.\",0,VLOOKUP(F130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},null,null,"n.a.","n.a.",{"$f":"IF(K130=\"n.a.\",0,VLOOKUP(K130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},null,null,"n.a.","n.a.",null,null,null,null,null,{"$f":"IF(U130=\"n.a.\",0,VLOOKUP(U130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":27.5},null,null,"n.a.","n.a.",{"$f":"IF(Z130=\"n.a.\",0,VLOOKUP(Z130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":27.5},null,null,"n.a.","n.a.",{"$f":"IF(AE130=\"n.a.\",0,VLOOKUP(AE130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",{"$f":"IF(AY130=\"n.a.\",0,VLOOKUP(AY130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":27.5},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC130=\"n.a.\",0,VLOOKUP(CC130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":27.5},null,null,"n.a.","n.a.",{"$f":"IF(CH130=\"n.a.\",0,VLOOKUP(CH130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":24.67},null,null,"n.a.","n.a.",{"$f":"IF(CM130=\"n.a.\",0,VLOOKUP(CM130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":21.15},null,null,"n.a.","n.a.",{"$f":"IF(CR130=\"n.a.\",0,VLOOKUP(CR130,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":27.5},null,null,"n.a.","n.a."]
["BC007b","BC507b",null,{"$f":"VLOOKUP(Data!A182,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of main output flow, process 2 (LHV)"},{"$f":"VLOOKUP(Data!A182,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F131=\"n.a.\",0,VLOOKUP(F131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},null,null,"n.a.","n.a.",{"$f":"IF(K131=\"n.a.\",0,VLOOKUP(K131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},null,null,"n.a.","n.a.",null,null,null,null,null,{"$f":"IF(U131=\"n.a.\",0,VLOOKUP(U131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":27.5},null,null,"n.a.","n.a.",{"$f":"IF(Z131=\"n.a.\",0,VLOOKUP(Z131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":27.5},null,null,"n.a.","n.a.",{"$f":"IF(AE131=\"n.a.\",0,VLOOKUP(AE131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",{"$f":"IF(AY131=\"n.a.\",0,VLOOKUP(AY131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":50},null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC131=\"n.a.\",0,VLOOKUP(CC131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":50},null,null,"n.a.","n.a.",{"$f":"IF(CH131=\"n.a.\",0,VLOOKUP(CH131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CM131=\"n.a.\",0,VLOOKUP(CM131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,"n.a.","n.a.",{"$f":"IF(CR131=\"n.a.\",0,VLOOKUP(CR131,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":50},null,null,"n.a.","n.a."]
["BC008a","BC508a",null,{"$f":"VLOOKUP(Data!A183,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate (output/input), process 1"},{"$f":"VLOOKUP(Data!A183,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJoutput /MJinput"},{"$f":"(F220*F181)/(((F197*(1-F19/100)*F41+F198*(1-F201/100)*F202+F203*(1-F205/100)*F206+F207*(1-F209/100)*F210))+0.001)","v":0.52999401737774465},0.51,0.55000000000000004,{"$f":"(H183-G183)/6","v":6.6666666666666723E-3},"normal",{"$f":"(K220*K181)/(((K197*(1-K19/100)*K41+K198*(1-K201/100)*K202+K203*(1-K205/100)*K206+K207*(1-K209/100)*K210))+0.001)","v":0.52999401737774465},0.51,0.55000000000000004,{"$f":"(M183-L183)/6","v":6.6666666666666723E-3},"normal",null,null,null,null,null,{"$f":"(U220*U181)/((U197*(1-U19/100)*U41+U198*(1-U201/100)*U202+U203*(1-U205/100)*U206+U207*(1-U209/100)*U210))","v":0.93500756325632584},0.04,4.3999999999999997E-2,{"$f":"(W183-V183)/6","v":6.666666666666661E-4},"normal",{"$f":"(Z220*Z181)/(((Z197*(1-Z19/100)*Z41+Z198*(1-Z201/100)*Z202+Z203*(1-Z205/100)*Z206+Z207*(1-Z209/100)*Z210))+0.001)","v":1.268086450502641},0.68,0.91,{"$f":"(AB183-AA183)/6","v":3.833333333333333E-2},"normal",{"$f":"(AE220*AE181)/(((AE197*(1-AE19/100)*AE41+AE198*(1-AE201/100)*AE202+AE203*(1-AE205/100)*AE206+AE207*(1-AE209/100)*AE210))+0.001)","v":0},0,0,{"$f":"(AG183-AF183)/6","v":0},"normal",null,null,null,{"$f":"(AL183-AK183)/6","v":0},"normal",null,null,null,{"$f":"(AQ183-AP183)/6","v":0},"normal",null,null,null,{"$f":"(AV183-AU183)/6","v":0},"normal",{"$f":"(AY220*AY181)/((AY197*(1-AY19/100)*AY41+AY198*(1-AY201/100)*AY202+AY203*(1-AY205/100)*AY206+AY207*(1-AY209/100)*AY210))","v":0.80960361497428091},null,null,{"$f":"(BA183-AZ183)/6","v":0},"normal",null,null,null,{"$f":"(BF183-BE183)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC220*CC181)/((CC197*(1-CC19/100)*CC41+CC203*(1-CC205/100)*CC206+CC198*(1-CC201/100)*CC202+CC207*(1-CC209/100)*CC210))","v":0.52627059392056785},null,null,{"$f":"(CE183-CD183)/6","v":0},"normal",{"$f":"(CH220*CH181)/((CH197*(1-CH19/100)*CH41+CH198*(1-CH201/100)*CH202+CH203*(1-CH205/100)*CH206+CH207*(1-CH209/100)*CH210))","v":0.62494769181320786},null,null,{"$f":"(CJ183-CI183)/6","v":0},"normal",{"$f":"(CM220*CM181)/((CM197*(1-CM19/100)*CM41+CM198*(1-CM201/100)*CM202+CM203*(1-CM205/100)*CM206+CM207*(1-CM209/100)*CM210))","v":0.63785796308103704},null,null,{"$f":"(CO183-CN183)/6","v":0},"normal",{"$f":"(CR220*CR181)/((CR197*(1-CR19/100)*CR41+CR198*(1-CR201/100)*CR202+CR203*(1-CR205/100)*CR206+CR207*(1-CR209/100)*CR210))","v":0.80960361497428091},null,null,{"$f":"(CT183-CS183)/6","v":0},"normal"]
["BC008b","BC508b",null,{"$f":"VLOOKUP(Data!A184,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Extraction rate (output/input), process 2"},{"$f":"VLOOKUP(Data!A184,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJoutput /MJinput"},{"$f":"F224*F182/((F220*F181)+0.001)","v":0.31987937632906788},0.3,0.34,6.6666666666666723E-3,"normal",{"$f":"K224*K182/((K220*K181)+0.001)","v":0.31987937632906788},0.3,0.34,6.6666666666666723E-3,"normal",null,null,null,null,null,{"$f":"U224*U182/((U220*U181)+0.001)","v":0.23643680485164861},0.96,0.99,5.0000000000000044E-3,"normal",{"$f":"Z224*Z182/((Z220*Z181)+0.001)","v":0.97999905997434233},0.96,0.99,5.0000000000000044E-3,"normal",{"$f":"AE224*AE182/((AE220*AE181)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"AY224*AY182/((AY220*AY181)+0.001)","v":0.42988509973027023},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC224*CC182/((CC220*CC181)+0.001)","v":0.55174806892279105},null,null,0,"normal",{"$f":"CH224*CH182/((CH220*CH181)+0.001)","v":0},null,null,0,"normal",{"$f":"CM224*CM182/((CM220*CM181)+0.001)","v":0},null,null,0,"normal",{"$f":"CR224*CR182/((CR220*CR181)+0.001)","v":0.42988509973027023},null,null,0,"normal"]
["BC009a0","BC509a0",null,{"$f":"VLOOKUP(Data!A185,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of main input, process 1"},{"$f":"VLOOKUP(Data!A185,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Fresh palm fruit bunches (FFB)",null,null,"n.a.","n.a.","Fresh palm fruit bunches (FFB)",null,null,"n.a.","n.a.",null,null,null,null,null,"Organic domestical waste",null,null,"n.a.","n.a.","Maize (corn)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","GFT",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Harvested grass",null,null,"n.a.","n.a.","Fatty residues",null,null,"n.a.","n.a.","Wood waste",null,null,"n.a.","n.a.","GFT",null,null,"n.a.","n.a."]
["BC009a1","BC509a1",null,{"$f":"VLOOKUP(Data!A186,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of material input flow 1, process 1"},{"$f":"VLOOKUP(Data!A186,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","Organic domestical waste",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Manure co- vergister ",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"GFT",null,null,"n.a.","n.a.","Methanol",null,null,"n.a.","n.a.","Digestate moerdijk",null,null,"n.a.","n.a.","Manure co- vergister ",null,null,"n.a.","n.a."]
["BC009a2","BC509a2",null,{"$f":"VLOOKUP(Data!A187,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of material input flow 2, process 1"},{"$f":"VLOOKUP(Data!A187,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Manure co- vergister ",null,null,"n.a.","n.a.","Sulphuric acid (H2SO4)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC009a3","BC509a3",null,{"$f":"VLOOKUP(Data!A188,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of material input flow 3, process 1"},{"$f":"VLOOKUP(Data!A188,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Glycerol",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a."]
["BC009b1","BC509b1",null,{"$f":"VLOOKUP(Data!A189,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of material input flow 1, process 2"},{"$f":"VLOOKUP(Data!A189,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Fuller's earth",null,null,"n.a.","n.a.","Fuller's earth",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC009b2","BC509b2",null,{"$f":"VLOOKUP(Data!A190,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of material input flow 2, process 2"},{"$f":"VLOOKUP(Data!A190,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC009c","BC509c",null,{"$f":"VLOOKUP(Data!A191,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of material output flow, process 1"},{"$f":"VLOOKUP(Data!A191,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"Compost Breda - tunnel",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Compost Breda - tunnel",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Biogas (55% CH4)",null,null,"n.a.","n.a.","Biodiesel",null,null,"n.a.","n.a.","Fast pyrolysis bio-oil",null,null,"n.a.","n.a.","Compost Breda - tunnel",null,null,"n.a.","n.a."]
["BC009c1","BC509c1",null,{"$f":"VLOOKUP(Data!A192,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of output flow, process 1 (electricity)"},{"$f":"VLOOKUP(Data!A192,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"Electricity from pyrolysis",null,null,null,null,"n.a."]
["BC009c2","BC509c2",null,{"$f":"VLOOKUP(Data!A193,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of output flow, process 1 (heat)"},{"$f":"VLOOKUP(Data!A193,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"Heat from pyrolysis",null,null,null,null,"n.a."]
["BC009d","BC509d",null,{"$f":"VLOOKUP(Data!A194,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of material output flow, process 2"},{"$f":"VLOOKUP(Data!A194,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"Biogas (55% CH4)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Liquid biomethane (LBM)",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Liquid biomethane (LBM)",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Liquid biomethane (LBM)",null,null,"n.a.","n.a."]
["BC009d1","BC509d1",null,{"$f":"VLOOKUP(Data!A195,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of output flow, process 2 (electricity)"},{"$f":"VLOOKUP(Data!A195,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a."]
["BC009d2","BC509d2",null,{"$f":"VLOOKUP(Data!A196,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of output flow, process 2 (heat)"},{"$f":"VLOOKUP(Data!A196,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a.",null,null,null,null,"n.a."]
["BC010a0","BC510a0",null,{"$f":"VLOOKUP(Data!A197,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Main input, process 1"},{"$f":"VLOOKUP(Data!A197,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},19000,null,null,null,null,19000,null,null,null,null,null,null,null,null,null,32000000,null,null,null,null,44000,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,32000000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,77777000,null,null,null,null,8000000,null,null,null,null,44737000,null,null,null,null,32000000]
["BC010a01","BC510a01",null,{"$f":"VLOOKUP(Data!A198,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Material input flow 1, process 1"},{"$f":"VLOOKUP(Data!A198,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,500000,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,8000000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,15799000,null,null,null,null,1680000,null,null,null,null,31079000,null,null,null,null,8000000]
["BC010a","BC510a",null,{"$f":"VLOOKUP(Data!A199,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of main input, process 1"},{"$f":"VLOOKUP(Data!A199,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgdm/MJoutput"},{"$f":"F197*(1-F19/100)/(F220*F181+0.001)","v":7.8617238875928711E-2},0,0,{"$f":"(H199-G199)/6","v":0},"normal",{"$f":"K197*(1-K19/100)/(K220*K181+0.001)","v":7.8617238875928711E-2},0,0,{"$f":"(M199-L199)/6","v":0},"normal",null,null,null,null,null,{"$f":"U197*(1-U19/100)/(U220*U181+0.001)","v":0.10589208566886006},0,0,{"$f":"(W199-V199)/6","v":0},"normal",{"$f":"Z197*(1-Z19/100)/(Z220*Z181+0.001)","v":3.7589863256167842E-3},0,0,{"$f":"(AB199-AA199)/6","v":0},"normal",{"$f":"AE197*(1-AE19/100)/(AE220*AE181+0.001)","v":0},0,0,{"$f":"(AG199-AF199)/6","v":0},"normal",null,null,null,{"$f":"(AL199-AK199)/6","v":0},"normal",null,null,null,{"$f":"(AQ199-AP199)/6","v":0},"normal",null,null,null,{"$f":"(AV199-AU199)/6","v":0},"normal",{"$f":"AY197*(1-AY19/100)/(AY220*AY181+0.001)","v":0.10589208566886006},0,0,{"$f":"(BA199-AZ199)/6","v":0},"normal",null,null,null,{"$f":"(BF199-BE199)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC197*(1-CC19/100)/(CC220*CC181+0.001)","v":9.3658974053971375E-2},0,0,{"$f":"(CE199-CD199)/6","v":0},"normal",{"$f":"CH197*(1-CH19/100)/(CH220*CH181+0.001)","v":4.1240564952526593E-2},0,0,{"$f":"(CJ199-CI199)/6","v":0},"normal",{"$f":"CM197*(1-CM19/100)/(CM220*CM181+0.001)","v":5.9197624303172665E-2},0,0,{"$f":"(CO199-CN199)/6","v":0},"normal",{"$f":"CR197*(1-CR19/100)/(CR220*CR181+0.001)","v":0.10589208566886006},0,0,{"$f":"(CT199-CS199)/6","v":0},"normal"]
["BC010a1","BC510a1",null,{"$f":"VLOOKUP(Data!A200,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material input flow 1, process 1"},{"$f":"VLOOKUP(Data!A200,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgdm/MJoutput"},{"$f":"F198*(1-F201/100)/(F220*F181+0.001)","v":0},0,0,{"$f":"(H200-G200)/6","v":0},"normal",{"$f":"K198*(1-K201/100)/(K220*K181+0.001)","v":0},0,0,{"$f":"(M200-L200)/6","v":0},"normal",null,null,null,null,null,{"$f":"U198*(1-U201/100)/(U220*U181+0.001)","v":0},0,0,{"$f":"(W200-V200)/6","v":0},"normal",{"$f":"Z198*(1-Z201/100)/(Z220*Z181+0.001)","v":7.1192922833651209E-2},0.16,0.2,{"$f":"(AB200-AA200)/6","v":6.666666666666668E-3},"normal",{"$f":"AE198*(1-AE201/100)/(AE220*AE181+0.001)","v":0},0,0,{"$f":"(AG200-AF200)/6","v":0},"normal",null,null,null,{"$f":"(AL200-AK200)/6","v":0},"normal",null,null,null,{"$f":"(AQ200-AP200)/6","v":0},"normal",null,null,null,{"$f":"(AV200-AU200)/6","v":0},"normal",{"$f":"AY198*(1-AY201/100)/(AY220*AY181+0.001)","v":1.2942366026194007E-2},0,0,{"$f":"(BA200-AZ200)/6","v":0},"normal",null,null,null,{"$f":"(BF200-BE200)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC198*(1-CC201/100)/(CC220*CC181+0.001)","v":2.4031752822264902E-2},0,0,{"$f":"(CE200-CD200)/6","v":0},"normal",{"$f":"CH198*(1-CH201/100)/(CH220*CH181+0.001)","v":0},0,0,{"$f":"(CJ200-CI200)/6","v":0},"normal",{"$f":"CM198*(1-CM201/100)/(CM220*CM181+0.001)","v":4.1124862322424467E-2},0,0,{"$f":"(CO200-CN200)/6","v":0},"normal",{"$f":"CR198*(1-CR201/100)/(CR220*CR181+0.001)","v":1.2942366026194007E-2},0,0,0,"normal"]
["BC010a10","BC510a10",null,{"$f":"VLOOKUP(Data!A201,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of material input flow 1, process 1"},{"$f":"VLOOKUP(Data!A201,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,78,null,null,null,null,50,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,78,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,52,null,null,null,null,100,null,null,null,null,5,null,null,null,null,78]
["BC010a11","BC510a11",null,{"$f":"VLOOKUP(Data!A202,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of input flow 1, process 1"},{"$f":"VLOOKUP(Data!A202,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F186=\"n.a.\",0,VLOOKUP(F186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(K186=\"n.a.\",0,VLOOKUP(K186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U186=\"n.a.\",0,VLOOKUP(U186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z186=\"n.a.\",0,VLOOKUP(Z186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":10.1},null,null,null,null,{"$f":"IF(AE186=\"n.a.\",0,VLOOKUP(AE186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY186=\"n.a.\",0,VLOOKUP(AY186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":12.8},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC186=\"n.a.\",0,VLOOKUP(CC186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":10.116},null,null,null,null,{"$f":"IF(CH186=\"n.a.\",0,VLOOKUP(CH186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":19.899999999999999},null,null,null,null,{"$f":"IF(CM186=\"n.a.\",0,VLOOKUP(CM186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":12.6},null,null,null,null,{"$f":"IF(CR186=\"n.a.\",0,VLOOKUP(CR186,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":12.8}]
["BC010a02","BC510a02",null,{"$f":"VLOOKUP(Data!A203,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Material input flow 2, process 1"},{"$f":"VLOOKUP(Data!A203,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5935000,null,null,null,null,2264000,null,null,null,null,0,null,null,null,null,0]
["BC010a2","BC510a2",null,{"$f":"VLOOKUP(Data!A204,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material input flow 2, process 1"},{"$f":"VLOOKUP(Data!A204,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgdm/MJoutput"},{"$f":"F203*(1-F205/100)/(F220*F181+0.001)","v":0},0,0,0,"normal",{"$f":"K203*(1-K205/100)/(K220*K181+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"U203*(1-U205/100)/(U220*U181+0.001)","v":0},0,0,0,"normal",{"$f":"Z203*(1-Z205/100)/(Z220*Z181+0.001)","v":0},0,0,0,"normal",{"$f":"AE203*(1-AE205/100)/(AE220*AE181+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"AY203*(1-AY205/100)/(AY220*AY181+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC203*(1-CC205/100)/(CC220*CC181+0.001)","v":3.0092295503964858E-3},0,0,0,"normal",{"$f":"CH203*(1-CH205/100)/(CH220*CH181+0.001)","v":0},0,0,{"$f":"(CJ204-CI204)/6","v":0},"normal",{"$f":"CM203*(1-CM205/100)/(CM220*CM181+0.001)","v":0},0,0,{"$f":"(CO204-CN204)/6","v":0},"normal",{"$f":"CR203*(1-CR205/100)/(CR220*CR181+0.001)","v":0},0,0,0,"normal"]
["BC010a20","BC510a20",null,{"$f":"VLOOKUP(Data!A205,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of material input flow 2, process 1"},{"$f":"VLOOKUP(Data!A205,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,84,null,null,null,null,100,null,null,null,null,0,null,null,null,null,0]
["BC010a21","BC510a21",null,{"$f":"VLOOKUP(Data!A206,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of input flow 2, process 1"},{"$f":"VLOOKUP(Data!A206,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F187=\"n.a.\",0,VLOOKUP(F187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(K187=\"n.a.\",0,VLOOKUP(K187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U187=\"n.a.\",0,VLOOKUP(U187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z187=\"n.a.\",0,VLOOKUP(Z187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(AE187=\"n.a.\",0,VLOOKUP(AE187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY187=\"n.a.\",0,VLOOKUP(AY187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC187=\"n.a.\",0,VLOOKUP(CC187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":12.8},null,null,null,null,{"$f":"IF(CH187=\"n.a.\",0,VLOOKUP(CH187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CM187=\"n.a.\",0,VLOOKUP(CM187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CR187=\"n.a.\",0,VLOOKUP(CR187,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0}]
["BC010a03","BC510a03",null,{"$f":"VLOOKUP(Data!A207,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Material input flow 3, process 1"},{"$f":"VLOOKUP(Data!A207,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1000000,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC010a3","BC510a3",null,{"$f":"VLOOKUP(Data!A208,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material input flow 3, process 1"},{"$f":"VLOOKUP(Data!A208,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgdm/MJoutput"},{"$f":"F207*(1-F209/100)/(F220*F181+0.001)","v":0},null,null,null,null,{"$f":"K207*(1-K209/100)/(K220*K181+0.001)","v":0},0,0,{"$f":"(M208-L208)/6","v":0},"normal",null,null,null,null,null,{"$f":"U207*(1-U209/100)/(U220*U181+0.001)","v":0},0,0,0,"normal",{"$f":"Z207*(1-Z209/100)/(Z220*Z181+0.001)","v":0},0,0,0,"normal",{"$f":"AE207*(1-AE209/100)/(AE220*AE181+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AY207*(1-AY209/100)/(AY220*AY181+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC207*(1-CC209/100)/(CC220*CC181+0.001)","v":4.7534165181073381E-4},0,0,0,"normal",{"$f":"CH207*(1-CH209/100)/(CH220*CH181+0.001)","v":0},0,0,0,"normal",{"$f":"CM207*(1-CM209/100)/(CM220*CM181+0.001)","v":0},0,0,0,"normal",{"$f":"CR207*(1-CR209/100)/(CR220*CR181+0.001)","v":0},0,0,{"$f":"(CT208-CS208)/6","v":0},"normal"]
["BC010a30","BC510a30",null,{"$f":"VLOOKUP(Data!A209,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of material input flow 3, process 1"},{"$f":"VLOOKUP(Data!A209,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,85,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC010a31","BC510a31",null,{"$f":"VLOOKUP(Data!A210,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of input flow 3, process 1"},{"$f":"VLOOKUP(Data!A210,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F188=\"n.a.\",0,VLOOKUP(F188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(K188=\"n.a.\",0,VLOOKUP(K188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U188=\"n.a.\",0,VLOOKUP(U188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z188=\"n.a.\",0,VLOOKUP(Z188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(AE188=\"n.a.\",0,VLOOKUP(AE188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY188=\"n.a.\",0,VLOOKUP(AY188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC188=\"n.a.\",0,VLOOKUP(CC188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":16},null,null,null,null,{"$f":"IF(CH188=\"n.a.\",0,VLOOKUP(CH188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CM188=\"n.a.\",0,VLOOKUP(CM188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CR188=\"n.a.\",0,VLOOKUP(CR188,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0}]
["BC010b1","BC510b1",null,{"$f":"VLOOKUP(Data!A211,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material input flow 1, process 2"},{"$f":"VLOOKUP(Data!A211,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/MJoutput"},{"$f":"F212*(1-F213/100)/(F224*F182+0.001)","v":0},0,0,0,"normal",{"$f":"K212*(1-K213/100)/(K224*K182+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"U212*(1-U213/100)/(U224*U182+0.001)","v":0},1E-4,2.9999999999999997E-4,3.3333333333333328E-5,"normal",{"$f":"Z212*(1-Z213/100)/(Z224*Z182+0.001)","v":0},0,0,0,"normal",{"$f":"AE212*(1-AE213/100)/(AE224*AE182+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"AY212*(1-AY213/100)/(AY224*AY182+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC212*(1-CC213/100)/(CC224*CC182+0.001)","v":0},0,0,0,"normal",{"$f":"CH212*(1-CH213/100)/(CH224*CH182+0.001)","v":0},0,0,{"$f":"(CJ211-CI211)/6","v":0},"normal",{"$f":"CM212*(1-CM213/100)/(CM224*CM182+0.001)","v":0},0,0,{"$f":"(CO211-CN211)/6","v":0},"normal",{"$f":"CR212*(1-CR213/100)/(CR224*CR182+0.001)","v":0},0,0,{"$f":"(CT211-CS211)/6","v":0},"normal"]
["BC010b10","BC510b10",null,{"$f":"VLOOKUP(Data!A212,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Material input flow 1, process 2"},{"$f":"VLOOKUP(Data!A212,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC010b11","BC510b11",null,{"$f":"VLOOKUP(Data!A213,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of material input flow 1, process 2"},{"$f":"VLOOKUP(Data!A213,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC010b12","BC510b12",null,{"$f":"VLOOKUP(Data!A214,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of input flow 1, process 2"},{"$f":"VLOOKUP(Data!A214,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F189=\"n.a.\",0,VLOOKUP(F189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(K189=\"n.a.\",0,VLOOKUP(K189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U189=\"n.a.\",0,VLOOKUP(U189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z189=\"n.a.\",0,VLOOKUP(Z189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(AE189=\"n.a.\",0,VLOOKUP(AE189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY189=\"n.a.\",0,VLOOKUP(AY189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC189=\"n.a.\",0,VLOOKUP(CC189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CH189=\"n.a.\",0,VLOOKUP(CH189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CM189=\"n.a.\",0,VLOOKUP(CM189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CR189=\"n.a.\",0,VLOOKUP(CR189,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0}]
["BC010b2","BC510b2",null,{"$f":"VLOOKUP(Data!A215,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material input flow 2, process 2"},{"$f":"VLOOKUP(Data!A215,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/MJoutput"},{"$f":"F216*(1-F217/100)/(F224*F182+0.001)","v":0},0,0,0,"normal",{"$f":"K216*(1-K217/100)/(K224*K182+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"U216*(1-U217/100)/(U224*U182+0.001)","v":0},0,0,0,"normal",{"$f":"Z216*(1-Z217/100)/(Z224*Z182+0.001)","v":0},0,0,0,"normal",{"$f":"AE216*(1-AE217/100)/(AE224*AE182+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"AY216*(1-AY217/100)/(AY224*AY182+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC216*(1-CC217/100)/(CC224*CC182+0.001)","v":0},0,0,0,"normal",{"$f":"CH216*(1-CH217/100)/(CH224*CH182+0.001)","v":0},0,0,0,"normal",{"$f":"CM216*(1-CM217/100)/(CM224*CM182+0.001)","v":0},0,0,0,"normal",{"$f":"CR216*(1-CR217/100)/(CR224*CR181+0.001)","v":0},0,0,0,"normal"]
["BC010b20","BC510b20",null,{"$f":"VLOOKUP(Data!A216,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Material input flow 2, process 2"},{"$f":"VLOOKUP(Data!A216,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC010b21","BC510b21",null,{"$f":"VLOOKUP(Data!A217,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Moisture content of material input flow 2, process 2"},{"$f":"VLOOKUP(Data!A217,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"%"},0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0,null,null,null,null,0]
["BC010b22","BC510b22",null,{"$f":"VLOOKUP(Data!A218,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Energy content of input flow 2, process 2"},{"$f":"VLOOKUP(Data!A218,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/kgdm"},{"$f":"IF(F190=\"n.a.\",0,VLOOKUP(F190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(K190=\"n.a.\",0,VLOOKUP(K190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,{"$f":"IF(U190=\"n.a.\",0,VLOOKUP(U190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(Z190=\"n.a.\",0,VLOOKUP(Z190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(AE190=\"n.a.\",0,VLOOKUP(AE190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(AY190=\"n.a.\",0,VLOOKUP(AY190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"IF(CC190=\"n.a.\",0,VLOOKUP(CC190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CH190=\"n.a.\",0,VLOOKUP(CH190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CM190=\"n.a.\",0,VLOOKUP(CM190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},null,null,null,null,{"$f":"IF(CR190=\"n.a.\",0,VLOOKUP(CR190,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0}]
["BC010c","BC510c",null,{"$f":"VLOOKUP(Data!A219,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material output flow, process 1"},{"$f":"VLOOKUP(Data!A219,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgdm/MJoutput"},{"$f":"F136*(1-F135/100)/((F220*F181)+0.001)","v":2.6636946173917474E-3},0,0,{"$f":"(H219-G219)/6","v":0},"normal",{"$f":"K136*(1-K135/100)/((K220*K181)+0.001)","v":2.6636946173917474E-3},0,0,{"$f":"(M219-L219)/6","v":0},"normal",null,null,null,null,null,{"$f":"U136*(1-U135/100)/((U220*U181)+0.001)","v":6.6942623402394028E-2},0,0,{"$f":"(W219-V219)/6","v":0},"normal",{"$f":"Z136*(1-Z135/100)/((Z220*Z181)+0.001)","v":0},0,0,{"$f":"(AB219-AA219)/6","v":0},"normal",{"$f":"AE136*(1-AE135/100)/((AE220*AE181)+0.001)","v":0},0,0,{"$f":"(AG219-AF219)/6","v":0},"normal",null,null,null,{"$f":"(AL219-AK219)/6","v":0},"normal",null,null,null,{"$f":"(AQ219-AP219)/6","v":0},"normal",null,null,null,{"$f":"(AV219-AU219)/6","v":0},"normal",{"$f":"AY136*(1-AY135/100)/((AY220*AY181)+0.001)","v":6.6942623402394028E-2},0,0,{"$f":"(BA219-AZ219)/6","v":0},"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC136*(1-CC135/100)/((CC220*CC181)+0.001)","v":9.3545963160725568E-2},0,0,0,"normal",{"$f":"CH136*(1-CH135/100)/((CH220*CH181)+0.001)","v":4.4354793260511696E-3},0,0,0,"normal",{"$f":"CM136*(1-CM135/100)/((CM220*CM181)+0.001)","v":1.255263781940045E-2},0,0,0,"normal",{"$f":"CR136*(1-CR135/100)/((CR220*CR181)+0.001)","v":6.6942623402394028E-2},0,0,0,"normal"]
["BC010c0","BC510c0",null,{"$f":"VLOOKUP(Data!A220,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Material output flow, process 1"},{"$f":"VLOOKUP(Data!A220,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},4311,null,null,null,null,4311,null,null,null,null,null,null,null,null,null,4945000,null,null,null,null,127694,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,4945000,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,11475000,null,null,null,null,7768000,null,null,null,null,33945000,null,null,null,null,4945000]
["BC010c1","BC510c1",null,{"$f":"VLOOKUP(Data!A221,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material output flow, process 1 (Electricity)"},{"$f":"VLOOKUP(Data!A221,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/MJoutput"},{"$f":"(F143*3600)/((F220*F181)+0.001)","v":0},null,null,null,null,{"$f":"(K143*3600)/((K220*K181)+0.001)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"(U143*3600)/((U220*U181)+0.001)","v":0},null,null,null,null,{"$f":"(Z143*3600)/((Z220*Z181)+0.001)","v":0},null,null,null,null,{"$f":"(AE143*3600)/((AE220*AE181)+0.001)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(AY143*3600)/((AY220*AY181)+0.001)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC143*3600)/((CC220*CC181)+0.001)","v":0},null,null,null,null,{"$f":"(CH143*3600)/((CH220*CH181)+0.001)","v":0},null,null,null,null,{"$f":"(CM143*3600)/((CM220*CM181)+0.001)","v":7.5757091414980826E-2},null,null,null,null,{"$f":"(CR143*3600)/((CR220*CR181)+0.001)","v":0}]
["BC010c2","BC510c2",null,{"$f":"VLOOKUP(Data!A222,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material output flow, process 1 (Heat)"},{"$f":"VLOOKUP(Data!A222,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJf_h/MJoutput"},{"$f":"F144/((F220*F181)+0.001)","v":0},null,null,null,null,{"$f":"K144/((K220*K181)+0.001)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"U144/((U220*U181)+0.001)","v":0},null,null,null,null,{"$f":"Z144/((Z220*Z181)+0.001)","v":0},null,null,null,null,{"$f":"AE144/((AE220*AE181)+0.001)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AY144/((AY220*AY181)+0.001)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC144/((CC220*CC181)+0.001)","v":0},null,null,null,null,{"$f":"CH144/((CH220*CH181)+0.001)","v":0},null,null,null,null,{"$f":"CM144/((CM220*CM181)+0.001)","v":0.46483064141727687},null,null,null,null,{"$f":"CR144/((CR220*CR181)+0.001)","v":0}]
["BC010d","BC510d",null,{"$f":"VLOOKUP(Data!A223,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material output flow, process 2"},{"$f":"VLOOKUP(Data!A223,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kgdm/MJoutput"},{"$f":"F147*(1-F146/100)/((F224*F182)+0.001)","v":0},0,0,0,"normal",{"$f":"K147*(1-K146/100)/((K224*K182)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"U147*(1-U146/100)/((U224*U182)+0.001)","v":0},0,0,0,"normal",{"$f":"Z147*(1-Z146/100)/((Z224*Z182)+0.001)","v":0},0,0,0,"normal",{"$f":"AE147*(1-AE146/100)/((AE224*AE182)+0.001)","v":0},0,0,{"$f":"(AG223-AF223)/6","v":0},"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,{"$f":"(AV223-AU223)/6","v":0},"normal",{"$f":"AY147*(1-AY146/100)/((AY224*AY182)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC147*(1-CC146/100)/((CC224*CC182)+0.001)","v":0},0,0,0,"normal",{"$f":"CH147*(1-CH146/100)/((CH224*CH182)+0.001)","v":0},0,0,0,"normal",{"$f":"CM147*(1-CM146/100)/((CM224*CM182)+0.001)","v":0},0,0,0,"normal",{"$f":"CR147*(1-CR146/100)/((CR224*CR182)+0.001)","v":0},0,0,0,"normal"]
["BC010d0","BC510d0",null,{"$f":"VLOOKUP(Data!A224,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Material output flow, process 2"},{"$f":"VLOOKUP(Data!A224,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"kg/year"},1379,null,null,null,null,1379,null,null,null,null,null,null,null,null,null,1169180,null,null,null,null,125140,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1169180,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"3482220","v":3482220},null,null,null,null,0,null,null,null,null,0,null,null,null,null,1169180]
["BC010d1","BC510d1",null,{"$f":"VLOOKUP(Data!A225,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material output flow, process 2 (Electricity)"},{"$f":"VLOOKUP(Data!A225,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/MJoutput"},{"$f":"F151*3600/((F224*F182)+0.001)","v":0},null,null,null,null,{"$f":"K151*3600/((K224*K182)+0.001)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"U151*3600/((U224*U182)+0.001)","v":0},null,null,null,null,{"$f":"Z151*3600/((Z224*Z182)+0.001)","v":0},null,null,null,null,{"$f":"AE151*3600/((AE224*AE182)+0.001)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AY151*3600/((AY224*AY182)+0.001)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC151*3600/((CC224*CC182)+0.001)","v":0},null,null,null,null,{"$f":"CH151*3600/((CH224*CH182)+0.001)","v":0},null,null,null,null,{"$f":"CM151*3600/((CM224*CM182)+0.001)","v":0},null,null,null,null,{"$f":"CR151*3600/((CR224*CR182)+0.001)","v":0}]
["BC010d2","BC510d2",null,{"$f":"VLOOKUP(Data!A226,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of material output flow, process 2 (Heat)"},{"$f":"VLOOKUP(Data!A226,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJf_h/MJoutput"},{"$f":"F152/((F224*F182)+0.001)","v":0},null,null,null,null,{"$f":"K152/((K224*K182)+0.001)","v":0},null,null,null,null,null,null,null,null,null,{"$f":"U152/((U224*U182)+0.001)","v":0},null,null,null,null,{"$f":"Z152/((Z224*Z182)+0.001)","v":0},null,null,null,null,{"$f":"AE152/((AE224*AE182)+0.001)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"AY152/((AY224*AY182)+0.001)","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC152/((CC224*CC182)+0.001)","v":0},null,null,null,null,{"$f":"CH152/((CH224*CH182)+0.001)","v":0},null,null,null,null,{"$f":"CM152/((CM224*CM182)+0.001)","v":0},null,null,null,null,{"$f":"CR152/((CR224*CR182)+0.001)","v":0}]
["BC011a1","BC511a1",null,{"$f":"VLOOKUP(Data!A227,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel/heat flow 1, process 1"},{"$f":"VLOOKUP(Data!A227,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"Heat from landfill gas CHP",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Heat from wood boiler CHP",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Heat from pyrolysis",null,null,"n.a.","n.a.","Heat from pyrolysis",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Heat from wood boiler CHP",null,null,"n.a.","n.a."]
["BC011a2","BC511a2",null,{"$f":"VLOOKUP(Data!A228,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel/heat flow 2, process 1"},{"$f":"VLOOKUP(Data!A228,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"Diesel",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Diesel",null,null,"n.a.","n.a."]
["BC011b1","BC511b1",null,{"$f":"VLOOKUP(Data!A229,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel/heat flow 1, process 2"},{"$f":"VLOOKUP(Data!A229,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Heat from NG boiler",null,null,"n.a.","n.a.","Heat from NG boiler",null,null,"n.a.","n.a.",null,null,null,null,null,"Heat from landfill gas CHP",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Heat from wood boiler CHP",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Heat from wood boiler CHP",null,null,"n.a.","n.a."]
["BC011b2","BC511b2",null,{"$f":"VLOOKUP(Data!A230,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of fuel/heat flow 2, process 2"},{"$f":"VLOOKUP(Data!A230,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC031a1","BC531a1",null,{"$f":"VLOOKUP(Data!A231,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of fuel/heat input 1, process 1"},{"$f":"VLOOKUP(Data!A231,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJf_h/MJoutput"},{"$f":"F232/((F220*F181)+0.001)","v":0},0,0,{"$f":"(H231-G231)/6","v":0},"normal",{"$f":"K232/((K220*K181)+0.001)","v":0},0,0,{"$f":"(M231-L231)/6","v":0},"normal",null,null,null,null,null,{"$f":"U232/((U220*U181)+0.001)","v":2.0876918834298177E-2},0,0,{"$f":"(W231-V231)/6","v":0},"normal",{"$f":"Z232/((Z220*Z181)+0.001)","v":0},0,0,{"$f":"(AB231-AA231)/6","v":0},"normal",{"$f":"AE232/((AE220*AE181)+0.001)","v":0},0,0,{"$f":"(AG231-AF231)/6","v":0},"normal",null,null,null,{"$f":"(AL231-AK231)/6","v":0},"normal",null,null,null,{"$f":"(AQ231-AP231)/6","v":0},"normal",null,null,null,{"$f":"(AV231-AU231)/6","v":0},"normal",{"$f":"AY232/((AY220*AY181)+0.001)","v":2.0876918834298177E-2},null,null,{"$f":"(BA231-AZ231)/6","v":0},"normal",null,null,null,{"$f":"(BF231-BE231)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC232/((CC220*CC181)+0.001)","v":5.54533571002402E-2},null,null,{"$f":"(CE231-CD231)/6","v":0},"normal",{"$f":"CH232/((CH220*CH181)+0.001)","v":4.4589612754243821E-2},null,null,{"$f":"(CJ231-CI231)/6","v":0},"normal",{"$f":"CM232/((CM220*CM181)+0.001)","v":0},null,null,{"$f":"(CO231-CN231)/6","v":0},"normal",{"$f":"CR232/((CR220*CR181)+0.001)","v":2.0876918834298177E-2},null,null,{"$f":"(CT231-CS231)/6","v":0},"normal"]
["BC031a10","BC531a10",null,{"$f":"VLOOKUP(Data!A232,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fuel/heat flow 1, process 1"},{"$f":"VLOOKUP(Data!A232,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/year"},0,0,0,{"$f":"(H232-G232)/6","v":0},"normal",0,0,0,{"$f":"(M232-L232)/6","v":0},"normal",null,null,null,null,null,2839000,0,0,{"$f":"(W232-V232)/6","v":0},"normal",0,0,0,{"$f":"(AB232-AA232)/6","v":0},"normal",0,0,0,{"$f":"(AG232-AF232)/6","v":0},"normal",null,null,null,{"$f":"(AL232-AK232)/6","v":0},"normal",null,null,null,{"$f":"(AQ232-AP232)/6","v":0},"normal",null,null,null,{"$f":"(AV232-AU232)/6","v":0},"normal",2839000,null,null,{"$f":"(BA232-AZ232)/6","v":0},"normal",null,null,null,{"$f":"(BF232-BE232)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,17499000,null,null,{"$f":"(CE232-CD232)/6","v":0},"normal",8545000,null,null,{"$f":"(CJ232-CI232)/6","v":0},"normal",0,null,null,{"$f":"(CO232-CN232)/6","v":0},"normal",2839000,null,null,{"$f":"(CT232-CS232)/6","v":0},"normal"]
["BC031a2","BC531a2",null,{"$f":"VLOOKUP(Data!A233,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of fuel/heat input 2, process 1"},{"$f":"VLOOKUP(Data!A233,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJf_h/MJoutput"},{"$f":"(F234)/((F220*F181)+0.001)","v":0},0,0,0,"normal",{"$f":"(K234)/((K220*K181)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"(U234)/((U220*U181)+0.001)","v":0},0,0,0,"normal",{"$f":"(Z234)/((Z220*Z181)+0.001)","v":0},0,0,0,"normal",{"$f":"(AE234)/((AE220*AE181)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"(AY234)/((AY220*AY181)+0.001)","v":0},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CC234)/((CC220*CC181)+0.001)","v":0},null,null,0,"normal",{"$f":"(CH234)/((CH220*CH181)+0.001)","v":0},null,null,0,"normal",{"$f":"(CM234)/((CM220*CM181)+0.001)","v":0},null,null,0,"normal",{"$f":"(CR234)/((CR220*CR181)+0.001)","v":0},null,null,0,"normal"]
["BC031a20","BC531a20",null,{"$f":"VLOOKUP(Data!A234,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fuel/heat flow 2, process 1"},{"$f":"VLOOKUP(Data!A234,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/year"},0,0,0,{"$f":"(H234-G234)/6","v":0},"normal",0,0,0,{"$f":"(M234-L234)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W234-V234)/6","v":0},"normal",0,0,0,{"$f":"(AB234-AA234)/6","v":0},"normal",0,0,0,{"$f":"(AG234-AF234)/6","v":0},"normal",null,null,null,{"$f":"(AL234-AK234)/6","v":0},"normal",null,null,null,{"$f":"(AQ234-AP234)/6","v":0},"normal",null,null,null,{"$f":"(AV234-AU234)/6","v":0},"normal",0,null,null,{"$f":"(BA234-AZ234)/6","v":0},"normal",null,null,null,{"$f":"(BF234-BE234)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE234-CD234)/6","v":0},"normal",0,null,null,{"$f":"(CJ234-CI234)/6","v":0},"normal",0,null,null,{"$f":"(CO234-CN234)/6","v":0},"normal",0,null,null,{"$f":"(CT234-CS234)/6","v":0},"normal"]
["BC031b1","BC531b1",null,{"$f":"VLOOKUP(Data!A235,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of fuel/heat input 1, process 2"},{"$f":"VLOOKUP(Data!A235,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJf_h/MJoutput"},{"$f":"F236/((F224*F182)+0.001)","v":7.9963936264744601E-3},0,0.02,3.3333333333333335E-3,"normal",{"$f":"K236/((K224*K182)+0.001)","v":7.9963936264744601E-3},0,0.02,3.3333333333333335E-3,"normal",null,null,null,null,null,{"$f":"U236/((U224*U182)+0.001)","v":0.24803708581311731},0,0,0,"normal",{"$f":"Z236/((Z224*Z182)+0.001)","v":0},0,0,0,"normal",{"$f":"AE236/((AE224*AE182)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"AY236/((AY224*AY182)+0.001)","v":0.13642039719912383},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC236/((CC224*CC182)+0.001)","v":0},null,null,0,"normal",{"$f":"CH236/((CH224*CH182)+0.001)","v":0},null,null,0,"normal",{"$f":"CM236/((CM224*CM182)+0.001)","v":0},null,null,0,"normal",{"$f":"CR236/((CR224*CR182)+0.001)","v":0.13642039719912383},null,null,0,"normal"]
["BC031b10","BC531b10",null,{"$f":"VLOOKUP(Data!A236,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fuel/heat flow 1, process 2"},{"$f":"VLOOKUP(Data!A236,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/year"},408,0,0,{"$f":"(H236-G236)/6","v":0},"normal",408,0,0,{"$f":"(M236-L236)/6","v":0},"normal",null,null,null,null,null,7975000,0,0,{"$f":"(W236-V236)/6","v":0},"normal",0,0,0,{"$f":"(AB236-AA236)/6","v":0},"normal",0,0,0,{"$f":"(AG236-AF236)/6","v":0},"normal",null,null,null,{"$f":"(AL236-AK236)/6","v":0},"normal",null,null,null,{"$f":"(AQ236-AP236)/6","v":0},"normal",null,null,null,{"$f":"(AV236-AU236)/6","v":0},"normal",7975000,null,null,{"$f":"(BA236-AZ236)/6","v":0},"normal",null,null,null,{"$f":"(BF236-BE236)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE236-CD236)/6","v":0},"normal",0,null,null,{"$f":"(CJ236-CI236)/6","v":0},"normal",0,null,null,{"$f":"(CO236-CN236)/6","v":0},"normal",7975000,null,null,{"$f":"(CT236-CS236)/6","v":0},"normal"]
["BC031b2","BC531b2",null,{"$f":"VLOOKUP(Data!A237,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of fuel/heat input 2, process 2"},{"$f":"VLOOKUP(Data!A237,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJf_h/MJoutput"},{"$f":"F238/((F224*F182)+0.001)","v":0},0,0,0,"normal",{"$f":"K238/((K224*K182)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"U238/((U224*U182)+0.001)","v":0},0,0,0,"normal",{"$f":"Z238/((Z224*Z182)+0.001)","v":0},0,0,0,"normal",{"$f":"AE238/((AE224*AE182)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"AY238/((AY224*AY182)+0.001)","v":0},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC238/((CC224*CC182)+0.001)","v":0},null,null,0,"normal",{"$f":"CH238/((CH224*CH182)+0.001)","v":0},null,null,0,"normal",{"$f":"CM238/((CM224*CM182)+0.001)","v":0},null,null,0,"normal",{"$f":"CR238/((CR224*CR182)+0.001)","v":0},null,null,0,"normal"]
["BC031b20","BC531b20",null,{"$f":"VLOOKUP(Data!A238,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fuel/heat flow 2, process 2"},{"$f":"VLOOKUP(Data!A238,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJ/year"},0,0,0,{"$f":"(H238-G238)/6","v":0},"normal",0,0,0,{"$f":"(M238-L238)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W238-V238)/6","v":0},"normal",0,0,0,{"$f":"(AB238-AA238)/6","v":0},"normal",0,0,0,{"$f":"(AG238-AF238)/6","v":0},"normal",null,null,null,{"$f":"(AL238-AK238)/6","v":0},"normal",null,null,null,{"$f":"(AQ238-AP238)/6","v":0},"normal",null,null,null,{"$f":"(AV238-AU238)/6","v":0},"normal",0,null,null,{"$f":"(BA238-AZ238)/6","v":0},"normal",null,null,null,{"$f":"(BF238-BE238)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE238-CD238)/6","v":0},"normal",0,null,null,{"$f":"(CJ238-CI238)/6","v":0},"normal",0,null,null,{"$f":"(CO238-CN238)/6","v":0},"normal",0,null,null,{"$f":"(CT238-CS238)/6","v":0},"normal"]
["BC026a","BC526a",null,{"$f":"VLOOKUP(Data!A239,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of electricity input 1, process 1"},{"$f":"VLOOKUP(Data!A239,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/MJoutput"},{"$f":"F240*3600/((F220*F181)+0.001)","v":0},0,0,0,"normal",{"$f":"K240*3600/((K220*K181)+0.001)","v":0},0,0,0,"normal",null,null,null,null,null,{"$f":"U240*3600/((U220*U181)+0.001)","v":6.3535251401316051E-2},0,0,0,"normal",{"$f":"Z240*3600/((Z220*Z181)+0.001)","v":0},0,0,0,"normal",{"$f":"AE240*3600/((AE220*AE181)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"AY240*3600/((AY220*AY181)+0.001)","v":6.3535251401316051E-2},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC240*3600/((CC220*CC181)+0.001)","v":6.6544028520288234E-2},null,null,0,"normal",{"$f":"CH240*3600/((CH220*CH181)+0.001)","v":8.7540707263334613E-3},null,null,0,"normal",{"$f":"CM240*3600/((CM220*CM181)+0.001)","v":0},null,null,0,"normal",{"$f":"CR240*3600/((CR220*CR181)+0.001)","v":6.3535251401316051E-2},null,null,0,"normal"]
["BC026a0","BC526a0",null,{"$f":"VLOOKUP(Data!A240,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity flow 1, process 1"},{"$f":"VLOOKUP(Data!A240,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MWh/year"},0,0,0,{"$f":"(H240-G240)/6","v":0},"normal",0,0,0,{"$f":"(M240-L240)/6","v":0},"normal",null,null,null,null,null,2400,0,0,{"$f":"(W240-V240)/6","v":0},"normal",0,0,0,{"$f":"(AB240-AA240)/6","v":0},"normal",0,0,0,{"$f":"(AG240-AF240)/6","v":0},"normal",null,null,null,{"$f":"(AL240-AK240)/6","v":0},"normal",null,null,null,{"$f":"(AQ240-AP240)/6","v":0},"normal",null,null,null,{"$f":"(AV240-AU240)/6","v":0},"normal",2400,null,null,{"$f":"(BA240-AZ240)/6","v":0},"normal",null,null,null,{"$f":"(BF240-BE240)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,5833,null,null,{"$f":"(CE240-CD240)/6","v":0},"normal",466,null,null,{"$f":"(CJ240-CI240)/6","v":0},"normal",0,null,null,{"$f":"(CO240-CN240)/6","v":0},"normal",2400,null,null,{"$f":"(CT240-CS240)/6","v":0},"normal"]
["BC026a1","BC526a1",null,{"$f":"VLOOKUP(Data!A241,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of electricity input 2, process 1"},{"$f":"VLOOKUP(Data!A241,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/MJoutput"},{"$f":"F242*3600/((F220*F181)+0.001)","v":0},0,0,{"$f":"(H241-G241)/6","v":0},"normal",{"$f":"K242*3600/((K220*K181)+0.001)","v":0},0,0,{"$f":"(M241-L241)/6","v":0},"normal",null,null,null,null,null,{"$f":"U242*3600/((U220*U181)+0.001)","v":0},0,0,{"$f":"(W241-V241)/6","v":0},"normal",{"$f":"Z242*3600/((Z220*Z181)+0.001)","v":0},0,0,{"$f":"(AB241-AA241)/6","v":0},"normal",{"$f":"AE242*3600/((AE220*AE181)+0.001)","v":0},0,0,{"$f":"(AG241-AF241)/6","v":0},"normal",null,null,null,{"$f":"(AL241-AK241)/6","v":0},"normal",null,null,null,{"$f":"(AQ241-AP241)/6","v":0},"normal",null,null,null,{"$f":"(AV241-AU241)/6","v":0},"normal",{"$f":"AY242*3600/((AY220*AY181)+0.001)","v":0},null,null,{"$f":"(BA241-AZ241)/6","v":0},"normal",null,null,null,{"$f":"(BF241-BE241)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC242*3600/((CC220*CC181)+0.001)","v":0},null,null,{"$f":"(CE241-CD241)/6","v":0},"normal",{"$f":"CH242*3600/((CH220*CH181)+0.001)","v":0},null,null,{"$f":"(CJ241-CI241)/6","v":0},"normal",{"$f":"CM242*3600/((CM220*CM181)+0.001)","v":0},null,null,{"$f":"(CO241-CN241)/6","v":0},"normal",{"$f":"CR242*3600/((CR220*CR181)+0.001)","v":0},null,null,0,"normal"]
["BC026a10","BC526a10",null,{"$f":"VLOOKUP(Data!A242,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity flow 2, process 1"},{"$f":"VLOOKUP(Data!A242,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MWh/year"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,{"$f":"(CT242-CS242)/6","v":0},"normal"]
["BC026b","BC526b",null,{"$f":"VLOOKUP(Data!A243,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of electricity input 1, process 2"},{"$f":"VLOOKUP(Data!A243,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/MJoutput"},{"$f":"F244*3600/((F224*F182)+0.001)","v":5.9972952198558455E-4},0,0,0,"normal",{"$f":"K244*3600/((K224*K182)+0.001)","v":5.9972952198558455E-4},0,0,0,"normal",null,null,null,null,null,{"$f":"U244*3600/((U224*U182)+0.001)","v":0.17925850129059345},0,0,0,"normal",{"$f":"Z244*3600/((Z224*Z182)+0.001)","v":0},0,0,0,"normal",{"$f":"AE244*3600/((AE224*AE182)+0.001)","v":0},0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",{"$f":"AY244*3600/((AY224*AY182)+0.001)","v":9.8592175711206279E-2},null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC244*3600/((CC224*CC182)+0.001)","v":6.1926012715670317E-2},null,null,0,"normal",{"$f":"CH244*3600/((CH224*CH182)+0.001)","v":0},null,null,0,"normal",{"$f":"CM244*3600/((CM224*CM182)+0.001)","v":0},null,null,0,"normal",{"$f":"CR244*3600/((CR224*CR182)+0.001)","v":9.8592175711206279E-2},null,null,0,"normal"]
["BC026b0","BC526b0",null,{"$f":"VLOOKUP(Data!A244,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity flow 1, process 2"},{"$f":"VLOOKUP(Data!A244,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MWh/year"},8.5000000000000006E-3,0,0,{"$f":"(H244-G244)/6","v":0},"normal",8.5000000000000006E-3,0,0,{"$f":"(M244-L244)/6","v":0},"normal",null,null,null,null,null,1601,0,0,{"$f":"(W244-V244)/6","v":0},"normal",0,0,0,{"$f":"(AB244-AA244)/6","v":0},"normal",0,0,0,{"$f":"(AG244-AF244)/6","v":0},"normal",null,null,null,{"$f":"(AL244-AK244)/6","v":0},"normal",null,null,null,{"$f":"(AQ244-AP244)/6","v":0},"normal",null,null,null,{"$f":"(AV244-AU244)/6","v":0},"normal",1601,null,null,{"$f":"(BA244-AZ244)/6","v":0},"normal",null,null,null,{"$f":"(BF244-BE244)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2995,null,null,{"$f":"(CE244-CD244)/6","v":0},"normal",0,null,null,{"$f":"(CJ244-CI244)/6","v":0},"normal",0,null,null,{"$f":"(CO244-CN244)/6","v":0},"normal",1601,null,null,{"$f":"(CT244-CS244)/6","v":0},"normal"]
["BC026b1","BC526b1",null,{"$f":"VLOOKUP(Data!A245,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Amount of electricity input 2, process 2"},{"$f":"VLOOKUP(Data!A245,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/MJoutput"},{"$f":"F246*3600/((F224*F182)+0.001)","v":0},0,0,{"$f":"(H245-G245)/6","v":0},"normal",{"$f":"K246*3600/((K224*K182)+0.001)","v":0},0,0,{"$f":"(M245-L245)/6","v":0},"normal",null,null,null,null,null,{"$f":"U246*3600/((U224*U182)+0.001)","v":0},0,0,{"$f":"(W245-V245)/6","v":0},"normal",{"$f":"Z246*3600/((Z224*Z182)+0.001)","v":0},0,0,{"$f":"(AB245-AA245)/6","v":0},"normal",{"$f":"AE246*3600/((AE224*AE182)+0.001)","v":0},0,0,{"$f":"(AG245-AF245)/6","v":0},"normal",null,null,null,{"$f":"(AL245-AK245)/6","v":0},"normal",null,null,null,{"$f":"(AQ245-AP245)/6","v":0},"normal",null,null,null,{"$f":"(AV245-AU245)/6","v":0},"normal",{"$f":"AY246*3600/((AY224*AY182)+0.001)","v":0},null,null,{"$f":"(BA245-AZ245)/6","v":0},"normal",null,null,null,{"$f":"(BF245-BE245)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"CC246*3600/((CC224*CC182)+0.001)","v":0},null,null,{"$f":"(CE245-CD245)/6","v":0},"normal",{"$f":"CH246*3600/((CH224*CH182)+0.001)","v":0},null,null,{"$f":"(CJ245-CI245)/6","v":0},"normal",{"$f":"CM246*3600/((CM224*CM182)+0.001)","v":0},null,null,{"$f":"(CO245-CN245)/6","v":0},"normal",{"$f":"CR246*3600/((CR224*CR182)+0.001)","v":0},null,null,0,"normal"]
["BC026b10","BC526b10",null,{"$f":"VLOOKUP(Data!A246,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity flow 2, process 2"},{"$f":"VLOOKUP(Data!A246,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MWh/year"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,{"$f":"(CT246-CS246)/6","v":0},"normal"]
["BC027a","BC527a",null,{"$f":"VLOOKUP(Data!A247,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of electricity flow 1, process 1"},{"$f":"VLOOKUP(Data!A247,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"Electricity from landfill gas CHP",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Electricity from wood boiler CHP",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Electricity from pyrolysis",null,null,"n.a.","n.a.","Electricity from pyrolysis",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Electricity from wood boiler CHP",null,null,"n.a.","n.a."]
["BC027a1","BC527a1",null,{"$f":"VLOOKUP(Data!A248,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of electricity flow 2, process 1"},{"$f":"VLOOKUP(Data!A248,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC027b","BC527b",null,{"$f":"VLOOKUP(Data!A249,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of electricity flow 1, process 2"},{"$f":"VLOOKUP(Data!A249,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Electricity EU mix LV",null,null,"n.a.","n.a.","Electricity EU mix LV",null,null,"n.a.","n.a.",null,null,null,null,null,"Electricity from landfill gas CHP",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Electricity from wood boiler CHP",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Electricity from pyrolysis",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Electricity from wood boiler CHP",null,null,"n.a.","n.a."]
["BC027b1","BC527b1",null,{"$f":"VLOOKUP(Data!A250,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Type of electricity flow 2, process 2"},{"$f":"VLOOKUP(Data!A250,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC060","BC560",null,{"$f":"VLOOKUP(Data!A251,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Heat energy use for treatment 2 (storage)"},{"$f":"VLOOKUP(Data!A251,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJh/MJinput"},0,0,0,{"$f":"(H251-G251)/6","v":0},"normal",0,0,0,{"$f":"(M251-L251)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W251-V251)/6","v":0},"normal",0,0,0,{"$f":"(AB251-AA251)/6","v":0},"normal",0,0,0,{"$f":"(AG251-AF251)/6","v":0},"normal",null,null,null,{"$f":"(AL251-AK251)/6","v":0},"normal",null,null,null,{"$f":"(AQ251-AP251)/6","v":0},"normal",null,null,null,{"$f":"(AV251-AU251)/6","v":0},"normal",0,null,null,{"$f":"(BA251-AZ251)/6","v":0},"normal",null,null,null,{"$f":"(BF251-BE251)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE251-CD251)/6","v":0},"normal",0,null,null,{"$f":"(CJ251-CI251)/6","v":0},"normal",0,null,null,{"$f":"(CO251-CN251)/6","v":0},"normal",0,null,null,{"$f":"(CT251-CS251)/6","v":0},"normal"]
["BC061","BC561",null,{"$f":"VLOOKUP(Data!A252,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Heat source for treatment 2 (storage)"},{"$f":"VLOOKUP(Data!A252,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC065","BC565",null,{"$f":"VLOOKUP(Data!A253,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity energy use for treatment 2 (storage)"},{"$f":"VLOOKUP(Data!A253,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/MJinput"},8.4000000000000003E-4,0,1E-3,{"$f":"(H253-G253)/6","v":1.6666666666666666E-4},"normal",8.4000000000000003E-4,0,1E-3,{"$f":"(M253-L253)/6","v":1.6666666666666666E-4},"normal",null,null,null,null,null,0,0,0,{"$f":"(W253-V253)/6","v":0},"normal",0,0,0,{"$f":"(AB253-AA253)/6","v":0},"normal",0,0,0,{"$f":"(AG253-AF253)/6","v":0},"normal",null,null,null,{"$f":"(AL253-AK253)/6","v":0},"normal",null,null,null,{"$f":"(AQ253-AP253)/6","v":0},"normal",null,null,null,{"$f":"(AV253-AU253)/6","v":0},"normal",0,null,null,{"$f":"(BA253-AZ253)/6","v":0},"normal",null,null,null,{"$f":"(BF253-BE253)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE253-CD253)/6","v":0},"normal",0,null,null,{"$f":"(CJ253-CI253)/6","v":0},"normal",0,null,null,{"$f":"(CO253-CN253)/6","v":0},"normal",0,null,null,{"$f":"(CT253-CS253)/6","v":0},"normal"]
["BC066","BC566",null,{"$f":"VLOOKUP(Data!A254,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity source for treatment 2 (storage)"},{"$f":"VLOOKUP(Data!A254,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC070","BC570",null,{"$f":"VLOOKUP(Data!A255,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Heat energy use for treatment 3 (storage)"},{"$f":"VLOOKUP(Data!A255,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJh/MJinput"},0,0,0,{"$f":"(H255-G255)/6","v":0},"normal",0,0,0,{"$f":"(M255-L255)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W255-V255)/6","v":0},"normal",0,0,0,{"$f":"(AB255-AA255)/6","v":0},"normal",0,0,0,{"$f":"(AG255-AF255)/6","v":0},"normal",null,null,null,{"$f":"(AL255-AK255)/6","v":0},"normal",null,null,null,{"$f":"(AQ255-AP255)/6","v":0},"normal",null,null,null,{"$f":"(AV255-AU255)/6","v":0},"normal",0,null,null,{"$f":"(BA255-AZ255)/6","v":0},"normal",null,null,null,{"$f":"(BF255-BE255)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE255-CD255)/6","v":0},"normal",0,null,null,{"$f":"(CJ255-CI255)/6","v":0},"normal",0,null,null,{"$f":"(CO255-CN255)/6","v":0},"normal",0,null,null,{"$f":"(CT255-CS255)/6","v":0},"normal"]
["BC071","BC571",null,{"$f":"VLOOKUP(Data!A256,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Heat source for treatment 3 (storage)"},{"$f":"VLOOKUP(Data!A256,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC075","BC575",null,{"$f":"VLOOKUP(Data!A257,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity energy use for treatment 3 (storage)"},{"$f":"VLOOKUP(Data!A257,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"MJe/MJinput"},8.4000000000000003E-4,0,1E-3,{"$f":"(H257-G257)/6","v":1.6666666666666666E-4},"normal",8.4000000000000003E-4,0,1E-3,{"$f":"(M257-L257)/6","v":1.6666666666666666E-4},"normal",null,null,null,null,null,0,0,0,{"$f":"(W257-V257)/6","v":0},"normal",0,0,0,{"$f":"(AB257-AA257)/6","v":0},"normal",0,0,0,{"$f":"(AG257-AF257)/6","v":0},"normal",null,null,null,{"$f":"(AL257-AK257)/6","v":0},"normal",null,null,null,{"$f":"(AQ257-AP257)/6","v":0},"normal",null,null,null,{"$f":"(AV257-AU257)/6","v":0},"normal",0,null,null,{"$f":"(BA257-AZ257)/6","v":0},"normal",null,null,null,{"$f":"(BF257-BE257)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE257-CD257)/6","v":0},"normal",0,null,null,{"$f":"(CJ257-CI257)/6","v":0},"normal",0,null,null,{"$f":"(CO257-CN257)/6","v":0},"normal",0,null,null,{"$f":"(CT257-CS257)/6","v":0},"normal"]
["BC076","BC576",null,{"$f":"VLOOKUP(Data!A258,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Electricity source for treatment 3 (storage)"},{"$f":"VLOOKUP(Data!A258,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a."]
["BC016a","BC516a",null,{"$f":"VLOOKUP(Data!A259,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 1"},{"$f":"VLOOKUP(Data!A259,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gNOX/MJoutput"},0,0,0,{"$f":"(H259-G259)/6","v":0},"normal",0,0,0,{"$f":"(M259-L259)/6","v":0},"normal",null,null,null,null,null,0,0,0,{"$f":"(W259-V259)/6","v":0},"normal",0,0,0,{"$f":"(AB259-AA259)/6","v":0},"normal",0,0,0,{"$f":"(AG259-AF259)/6","v":0},"normal",null,null,null,{"$f":"(AL259-AK259)/6","v":0},"normal",null,null,null,{"$f":"(AQ259-AP259)/6","v":0},"normal",null,null,null,{"$f":"(AV259-AU259)/6","v":0},"normal",0,null,null,{"$f":"(BA259-AZ259)/6","v":0},"normal",null,null,null,{"$f":"(BF259-BE259)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,{"$f":"(CE259-CD259)/6","v":0},"normal",0,null,null,{"$f":"(CJ259-CI259)/6","v":0},"normal",0,null,null,{"$f":"(CO259-CN259)/6","v":0},"normal",0,null,null,{"$f":"(CT259-CS259)/6","v":0},"normal"]
["BC016b","BC516b",null,{"$f":"VLOOKUP(Data!A260,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 1"},{"$f":"VLOOKUP(Data!A260,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gSOX/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC016c","BC516c",null,{"$f":"VLOOKUP(Data!A261,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 1"},{"$f":"VLOOKUP(Data!A261,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gNH3/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,5,15,1.6666666666666667,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC016d","BC516d",null,{"$f":"VLOOKUP(Data!A262,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 1"},{"$f":"VLOOKUP(Data!A262,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gNO3/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,5,15,1.6666666666666667,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC016e","BC516e",null,{"$f":"VLOOKUP(Data!A263,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 1"},{"$f":"VLOOKUP(Data!A263,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gNH4/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC016f","BC516f",null,{"$f":"VLOOKUP(Data!A264,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 1"},{"$f":"VLOOKUP(Data!A264,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gPO4/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC016g","BC516g",null,{"$f":"VLOOKUP(Data!A265,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 1"},{"$f":"VLOOKUP(Data!A265,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gCOD/MJoutput"},20,15,25,1.6666666666666667,"normal",20,15,25,1.6666666666666667,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC017a","BC517a",null,{"$f":"VLOOKUP(Data!A266,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 2"},{"$f":"VLOOKUP(Data!A266,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gNOX/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC017b","BC517b",null,{"$f":"VLOOKUP(Data!A267,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 2"},{"$f":"VLOOKUP(Data!A267,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gSOX/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC017c","BC517c",null,{"$f":"VLOOKUP(Data!A268,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 2"},{"$f":"VLOOKUP(Data!A268,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gNH3/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC017d","BC517d",null,{"$f":"VLOOKUP(Data!A269,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 2"},{"$f":"VLOOKUP(Data!A269,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gNO3/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC017e","BC517e",null,{"$f":"VLOOKUP(Data!A270,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 2"},{"$f":"VLOOKUP(Data!A270,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gNH4/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC017f","BC517f",null,{"$f":"VLOOKUP(Data!A271,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 2"},{"$f":"VLOOKUP(Data!A271,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gPO4/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC017g","BC517g",null,{"$f":"VLOOKUP(Data!A272,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 2"},{"$f":"VLOOKUP(Data!A272,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"gCOD/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC100a","BC600a",null,{"$f":"VLOOKUP(Data!A273,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Water use for conversion process 1"},{"$f":"VLOOKUP(Data!A273,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"m³/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC101a","BC601a",null,{"$f":"VLOOKUP(Data!A274,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},{"$f":"VLOOKUP(Data!A274,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"m³/MJinput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC102a","BC602a",null,{"$f":"VLOOKUP(Data!A275,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Water use for conversion process 2"},{"$f":"VLOOKUP(Data!A275,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"m³/MJoutput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC103a","BC603a",null,{"$f":"VLOOKUP(Data!A276,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},{"$f":"VLOOKUP(Data!A276,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"m³/MJinput"},0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,null,null,0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal",0,null,null,0,"normal"]
["BC150a","BC650a",null,{"$f":"VLOOKUP(Data!A277,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No forced labour, process 1"},{"$f":"VLOOKUP(Data!A277,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC150b","BC650b",null,{"$f":"VLOOKUP(Data!A278,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No child labour, process 1"},{"$f":"VLOOKUP(Data!A278,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC150c","BC650c",null,{"$f":"VLOOKUP(Data!A279,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Good social practices regarding human rights, process 1"},{"$f":"VLOOKUP(Data!A279,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC150d","BC650d",null,{"$f":"VLOOKUP(Data!A280,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No discrimination, process 1"},{"$f":"VLOOKUP(Data!A280,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC150f","BC650f",null,{"$f":"VLOOKUP(Data!A281,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 1"},{"$f":"VLOOKUP(Data!A281,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC151a","BC651a",null,{"$f":"VLOOKUP(Data!A282,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fair legal contracts, process 1"},{"$f":"VLOOKUP(Data!A282,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC151b","BC651b",null,{"$f":"VLOOKUP(Data!A283,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Workers rights, process 1"},{"$f":"VLOOKUP(Data!A283,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC151c","BC651c",null,{"$f":"VLOOKUP(Data!A284,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 1"},{"$f":"VLOOKUP(Data!A284,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC151d","BC651d",null,{"$f":"VLOOKUP(Data!A285,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fair wages and compensation rules, process 1"},{"$f":"VLOOKUP(Data!A285,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC151e","BC651e",null,{"$f":"VLOOKUP(Data!A286,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Health, safety and hygiene policy, process 1"},{"$f":"VLOOKUP(Data!A286,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC151f","BC651f",null,{"$f":"VLOOKUP(Data!A287,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 1"},{"$f":"VLOOKUP(Data!A287,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC151g","BC651g",null,{"$f":"VLOOKUP(Data!A288,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Health and safety training, process 1"},{"$f":"VLOOKUP(Data!A288,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC152a","BC652a",null,{"$f":"VLOOKUP(Data!A289,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No forced labour, process 2"},{"$f":"VLOOKUP(Data!A289,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC152b","BC652b",null,{"$f":"VLOOKUP(Data!A290,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No child labour, process 2"},{"$f":"VLOOKUP(Data!A290,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC152c","BC652c",null,{"$f":"VLOOKUP(Data!A291,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Good social practices regarding human rights, process 2"},{"$f":"VLOOKUP(Data!A291,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC152d","BC652d",null,{"$f":"VLOOKUP(Data!A292,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"No discrimination, process 2"},{"$f":"VLOOKUP(Data!A292,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC152f","BC652f",null,{"$f":"VLOOKUP(Data!A293,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 2"},{"$f":"VLOOKUP(Data!A293,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC153a","BC653a",null,{"$f":"VLOOKUP(Data!A294,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fair legal contracts, process 2"},{"$f":"VLOOKUP(Data!A294,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC153b","BC653b",null,{"$f":"VLOOKUP(Data!A295,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Workers rights, process 2"},{"$f":"VLOOKUP(Data!A295,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC153c","BC653c",null,{"$f":"VLOOKUP(Data!A296,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 2"},{"$f":"VLOOKUP(Data!A296,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC153d","BC653d",null,{"$f":"VLOOKUP(Data!A297,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Fair wages and compensation rules, process 2"},{"$f":"VLOOKUP(Data!A297,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC153e","BC653e",null,{"$f":"VLOOKUP(Data!A298,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Health, safety and hygiene policy, process 2"},{"$f":"VLOOKUP(Data!A298,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC153f","BC653f",null,{"$f":"VLOOKUP(Data!A299,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 2"},{"$f":"VLOOKUP(Data!A299,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
["BC153g","BC653g",null,{"$f":"VLOOKUP(Data!A300,'ID-numbers'!A$2:B$1640,2,FALSE)","v":"Health and safety training, process 2"},{"$f":"VLOOKUP(Data!A300,'ID-numbers'!A$2:C$1640,3,FALSE)","v":"-"},"Not fulfilled",null,null,"n.a.","n.a.","Not fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a."]
[]
["FC000",null,null,{"$f":"VLOOKUP(Data!A302,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Final conversion process"},{"$f":"VLOOKUP(Data!A302,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","CHP - biogas",null,null,"n.a.","n.a.","CHP - pure plant oil",null,null,"n.a.","n.a.","CHP - dual fuel",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","No final conversion",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC030",null,null,{"$f":"VLOOKUP(Data!A303,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Functional unit"},{"$f":"VLOOKUP(Data!A303,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","MJ heat",null,null,"n.a.","n.a.","MJ heat",null,null,"n.a.","n.a.","MJ heat",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","MJ biogas",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC001a",null,null,{"$f":"VLOOKUP(Data!A304,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Type of input flow, feedstock 1"},{"$f":"VLOOKUP(Data!A304,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Purified biogas (55% CH4)",null,null,"n.a.","n.a.","Palm stearin",null,null,"n.a.","n.a.","Palm stearin",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Liquid biomethane (LBM)",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC001b",null,null,{"$f":"VLOOKUP(Data!A305,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Type of input flow, feedstock 2"},{"$f":"VLOOKUP(Data!A305,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","Purified biogas (55% CH4)",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC002a",null,null,{"$f":"VLOOKUP(Data!A306,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Share of input flow 1 (caloric)"},{"$f":"VLOOKUP(Data!A306,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"%"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,{"$f":"(AG306-AF306)/6","v":0},"normal",100,null,null,"n.a.","n.a.",100,null,null,"n.a.","n.a.",28.78,null,null,"n.a.","n.a.",null,null,null,{"$f":"(BA306-AZ306)/6","v":0},"normal",100,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CE306-CD306)/6","v":0},"normal",null,null,null,{"$f":"(CJ306-CI306)/6","v":0},"normal",null,null,null,{"$f":"(CO306-CN306)/6","v":0},"normal",null,null,null,{"$f":"(CT306-CS306)/6","v":0},"normal"]
["FC002b",null,null,{"$f":"VLOOKUP(Data!A307,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Share of input flow 2 (caloric)"},{"$f":"VLOOKUP(Data!A307,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"%"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,0,"normal",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",71.22,null,null,"n.a.","n.a.",null,null,null,0,"normal",0,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC003a",null,null,{"$f":"VLOOKUP(Data!A308,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Net electrical efficiency, final conversion"},{"$f":"VLOOKUP(Data!A308,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"%"},null,null,null,{"$f":"(H308-G308)/6","v":0},"normal",null,null,null,{"$f":"(M308-L308)/6","v":0},"normal",null,null,null,null,null,null,null,null,{"$f":"(W308-V308)/6","v":0},"normal",null,null,null,{"$f":"(AB308-AA308)/6","v":0},"normal",null,null,null,0,"normal",38,24,32,{"$f":"(AL308-AK308)/6","v":1.3333333333333333},"normal",34,32,36,{"$f":"(AQ308-AP308)/6","v":0.66666666666666663},"normal",29,24,32,{"$f":"(AV308-AU308)/6","v":1.3333333333333333},"normal",null,null,null,0,"normal",0,0,0,{"$f":"(BF308-BE308)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC003b",null,null,{"$f":"VLOOKUP(Data!A309,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Net thermal efficiency, final conversion"},{"$f":"VLOOKUP(Data!A309,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"%"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",40,22,28,1,"normal",37,33,39,1,"normal",25,22,28,1,"normal",null,null,null,0,"normal",0,0,0,{"$f":"(BF309-BE309)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC003c",null,null,{"$f":"VLOOKUP(Data!A310,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Net conversion efficiency, final conversion - other than electricity or heat"},{"$f":"VLOOKUP(Data!A310,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"%"},null,null,null,{"$f":"(H310-G310)/6","v":0},"normal",null,null,null,{"$f":"(M310-L310)/6","v":0},"normal",null,null,null,null,null,null,null,null,{"$f":"(W310-V310)/6","v":0},"normal",null,null,null,{"$f":"(AB310-AA310)/6","v":0},"normal",null,null,null,{"$f":"(AG310-AF310)/6","v":0},"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,{"$f":"(BA310-AZ310)/6","v":0},"normal",100,0,0,{"$f":"(BF310-BE310)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC037a",null,null,{"$f":"VLOOKUP(Data!A311,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Gross electrical efficiency, final conversion"},{"$f":"VLOOKUP(Data!A311,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"%"},null,null,null,{"$f":"(H311-G311)/6","v":0},"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",38,37,42,0.83333333333333337,"normal",39,37,42,{"$f":"(AQ311-AP311)/6","v":0.83333333333333337},"normal",39,37,42,0.83333333333333337,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC037b",null,null,{"$f":"VLOOKUP(Data!A312,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Gross thermal efficiency, final conversion"},{"$f":"VLOOKUP(Data!A312,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"%"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",40,38,42,0.66666666666666663,"normal",40,38,42,0.66666666666666663,"normal",40,38,42,0.66666666666666663,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC038",null,null,{"$f":"VLOOKUP(Data!A313,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Temperature of useful heat"},{"$f":"VLOOKUP(Data!A313,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"°C"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",95,90,100,1.6666666666666667,"normal",95,90,100,1.6666666666666667,"normal",95,90,100,1.6666666666666667,"normal",null,null,null,0,"normal","n.a.",0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC004a",null,null,{"$f":"VLOOKUP(Data!A314,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Type of by-product 1, final conversion"},{"$f":"VLOOKUP(Data!A314,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC004b",null,null,{"$f":"VLOOKUP(Data!A315,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Type of by-product 2, final conversion"},{"$f":"VLOOKUP(Data!A315,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC005a",null,null,{"$f":"VLOOKUP(Data!A316,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Extraction rate of by-product 1, final conversion (kg)"},{"$f":"VLOOKUP(Data!A316,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"kgbyproduct /kginput"},null,null,null,{"$f":"(H316-G316)/6","v":0},"normal",null,null,null,{"$f":"(M316-L316)/6","v":0},"normal",null,null,null,null,null,null,null,null,{"$f":"(W316-V316)/6","v":0},"normal",null,null,null,{"$f":"(AB316-AA316)/6","v":0},"normal",null,null,null,{"$f":"(AG316-AF316)/6","v":0},"normal",0,0,0,{"$f":"(AL316-AK316)/6","v":0},"normal",0,0,0,{"$f":"(AQ316-AP316)/6","v":0},"normal",0,0,0,{"$f":"(AV316-AU316)/6","v":0},"normal",null,null,null,{"$f":"(BA316-AZ316)/6","v":0},"normal",0,0,0,{"$f":"(BF316-BE316)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CE316-CD316)/6","v":0},"normal",null,null,null,{"$f":"(CJ316-CI316)/6","v":0},"normal",null,null,null,{"$f":"(CO316-CN316)/6","v":0},"normal",null,null,null,{"$f":"(CT316-CS316)/6","v":0},"normal"]
["FC005b",null,null,{"$f":"VLOOKUP(Data!A317,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Extraction rate of by-product 2, final conversion (kg)"},{"$f":"VLOOKUP(Data!A317,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"kgbyproduct /kginput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,{"$f":"(AV317-AU317)/6","v":0},"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC006a",null,null,{"$f":"VLOOKUP(Data!A318,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Extraction rate of by-product 1, final conversion (MJ)"},{"$f":"VLOOKUP(Data!A318,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"MJbyproduct /MJinput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC006b",null,null,{"$f":"VLOOKUP(Data!A319,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Extraction rate of by-product 2, final conversion (MJ)"},{"$f":"VLOOKUP(Data!A319,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"MJbyproduct /MJinput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC008a",null,null,{"$f":"VLOOKUP(Data!A320,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Valorisation of by-product 1, final conversion"},{"$f":"VLOOKUP(Data!A320,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"binary"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC008b",null,null,{"$f":"VLOOKUP(Data!A321,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Valorisation of by-product 2, final conversion"},{"$f":"VLOOKUP(Data!A321,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"binary"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",0,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC009a",null,null,{"$f":"VLOOKUP(Data!A322,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Type of material input flow 1, final conversion"},{"$f":"VLOOKUP(Data!A322,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC009b",null,null,{"$f":"VLOOKUP(Data!A323,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Type of material input flow 2, final conversion"},{"$f":"VLOOKUP(Data!A323,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC010a",null,null,{"$f":"VLOOKUP(Data!A324,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Amount of material input flow 1, final conversion"},{"$f":"VLOOKUP(Data!A324,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"kg/MJinput"},null,null,null,{"$f":"(H324-G324)/6","v":0},"normal",null,null,null,{"$f":"(M324-L324)/6","v":0},"normal",null,null,null,null,null,null,null,null,{"$f":"(W324-V324)/6","v":0},"normal",null,null,null,{"$f":"(AB324-AA324)/6","v":0},"normal",null,null,null,{"$f":"(AG324-AF324)/6","v":0},"normal",0,0,0,{"$f":"(AL324-AK324)/6","v":0},"normal",0,0,0,{"$f":"(AQ324-AP324)/6","v":0},"normal",0,0,0,{"$f":"(AV324-AU324)/6","v":0},"normal",null,null,null,{"$f":"(BA324-AZ324)/6","v":0},"normal",0,0,0,{"$f":"(BF324-BE324)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CE324-CD324)/6","v":0},"normal",null,null,null,{"$f":"(CJ324-CI324)/6","v":0},"normal",null,null,null,{"$f":"(CO324-CN324)/6","v":0},"normal",null,null,null,{"$f":"(CT324-CS324)/6","v":0},"normal"]
["FC010b",null,null,{"$f":"VLOOKUP(Data!A325,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Amount of material input flow 2, final conversion"},{"$f":"VLOOKUP(Data!A325,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"kg/MJinput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC011a",null,null,{"$f":"VLOOKUP(Data!A326,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Type of fuel/heat flow 1, final conversion"},{"$f":"VLOOKUP(Data!A326,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC011b",null,null,{"$f":"VLOOKUP(Data!A327,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Type of fuel/heat flow 2, final conversion"},{"$f":"VLOOKUP(Data!A327,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC012a",null,null,{"$f":"VLOOKUP(Data!A328,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Amount of fuel/heat flow 1, final conversion"},{"$f":"VLOOKUP(Data!A328,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"MJf_h/MJinput"},null,null,null,{"$f":"(H328-G328)/6","v":0},"normal",null,null,null,{"$f":"(M328-L328)/6","v":0},"normal",null,null,null,null,null,null,null,null,{"$f":"(W328-V328)/6","v":0},"normal",null,null,null,{"$f":"(AB328-AA328)/6","v":0},"normal",null,null,null,{"$f":"(AG328-AF328)/6","v":0},"normal",0,0,0,{"$f":"(AL328-AK328)/6","v":0},"normal",0,0,0,{"$f":"(AQ328-AP328)/6","v":0},"normal",0,0,0,{"$f":"(AV328-AU328)/6","v":0},"normal",null,null,null,{"$f":"(BA328-AZ328)/6","v":0},"normal",0,0,0,{"$f":"(BF328-BE328)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CE328-CD328)/6","v":0},"normal",null,null,null,{"$f":"(CJ328-CI328)/6","v":0},"normal",null,null,null,{"$f":"(CO328-CN328)/6","v":0},"normal",null,null,null,{"$f":"(CT328-CS328)/6","v":0},"normal"]
["FC012b",null,null,{"$f":"VLOOKUP(Data!A329,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Amount of fuel/heat flow 2, final conversion"},{"$f":"VLOOKUP(Data!A329,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"MJf_h/MJinput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC013",null,null,{"$f":"VLOOKUP(Data!A330,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Net amount of electricity input, final conversion"},{"$f":"VLOOKUP(Data!A330,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"MJe/MJinput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC014",null,null,{"$f":"VLOOKUP(Data!A331,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Electricity source, final conversion"},{"$f":"VLOOKUP(Data!A331,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","n.a.",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC028a",null,null,{"$f":"VLOOKUP(Data!A332,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"NOX emissions to air (not from material/energy input), final conversion"},{"$f":"VLOOKUP(Data!A332,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"gNOX/MJoutput"},null,null,null,{"$f":"(H332-G332)/6","v":0},"normal",null,null,null,{"$f":"(M332-L332)/6","v":0},"normal",null,null,null,null,null,null,null,null,{"$f":"(W332-V332)/6","v":0},"normal",null,null,null,{"$f":"(AB332-AA332)/6","v":0},"normal",null,null,null,{"$f":"(AG332-AF332)/6","v":0},"normal",0,0,0,{"$f":"(AL332-AK332)/6","v":0},"normal",0,0,0,{"$f":"(AQ332-AP332)/6","v":0},"normal",0,0,0,0,"normal",null,null,null,{"$f":"(BA332-AZ332)/6","v":0},"normal",0,0,0,{"$f":"(BF332-BE332)/6","v":0},"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"(CE332-CD332)/6","v":0},"normal",null,null,null,{"$f":"(CJ332-CI332)/6","v":0},"normal",null,null,null,{"$f":"(CO332-CN332)/6","v":0},"normal",null,null,null,{"$f":"(CT332-CS332)/6","v":0},"normal"]
["FC028b",null,null,{"$f":"VLOOKUP(Data!A333,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"SOX emissions to air (not from material/energy input), final conversion"},{"$f":"VLOOKUP(Data!A333,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"gSOX/MJoutput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC028c",null,null,{"$f":"VLOOKUP(Data!A334,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), final conversion"},{"$f":"VLOOKUP(Data!A334,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"gNH3/MJoutput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC028d",null,null,{"$f":"VLOOKUP(Data!A335,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), final conversion"},{"$f":"VLOOKUP(Data!A335,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"gNO3/MJoutput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC028e",null,null,{"$f":"VLOOKUP(Data!A336,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), final conversion"},{"$f":"VLOOKUP(Data!A336,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"gNH4/MJoutput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC028f",null,null,{"$f":"VLOOKUP(Data!A337,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), final conversion"},{"$f":"VLOOKUP(Data!A337,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"gPO4/MJoutput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC028g",null,null,{"$f":"VLOOKUP(Data!A338,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"COD emissions to water (not from material/energy input), final conversion"},{"$f":"VLOOKUP(Data!A338,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"gCOD/MJoutput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC058a",null,null,{"$f":"VLOOKUP(Data!A339,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Water use for final conversion process"},{"$f":"VLOOKUP(Data!A339,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"m³/MJinput"},null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",0,0,0,0,"normal",null,null,null,0,"normal",0,0,0,0,"normal",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal",null,null,null,0,"normal"]
["FC080a",null,null,{"$f":"VLOOKUP(Data!A340,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"No forced labour, final conversion"},{"$f":"VLOOKUP(Data!A340,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC080b",null,null,{"$f":"VLOOKUP(Data!A341,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"No child labour, final conversion"},{"$f":"VLOOKUP(Data!A341,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC080c",null,null,{"$f":"VLOOKUP(Data!A342,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Good social practices regarding human rights, final conversion"},{"$f":"VLOOKUP(Data!A342,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC080d",null,null,{"$f":"VLOOKUP(Data!A343,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"No discrimination, final conversion"},{"$f":"VLOOKUP(Data!A343,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC080f",null,null,{"$f":"VLOOKUP(Data!A344,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, final conversion"},{"$f":"VLOOKUP(Data!A344,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC081a",null,null,{"$f":"VLOOKUP(Data!A345,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Fair legal contracts, final conversion"},{"$f":"VLOOKUP(Data!A345,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC081b",null,null,{"$f":"VLOOKUP(Data!A346,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Workers rights, final conversion"},{"$f":"VLOOKUP(Data!A346,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC081c",null,null,{"$f":"VLOOKUP(Data!A347,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, final conversion"},{"$f":"VLOOKUP(Data!A347,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC081d",null,null,{"$f":"VLOOKUP(Data!A348,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Fair wages and compensation rules, final conversion"},{"$f":"VLOOKUP(Data!A348,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC081e",null,null,{"$f":"VLOOKUP(Data!A349,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Health, safety and hygiene policy, final conversion"},{"$f":"VLOOKUP(Data!A349,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC081f",null,null,{"$f":"VLOOKUP(Data!A350,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, final conversion"},{"$f":"VLOOKUP(Data!A350,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]
["FC081g",null,null,{"$f":"VLOOKUP(Data!A351,'ID-numbers'!A$2:B$2139,2,FALSE)","v":"Health and safety training, final conversion"},{"$f":"VLOOKUP(Data!A351,'ID-numbers'!A$2:C$2139,3,FALSE)","v":"-"},null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.","Fulfilled",null,null,"n.a.","n.a.",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a.",null,null,null,"n.a.","n.a."]

{"sheet":"Lists","index":15,"n_rows":55,"n_cols":27,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
["Pathways inserted in database","Pathways feedstock 2","Conversion techniques","Output","Functional Unit","Transport efficiencies","Transport fuels","Electricity","Heat","Heat and fuels","Conversion inputs/outputs","Feedstocks-byproducts","Climate region","Soil type","Land use","Management","Input","Land use_specific","Climate region_specific","Domain","Ecological zone","Continent","Type","Nutrient level","Binary","Yesno","OKnotOK"]
["Palm oil (stearin) from palm fruits, refinery","Palm oil (stearin) from palm fruits, refinery","CHP - gas","Electricity and heat","MJ heat","Truck for dry product (diesel)","Diesel","Electricity EU mix MV","Heat EU mix","Heat EU mix","Manure co- vergister ","Hard coal","Boreal Dry","High Activity Clay Soils","Annual cropland","Full tillage","Low","Sugar cane","Boreal dry","Tropical","Tropical rain forest","Africa","<= 20 y","Nutrient rich",0,"yes","Fulfilled"]
["Palm oil (olein) from palm fruits, refinery","Palm oil (olein) from palm fruits, refinery","CHP - pure plant oil","Electricity","MJ electricity","Truck for liquids (diesel)","Gasoline","Electricity EU mix LV","Heat from NG boiler","Heat from NG boiler","Cattle manure","Lignite","Boreal Moist","Low Activity Clay Soils","Perennial cropland","Reduced tillage","Medium","All other annual crops","Boreal moist","Subtropical","Tropical moist forest","Asia continental","> 20 y","Nutrient poor",1,"no","Not fulfilled"]
["Biogas from organic residues, anaerobic digestion","Biogas from organic residues, anaerobic digestion","CHP - dual fuel (gas + ppo)","Heat","MJ gas","Truck for FFB transport (diesel)","Heavy fuel oil (HFO)","Electricity (NG CCGT)","Heat from NG CHP","Heat from NG CHP","Pig manure","Maize (corn)","Cool Temperate Dry","Sandy Soils","Grassland and savannah","No till","High with manure","Coconut","Cool temperate dry","Temperate","Tropical moist deciduous forest","Asia insular","Broadleaf > 20 y","n.a.",null,null,"Maybe not fulfilled"]
["Biogas from maize + organic residues, anaerobic digestion + purification","Biogas from maize + organic residues, anaerobic digestion + purification","No final conversion, only biofuel production",null,"MJ diesel","Tanker truck MB2218 for vinasse transport","HFO for maritime transport","Electricity (Lignite ST)","Heat from Lignite CHP","Heat from Lignite CHP","Chicken manure","Empty palm fruit bunches","Cool Temperate Moist","Spodic Soils","Native forest non degraded","Improved","High without manure","Jatropha","Cool temperate moist","Boreal","Tropical dry forest","Central and South America","Broadleaf <= 20 y"]
["LBM from GFT, anaerobic digestion + upgrading","LBM from GFT, anaerobic digestion + upgrading",null,null,"MJ heavy fuel oil","Tanker truck with water cannons for vinasse transport","Electricity EU mix MV","Electricity (Straw ST)","Heat from Straw CHP","Heat from Straw CHP","Sheep manure","Filter mud cake","Warm Temperate Dry","Volcanic Soils","Managed forest","Nominally managed","High","Jojoba","Warm temperate dry","n.a.","Tropical shrubland","North America","Broadleaf"]
["LBM from harvested grass, anaerobic digestion + upgrading","LBM from harvested grass, anaerobic digestion + upgrading",null,null,null,"Dumpster truck MB2213 for filter mud transport","Electricity EU mix LV","n.a.","Heat from NG gas engine","Heat from NG gas engine","Agricultural residues","Fresh palm fruit bunches (FFB)","Warm Temperate Moist","Wetland Soils","Shifting cultivation shortened fallow","Moderately degraded","n.a.","Oil palm","Warm temperate moist",null,"Tropical mountain systems","Europe","Coniferous > 20 y"]
["Biodiesel from fatty residues, esterification","Biodiesel from fatty residues, esterification",null,null,null,"Ocean bulk carrier (HFO maritime)","Electricity (NG CCGT)","Electricity from wood boiler CHP","n.a.","Natural gas (4000 km, Russian NG quality)","Organic domestical waste","Fresh palm fruit","Tropical Dry","Organic","Shifting cultivation mature fallow","Severely degraded",null,"All other perennial crops","Tropical dry",null,"Subtropical humid forest","Australia","Coniferous <= 20 y"]
["Bio-oil from wood waste, fast pyrolysis","Bio-oil from wood waste, fast pyrolysis",null,null,null,"Ship /product tanker 50kt (HFO maritime)","Electricity (Lignite ST)","Electricity from pyrolysis","Heat from wood boiler CHP","Natural gas (4000 km, EU Mix qualilty)","Organic residues (general)","Manure co- vergister ","Tropical Moist","Other Areas",null,"n.a.",null,"Grassland and savannah","Tropical moist",null,"Subtropical dry forest","New Zealand","Pinus sp. > 20 y"]
["None","None",null,null,null,"Local (10 km) pipeline","Electricity (Straw ST)","Electricity from landfill gas CHP","Heat from pyrolysis","Methane","Pig manure","Cattle manure","Tropical Wet","n.a. ",null,null,null,"Miscanthus","Tropical wet",null,"Subtropical steppe","Global","Pinus sp. <= 20 y"]
[null,null,null,null,null,"Rail (Electric, MV)","Hydrotreated vegetable oil",null,"Heat from landfill gas CHP","Diesel","n-Hexane","Pig manure","Tropical Montane",null,null,null,null,"Scrubland","Tropical montane",null,"Subtropical mountain system","n.a.","Pinus sp."]
[null,null,null,null,null,"n.a.","Pure vegetable oil",null,null,"Gasoline","Phosphoric acid (H3PO4)","Chicken manure","n.a. ",null,null,null,null,"Forest land_excluding plantations_10% to 30% canopy cover","n.a.",null,"Temperate oceanic forest",null,"Eucalyptus sp."]
[null,null,null,null,null,null,"n.a.",null,null,"Heavy fuel oil (HFO)","Fuller's earth","Sheep manure",null,null,null,null,null,"Forest land_excluding plantations_>30% canopy cover",null,null,"Temperate continental forest",null,"Tectona grandis"]
[null,null,null,null,null,null,null,null,null,"HFO for maritime transport","Hydrochloric acid (HCl)","Agricultural residues",null,null,null,null,null,"Forest plantations",null,null,"Temperate mountain systems",null,"Other broadleaf"]
[null,null,null,null,null,null,null,null,null,"Ethanol","Sodium carbonate (Na2CO3)","Organic domestical waste",null,null,null,null,null,null,null,null,"Boreal coniferous forest",null,"Other"]
[null,null,null,null,null,null,null,null,null,"Methanol","Sodium hydroxide (NaOH)","Organic residues (general)",null,null,null,null,null,null,null,null,"Boreal tundra woodland",null,"n.a."]
["Biogas from maize, anaerobic digestion + purification","Biogas from maize, anaerobic digestion + purification",null,null,null,null,null,null,null,"FAME","Potassium hydroxide (KOH)","Digestate breda",null,null,null,null,null,null,null,null,"Boreal mountain systems"]
["HVO from rapeseed, oil extraction + hydrogenation"," HVO from rapeseed, oil extraction + hydrogenation",null,null,null,null,null,null,null,"Syn diesel (BtL)","Hydrogen (for HVO)","Biogas (55% CH4)",null,null,null,null,null,null,null,null,"n.a."]
["HVO from sunflowerseed, oil extraction + hydrogenation","HVO from sunflowerseed, oil extraction + hydrogenation",null,null,null,null,null,null,null,"Hydrotreated vegetable oil","Pure CaO for processes","Purified biogas (55% CH4)"]
["Biogas from cow manure, anaerobic digestion + purification","Biogas from cow manure, anaerobic digestion + purification",null,null,null,null,null,null,null,"Pure vegetable oil","Sulphuric acid (H2SO4)","Liquid biomethane (LBM)"]
[null,null,null,null,null,null,null,null,null,"Hard coal","Ammonia","Rapeseed"]
[null,null,null,null,null,null,null,null,null,"Lignite","Cycle-hexane","Soybeans"]
[null,null,null,null,null,null,null,null,null,"n.a.","Digestate","Sugar beet"]
[null,null,null,null,null,null,null,null,null,"Heat from wood boiler CHP","Compost Breda - tunnel","Sugar cane"]
[null,null,null,null,null,null,null,null,null,"Heat from pyrolysis","n.a.","Sunflowerseed"]
[null,null,null,null,null,null,null,null,null,"Heat from landfill gas CHP","Digestate breda","Wheat"]
[null,null,null,null,null,null,null,null,null,null,"Liquid biomethane (LBM)","Waste vegetable / animal oil"]
[null,null,null,null,null,null,null,null,null,null,"GFT","BioOil (co-product FAME from waste oil)"]
[null,null,null,null,null,null,null,null,null,null,"Glycerol","Crude vegetable oil"]
[null,null,null,null,null,null,null,null,null,null,"Methanol","DDGS (10 wt% moisture)"]
[null,null,null,null,null,null,null,null,null,null,"Sulphuric acid (H2SO4)","Glycerol"]
[null,null,null,null,null,null,null,null,null,null,"Digestate moerdijk","Palm kernel meal"]
[null,null,null,null,null,null,null,null,null,null,"Biogas (55% CH4)","Crude palm oil"]
[null,null,null,null,null,null,null,null,null,null,"Biodiesel","Palm olein"]
[null,null,null,null,null,null,null,null,null,null,"Fast pyrolysis bio-oil","Palm stearin"]
[null,null,null,null,null,null,null,null,null,null,"Harvested grass","Rapeseed meal"]
[null,null,null,null,null,null,null,null,null,null,"Fatty residues","Soybean oil"]
[null,null,null,null,null,null,null,null,null,null,"Wood waste","Soy bean meal"]
[null,null,null,null,null,null,null,null,null,null,"Electricity from pyrolysis","Sugar beet pulp"]
[null,null,null,null,null,null,null,null,null,null,"Heat from pyrolysis","Sugar beet slops"]
[null,null,null,null,null,null,null,null,null,null,"Sunflowerseed","Vinasse"]
[null,null,null,null,null,null,null,null,null,null,"Rapeseed","Wheat straw"]
[null,null,null,null,null,null,null,null,null,null,"Maize (corn)","Compost"]
[null,null,null,null,null,null,null,null,null,null,"Fresh palm fruit bunches (FFB)","No crop"]
[null,null,null,null,null,null,null,null,null,null,null,"n.a."]
[null,null,null,null,null,null,null,null,null,null,null,"Compost Breda - tunnel"]
[null,null,null,null,null,null,null,null,null,null,null,"Harvested grass"]
[null,null,null,null,null,null,null,null,null,null,null,"Fatty residues"]
[null,null,null,null,null,null,null,null,null,null,null,"Biodiesel"]
[null,null,null,null,null,null,null,null,null,null,null,"Wood waste"]
[null,null,null,null,null,null,null,null,null,null,null,"Heat from pyrolysis"]
[null,null,null,null,null,null,null,null,null,null,null,"Electricity from pyrolysis"]
[null,null,null,null,null,null,null,null,null,null,null,"Fast pyrolysis bio-oil"]
[null,null,null,null,null,null,null,null,null,null,null,"Digestate moerdijk"]
[null,null,null,null,null,null,null,null,null,null,null,"Wood ash"]

{"sheet":"Standard Values","index":16,"n_rows":167,"n_cols":37,"rows_kept":167,"cut":false,"hidden":false,"merged":[[2,15,2,16],[3,1,3,8],[3,9,3,10],[3,15,3,16],[3,19,3,20],[2,25,2,34],[3,25,3,34],[5,25,5,26],[5,27,5,28],[5,29,5,30]]}
["STANDARD VALUES"]
["based on BioGrace + own additions (red font)",2,3,4,5,6,7,8,9,10,11,12,13,14,15,16,17,18,19,20,21,22,23,24,25,26,27,28,29,30,31,32,33,34,35,19,19]
[null,null,null,null,null,null,null,null,null,null,null,null,"Moisture",null,"Fuel","Transport exhaust",null,null,"Carbon",null,null,"Water","Land","Acidification","Eutrophication"]
["parameter: ","GHG emission coefficient",null,null,null,null,null,null,null,"Fossil energy input",null,"Density","content","LHV","efficiency","gas emissions",null,"Valorisation","emissions","Primary energy input",null,"use","use",null,null,"Other emission coefficients",null,null,null,null,null,null,null,null,null,"Source","Remark / question"]
["unit: ","gCO2/kg","gCH4/kg","gN2O/kg","gCO2-eq/kg","gCO2/MJ","gCH4/MJ","gN2O/MJ","gCO2-eq/MJ","MJfossil/kg","MJfossil/MJ","kg/m3","%","MJ/kg (at 0% water,","MJ/t.km","gCH4/t.km","gN2O/t.km","yes = 1","tC/ha.y","MJprim/kg","MJprim/MJ","m³/GJ","ha/GJ","gSO2-eq/g","gPO4-eq/g","gNOX/kg","gNOX/MJ","gSOX/kg","gSOX/MJ","gNH3/kg","gNH3/MJ"]
[null,1,23,296,null,null,null,null,null,null,null,null,null,"unless otherwise stated)",null,null,null,"no = 0",null,null,null,null,null,"gSO2-eq/MJ","gPO4-eq/MJ","to air",null,"to air",null,"to air"]
["Seeds"]
["Maize (corn)",0,0,0,{"$f":"B8*$B$6+C8*$C$6+D8*$D$6","v":0},null,null,null,null,0,null,null,null,null,null,null,null,null,null,{"$f":"J8*1.5","v":0},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Fresh palm fruit bunches (FFB)",0,0,0,{"$f":"B9*$B$6+C9*$C$6+D9*$D$6","v":0},null,null,null,null,0,null,null,null,null,null,null,null,null,null,{"$f":"J9*1.5","v":0}]
["Rapeseed",412.08109999999999,0.91269999999999996,1.0027999999999999,729.90200000000004,null,null,null,null,7.86564,null,null,null,null,null,null,null,null,null,11.79846,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Soy bean",0,0,0,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sugarbeet",2187.7141000000001,4.6003999999999996,4.2119999999999997,3540.2753000000002,null,null,null,null,36.294119999999999,null,null,null,null,null,null,null,null,null,54.441180000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sugarcane",1.6397999999999999,1E-4,0,1.6420999999999999,null,null,null,null,2.1600000000000001E-2,null,null,null,null,null,null,null,null,null,{"$f":"J13*1.5","v":3.2399999999999998E-2},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sunflowerseed",412.08109999999999,0.91269999999999996,1.0027999999999999,729.90200000000004,null,null,null,null,7.86564,null,null,null,null,null,null,null,null,null,11.79846,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Wheat",151.0557,0.27710000000000001,0.40029999999999999,275.9178,null,null,null,null,2.6074799999999998,null,null,null,null,null,null,null,null,null,3.9112199999999997,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["No crop",0,0,0,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,{"$f":"J16*1.5","v":0}]
[]
["Agro inputs "]
["N",2827.0048999999999,8.6788000000000007,9.6417999999999999,{"$f":"B19*$B$6+C19*$C$6+D19*$D$6","v":5880.5900999999994},null,null,null,null,48.990600000000001,null,null,null,null,null,null,null,null,null,{"$f":"J19*1.5","v":73.485900000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["P2O5",964.88649999999996,1.331,5.1499999999999997E-2,{"$f":"B20*$B$6+C20*$C$6+D20*$D$6","v":1010.7434999999999},null,null,null,null,15.2334,null,null,null,null,null,null,null,null,null,{"$f":"J20*1.5","v":22.850099999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["K2O",536.31089999999995,1.5709,1.23E-2,{"$f":"B21*$B$6+C21*$C$6+D21*$D$6","v":576.08240000000001},null,null,null,null,9.67896,null,null,null,null,null,null,null,null,null,14.51844,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["CaO",119.116,0.21590000000000001,1.83E-2,{"$f":"B22*$B$6+C22*$C$6+D22*$D$6","v":129.49850000000001},null,null,null,null,1.9735200000000002,null,null,null,null,null,null,null,null,null,2.96028,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Pesticides",9886.5020000000004,25.527100000000001,1.6814,{"$f":"B23*$B$6+C23*$C$6+D23*$D$6","v":10971.3197},null,null,null,null,268.39980000000003,null,null,null,null,null,null,null,null,null,402.59970000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
[]
["Fuels- gasses "]
["Natural gas (4000 km, Russian NG quality)",null,null,null,null,61.575111111111113,0.19813888888888889,2.2222222222222223E-4,{"$f":"F26*$B$6+G26*$C$6+H26*$D$6","v":66.198083333333344},null,1.1281000000000001,null,null,null,null,null,null,null,null,null,{"$f":"K26*1.5","v":1.6921500000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Natural gas (4000 km, EU Mix qualilty)",null,null,null,null,62.963999999999999,0.19813888888888889,2.2222222222222223E-4,{"$f":"F27*$B$6+G27*$C$6+H27*$D$6","v":67.586972222222229},null,1.1281000000000001,null,null,48,null,null,null,null,null,null,{"$f":"K27*1.5","v":1.6921500000000003},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["LNG",null,null,null,null,null,null,null,null,null,null,null,null,48.6,null,null,null,null,null,null,0.31]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
[]
["Fuels- liquids (also conversion inputs)"]
["Diesel",{"$f":"F32*$N32","v":0},{"$f":"G32*$N32","v":0},{"$f":"H32*$N32","v":0},{"$f":"I32*$N32","v":3777.2361111111118},null,null,null,87.6388888888889,{"$f":"K32*N32","v":49.995999999999995},1.1599999999999999,832,null,43.1,null,null,null,null,null,{"$f":"U32*N32","v":74.993999999999986},{"$f":"K32*1.5","v":1.7399999999999998},null,null,null,null,{"$f":"AA32*$N32","v":38.272800000000004},0.88800000000000001,{"$f":"AC32*N32","v":14.869499999999999},0.34499999999999997,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008); Achten, 2010"]
["Gasoline",null,null,null,null,null,null,null,86,{"$f":"K33*N33","v":49.247999999999998},1.1399999999999999,745,null,43.2,null,null,null,null,null,{"$f":"U33*N33","v":73.872},{"$f":"K33*1.5","v":1.71},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Heavy fuel oil (HFO)",{"$f":"F34*$N34","v":0},0,0,3441.6000000000008,null,null,null,84.977777777777803,{"$f":"K34*N34","v":44.064},1.0880000000000001,970,null,40.5,null,null,null,null,null,{"$f":"U34*N34","v":66.096000000000004},{"$f":"K34*1.5","v":1.6320000000000001},null,null,null,null,{"$f":"AA34*$N34","v":35.963999999999999},0.88800000000000001,{"$f":"AC34*N34","v":13.972499999999998},0.34499999999999997,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["HFO for maritime transport",0,0,0,3531.6,null,null,null,87.2,{"$f":"K35*N35","v":44.064},1.0880000000000001,970,null,40.5,null,null,null,null,null,{"$f":"U35*N35","v":66.096000000000004},{"$f":"K35*1.5","v":1.6320000000000001},null,null,null,null,{"$f":"AA35*$N35","v":35.963999999999999},0.88800000000000001,{"$f":"AC35*N35","v":13.972499999999998},0.34499999999999997,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Ethanol",null,null,null,null,null,null,null,null,null,null,794,null,26.81,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Methanol",{"$f":"F37*$N37","v":1846.6691444444452},{"$f":"G37*$N37","v":5.7715527777777771},{"$f":"H37*$N37","v":6.6333333333333322E-3},{"$f":"I37*$N37","v":1981.378325000001},92.797444444444494,0.29002777777777777,3.3333333333333332E-4,{"$f":"F37*$B$6+G37*$C$6+H37*$D$6","v":99.566750000000056},{"$f":"K37*N37","v":33.022059999999996},1.6594,793,null,19.899999999999999,null,null,null,null,null,{"$f":"U37*N37","v":49.533090000000001},{"$f":"K37*1.5","v":2.4891000000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["FAME",null,null,null,null,null,null,null,null,null,null,890,null,37.200000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)","or \"XME\" which is RME, PME, SME etc"]
["Syn diesel (BtL)",null,null,null,null,null,null,null,null,null,null,780,null,44,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Hydrotreated vegetable oil",null,null,null,null,null,null,null,null,null,null,780,null,44,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Pure vegetable oil",null,null,null,null,null,null,null,null,null,null,null,null,36]
[]
["Fuels / feedstock / co-products - solids"]
["Hard coal",null,null,null,null,102.38424999999999,0.3835277777777778,2.5000000000000001E-4,{"$f":"F44*$B$6+G44*$C$6+H44*$D$6","v":111.27938888888887},{"$f":"K44*N44","v":28.882735199999996},1.0885999999999998,null,null,26.532,null,null,null,1,null,{"$f":"U44*N44","v":43.324102799999991},{"$f":"K44*1.5","v":1.6328999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Lignite",null,null,null,null,116.75711111111112,9.0555555555555545E-3,5.5555555555555558E-5,{"$f":"F45*$B$6+G45*$C$6+H45*$D$6","v":116.98183333333334},{"$f":"K45*N45","v":9.3780503999999993},1.0155999999999998,null,null,9.234,null,null,null,1,null,{"$f":"U45*N45","v":14.067075599999997},{"$f":"K45*1.5","v":1.5233999999999996},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Maize (corn)",null,null,null,null,null,null,null,null,null,null,null,null,18.5,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Empty palm fruit bunches",0,0,0,{"$f":"B47*$B$6+C47*$C$6+D47*$D$6","v":0},null,null,null,null,0,null,null,null,null,null,null,null,0,null,{"$f":"J47*1.5","v":0}]
["Filter mud cake",0,0,0,{"$f":"B48*$B$6+C48*$C$6+D48*$D$6","v":0},null,null,null,null,0,null,null,null,null,null,null,null,0,null,0]
["Fresh palm fruit bunches (FFB)",null,null,null,null,null,null,null,null,null,null,null,null,24,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Fresh palm fruit",null,null,null,null,null,null,null,null,0,null,null,null,24,null,null,null,1,null,{"$f":"J50*1.5","v":0}]
["Manure co- vergister ",0,{"$f":"3.225*0.05","v":0.16125},{"$f":"6*0.001*0.05","v":3.0000000000000003E-4},{"$f":"B51*$B$6+C51*$C$6+D51*$D$6","v":3.7975500000000002},null,null,null,null,0,null,null,null,12.8,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,0.154,null,null,null,null,null,"JEC E3-database (version 31-7-2008)","No GHG emissions or fossil energy input because it is a residue"]
["Cattle manure",null,null,null,0,null,null,null,null,0,null,null,null,12.814,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Pig manure",null,null,null,0,null,null,null,null,0,null,null,null,12.829000000000001,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Chicken manure",null,null,null,0,null,null,null,null,0,null,null,null,15.27,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Sheep manure",null,null,null,0,null,null,null,null,0,null,null,null,14.907999999999999,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Agricultural residues",null,null,null,0,null,null,null,null,0,null,null,null,15,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Organic domestical waste",null,{"$f":"3.1*0.05","v":0.15500000000000003},{"$f":"1.3*0.001*0.05","v":6.5000000000000008E-5},{"$f":"B57*$B$6+C57*$C$6+D57*$D$6","v":3.5842400000000003},null,null,null,null,0,null,null,null,10.1,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Organic residues (general)",null,null,null,{"$f":"B58*$B$6+C58*$C$6+D58*$D$6","v":0},null,null,null,null,0,null,null,null,15.4,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Compost from digestate ",null,null,null,0,null,null,null,null,null,null,null,null,12.4]
["Digestate breda",null,0.61899999999999999,null,14.237,null,null,null,null,null,null,null,null,8.5500000000000007,null,null,null,0,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Biogas (55% CH4)",null,null,null,null,null,null,null,null,null,null,null,null,27.5,null,null,null,1,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Purified biogas (55% CH4)",null,5.5,null,{"$f":"B62*$B$6+C62*$C$6+D62*$D$6","v":126.5},null,null,null,null,null,null,null,null,27.5,null,null,null,1,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ECN Phyllis"]
["Liquid biomethane (LBM)",null,{"$f":"0.93+5.5","v":6.43},null,147.88999999999999,null,{"$f":"1/50","v":0.02},null,{"$f":"F63*$B$6+G63*$C$6+H63*$D$6","v":0.46},null,null,null,null,50,null,null,null,1,null,0]
["Rapeseed",null,null,null,null,null,null,null,43,{"$f":"K64*N64","v":12.803999999999998},0.48499999999999999,null,null,26.4,null,null,null,1,null,{"$f":"U64*N64","v":19.206},{"$f":"K64*1.5","v":0.72750000000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Soybeans",null,null,null,null,null,null,null,null,null,null,null,null,23.529411764705884,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sugar beet",null,null,null,null,null,null,null,null,null,null,null,null,16.3,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sugar cane",null,null,null,null,null,null,null,null,null,null,null,null,19.600000000000001,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sunflowerseed",null,null,null,null,null,null,null,36,{"$f":"K68*N68","v":9.8999999999999986},0.375,null,null,26.4,null,null,null,1,null,{"$f":"U68*N68","v":14.85},{"$f":"K68*1.5","v":0.5625},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Wheat",null,null,null,null,null,null,null,null,null,null,null,null,17,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Waste vegetable / animal oil",null,null,null,null,null,null,null,null,null,null,null,null,37.1,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["BioOil (co-product FAME from waste oil)",null,null,null,null,null,null,null,null,null,null,null,null,21.8,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Crude vegetable oil",null,null,null,null,null,null,null,null,null,null,null,null,36,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["DDGS (10 wt% moisture)",null,null,null,null,null,null,null,null,null,null,null,null,16,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Glycerol",null,null,null,19.710999999999999,null,null,null,null,null,null,null,null,16,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)","The value of cell E5 has been calculated specifically for Moerdijk case"]
["Palm kernel meal",null,null,null,null,null,null,null,null,null,null,null,null,17,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Crude palm oil",null,null,null,null,null,null,null,null,null,null,null,null,37,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Palm olein",null,null,null,null,null,null,null,null,null,null,null,null,37,null,null,null,1]
["Palm stearin",null,null,null,null,null,null,null,null,null,null,null,null,37,null,null,null,1]
["Rapeseed meal",null,null,null,null,null,null,null,null,null,null,null,null,18.649999999999999,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Soybean oil",null,null,null,null,null,null,null,null,null,null,null,null,36.6,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Soy bean meal",null,null,null,null,null,null,null,null,null,null,null,null,"-",null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)","No LHV given in the E3 database. Allocation to soy bean meal should be performed in same way as done by JEC consortium"]
["Sugar beet pulp",null,null,null,null,null,null,null,null,null,null,null,null,15.6,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sugar beet slops",null,null,null,null,null,null,null,null,null,null,null,null,15.6,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Vinasse",0,0,0,{"$f":"B84*$B$6+C84*$C$6+D84*$D$6","v":0},null,null,null,null,0,null,null,null,null,null,null,null,1]
["Wheat straw",null,null,null,null,1.7515833333333333,1.3333333333333333E-3,5.5555555555555558E-5,{"$f":"F85*$B$6+G85*$C$6+H85*$D$6","v":1.7986944444444444},null,2.5400000000000002E-2,null,null,17.2,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)","Transport plus fertiliser debit because more fertiliser is required at the cultivation stage if the straw is removed"]
["Compost ",null,null,null,0,null,null,null,0,0,null,null,null,4,null,null,null,0]
["No crop",null,null,null,0,null,null,null,0,0,null,null,null,0,null,null,null,0]
["GFT",null,null,null,23.99,null,null,null,0,0,null,null,null,10.116,null,null,null,0]
["Compost Breda - tunnel",null,0.17,7.0000000000000007E-2,{"$f":"B89*$B$6+C89*$C$6+D89*$D$6","v":24.630000000000003},null,null,null,null,null,null,null,null,14.7,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Alterra rapport"]
["Harvested grass",null,null,null,0,null,null,null,null,null,null,null,null,17.2,null,null,null,0]
["Fatty residues",null,null,null,0,null,null,null,null,null,null,null,null,38.799999999999997,null,null,null,0]
["Biodiesel",null,null,null,0,null,null,null,null,null,null,null,null,24.67,null,null,null,1]
["Wood waste",null,null,null,0,null,null,null,null,null,null,null,null,17.73,null,null,null,0]
["Fast pyrolysis bio-oil",null,null,null,0,null,null,null,null,null,null,null,null,21.15,null,null,null,1]
["Electricity from pyrolysis",null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,0]
["Heat from pyrolysis",null,null,null,0,null,null,null,null,null,4.7E-2,null,null,null,null,null,null,0,null,null,{"$f":"K96*1.5","v":7.0500000000000007E-2}]
["Digestate moerdijk",null,0.89,null,20.47,null,null,null,null,null,null,null,null,12.6,null,null,null,1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"The value of cell E5 has been calculated specifically for Moerdijk case"]
["Wood ash",null,null,null,null,null,null,null,null,null,null,null,null,17.82,null,null,null,1]
["Methanol",{"$f":"F99*$N99","v":1846.6691444444452},{"$f":"G99*$N99","v":5.7715527777777771},{"$f":"H99*$N99","v":6.6333333333333322E-3},{"$f":"I99*$N99","v":1981.378325000001},92.797444444444494,0.29002777777777777,3.3333333333333332E-4,{"$f":"F99*$B$6+G99*$C$6+H99*$D$6","v":99.566750000000056},{"$f":"K99*N99","v":33.022059999999996},1.6594,793,null,19.899999999999999,null,null,null,null,null,{"$f":"U99*N99","v":49.533090000000001},{"$f":"K99*1.5","v":2.4891000000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sulphuric acid (H2SO4)",193.8502,0.54569999999999996,4.4999999999999997E-3,{"$f":"B100*$B$6+C100*$C$6+D100*$D$6","v":207.73329999999999},null,null,null,null,3.8959200000000003,null,null,null,null,null,null,null,null,null,{"$f":"J100*1.5","v":5.8438800000000004},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Greenwaste",null,null,null,5.2,null,null,null,null,null,null,null,null,13,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC Well-to-tank report (version 03-11-2008)"]
["Fuller's earth",197,3.73E-2,6.3E-3,199.7227,null,null,null,null,2.5405200000000003,null,null,null,0,null,null,null,null,null,3.8107800000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Electricity"]
["Electricity EU mix MV",null,null,null,null,119.36216666666667,0.29108333333333336,5.3888888888888892E-3,{"$f":"F104*$B$6+G104*$C$6+H104*$D$6","v":127.65219444444445},null,2.6951000000000001,null,null,null,null,null,null,null,null,null,{"$f":"K104*1.5","v":4.0426500000000001},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Electricity EU mix LV",null,null,null,null,120.7945,0.29458333333333331,5.4722222222222221E-3,{"$f":"F105*$B$6+G105*$C$6+H105*$D$6","v":129.18969444444446},null,2.7275,null,null,null,null,null,null,null,null,null,{"$f":"K105*1.5","v":4.0912500000000005},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Electricity (NG CCGT)",null,null,null,null,114.48,0.36788585858585859,4.9845959595959596E-3,{"$f":"F106*$B$6+G106*$C$6+H106*$D$6","v":124.41681515151515},null,2.0510909090909091,null,null,null,null,null,null,null,null,null,3.0766363636363634,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Electricity (Lignite ST)",null,null,null,null,284.77059400000002,2.5857055555555553E-2,7.7782777777777781E-3,{"$f":"F107*$B$6+G107*$C$6+H107*$D$6","v":287.66767650000003},null,2.4770483999999997,null,null,null,null,null,null,null,null,null,3.7155725999999998,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Electricity (Straw ST)",null,null,null,null,5.5605764499999992,4.2328000000000001E-3,1.7636666666666668E-4,{"$f":"F108*$B$6+G108*$C$6+H108*$D$6","v":5.7101353833333333},null,8.0634839999999999E-2,null,null,null,null,null,null,null,null,null,0.12095226000000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Electricity EU fossil comparator",null,null,null,null,null,null,null,129.19,null,2.7275,null,null,null,null,null,null,null,null,null,4.0913000000000004,0.61,0,2.46,0.6,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Electricity from landfill gas CHP",null,null,null,null,null,null,null,7.7,null,{"$f":"-0.08","v":-0.08},null,null,null,null,null,null,null,null,null,{"$f":"3.2","v":3.2}]
["Electricity from wood boiler CHP",null,null,null,null,null,null,null,3.1,null,0.16,null,null,null,null,null,null,null,null,null,11.25,null,null,null,1.46E-2,null,{"$f":"0.1125","v":0.1125},null,null,null,null,null,null,null,null,"JEC Well-to-tank report (version 03-11-2008)"]
["Electricity from biogas CHP",null,null,null,null,null,null,null,7.7,null,{"$f":"0.08","v":0.08},null,null,null,null,null,null,null,null,null,{"$f":"(1949625*20.65)/((3186+991)*3600)","v":2.6773439370361505}]
["Electricity from pyrolysis",null,null,null,null,null,null,null,null,null,{"$f":"0.001*0.04","v":4.0000000000000003E-5},null,null,null,null,null,null,null,null,null,{"$f":"1.64*0.03","v":4.9199999999999994E-2}]
["Heat (per MJ steam or heat)"]
["Heat EU mix",null,null,null,null,77,0.33,2E-3,{"$f":"F115*$B$6+G115*$C$6+H115*$D$6","v":85.182000000000002},null,1.43,null,null,null,null,null,null,null,null,null,{"$f":"K115*1.5","v":2.145},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC database (version 18-11-2008)"]
["Heat from NG boiler",null,null,null,null,71.58,2.7777777777777779E-3,1.1111111111111111E-3,71.972777777777765,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Heat from NG CHP",null,null,null,null,72.63,0,0,72.63,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Heat from Lignite CHP",null,null,null,null,72,2.3055555555555598E-3,1.2611111111111111E-2,75.785916666666665,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Heat from wood boiler CHP",null,null,null,null,null,null,null,{"$f":"3.1/2.5","v":1.24},null,{"$f":"0.02","v":0.02},null,null,null,null,null,null,null,null,null,{"$f":"1.26","v":1.26},null,null,null,{"$f":"0.13*AA119","v":9.75E-3},null,{"$f":"0.075","v":7.4999999999999997E-2},null,null,null,null,null,null,null,null,"JEC Well-to-tank report (version 03-11-2008)"]
["Heat from landfill gas CHP",null,null,null,null,null,null,null,16.2,null,{"$f":"0.15","v":0.15},null,null,null,null,null,null,null,null,null,{"$f":"0.86","v":0.86},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC Well-to-tank report (version 03-11-2008)"]
["Heat from Straw CHP",null,null,null,null,1.55,0,0,1.55,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Heat from NG gas engine",null,null,null,null,72,{"$f":"0.192/3.6","v":5.333333333333333E-2},0,73.226666666666659,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Heat EU fossil comparator",null,null,null,null,null,null,null,85.18,null,1.43,null,null,null,null,null,null,null,null,null,2.145,0.76,0,1.53,0.4,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Heat from pyrolysis",null,null,null,null,null,null,null,null,null,{"$f":"0.001*0.31","v":3.1E-4},null,null,null,null,null,null,null,null,null,{"$f":"1.64*0.33","v":0.54120000000000001}]
["Heat from biogas CHP",null,null,null,null,null,null,null,16.2,null,{"$f":"0.01","v":0.01},null,null,null,null,null,null,null,null,null,{"$f":"(1949625*20.65)/((3788+1062)*3600)","v":2.3058279639175256},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC Well-to-tank report (version 03-11-2008)"]
["Conversion inputs/outputs"]
["n-Hexane",null,null,null,null,80.083333333333329,1.4555555555555556E-2,2.7777777777777778E-4,{"$f":"F127*$B$6+G127*$C$6+H127*$D$6","v":80.50033333333333},null,0.32036111111111115,null,null,45.107999999999997,null,null,null,null,null,null,{"$f":"I127*1.5","v":120.75049999999999},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Phosphoric acid (H3PO4)",2776,8.9268000000000001,0.1028,{"$f":"B128*$B$6+C128*$C$6+D128*$D$6","v":3011.7452000000003},null,null,null,null,28.570320000000002,null,null,null,null,null,null,null,null,null,{"$f":"J128*1.5","v":42.85548},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Fuller's earth",197,3.73E-2,6.3E-3,{"$f":"B129*$B$6+C129*$C$6+D129*$D$6","v":199.7227},null,null,null,null,2.5405200000000003,null,null,null,12,null,null,null,null,null,3.8107800000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Hydrochloric acid (HCl)",717.37800000000004,1.129,2.5399999999999999E-2,750.86340000000007,null,null,null,null,15.433495199999999,null,null,null,null,null,null,null,null,null,23.150242800000001,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sodium carbonate (Na2CO3)",1046,6.2,5.4999999999999997E-3,1190.2279999999998,null,null,null,null,13.785480000000002,null,null,null,null,null,null,null,null,null,20.678220000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sodium hydroxide (NaOH)",438.4932,1.0301,2.4E-2,469.28949999999998,null,null,null,null,10.2204,null,null,null,null,null,null,null,null,null,15.3306,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Potassium hydroxide (KOH)",0,0,0,0,null,null,null,null,0,null,null,null,null,null,null,null,null,null,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"No emission factors and LHV given in E3 database. Emissions assumed to be zero."]
["Hydrogen (for HVO)",null,null,null,null,80.868472222222223,0.27647222222222223,3.0555555555555555E-4,{"$f":"F134*$B$6+G134*$C$6+H134*$D$6","v":87.317777777777778},null,1.4835,null,null,null,null,null,null,null,null,null,{"$f":"I134*1.5","v":130.97666666666666},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Pure CaO for processes",1013,0.64900000000000002,7.6E-3,1030.1766,null,null,null,null,4.5979199999999993,null,null,null,null,null,null,null,null,null,6.8968799999999995,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Sulphuric acid (H2SO4)",193.8502,0.54569999999999996,4.4999999999999997E-3,207.73329999999999,null,null,null,null,3.8959200000000003,null,null,null,null,null,null,null,null,null,5.8438800000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Ammonia",2478.0410000000002,7.8360000000000003,8.6999999999999994E-3,2660.8442000000005,null,null,null,null,44.388359999999999,null,null,null,null,null,null,null,null,null,66.582539999999995,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Cycle-hexane",723,0,0,723,null,null,null,null,53.1,null,null,null,null,null,null,null,null,null,79.650000000000006,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Lubricants",947,0,0,947,null,null,null,null,53.28,null,null,null,null,null,null,null,null,null,79.92,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
[]
["Transport modes"]
["Truck for dry product (diesel)",null,null,null,null,null,null,null,87.64,{"$f":"K142*N142","v":0},1.1599999999999999,null,null,null,0.93600000000000005,5.0000000000000001E-3,0,null,null,{"$f":"U142*N142","v":0},{"$f":"K142*1.5","v":1.7399999999999998},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Truck for liquids (diesel)",null,null,null,null,null,null,null,null,null,null,null,null,null,1.008,5.0000000000000001E-3,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Calculated from value above, correction for weight of liquid container (2 ton) in comparison to loaded truck weight (26 ton)"]
["Truck for FFB transport (diesel)",null,null,null,null,null,null,null,null,null,null,null,null,null,2.0122857142857145,5.0000000000000001E-3,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Tanker truck MB2218 for vinasse transport",null,null,null,null,null,null,null,null,null,null,null,null,null,2.16,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Tanker truck with water cannons for vinasse transport",null,null,null,null,null,null,null,null,null,null,null,null,null,0.94,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Dumpster truck MB2213 for filter mud transport",null,null,null,null,null,null,null,null,null,null,null,null,null,3.6,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Ocean bulk carrier (HFO maritime)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.20358000000000001,2.9999999999999997E-4,7.2000000000000005E-4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Ship /product tanker 50kt (HFO maritime)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.12384000000000001,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Local (10 km) pipeline",null,null,null,null,null,null,null,null,null,null,null,null,null,0,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
["Rail (Electric, MV)",null,null,null,null,null,null,null,null,null,null,null,null,null,0.21,0,0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"JEC E3-database (version 31-7-2008)"]
[]
["Land use change"]
["Previously degraded land",null,null,null,null,null,null,null,29,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"RED"]
["Peatland",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,20,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"IPCC 2006 chapter 4"]
[]
["Emissions"]
["NH3",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1.88,0.35]
["NH4+ to water",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.33]
["N to air",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.42]
["N to water",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.42]
["NO3- to water",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.1]
["NOx",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,0.7,0.13]
["SOx",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
["P to water",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,3.06]
["PO43-",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,1]
["COD",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.1999999999999999E-2]

{"sheet":"IPCC Values","index":17,"n_rows":461,"n_cols":52,"rows_kept":461,"cut":false,"hidden":false,"merged":[]}
["IPCC VALUES"]
["based on IPCC Guidelines 2006",null,1,2,3,4,null,1,2,3,4,5,6,7,8,null,1,2,3,4,5,6,7,8,9,null,null,null,null,1,2,3,4,5,6,7,8,9,10,null,null,1,2,3,4,5,6,7]
[null,null,"Standard soil organic carbon (tC/ha)",null,null,null,null,"Factors land use, management and input",null,null,null,null,null,null,null,null,"Carbon stock values for above and below ground vegetation carbon stock",null,null,null,null,null,null,null,null,null,"Carbon fraction",null,null,"Default factors for estimation of N added to soils from crop resiudes",null,null,null,null,null,null,null,null,null,null,null,"Emission factors_N20 emissions",null,null,null,null,null,null,null,"Fresh water availability"]
[null,null,"ID","Climate region","Soil type","Standard soil organic carbon",null,"ID","Land use","Climate region","Management","Input","Land use factor ","Management factor ","Input factor",null,"ID","Land use_more specific","Domain","Climate region","Ecological zone","Continent","Type","Carbon stock ","R",null,"Material","Column1",null,"Crop","Slope","± 2 s.d. as % of mean","Intercept","± 2 s.d. as % of mean2","R² adj","N content of above-ground residues","N content of below-ground residues","Ratio of below-ground residues to above ground biomass","± 2 s.d. as % of mean22",null,null,"Emission factor","Climate region","Land use","Nutrient level","Value","Min","Max",null,"Country","freshwater availiability (m³/capita.yr)","water level"]
["Data matrices",null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal dry High Activity Clay Soils"},"Boreal dry","High Activity Clay Soils",68,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry Full tillage Low"},"Annual cropland","Boreal dry","Full tillage","Low",0.8,1,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical dry Tropical dry forest Africa n.a."},"Sugar cane","n.a.","Tropical dry","Tropical dry forest","Africa","n.a.",4.2,null,null,"dry matter in living biomass",0.47,null,"Maize (corn)",1.03,3,0.61,19,0.76,6.0000000000000001E-3,7.0000000000000001E-3,0.22,26,null,null,"EF1",null,null,null,0.01,3.0000000000000001E-3,0.03,null,"Afghanistan",2610,{"$f":"IF(AY5<1000,\"scarce\",IF(AY5<1700,\"stress\",IF(AY5<2500,\"vulnerable\",IF(AY5<6000,\"low but not vulnerable\",IF(AY5<15000,\"medium\",IF(AY5<70000,\"high\",\"very high\"))))))","v":"low but not vulnerable"}]
[{"$f":"C3","v":"Standard soil organic carbon (tC/ha)"},null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal dry Low Activity Clay Soils"},"Boreal dry","Low Activity Clay Soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry Full tillage Medium"},"Annual cropland","Boreal dry","Full tillage","Medium",0.8,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical dry Tropical dry forest Asia continental n.a."},"Sugar cane","n.a.","Tropical dry","Tropical dry forest","Asia continental","n.a.",4,null,null,"dry matter in dead wood",0.5,null,"Wheat",1.51,3,0.52,17,0.68,6.0000000000000001E-3,8.9999999999999993E-3,0.24,32,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Annual cropland n.a."},"Boreal dry","Annual cropland","n.a.","n.a.","n.a.","n.a.",null,"Albania",13060,"medium"]
[{"$f":"H3","v":"Factors land use, management and input"},null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal dry Sandy Soils"},"Boreal dry","Sandy Soils",10,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry Full tillage High with manure"},"Annual cropland","Boreal dry","Full tillage","High with manure",0.8,1,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical dry Tropical dry forest Asia insular n.a."},"Sugar cane","n.a.","Tropical dry","Tropical dry forest","Asia insular","n.a.",4,null,null,"dry matter in litter",0.4,null,"Soybeans",0.93,31,1.35,49,0.16,8.0000000000000002E-3,7.3999999999999996E-2,0.19,45,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Perennial cropland n.a."},"Boreal dry","Perennial cropland","n.a.","n.a.","n.a.","n.a.",null,"Algeria",440,"scarce"]
[{"$f":"Q3","v":"Carbon stock values for above and below ground vegetation carbon stock"},null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal dry Spodic Soils"},"Boreal dry","Spodic Soils",117,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry Full tillage High without manure"},"Annual cropland","Boreal dry","Full tillage","High without manure",0.8,1,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical dry Tropical shrubland Asia continental n.a."},"Sugar cane","n.a.","Tropical dry","Tropical shrubland","Asia continental","n.a.",4,null,null,null,null,null,"Sugar beet",0.1,69,1.06,70,0.18,1.9E-2,1.4E-2,0.2,50,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Grassland and savannah n.a."},"Boreal dry","Grassland and savannah","n.a.","n.a.","n.a.","n.a.",null,"Angola",10510,"medium"]
[{"$f":"AA3","v":"Carbon fraction"},null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal dry Volcanic Soils"},"Boreal dry","Volcanic Soils",20,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry Reduced tillage Low"},"Annual cropland","Boreal dry","Reduced tillage","Low",0.8,1.02,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical dry Tropical shrubland Asia insular n.a."},"Sugar cane","n.a.","Tropical dry","Tropical shrubland","Asia insular","n.a.",4,null,null,null,null,null,"Rapeseed",1.5,null,0,null,null,1.0999999999999999E-2,1.7000000000000001E-2,0.19,null,"BioGrace",null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Shifting cultivation shortened fallow n.a."},"Boreal dry","Shifting cultivation shortened fallow","n.a.","n.a.","n.a.","n.a.",null,"Antigua and Barbuda",710,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal dry Wetland Soils"},"Boreal dry","Wetland Soils",146,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry Reduced tillage Medium"},"Annual cropland","Boreal dry","Reduced tillage","Medium",0.8,1.02,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical moist Tropical moist deciduous forest Africa n.a."},"Sugar cane","n.a.","Tropical moist","Tropical moist deciduous forest","Africa","n.a.",4.2,null,null,null,null,null,"Sunflowerseed",2.1,null,0,null,null,7.0000000000000001E-3,7.0000000000000001E-3,0.22,null,"BioGrace",null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Shifting cultivation mature fallow n.a."},"Boreal dry","Shifting cultivation mature fallow","n.a.","n.a.","n.a.","n.a.",null,"Argentina",20940,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal moist High activity clay soils"},"Boreal moist","High activity clay soils",68,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry Reduced tillage High with manure"},"Annual cropland","Boreal dry","Reduced tillage","High with manure",0.8,1.02,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical moist Tropical moist deciduous forest Central and South America n.a."},"Sugar cane","n.a.","Tropical moist","Tropical moist deciduous forest","Central and South America","n.a.",5,null,null,null,null,null,"Fresh palm fruit bunches (FFB)","n.a.",null,"n.a.",null,null,1.0999999999999999E-2,1.0999999999999999E-2,0,null,"BioGrace",null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Native forest non degraded Nutrient rich"},"Boreal dry","Native forest non degraded","Nutrient rich",0.6,0.16,2.4,null,"Armenia",3450,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal moist Low activity clay soils"},"Boreal moist","Low activity clay soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry Reduced tillage High without manure"},"Annual cropland","Boreal dry","Reduced tillage","High without manure",0.8,1.02,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical wet Tropical rain forest Asia continental n.a."},"Sugar cane","n.a.","Tropical wet","Tropical rain forest","Asia continental","n.a.",4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Native forest non degraded Nutrient poor"},"Boreal dry","Native forest non degraded","Nutrient poor",0.1,0.02,0.3,null,"Australia",24710,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal moist Sandy soils"},"Boreal moist","Sandy soils",10,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry No till Low"},"Annual cropland","Boreal dry","No till","Low",0.8,1.1000000000000001,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical wet Tropical rain forest Asia insular n.a."},"Sugar cane","n.a.","Tropical wet","Tropical rain forest","Asia insular","n.a.",4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Managed forest Nutrient rich"},"Boreal dry","Managed forest","Nutrient rich",0.6,0.16,2.4,null,"Austria",9570,"medium"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal moist Spodic soils"},"Boreal moist","Spodic soils",117,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry No till Medium"},"Annual cropland","Boreal dry","No till","Medium",0.8,1.1000000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Tropical wet Tropical rain forest Central and South America n.a."},"Sugar cane","n.a.","Tropical wet","Tropical rain forest","Central and South America","n.a.",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal dry Managed forest Nutrient poor"},"Boreal dry","Managed forest","Nutrient poor",0.1,0.02,0.3,null,"Azerbaijan",3580,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal moist Volcanic soils"},"Boreal moist","Volcanic soils",20,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry No till High with manure"},"Annual cropland","Boreal dry","No till","High with manure",0.8,1.1000000000000001,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Warm temperate dry Subtropical steppe North America n.a."},"Sugar cane","n.a.","Warm temperate dry","Subtropical steppe","North America","n.a.",4.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Annual cropland n.a."},"Boreal moist","Annual cropland","n.a.","n.a.","n.a.","n.a.",null,"Bahamas",63,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Boreal moist Wetland soils"},"Boreal moist","Wetland soils",146,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal dry No till High without manure"},"Annual cropland","Boreal dry","No till","High without manure",0.8,1.1000000000000001,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Warm temperate moist Subtropical humid forest Central and South America n.a."},"Sugar cane","n.a.","Warm temperate moist","Subtropical humid forest","Central and South America","n.a.",5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Perennial cropland n.a."},"Boreal moist","Perennial cropland","n.a.","n.a.","n.a.","n.a.",null,"Bahrain",157,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate dry High activity clay soils"},"Cool temperate dry","High activity clay soils",50,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist Full tillage Low"},"Annual cropland","Boreal moist","Full tillage","Low",0.69,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Sugar cane n.a. Warm temperate moist Subtropical humid forest North America n.a."},"Sugar cane","n.a.","Warm temperate moist","Subtropical humid forest","North America","n.a.",4.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Grassland and savannah n.a."},"Boreal moist","Grassland and savannah","n.a.","n.a.","n.a.","n.a.",null,"Bangladesh",8090,"medium"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate dry Low activity clay soils"},"Cool temperate dry","Low activity clay soils",33,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist Full tillage Medium"},"Annual cropland","Boreal moist","Full tillage","Medium",0.69,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Boreal dry n.a. n.a. n.a."},"All other annual crops","n.a.","Boreal dry","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Shifting cultivation shortened fallow n.a."},"Boreal moist","Shifting cultivation shortened fallow","n.a.","n.a.","n.a.","n.a.",null,"Barbados",296,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate dry Sandy soils"},"Cool temperate dry","Sandy soils",34,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist Full tillage High with manure"},"Annual cropland","Boreal moist","Full tillage","High with manure",0.69,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Boreal moist n.a. n.a. n.a."},"All other annual crops","n.a.","Boreal moist","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Shifting cultivation mature fallow n.a."},"Boreal moist","Shifting cultivation mature fallow","n.a.","n.a.","n.a.","n.a.",null,"Belarus",5890,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate dry Spodic soils"},"Cool temperate dry","Spodic soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist Full tillage High without manure"},"Annual cropland","Boreal moist","Full tillage","High without manure",0.69,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Cool temperate dry n.a. n.a. n.a."},"All other annual crops","n.a.","Cool temperate dry","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Native forest non degraded Nutrient rich"},"Boreal moist","Native forest non degraded","Nutrient rich",0.6,0.16,2.4,null,"Belgium",1770,"vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate dry Volcanic soils"},"Cool temperate dry","Volcanic soils",20,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist Reduced tillage Low"},"Annual cropland","Boreal moist","Reduced tillage","Low",0.69,1.08,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Cool temperate moist n.a. n.a. n.a."},"All other annual crops","n.a.","Cool temperate moist","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Native forest non degraded Nutrient poor"},"Boreal moist","Native forest non degraded","Nutrient poor",0.1,0.02,0.3,null,"Belize","71 090","very high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate dry Wetland soils"},"Cool temperate dry","Wetland soils",87,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist Reduced tillage Medium"},"Annual cropland","Boreal moist","Reduced tillage","Medium",0.69,1.08,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Warm temperate dry n.a. n.a. n.a."},"All other annual crops","n.a.","Warm temperate dry","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Managed forest Nutrient rich"},"Boreal moist","Managed forest","Nutrient rich",0.6,0.16,2.4,null,"Benin","3 820","very high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate moist High activity clay soils"},"Cool temperate moist","High activity clay soils",95,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist Reduced tillage High with manure"},"Annual cropland","Boreal moist","Reduced tillage","High with manure",0.69,1.08,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Warm temperate moist n.a. n.a. n.a."},"All other annual crops","n.a.","Warm temperate moist","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Boreal moist Managed forest Nutrient poor"},"Boreal moist","Managed forest","Nutrient poor",0.1,0.02,0.3,null,"Bhutan",40860,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate moist Low activity clay soils"},"Cool temperate moist","Low activity clay soils",85,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist Reduced tillage High without manure"},"Annual cropland","Boreal moist","Reduced tillage","High without manure",0.69,1.08,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Tropical dry n.a. n.a. n.a."},"All other annual crops","n.a.","Tropical dry","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Annual cropland n.a."},"Cool temperate dry","Annual cropland","n.a.",8,2,24,null,"Bolivia",69380,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate moist Sandy soils"},"Cool temperate moist","Sandy soils",71,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist No till Low"},"Annual cropland","Boreal moist","No till","Low",0.69,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Tropical moist n.a. n.a. n.a."},"All other annual crops","n.a.","Tropical moist","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Perennial cropland n.a."},"Cool temperate dry","Perennial cropland","n.a.",8,2,24,null,"Bosnia and Herzegovina",8960,"medium"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate moist Spodic soils"},"Cool temperate moist","Spodic soils",115,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist No till Medium"},"Annual cropland","Boreal moist","No till","Medium",0.69,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Tropical wet n.a. n.a. n.a."},"All other annual crops","n.a.","Tropical wet","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Grassland and savannah n.a."},"Cool temperate dry","Grassland and savannah","n.a.",8,2,24,null,"Botswana",6820,"medium"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate moist Volcanic soils"},"Cool temperate moist","Volcanic soils",130,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist No till High with manure"},"Annual cropland","Boreal moist","No till","High with manure",0.69,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other annual crops n.a. Tropical montane n.a. n.a. n.a."},"All other annual crops","n.a.","Tropical montane","n.a.","n.a.","n.a.",0,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Shifting cultivation shortened fallow n.a."},"Cool temperate dry","Shifting cultivation shortened fallow","n.a.",8,2,24,null,"Brazil",45570,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Cool temperate moist Wetland soils"},"Cool temperate moist","Wetland soils",87,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Boreal moist No till High without manure"},"Annual cropland","Boreal moist","No till","High without manure",0.69,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Boreal dry n.a. n.a. n.a."},"Coconut","n.a.","Boreal dry","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Shifting cultivation mature fallow n.a."},"Cool temperate dry","Shifting cultivation mature fallow","n.a.",8,2,24,null,"Brunei Darussalam",23220,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate dry High activity clay soils"},"Warm temperate dry","High activity clay soils",38,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry Full tillage Low"},"Annual cropland","Cool temperate dry","Full tillage","Low",0.8,1,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Boreal moist n.a. n.a. n.a."},"Coconut","n.a.","Boreal moist","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Native forest non degraded Nutrient rich"},"Cool temperate dry","Native forest non degraded","Nutrient rich",0.6,0.16,2.4,null,"Bulgaria",2720,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate dry Low activity clay soils"},"Warm temperate dry","Low activity clay soils",24,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry Full tillage Medium"},"Annual cropland","Cool temperate dry","Full tillage","Medium",0.8,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Cool temperate dry n.a. n.a. n.a."},"Coconut","n.a.","Cool temperate dry","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Native forest non degraded Nutrient poor"},"Cool temperate dry","Native forest non degraded","Nutrient poor",0.1,0.02,0.3,null,"Burkina Faso",930,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate dry Sandy soils"},"Warm temperate dry","Sandy soils",19,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry Full tillage High with manure"},"Annual cropland","Cool temperate dry","Full tillage","High with manure",0.8,1,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Cool temperate moist n.a. n.a. n.a."},"Coconut","n.a.","Cool temperate moist","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Managed forest Nutrient rich"},"Cool temperate dry","Managed forest","Nutrient rich",0.6,0.16,2.4,null,"Burundi",2190,"vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate dry Spodic soils"},"Warm temperate dry","Spodic soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry Full tillage High without manure"},"Annual cropland","Cool temperate dry","Full tillage","High without manure",0.8,1,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Warm temperate dry n.a. n.a. n.a."},"Coconut","n.a.","Warm temperate dry","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate dry Managed forest Nutrient poor"},"Cool temperate dry","Managed forest","Nutrient poor",0.1,0.02,0.3,null,"Cambodia",32880,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate dry Volcanic soils"},"Warm temperate dry","Volcanic soils",70,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry Reduced tillage Low"},"Annual cropland","Cool temperate dry","Reduced tillage","Low",0.8,1.02,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Warm temperate moist n.a. n.a. n.a."},"Coconut","n.a.","Warm temperate moist","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Annual cropland n.a."},"Cool temperate moist","Annual cropland","n.a.",8,2,24,null,"Cameroon",17520,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate dry Wetland soils"},"Warm temperate dry","Wetland soils",88,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry Reduced tillage Medium"},"Annual cropland","Cool temperate dry","Reduced tillage","Medium",0.8,1.02,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Tropical dry n.a. n.a. n.a."},"Coconut","n.a.","Tropical dry","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Perennial cropland n.a."},"Cool temperate moist","Perennial cropland","n.a.",8,2,24,null,"Canada",91420,"very high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate moist High activity clay soils"},"Warm temperate moist","High activity clay soils",88,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry Reduced tillage High with manure"},"Annual cropland","Cool temperate dry","Reduced tillage","High with manure",0.8,1.02,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Tropical moist n.a. n.a. n.a."},"Coconut","n.a.","Tropical moist","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Grassland and savannah n.a."},"Cool temperate moist","Grassland and savannah","n.a.",8,2,24,null,"Cape Verde",630,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate moist Low activity clay soils"},"Warm temperate moist","Low activity clay soils",63,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry Reduced tillage High without manure"},"Annual cropland","Cool temperate dry","Reduced tillage","High without manure",0.8,1.02,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Tropical wet n.a. n.a. n.a."},"Coconut","n.a.","Tropical wet","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Shifting cultivation shortened fallow n.a."},"Cool temperate moist","Shifting cultivation shortened fallow","n.a.",8,2,24,null,"Central African Rep.",36910,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate moist Sandy soils"},"Warm temperate moist","Sandy soils",34,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry No till Low"},"Annual cropland","Cool temperate dry","No till","Low",0.8,1.1000000000000001,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Coconut n.a. Tropical montane n.a. n.a. n.a."},"Coconut","n.a.","Tropical montane","n.a.","n.a.","n.a.",75,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Shifting cultivation mature fallow n.a."},"Cool temperate moist","Shifting cultivation mature fallow","n.a.",8,2,24,null,"Chad",4860,{"$f":"IF(AY37<1000,\"scarce\",IF(AY37<1700,\"stress\",IF(AY37<2500,\"vulnerable\",IF(AY37<6000,\"low but not vulnerable\",IF(AY37<15000,\"medium\",IF(AY37<70000,\"high\",\"very high\"))))))","v":"low but not vulnerable"}]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate moist Spodic soils"},"Warm temperate moist","Spodic soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry No till Medium"},"Annual cropland","Cool temperate dry","No till","Medium",0.8,1.1000000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Boreal dry n.a. n.a. n.a."},"Jatropha","n.a.","Boreal dry","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Native forest non degraded Nutrient rich"},"Cool temperate moist","Native forest non degraded","Nutrient rich",0.6,0.16,2.4,null,"Chile",57640,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate moist Volcanic soils"},"Warm temperate moist","Volcanic soils",80,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry No till High with manure"},"Annual cropland","Cool temperate dry","No till","High with manure",0.8,1.1000000000000001,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Boreal moist n.a. n.a. n.a."},"Jatropha","n.a.","Boreal moist","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Native forest non degraded Nutrient poor"},"Cool temperate moist","Native forest non degraded","Nutrient poor",0.1,0.02,0.3,null,"China",2140,"vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Warm temperate moist Wetland soils"},"Warm temperate moist","Wetland soils",88,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate dry No till High without manure"},"Annual cropland","Cool temperate dry","No till","High without manure",0.8,1.1000000000000001,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Cool temperate dry n.a. n.a. n.a."},"Jatropha","n.a.","Cool temperate dry","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Managed forest Nutrient rich"},"Cool temperate moist","Managed forest","Nutrient rich",0.6,0.16,2.4,null,"China, Taiwan Prov.",2930,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical dry High activity clay soils"},"Tropical dry","High activity clay soils",38,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist Full tillage Low"},"Annual cropland","Cool temperate moist","Full tillage","Low",0.69,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Cool temperate moist n.a. n.a. n.a."},"Jatropha","n.a.","Cool temperate moist","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Cool temperate moist Managed forest Nutrient poor"},"Cool temperate moist","Managed forest","Nutrient poor",0.1,0.02,0.3,null,"Colombia",47470,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical dry Low activity clay soils"},"Tropical dry","Low activity clay soils",35,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist Full tillage Medium"},"Annual cropland","Cool temperate moist","Full tillage","Medium",0.69,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Warm temperate dry n.a. n.a. n.a."},"Jatropha","n.a.","Warm temperate dry","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Annual cropland n.a."},"Warm temperate dry","Annual cropland","n.a.",8,2,24,null,"Comoros",1520,"stress"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical dry Sandy soils"},"Tropical dry","Sandy soils",31,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist Full tillage High with manure"},"Annual cropland","Cool temperate moist","Full tillage","High with manure",0.69,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Warm temperate moist n.a. n.a. n.a."},"Jatropha","n.a.","Warm temperate moist","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Perennial cropland n.a."},"Warm temperate dry","Perennial cropland","n.a.",8,2,24,null,"Congo, Dem Rep.",23580,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical dry Spodic soils"},"Tropical dry","Spodic soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist Full tillage High without manure"},"Annual cropland","Cool temperate moist","Full tillage","High without manure",0.69,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Tropical dry n.a. n.a. n.a."},"Jatropha","n.a.","Tropical dry","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Grassland and savannah n.a."},"Warm temperate dry","Grassland and savannah","n.a.",8,2,24,null,"Congo",217920,"very high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical dry Volcanic soils"},"Tropical dry","Volcanic soils",50,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist Reduced tillage Low"},"Annual cropland","Cool temperate moist","Reduced tillage","Low",0.69,1.08,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Tropical moist n.a. n.a. n.a."},"Jatropha","n.a.","Tropical moist","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Shifting cultivation shortened fallow n.a."},"Warm temperate dry","Shifting cultivation shortened fallow","n.a.",8,2,24,null,"Costa Rica",26450,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical dry Wetland soils"},"Tropical dry","Wetland soils",86,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist Reduced tillage Medium"},"Annual cropland","Cool temperate moist","Reduced tillage","Medium",0.69,1.08,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Tropical wet n.a. n.a. n.a."},"Jatropha","n.a.","Tropical wet","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Shifting cultivation mature fallow n.a."},"Warm temperate dry","Shifting cultivation mature fallow","n.a.",8,2,24,null,"Côte d'Ivoire",4790,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical moist High activity clay soils"},"Tropical moist","High activity clay soils",65,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist Reduced tillage High with manure"},"Annual cropland","Cool temperate moist","Reduced tillage","High with manure",0.69,1.08,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jatropha n.a. Tropical montane n.a. n.a. n.a."},"Jatropha","n.a.","Tropical montane","n.a.","n.a.","n.a.",17.5,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Native forest non degraded Nutrient rich"},"Warm temperate dry","Native forest non degraded","Nutrient rich",0.6,0.16,2.4,null,"Croatia",23890,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical moist Low activity clay soils"},"Tropical moist","Low activity clay soils",47,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist Reduced tillage High without manure"},"Annual cropland","Cool temperate moist","Reduced tillage","High without manure",0.69,1.08,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Boreal dry n.a. n.a. n.a."},"Jojoba","n.a.","Boreal dry","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Native forest non degraded Nutrient poor"},"Warm temperate dry","Native forest non degraded","Nutrient poor",0.1,0.02,0.3,null,"Cuba",3370,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical moist Sandy soils"},"Tropical moist","Sandy soils",39,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist No till Low"},"Annual cropland","Cool temperate moist","No till","Low",0.69,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Boreal moist n.a. n.a. n.a."},"Jojoba","n.a.","Boreal moist","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Managed forest Nutrient rich"},"Warm temperate dry","Managed forest","Nutrient rich",0.6,0.16,2.4,null,"Cyprus",970,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical moist Spodic soils"},"Tropical moist","Spodic soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist No till Medium"},"Annual cropland","Cool temperate moist","No till","Medium",0.69,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Cool temperate dry n.a. n.a. n.a."},"Jojoba","n.a.","Cool temperate dry","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate dry Managed forest Nutrient poor"},"Warm temperate dry","Managed forest","Nutrient poor",0.1,0.02,0.3,null,"Czech Rep",1290,"stress"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical moist Volcanic soils"},"Tropical moist","Volcanic soils",70,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist No till High with manure"},"Annual cropland","Cool temperate moist","No till","High with manure",0.69,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Cool temperate moist n.a. n.a. n.a."},"Jojoba","n.a.","Cool temperate moist","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Annual cropland n.a."},"Warm temperate moist","Annual cropland","n.a.",8,2,24,null,"Denmark",1120,"stress"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical moist Wetland soils"},"Tropical moist","Wetland soils",86,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Cool temperate moist No till High without manure"},"Annual cropland","Cool temperate moist","No till","High without manure",0.69,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Warm temperate dry n.a. n.a. n.a."},"Jojoba","n.a.","Warm temperate dry","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Perennial cropland n.a."},"Warm temperate moist","Perennial cropland","n.a.",8,2,24,null,"Djibouti",420,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical wet High activity clay soils"},"Tropical wet","High activity clay soils",44,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry Full tillage Low"},"Annual cropland","Warm temperate dry","Full tillage","Low",0.8,1,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Warm temperate moist n.a. n.a. n.a."},"Jojoba","n.a.","Warm temperate moist","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Grassland and savannah n.a."},"Warm temperate moist","Grassland and savannah","n.a.",8,2,24,null,"Dominican Republic",2370,"vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical wet Low activity clay soils"},"Tropical wet","Low activity clay soils",60,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry Full tillage Medium"},"Annual cropland","Warm temperate dry","Full tillage","Medium",0.8,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Tropical dry n.a. n.a. n.a."},"Jojoba","n.a.","Tropical dry","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Shifting cultivation shortened fallow n.a."},"Warm temperate moist","Shifting cultivation shortened fallow","n.a.",8,2,24,null,"Ecuador",32170,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical wet Sandy soils"},"Tropical wet","Sandy soils",66,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry Full tillage High with manure"},"Annual cropland","Warm temperate dry","Full tillage","High with manure",0.8,1,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Tropical moist n.a. n.a. n.a."},"Jojoba","n.a.","Tropical moist","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Shifting cultivation mature fallow n.a."},"Warm temperate moist","Shifting cultivation mature fallow","n.a.",8,2,24,null,"Egypt",790,"scarce"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical wet Spodic soils"},"Tropical wet","Spodic soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry Full tillage High without manure"},"Annual cropland","Warm temperate dry","Full tillage","High without manure",0.8,1,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Tropical wet n.a. n.a. n.a."},"Jojoba","n.a.","Tropical wet","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Native forest non degraded Nutrient rich"},"Warm temperate moist","Native forest non degraded","Nutrient rich",0.6,0.16,2.4,null,"El Salvador",3810,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical wet Volcanic soils"},"Tropical wet","Volcanic soils",130,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry Reduced tillage Low"},"Annual cropland","Warm temperate dry","Reduced tillage","Low",0.8,1.02,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Jojoba n.a. Tropical montane n.a. n.a. n.a."},"Jojoba","n.a.","Tropical montane","n.a.","n.a.","n.a.",2.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Native forest non degraded Nutrient poor"},"Warm temperate moist","Native forest non degraded","Nutrient poor",0.1,0.02,0.3,null,"Equatorial Guinea",51280,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical wet Wetland soils"},"Tropical wet","Wetland soils",86,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry Reduced tillage Medium"},"Annual cropland","Warm temperate dry","Reduced tillage","Medium",0.8,1.02,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Boreal dry n.a. n.a. n.a."},"Oil palm","n.a.","Boreal dry","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Managed forest Nutrient rich"},"Warm temperate moist","Managed forest","Nutrient rich",0.6,0.16,2.4,null,"Eritrea",1470,"stress"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical montane High activity clay soils"},"Tropical montane","High activity clay soils",88,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry Reduced tillage High with manure"},"Annual cropland","Warm temperate dry","Reduced tillage","High with manure",0.8,1.02,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Boreal moist n.a. n.a. n.a."},"Oil palm","n.a.","Boreal moist","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Warm temperate moist Managed forest Nutrient poor"},"Warm temperate moist","Managed forest","Nutrient poor",0.1,0.02,0.3,null,"Estonia",9790,"medium"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical montane Low activity clay soils"},"Tropical montane","Low activity clay soils",63,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry Reduced tillage High without manure"},"Annual cropland","Warm temperate dry","Reduced tillage","High without manure",0.8,1.02,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Cool temperate dry n.a. n.a. n.a."},"Oil palm","n.a.","Cool temperate dry","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical dry Annual cropland n.a."},"Tropical dry","Annual cropland","n.a.",16,5,48,null,"Ethiopia",1680,"stress"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical montane Sandy soils"},"Tropical montane","Sandy soils",34,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry No till Low"},"Annual cropland","Warm temperate dry","No till","Low",0.8,1.1000000000000001,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Cool temperate moist n.a. n.a. n.a."},"Oil palm","n.a.","Cool temperate moist","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical dry Perennial cropland n.a."},"Tropical dry","Perennial cropland","n.a.",16,5,48,null,"Fiji",33710,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical montane Spodic soils"},"Tropical montane","Spodic soils","n.a.",null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry No till Medium"},"Annual cropland","Warm temperate dry","No till","Medium",0.8,1.1000000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Warm temperate dry n.a. n.a. n.a."},"Oil palm","n.a.","Warm temperate dry","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical dry Grassland and savannah n.a."},"Tropical dry","Grassland and savannah","n.a.",16,5,48,null,"Finland",21090,"high"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical montane Volcanic soils"},"Tropical montane","Volcanic soils",80,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry No till High with manure"},"Annual cropland","Warm temperate dry","No till","High with manure",0.8,1.1000000000000001,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Warm temperate moist n.a. n.a. n.a."},"Oil palm","n.a.","Warm temperate moist","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical dry Shifting cultivation shortened fallow n.a."},"Tropical dry","Shifting cultivation shortened fallow","n.a.",16,5,48,null,"France",3370,"low but not vulnerable"]
[null,null,{"$f":"Table_IPCC_SOC[[#This Row],[Climate region]]&\" \"&Table_IPCC_SOC[[#This Row],[Soil type]]","v":"Tropical montane Wetland soils"},"Tropical montane","Wetland soils",86,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate dry No till High without manure"},"Annual cropland","Warm temperate dry","No till","High without manure",0.8,1.1000000000000001,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Tropical dry n.a. n.a. n.a."},"Oil palm","n.a.","Tropical dry","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical dry Shifting cultivation mature fallow n.a."},"Tropical dry","Shifting cultivation mature fallow","n.a.",16,5,48,null,"French Guiana",736260,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist Full tillage Low"},"Annual cropland","Warm temperate moist","Full tillage","Low",0.69,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Tropical moist n.a. n.a. n.a."},"Oil palm","n.a.","Tropical moist","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical dry Native forest non degraded n.a."},"Tropical dry","Native forest non degraded","n.a.",8,0,24,null,"Gabon",121390,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist Full tillage Medium"},"Annual cropland","Warm temperate moist","Full tillage","Medium",0.69,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Tropical wet n.a. n.a. n.a."},"Oil palm","n.a.","Tropical wet","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical dry Managed forest n.a."},"Tropical dry","Managed forest","n.a.",8,0,24,null,"Gambia",5470,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist Full tillage High with manure"},"Annual cropland","Warm temperate moist","Full tillage","High with manure",0.69,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Oil palm n.a. Tropical montane n.a. n.a. n.a."},"Oil palm","n.a.","Tropical montane","n.a.","n.a.","n.a.",60,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical moist Annual cropland n.a."},"Tropical moist","Annual cropland","n.a.",16,5,48,null,"Gaza Strip, Palestinian Territories",41,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist Full tillage High without manure"},"Annual cropland","Warm temperate moist","Full tillage","High without manure",0.69,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other perennial crops n.a. Cool temperate dry n.a. n.a. n.a."},"All other perennial crops","n.a.","Cool temperate dry","n.a.","n.a.","n.a.",43.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical moist Perennial cropland n.a."},"Tropical moist","Perennial cropland","n.a.",16,5,48,null,"Georgia",12480,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist Reduced tillage Low"},"Annual cropland","Warm temperate moist","Reduced tillage","Low",0.69,1.08,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other perennial crops n.a. Cool temperate moist n.a. n.a. n.a."},"All other perennial crops","n.a.","Cool temperate moist","n.a.","n.a.","n.a.",43.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical moist Grassland and savannah n.a."},"Tropical moist","Grassland and savannah","n.a.",16,5,48,null,"Germany",1870,{"$f":"IF(AY69<1000,\"scarce\",IF(AY69<1700,\"stress\",IF(AY69<2500,\"vulnerable\",IF(AY69<6000,\"low but not vulnerable\",IF(AY69<15000,\"medium\",IF(AY69<70000,\"high\",\"very high\"))))))","v":"vulnerable"}]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist Reduced tillage Medium"},"Annual cropland","Warm temperate moist","Reduced tillage","Medium",0.69,1.08,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other perennial crops n.a. Warm temperate dry n.a. n.a. n.a."},"All other perennial crops","n.a.","Warm temperate dry","n.a.","n.a.","n.a.",43.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical moist Shifting cultivation shortened fallow n.a."},"Tropical moist","Shifting cultivation shortened fallow","n.a.",16,5,48,null,"Ghana",2490,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist Reduced tillage High with manure"},"Annual cropland","Warm temperate moist","Reduced tillage","High with manure",0.69,1.08,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other perennial crops n.a. Warm temperate moist n.a. n.a. n.a."},"All other perennial crops","n.a.","Warm temperate moist","n.a.","n.a.","n.a.",43.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical moist Shifting cultivation mature fallow n.a."},"Tropical moist","Shifting cultivation mature fallow","n.a.",16,5,48,null,"Greece",6760,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist Reduced tillage High without manure"},"Annual cropland","Warm temperate moist","Reduced tillage","High without manure",0.69,1.08,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other perennial crops n.a. Tropical dry n.a. n.a. n.a."},"All other perennial crops","n.a.","Tropical dry","n.a.","n.a.","n.a.",6.2,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical moist Native forest non degraded n.a."},"Tropical moist","Native forest non degraded","n.a.",8,0,24,null,"Greenland",10578950,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist No till Low"},"Annual cropland","Warm temperate moist","No till","Low",0.69,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other perennial crops n.a. Tropical moist n.a. n.a. n.a."},"All other perennial crops","n.a.","Tropical moist","n.a.","n.a.","n.a.",14.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical moist Managed forest n.a."},"Tropical moist","Managed forest","n.a.",8,0,24,null,"Guatemala",8790,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist No till Medium"},"Annual cropland","Warm temperate moist","No till","Medium",0.69,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"All other perennial crops n.a. Tropical wet n.a. n.a. n.a."},"All other perennial crops","n.a.","Tropical wet","n.a.","n.a.","n.a.",34.299999999999997,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical wet Annual cropland n.a."},"Tropical wet","Annual cropland","n.a.",16,5,48,null,"Guinea",26220,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist No till High with manure"},"Annual cropland","Warm temperate moist","No till","High with manure",0.69,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Boreal dry n.a. n.a. n.a."},"Grassland and savannah","n.a.","Boreal dry","n.a.","n.a.","n.a.",4.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical wet Perennial cropland n.a."},"Tropical wet","Perennial cropland","n.a.",16,5,48,null,"Guinea-Bissau",20160,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Warm temperate moist No till High without manure"},"Annual cropland","Warm temperate moist","No till","High without manure",0.69,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Boreal moist n.a. n.a. n.a."},"Grassland and savannah","n.a.","Boreal moist","n.a.","n.a.","n.a.",4.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical wet Grassland and savannah n.a."},"Tropical wet","Grassland and savannah","n.a.",16,5,48,null,"Guyana",314210,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry Full tillage Low"},"Annual cropland","Tropical dry","Full tillage","Low",0.57999999999999996,1,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Cool temperate dry n.a. n.a. n.a."},"Grassland and savannah","n.a.","Cool temperate dry","n.a.","n.a.","n.a.",3.3,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical wet Shifting cultivation shortened fallow n.a."},"Tropical wet","Shifting cultivation shortened fallow","n.a.",16,5,48,null,"Haiti",1660,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry Full tillage Medium"},"Annual cropland","Tropical dry","Full tillage","Medium",0.57999999999999996,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Cool temperate moist n.a. n.a. n.a."},"Grassland and savannah","n.a.","Cool temperate moist","n.a.","n.a.","n.a.",6.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical wet Shifting cultivation mature fallow n.a."},"Tropical wet","Shifting cultivation mature fallow","n.a.",16,5,48,null,"Honduras",13510,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry Full tillage High with manure"},"Annual cropland","Tropical dry","Full tillage","High with manure",0.57999999999999996,1,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Warm temperate dry n.a. n.a. n.a."},"Grassland and savannah","n.a.","Warm temperate dry","n.a.","n.a.","n.a.",3.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical wet Native forest non degraded n.a."},"Tropical wet","Native forest non degraded","n.a.",8,0,24,null,"Hungary",10580,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry Full tillage High without manure"},"Annual cropland","Tropical dry","Full tillage","High without manure",0.57999999999999996,1,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Warm temperate moist n.a. n.a. n.a."},"Grassland and savannah","n.a.","Warm temperate moist","n.a.","n.a.","n.a.",6.8,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical wet Managed forest n.a."},"Tropical wet","Managed forest","n.a.",8,0,24,null,"Iceland",582190,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry Reduced tillage Low"},"Annual cropland","Tropical dry","Reduced tillage","Low",0.57999999999999996,1.0900000000000001,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Tropical dry n.a. n.a. n.a."},"Grassland and savannah","n.a.","Tropical dry","n.a.","n.a.","n.a.",4.4000000000000004,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical montane Annual cropland n.a."},"Tropical montane","Annual cropland","n.a.",16,5,48,null,"India",1750,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry Reduced tillage Medium"},"Annual cropland","Tropical dry","Reduced tillage","Medium",0.57999999999999996,1.0900000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Tropical moist n.a. n.a. n.a."},"Grassland and savannah","n.a.","Tropical moist","n.a.","n.a.","n.a.",8.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical montane Perennial cropland n.a."},"Tropical montane","Perennial cropland","n.a.",16,5,48,null,"Indonesia",12750,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry Reduced tillage High with manure"},"Annual cropland","Tropical dry","Reduced tillage","High with manure",0.57999999999999996,1.0900000000000001,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Grassland and savannah n.a. Tropical wet n.a. n.a. n.a."},"Grassland and savannah","n.a.","Tropical wet","n.a.","n.a.","n.a.",8.1,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical montane Grassland and savannah n.a."},"Tropical montane","Grassland and savannah","n.a.",16,5,48,null,"Iran, Islamic Rep.",1970,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry Reduced tillage High without manure"},"Annual cropland","Tropical dry","Reduced tillage","High without manure",0.57999999999999996,1.0900000000000001,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Miscanthus n.a. Warm temperate dry Subtropical dry forest Europe n.a."},"Miscanthus","n.a.","Warm temperate dry","Subtropical dry forest","Europe","n.a.",10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical montane Shifting cultivation shortened fallow n.a."},"Tropical montane","Shifting cultivation shortened fallow","n.a.",16,5,48,null,"Iraq",2920,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry No till Low"},"Annual cropland","Tropical dry","No till","Low",0.57999999999999996,1.17,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Miscanthus n.a. Warm temperate dry Subtropical dry forest North America n.a."},"Miscanthus","n.a.","Warm temperate dry","Subtropical dry forest","North America","n.a.",14.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical montane Shifting cultivation mature fallow n.a."},"Tropical montane","Shifting cultivation mature fallow","n.a.",16,5,48,null,"Ireland",13000,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry No till Medium"},"Annual cropland","Tropical dry","No till","Medium",0.57999999999999996,1.17,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Miscanthus n.a. Warm temperate dry Subtropical steppe North America n.a."},"Miscanthus","n.a.","Warm temperate dry","Subtropical steppe","North America","n.a.",14.9,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical montane Native forest non degraded n.a."},"Tropical montane","Native forest non degraded","n.a.",8,0,24,null,"Israel",250,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry No till High with manure"},"Annual cropland","Tropical dry","No till","High with manure",0.57999999999999996,1.17,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Tropical n.a. n.a. Africa n.a."},"Scrubland","Tropical","n.a.","n.a.","Africa","n.a.",46,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF2 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Climate region]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]&\" \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Nutrient level]]","v":"EF2 Tropical montane Managed forest n.a."},"Tropical montane","Managed forest","n.a.",8,0,24,null,"Italy",3340,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical dry No till High without manure"},"Annual cropland","Tropical dry","No till","High without manure",0.57999999999999996,1.17,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Tropical n.a. n.a. North America n.a."},"Scrubland","Tropical","n.a.","n.a.","North America","n.a.",53,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF3 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]","v":"EF3 Cattle poultry pigs"},null,"Cattle poultry pigs",null,0.02,7.0000000000000001E-3,0.06,null,"Jamaica",3510,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist Full tillage Low"},"Annual cropland","Tropical moist","Full tillage","Low",0.48,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Tropical n.a. n.a. Central and South America n.a."},"Scrubland","Tropical","n.a.","n.a.","Central and South America","n.a.",53,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"\"EF3 \"&Table_IPCC_emissionfactorsN2O[[#This Row],[Land use]]","v":"EF3 Sheep and other"},null,"Sheep and other",null,0.01,3.0000000000000001E-3,0.03,null,"Japan",3360,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist Full tillage Medium"},"Annual cropland","Tropical moist","Full tillage","Medium",0.48,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Tropical n.a. n.a. Asia continental n.a."},"Scrubland","Tropical","n.a.","n.a.","Asia continental","n.a.",39,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EF4",null,null,null,0.01,2E-3,0.05,null,"Jordan",160,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist Full tillage High with manure"},"Annual cropland","Tropical moist","Full tillage","High with manure",0.48,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Tropical n.a. n.a. Asia insular n.a."},"Scrubland","Tropical","n.a.","n.a.","Asia insular","n.a.",46,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EF5",null,null,null,7.4999999999999997E-3,5.0000000000000001E-4,2.5000000000000001E-2,null,"Kazakhstan",7120,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist Full tillage High without manure"},"Annual cropland","Tropical moist","Full tillage","High without manure",0.48,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Tropical n.a. n.a. Australia n.a."},"Scrubland","Tropical","n.a.","n.a.","Australia","n.a.",46,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRACgasf",null,null,null,0.1,0.03,0.3,null,"Kenya",930,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist Reduced tillage Low"},"Annual cropland","Tropical moist","Reduced tillage","Low",0.48,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Subtropical n.a. n.a. Africa n.a."},"Scrubland","Subtropical","n.a.","n.a.","Africa","n.a.",43,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRACgasm",null,null,null,0.2,0.05,0.5,null,"Korea, Dem. People's Rep.",3390,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist Reduced tillage Medium"},"Annual cropland","Tropical moist","Reduced tillage","Medium",0.48,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Subtropical n.a. n.a. North America n.a."},"Scrubland","Subtropical","n.a.","n.a.","North America","n.a.",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FRACleach",null,null,null,0.3,0.1,0.8,null,"Korea, Rep.",1450,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist Reduced tillage High with manure"},"Annual cropland","Tropical moist","Reduced tillage","High with manure",0.48,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Subtropical n.a. n.a. Central and South America n.a."},"Scrubland","Subtropical","n.a.","n.a.","Central and South America","n.a.",50,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kuwait",8,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist Reduced tillage High without manure"},"Annual cropland","Tropical moist","Reduced tillage","High without manure",0.48,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Subtropical n.a. n.a. Asia continental n.a."},"Scrubland","Subtropical","n.a.","n.a.","Asia continental","n.a.",37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Kyrgyzstan",3950,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist No till Low"},"Annual cropland","Tropical moist","No till","Low",0.48,1.22,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Subtropical n.a. n.a. Europe n.a."},"Scrubland","Subtropical","n.a.","n.a.","Europe","n.a.",37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lao Peoples Dem. Rep.",57640,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist No till Medium"},"Annual cropland","Tropical moist","No till","Medium",0.48,1.22,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Subtropical n.a. n.a. Asia insular n.a."},"Scrubland","Subtropical","n.a.","n.a.","Asia insular","n.a.",43,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Latvia",15510,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist No till High with manure"},"Annual cropland","Tropical moist","No till","High with manure",0.48,1.22,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Scrubland Temperate n.a. n.a. Global n.a."},"Scrubland","Temperate","n.a.","n.a.","Global","n.a.",7.4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lebanon",1190,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical moist No till High without manure"},"Annual cropland","Tropical moist","No till","High without manure",0.48,1.22,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical rain forest Africa n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical rain forest","Africa","n.a.",40,0.37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lesotho",1680,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet Full tillage Low"},"Annual cropland","Tropical wet","Full tillage","Low",0.48,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical rain forest North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical rain forest","North America","n.a.",39,0.37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Liberia",66530,{"$f":"IF(AY101<1000,\"scarce\",IF(AY101<1700,\"stress\",IF(AY101<2500,\"vulnerable\",IF(AY101<6000,\"low but not vulnerable\",IF(AY101<15000,\"medium\",IF(AY101<70000,\"high\",\"very high\"))))))","v":"high"}]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet Full tillage Medium"},"Annual cropland","Tropical wet","Full tillage","Medium",0.48,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical rain forest Central and South America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical rain forest","Central and South America","n.a.",39,0.37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Libyan Arab Jamahiriya",106,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet Full tillage High with manure"},"Annual cropland","Tropical wet","Full tillage","High with manure",0.48,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical rain forest Asia continental n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical rain forest","Asia continental","n.a.",36,0.37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Lithuania",7280,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet Full tillage High without manure"},"Annual cropland","Tropical wet","Full tillage","High without manure",0.48,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical rain forest Asia insular n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical rain forest","Asia insular","n.a.",45,0.37,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Luxemburg",6750,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet Reduced tillage Low"},"Annual cropland","Tropical wet","Reduced tillage","Low",0.48,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical moist forest Africa n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical moist forest","Africa","n.a.",30,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Macedonia, Fr Yugoslav Rep.",3100,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet Reduced tillage Medium"},"Annual cropland","Tropical wet","Reduced tillage","Medium",0.48,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical moist forest North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical moist forest","North America","n.a.",26,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Madagascar",18830,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet Reduced tillage High with manure"},"Annual cropland","Tropical wet","Reduced tillage","High with manure",0.48,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical moist forest Central and South America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical moist forest","Central and South America","n.a.",26,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Malawi",1400,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet Reduced tillage High without manure"},"Annual cropland","Tropical wet","Reduced tillage","High without manure",0.48,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical moist forest Asia continental n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical moist forest","Asia continental","n.a.",21,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Malaysia",23320,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet No till Low"},"Annual cropland","Tropical wet","No till","Low",0.48,1.22,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical moist forest Asia insular n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical moist forest","Asia insular","n.a.",34,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Maldives",91,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet No till Medium"},"Annual cropland","Tropical wet","No till","Medium",0.48,1.22,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical dry forest Africa n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical dry forest","Africa","n.a.",14,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mali",7460,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet No till High with manure"},"Annual cropland","Tropical wet","No till","High with manure",0.48,1.22,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical dry forest North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical dry forest","North America","n.a.",25,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Malta",130,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical wet No till High without manure"},"Annual cropland","Tropical wet","No till","High without manure",0.48,1.22,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical dry forest Central and South America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical dry forest","Central and South America","n.a.",25,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mauritania",3830,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane Full tillage Low"},"Annual cropland","Tropical montane","Full tillage","Low",0.64,1,0.94,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical dry forest Asia continental n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical dry forest","Asia continental","n.a.",16,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mauritius",2230,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane Full tillage Medium"},"Annual cropland","Tropical montane","Full tillage","Medium",0.64,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical dry forest Asia insular n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical dry forest","Asia insular","n.a.",19,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mexico",4360,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane Full tillage High with manure"},"Annual cropland","Tropical montane","Full tillage","High with manure",0.64,1,1.41,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical mountain systems Africa n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical mountain systems","Africa","n.a.",13,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Moldova, Rep.",2730,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane Full tillage High without manure"},"Annual cropland","Tropical montane","Full tillage","High without manure",0.64,1,1.08,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical mountain systems North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical mountain systems","North America","n.a.",17,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mongolia",13230,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane Reduced tillage Low"},"Annual cropland","Tropical montane","Reduced tillage","Low",0.64,1.0900000000000001,0.94,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical mountain systems Central and South America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical mountain systems","Central and South America","n.a.",17,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Morocco",930,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane Reduced tillage Medium"},"Annual cropland","Tropical montane","Reduced tillage","Medium",0.64,1.0900000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical mountain systems Asia continental n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical mountain systems","Asia continental","n.a.",16,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Mozambique",11320,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane Reduced tillage High with manure"},"Annual cropland","Tropical montane","Reduced tillage","High with manure",0.64,1.0900000000000001,1.41,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Tropical n.a. Tropical mountain systems Asia insular n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Tropical","n.a.","Tropical mountain systems","Asia insular","n.a.",26,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Myanmar",20870,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane Reduced tillage High without manure"},"Annual cropland","Tropical montane","Reduced tillage","High without manure",0.64,1.0900000000000001,1.08,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical humid forest North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical humid forest","North America","n.a.",26,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Namibia",8810,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane No till Low"},"Annual cropland","Tropical montane","No till","Low",0.64,1.1599999999999999,0.94,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical humid forest Central and South America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical humid forest","Central and South America","n.a.",26,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nepal",8170,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane No till Medium"},"Annual cropland","Tropical montane","No till","Medium",0.64,1.1599999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical humid forest Asia continental n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical humid forest","Asia continental","n.a.",22,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Netherlands",5610,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane No till High with manure"},"Annual cropland","Tropical montane","No till","High with manure",0.64,1.1599999999999999,1.41,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical humid forest Asia insular n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical humid forest","Asia insular","n.a.",35,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"New Zealand",83760,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Annual cropland Tropical montane No till High without manure"},"Annual cropland","Tropical montane","No till","High without manure",0.64,1.1599999999999999,1.08,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical dry forest Africa n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical dry forest","Africa","n.a.",17,0.28000000000000003,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nicaragua",35140,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry Full tillage Low"},"Perennial cropland","Boreal dry","Full tillage","Low",1,1,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical dry forest North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical dry forest","North America","n.a.",26,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Niger",2710,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry Full tillage Medium"},"Perennial cropland","Boreal dry","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical dry forest Central and South America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical dry forest","Central and South America","n.a.",26,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Nigeria",2250,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry Full tillage High with manure"},"Perennial cropland","Boreal dry","Full tillage","High with manure",1,1,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical dry forest Asia continental n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical dry forest","Asia continental","n.a.",16,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Norway",83920,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry Full tillage High without manure"},"Perennial cropland","Boreal dry","Full tillage","High without manure",1,1,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical dry forest Asia insular n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical dry forest","Asia insular","n.a.",20,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Oman",340,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry Reduced tillage Low"},"Perennial cropland","Boreal dry","Reduced tillage","Low",1,1.02,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical steppe Africa n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical steppe","Africa","n.a.",9,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Pakistan","1 420","very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry Reduced tillage Medium"},"Perennial cropland","Boreal dry","Reduced tillage","Medium",1,1.02,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical steppe North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical steppe","North America","n.a.",10,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Panama",46580,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry Reduced tillage High with manure"},"Perennial cropland","Boreal dry","Reduced tillage","High with manure",1,1.02,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical steppe Central and South America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical steppe","Central and South America","n.a.",10,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Papua New Guinea",137250,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry Reduced tillage High without manure"},"Perennial cropland","Boreal dry","Reduced tillage","High without manure",1,1.02,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical steppe Asia continental n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical steppe","Asia continental","n.a.",7,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Paraguay",55830,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry No till Low"},"Perennial cropland","Boreal dry","No till","Low",1,1.1000000000000001,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Subtropical n.a. Subtropical steppe Asia insular n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Subtropical","n.a.","Subtropical steppe","Asia insular","n.a.",9,0.32,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Peru",69390,{"$f":"IF(AY133<1000,\"scarce\",IF(AY133<1700,\"stress\",IF(AY133<2500,\"vulnerable\",IF(AY133<6000,\"low but not vulnerable\",IF(AY133<15000,\"medium\",IF(AY133<70000,\"high\",\"very high\"))))))","v":"high"}]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry No till Medium"},"Perennial cropland","Boreal dry","No till","Medium",1,1.1000000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate oceanic forest Europe n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate oceanic forest","Europe","n.a.",14,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Philippines","5 880","very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry No till High with manure"},"Perennial cropland","Boreal dry","No till","High with manure",1,1.1000000000000001,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate oceanic forest North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate oceanic forest","North America","n.a.",79,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Poland",1600,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal dry No till High without manure"},"Perennial cropland","Boreal dry","No till","High without manure",1,1.1000000000000001,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate oceanic forest New Zealand n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate oceanic forest","New Zealand","n.a.",43,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Portugal",6820,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist Full tillage Low"},"Perennial cropland","Boreal moist","Full tillage","Low",1,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate oceanic forest Central and South America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate oceanic forest","Central and South America","n.a.",21,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Puerto Rico",1820,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist Full tillage Medium"},"Perennial cropland","Boreal moist","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest Asia continental <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","Asia continental","<= 20 y",2,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Qatar",86,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist Full tillage High with manure"},"Perennial cropland","Boreal moist","Full tillage","High with manure",1,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest Asia continental > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","Asia continental","> 20 y",14,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Reunion",6520,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist Full tillage High without manure"},"Perennial cropland","Boreal moist","Full tillage","High without manure",1,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest Asia insular <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","Asia insular","<= 20 y",2,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Romania",9510,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist Reduced tillage Low"},"Perennial cropland","Boreal moist","Reduced tillage","Low",1,1.08,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest Asia insular > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","Asia insular","> 20 y",14,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Russian Federation",31650,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist Reduced tillage Medium"},"Perennial cropland","Boreal moist","Reduced tillage","Medium",1,1.08,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest Europe <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","Europe","<= 20 y",2,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Rwanda",610,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist Reduced tillage High with manure"},"Perennial cropland","Boreal moist","Reduced tillage","High with manure",1,1.08,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest Europe > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","Europe","> 20 y",14,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Saint Kitts and Nevis",560,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist Reduced tillage High without manure"},"Perennial cropland","Boreal moist","Reduced tillage","High without manure",1,1.08,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest North America <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","North America","<= 20 y",7,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sao Tome and Principe",13210,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist No till Low"},"Perennial cropland","Boreal moist","No till","Low",1,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest North America > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","North America","> 20 y",16,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Saudi Arabia",96,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist No till Medium"},"Perennial cropland","Boreal moist","No till","Medium",1,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest Central and South America <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","Central and South America","<= 20 y",7,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Senegal",3810,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist No till High with manure"},"Perennial cropland","Boreal moist","No till","High with manure",1,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate continental forest Central and South America > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate continental forest","Central and South America","> 20 y",16,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Serbia and Montenegro",19820,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Boreal moist No till High without manure"},"Perennial cropland","Boreal moist","No till","High without manure",1,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems Asia continental <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","Asia continental","<= 20 y",12,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sierra Leone",30960,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry Full tillage Low"},"Perennial cropland","Cool temperate dry","Full tillage","Low",1,1,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems Asia continental > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","Asia continental","> 20 y",16,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Singapore",139,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry Full tillage Medium"},"Perennial cropland","Cool temperate dry","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems Asia insular <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","Asia insular","<= 20 y",12,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Slovakia",9270,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry Full tillage High with manure"},"Perennial cropland","Cool temperate dry","Full tillage","High with manure",1,1,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems Asia insular > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","Asia insular","> 20 y",16,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Slovenia",16080,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry Full tillage High without manure"},"Perennial cropland","Cool temperate dry","Full tillage","High without manure",1,1,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems Europe <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","Europe","<= 20 y",12,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Solomon Islands",91040,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry Reduced tillage Low"},"Perennial cropland","Cool temperate dry","Reduced tillage","Low",1,1.02,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems Europe > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","Europe","> 20 y",16,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Somalia",1380,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry Reduced tillage Medium"},"Perennial cropland","Cool temperate dry","Reduced tillage","Medium",1,1.02,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems North America <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","North America","<= 20 y",6,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"South Africa",1110,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry Reduced tillage High with manure"},"Perennial cropland","Cool temperate dry","Reduced tillage","High with manure",1,1.02,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems North America > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","North America","> 20 y",6,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Spain",2710,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry Reduced tillage High without manure"},"Perennial cropland","Cool temperate dry","Reduced tillage","High without manure",1,1.02,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems Central and South America <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","Central and South America","<= 20 y",6,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sri Lanka",2600,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry No till Low"},"Perennial cropland","Cool temperate dry","No till","Low",1,1.1000000000000001,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Temperate n.a. Temperate mountain systems Central and South America > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Temperate","n.a.","Temperate mountain systems","Central and South America","> 20 y",6,0.27,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sudan",1880,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry No till Medium"},"Perennial cropland","Cool temperate dry","No till","Medium",1,1.1000000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal coniferous forest Asia continental n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal coniferous forest","Asia continental","n.a.",12,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Suriname",277900,"very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry No till High with manure"},"Perennial cropland","Cool temperate dry","No till","High with manure",1,1.1000000000000001,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal coniferous forest Asia insular n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal coniferous forest","Asia insular","n.a.",12,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Swaziland",4160,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate dry No till High without manure"},"Perennial cropland","Cool temperate dry","No till","High without manure",1,1.1000000000000001,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal coniferous forest Europe n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal coniferous forest","Europe","n.a.",12,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Sweden",19580,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist Full tillage Low"},"Perennial cropland","Cool temperate moist","Full tillage","Low",1,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal coniferous forest North America n.a."},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal coniferous forest","North America","n.a.",12,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Switzerland",7470,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist Full tillage Medium"},"Perennial cropland","Cool temperate moist","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal tundra woodland Asia continental <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Asia continental","<= 20 y",0,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Syrian Arab Rep.",1440,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist Full tillage High with manure"},"Perennial cropland","Cool temperate moist","Full tillage","High with manure",1,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal tundra woodland Asia continental > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Asia continental","> 20 y",2,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tajikistan",2540,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist Full tillage High without manure"},"Perennial cropland","Cool temperate moist","Full tillage","High without manure",1,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal tundra woodland Asia insular <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Asia insular","<= 20 y",0,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tanzania",2420,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist Reduced tillage Low"},"Perennial cropland","Cool temperate moist","Reduced tillage","Low",1,1.08,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal tundra woodland Asia insular > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Asia insular","> 20 y",2,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Thailand",6460,{"$f":"IF(AY165<1000,\"scarce\",IF(AY165<1700,\"stress\",IF(AY165<2500,\"vulnerable\",IF(AY165<6000,\"low but not vulnerable\",IF(AY165<15000,\"medium\",IF(AY165<70000,\"high\",\"very high\"))))))","v":"medium"}]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist Reduced tillage Medium"},"Perennial cropland","Cool temperate moist","Reduced tillage","Medium",1,1.08,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal tundra woodland Europe <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Europe","<= 20 y",0,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Togo",2930,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist Reduced tillage High with manure"},"Perennial cropland","Cool temperate moist","Reduced tillage","High with manure",1,1.08,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal tundra woodland Europe > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Europe","> 20 y",2,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Trinidad and Tobago",2940,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist Reduced tillage High without manure"},"Perennial cropland","Cool temperate moist","Reduced tillage","High without manure",1,1.08,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal tundra woodland North America <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal tundra woodland","North America","<= 20 y",0,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Tunisia",460,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist No till Low"},"Perennial cropland","Cool temperate moist","No till","Low",1,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal tundra woodland North America > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal tundra woodland","North America","> 20 y",2,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Turkey",2950,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist No till Medium"},"Perennial cropland","Cool temperate moist","No till","Medium",1,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal mountain systems Asia continental <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal mountain systems","Asia continental","<= 20 y",2,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Turkmenistan",5000,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist No till High with manure"},"Perennial cropland","Cool temperate moist","No till","High with manure",1,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal mountain systems Asia continental > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal mountain systems","Asia continental","> 20 y",6,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uganda",2470,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Cool temperate moist No till High without manure"},"Perennial cropland","Cool temperate moist","No till","High without manure",1,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal mountain systems Asia insular <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal mountain systems","Asia insular","<= 20 y",2,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Ukraine",2900,"low but not vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry Full tillage Low"},"Perennial cropland","Warm temperate dry","Full tillage","Low",1,1,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal mountain systems Asia insular > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal mountain systems","Asia insular","> 20 y",6,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"United Arab Emirates","4 900","very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry Full tillage Medium"},"Perennial cropland","Warm temperate dry","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal mountain systems Europe <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal mountain systems","Europe","<= 20 y",2,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"United Kingdom",2460,"vulnerable"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry Full tillage High with manure"},"Perennial cropland","Warm temperate dry","Full tillage","High with manure",1,1,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal mountain systems Europe > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal mountain systems","Europe","> 20 y",6,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"United States of America","10 270","very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry Full tillage High without manure"},"Perennial cropland","Warm temperate dry","Full tillage","High without manure",1,1,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal mountain systems North America <= 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal mountain systems","North America","<= 20 y",2,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uruguay",40420,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry Reduced tillage Low"},"Perennial cropland","Warm temperate dry","Reduced tillage","Low",1,1.02,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_10% to 30% canopy cover Boreal n.a. Boreal mountain systems North America > 20 y"},"Forest land_excluding plantations_10% to 30% canopy cover","Boreal","n.a.","Boreal mountain systems","North America","> 20 y",6,0.24,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Uzbekistan","1 900","very high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry Reduced tillage Medium"},"Perennial cropland","Warm temperate dry","Reduced tillage","Medium",1,1.02,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical rain forest Africa n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical rain forest","Africa","n.a.",204,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Venezuela, Bolivarian Rep.",47120,"high"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry Reduced tillage High with manure"},"Perennial cropland","Warm temperate dry","Reduced tillage","High with manure",1,1.02,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical rain forest North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical rain forest","North America","n.a.",198,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Viet Nam",10810,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry Reduced tillage High without manure"},"Perennial cropland","Warm temperate dry","Reduced tillage","High without manure",1,1.02,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical rain forest Central and South America n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical rain forest","Central and South America","n.a.",198,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"West Bank, Palestinian Territories",320,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry No till Low"},"Perennial cropland","Warm temperate dry","No till","Low",1,1.1000000000000001,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical rain forest Asia continental n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical rain forest","Asia continental","n.a.",185,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Yemen",198,"scarce"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry No till Medium"},"Perennial cropland","Warm temperate dry","No till","Medium",1,1.1000000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical rain forest Asia insular n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical rain forest","Asia insular","n.a.",230,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zambia",9630,"medium"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry No till High with manure"},"Perennial cropland","Warm temperate dry","No till","High with manure",1,1.1000000000000001,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical moist deciduous forest Africa n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical moist deciduous forest","Africa","n.a.",156,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Zimbabwe",1550,"stress"]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate dry No till High without manure"},"Perennial cropland","Warm temperate dry","No till","High without manure",1,1.1000000000000001,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical moist deciduous forest North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical moist deciduous forest","North America","n.a.",133]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist Full tillage Low"},"Perennial cropland","Warm temperate moist","Full tillage","Low",1,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical moist deciduous forest Central and South America n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical moist deciduous forest","Central and South America","n.a.",133]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist Full tillage Medium"},"Perennial cropland","Warm temperate moist","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical moist deciduous forest Asia continental n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical moist deciduous forest","Asia continental","n.a.",110]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist Full tillage High with manure"},"Perennial cropland","Warm temperate moist","Full tillage","High with manure",1,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical moist deciduous forest Asia insular n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical moist deciduous forest","Asia insular","n.a.",174]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist Full tillage High without manure"},"Perennial cropland","Warm temperate moist","Full tillage","High without manure",1,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical dry forest Africa n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical dry forest","Africa","n.a.",77]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist Reduced tillage Low"},"Perennial cropland","Warm temperate moist","Reduced tillage","Low",1,1.08,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical dry forest North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical dry forest","North America","n.a.",131]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist Reduced tillage Medium"},"Perennial cropland","Warm temperate moist","Reduced tillage","Medium",1,1.08,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical dry forest Central and South America n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical dry forest","Central and South America","n.a.",131]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist Reduced tillage High with manure"},"Perennial cropland","Warm temperate moist","Reduced tillage","High with manure",1,1.08,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical dry forest Asia continental n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical dry forest","Asia continental","n.a.",83]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist Reduced tillage High without manure"},"Perennial cropland","Warm temperate moist","Reduced tillage","High without manure",1,1.08,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical dry forest Asia insular n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical dry forest","Asia insular","n.a.",101]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist No till Low"},"Perennial cropland","Warm temperate moist","No till","Low",1,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical mountain systems Africa n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical mountain systems","Africa","n.a.",77]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist No till Medium"},"Perennial cropland","Warm temperate moist","No till","Medium",1,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical mountain systems North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical mountain systems","North America","n.a.",94]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist No till High with manure"},"Perennial cropland","Warm temperate moist","No till","High with manure",1,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical mountain systems Central and South America n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical mountain systems","Central and South America","n.a.",94]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Warm temperate moist No till High without manure"},"Perennial cropland","Warm temperate moist","No till","High without manure",1,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical mountain systems Asia continental n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical mountain systems","Asia continental","n.a.",88]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry Full tillage Low"},"Perennial cropland","Tropical dry","Full tillage","Low",1,1,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Tropical n.a. Tropical mountain systems Asia insular n.a."},"Forest land_excluding plantations_>30% canopy cover","Tropical","n.a.","Tropical mountain systems","Asia insular","n.a.",130]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry Full tillage Medium"},"Perennial cropland","Tropical dry","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical humid forest North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical humid forest","North America","n.a.",132]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry Full tillage High with manure"},"Perennial cropland","Tropical dry","Full tillage","High with manure",1,1,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical humid forest Central and South America n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical humid forest","Central and South America","n.a.",132]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry Full tillage High without manure"},"Perennial cropland","Tropical dry","Full tillage","High without manure",1,1,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical humid forest Asia continental n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical humid forest","Asia continental","n.a.",109]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry Reduced tillage Low"},"Perennial cropland","Tropical dry","Reduced tillage","Low",1,1.0900000000000001,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical humid forest Asia insular n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical humid forest","Asia insular","n.a.",173]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry Reduced tillage Medium"},"Perennial cropland","Tropical dry","Reduced tillage","Medium",1,1.0900000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical dry forest Africa n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical dry forest","Africa","n.a.",88]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry Reduced tillage High with manure"},"Perennial cropland","Tropical dry","Reduced tillage","High with manure",1,1.0900000000000001,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical dry forest North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical dry forest","North America","n.a.",130]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry Reduced tillage High without manure"},"Perennial cropland","Tropical dry","Reduced tillage","High without manure",1,1.0900000000000001,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical dry forest Central and South America n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical dry forest","Central and South America","n.a.",130]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry No till Low"},"Perennial cropland","Tropical dry","No till","Low",1,1.17,0.95,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical dry forest Asia continental n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical dry forest","Asia continental","n.a.",82]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry No till Medium"},"Perennial cropland","Tropical dry","No till","Medium",1,1.17,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical dry forest Asia insular n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical dry forest","Asia insular","n.a.",100]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry No till High with manure"},"Perennial cropland","Tropical dry","No till","High with manure",1,1.17,1.37,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical steppe Africa n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical steppe","Africa","n.a.",46]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical dry No till High without manure"},"Perennial cropland","Tropical dry","No till","High without manure",1,1.17,1.04,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical steppe North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical steppe","North America","n.a.",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist Full tillage Low"},"Perennial cropland","Tropical moist","Full tillage","Low",1,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical steppe Central and South America n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical steppe","Central and South America","n.a.",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist Full tillage Medium"},"Perennial cropland","Tropical moist","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical steppe Asia continental n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical steppe","Asia continental","n.a.",41]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist Full tillage High with manure"},"Perennial cropland","Tropical moist","Full tillage","High with manure",1,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Subtropical n.a. Subtropical steppe Asia insular n.a."},"Forest land_excluding plantations_>30% canopy cover","Subtropical","n.a.","Subtropical steppe","Asia insular","n.a.",47]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist Full tillage High without manure"},"Perennial cropland","Tropical moist","Full tillage","High without manure",1,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate oceanic forest Europe n.a."},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate oceanic forest","Europe","n.a.",84]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist Reduced tillage Low"},"Perennial cropland","Tropical moist","Reduced tillage","Low",1,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate oceanic forest North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate oceanic forest","North America","n.a.",406]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist Reduced tillage Medium"},"Perennial cropland","Tropical moist","Reduced tillage","Medium",1,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate oceanic forest New Zealand n.a."},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate oceanic forest","New Zealand","n.a.",227]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist Reduced tillage High with manure"},"Perennial cropland","Tropical moist","Reduced tillage","High with manure",1,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate oceanic forest Central and South America n.a."},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate oceanic forest","Central and South America","n.a.",120]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist Reduced tillage High without manure"},"Perennial cropland","Tropical moist","Reduced tillage","High without manure",1,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest Asia continental <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","Asia continental","<= 20 y",27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist No till Low"},"Perennial cropland","Tropical moist","No till","Low",1,1.22,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest Asia continental > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","Asia continental","> 20 y",87]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist No till Medium"},"Perennial cropland","Tropical moist","No till","Medium",1,1.22,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest Asia insular <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","Asia insular","<= 20 y",27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist No till High with manure"},"Perennial cropland","Tropical moist","No till","High with manure",1,1.22,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest Asia insular > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","Asia insular","> 20 y",87]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical moist No till High without manure"},"Perennial cropland","Tropical moist","No till","High without manure",1,1.22,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest Europe <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","Europe","<= 20 y",27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet Full tillage Low"},"Perennial cropland","Tropical wet","Full tillage","Low",1,1,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest Europe > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","Europe","> 20 y",87]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet Full tillage Medium"},"Perennial cropland","Tropical wet","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest North America <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","North America","<= 20 y",51]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet Full tillage High with manure"},"Perennial cropland","Tropical wet","Full tillage","High with manure",1,1,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest North America > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","North America","> 20 y",93]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet Full tillage High without manure"},"Perennial cropland","Tropical wet","Full tillage","High without manure",1,1,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest Central and South America <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","Central and South America","<= 20 y",51]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet Reduced tillage Low"},"Perennial cropland","Tropical wet","Reduced tillage","Low",1,1.1499999999999999,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate continental forest Central and South America > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate continental forest","Central and South America","> 20 y",93]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet Reduced tillage Medium"},"Perennial cropland","Tropical wet","Reduced tillage","Medium",1,1.1499999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems Asia continental <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","Asia continental","<= 20 y",75]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet Reduced tillage High with manure"},"Perennial cropland","Tropical wet","Reduced tillage","High with manure",1,1.1499999999999999,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems Asia continental > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","Asia continental","> 20 y",93]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet Reduced tillage High without manure"},"Perennial cropland","Tropical wet","Reduced tillage","High without manure",1,1.1499999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems Asia insular <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","Asia insular","<= 20 y",75]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet No till Low"},"Perennial cropland","Tropical wet","No till","Low",1,1.22,0.92,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems Asia insular > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","Asia insular","> 20 y",93]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet No till Medium"},"Perennial cropland","Tropical wet","No till","Medium",1,1.22,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems Europe <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","Europe","<= 20 y",75]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet No till High with manure"},"Perennial cropland","Tropical wet","No till","High with manure",1,1.22,1.44,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems Europe > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","Europe","> 20 y",93]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical wet No till High without manure"},"Perennial cropland","Tropical wet","No till","High without manure",1,1.22,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems North America <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","North America","<= 20 y",45]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane Full tillage Low"},"Perennial cropland","Tropical montane","Full tillage","Low",1,1,0.94,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems North America > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","North America","> 20 y",93]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane Full tillage Medium"},"Perennial cropland","Tropical montane","Full tillage","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems Central and South America <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","Central and South America","<= 20 y",45]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane Full tillage High with manure"},"Perennial cropland","Tropical montane","Full tillage","High with manure",1,1,1.41,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Temperate n.a. Temperate mountain systems Central and South America > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Temperate","n.a.","Temperate mountain systems","Central and South America","> 20 y",93]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane Full tillage High without manure"},"Perennial cropland","Tropical montane","Full tillage","High without manure",1,1,1.08,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal coniferous forest Asia continental n.a."},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal coniferous forest","Asia continental","n.a.",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane Reduced tillage Low"},"Perennial cropland","Tropical montane","Reduced tillage","Low",1,1.0900000000000001,0.94,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal coniferous forest Asia insular n.a."},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal coniferous forest","Asia insular","n.a.",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane Reduced tillage Medium"},"Perennial cropland","Tropical montane","Reduced tillage","Medium",1,1.0900000000000001,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal coniferous forest Europe n.a."},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal coniferous forest","Europe","n.a.",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane Reduced tillage High with manure"},"Perennial cropland","Tropical montane","Reduced tillage","High with manure",1,1.0900000000000001,1.41,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal coniferous forest North America n.a."},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal coniferous forest","North America","n.a.",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane Reduced tillage High without manure"},"Perennial cropland","Tropical montane","Reduced tillage","High without manure",1,1.0900000000000001,1.08,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal tundra woodland Asia continental <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Asia continental","<= 20 y",26]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane No till Low"},"Perennial cropland","Tropical montane","No till","Low",1,1.1599999999999999,0.94,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal tundra woodland Asia continental > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Asia continental","> 20 y",35]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane No till Medium"},"Perennial cropland","Tropical montane","No till","Medium",1,1.1599999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal tundra woodland Asia insular <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Asia insular","<= 20 y",26]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane No till High with manure"},"Perennial cropland","Tropical montane","No till","High with manure",1,1.1599999999999999,1.41,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal tundra woodland Asia insular > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Asia insular","> 20 y",35]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Perennial cropland Tropical montane No till High without manure"},"Perennial cropland","Tropical montane","No till","High without manure",1,1.1599999999999999,1.08,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal tundra woodland Europe <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Europe","<= 20 y",26]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal dry Improved Medium"},"Grassland and savannah","Boreal dry","Improved","Medium",1,1.1399999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal tundra woodland Europe > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal tundra woodland","Europe","> 20 y",35]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal dry Improved High"},"Grassland and savannah","Boreal dry","Improved","High",1,1.1399999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal tundra woodland North America <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal tundra woodland","North America","<= 20 y",26]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal dry Nominally managed Medium"},"Grassland and savannah","Boreal dry","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal tundra woodland North America > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal tundra woodland","North America","> 20 y",35]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal dry Moderately degraded Medium"},"Grassland and savannah","Boreal dry","Moderately degraded","Medium",1,0.95,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal mountain systems Asia continental <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal mountain systems","Asia continental","<= 20 y",32]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal dry Severely degraded Medium"},"Grassland and savannah","Boreal dry","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal mountain systems Asia continental > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal mountain systems","Asia continental","> 20 y",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal moist Improved Medium"},"Grassland and savannah","Boreal moist","Improved","Medium",1,1.1399999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal mountain systems Asia insular <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal mountain systems","Asia insular","<= 20 y",32]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal moist Improved High"},"Grassland and savannah","Boreal moist","Improved","High",1,1.1399999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal mountain systems Asia insular > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal mountain systems","Asia insular","> 20 y",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal moist Nominally managed Medium"},"Grassland and savannah","Boreal moist","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal mountain systems Europe <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal mountain systems","Europe","<= 20 y",32]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal moist Moderately degraded Medium"},"Grassland and savannah","Boreal moist","Moderately degraded","Medium",1,0.95,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal mountain systems Europe > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal mountain systems","Europe","> 20 y",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Boreal moist Severely degraded Medium"},"Grassland and savannah","Boreal moist","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal mountain systems North America <= 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal mountain systems","North America","<= 20 y",32]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate dry Improved Medium"},"Grassland and savannah","Cool temperate dry","Improved","Medium",1,1.1399999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest land_excluding plantations_>30% canopy cover Boreal n.a. Boreal mountain systems North America > 20 y"},"Forest land_excluding plantations_>30% canopy cover","Boreal","n.a.","Boreal mountain systems","North America","> 20 y",53]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate dry Improved High"},"Grassland and savannah","Cool temperate dry","Improved","High",1,1.1399999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Africa Broadleaf > 20 y"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Africa","Broadleaf > 20 y",87,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate dry Nominally managed Medium"},"Grassland and savannah","Cool temperate dry","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Africa Broadleaf <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Africa","Broadleaf <= 20 y",29,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate dry Moderately degraded Medium"},"Grassland and savannah","Cool temperate dry","Moderately degraded","Medium",1,0.95,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Africa Pinus sp. > 20 y"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Africa","Pinus sp. > 20 y",58,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate dry Severely degraded Medium"},"Grassland and savannah","Cool temperate dry","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Africa Pinus sp. <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Africa","Pinus sp. <= 20 y",17,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate moist Improved Medium"},"Grassland and savannah","Cool temperate moist","Improved","Medium",1,1.1399999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest North America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical rain forest","North America","Eucalyptus sp.",58,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate moist Improved High"},"Grassland and savannah","Cool temperate moist","Improved","High",1,1.1399999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest North America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical rain forest","North America","Pinus sp.",87,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate moist Nominally managed Medium"},"Grassland and savannah","Cool temperate moist","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest North America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical rain forest","North America","Tectona grandis",70,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate moist Moderately degraded Medium"},"Grassland and savannah","Cool temperate moist","Moderately degraded","Medium",1,0.95,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest North America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical rain forest","North America","Other broadleaf",44,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Cool temperate moist Severely degraded Medium"},"Grassland and savannah","Cool temperate moist","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Central and South America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical rain forest","Central and South America","Eucalyptus sp.",58,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate dry Improved Medium"},"Grassland and savannah","Warm temperate dry","Improved","Medium",1,1.1399999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Central and South America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical rain forest","Central and South America","Pinus sp.",87,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate dry Improved High"},"Grassland and savannah","Warm temperate dry","Improved","High",1,1.1399999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Central and South America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Central and South America","Tectona grandis",70,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate dry Nominally managed Medium"},"Grassland and savannah","Warm temperate dry","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Central and South America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Central and South America","Other broadleaf",44,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate dry Moderately degraded Medium"},"Grassland and savannah","Warm temperate dry","Moderately degraded","Medium",1,0.95,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Asia continental Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Asia continental","Broadleaf",64,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate dry Severely degraded Medium"},"Grassland and savannah","Warm temperate dry","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Asia continental Other"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Asia continental","Other",38,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate moist Improved Medium"},"Grassland and savannah","Warm temperate moist","Improved","Medium",1,1.1399999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Asia insular Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Asia insular","Broadleaf",64,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate moist Improved High"},"Grassland and savannah","Warm temperate moist","Improved","High",1,1.1399999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical rain forest Asia insular Other"},"Forest plantations","Tropical","n.a.","Tropical rain forest","Asia insular","Other",38,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate moist Nominally managed Medium"},"Grassland and savannah","Warm temperate moist","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Africa Broadleaf > 20 y"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Africa","Broadleaf > 20 y",44,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate moist Moderately degraded Medium"},"Grassland and savannah","Warm temperate moist","Moderately degraded","Medium",1,0.95,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Africa Broadleaf <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Africa","Broadleaf <= 20 y",23,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Warm temperate moist Severely degraded Medium"},"Grassland and savannah","Warm temperate moist","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Africa Pinus sp. > 20 y"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Africa","Pinus sp. > 20 y",35,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical dry Improved Medium"},"Grassland and savannah","Tropical dry","Improved","Medium",1,1.17,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Africa Pinus sp. <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Africa","Pinus sp. <= 20 y",12,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical dry Improved High"},"Grassland and savannah","Tropical dry","Improved","High",1,1.17,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest North America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","North America","Eucalyptus sp.",26,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical dry Nominally managed Medium"},"Grassland and savannah","Tropical dry","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest North America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","North America","Pinus sp.",79,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical dry Moderately degraded Medium"},"Grassland and savannah","Tropical dry","Moderately degraded","Medium",1,0.97,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest North America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","North America","Tectona grandis",35,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical dry Severely degraded Medium"},"Grassland and savannah","Tropical dry","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest North America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","North America","Other broadleaf",29,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical moist Improved Medium"},"Grassland and savannah","Tropical moist","Improved","Medium",1,1.17,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Central and South America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Central and South America","Eucalyptus sp.",26,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical moist Improved High"},"Grassland and savannah","Tropical moist","Improved","High",1,1.17,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Central and South America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Central and South America","Pinus sp.",79,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical moist Nominally managed Medium"},"Grassland and savannah","Tropical moist","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Central and South America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Central and South America","Tectona grandis",35,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical moist Moderately degraded Medium"},"Grassland and savannah","Tropical moist","Moderately degraded","Medium",1,0.97,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Central and South America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Central and South America","Other broadleaf",29,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical moist Severely degraded Medium"},"Grassland and savannah","Tropical moist","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Asia continental Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Asia continental","Broadleaf",52,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical wet Improved Medium"},"Grassland and savannah","Tropical wet","Improved","Medium",1,1.17,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Asia continental Other"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Asia continental","Other",29,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical wet Improved High"},"Grassland and savannah","Tropical wet","Improved","High",1,1.17,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Asia insular Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Asia insular","Broadleaf",52,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical wet Nominally managed Medium"},"Grassland and savannah","Tropical wet","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical moist deciduous forest Asia insular Other"},"Forest plantations","Tropical","n.a.","Tropical moist deciduous forest","Asia insular","Other",29,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical wet Moderately degraded Medium"},"Grassland and savannah","Tropical wet","Moderately degraded","Medium",1,0.97,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Africa Broadleaf > 20 y"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Africa","Broadleaf > 20 y",21,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical wet Severely degraded Medium"},"Grassland and savannah","Tropical wet","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Africa Broadleaf <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Africa","Broadleaf <= 20 y",9,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical montane Improved Medium"},"Grassland and savannah","Tropical montane","Improved","Medium",1,1.1599999999999999,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Africa Pinus sp. > 20 y"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Africa","Pinus sp. > 20 y",18,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical montane Improved High"},"Grassland and savannah","Tropical montane","Improved","High",1,1.1599999999999999,1.1100000000000001,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Africa Pinus sp. <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Africa","Pinus sp. <= 20 y",6,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical montane Nominally managed Medium"},"Grassland and savannah","Tropical montane","Nominally managed","Medium",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest North America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical dry forest","North America","Eucalyptus sp.",27,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical montane Moderately degraded Medium"},"Grassland and savannah","Tropical montane","Moderately degraded","Medium",1,0.96,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest North America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical dry forest","North America","Pinus sp.",33,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Grassland and savannah Tropical montane Severely degraded Medium"},"Grassland and savannah","Tropical montane","Severely degraded","Medium",1,0.7,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest North America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical dry forest","North America","Tectona grandis",27,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Boreal dry n.a. n.a."},"Native forest non degraded","Boreal dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest North America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical dry forest","North America","Other broadleaf",18,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Boreal moist n.a. n.a."},"Native forest non degraded","Boreal moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Central and South America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical dry forest","Central and South America","Eucalyptus sp.",27,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Cool temperate dry n.a. n.a."},"Native forest non degraded","Cool temperate dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Central and South America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical dry forest","Central and South America","Pinus sp.",33,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Cool temperate moist n.a. n.a."},"Native forest non degraded","Cool temperate moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Central and South America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Central and South America","Tectona grandis",27,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Warm temperate dry n.a. n.a."},"Native forest non degraded","Warm temperate dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Central and South America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Central and South America","Other broadleaf",18,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Warm temperate moist n.a. n.a."},"Native forest non degraded","Warm temperate moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Asia continental Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Asia continental","Broadleaf",27,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Tropical dry n.a. n.a."},"Native forest non degraded","Tropical dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Asia continental Other"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Asia continental","Other",18,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Tropical moist n.a. n.a."},"Native forest non degraded","Tropical moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Asia insular Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Asia insular","Broadleaf",27,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Tropical wet n.a. n.a."},"Native forest non degraded","Tropical wet","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical dry forest Asia insular Other"},"Forest plantations","Tropical","n.a.","Tropical dry forest","Asia insular","Other",18,0.28000000000000003]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Native forest non degraded Tropical montane n.a. n.a."},"Native forest non degraded","Tropical montane","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Africa Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Africa","Broadleaf",6,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Boreal dry n.a. n.a."},"Managed forest","Boreal dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Africa Pinus sp. > 20 y"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Africa","Pinus sp. > 20 y",6,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Boreal moist n.a. n.a."},"Managed forest","Boreal moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Africa Pinus sp. <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Africa","Pinus sp. <= 20 y",4,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Cool temperate dry n.a. n.a."},"Managed forest","Cool temperate dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland North America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical shrubland","North America","Eucalyptus sp.",18,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Cool temperate moist n.a. n.a."},"Managed forest","Cool temperate moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland North America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical shrubland","North America","Pinus sp.",18,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Warm temperate dry n.a. n.a."},"Managed forest","Warm temperate dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland North America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical shrubland","North America","Tectona grandis",15,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Warm temperate moist n.a. n.a."},"Managed forest","Warm temperate moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland North America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical shrubland","North America","Other broadleaf",9,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Tropical dry n.a. n.a."},"Managed forest","Tropical dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Central and South America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical shrubland","Central and South America","Eucalyptus sp.",18,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Tropical moist n.a. n.a."},"Managed forest","Tropical moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Central and South America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical shrubland","Central and South America","Pinus sp.",18,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Tropical wet n.a. n.a."},"Managed forest","Tropical wet","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Central and South America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Central and South America","Tectona grandis",15,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Managed forest Tropical montane n.a. n.a."},"Managed forest","Tropical montane","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Central and South America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Central and South America","Other broadleaf",9,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Boreal dry n.a. n.a."},"Shifting cultivation shortened fallow","Boreal dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Asia continental Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Asia continental","Broadleaf",12,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Boreal moist n.a. n.a."},"Shifting cultivation shortened fallow","Boreal moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Asia continental Other"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Asia continental","Other",9,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Cool temperate dry n.a. n.a."},"Shifting cultivation shortened fallow","Cool temperate dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Asia insular Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Asia insular","Broadleaf",12,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Cool temperate moist n.a. n.a."},"Shifting cultivation shortened fallow","Cool temperate moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical shrubland Asia insular Other"},"Forest plantations","Tropical","n.a.","Tropical shrubland","Asia insular","Other",9,0.27]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Warm temperate dry n.a. n.a."},"Shifting cultivation shortened fallow","Warm temperate dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Africa Broadleaf > 20 y"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Africa","Broadleaf > 20 y",31,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Warm temperate moist n.a. n.a."},"Shifting cultivation shortened fallow","Warm temperate moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Africa Broadleaf <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Africa","Broadleaf <= 20 y",20,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Tropical dry n.a. n.a."},"Shifting cultivation shortened fallow","Tropical dry","n.a.","n.a.",0.64,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Africa Pinus sp. > 20 y"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Africa","Pinus sp. > 20 y",19,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Tropical moist n.a. n.a."},"Shifting cultivation shortened fallow","Tropical moist","n.a.","n.a.",0.64,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Africa Pinus sp. <= 20 y"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Africa","Pinus sp. <= 20 y",7,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Tropical wet n.a. n.a."},"Shifting cultivation shortened fallow","Tropical wet","n.a.","n.a.",0.64,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems North America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical mountain systems","North America","Eucalyptus sp.",22,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation shortened fallow Tropical montane n.a. n.a."},"Shifting cultivation shortened fallow","Tropical montane","n.a.","n.a.",0.64,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems North America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical mountain systems","North America","Pinus sp.",29,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Boreal dry n.a. n.a."},"Shifting cultivation mature fallow","Boreal dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems North America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","North America","Tectona grandis",23,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Boreal moist n.a. n.a."},"Shifting cultivation mature fallow","Boreal moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems North America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","North America","Other broadleaf",16,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Cool temperate dry n.a. n.a."},"Shifting cultivation mature fallow","Cool temperate dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Central and South America Eucalyptus sp."},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Central and South America","Eucalyptus sp.",22,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Cool temperate moist n.a. n.a."},"Shifting cultivation mature fallow","Cool temperate moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Central and South America Pinus sp."},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Central and South America","Pinus sp.",29,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Warm temperate dry n.a. n.a."},"Shifting cultivation mature fallow","Warm temperate dry","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Central and South America Tectona grandis"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Central and South America","Tectona grandis",23,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Warm temperate moist n.a. n.a."},"Shifting cultivation mature fallow","Warm temperate moist","n.a.","n.a.",1,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Central and South America Other broadleaf"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Central and South America","Other broadleaf",16,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Tropical dry n.a. n.a."},"Shifting cultivation mature fallow","Tropical dry","n.a.","n.a.",0.8,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Asia continental Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Asia continental","Broadleaf",28,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Tropical moist n.a. n.a."},"Shifting cultivation mature fallow","Tropical moist","n.a.","n.a.",0.8,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Asia continental Other"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Asia continental","Other",15,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Tropical wet n.a. n.a."},"Shifting cultivation mature fallow","Tropical wet","n.a.","n.a.",0.8,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Asia insular Broadleaf"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Asia insular","Broadleaf",28,0.24]
[null,null,null,null,null,null,null,{"$f":"Table_IPCC_factors[[#This Row],[Land use]]&\" \"&Table_IPCC_factors[[#This Row],[Climate region]]&\" \"&Table_IPCC_factors[[#This Row],[Management]]&\" \"&Table_IPCC_factors[[#This Row],[Input]]","v":"Shifting cultivation mature fallow Tropical montane n.a. n.a."},"Shifting cultivation mature fallow","Tropical montane","n.a.","n.a.",0.8,1,1,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Tropical n.a. Tropical mountain systems Asia insular Other"},"Forest plantations","Tropical","n.a.","Tropical mountain systems","Asia insular","Other",15,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest North America Eucalyptus sp."},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","North America","Eucalyptus sp.",42,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest North America Pinus sp."},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","North America","Pinus sp.",81,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest North America Tectona grandis"},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","North America","Tectona grandis",36,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest North America Other broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","North America","Other broadleaf",30,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest Central and South America Eucalyptus sp."},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","Central and South America","Eucalyptus sp.",42,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest Central and South America Pinus sp."},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","Central and South America","Pinus sp.",81,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest Central and South America Tectona grandis"},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","Central and South America","Tectona grandis",36,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest Central and South America Other broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","Central and South America","Other broadleaf",30,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest Asia continental Broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","Asia continental","Broadleaf",54,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest Asia continental Other"},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","Asia continental","Other",30,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest Asia insular Broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","Asia insular","Broadleaf",54,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical humid forest Asia insular Other"},"Forest plantations","Subtropical","n.a.","Subtropical humid forest","Asia insular","Other",30,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Africa Broadleaf > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Africa","Broadleaf > 20 y",21,0.28000000000000003]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Africa Broadleaf <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Africa","Broadleaf <= 20 y",9,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Africa Pinus sp. > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Africa","Pinus sp. > 20 y",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Africa Pinus sp. <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Africa","Pinus sp. <= 20 y",6,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest North America Eucalyptus sp."},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","North America","Eucalyptus sp.",34,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest North America Pinus sp."},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","North America","Pinus sp.",34,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest North America Tectona grandis"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","North America","Tectona grandis",28,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest North America Other broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","North America","Other broadleaf",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Central and South America Eucalyptus sp."},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Central and South America","Eucalyptus sp.",34,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Central and South America Pinus sp."},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Central and South America","Pinus sp.",34,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Central and South America Tectona grandis"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Central and South America","Tectona grandis",28,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Central and South America Other broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Central and South America","Other broadleaf",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Asia continental Broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Asia continental","Broadleaf",28,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Asia continental Other"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Asia continental","Other",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Asia insular Broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Asia insular","Broadleaf",28,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical dry forest Asia insular Other"},"Forest plantations","Subtropical","n.a.","Subtropical dry forest","Asia insular","Other",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Africa Broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Africa","Broadleaf",6,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Africa Pinus sp. > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Africa","Pinus sp. > 20 y",6,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Africa Pinus sp. <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Africa","Pinus sp. <= 20 y",5,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe North America Eucalyptus sp."},"Forest plantations","Subtropical","n.a.","Subtropical steppe","North America","Eucalyptus sp.",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe North America Pinus sp."},"Forest plantations","Subtropical","n.a.","Subtropical steppe","North America","Pinus sp.",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe North America Tectona grandis"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","North America","Tectona grandis",16,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe North America Other broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","North America","Other broadleaf",9,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Central and South America Eucalyptus sp."},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Central and South America","Eucalyptus sp.",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Central and South America Pinus sp."},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Central and South America","Pinus sp.",19,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Central and South America Tectona grandis"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Central and South America","Tectona grandis",16,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Central and South America Other broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Central and South America","Other broadleaf",9,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Asia continental Broadleaf > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Asia continental","Broadleaf > 20 y",25,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Asia continental Broadleaf <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Asia continental","Broadleaf <= 20 y",3,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Asia continental Coniferous > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Asia continental","Coniferous > 20 y",6,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Asia continental Coniferous <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Asia continental","Coniferous <= 20 y",34,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Asia insular Broadleaf > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Asia insular","Broadleaf > 20 y",25,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Asia insular Broadleaf <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Asia insular","Broadleaf <= 20 y",3,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Asia insular Coniferous > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Asia insular","Coniferous > 20 y",6,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical steppe Asia insular Coniferous <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical steppe","Asia insular","Coniferous <= 20 y",34,0.32]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Africa Broadleaf > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Africa","Broadleaf > 20 y",31,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Africa Broadleaf <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Africa","Broadleaf <= 20 y",20,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Africa Pinus sp. > 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Africa","Pinus sp. > 20 y",19,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Africa Pinus sp. <= 20 y"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Africa","Pinus sp. <= 20 y",7,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system North America Eucalyptus sp."},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","North America","Eucalyptus sp.",22,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system North America Pinus sp."},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","North America","Pinus sp.",34,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system North America Tectona grandis"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","North America","Tectona grandis",23,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system North America Other broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","North America","Other broadleaf",16,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Central and South America Eucalyptus sp."},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Central and South America","Eucalyptus sp.",22,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Central and South America Pinus sp."},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Central and South America","Pinus sp.",34,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Central and South America Tectona grandis"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Central and South America","Tectona grandis",23,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Central and South America Other broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Central and South America","Other broadleaf",16,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Asia continental Broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Asia continental","Broadleaf",28,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Asia continental Other"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Asia continental","Other",15,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Asia insular Broadleaf"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Asia insular","Broadleaf",28,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Subtropical n.a. Subtropical mountain system Asia insular Other"},"Forest plantations","Subtropical","n.a.","Subtropical mountain system","Asia insular","Other",15,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Asia continental Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Asia continental","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Asia continental Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Asia continental","Broadleaf <= 20 y",9,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Asia continental Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Asia continental","Coniferous > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Asia continental Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Asia continental","Coniferous <= 20 y",12,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Asia insular Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Asia insular","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Asia insular Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Asia insular","Broadleaf <= 20 y",9,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Asia insular Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Asia insular","Coniferous > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Asia insular Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Asia insular","Coniferous <= 20 y",12,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Europe Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Europe","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Europe Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Europe","Broadleaf <= 20 y",9,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Europe Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Europe","Coniferous > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Europe Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Europe","Coniferous <= 20 y",12,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest North America n.a."},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","North America","n.a.",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest New Zealand n.a."},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","New Zealand","n.a.",75,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate oceanic forest Central and South America n.a."},"Forest plantations","Temperate","n.a.","Temperate oceanic forest","Central and South America","n.a.",31,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Asia continental Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Asia continental","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Asia continental Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Asia continental","Broadleaf <= 20 y",4,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Asia continental Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Asia continental","Coniferous > 20 y",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Asia continental Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Asia continental","Coniferous <= 20 y",7,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Asia insular Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Asia insular","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Asia insular Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Asia insular","Broadleaf <= 20 y",4,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Asia insular Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Asia insular","Coniferous > 20 y",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Asia insular Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Asia insular","Coniferous <= 20 y",7,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Europe Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Europe","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Europe Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Europe","Broadleaf <= 20 y",4,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Europe Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Europe","Coniferous > 20 y",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Europe Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate continental forest","Europe","Coniferous <= 20 y",7,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest North America n.a."},"Forest plantations","Temperate","n.a.","Temperate continental forest","North America","n.a.",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate continental forest Central and South America n.a."},"Forest plantations","Temperate","n.a.","Temperate continental forest","Central and South America","n.a.",31,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Asia continental Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Asia continental","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Asia continental Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Asia continental","Broadleaf <= 20 y",4,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Asia continental Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Asia continental","Coniferous > 20 y",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Asia continental Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Asia continental","Coniferous <= 20 y",7,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Asia insular Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Asia insular","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Asia insular Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Asia insular","Broadleaf <= 20 y",4,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Asia insular Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Asia insular","Coniferous > 20 y",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Asia insular Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Asia insular","Coniferous <= 20 y",7,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Europe Broadleaf > 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Europe","Broadleaf > 20 y",60,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Europe Broadleaf <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Europe","Broadleaf <= 20 y",4,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Europe Coniferous > 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Europe","Coniferous > 20 y",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Europe Coniferous <= 20 y"},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Europe","Coniferous <= 20 y",7,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems North America n.a."},"Forest plantations","Temperate","n.a.","Temperate mountain systems","North America","n.a.",52,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Temperate n.a. Temperate mountain systems Central and South America n.a."},"Forest plantations","Temperate","n.a.","Temperate mountain systems","Central and South America","n.a.",31,0.27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal coniferous forest Asia continental Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal coniferous forest","Asia continental","Broadleaf > 20 y",12,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal coniferous forest Asia continental Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal coniferous forest","Asia continental","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal coniferous forest Asia insular Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal coniferous forest","Asia insular","Broadleaf > 20 y",12,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal coniferous forest Asia insular Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal coniferous forest","Asia insular","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal coniferous forest Europe Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal coniferous forest","Europe","Broadleaf > 20 y",12,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal coniferous forest Europe Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal coniferous forest","Europe","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal coniferous forest North America n.a."},"Forest plantations","Boreal","n.a.","Boreal coniferous forest","North America","n.a.",13,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal mountain systems Asia continental Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal mountain systems","Asia continental","Broadleaf > 20 y",12,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal mountain systems Asia continental Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal mountain systems","Asia continental","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal mountain systems Asia insular Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal mountain systems","Asia insular","Broadleaf > 20 y",12,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal mountain systems Asia insular Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal mountain systems","Asia insular","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal mountain systems Europe Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal mountain systems","Europe","Broadleaf > 20 y",12,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal mountain systems Europe Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal mountain systems","Europe","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal mountain systems North America n.a."},"Forest plantations","Boreal","n.a.","Boreal mountain systems","North America","n.a.",13,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal tundra woodland Asia continental Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal tundra woodland","Asia continental","Broadleaf > 20 y",7,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal tundra woodland Asia continental Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal tundra woodland","Asia continental","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal tundra woodland Asia insular Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal tundra woodland","Asia insular","Broadleaf > 20 y",7,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal tundra woodland Asia insular Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal tundra woodland","Asia insular","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal tundra woodland Europe Broadleaf > 20 y"},"Forest plantations","Boreal","n.a.","Boreal tundra woodland","Europe","Broadleaf > 20 y",7,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal tundra woodland Europe Broadleaf <= 20 y"},"Forest plantations","Boreal","n.a.","Boreal tundra woodland","Europe","Broadleaf <= 20 y",1,0.24]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"Table_IPCC_Cvegetation[[#This Row],[Land use_more specific]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Domain]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Climate region]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Ecological zone]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Continent]]&\" \"&Table_IPCC_Cvegetation[[#This Row],[Type]]","v":"Forest plantations Boreal n.a. Boreal tundra woodland North America n.a."},"Forest plantations","Boreal","n.a.","Boreal tundra woodland","North America","n.a.",7,0.24]

{"sheet":"Production feedstock1","index":18,"n_rows":339,"n_cols":8,"rows_kept":339,"cut":false,"hidden":true,"merged":[]}
["Monitoring framework - Production feedstock 1 (per year)"]
[]
[null,null,"From input"]
[null,null,"Standard value"]
[null,null,"Calculated from other fields"]
[null,null,"Determines value in other field"]
[]
["MASS BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Feedstock characteristics"]
[null,{"$f":"VLOOKUP($D10,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Feedstock type 1"},null,"FP001","-",{"$f":"VLOOKUP(D10,Parameters!$1:$1958,6,FALSE)","v":"Fresh palm fruit bunches (FFB)"},{"$f":"F10","v":"Fresh palm fruit bunches (FFB)"}]
[null,{"$f":"VLOOKUP($D11,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Origin of the feedstock"},null,"FP002","-",{"$f":"VLOOKUP(D11,Parameters!$1:$1958,6,FALSE)","v":"Malaysia"},{"$f":"F11","v":"Malaysia"}]
[null,{"$f":"VLOOKUP($D12,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 1 per ha"},null,"FP003a","kg/ha",{"$f":"VLOOKUP(D12,Parameters!$1:$1958,6,FALSE)","v":19000},{"$f":"F12","v":19000}]
[null,{"$f":"VLOOKUP($D13,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (dry) of feedstock 1 per ha"},null,"FP003b","kgdm/ha",null,{"$f":"G12*(100-G18)/100","v":12540},"=FP003a*(100-FP009)/100"]
[null,{"$f":"VLOOKUP($D14,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of feedstock 1 per ha"},null,"FP003c","MJ/ha",null,{"$f":"G13*G17","v":300960},"=FP003b*FP010"]
[null,{"$f":"VLOOKUP($D15,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Number of harvests per year"},null,"FP005","1/yr",{"$f":"VLOOKUP(D15,Parameters!$1:$1958,6,FALSE)","v":1},{"$f":"F15","v":1}]
[null,{"$f":"VLOOKUP($D16,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Rotation system"},null,"FP006","-"]
[null,{"$f":"VLOOKUP($D17,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of the dry energy crop (LHV)"},null,"FP010","MJ/kgdm",{"$f":"VLOOKUP(G87,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":24},{"$f":"F17","v":24}]
[null,{"$f":"VLOOKUP($D18,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of the harvested crop"},null,"FP009","%",{"$f":"VLOOKUP(D18,Parameters!$1:$1958,6,FALSE)","v":34},{"$f":"F18","v":34}]
["Seeds"]
[null,{"$f":"VLOOKUP($D20,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of seeds"},null,"FP022","kg/ha",{"$f":"VLOOKUP(D20,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F20","v":0}]
[null,null,{"$f":"VLOOKUP($D21,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of seeds"},"FP050f","MJ/kgseeds",{"$f":"VLOOKUP($F$10,matrix_standardvalues_seeds,10,FALSE)","v":0},{"$f":"F21","v":0}]
[null,null,{"$f":"VLOOKUP($D22,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Seeds: specific GHG emissions"},"FP067f","gCO2_eq/kgseeds",{"$f":"VLOOKUP($G$10,matrix_standardvalues_seeds,10,FALSE)","v":0},{"$f":"F22","v":0}]
["Fertilizers"]
[null,{"$f":"VLOOKUP($D24,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of N fertiliser (synthetic)"},null,"FP023a","kg/ha",{"$f":"VLOOKUP(D24,Parameters!$1:$1958,6,FALSE)","v":127.908},{"$f":"F24","v":127.908}]
[null,null,{"$f":"VLOOKUP($D25,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of N fertiliser"},"FP050a","MJ/kgfertiliser",{"$f":"VLOOKUP(\"N\",matrix_standardvalues,10,FALSE)","v":48.990600000000001},{"$f":"F25","v":48.990600000000001}]
[null,null,{"$f":"VLOOKUP($D26,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N: specific GHG emissions"},"FP067a","gCO2_eq/kgfertiliser",{"$f":"VLOOKUP(\"N\",matrix_standardvalues,5,FALSE)","v":5880.5900999999994},5880.5900999999994]
[null,{"$f":"VLOOKUP($D27,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of P2O5 fertiliser"},null,"FP023b","kg/ha",{"$f":"VLOOKUP(D27,Parameters!$1:$1958,6,FALSE)","v":143.792},143.792]
[null,null,{"$f":"VLOOKUP($D28,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of P fertiliser"},"FP050b","MJ/kgfertiliser",{"$f":"VLOOKUP(\"P2O5\",matrix_standardvalues,10,FALSE)","v":15.2334},15.2334]
[null,null,{"$f":"VLOOKUP($D29,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"P2O5: specific GHG emissions"},"FP067b","gCO2_eq/kgfertiliser",{"$f":"VLOOKUP(\"P2O5\",matrix_standardvalues,5,FALSE)","v":1010.7434999999999},1010.7434999999999]
[null,{"$f":"VLOOKUP($D30,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of K2O fertiliser"},null,"FP023c","kg/ha",{"$f":"VLOOKUP(D30,Parameters!$1:$1958,6,FALSE)","v":199.804},199.804]
[null,null,{"$f":"VLOOKUP($D31,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of K fertiliser"},"FP050c","MJ/kgfertiliser",{"$f":"VLOOKUP(\"K2O\",matrix_standardvalues,10,FALSE)","v":9.67896},9.67896]
[null,null,{"$f":"VLOOKUP($D32,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"K2O: specific GHG emissions"},"FP067c","gCO2_eq/kgfertiliser",{"$f":"VLOOKUP(\"K2O\",matrix_standardvalues,5,FALSE)","v":576.08240000000001},576.08240000000001]
[null,{"$f":"VLOOKUP($D33,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of CaO fertiliser"},null,"FP023d","kg/ha",{"$f":"VLOOKUP(D33,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D34,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of Ca fertiliser"},"FP050d","MJ/kgfertiliser",{"$f":"VLOOKUP(\"CaO\",matrix_standardvalues,10,FALSE)","v":1.9735200000000002},1.9735200000000002]
[null,null,{"$f":"VLOOKUP($D35,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"CaO: specific GHG emissions"},"FP067d","gCO2_eq/kgfertiliser",{"$f":"VLOOKUP(\"CaO\",matrix_standardvalues,5,FALSE)","v":129.49850000000001},129.49850000000001]
["Pesticides"]
[null,{"$f":"VLOOKUP($D37,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of pesticides"},null,"FP023e","kg/ha",{"$f":"VLOOKUP(D37,Parameters!$1:$1958,6,FALSE)","v":8.36},{"$f":"F37","v":8.36}]
[null,null,{"$f":"VLOOKUP($D38,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of pesticides"},"FP050e","MJ/kgpesticides",{"$f":"VLOOKUP(\"Pesticides\",matrix_standardvalues,10,FALSE)","v":268.39980000000003},{"$f":"F38","v":268.39980000000003}]
[null,null,{"$f":"VLOOKUP($D39,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Pesticides: specific GHG emissions"},"FP067e","gCO2_eq/kgpesticides",{"$f":"VLOOKUP(\"Pesticides\",matrix_standardvalues,5,FALSE)","v":10971.3197},{"$f":"F39","v":10971.3197}]
["Agrifuel"]
[null,{"$f":"VLOOKUP($D41,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for agricultural machinery"},null,"FP034","-",{"$f":"VLOOKUP(D41,Parameters!$1:$1958,6,FALSE)","v":"Diesel"},{"$f":"F41","v":"Diesel"}]
[null,{"$f":"VLOOKUP($D42,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used in agricultural machinery"},null,"FP037","kg/ha",{"$f":"VLOOKUP(D42,Parameters!$1:$1958,6,FALSE)","v":47.902000000000001},47.902000000000001]
[null,null,{"$f":"VLOOKUP($D43,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of fuel used in agricultural machinery"},"FP036","MJ/kgfuel",{"$f":"IF(G41=\"n.a.\",0,VLOOKUP(G41,matrix_standardvalues,10,FALSE))","v":49.995999999999995},49.995999999999995]
[null,null,{"$f":"VLOOKUP($D44,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions of the fuel used in agricultural machinery"},"FP059","gCO2_eq/kgfuel",{"$f":"IF(G41=\"n.a.\",0,VLOOKUP(G41,matrix_standardvalues,5,FALSE))","v":3777.2361111111118},3777.2361111111118]
[null,null,{"$f":"VLOOKUP($D45,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Agrifuel NOx emissions factor"},"FP111a","gNOX/kgfuel",{"$f":"IF(G41=\"n.a.\",0,VLOOKUP(G41,matrix_standardvalues,26,FALSE))","v":38.272800000000004},38.272800000000004]
[null,null,{"$f":"VLOOKUP($D46,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Agrifuel SOx emissions factor"},"FP111b","gSOX/kgfuel",{"$f":"IF(G41=\"n.a.\",0,VLOOKUP(G41,matrix_standardvalues,28,FALSE))","v":14.869499999999999},14.869499999999999]
["By-products"]
[null,"By-product 1"]
[null,{"$f":"VLOOKUP($D49,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 1"},null,"FP016a","-",{"$f":"VLOOKUP(D49,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F49","v":"n.a."}]
[null,{"$f":"VLOOKUP($D50,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of by-product 1 per ha"},null,"FP017a","kg/ha",{"$f":"VLOOKUP(D50,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"IF(F50=\"n.a.\",0,F50)","v":0}]
[null,{"$f":"VLOOKUP($D51,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of by-product 1 per ha"},null,"FP018a","MJ/ha",null,{"$f":"G50*G52*(100-G53)/100","v":0},"=FP017a*FP020a*(100-FP019a)/100"]
[null,{"$f":"VLOOKUP($D52,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of the dry by-product 1 (LHV)"},null,"FP020a","MJ/kgdm",{"$f":"IF(G49=\"n.a.\",0,VLOOKUP(G49, matrix_standardvalues,14,FALSE))","v":0},{"$f":"F52","v":0}]
[null,{"$f":"VLOOKUP($D53,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 1"},null,"FP019a","%",{"$f":"IF(G49=\"n.a.\",0,VLOOKUP(G49, matrix_standardvalues,13,FALSE))","v":0},{"$f":"F53","v":0}]
[null,{"$f":"VLOOKUP($D54,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 1"},null,"FP021a","binary",{"$f":"IF(G49=\"n.a.\",0,VLOOKUP(G49, matrix_standardvalues,18,FALSE))","v":0},{"$f":"F54","v":0}]
[null,{"$f":"VLOOKUP($D55,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 1"},null,"FP031a","%",null,{"$f":"IF(G54=1,G51/(G51+G59+G14)*100,0)","v":0},"=FP018a/(FP018a+FP018b+FP003c)*100"]
[null,"By-product 2"]
[null,{"$f":"VLOOKUP($D57,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 2"},null,"FP016b","-",{"$f":"VLOOKUP(D57,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F57","v":"n.a."}]
[null,{"$f":"VLOOKUP($D58,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of by-product 2 per ha"},null,"FP017b","kg/ha",{"$f":"VLOOKUP(D58,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"IF(F58=\"n.a.\",0,F58)","v":0}]
[null,{"$f":"VLOOKUP($D59,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of by-product 2 per ha"},null,"FP018b","MJ/ha",null,{"$f":"G58*G60*(100-G61)/100","v":0},"=FP017b*FP020b*(100-FP019b)/100"]
[null,{"$f":"VLOOKUP($D60,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of the dry by-product 2 (LHV)"},null,"FP020b","MJ/kgdm",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues,14,FALSE))","v":0},{"$f":"F60","v":0}]
[null,{"$f":"VLOOKUP($D61,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 2"},null,"FP019b","%",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues,13,FALSE))","v":0},{"$f":"F61","v":0}]
[null,{"$f":"VLOOKUP($D62,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 2"},null,"FP021b","binary",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues,18,FALSE))","v":0},{"$f":"F62","v":0}]
[null,{"$f":"VLOOKUP($D63,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 2"},null,"FP031b","%",null,{"$f":"IF(G62=1,G59/(G51+G59+G14)*100,0)","v":0},"=FP018b/(FP018a+FP018b+FP003c)*100"]
["Allocation"]
[null,{"$f":"VLOOKUP($D65,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to energy crop"},null,"FP030","%",null,{"$f":"IF(G10=\"No crop\",0,100-G66)","v":100},"=100-FP031"]
[null,{"$f":"VLOOKUP($D66,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-products"},null,"FP031","%",null,{"$f":"G55+G63","v":0},"=FP031a+FP031b"]
["Transport losses"]
[null,{"$f":"VLOOKUP($D68,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield loss through treatment and transport of feedstock 1"},null,"FP054","%",{"$f":"VLOOKUP(D68,Parameters!$1:$1958,6,FALSE)","v":2},{"$f":"F68","v":2}]
[null,{"$f":"VLOOKUP($D69,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of pretreated feedstock 1 before conversion"},null,"FP055a","kg/ha",null,{"$f":"G12*(100-G68)/100","v":18620},"=FP003a*(100-FP054)/100"]
[null,{"$f":"VLOOKUP($D70,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (dry) of pretreated feedstock 1 before conversion"},null,"FP055b","kgdm/ha",null,{"$f":"G13*(100-G68)/100","v":12289.2},"=FP003b*(100-FP054)/100"]
[null,{"$f":"VLOOKUP($D71,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of pretreated feedstock 1 before conversion"},null,"FP055c","MJ/ha",null,{"$f":"G14*(100-G68)/100","v":294940.79999999999},"=FP003c*(100-FP054)/100"]
["Drying & storage (part of 'treatment & transport 1')"]
[null,{"$f":"VLOOKUP($D73,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat energy use for drying and storage of the crop"},null,"FP040","MJheat/kgfm",{"$f":"VLOOKUP(D73,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"IF(F73=\"n.a.\",0,F73)","v":0}]
[null,{"$f":"VLOOKUP($D74,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat source"},null,"FP041","-",{"$f":"VLOOKUP(D74,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F74","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D75,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of heat production for crop drying and storage"},"FP042a","MJ/MJheat",{"$f":"IF(F74=\"n.a.\",0,VLOOKUP(F74, matrix_standardvalues,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D76,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy coefficient of heat production for crop drying and storage"},"FP042b","MJ/MJheat",{"$f":"IF(F74=\"n.a.\",0,VLOOKUP(F74, matrix_standardvalues,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D77,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG coefficient of heat production for crop drying and storage"},"FP042c","gCO2_eq/MJheat",{"$f":"IF(F74=\"n.a.\",0,VLOOKUP(F74, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D78,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of heat production for crop drying and storage"},"FP042d","gNOX/MJheat",{"$f":"IF(G74=\"n.a.\",0,VLOOKUP(G74, matrix_standardvalues,27,FALSE))","v":0},{"$f":"F78","v":0}]
[null,null,{"$f":"VLOOKUP($D79,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of heat production for crop drying and storage"},"FP042e","gSOX/MJheat",{"$f":"IF(G74=\"n.a.\",0,VLOOKUP(G74, matrix_standardvalues,29,FALSE))","v":0},{"$f":"F79","v":0}]
[null,{"$f":"VLOOKUP($D80,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity energy use for drying and storage of the crop"},null,"FP043","MJe/kgfm",{"$f":"VLOOKUP(D80,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"IF(F80=\"n.a.\",0,F80)","v":0}]
[null,{"$f":"VLOOKUP($D81,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity source"},null,"FP044","-",{"$f":"VLOOKUP(D81,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D82,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of electricity for crop drying and storage"},"FP045a","MJ/MJe",{"$f":"IF(F81=\"n.a.\",0,VLOOKUP(F81, matrix_standardvalues,11,FALSE))","v":0},{"$f":"F82","v":0}]
[null,null,{"$f":"VLOOKUP($D83,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy coefficient of electricity for crop drying and storage"},"FP045b","MJ/MJe",{"$f":"IF(F81=\"n.a.\",0,VLOOKUP(F81, matrix_standardvalues,21,FALSE))","v":0},{"$f":"F83","v":0}]
[null,null,{"$f":"VLOOKUP($D84,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG coefficient of electricity for crop drying and storage"},"FP045c","gCO2_eq/MJe",{"$f":"IF(F81=\"n.a.\",0,VLOOKUP(F81, matrix_standardvalues,5,FALSE))","v":0},{"$f":"F84","v":0}]
[null,null,{"$f":"VLOOKUP($D85,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity for crop drying and storage"},"FP045d","gNOX/MJe",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,27,FALSE))","v":0},{"$f":"F85","v":0}]
[null,null,{"$f":"VLOOKUP($D86,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity for crop drying and storage"},"FP045e","gSOX/MJe",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,29,FALSE))","v":0},{"$f":"F86","v":0}]
[null,{"$f":"VLOOKUP($D87,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Pretreated feedstock"},null,"FP047","-",{"$f":"VLOOKUP(D87,Parameters!$1:$1958,6,FALSE)","v":"Fresh palm fruit bunches (FFB)"},{"$f":"F87","v":"Fresh palm fruit bunches (FFB)"}]
[]
["ENERGY BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Feedstock production"]
[null,{"$f":"VLOOKUP($D91,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy used for feedstock production"},null,"FP028a","MJ/kgdm",null,{"$f":"IF(G13=0,0,(G95+G97)/G13)","v":1.1985132664625198},"=(FP035a+FP046a)/FP003b"]
[null,null,null,"FP028b","MJ/ha",null,{"$f":"G95+G97","v":15029.356361439999},"=FP035a+FP046a"]
[null,{"$f":"VLOOKUP($D93,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy used for feedstock production"},null,"FP029a","MJ/kgdm",null,{"$f":"IF(G13=0,0,(G96+G98)/G13)","v":1.1985132664625198},"=(FP035b+FP046b)/FP003b"]
[null,null,null,"FP029b","MJ/ha",null,{"$f":"G96+G98","v":15029.356361439999},"=FP035b+FP046b"]
[null,{"$f":"VLOOKUP($D95,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to agrifuel use"},null,"FP035a","MJ/ha",null,{"$f":"IF(G12>0,G43*G42,0)","v":2394.9083919999998},"=FP036*FP037"]
[null,{"$f":"VLOOKUP($D96,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to agrifuel use"},null,"FP035b","MJ/ha",null,{"$f":"IF(G12>0,G43*G42,0)","v":2394.9083919999998},"=FP036*FP037"]
[null,{"$f":"VLOOKUP($D97,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use of seeds, fertilisers and pesticides"},null,"FP046a","MJ/ha",null,{"$f":"IF(G12>0,G20*G21+G24*G25+G27*G28+G30*G31+G33*G34+G37*G38,0)","v":12634.44796944},"=FP022*FP050f+FP023a*FP050a+FP023b*FP050b+FP023c*FP050c+FP023d*FP050d+FP023e*FP050e"]
[null,{"$f":"VLOOKUP($D98,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use of seeds, fertilisers and pesticides"},null,"FP046b","MJ/ha",null,{"$f":"IF(G12>0,G20*G21+G24*G25+G27*G28+G30*G31+G33*G34+G37*G38,0)","v":12634.44796944},"=FP022*FP050f+FP023a*FP050a+FP023b*FP050b+FP023c*FP050c+FP023d*FP050d+FP023e*FP050e"]
["Energy use after allocation 1"]
[null,{"$f":"VLOOKUP($D100,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated fossil energy requirement for feedstock production"},null,"FP032a","MJfossil/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G92*'Conversion feedstock1'!G65/100/'Conversion feedstock1'!G176)","v":0},"=FP028b*FP030/100/BC015c"]
[null,{"$f":"VLOOKUP($D101,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated primary energy requirement for feedstock production"},null,"FP032b","MJprim/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G94*G65/100/'Conversion feedstock1'!G176)","v":0.30057186106149514},"=FP029b*FP030/100/BC015c"]
["Totally allocated energy use for feedstock production"]
[null,{"$f":"VLOOKUP($D103,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for feedstock production"},null,"FP024a","MJfossil/MJendfuel_fs1",null,{"$f":"G100*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":0},"= FP032a*BC050a/100*BC050b/100"]
[null,{"$f":"VLOOKUP($D104,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for feedstock production"},null,"FP024b","MJprim/MJendfuel_fs1",null,{"$f":"G101*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":0.28755075519938561},"= FP032b*BC050a/100*BC050b/100"]
[null,{"$f":"VLOOKUP($D105,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for feedstock production"},null,"FP025a","MJfossil/MJFU",null,{"$f":"G100*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= FP032a*BC050a/100*BC050b/100*FC025c/100*FC033"]
[null,{"$f":"VLOOKUP($D106,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for feedstock production"},null,"FP025b","MJprim/MJFU",null,{"$f":"G101*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":0.28755075519938561},"= FP032b*BC050a/100*BC050b/100*FC025c/100*FC033"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D108,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy used for heat and electricity for drying and storage per kg"},null,"FP038a","MJfossil/kgfm",null,{"$f":"G73*G75+G80*G82","v":0},"=FP040*FP042a+FP043*FP045a"]
[null,{"$f":"VLOOKUP($D109,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy used for heat and electricity for drying and storage per kg"},null,"FP038b","MJprim/kgfm",null,{"$f":"G73*G76+G80*G83","v":0},"=FP040*FP042b+FP043*FP045b"]
[null,{"$f":"VLOOKUP($D110,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy used for heat and electricity for drying and storage per MJ endfuel"},null,"FP039a","MJfossil/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G108*G12/'Conversion feedstock1'!G176)","v":0},"=FP038a*FP003a/BC015c"]
[null,{"$f":"VLOOKUP($D111,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy used for heat and electricity for drying and storage per MJ endfuel"},null,"FP039b","MJprim/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G109*G12/'Conversion feedstock1'!G176)","v":0},"=FP038b*FP003a/BC015c"]
[]
["GLOBAL WARMING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Field characteristics"]
[null,null,{"$f":"VLOOKUP($D115,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Actual land use"},"FP069a","-",{"$f":"VLOOKUP(D115,Parameters!$1:$1958,6,FALSE)","v":"Perennial cropland"},{"$f":"F115","v":"Perennial cropland"}]
[null,null,{"$f":"VLOOKUP($D116,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previous land use (January 1st, 2008)"},"FP069b","-",{"$f":"VLOOKUP(D116,Parameters!$1:$1958,6,FALSE)","v":"Perennial cropland"},"Perennial cropland"]
[null,null,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previously degraded land"},"FP092a","-",{"$f":"VLOOKUP(D117,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D118,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Climate region"},"FP070a","-",{"$f":"VLOOKUP(D118,Parameters!$1:$1958,6,FALSE)","v":"Tropical Wet"},"Tropical Wet"]
[null,null,{"$f":"VLOOKUP($D119,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Soil type"},"FP070b","-",{"$f":"VLOOKUP(D119,Parameters!$1:$1958,6,FALSE)","v":"Low activity clay soils"},"Low activity clay soils"]
[null,null,{"$f":"VLOOKUP($D120,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Soil water saturation (yes=1,no=0)"},"FP131","binary",{"$f":"VLOOKUP(D120,Parameters!$1:$1958,6,FALSE)","v":1},1]
[null,null,{"$f":"VLOOKUP($D121,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Field renewal (annual crops = 1)"},"FP132","years",{"$f":"VLOOKUP(D121,Parameters!$1:$1958,6,FALSE)","v":1},1]
[null,null,{"$f":"VLOOKUP($D122,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of crop residue returned to the field (only for palm)"},"FP133","kgdm/kgfm",{"$f":"VLOOKUP(D122,Parameters!$1:$1958,6,FALSE)","v":0.22},0.22]
[null,null,{"$f":"VLOOKUP($D123,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Organic soil (yes=1,no=0)"},"FP134","binary",{"$f":"VLOOKUP(D123,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D124,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Nutrient level (only for ORGANIC soils + temperate/boreal climate + forest (native and managed))"},"FP135","-",{"$f":"VLOOKUP(D124,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D125,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previous land use is cropland (yes=1,no=0)"},"FP153","binary",null,{"$f":"IF(G116=\"Grassland and savannah\",0,IF(G116=\"Native forest non degraded\",0,IF(G116=\"Managed forest\",0,1)))","v":1}]
["GHG emissions from inputs for feedstock production"]
[null,{"$f":"VLOOKUP($D128,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with inputs for feedstock production"},null,"FP056a","gCO2-eq/kgdm",null,{"$f":"IF(G12>0,(G129+G130)/G13,0)","v":102.49380483244373},"=(FP058+FP064)/FP003b"]
[null,null,null,"FP056b","gCO2-eq/ha",null,{"$f":"IF(G12>0,G129+G130,0)","v":1285272.3125988443},"=FP058+FP064"]
[null,null,{"$f":"VLOOKUP($D129,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with fuel used in agricultural machinery"},"FP058","gCO2-eq/ha",null,{"$f":"G42*G44","v":180937.16419444449},"=FP037*FP059"]
[null,null,{"$f":"VLOOKUP($D130,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with production of seeds, fertilisers and pesticides"},"FP064","gCO2-eq/ha",null,{"$f":"G20*G22+G24*G26+G27*G29+G30*G32+G33*G35+G37*G39","v":1104335.1484043999},"=FP022*FP067f+FP023a*FP067a+FP023b*FP067b+FP023c*FP067c+FP023d*FP067d+FP023e*FP067e"]
["Field N2O emissions"]
[null,{"$f":"VLOOKUP($D132,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total (direct + indirect) N2O emissions from managed soils"},null,"FP130a","gN20/ha",null,{"$f":"IF(G10=\"No crop\",0,(G140+G164)*1000)","v":3548.3422857142855},"=(FP138b+FP155b)*1000"]
[null,{"$f":"VLOOKUP($D133,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total (direct + indirect) N2O emissions from managed soils"},null,"FP130b","gCO2-eq/ha",null,{"$f":"G132*'Standard Values'!D6","v":1050309.3165714284},"=FP130a*GWP_N20"]
[null,null,{"$f":"VLOOKUP($D134,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for direct N2O emissions from N inputs"},"FP137a","kgN20_N/kgN_input",{"$f":"VLOOKUP(\"EF1\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.01},{"$f":"F134","v":0.01}]
[null,null,{"$f":"VLOOKUP($D135,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for direct N2O emissions from drained/managed organic soils"},"FP137b","kgN20_N/ha",{"$f":"VLOOKUP(\"EF2 \"&G118&\" \"&G115&\" \"&G124,Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":16},{"$f":"IF(G10=\"No crop\",0,IF(F135=\"n.a.\",0,F135))","v":16}]
[null,null,{"$f":"VLOOKUP($D136,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for direct N2O emissions from urine and dung N deposited by grazing animals"},"FP137c","kgN20_N/kgN_input"]
[null,null,{"$f":"VLOOKUP($D137,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for indirect N2O emissions from atmospheric deposition of N"},"FP137d","kgN20_N/kgN_volatilised",{"$f":"VLOOKUP(\"EF4\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.01},{"$f":"F137","v":0.01}]
[null,null,{"$f":"VLOOKUP($D138,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for indirect N2O emissions from leaching and runoff"},"FP137e","kgN20_N/kgN_leached+runoff",{"$f":"VLOOKUP(\"EF5\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":7.4999999999999997E-3},{"$f":"F138","v":7.4999999999999997E-3}]
[null,{"$f":"VLOOKUP($D139,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Direct N2O_N emissions from managed soils"},null,"FP138a","kgN20_N/ha",null,{"$f":"G141+G162","v":1.73888},"=FP139+FP154"]
[null,{"$f":"VLOOKUP($D140,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Direct N2O emissions from managed soils"},null,"FP138b","kgN20/ha",null,{"$f":"G139*44/28","v":2.732525714285714},"=FP138a*44/28"]
[null,{"$f":"VLOOKUP($D141,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Direct N2O_N emissions from N inputs to managed mineral soils"},null,"FP139","kgN20_N/ha",null,{"$f":"(G24+G142+G147+G159)*G134","v":1.73888},"=(FP023a+FP140+FP142+FP150)*FP137a"]
[null,{"$f":"VLOOKUP($D142,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total amount of organic N fertiliser applied to soil (other than by grazing animals)"},null,"FP140","kgN/ha",null,{"$f":"IF(G123=1,0,G143+G144+G145+G146)","v":0},"=FP141a+FP141b+FP141c+FP141d"]
[null,null,{"$f":"VLOOKUP($D143,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of animal manure N applied to soil (other than by grazing animals)"},"FP141a","kgN/ha",{"$f":"VLOOKUP(D143,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F143","v":0}]
[null,null,{"$f":"VLOOKUP($D144,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of total sewage N applied to soil"},"FP141b","kgN/ha",{"$f":"VLOOKUP(D144,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F144","v":0}]
[null,null,{"$f":"VLOOKUP($D145,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of total compost N applied to soil"},"FP141c","kgN/ha",{"$f":"VLOOKUP(D145,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F145","v":0}]
[null,null,{"$f":"VLOOKUP($D146,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of N of other organic amendments applied to soil (used as fertiliser)"},"FP141d","kgN/ha",{"$f":"VLOOKUP(D146,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F146","v":0}]
[null,{"$f":"VLOOKUP($D147,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total amount of N in crop residues (including N-fixing crops and renewal) returned to soil"},null,"FP142","kgN/ha",null,{"$f":"IF(G10=\"No crop\",0,IF(G123=1,0,G13/G121*(G149*G156*(1-G158)+G154*G157)))","v":45.98},"=FP003b/FP132*(FP143b*FP148a*(1-FP149)+FP146b*FP148b)"]
[null,null,{"$f":"VLOOKUP($D148,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of above-ground residues to harvested yield_calculated"},"FP143a","kgdm/kgdm",null,{"$f":"IF(G13=0,0,G150*1000/G13)","v":0.33333333333333331},"=FP144*1000/FP003b"]
[null,null,{"$f":"VLOOKUP($D149,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of above-ground residues to harvested yield_final"},"FP143b","kgdm/kgdm",{"$f":"VLOOKUP(D149,Parameters!$1:$1958,6,FALSE)","v":0.33333333333333331},{"$f":"F149","v":0.33333333333333331}]
[null,null,{"$f":"VLOOKUP($D150,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above-ground residue (dry) (=AGDM(T))"},"FP144","t/ha",null,{"$f":"IF(G10=\"Fresh palm fruit bunches (FFB)\",G12*G122/1000,G13*G151/1000+G152)","v":4.18},"FFB: =FP003a*FP133/1000 ; Other: =FP003b*FP145a/1000+FP145b"]
[null,null,{"$f":"VLOOKUP($D151,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Slope to calculate above-ground residue"},"FP145a","-",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],2,FALSE)","v":"n.a."},{"$f":"IF(G10=\"No crop\",0,F151)","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D152,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Intercept to calculate above-ground residue"},"FP145b","-",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],4,FALSE)","v":"n.a."},{"$f":"IF(G10=\"No crop\",0,F152)","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D153,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below-ground residues to harvested yield_calculated"},"FP146a","kgdm/kgdm",null,{"$f":"IF(G13=0,0,G155*(G150*1000+G13)/G13)","v":0},"=FP147*(FP144*1000+FP003b)/FP003b"]
[null,null,{"$f":"VLOOKUP($D154,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below-ground residues to harvested yield_final"},"FP146b","kgdm/kgdm",{"$f":"VLOOKUP(D154,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F154","v":0}]
[null,null,{"$f":"VLOOKUP($D155,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below-ground residues to above-ground biomass"},"FP147","kgdm/kgdm",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],9,FALSE)","v":0},{"$f":"IF(G10=\"No crop\",0,F155)","v":0}]
[null,null,{"$f":"VLOOKUP($D156,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N content of above-ground residues"},"FP148a","kgN/kgdm",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],7,FALSE)","v":1.0999999999999999E-2},{"$f":"IF(G10=\"No crop\",0,F156)","v":1.0999999999999999E-2}]
[null,null,{"$f":"VLOOKUP($D157,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N content of below-ground residues"},"FP148b","kgN/kgdm",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],8,FALSE)","v":1.0999999999999999E-2},{"$f":"IF(G10=\"No crop\",0,F157)","v":1.0999999999999999E-2}]
[null,null,{"$f":"VLOOKUP($D158,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fraction of above-ground residues removed"},"FP149","%",{"$f":"VLOOKUP(D158,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F158","v":0}]
[null,{"$f":"VLOOKUP($D159,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total amount of N mineralised in mineral soil due to carbon loss through land use change"},null,"FP150","kgN/ha",null,{"$f":"IF(G123=1,0,G160/G161*1000)","v":0},"=FP151/FP152*1000"]
[null,null,{"$f":"VLOOKUP($D160,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Average annual loss of soil carbon"},"FP151","tC/ha",null,{"$f":"(G202-G174)/20","v":0},"=(FP072-FP071)/20"]
[null,null,{"$f":"VLOOKUP($D161,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"C:N ratio of the soil organic matter"},"FP152","-",null,{"$f":"IF(G125=1,10,15)","v":10}]
[null,{"$f":"VLOOKUP($D162,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Direct N2O_N emissions from managed organic soils"},null,"FP154","kgN20_N/ha",null,{"$f":"IF(G123=1,G135,0)","v":0}]
[null,{"$f":"VLOOKUP($D163,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Indirect N2O_N emissions from managed soils"},null,"FP155a","kgN20_N/ha",null,{"$f":"G165+G168","v":0.51915599999999995},"=FP156+FP159"]
[null,{"$f":"VLOOKUP($D164,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Indirect N2O emissions from managed soils"},null,"FP155b","kgN20/ha",null,{"$f":"G163*44/28","v":0.81581657142857134},"=FP155a*44/28"]
[null,{"$f":"VLOOKUP($D165,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Indirect N2O_N emissions from atmospheric deposition of N volatilized from managed soils"},null,"FP156","kgN20_N/ha",null,{"$f":"(G24*G166+G142*G167)*G137","v":0.12790800000000002},"=(FP023a*FP157+FP140*FP158)*FP137d"]
[null,null,{"$f":"VLOOKUP($D166,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fraction of synthetic fertiliser N that volatilises as NH3 and NOx"},"FP157","kgN_volatilised/kgN_applied",{"$f":"VLOOKUP(\"FRACgasf\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.1},{"$f":"F166","v":0.1}]
[null,null,{"$f":"VLOOKUP($D167,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fraction of organic fertiliser N that volatilises as NH3 and NOx"},"FP158","kgN_volatilised/kgN_applied",{"$f":"VLOOKUP(\"FRACgasm\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.2},{"$f":"F167","v":0.2}]
[null,{"$f":"VLOOKUP($D168,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Indirect N2O_N emissions from N leaching/runoff from managed soils"},null,"FP159","kgN20_N/ha",null,{"$f":"(G24+G142+G147+G159)*G169*G138","v":0.39124799999999998},"=(FP023a+FP140+FP142+FP150)*FP160*FP137e"]
[null,null,{"$f":"VLOOKUP($D169,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fraction of all N added to managed soils that is lost through leaching and runoff"},"FP160","kgN_leached/kgN_applied",{"$f":"VLOOKUP(\"FRACleach\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.3},{"$f":"F169","v":0.3}]
["Carbon stock changes from land use change"]
[null,{"$f":"VLOOKUP($D171,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with land use change (carbon stock changes) per MJ"},null,"FP068a","gCO2-eq/MJendfuel_fs1 (over 20yr)",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G172/'Conversion feedstock1'!G176)","v":0},"=FP068b/BC015c"]
[null,null,null,"FP068b","gCO2-eq/ha (over 20yr)",null,{"$f":"IF(G10=\"No crop\",0,((G202-G174)/20+G123*G230)*1000000*3.664-G231*G117*'Conversion feedstock1'!G176)","v":0},"=((FP072-FP071)/20+FP091a*FP091b)*1000000*3.664-FP092a*FP092b*BC015c"]
[null,null,{"$f":"VLOOKUP($D173,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Standard soil organic carbon_feedstock 1"},"FP074","tC/ha",{"$f":"VLOOKUP(G118&\" \"&G119,Table_IPCC_SOC[],4,FALSE)","v":60},{"$f":"IF(G10=\"No crop\",0,F173)","v":60}]
[null,{"$f":"VLOOKUP($D174,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock actual land use"},null,"FP071","tC/ha",null,{"$f":"G183+G187","v":141.25200000000001},"=FP073a+FP078a"]
[null,null,{"$f":"VLOOKUP($D175,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Actual land use_specific for carbon stock veg"},"FP069c","-",{"$f":"VLOOKUP(D175,Parameters!$1:$1958,6,FALSE)","v":"Oil palm"},{"$f":"F175","v":"Oil palm"}]
[null,null,{"$f":"VLOOKUP($D176,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Climate region_specific for carbon stock_actual land use"},"FP070c","-",{"$f":"VLOOKUP(D176,Parameters!$1:$1958,6,FALSE)","v":"Tropical wet"},{"$f":"F176","v":"Tropical wet"}]
[null,null,{"$f":"VLOOKUP($D177,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land management actual land use"},"FP093a","-",{"$f":"VLOOKUP(D177,Parameters!$1:$1958,6,FALSE)","v":"No till"},{"$f":"F177","v":"No till"}]
[null,null,{"$f":"VLOOKUP($D178,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input actual land use"},"FP094a","-",{"$f":"VLOOKUP(D178,Parameters!$1:$1958,6,FALSE)","v":"High without manure"},"High without manure"]
[null,null,{"$f":"VLOOKUP($D179,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Domain actual land use"},"FP095a","-",{"$f":"VLOOKUP(D179,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D180,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ecological zone actual land use"},"FP096a","-",{"$f":"VLOOKUP(D180,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D181,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Continent actual land use"},"FP097a","-",{"$f":"VLOOKUP(D181,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D182,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type actual land use"},"FP098a","-",{"$f":"VLOOKUP(D182,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,{"$f":"VLOOKUP($D183,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Soil organic carbon actual land use"},null,"FP073a","tC/ha",null,{"$f":"G173*G184*G185*G186","v":81.25200000000001},"=FP074*FP075a*FP076a*FP077a"]
[null,null,{"$f":"VLOOKUP($D184,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use factor actual land use"},"FP075a","-",{"$f":"VLOOKUP(G115&\" \"&G118&\" \"&G177&\" \"&G178,Table_IPCC_factors[],6,FALSE)","v":1},{"$f":"IF(G10=\"No crop\",0,F184)","v":1}]
[null,null,{"$f":"VLOOKUP($D185,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Management factor actual land use"},"FP076a","-",{"$f":"VLOOKUP(G115&\" \"&G118&\" \"&G177&\" \"&G178,Table_IPCC_factors[],7,FALSE)","v":1.22},{"$f":"IF(G10=\"No crop\",0,F185)","v":1.22}]
[null,null,{"$f":"VLOOKUP($D186,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input factor actual land use"},"FP077a","-",{"$f":"VLOOKUP(G115&\" \"&G118&\" \"&G177&\" \"&G178,Table_IPCC_factors[],8,FALSE)","v":1.1100000000000001},{"$f":"IF(G10=\"No crop\",0,F186)","v":1.1100000000000001}]
[null,{"$f":"VLOOKUP($D187,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock actual land use"},null,"FP078a","tC/ha",null,{"$f":"IF(G10=\"No crop\",0,IF(G188=0,VLOOKUP(G175&\" \"&G179&\" \"&G176&\" \"&G180&\" \"&G181&\" \"&G182,Table_IPCC_Cvegetation[],8,FALSE),G188+G197))","v":60},"=FP079a + FP086a"]
[null,null,{"$f":"VLOOKUP($D188,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock in living biomass actual land use"},"FP079a","tC/ha",null,{"$f":"G189+G195","v":0},"=FP080a + FP084a"]
[null,null,{"$f":"VLOOKUP($D189,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above ground vegetation carbon stock in living biomass actual land use"},"FP080a","tC/ha",null,{"$f":"G190*G191","v":0},"=FP081a*FP082aa"]
[null,null,{"$f":"VLOOKUP($D190,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of above ground living biomass actual land use"},"FP081a","t/ha",{"$f":"VLOOKUP(D190,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F190","v":0}]
[null,null,{"$f":"VLOOKUP($D191,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in living biomass actual land use"},"FP082aa","-",{"$f":"VLOOKUP(D191,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F191","v":0}]
[null,null,{"$f":"VLOOKUP($D192,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in dead wood actual land use"},"FP082ba","-",{"$f":"VLOOKUP(D192,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D193,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in litter actual land use"},"FP082ca","-",{"$f":"VLOOKUP(D193,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D194,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below ground carbon stock to above ground carbon stock in living biomass actual land use"},"FP083a","-",{"$f":"VLOOKUP(D194,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F194","v":0}]
[null,null,{"$f":"VLOOKUP($D195,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Below ground vegetation carbon stock in living biomass actual land use"},"FP084a","tC/ha",null,{"$f":"IF(G196=0,G189*G194,G196*G191)","v":0},"=FP085a*FP082aa of FP080a*FP083a"]
[null,null,{"$f":"VLOOKUP($D196,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of below ground living biomass actual land use"},"FP085a","t/ha",{"$f":"VLOOKUP(D196,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F196","v":0}]
[null,null,{"$f":"VLOOKUP($D197,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock in dead organic matter actual land use"},"FP086a","tC/ha",null,{"$f":"G198+G200","v":0},"=FP087a + FP089a"]
[null,null,{"$f":"VLOOKUP($D198,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock in dead wood pool actual land use"},"FP087a","tC/ha",null,{"$f":"G199*G192","v":0},"=FP088a*FP082ba"]
[null,null,{"$f":"VLOOKUP($D199,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of dead wood pool actual land use"},"FP088a","t/ha",{"$f":"VLOOKUP(D199,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F199","v":0}]
[null,null,{"$f":"VLOOKUP($D200,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock in litter actual land use"},"FP089a","tC/ha",null,{"$f":"G201*G193","v":0},"=FP090a*FP082ca"]
[null,null,{"$f":"VLOOKUP($D201,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of litter actual land use"},"FP090a","t/ha",{"$f":"VLOOKUP(D201,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F201","v":0}]
[null,{"$f":"VLOOKUP($D202,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock previous land use"},null,"FP072","tC/ha",null,{"$f":"G211+G215","v":141.25200000000001},"=FP073b+FP078b"]
[null,null,{"$f":"VLOOKUP($D203,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previous land use (January 1st, 2008)_specific for carbon stock veg"},"FP069d","-",{"$f":"VLOOKUP(D203,Parameters!$1:$1958,6,FALSE)","v":"Oil palm"},{"$f":"F203","v":"Oil palm"}]
[null,null,{"$f":"VLOOKUP($D204,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Climate region_specific for carbon stock_previous land use"},"FP070d","-",{"$f":"VLOOKUP(D204,Parameters!$1:$1958,6,FALSE)","v":"Tropical wet"},{"$f":"F204","v":"Tropical wet"}]
[null,null,{"$f":"VLOOKUP($D205,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land management previous land use"},"FP093b","-",{"$f":"VLOOKUP(D205,Parameters!$1:$1958,6,FALSE)","v":"No till"},{"$f":"F205","v":"No till"}]
[null,null,{"$f":"VLOOKUP($D206,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input previous land use"},"FP094b","-",{"$f":"VLOOKUP(D206,Parameters!$1:$1958,6,FALSE)","v":"High without manure"},"High without manure"]
[null,null,{"$f":"VLOOKUP($D207,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Domain previous land use"},"FP095b","-",{"$f":"VLOOKUP(D207,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D208,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ecological zone previous land use"},"FP096b","-",{"$f":"VLOOKUP(D208,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D209,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Continent previous land use"},"FP097b","-",{"$f":"VLOOKUP(D209,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D210,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type previous land use"},"FP098b","-",{"$f":"VLOOKUP(D210,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,{"$f":"VLOOKUP($D211,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Soil organic carbon previous land use"},null,"FP073b","tC/ha",null,{"$f":"G173*G212*G213*G214","v":81.25200000000001},"=FP074*FP075b*FP076b*FP077b"]
[null,null,{"$f":"VLOOKUP($D212,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use factor previous land use"},"FP075b","-",{"$f":"VLOOKUP(G116&\" \"&G118&\" \"&G205&\" \"&G206,Table_IPCC_factors[],6,FALSE)","v":1},{"$f":"IF(G10=\"No crop\",0,F212)","v":1}]
[null,null,{"$f":"VLOOKUP($D213,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Management factor previous land use"},"FP076b","-",{"$f":"VLOOKUP(G116&\" \"&G118&\" \"&G205&\" \"&G206,Table_IPCC_factors[],7,FALSE)","v":1.22},{"$f":"IF(G10=\"No crop\",0,F213)","v":1.22}]
[null,null,{"$f":"VLOOKUP($D214,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input factor previous land use"},"FP077b","-",{"$f":"VLOOKUP(G116&\" \"&G118&\" \"&G205&\" \"&G206,Table_IPCC_factors[],8,FALSE)","v":1.1100000000000001},{"$f":"IF(G10=\"No crop\",0,F214)","v":1.1100000000000001}]
[null,{"$f":"VLOOKUP($D215,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock previous land use"},null,"FP078b","tC/ha",null,{"$f":"IF(G10=\"No crop\",0,IF(G216=0,VLOOKUP(G203&\" \"&G207&\" \"&G204&\" \"&G208&\" \"&G209&\" \"&G210,Table_IPCC_Cvegetation[],8,FALSE),G216+G225))","v":60},"=FP079b + FP086b"]
[null,null,{"$f":"VLOOKUP($D216,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock in living biomass previous land use"},"FP079b","tC/ha",null,{"$f":"G217+G223","v":0},"=FP080b + FP084b"]
[null,null,{"$f":"VLOOKUP($D217,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above ground vegetation carbon stock in living biomass previous land use"},"FP080b","tC/ha",null,{"$f":"G218*G219","v":0},"=FP081b*FP082ab"]
[null,null,{"$f":"VLOOKUP($D218,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of above ground living biomass previous land use"},"FP081b","t/ha",{"$f":"VLOOKUP(D218,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F218","v":0}]
[null,null,{"$f":"VLOOKUP($D219,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in living biomass previous land use"},"FP082ab","-",{"$f":"VLOOKUP(D219,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F219","v":0}]
[null,null,{"$f":"VLOOKUP($D220,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in dead wood previous land use"},"FP082bb","-",{"$f":"VLOOKUP(D220,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D221,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in litter previous land use"},"FP082cb","-",{"$f":"VLOOKUP(D221,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D222,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below ground carbon stock to above ground carbon stock in living biomass previous land use"},"FP083b","-",{"$f":"VLOOKUP(D222,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F222","v":0}]
[null,null,{"$f":"VLOOKUP($D223,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Below ground vegetation carbon stock in living biomass previous land use"},"FP084b","tC/ha",null,{"$f":"IF(G224=0,G217*G222,G224*G219)","v":0},"=FP085b*FP082ab of FP080b*FP083b"]
[null,null,{"$f":"VLOOKUP($D224,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of below ground living biomass previous land use"},"FP085b","t/ha",{"$f":"VLOOKUP(D224,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F224","v":0}]
[null,null,{"$f":"VLOOKUP($D225,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock in dead organic matter previous land use"},"FP086b","tC/ha",null,{"$f":"G226+G228","v":0},"=FP087b + FP089b"]
[null,null,{"$f":"VLOOKUP($D226,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock in dead wood pool previous land use"},"FP087b","tC/ha",null,{"$f":"G227*G220","v":0},"=FP088b*FP082bb"]
[null,null,{"$f":"VLOOKUP($D227,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of dead wood pool previous land use"},"FP088b","t/ha",{"$f":"VLOOKUP(D227,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F227","v":0}]
[null,null,{"$f":"VLOOKUP($D228,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock in litter previous land use"},"FP089b","tC/ha",null,{"$f":"G229*G221","v":0},"=FP090b*FP082cb"]
[null,null,{"$f":"VLOOKUP($D229,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of litter previous land use"},"FP090b","t/ha",{"$f":"VLOOKUP(D229,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F229","v":0}]
[null,null,{"$f":"VLOOKUP($D230,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor soil organic carbon_peatland"},"FP091b","tC/ha",{"$f":"'Standard Values'!S155","v":20},{"$f":"F230","v":20}]
[null,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previously degraded land"},null,"FP092b","gCO2-eq/MJ (per year)",{"$f":"'Standard Values'!I154","v":29},{"$f":"F231","v":29}]
[null,{"$f":"VLOOKUP($D232,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with indirect land use change (soil carbon release)"},null,"FP099","gCO2-eq/ha (spread over 20yr)"]
["GHG emissions after allocation 1"]
[null,{"$f":"VLOOKUP($D234,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated GHG emissions from feedstock production"},null,"FP057","gCO2_eq/MJendfuel_fs1",null,{"$f":"IF(G10=\"No crop\",0,(G128+G133+G172)*G65/100/'Conversion feedstock1'!G176)","v":46.709260201046042},"=(FP056b+FP130b+FP068b)*FP030/100/BC015c"]
["Totally allocated GHG emissions from feedstock production"]
[null,{"$f":"VLOOKUP($D236,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from feedstock production"},null,"FP061a","gCO2_eq/MJendfuel_fs1",null,{"$f":"G234*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":44.685763325221714},"=FP057*BC050a/100*BC050b/100"]
[null,{"$f":"VLOOKUP($D237,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from feedstock production"},null,"FP061b","gCO2_eq/MJFU",null,{"$f":"G234*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":44.685763325221714},"=FP057*BC050a/100*BC050b/100*FC025c/100*FC033"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D239,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with heat and electricity for drying and storage per kg"},null,"FP062a","gCO2-eq/kgfm",null,{"$f":"G73*G77+G80*G84","v":0},"=FP040*FP042c+FP043*FP045c"]
[null,{"$f":"VLOOKUP($D240,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with heat and electricity for drying and storage per MJ endfuel"},null,"FP062b","gCO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G239*G12/'Conversion feedstock1'!G176)","v":0},"=FP062a*FP003a/BC015c"]
["Carbon debt & repayment time"]
[null,{"$f":"VLOOKUP($D242,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon debt due to land use change"},null,"FP107a","gCO2-eq/ha",null,{"$f":"G172*20","v":0},"=FP068b*20"]
[null,{"$f":"VLOOKUP($D243,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated carbon debt"},null,"FP107b","gCO2-eq/ha",null,{"$f":"G242*G65/100","v":0},"=FP107a*FP030/100"]
[null,{"$f":"VLOOKUP($D244,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated carbon debt"},null,"FP107c","gCO2-eq/ha",null,{"$f":"G243*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100","v":0},"=FP107b*BC050a/100*BC050b/100*FC025c/100"]
[null,{"$f":"VLOOKUP($D245,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated GHG emissions from feedstock production without LUC emissions"},null,"FP108","gCO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,(G128+G133)*G65/100/'Conversion feedstock1'!G176)","v":46.709260201046042},"=(FP056b+FP130b)*FP030/100/BC015c"]
[]
["RESOURCE USE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["USE OF WATER"]
[null,{"$f":"VLOOKUP($D249,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock production"},null,"FP100","m³/ha",{"$f":"VLOOKUP(D249,Parameters!$1:$1958,6,FALSE)","v":22067.5},{"$f":"F249","v":22067.5}]
[null,{"$f":"VLOOKUP($D250,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Country freshwater availability"},null,"FP104a","m³/capita.yr",{"$f":"IF(G11=\"n.a.\",0,VLOOKUP(G11,table_FAO_water[],2,FALSE))","v":23320},{"$f":"F250","v":23320}]
[null,{"$f":"VLOOKUP($D251,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Country freshwater level"},null,"FP104b","-",{"$f":"IF(G11=\"n.a.\",0,VLOOKUP(G11,table_FAO_water[],3,FALSE))","v":"high"},{"$f":"F251","v":"high"}]
["Use of water after allocation 1"]
[null,{"$f":"VLOOKUP($D253,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated water use for feedstock production"},null,"FP101","m³/GJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G249*G65/100/'Conversion feedstock1'!G176*1000)","v":441.32758479212958},"=FP100*FP030/100/BC015c*1000"]
["Totally allocated water use for feedstock production"]
[null,{"$f":"VLOOKUP($D255,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use for feedstock production"},null,"FP102a","m³/GJendfuel_fs1",null,{"$f":"G253*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":422.20878511090552},"= FP101*BC050a/100*BC050b/100"]
[null,{"$f":"VLOOKUP($D256,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use for feedstock production"},null,"FP102b","m³/GJFU",null,{"$f":"G253*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":422.20878511090552},"= FP101*BC050a/100*BC050b/100*FC025c/100*FC033"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D258,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},null,"FP103a","m³/kgfm",{"$f":"VLOOKUP(D258,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F258","v":0}]
[null,{"$f":"VLOOKUP($D259,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},null,"FP103b","m³/GJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G258*G12/'Conversion feedstock1'!G176*1000)","v":0},"=FP103a*FP003a/BC015c*1000"]
["USE OF LAND"]
["Use of land after allocation 1"]
[null,{"$f":"VLOOKUP($D262,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated land use for feedstock production"},null,"FP105","ha/GJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G65/'Conversion feedstock1'!G176*10)","v":1.9998984243440789E-2},"=FP030/100/BC015c*1000"]
["Totally allocated land use for feedstock production"]
[null,{"$f":"VLOOKUP($D264,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated land use for feedstock production"},null,"FP106a","ha/GJendfuel_fs1",null,{"$f":"G262*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":1.9132606099961733E-2},"= FP105*BC050a/100*BC050b/100"]
[null,{"$f":"VLOOKUP($D265,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated land use for feedstock production"},null,"FP106b","ha/GJFU",null,{"$f":"G264*'Final conversion'!G68/100*'Final conversion'!G22","v":1.9132606099961733E-2},"= FP106a*FC025c/100*FC033"]
[]
["ENVIRONMENTAL QUALITY",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["ACIDIFICATION POTENTIAL"]
["Feedstock production"]
[null,{"$f":"VLOOKUP($D270,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential from feedstock production"},null,"FP112","gSO2_eq/ha",null,{"$f":"G272*G273+G42*G45*G274+G42*G46*G275","v":41003.664154919999},"=FP113*FP110a+FP037*FP111a*FP110b+FP037*FP111b*FP110c"]
[null,null,{"$f":"VLOOKUP($D271,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input of N-fixing crop residue to the soil"},"FP109","kg/ha",{"$f":"VLOOKUP(D271,Parameters!$1:$1958,6,FALSE)","v":45},{"$f":"F271","v":45}]
[null,null,{"$f":"VLOOKUP($D272,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH3 volatilization from fertiliser use"},"FP113","gNH3/ha",null,{"$f":"(G24+G271)*1000*0.12","v":20748.960000000003},"=(FP023a+FP109)*1000*volatilization fraction NH3"]
[null,null,{"$f":"VLOOKUP($D273,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of NH3"},"FP110a","gSO2_eq/gNH3",{"$f":"VLOOKUP(\"NH3\",matrix_standardvalues_emissions,24,FALSE)","v":1.88},{"$f":"F273","v":1.88}]
[null,null,{"$f":"VLOOKUP($D274,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of NOx"},"FP110b","gSO2_eq/gNOx",{"$f":"VLOOKUP(\"NOx\",matrix_standardvalues_emissions,24,FALSE)","v":0.7},{"$f":"F274","v":0.7}]
[null,null,{"$f":"VLOOKUP($D275,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of SOx"},"FP110c","gSO2_eq/gSOx",{"$f":"VLOOKUP(\"SOx\",matrix_standardvalues_emissions,24,FALSE)","v":1},{"$f":"F275","v":1}]
["Acidification potential after allocation 1"]
[null,{"$f":"VLOOKUP($D277,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated acidification potential from feedstock production"},null,"FP114","gSO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G270*G65/100/'Conversion feedstock1'!G176)","v":0.82003163335758289},"=FP112*FP030/100/BC015c"]
["Totally allocated acidification potential from feedstock production"]
[null,{"$f":"VLOOKUP($D279,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from feedstock production"},null,"FP115a","gSO2_eq/MJendfuel_fs1",null,{"$f":"G277*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":0.78450695493120459},"=FP114*BC050a/100*BC050b/100"]
[null,{"$f":"VLOOKUP($D280,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from feedstock production"},null,"FP115b","gSO2_eq/MJFU",null,{"$f":"G279*'Final conversion'!G68/100*'Final conversion'!G22","v":0.78450695493120459},"=FP115a*FC025c/100*FC033"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D282,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with heat and electricity for drying and storage per kg"},null,"FP116a","gSO2-eq/kgfm",null,{"$f":"G73*G78*G274+G73*G79*G275+G80*G85*G274+G80*G86*G275","v":0},"=FP040*FP042d*FP110b+FP040*FP042e*FP110c+FP043*FP045d*FP110b+FP043*FP045e*FP110c"]
[null,{"$f":"VLOOKUP($D283,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with heat and electricity for drying and storage per MJ endfuel"},null,"FP116b","gSO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G282*G12/'Conversion feedstock1'!G176)","v":0},"=FP116a*FP003a/BC015c"]
["EUTROPHICATION POTENTIAL"]
["Feedstock production"]
[null,{"$f":"VLOOKUP($D286,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of feedstock production"},null,"FP122","gPO4_eq/ha",null,{"$f":"G287*G288+G42*G45*G289+G291*G292+G295*G296","v":104087.47707652803},"=FP123a*FP120a+FP037*FP111a*FP120b+FP123d*FP120d+FP123g*FP120g"]
[null,null,{"$f":"VLOOKUP($D287,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N volatilization from fertiliser use (including NOx and NH3)"},"FP123a","gN/ha",null,{"$f":"(G24+G271)*1000*0.1","v":17290.800000000003},"=(FP023a+FP108)*1000*volatilization fraction N"]
[null,null,{"$f":"VLOOKUP($D288,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of N to air"},"FP120a","gPO4_eq/gN",{"$f":"VLOOKUP(\"N to air\",matrix_standardvalues_emissions,25,FALSE)","v":0.42},{"$f":"F288","v":0.42}]
[null,null,{"$f":"VLOOKUP($D289,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of NOx to air"},"FP120b","gPO4_eq/gNOx",{"$f":"VLOOKUP(\"NOx\",matrix_standardvalues_emissions,25,FALSE)","v":0.13},0.13]
[null,null,{"$f":"VLOOKUP($D290,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of NH3 to air"},"FP120c","gPO4_eq/gNH3",{"$f":"VLOOKUP(\"NH3\",matrix_standardvalues_emissions,25,FALSE)","v":0.35},0.35]
[null,null,{"$f":"VLOOKUP($D291,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N leaching from fertiliser use (including NO3- and NH4+)"},"FP123d","gN/ha",null,{"$f":"(G24+G271)*1000*0.3","v":51872.400000000009},"=(FP023a+FP108)*1000*leaching fraction N"]
[null,null,{"$f":"VLOOKUP($D292,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of N to water"},"FP120d","gPO4_eq/gN",{"$f":"VLOOKUP(\"N to water\",matrix_standardvalues_emissions,25,FALSE)","v":0.42},0.42]
[null,null,{"$f":"VLOOKUP($D293,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of NO3- to water"},"FP120e","gPO4_eq/gNO3",{"$f":"VLOOKUP(\"NO3- to water\",matrix_standardvalues_emissions,25,FALSE)","v":0.1},0.1]
[null,null,{"$f":"VLOOKUP($D294,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of NH4+ to water"},"FP120f","gPO4_eq/gNH4+",{"$f":"VLOOKUP(\"NH4+ to water\",matrix_standardvalues_emissions,25,FALSE)","v":0.33},0.33]
[null,null,{"$f":"VLOOKUP($D295,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"P leaching from fertiliser use (total P to water)"},"FP123g","gP/ha",null,{"$f":"G27*1000*0.17","v":24444.640000000003},"=FP023b*1000*leaching fraction P"]
[null,null,{"$f":"VLOOKUP($D296,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of P to water"},"FP120g","gPO4_eq/gP",{"$f":"VLOOKUP(\"P to water\",matrix_standardvalues_emissions,25,FALSE)","v":3.06},3.06]
[null,null,{"$f":"VLOOKUP($D297,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of PO43-"},"FP120h","gPO4_eq/gPO4",{"$f":"VLOOKUP(\"PO43-\",matrix_standardvalues_emissions,25,FALSE)","v":1},1]
[null,null,{"$f":"VLOOKUP($D298,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of COD"},"FP120i","gPO4_eq/gCOD",{"$f":"VLOOKUP(\"COD\",matrix_standardvalues_emissions,25,FALSE)","v":2.1999999999999999E-2},2.1999999999999999E-2]
["Eutrophication potential after allocation 1"]
[null,{"$f":"VLOOKUP($D300,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated eutrophication potential from feedstock production"},null,"FP124","gPO4_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G286*G65/100/'Conversion feedstock1'!G176)","v":2.0816438139929887},"=FP122*FP030/100/BC015c"]
["Totally allocated eutrophication potential from feedstock production"]
[null,{"$f":"VLOOKUP($D302,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from feedstock production"},null,"FP125a","gPO4_eq/MJendfuel_fs1",null,{"$f":"G300*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":1.9914646988440075},"=FP124*BC050a/100*BC050b/100"]
[null,{"$f":"VLOOKUP($D303,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from feedstock production"},null,"FP125b","gPO4_eq/MJFU",null,{"$f":"G302*'Final conversion'!G68/100*'Final conversion'!G22","v":1.9914646988440075},"=FP125a*FC025c/100*FC033"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D305,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with heat and electricity for drying and storage per kg"},null,"FP126a","gPO4-eq/kgfm",null,{"$f":"G73*G78*G289+G80*G85*G289","v":0},"=FP040*FP042d*FP120b+FP043*FP045d*FP120b"]
[null,{"$f":"VLOOKUP($D306,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with heat and electricity for drying and storage per MJ endfuel"},null,"FP126b","gPO4_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G305*G12/'Conversion feedstock1'!G176)","v":0},"=FP126a*FP003a/BC015c"]
[]
["BIODIVERSITY & HIGH CARBON STOCK",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Land with high biodiversity value"]
[null,{"$f":"VLOOKUP($D310,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in or after January 2008 = undisturbed forest (yes=1,no=0)"},null,"FP161","binary",{"$f":"VLOOKUP(D310,Parameters!$1:$1958,6,FALSE)","v":1},{"$f":"F310","v":1}]
[null,{"$f":"VLOOKUP($D311,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in or after January 2008 = nature protection area"},null,"FP162","binary",{"$f":"VLOOKUP(D311,Parameters!$1:$1958,6,FALSE)","v":1},{"$f":"F311","v":1}]
[null,{"$f":"VLOOKUP($D312,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in or after January 2008 = highly biodiverse grassland"},null,"FP163","binary",{"$f":"VLOOKUP(D312,Parameters!$1:$1958,6,FALSE)","v":0},0]
["Land with high carbon stock"]
[null,{"$f":"VLOOKUP($D314,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in January 2008 and not longer now = wetland"},null,"FP164","binary",{"$f":"VLOOKUP(D314,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F314","v":0}]
[null,{"$f":"VLOOKUP($D315,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in January 2008 and not longer now = continuously forested area"},null,"FP165","binary",{"$f":"VLOOKUP(D315,Parameters!$1:$1958,6,FALSE)","v":1},{"$f":"F315","v":1}]
[null,{"$f":"VLOOKUP($D316,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in January 2008 and not longer now = peatland"},null,"FP166","binary",{"$f":"VLOOKUP(D316,Parameters!$1:$1958,6,FALSE)","v":0},0]
["Criterium RED"]
[null,{"$f":"VLOOKUP($D318,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"The requirements of the RED concerning biodiversity & high carbon stocks are met"},null,"FP167","binary",null,{"$f":"IF(G310=\"1\",0,IF(G311=\"1\",0,IF(G312=\"1\",0,IF(G314=\"1\",0,IF(G315=\"1\",0,IF(G316=\"1\",0,1))))))","v":1},"= 0 if one of the above is equal to 1"]
[]
["LOCAL WELL-BEING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Human and property rights"]
[null,{"$f":"VLOOKUP($D322,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour"},null,"FP170a","-",{"$f":"VLOOKUP(D322,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F322=\"n.a.\",0,IF(F322=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D323,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour "},null,"FP170b","-",{"$f":"VLOOKUP(D323,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F323=\"n.a.\",0,IF(F323=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D324,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights"},null,"FP170c","-",{"$f":"VLOOKUP(D324,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D325,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination"},null,"FP170d","-",{"$f":"VLOOKUP(D325,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D326,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured"},null,"FP170e","-",{"$f":"VLOOKUP(D326,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D327,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders"},null,"FP170f","-",{"$f":"VLOOKUP(D327,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D328,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security"},null,"FP170g","-",{"$f":"VLOOKUP(D328,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
["Labour rights and conditions"]
[null,{"$f":"VLOOKUP($D330,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts"},null,"FP171a","-",{"$f":"VLOOKUP(D330,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F330=\"n.a.\",0,IF(F330=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D331,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights"},null,"FP171b","-",{"$f":"VLOOKUP(D331,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F331=\"n.a.\",0,IF(F331=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D332,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves"},null,"FP171c","-",{"$f":"VLOOKUP(D332,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D333,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules"},null,"FP171d","-",{"$f":"VLOOKUP(D333,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D334,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy"},null,"FP171e","-",{"$f":"VLOOKUP(D334,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D335,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions"},null,"FP171f","-",{"$f":"VLOOKUP(D335,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D336,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training"},null,"FP171g","-",{"$f":"VLOOKUP(D336,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
["Scores"]
[null,{"$f":"VLOOKUP($D338,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights_score"},null,"FP172","-",null,{"$f":"SUM(G322:G328)","v":7},"= FP170a + FP170b + FP170c + FP170d + FP170e + FP170f + FP170g"]
[null,{"$f":"VLOOKUP($D339,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions_score"},null,"FP173","-",null,{"$f":"SUM(G330:G336)","v":7},"= FP171a + FP171b + FP171c + FP171d + FP171e + FP171f + FP171g"]

{"sheet":"Production feedstock2","index":19,"n_rows":339,"n_cols":8,"rows_kept":339,"cut":false,"hidden":true,"merged":[]}
["Monitoring framework - Production feedstock 2 (per year)"]
[]
[null,null,"From input"]
[null,null,"Standard value"]
[null,null,"Calculated from other fields"]
[null,null,"Determines value in other field"]
[]
["MASS BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Feedstock characteristics"]
[null,{"$f":"VLOOKUP($D10,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Feedstock type 2"},null,"FP501","-",{"$f":"VLOOKUP(D10,Parameters!$1:$1958,6,FALSE)","v":"No crop"},{"$f":"F10","v":"No crop"}]
[null,{"$f":"VLOOKUP($D11,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Origin of the feedstock"},null,"FP502","-",{"$f":"VLOOKUP(D11,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F11","v":"n.a."}]
[null,{"$f":"VLOOKUP($D12,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 2 per ha"},null,"FP503a","kg/ha",{"$f":"VLOOKUP(D12,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F12","v":0}]
[null,{"$f":"VLOOKUP($D13,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (dry) of feedstock 2 per ha"},null,"FP503b","kgdm/ha",null,{"$f":"G12*(100-G18)/100","v":0},"=FP503a*(100-FP509)/100"]
[null,{"$f":"VLOOKUP($D14,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of feedstock 2 per ha"},null,"FP503c","MJ/ha",null,{"$f":"G13*G17","v":0},"=FP503b*FP510"]
[null,{"$f":"VLOOKUP($D15,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Number of harvests per year"},null,"FP505","1/yr",{"$f":"VLOOKUP(D15,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F15","v":0}]
[null,{"$f":"VLOOKUP($D16,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Rotation system"},null,"FP506","-"]
[null,{"$f":"VLOOKUP($D17,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of the dry energy crop (LHV)"},null,"FP510","MJ/kgdm",{"$f":"IF(G10=\"No crop\",VLOOKUP(G87,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE),VLOOKUP(G10,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F17","v":0}]
[null,{"$f":"VLOOKUP($D18,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of the harvested crop"},null,"FP509","%",{"$f":"VLOOKUP(D18,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F18","v":0}]
["Seeds"]
[null,{"$f":"VLOOKUP($D20,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of seeds"},null,"FP522","kg/ha",{"$f":"VLOOKUP(D20,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F20","v":0}]
[null,null,{"$f":"VLOOKUP($D21,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of seeds"},"FP550f","MJ/kg",{"$f":"VLOOKUP($F$10,matrix_standardvalues_seeds,10,FALSE)","v":0},{"$f":"F21","v":0}]
[null,null,{"$f":"VLOOKUP($D22,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Seeds: specific GHG emissions"},"FP567f","gCO2_eq/kgseeds",{"$f":"VLOOKUP($F$10,matrix_standardvalues_seeds,10,FALSE)","v":0},{"$f":"F22","v":0}]
["Fertilizers"]
[null,{"$f":"VLOOKUP($D24,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of N-fertiliser (synthetic)"},null,"FP523a","kg/ha",{"$f":"VLOOKUP(D24,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F24","v":0}]
[null,null,{"$f":"VLOOKUP($D25,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of N fertiliser"},"FP550a","MJ/kg",{"$f":"VLOOKUP(\"N\",matrix_standardvalues_agroinputs,10,FALSE)","v":48.990600000000001},{"$f":"F25","v":48.990600000000001}]
[null,null,{"$f":"VLOOKUP($D26,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N: specific GHG emissions"},"FP567a","gCO2_eq/kgfertiliser",{"$f":"VLOOKUP(\"N\",matrix_standardvalues_agroinputs,5,FALSE)","v":5880.5900999999994},5880.5900999999994]
[null,{"$f":"VLOOKUP($D27,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of P2O5-fertiliser"},null,"FP523b","kg/ha",{"$f":"VLOOKUP(D27,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D28,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of P fertiliser"},"FP550b","MJ/kg",{"$f":"VLOOKUP(\"P2O5\",matrix_standardvalues_agroinputs,10,FALSE)","v":15.2334},15.2334]
[null,null,{"$f":"VLOOKUP($D29,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"P2O5: specific GHG emissions"},"FP567b","gCO2_eq/kgfertiliser",{"$f":"VLOOKUP(\"P2O5\",matrix_standardvalues_agroinputs,5,FALSE)","v":1010.7434999999999},1010.7434999999999]
[null,{"$f":"VLOOKUP($D30,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of K2O-fertiliser"},null,"FP523c","kg/ha",{"$f":"VLOOKUP(D30,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D31,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of K fertiliser"},"FP550c","MJ/kg",{"$f":"VLOOKUP(\"K2O\",matrix_standardvalues_agroinputs,10,FALSE)","v":9.67896},9.67896]
[null,null,{"$f":"VLOOKUP($D32,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"K2O: specific GHG emissions"},"FP567c","gCO2_eq/kgfertiliser",{"$f":"VLOOKUP(\"K2O\",matrix_standardvalues_agroinputs,5,FALSE)","v":576.08240000000001},576.08240000000001]
[null,{"$f":"VLOOKUP($D33,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of CaO-fertiliser"},null,"FP523d","kg/ha",{"$f":"VLOOKUP(D33,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D34,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of Ca fertiliser"},"FP550d","MJ/kg",{"$f":"VLOOKUP(\"CaO\",matrix_standardvalues_agroinputs,10,FALSE)","v":1.9735200000000002},1.9735200000000002]
[null,null,{"$f":"VLOOKUP($D35,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"CaO: specific GHG emissions"},"FP567d","gCO2_eq/kgfertiliser",{"$f":"VLOOKUP(\"CaO\",matrix_standardvalues_agroinputs,5,FALSE)","v":129.49850000000001},129.49850000000001]
["Pesticides"]
[null,{"$f":"VLOOKUP($D37,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Use of pesticides"},null,"FP523e","kg/ha",{"$f":"VLOOKUP(D37,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F37","v":0}]
[null,null,{"$f":"VLOOKUP($D38,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of pesticides"},"FP550e","MJ/kg",{"$f":"VLOOKUP(\"Pesticides\",matrix_standardvalues_agroinputs,10,FALSE)","v":268.39980000000003},{"$f":"F38","v":268.39980000000003}]
[null,null,{"$f":"VLOOKUP($D39,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Pesticides: specific GHG emissions"},"FP567e","gCO2_eq/kgpesticides",{"$f":"VLOOKUP(\"Pesticides\",matrix_standardvalues_agroinputs,5,FALSE)","v":10971.3197},{"$f":"F39","v":10971.3197}]
["Agrifuel"]
[null,{"$f":"VLOOKUP($D41,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for agricultural machinery"},null,"FP534","-",{"$f":"VLOOKUP(D41,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F41","v":"n.a."}]
[null,{"$f":"VLOOKUP($D42,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used in agricultural machinery"},null,"FP537","kg/ha",{"$f":"VLOOKUP(D42,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D43,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of fuel used in agricultural machinery"},"FP536","MJ/kgfuel",{"$f":"IF(G41=\"n.a.\",0,VLOOKUP(G41,matrix_standardvalues_fuelsall,10,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D44,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions of the fuel used in agricultural machinery"},"FP559","gCO2_eq/kgfuel",{"$f":"IF(G41=\"n.a.\",0,VLOOKUP(G41,matrix_standardvalues_fuelsall,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D45,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Agrifuel NOx emissions factor"},"FP611a","gNOX/kgfuel",{"$f":"IF(G41=\"n.a.\",0,VLOOKUP(G41,matrix_standardvalues_fuelsall,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D46,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Agrifuel SOx emissions factor"},"FP611b","gSOX/kgfuel",{"$f":"IF(G41=\"n.a.\",0,VLOOKUP(G41,matrix_standardvalues_fuelsall,28,FALSE))","v":0},0]
["By-products"]
[null,"By-product 1"]
[null,{"$f":"VLOOKUP($D49,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 1"},null,"FP516a","-",{"$f":"VLOOKUP(D49,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F49","v":"n.a."}]
[null,{"$f":"VLOOKUP($D50,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of by-product 1 per ha"},null,"FP517a","kg/ha",{"$f":"VLOOKUP(D50,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"IF(F50=\"n.a.\",0,F50)","v":0}]
[null,{"$f":"VLOOKUP($D51,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of by-product 1 per ha"},null,"FP518a","MJ/ha",null,{"$f":"G50*G52*(100-G53)/100","v":0},"=FP517a*FP520a*(100-FP519a)/100"]
[null,{"$f":"VLOOKUP($D52,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of the dry by-product 1 (LHV)"},null,"FP520a","MJ/kgdm",{"$f":"IF(G49=\"n.a.\",0,VLOOKUP(G49, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F52","v":0}]
[null,{"$f":"VLOOKUP($D53,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 1"},null,"FP519a","%",{"$f":"IF(G49=\"n.a.\",0,VLOOKUP(G49, matrix_standardvalues_fuelsfeedstockcoproductssolids,13,FALSE))","v":0},{"$f":"F53","v":0}]
[null,{"$f":"VLOOKUP($D54,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 1"},null,"FP521a","binary",{"$f":"IF(G49=\"n.a.\",0,VLOOKUP(G49, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"F54","v":0}]
[null,{"$f":"VLOOKUP($D55,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 1"},null,"FP531a","%",null,{"$f":"IF(G54=1,G51/(G51+G59+G14)*100,0)","v":0},"=FP518a/(FP518a+FP518b+FP503c)*100"]
[null,"By-product 2"]
[null,{"$f":"VLOOKUP($D57,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 2"},null,"FP516b","-",{"$f":"VLOOKUP(D57,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F57","v":"n.a."}]
[null,{"$f":"VLOOKUP($D58,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of by-product 2 per ha"},null,"FP517b","kg/ha",{"$f":"VLOOKUP(D58,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"IF(F58=\"n.a.\",0,F58)","v":0}]
[null,{"$f":"VLOOKUP($D59,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of by-product 2 per ha"},null,"FP518b","MJ/ha",null,{"$f":"G58*G60*(100-G61)/100","v":0},"=FP517b*FP520b*(100-FP519b)/100"]
[null,{"$f":"VLOOKUP($D60,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of the dry by-product 2 (LHV)"},null,"FP520b","MJ/kgdm",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F60","v":0}]
[null,{"$f":"VLOOKUP($D61,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 2"},null,"FP519b","%",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsfeedstockcoproductssolids,13,FALSE))","v":0},{"$f":"F61","v":0}]
[null,{"$f":"VLOOKUP($D62,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 2"},null,"FP521b","binary",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"F62","v":0}]
[null,{"$f":"VLOOKUP($D63,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 2"},null,"FP531b","%",null,{"$f":"IF(G62=1,G59/(G51+G59+G14)*100,0)","v":0},"=FP518b/(FP518a+FP518b+FP503c)*100"]
["Allocation"]
[null,{"$f":"VLOOKUP($D65,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to energy crop"},null,"FP530","%",null,{"$f":"100-G66","v":100},"=100-FP531"]
[null,{"$f":"VLOOKUP($D66,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-products"},null,"FP531","%",null,{"$f":"G55+G63","v":0},"=FP531a+FP531b"]
["Transport losses"]
[null,{"$f":"VLOOKUP($D68,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield loss through treatment and transport of feedstock 2"},null,"FP554","%",{"$f":"VLOOKUP(D68,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F68","v":0}]
[null,{"$f":"VLOOKUP($D69,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of pretreated feedstock 2 before conversion"},null,"FP555a","kg/ha",null,{"$f":"G12*(100-G68)/100","v":0},"=FP503a*(100-FP554)/100"]
[null,{"$f":"VLOOKUP($D70,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (dry) of pretreated feedstock 2 before conversion"},null,"FP555b","kgdm/ha",null,{"$f":"G13*(100-G68)/100","v":0},"=FP503b*(100-FP554)/100"]
[null,{"$f":"VLOOKUP($D71,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of pretreated feedstock 2 before conversion"},null,"FP555c","MJ/ha",null,{"$f":"G14*(100-G68)/100","v":0},"=FP503c*(100-FP554)/100"]
["Drying & storage (part of 'treatment & transport 1')"]
[null,{"$f":"VLOOKUP($D73,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat energy use for drying and storage of the crop"},null,"FP540","MJheat/kgfm",{"$f":"VLOOKUP(D73,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F73","v":0}]
[null,{"$f":"VLOOKUP($D74,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat source"},null,"FP541","-",{"$f":"VLOOKUP(D74,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F74","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D75,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of heat production for crop drying and storage"},"FP542a","MJ/MJheat",{"$f":"IF(F74=\"n.a.\",0,VLOOKUP(F74, matrix_standardvalues_heat,11,FALSE))","v":0},{"$f":"F75","v":0}]
[null,null,{"$f":"VLOOKUP($D76,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy coefficient of heat production for crop drying and storage"},"FP542b","MJ/MJheat",{"$f":"IF(F74=\"n.a.\",0,VLOOKUP(F74, matrix_standardvalues_heat,21,FALSE))","v":0},{"$f":"F76","v":0}]
[null,null,{"$f":"VLOOKUP($D77,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG coefficient of heat production for crop drying and storage"},"FP542c","gCO2_eq/MJheat",{"$f":"IF(F74=\"n.a.\",0,VLOOKUP(F74, matrix_standardvalues_heat,5,FALSE))","v":0},{"$f":"F77","v":0}]
[null,null,{"$f":"VLOOKUP($D78,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of heat production for crop drying and storage"},"FP542d","gNOX/MJheat",{"$f":"IF(F74=\"n.a.\",0,VLOOKUP(F74, matrix_standardvalues_heat,27,FALSE))","v":0},{"$f":"F78","v":0}]
[null,null,{"$f":"VLOOKUP($D79,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of heat production for crop drying and storage"},"FP542e","gSOX/MJheat",{"$f":"IF(F74=\"n.a.\",0,VLOOKUP(F74, matrix_standardvalues_heat,29,FALSE))","v":0},0]
[null,{"$f":"VLOOKUP($D80,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity energy use for drying and storage of the crop"},null,"FP543","MJe/kgfm",{"$f":"VLOOKUP(D80,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,{"$f":"VLOOKUP($D81,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity source"},null,"FP544","-",{"$f":"VLOOKUP(D81,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D82,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy coefficient of electricity for crop drying and storage"},"FP545a","MJ/MJe",{"$f":"IF(F81=\"n.a.\",0,VLOOKUP(F81, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D83,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy coefficient of electricity for crop drying and storage"},"FP545b","MJ/MJe",{"$f":"IF(F81=\"n.a.\",0,VLOOKUP(F81, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D84,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG coefficient of electricity for crop drying and storage"},"FP545c","gCO2_eq/MJe",{"$f":"IF(F81=\"n.a.\",0,VLOOKUP(F81, matrix_standardvalues_electricity,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D85,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity for crop drying and storage"},"FP545d","gNOX/MJe",{"$f":"IF(F81=\"n.a.\",0,VLOOKUP(F81, matrix_standardvalues_electricity,27,FALSE))","v":0},{"$f":"F85","v":0}]
[null,null,{"$f":"VLOOKUP($D86,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity for crop drying and storage"},"FP545e","gSOX/MJe",{"$f":"IF(F81=\"n.a.\",0,VLOOKUP(F81, matrix_standardvalues_electricity,29,FALSE))","v":0},{"$f":"F86","v":0}]
[null,{"$f":"VLOOKUP($D87,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Pretreated feedstock"},null,"FP547","-",{"$f":"VLOOKUP(D87,Parameters!$1:$1958,6,FALSE)","v":"No crop"},{"$f":"F87","v":"No crop"}]
[]
["ENERGY BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Feedstock production"]
[null,{"$f":"VLOOKUP($D91,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy used for feedstock production"},null,"FP528a","MJ/kgdm",null,{"$f":"IF(G13=0,0,(G95+G97)/G13)","v":0},"=(FP535a+FP546a)/FP503b"]
[null,null,null,"FP528b","MJ/ha",null,{"$f":"G95+G97","v":0},"=FP535a+FP546a"]
[null,{"$f":"VLOOKUP($D93,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy used for feedstock production"},null,"FP529a","MJ/kgdm",null,{"$f":"IF(G13=0,0,(G96+G98)/G13)","v":0},"=(FP535b+FP546b)/FP503b"]
[null,null,null,"FP529b","MJ/ha",null,{"$f":"G96+G98","v":0},"=FP535b+FP546b"]
[null,{"$f":"VLOOKUP($D95,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to agrifuel use"},null,"FP535a","MJ/ha",null,{"$f":"IF(G12>0,G43*G42,0)","v":0},"=FP536*FP537"]
[null,{"$f":"VLOOKUP($D96,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to agrifuel use"},null,"FP535b","MJ/ha",null,{"$f":"IF(G12>0,G43*G42,0)","v":0},"=FP536*FP537"]
[null,{"$f":"VLOOKUP($D97,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use of seeds, fertilisers and pesticides"},null,"FP546a","MJ/ha",null,{"$f":"IF(G12>0,G20*G21+G24*G25+G27*G28+G30*G31+G33*G34+G37*G38,0)","v":0},"=FP522*FP550f+FP523a*FP550a+FP523b*FP550b+FP523c*FP550c+FP523d*FP550d+FP523e*FP550e"]
[null,{"$f":"VLOOKUP($D98,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use of seeds, fertilisers and pesticides"},null,"FP546b","MJ/ha",null,{"$f":"IF(G12>0,G20*G21+G24*G25+G27*G28+G30*G31+G33*G34+G37*G38,0)","v":0},"=FP522*FP550f+FP523a*FP550a+FP523b*FP550b+FP523c*FP550c+FP523d*FP550d+FP523e*FP550e"]
["Energy use after allocation 1"]
[null,{"$f":"VLOOKUP($D100,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated fossil energy requirement for feedstock production"},null,"FP532a","MJfossil/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G92*G65/100/'Conversion feedstock2'!G176)","v":0},"=FP528b*FP530/100/BC515c"]
[null,{"$f":"VLOOKUP($D101,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated primary energy requirement for feedstock production"},null,"FP532b","MJprim/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G94*G65/100/'Conversion feedstock2'!G176)","v":0},"=FP529b*FP530/100/BC515c"]
["Totally allocated energy use for feedstock production"]
[null,{"$f":"VLOOKUP($D103,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for feedstock production"},null,"FP524a","MJfossil/MJendfuel_fs2",null,{"$f":"G100*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FP532a*BC550a/100*BC550b/100"]
[null,{"$f":"VLOOKUP($D104,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for feedstock production"},null,"FP524b","MJprim/MJendfuel_fs2",null,{"$f":"G101*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FP532b*BC550a/100*BC550b/100"]
[null,{"$f":"VLOOKUP($D105,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for feedstock production"},null,"FP525a","MJfossil/MJFU",null,{"$f":"G100*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FP532a*BC550a/100*BC550b/100*FC025c/100*FC034"]
[null,{"$f":"VLOOKUP($D106,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for feedstock production"},null,"FP525b","MJprim/MJFU",null,{"$f":"G101*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FP532b*BC550a/100*BC550b/100*FC025c/100*FC034"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D108,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy used for heat and electricity for drying and storage per kg"},null,"FP538a","MJfossil/kgfm",null,{"$f":"G73*G75+G80*G82","v":0},"=FP540*FP542a+FP543*FP545a"]
[null,{"$f":"VLOOKUP($D109,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy used for heat and electricity for drying and storage per kg"},null,"FP538b","MJprim/kgfm",null,{"$f":"G73*G76+G80*G83","v":0},"=FP540*FP542b+FP543*FP545b"]
[null,{"$f":"VLOOKUP($D110,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy used for heat and electricity for drying and storage per MJ endfuel"},null,"FP539a","MJfossil/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G108*G12/'Conversion feedstock2'!G176)","v":0},"=FP538a*FP503a/BC515c"]
[null,{"$f":"VLOOKUP($D111,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy used for heat and electricity for drying and storage per MJ endfuel"},null,"FP539b","MJprim/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G109*G12/'Conversion feedstock2'!G176)","v":0},"=FP538b*FP503a/BC515c"]
[]
["GLOBAL WARMING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Field characteristics"]
[null,null,{"$f":"VLOOKUP($D115,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Actual land use"},"FP569a","-",{"$f":"VLOOKUP(D115,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F115","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D116,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previous land use (January 1st, 2008)"},"FP569b","-",{"$f":"VLOOKUP(D116,Parameters!$1:$1958,6,FALSE)","v":"Annual cropland"},"Annual cropland"]
[null,null,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previously degraded land"},"FP592a","-",{"$f":"VLOOKUP(D117,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D118,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Climate region"},"FP570a","-",{"$f":"VLOOKUP(D118,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D119,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Soil type"},"FP570b","-",{"$f":"VLOOKUP(D119,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D120,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Soil water saturation (yes=1,no=0)"},"FP631","binary",{"$f":"VLOOKUP(D120,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D121,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Field renewal (annual crops = 1)"},"FP632","years",{"$f":"VLOOKUP(D121,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D122,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of crop residue returned to the field (only for palm)"},"FP633","kgdm/kgfm",{"$f":"VLOOKUP(D122,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D123,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Organic soil (yes=1,no=0)"},"FP634","binary",{"$f":"VLOOKUP(D123,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D124,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Nutrient level (only for ORGANIC soils + temperate/boreal climate + forest (native and managed))"},"FP635","-",{"$f":"VLOOKUP(D124,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D125,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previous land use is cropland (yes=1,no=0)"},"FP653","binary",null,{"$f":"IF(G116=\"Grassland and savannah\",0,IF(G116=\"Native forest non degraded\",0,IF(G116=\"Managed forest\",0,1)))","v":1}]
["GHG emissions from inputs for feedstock production"]
[null,{"$f":"VLOOKUP($D128,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with inputs for feedstock production"},null,"FP556a","gCO2-eq/kgdm",null,{"$f":"IF(G12>0,(G129+G130)/G13,0)","v":0},"=(FP558+FP564)/FP503b"]
[null,null,null,"FP556b","gCO2-eq/ha",null,{"$f":"IF(G12>0,G129+G130,0)","v":0},"=FP558+FP564"]
[null,null,{"$f":"VLOOKUP($D129,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with fuel used in agricultural machinery"},"FP558","gCO2-eq/ha",null,{"$f":"G42*G44","v":0},"=FP537*FP559"]
[null,null,{"$f":"VLOOKUP($D130,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with production of seeds, fertilisers and pesticides"},"FP564","gCO2-eq/ha",null,{"$f":"G20*G22+G24*G26+G27*G29+G30*G32+G33*G35+G37*G39","v":0},"=FP522*FP567f+FP523a*FP567a+FP523b*FP567b+FP523c*FP567c+FP523d*FP567d+FP523e*FP567e"]
["Field N2O emissions"]
[null,{"$f":"VLOOKUP($D132,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total (direct + indirect) N2O emissions from managed soils"},null,"FP630a","gN20/ha",null,{"$f":"IF(G10=\"No crop\",0,(G140+G164)*1000)","v":0},"=(FP638b+FP655b)*1000"]
[null,{"$f":"VLOOKUP($D133,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total (direct + indirect) N2O emissions from managed soils"},null,"FP630b","gCO2-eq/ha",null,{"$f":"G132*'Standard Values'!D6","v":0},"=FP630a*GWP_N20"]
[null,null,{"$f":"VLOOKUP($D134,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for direct N2O emissions from N inputs"},"FP637a","kgN20_N/kgN_input",{"$f":"VLOOKUP(\"EF1\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.01},{"$f":"F134","v":0.01}]
[null,null,{"$f":"VLOOKUP($D135,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for direct N2O emissions from drained/managed organic soils"},"FP637b","kgN20_N/ha",{"$f":"VLOOKUP(\"EF2 \"&G118&\" \"&G115&\" \"&G124,Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,IF(F135=\"n.a.\",0,F135))","v":0}]
[null,null,{"$f":"VLOOKUP($D136,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for direct N2O emissions from urine and dung N deposited by grazing animals"},"FP637c","kgN20_N/kgN_input"]
[null,null,{"$f":"VLOOKUP($D137,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for indirect N2O emissions from atmospheric deposition of N"},"FP637d","kgN20_N/kgN_volatilised",{"$f":"VLOOKUP(\"EF4\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.01},{"$f":"F137","v":0.01}]
[null,null,{"$f":"VLOOKUP($D138,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor for indirect N2O emissions from leaching and runoff"},"FP637e","kgN20_N/kgN_leached+runoff",{"$f":"VLOOKUP(\"EF5\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":7.4999999999999997E-3},{"$f":"F138","v":7.4999999999999997E-3}]
[null,{"$f":"VLOOKUP($D139,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Direct N2O_N emissions from managed soils"},null,"FP638a","kgN20_N/ha",null,{"$f":"G141+G162","v":0},"=FP639+FP654"]
[null,{"$f":"VLOOKUP($D140,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Direct N2O emissions from managed soils"},null,"FP638b","kgN20/ha",null,{"$f":"G139*44/28","v":0},"=FP638a*44/28"]
[null,{"$f":"VLOOKUP($D141,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Direct N2O_N emissions from N inputs to managed mineral soils"},null,"FP639","kgN20_N/ha",null,{"$f":"(G24+G142+G147+G159)*G134","v":0},"=(FP523a+FP640+FP642+FP650)*FP637a"]
[null,{"$f":"VLOOKUP($D142,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total amount of organic N fertiliser applied to soil (other than by grazing animals)"},null,"FP640","kgN/ha",null,{"$f":"IF(G123=1,0,G143+G144+G145+G146)","v":0},"=FP641a+FP641b+FP641c+FP641d"]
[null,null,{"$f":"VLOOKUP($D143,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of animal manure N applied to soil (other than by grazing animals)"},"FP641a","kgN/ha",{"$f":"VLOOKUP(D143,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F143","v":0}]
[null,null,{"$f":"VLOOKUP($D144,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of total sewage N applied to soil"},"FP641b","kgN/ha",{"$f":"VLOOKUP(D144,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F144","v":0}]
[null,null,{"$f":"VLOOKUP($D145,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of total compost N applied to soil"},"FP641c","kgN/ha",{"$f":"VLOOKUP(D145,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F145","v":0}]
[null,null,{"$f":"VLOOKUP($D146,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of N of other organic amendments applied to soil (used as fertiliser)"},"FP641d","kgN/ha",{"$f":"VLOOKUP(D146,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F146","v":0}]
[null,{"$f":"VLOOKUP($D147,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total amount of N in crop residues (including N-fixing crops and renewal) returned to soil"},null,"FP642","kgN/ha",null,{"$f":"IF(G10=\"No crop\",0,IF(G123=1,0,G13/G121*(G149*G156*(1-G158)+G154*G157)))","v":0},"=FP503b/FP632*(FP643b*FP648a*(1-FP649)+FP646b*FP648b)"]
[null,null,{"$f":"VLOOKUP($D148,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of above-ground residues to harvested yield_calculated"},"FP643a","kgdm/kgdm",null,{"$f":"IF(G13=0,0,G150*1000/G13)","v":0},"=FP644*1000/FP503b"]
[null,null,{"$f":"VLOOKUP($D149,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of above-ground residues to harvested yield_final"},"FP643b","kgdm/kgdm",{"$f":"VLOOKUP(D149,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F149","v":0}]
[null,null,{"$f":"VLOOKUP($D150,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above-ground residue (dry) (=AGDM(T))"},"FP644","t/ha",null,{"$f":"IF(G10=\"Fresh palm fruit bunches (FFB)\",G12*G122/1000,G13*G151/1000+G152)","v":0},"FFB: =FP503a*FP633/1000 ; Other: =FP503b*FP645a/1000+FP645b"]
[null,null,{"$f":"VLOOKUP($D151,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Slope to calculate above-ground residue"},"FP645a","-",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],2,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F151)","v":0}]
[null,null,{"$f":"VLOOKUP($D152,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Intercept to calculate above-ground residue"},"FP645b","-",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F152)","v":0}]
[null,null,{"$f":"VLOOKUP($D153,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below-ground residues to harvested yield_calculated"},"FP646a","kgdm/kgdm",null,{"$f":"IF(G13=0,0,G155*(G150*1000+G13)/G13)","v":0},"=FP647*(FP644*1000+FP503b)/FP503b"]
[null,null,{"$f":"VLOOKUP($D154,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below-ground residues to harvested yield_final"},"FP646b","kgdm/kgdm",{"$f":"VLOOKUP(D154,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F154","v":0}]
[null,null,{"$f":"VLOOKUP($D155,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below-ground residues to above-ground biomass"},"FP647","kgdm/kgdm",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],9,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F155)","v":0}]
[null,null,{"$f":"VLOOKUP($D156,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N content of above-ground residues"},"FP648a","kgN/kgdm",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],7,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F156)","v":0}]
[null,null,{"$f":"VLOOKUP($D157,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N content of below-ground residues"},"FP648b","kgN/kgdm",{"$f":"VLOOKUP(G10,Table_IPCC_N2O[],8,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F157)","v":0}]
[null,null,{"$f":"VLOOKUP($D158,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fraction of above-ground residues removed"},"FP649","%",{"$f":"VLOOKUP(D158,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F158","v":0}]
[null,{"$f":"VLOOKUP($D159,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total amount of N mineralised in mineral soil due to carbon loss through land use change"},null,"FP650","kgN/ha",null,{"$f":"IF(G123=1,0,G160/G161*1000)","v":0},"=FP651/FP652*1000"]
[null,null,{"$f":"VLOOKUP($D160,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Average annual loss of soil carbon"},"FP651","tC/ha",null,{"$f":"(G202-G174)/20","v":0},"=(FP572-FP571)/20"]
[null,null,{"$f":"VLOOKUP($D161,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"C:N ratio of the soil organic matter"},"FP652","-",null,{"$f":"IF(G125=1,10,15)","v":10}]
[null,{"$f":"VLOOKUP($D162,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Direct N2O_N emissions from managed organic soils"},null,"FP654","kgN20_N/ha",null,{"$f":"IF(G123=1,G135,0)","v":0}]
[null,{"$f":"VLOOKUP($D163,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Indirect N2O_N emissions from managed soils"},null,"FP655a","kgN20_N/ha",null,{"$f":"G165+G168","v":0},"=FP656+FP659"]
[null,{"$f":"VLOOKUP($D164,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Indirect N2O emissions from managed soils"},null,"FP655b","kgN20/ha",null,{"$f":"G163*44/28","v":0},"=FP655a*44/28"]
[null,{"$f":"VLOOKUP($D165,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Indirect N2O_N emissions from atmospheric deposition of N volatilized from managed soils"},null,"FP656","kgN20_N/ha",null,{"$f":"(G24*G166+G142*G167)*G137","v":0},"=(FP523a*FP657+FP640*FP658)*FP637d"]
[null,null,{"$f":"VLOOKUP($D166,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fraction of synthetic fertiliser N that volatilises as NH3 and NOx"},"FP657","kgN_volatilised/kgN_applied",{"$f":"VLOOKUP(\"FRACgasf\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.1},{"$f":"F166","v":0.1}]
[null,null,{"$f":"VLOOKUP($D167,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fraction of organic fertiliser N that volatilises as NH3 and NOx"},"FP658","kgN_volatilised/kgN_applied",{"$f":"VLOOKUP(\"FRACgasm\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.2},{"$f":"F167","v":0.2}]
[null,{"$f":"VLOOKUP($D168,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Indirect N2O_N emissions from N leaching/runoff from managed soils"},null,"FP659","kgN20_N/ha",null,{"$f":"(G24+G142+G147+G159)*G169*G138","v":0},"=(FP523a+FP640+FP642+FP650)*FP660*FP637e"]
[null,null,{"$f":"VLOOKUP($D169,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fraction of all N added to managed soils that is lost through leaching and runoff"},"FP660","kgN_leached/kgN_applied",{"$f":"VLOOKUP(\"FRACleach\",Table_IPCC_emissionfactorsN2O[],5,FALSE)","v":0.3},{"$f":"F169","v":0.3}]
["Carbon stock changes from land use change"]
[null,{"$f":"VLOOKUP($D171,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with land use change (carbon stock changes) per MJ"},null,"FP568a","gCO2-eq/MJendfuel_fs2 (over 20yr)",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G172/'Conversion feedstock2'!G176)","v":0},"=FP568b/BC515c"]
[null,null,null,"FP568b","gCO2-eq/ha (over 20yr)",null,{"$f":"IF(G10=\"No crop\",0,((G202-G174)/20+G123*G230)*1000000*3.664-G231*G117*'Conversion feedstock2'!G176)","v":0},"=((FP572-FP571)/20+FP591a*FP591b)*1000000*3.664-FP592a*FP592b*BC515c"]
[null,null,{"$f":"VLOOKUP($D173,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Standard soil organic carbon_feedstock 2"},"FP574","tC/ha",{"$f":"VLOOKUP(G118&\" \"&G119,Table_IPCC_SOC[],4,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F173)","v":0}]
[null,{"$f":"VLOOKUP($D174,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock actual land use"},null,"FP571","tC/ha",null,{"$f":"G183+G187","v":0},"=FP573a+FP578a"]
[null,null,{"$f":"VLOOKUP($D175,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Actual land use_specific for carbon stock veg"},"FP569c","-",{"$f":"VLOOKUP(D175,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F175","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D176,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Climate region_specific for carbon stock_actual land use"},"FP570c","-",{"$f":"VLOOKUP(D176,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F176","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D177,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land management actual land use"},"FP593a","-",{"$f":"VLOOKUP(D177,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F177","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D178,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input actual land use"},"FP594a","-",{"$f":"VLOOKUP(D178,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D179,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Domain actual land use"},"FP595a","-",{"$f":"VLOOKUP(D179,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D180,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ecological zone actual land use"},"FP596a","-",{"$f":"VLOOKUP(D180,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D181,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Continent actual land use"},"FP597a","-",{"$f":"VLOOKUP(D181,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D182,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type actual land use"},"FP598a","-",{"$f":"VLOOKUP(D182,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,{"$f":"VLOOKUP($D183,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Soil organic carbon actual land use"},null,"FP573a","tC/ha",null,{"$f":"G173*G184*G185*G186","v":0},"=FP574*FP575a*FP576a*FP577a"]
[null,null,{"$f":"VLOOKUP($D184,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use factor actual land use"},"FP575a","-",{"$f":"VLOOKUP(G115&\" \"&G118&\" \"&G177&\" \"&G178,Table_IPCC_factors[],6,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F184)","v":0}]
[null,null,{"$f":"VLOOKUP($D185,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Management factor actual land use"},"FP576a","-",{"$f":"VLOOKUP(G115&\" \"&G118&\" \"&G177&\" \"&G178,Table_IPCC_factors[],7,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F185)","v":0}]
[null,null,{"$f":"VLOOKUP($D186,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input factor actual land use"},"FP577a","-",{"$f":"VLOOKUP(G115&\" \"&G118&\" \"&G177&\" \"&G178,Table_IPCC_factors[],8,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F186)","v":0}]
[null,{"$f":"VLOOKUP($D187,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock actual land use"},null,"FP578a","tC/ha",null,{"$f":"IF(G10=\"No crop\",0,IF(G188=0,VLOOKUP(G175&\" \"&G179&\" \"&G176&\" \"&G180&\" \"&G181&\" \"&G182,Table_IPCC_Cvegetation[],8,FALSE),G188+G197))","v":0},"=FP579a + FP586a"]
[null,null,{"$f":"VLOOKUP($D188,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock in living biomass actual land use"},"FP579a","tC/ha",null,{"$f":"G189+G195","v":0},"=FP580a + FP584a"]
[null,null,{"$f":"VLOOKUP($D189,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above ground vegetation carbon stock in living biomass actual land use"},"FP580a","tC/ha",null,{"$f":"G190*G191","v":0},"=FP581a*FP582a"]
[null,null,{"$f":"VLOOKUP($D190,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of above ground living biomass actual land use"},"FP581a","t/ha",{"$f":"VLOOKUP(D190,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F190","v":0}]
[null,null,{"$f":"VLOOKUP($D191,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in living biomass actual land use"},"FP582aa","-",{"$f":"VLOOKUP(D191,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F191","v":0}]
[null,null,{"$f":"VLOOKUP($D192,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in dead wood actual land use"},"FP582ba","-",{"$f":"VLOOKUP(D192,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D193,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in litter actual land use"},"FP582ca","-",{"$f":"VLOOKUP(D193,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D194,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below ground carbon stock to above ground carbon stock in living biomass actual land use"},"FP583a","-",{"$f":"VLOOKUP(D194,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F194","v":0}]
[null,null,{"$f":"VLOOKUP($D195,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Below ground vegetation carbon stock in living biomass actual land use"},"FP584a","tC/ha",null,{"$f":"IF(G196=0,G189*G194,G196*G191)","v":0},"=FP585a*FP582a of FP580a*FP583a"]
[null,null,{"$f":"VLOOKUP($D196,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of below ground living biomass actual land use"},"FP585a","t/ha",{"$f":"VLOOKUP(D196,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F196","v":0}]
[null,null,{"$f":"VLOOKUP($D197,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock in dead organic matter actual land use"},"FP586a","tC/ha",null,{"$f":"G198+G200","v":0},"=FP587a + FP589a"]
[null,null,{"$f":"VLOOKUP($D198,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock in dead wood pool actual land use"},"FP587a","tC/ha",null,{"$f":"G199*G192","v":0},"=FP588a*FP582b"]
[null,null,{"$f":"VLOOKUP($D199,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of dead wood pool actual land use"},"FP588a","t/ha",{"$f":"VLOOKUP(D199,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F199","v":0}]
[null,null,{"$f":"VLOOKUP($D200,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock in litter actual land use"},"FP589a","tC/ha",null,{"$f":"G201*G193","v":0},"=FP590a*FP582c"]
[null,null,{"$f":"VLOOKUP($D201,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of litter actual land use"},"FP590a","t/ha",{"$f":"VLOOKUP(D201,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F201","v":0}]
[null,{"$f":"VLOOKUP($D202,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock previous land use"},null,"FP572","tC/ha",null,{"$f":"G211+G215","v":0},"=FP573b+FP578b"]
[null,null,{"$f":"VLOOKUP($D203,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previous land use (January 1st, 2008)_specific for carbon stock veg"},"FP569d","-",{"$f":"VLOOKUP(D203,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F203","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D204,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Climate region_specific for carbon stock_previous land use"},"FP570d","-",{"$f":"VLOOKUP(D204,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F204","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D205,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land management previous land use"},"FP593b","-",{"$f":"VLOOKUP(D205,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"F205","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D206,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input previous land use"},"FP594b","-",{"$f":"VLOOKUP(D206,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D207,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Domain previous land use"},"FP595b","-",{"$f":"VLOOKUP(D207,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D208,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ecological zone previous land use"},"FP596b","-",{"$f":"VLOOKUP(D208,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D209,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Continent previous land use"},"FP597b","-",{"$f":"VLOOKUP(D209,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D210,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type previous land use"},"FP598b","-",{"$f":"VLOOKUP(D210,Parameters!$1:$1958,6,FALSE)","v":"n.a."},"n.a."]
[null,{"$f":"VLOOKUP($D211,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Soil organic carbon previous land use"},null,"FP573b","tC/ha",null,{"$f":"G173*G212*G213*G214","v":0},"=FP574*FP575b*FP576b*FP577b"]
[null,null,{"$f":"VLOOKUP($D212,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use factor previous land use"},"FP575b","-",{"$f":"VLOOKUP(G116&\" \"&G118&\" \"&G205&\" \"&G206,Table_IPCC_factors[],6,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F212)","v":0}]
[null,null,{"$f":"VLOOKUP($D213,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Management factor previous land use"},"FP576b","-",{"$f":"VLOOKUP(G116&\" \"&G118&\" \"&G205&\" \"&G206,Table_IPCC_factors[],7,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F213)","v":0}]
[null,null,{"$f":"VLOOKUP($D214,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input factor previous land use"},"FP577b","-",{"$f":"VLOOKUP(G116&\" \"&G118&\" \"&G205&\" \"&G206,Table_IPCC_factors[],8,FALSE)","v":{"$error":"#N/A"}},{"$f":"IF(G10=\"No crop\",0,F214)","v":0}]
[null,{"$f":"VLOOKUP($D215,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock previous land use"},null,"FP578b","tC/ha",null,{"$f":"IF(G10=\"No crop\",0,IF(G216=0,VLOOKUP(G203&\" \"&G207&\" \"&G204&\" \"&G208&\" \"&G209&\" \"&G210,Table_IPCC_Cvegetation[],8,FALSE),G216+G225))","v":0},"=FP579b + FP586b"]
[null,null,{"$f":"VLOOKUP($D216,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock in living biomass previous land use"},"FP579b","tC/ha",null,{"$f":"G217+G223","v":0},"=FP580b + FP584b"]
[null,null,{"$f":"VLOOKUP($D217,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above ground vegetation carbon stock in living biomass previous land use"},"FP580b","tC/ha",null,{"$f":"G218*G219","v":0},"=FP581b*FP582a"]
[null,null,{"$f":"VLOOKUP($D218,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of above ground living biomass previous land use"},"FP581b","t/ha",{"$f":"VLOOKUP(D218,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F218","v":0}]
[null,null,{"$f":"VLOOKUP($D219,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in living biomass previous land use"},"FP582ab","-",{"$f":"VLOOKUP(D219,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F219","v":0}]
[null,null,{"$f":"VLOOKUP($D220,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in dead wood previous land use"},"FP582bb","-",{"$f":"VLOOKUP(D220,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D221,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon fraction of dry matter in litter previous land use"},"FP582cb","-",{"$f":"VLOOKUP(D221,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D222,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Ratio of below ground carbon stock to above ground carbon stock in living biomass previous land use"},"FP583b","-",{"$f":"VLOOKUP(D222,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F222","v":0}]
[null,null,{"$f":"VLOOKUP($D223,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Below ground vegetation carbon stock in living biomass previous land use"},"FP584b","tC/ha",null,{"$f":"IF(G224=0,G217*G222,G224*G219)","v":0},"=FP585b*FP582b of FP580b*FP583b"]
[null,null,{"$f":"VLOOKUP($D224,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of below ground living biomass previous land use"},"FP585b","t/ha",{"$f":"VLOOKUP(D224,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F224","v":0}]
[null,null,{"$f":"VLOOKUP($D225,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Above and below vegetation carbon stock in dead organic matter previous land use"},"FP586b","tC/ha",null,{"$f":"G226+G228","v":0},"=FP587b + FP589b"]
[null,null,{"$f":"VLOOKUP($D226,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock in dead wood pool previous land use"},"FP587b","tC/ha",null,{"$f":"G227*G220","v":0},"=FP588b*FP582b"]
[null,null,{"$f":"VLOOKUP($D227,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of dead wood pool previous land use"},"FP588b","t/ha",{"$f":"VLOOKUP(D227,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F227","v":0}]
[null,null,{"$f":"VLOOKUP($D228,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon stock in litter previous land use"},"FP589b","tC/ha",null,{"$f":"G229*G221","v":0},"=FP590b*FP582c"]
[null,null,{"$f":"VLOOKUP($D229,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Weight of litter previous land use"},"FP590b","t/ha",{"$f":"VLOOKUP(D229,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F229","v":0}]
[null,null,{"$f":"VLOOKUP($D230,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Emission factor soil organic carbon_peatland"},"FP591b","tC/ha",{"$f":"'Standard Values'!S155","v":20},{"$f":"F230","v":20}]
[null,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Previously degraded land"},null,"FP592b","gCO2-eq/MJ (per year)",{"$f":"'Standard Values'!I154","v":29},{"$f":"F231","v":29}]
[null,{"$f":"VLOOKUP($D232,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with indirect land use change (soil carbon release)"},null,"FP599","gCO2-eq/ha (spread over 20yr)"]
["GHG emissions after allocation 1"]
[null,{"$f":"VLOOKUP($D234,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated GHG emissions from feedstock production"},null,"FP557","gCO2_eq/MJendfuel_fs2",null,{"$f":"IF(G10=\"No crop\",0,(G128+G133+G172)*G65/100/'Conversion feedstock2'!G176)","v":0},"=(FP556b+FP630b+FP568b)*FP530/100/BC515c"]
["Totally allocated GHG emissions from feedstock production"]
[null,{"$f":"VLOOKUP($D236,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from feedstock production"},null,"FP561a","gCO2_eq/MJendfuel_fs2",null,{"$f":"G234*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FP557*BC550a/100*BC550b/100"]
[null,{"$f":"VLOOKUP($D237,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from feedstock production"},null,"FP561b","gCO2_eq/MJFU",null,{"$f":"G234*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FP557*BC550a/100*BC550b/100*FC025c/100*FC034"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D239,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with heat and electricity for drying and storage per kg"},null,"FP562a","gCO2-eq/kgfm",null,{"$f":"G73*G77+G80*G84","v":0},"=FP540*FP542c+FP543*FP545c"]
[null,{"$f":"VLOOKUP($D240,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with heat and electricity for drying and storage per MJ endfuel"},null,"FP562b","gCO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G239*G12/'Conversion feedstock2'!G176)","v":0},"=FP562a*FP503a/BC515c"]
["Carbon debt & repayment time"]
[null,{"$f":"VLOOKUP($D242,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carbon debt due to land use change"},null,"FP607a","gCO2-eq/ha",null,{"$f":"G172*20","v":0},"=FP568b*20"]
[null,{"$f":"VLOOKUP($D243,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated carbon debt"},null,"FP607b","gCO2-eq/ha",null,{"$f":"G242*G65/100","v":0},"=FP607a*FP530/100"]
[null,{"$f":"VLOOKUP($D244,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated carbon debt"},null,"FP607c","gCO2-eq/ha",null,{"$f":"G243*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100","v":0},"=FP607b*BC550a/100*BC550b/100*FC025c/100"]
[null,{"$f":"VLOOKUP($D245,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated GHG emissions from feedstock production without LUC emissions"},null,"FP608","gCO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G128+G133)*G65/100/'Conversion feedstock2'!G176)","v":0},"=(FP556b+FP630b)*FP530/100/BC515c"]
[]
["RESOURCE USE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["USE OF WATER"]
[null,{"$f":"VLOOKUP($D249,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock production"},null,"FP600","m³/ha",{"$f":"VLOOKUP(D249,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F249","v":0}]
[null,{"$f":"VLOOKUP($D250,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Country freshwater availability"},null,"FP604a","m³/capita.yr",{"$f":"IF(G11=\"n.a.\",0,VLOOKUP(G11,table_FAO_water[],2,FALSE))","v":0},{"$f":"F250","v":0}]
[null,{"$f":"VLOOKUP($D251,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Country freshwater level"},null,"FP604b","-",{"$f":"IF(G11=\"n.a.\",0,VLOOKUP(G11,table_FAO_water[],3,FALSE))","v":0},{"$f":"F251","v":0}]
["Use of water after allocation 1"]
[null,{"$f":"VLOOKUP($D253,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated water use for feedstock production"},null,"FP601","m³/GJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G249*G65/100/'Conversion feedstock2'!G176*1000)","v":0},"=FP600*FP530/100/BC515c*1000"]
["Totally allocated water use for feedstock production"]
[null,{"$f":"VLOOKUP($D255,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use for feedstock production"},null,"FP602a","m³/GJendfuel_fs2",null,{"$f":"G253*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FP601*BC550a/100*BC550b/100"]
[null,{"$f":"VLOOKUP($D256,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use for feedstock production"},null,"FP602b","m³/GJFU",null,{"$f":"G253*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FP601*BC550a/100*BC550b/100*FC025c/100*FC034"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D258,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},null,"FP603a","m³/kgfm",{"$f":"VLOOKUP(D258,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F258","v":0}]
[null,{"$f":"VLOOKUP($D259,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 1 (drying and storage)"},null,"FP603b","m³/GJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G258*G12/'Conversion feedstock2'!G176*1000)","v":0},"=FP603a*FP503a/BC515c*1000"]
["USE OF LAND"]
["Use of land after allocation 1"]
[null,{"$f":"VLOOKUP($D262,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated land use for feedstock production"},null,"FP605","ha/GJendfuel_fs1",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G65/'Conversion feedstock2'!G176*10)","v":0},"=FP530/100/BC515c*1000"]
["Totally allocated water use for feedstock production"]
[null,{"$f":"VLOOKUP($D264,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated land use for feedstock production"},null,"FP606a","ha/GJendfuel_fs1",null,{"$f":"G262*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FP605*BC550a/100*BC550b/100"]
[null,{"$f":"VLOOKUP($D265,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated land use for feedstock production"},null,"FP606b","ha/GJFU",null,{"$f":"G262*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FP605*BC550a/100*BC550b/100*FC025c/100*FC034"]
[]
["ENVIRONMENTAL QUALITY",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["ACIDIFICATION POTENTIAL"]
["Feedstock production"]
[null,{"$f":"VLOOKUP($D270,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential from feedstock production"},null,"FP612","gSO2_eq/ha",null,{"$f":"G272*G273+G42*G45*G274+G42*G46*G275","v":0},"=FP613*FP610a+FP537*FP611a*FP610b+FP537*FP611b*FP610c"]
[null,null,{"$f":"VLOOKUP($D271,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input of N-fixing crop residue to the soil"},"FP609","kg/ha",{"$f":"VLOOKUP(D271,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F271","v":0}]
[null,null,{"$f":"VLOOKUP($D272,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH3 volatilization from fertiliser use"},"FP613","gNH3/ha",null,{"$f":"(G24+G271)*1000*0.12","v":0},"=(FP523a+FP608)*1000*volatilization fraction NH3"]
[null,null,{"$f":"VLOOKUP($D273,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of NH3"},"FP610a","gSO2_eq/gNH3",{"$f":"VLOOKUP(\"NH3\",matrix_standardvalues_emissions,24,FALSE)","v":1.88},{"$f":"F273","v":1.88}]
[null,null,{"$f":"VLOOKUP($D274,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of NOx"},"FP610b","gSO2_eq/gNOx",{"$f":"VLOOKUP(\"NOx\",matrix_standardvalues_emissions,24,FALSE)","v":0.7},{"$f":"F274","v":0.7}]
[null,null,{"$f":"VLOOKUP($D275,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of SOx"},"FP610c","gSO2_eq/gSOx",{"$f":"VLOOKUP(\"SOx\",matrix_standardvalues_emissions,24,FALSE)","v":1},{"$f":"F275","v":1}]
["Acidification potential after allocation 1"]
[null,{"$f":"VLOOKUP($D277,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated acidification potential from feedstock production"},null,"FP614","gSO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G270*G65/100/'Conversion feedstock2'!G176)","v":0},"=FP612*FP530/100/BC515c"]
["Totally allocated acidification potential from feedstock production"]
[null,{"$f":"VLOOKUP($D279,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from feedstock production"},null,"FP615a","gSO2_eq/MJendfuel_fs2",null,{"$f":"G277*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"=FP614*BC550a/100*BC550b/100"]
[null,{"$f":"VLOOKUP($D280,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from feedstock production"},null,"FP615b","gSO2_eq/MJFU",null,{"$f":"G279*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"=FP615a*FC025c/100*FC034"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D282,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with heat and electricity for drying and storage per kg"},null,"FP616a","gSO2-eq/kgfm",null,{"$f":"G73*G78*G274+G73*G79*G275+G80*G85*G274+G80*G86*G275","v":0},"=FP540*FP542d*FP610b+FP540*FP542e*FP510c+FP543*FP545d*FP610b+FP543*FP545e*FP610c"]
[null,{"$f":"VLOOKUP($D283,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with heat and electricity for drying and storage per MJ endfuel"},null,"FP616b","gSO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G282*G12/'Conversion feedstock2'!G176)","v":0},"=FP616a*FP503a/BC515c"]
["EUTROPHICATION POTENTIAL"]
["Feedstock production"]
[null,{"$f":"VLOOKUP($D286,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of feedstock production"},null,"FP622","gPO4_eq/ha",null,{"$f":"G287*G288+G42*G45*G289+G291*G292+G295*G296","v":0},"=FP623a*FP620a+FP537*FP611a*FP620b+FP623d*FP620d+FP623g*FP620g"]
[null,null,{"$f":"VLOOKUP($D287,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N volatilization from fertiliser use (including NOx and NH3)"},"FP623a","gN/ha",null,{"$f":"(G24+G271)*1000*0.1","v":0},"=(FP523a+FP608)*1000*volatilization fraction N"]
[null,null,{"$f":"VLOOKUP($D288,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of N to air"},"FP620a","gPO4_eq/gN",{"$f":"VLOOKUP(\"N to air\",matrix_standardvalues_emissions,25,FALSE)","v":0.42},{"$f":"F288","v":0.42}]
[null,null,{"$f":"VLOOKUP($D289,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of NOx to air"},"FP620b","gPO4_eq/gNOx",{"$f":"VLOOKUP(\"NOx\",matrix_standardvalues_emissions,25,FALSE)","v":0.13},0.13]
[null,null,{"$f":"VLOOKUP($D290,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of NH3 to air"},"FP620c","gPO4_eq/gNH3",{"$f":"VLOOKUP(\"NH3\",matrix_standardvalues_emissions,25,FALSE)","v":0.35},0.35]
[null,null,{"$f":"VLOOKUP($D291,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"N leaching from fertiliser use (including NO3- and NH4+)"},"FP623d","gN/ha",null,{"$f":"(G24+G271)*1000*0.3","v":0},"=(FP523a+FP608)*1000*leaching fraction N"]
[null,null,{"$f":"VLOOKUP($D292,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of N to water"},"FP620d","gPO4_eq/gN",{"$f":"VLOOKUP(\"N to water\",matrix_standardvalues_emissions,25,FALSE)","v":0.42},0.42]
[null,null,{"$f":"VLOOKUP($D293,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of NO3- to water"},"FP620e","gPO4_eq/gNO3",{"$f":"VLOOKUP(\"NO3- to water\",matrix_standardvalues_emissions,25,FALSE)","v":0.1},0.1]
[null,null,{"$f":"VLOOKUP($D294,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of NH4+ to water"},"FP620f","gPO4_eq/gNH4+",{"$f":"VLOOKUP(\"NH4+ to water\",matrix_standardvalues_emissions,25,FALSE)","v":0.33},0.33]
[null,null,{"$f":"VLOOKUP($D295,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"P leaching from fertiliser use (total P to water)"},"FP623g","gP/ha",null,{"$f":"G27*1000*0.17","v":0},"=FP523b*1000*leaching fraction P"]
[null,null,{"$f":"VLOOKUP($D296,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of P to water"},"FP620g","gPO4_eq/gP",{"$f":"VLOOKUP(\"P to water\",matrix_standardvalues_emissions,25,FALSE)","v":3.06},3.06]
[null,null,{"$f":"VLOOKUP($D297,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of PO43-"},"FP620h","gPO4_eq/gPO4",{"$f":"VLOOKUP(\"PO43-\",matrix_standardvalues_emissions,25,FALSE)","v":1},1]
[null,null,{"$f":"VLOOKUP($D298,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of COD"},"FP620i","gPO4_eq/gCOD",{"$f":"VLOOKUP(\"COD\",matrix_standardvalues_emissions,25,FALSE)","v":2.1999999999999999E-2},2.1999999999999999E-2]
["Eutrophication potential after allocation 1"]
[null,{"$f":"VLOOKUP($D300,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated eutrophication potential from feedstock production"},null,"FP624","gPO4_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G286*G65/100/'Conversion feedstock2'!G176)","v":0},"=FP622*FP530/100/BC515c"]
["Totally allocated eutrophication potential from feedstock production"]
[null,{"$f":"VLOOKUP($D302,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from feedstock production"},null,"FP625a","gPO4_eq/MJendfuel_fs2",null,{"$f":"G300*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"=FP624*BC550a/100*BC550b/100"]
[null,{"$f":"VLOOKUP($D303,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from feedstock production"},null,"FP625b","gPO4_eq/MJFU",null,{"$f":"G302*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"=FP625a*FC025c/100*FC034"]
["Feedstock treatment 1 (drying & storage)"]
[null,{"$f":"VLOOKUP($D305,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with heat and electricity for drying and storage per kg"},null,"FP626a","gPO4-eq/kgfm",null,{"$f":"G73*G78*G289+G80*G85*G289","v":0},"=FP540*FP542d*FP620b+FP543*FP545d*FP620b"]
[null,{"$f":"VLOOKUP($D306,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with heat and electricity for drying and storage per MJ endfuel"},null,"FP626b","gPO4_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G305*G12/'Conversion feedstock2'!G176)","v":0},"=FP626a*FP503a/BC515c"]
[]
["BIODIVERSITY & HIGH CARBON STOCK",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Land with high biodiversity value"]
[null,{"$f":"VLOOKUP($D310,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in or after January 2008 = undisturbed forest (yes=1,no=0)"},null,"FP661","binary",{"$f":"VLOOKUP(D310,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"IF(F310=\"n.a.\",0,F310)","v":0}]
[null,{"$f":"VLOOKUP($D311,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in or after January 2008 = nature protection area"},null,"FP662","binary",{"$f":"VLOOKUP(D311,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"IF(F311=\"n.a.\",0,F311)","v":0}]
[null,{"$f":"VLOOKUP($D312,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in or after January 2008 = highly biodiverse grassland"},null,"FP663","binary",{"$f":"VLOOKUP(D312,Parameters!$1:$1958,6,FALSE)","v":0},0]
["Land with high carbon stock"]
[null,{"$f":"VLOOKUP($D314,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in January 2008 and not longer now = wetland"},null,"FP664","binary",{"$f":"VLOOKUP(D314,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,{"$f":"VLOOKUP($D315,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in January 2008 and not longer now = continuously forested area"},null,"FP665","binary",{"$f":"VLOOKUP(D315,Parameters!$1:$1958,6,FALSE)","v":0},0]
[null,{"$f":"VLOOKUP($D316,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land status in January 2008 and not longer now = peatland"},null,"FP666","binary",{"$f":"VLOOKUP(D316,Parameters!$1:$1958,6,FALSE)","v":0},0]
["Criterium RED"]
[null,{"$f":"VLOOKUP($D318,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"The requirements of the RED concerning biodiversity & high carbon stocks are met"},null,"FP667","binary",null,{"$f":"IF(G310=\"1\",0,IF(G311=\"1\",0,IF(G312=\"1\",0,IF(G314=\"1\",0,IF(G315=\"1\",0,IF(G316=\"1\",0,1))))))","v":1},"= 0 if one of the above is equal to 1"]
[]
["LOCAL WELL-BEING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Human and property rights"]
[null,{"$f":"VLOOKUP($D322,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour"},null,"FP670a","-",{"$f":"VLOOKUP(D322,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F322=\"n.a.\",0,IF(F322=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D323,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour "},null,"FP670b","-",{"$f":"VLOOKUP(D323,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F323=\"n.a.\",0,IF(F323=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D324,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights"},null,"FP670c","-",{"$f":"VLOOKUP(D324,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D325,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination"},null,"FP670d","-",{"$f":"VLOOKUP(D325,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D326,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured"},null,"FP670e","-",{"$f":"VLOOKUP(D326,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D327,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders"},null,"FP670f","-",{"$f":"VLOOKUP(D327,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D328,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security"},null,"FP670g","-",{"$f":"VLOOKUP(D328,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
["Labour rights and conditions"]
[null,{"$f":"VLOOKUP($D330,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts"},null,"FP671a","-",{"$f":"VLOOKUP(D330,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F330=\"n.a.\",0,IF(F330=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D331,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights"},null,"FP671b","-",{"$f":"VLOOKUP(D331,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F331=\"n.a.\",0,IF(F331=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D332,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves"},null,"FP671c","-",{"$f":"VLOOKUP(D332,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D333,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules"},null,"FP671d","-",{"$f":"VLOOKUP(D333,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D334,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy"},null,"FP671e","-",{"$f":"VLOOKUP(D334,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D335,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions"},null,"FP671f","-",{"$f":"VLOOKUP(D335,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D336,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training"},null,"FP671g","-",{"$f":"VLOOKUP(D336,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
["Scores"]
[null,{"$f":"VLOOKUP($D338,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights_score"},null,"FP672","-",null,{"$f":"SUM(G322:G328)","v":0},"= FP670a + FP670b + FP670c + FP670d + FP670e + FP670f + FP670g"]
[null,{"$f":"VLOOKUP($D339,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions_score"},null,"FP673","-",null,{"$f":"SUM(G330:G336)","v":0},"= FP671a + FP671b + FP671c + FP671d + FP671e + FP671f + FP671g"]

{"sheet":"Transport feedstock1","index":20,"n_rows":237,"n_cols":8,"rows_kept":237,"cut":false,"hidden":true,"merged":[]}
["Monitoring framework - Transport feedstock 1 (per year)"]
[]
[null,null,"From input"]
[null,null,"Standard value"]
[null,null,"Calculated from other fields"]
[null,null,"Determines value in other field"]
[]
["MASS BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Feedstock 1 - Transport 1"]
[null,{"$f":"VLOOKUP($D10,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 1"},null,"FT001a","-",{"$f":"VLOOKUP(D10,Parameters!$1:$2804,6,FALSE)","v":"Truck for FFB transport (Diesel)"},{"$f":"F10","v":"Truck for FFB transport (Diesel)"}]
[null,null,{"$f":"VLOOKUP($D11,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 1"},"FT002a","tkm/ha",null,{"$f":"('Production feedstock1'!G12/1000)*'Transport feedstock1'!G12","v":950},"=FP003a*FT003a/1000"]
[null,null,{"$f":"VLOOKUP($D12,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 1"},"FT003a","km",{"$f":"VLOOKUP(D12,Parameters!$1:$2804,6,FALSE)","v":50},{"$f":"IF(F12=\"n.a.\",0,F12)","v":50}]
[null,null,{"$f":"VLOOKUP($D13,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 1"},"FT004a","-",{"$f":"VLOOKUP(D13,Parameters!$1:$2804,6,FALSE)","v":"Diesel"},{"$f":"F13","v":"Diesel"}]
[null,null,{"$f":"VLOOKUP($D14,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 1"},"FT005a","MJfuel/tkm",{"$f":"IF(G10=\"n.a.\",0,VLOOKUP(G10,matrix_standardvalues_transportmodes,15,FALSE))","v":2.0122857142857145},2.0122857142857145]
[null,null,{"$f":"VLOOKUP($D15,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 1"},"FT006a","MJfossil/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13, matrix_standardvalues_fuelsall,11,FALSE))","v":1.1599999999999999},1.1599999999999999]
[null,null,{"$f":"VLOOKUP($D16,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 1"},"FT007a","MJprim/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13, matrix_standardvalues_fuelsall,21,FALSE))","v":1.7399999999999998},1.7399999999999998]
[null,null,{"$f":"VLOOKUP($D17,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 1"},"FT008a","gCO2-eq/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13, matrix_standardvalues_fuelsall,9,FALSE))","v":87.6388888888889},87.6388888888889]
[null,null,{"$f":"VLOOKUP($D18,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 1"},"FT037a","gNOX/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13,matrix_standardvalues_fuelsall,27,FALSE))","v":0.88800000000000001},0.88800000000000001]
[null,null,{"$f":"VLOOKUP($D19,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 1"},"FT038a","gSOX/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13,matrix_standardvalues_fuelsall,29,FALSE))","v":0.34499999999999997},0.34499999999999997]
["Feedstock 1 - Transport 2"]
[null,{"$f":"VLOOKUP($D21,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 2"},null,"FT001b","-",{"$f":"VLOOKUP(D21,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F21","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D22,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 2"},"FT002b","tkm/ha",null,{"$f":"'Conversion feedstock1'!G62*'Transport feedstock1'!G23/1000","v":0},"=FP003a*FT003b/1000"]
[null,null,{"$f":"VLOOKUP($D23,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 2"},"FT003b","km",{"$f":"VLOOKUP(D23,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F23=\"n.a.\",0,F23)","v":0}]
[null,null,{"$f":"VLOOKUP($D24,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 2"},"FT004b","-",{"$f":"VLOOKUP(D24,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F24","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D25,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 2"},"FT005b","MJfuel/tkm",{"$f":"IF(G21=\"n.a.\",0,VLOOKUP(G21,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D26,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 2"},"FT006b","MJfossil/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D27,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 2"},"FT007b","MJprim/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D28,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 2"},"FT008b","gCO2-eq/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D29,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 2"},"FT037b","gNOX/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D30,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 2"},"FT038b","gSOX/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 3"]
[null,{"$f":"VLOOKUP($D32,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 3"},null,"FT001c","-",{"$f":"VLOOKUP(D32,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F32","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D33,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 3"},"FT002c","tkm/ha",null,{"$f":"'Conversion feedstock1'!G72*'Transport feedstock1'!G34/1000","v":0},"=FP003a*FT003c/1000"]
[null,null,{"$f":"VLOOKUP($D34,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 3"},"FT003c","km",{"$f":"VLOOKUP(D34,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F34=\"n.a.\",0,F34)","v":0}]
[null,null,{"$f":"VLOOKUP($D35,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 3"},"FT004c","-",{"$f":"VLOOKUP(D35,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F35","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D36,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 3"},"FT005c","MJfuel/tkm",{"$f":"IF(G32=\"n.a.\",0,VLOOKUP(G32,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D37,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 3"},"FT006c","MJfossil/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D38,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 3"},"FT007c","MJprim/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D39,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 3"},"FT008c","gCO2-eq/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D40,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 3"},"FT037c","gNOX/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D41,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 3"},"FT038c","gSOX/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 4"]
[null,{"$f":"VLOOKUP($D43,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 4"},null,"FT001d","-",{"$f":"VLOOKUP(D43,Parameters!$1:$2804,6,FALSE)","v":"Truck for liquids (Diesel)"},{"$f":"F43","v":"Truck for liquids (Diesel)"}]
[null,null,{"$f":"VLOOKUP($D44,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 4"},"FT002d","tkm/ha",null,{"$f":"'Conversion feedstock1'!G19*'Transport feedstock1'!G45/1000","v":633.71699789434831},"=BC014a*FT003d/1000"]
[null,null,{"$f":"VLOOKUP($D45,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 4"},"FT003d","km",{"$f":"VLOOKUP(D45,Parameters!$1:$2804,6,FALSE)","v":150},{"$f":"IF(F45=\"n.a.\",0,F45)","v":150}]
[null,null,{"$f":"VLOOKUP($D46,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 4"},"FT004d","-",{"$f":"VLOOKUP(D46,Parameters!$1:$2804,6,FALSE)","v":"Diesel"},{"$f":"F46","v":"Diesel"}]
[null,null,{"$f":"VLOOKUP($D47,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 4"},"FT005d","MJfuel/tkm",{"$f":"IF(G43=\"n.a.\",0,VLOOKUP(G43,matrix_standardvalues_transportmodes,15,FALSE))","v":1.008},1.008]
[null,null,{"$f":"VLOOKUP($D48,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 4"},"FT006d","MJfossil/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46, matrix_standardvalues_fuelsall,11,FALSE))","v":1.1599999999999999},1.1599999999999999]
[null,null,{"$f":"VLOOKUP($D49,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 4"},"FT007d","MJprim/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46, matrix_standardvalues_fuelsall,21,FALSE))","v":1.7399999999999998},1.7399999999999998]
[null,null,{"$f":"VLOOKUP($D50,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 4"},"FT008d","gCO2-eq/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46, matrix_standardvalues_fuelsall,9,FALSE))","v":87.6388888888889},87.6388888888889]
[null,null,{"$f":"VLOOKUP($D51,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 4"},"FT037d","gNOX/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46,matrix_standardvalues_fuelsall,27,FALSE))","v":0.88800000000000001},0.88800000000000001]
[null,null,{"$f":"VLOOKUP($D52,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 4"},"FT038d","gSOX/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46,matrix_standardvalues_fuelsall,29,FALSE))","v":0.34499999999999997},0.34499999999999997]
["Feedstock 1 - Transport 5"]
[null,{"$f":"VLOOKUP($D54,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 5"},null,"FT001e","-",{"$f":"VLOOKUP(D54,Parameters!$1:$2804,6,FALSE)","v":"Ship /product tanker 50kt (HFO maritime)"},{"$f":"F54","v":"Ship /product tanker 50kt (HFO maritime)"}]
[null,null,{"$f":"VLOOKUP($D55,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 5"},"FT002e","tkm/ha",null,{"$f":"'Conversion feedstock1'!G19*'Transport feedstock1'!G56/1000","v":43033.608937012214},"=BC014a*FT003e/1000"]
[null,null,{"$f":"VLOOKUP($D56,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 5"},"FT003e","km",{"$f":"VLOOKUP(D56,Parameters!$1:$2804,6,FALSE)","v":10186},{"$f":"IF(F56=\"n.a.\",0,F56)","v":10186}]
[null,null,{"$f":"VLOOKUP($D57,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 5"},"FT004e","-",{"$f":"VLOOKUP(D57,Parameters!$1:$2804,6,FALSE)","v":"HFO for maritime transport"},{"$f":"F57","v":"HFO for maritime transport"}]
[null,null,{"$f":"VLOOKUP($D58,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 5"},"FT005e","MJfuel/tkm",{"$f":"IF(G54=\"n.a.\",0,VLOOKUP(G54,matrix_standardvalues_transportmodes,15,FALSE))","v":0.12384000000000001},0.12384000000000001]
[null,null,{"$f":"VLOOKUP($D59,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 5"},"FT006e","MJfossil/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsall,11,FALSE))","v":1.0880000000000001},1.0880000000000001]
[null,null,{"$f":"VLOOKUP($D60,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 5"},"FT007e","MJprim/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsall,21,FALSE))","v":1.6320000000000001},1.6320000000000001]
[null,null,{"$f":"VLOOKUP($D61,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 5"},"FT008e","gCO2-eq/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsall,9,FALSE))","v":87.2},87.2]
[null,null,{"$f":"VLOOKUP($D62,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 5"},"FT037e","gNOX/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57,matrix_standardvalues_fuelsall,27,FALSE))","v":0.88800000000000001},0.88800000000000001]
[null,null,{"$f":"VLOOKUP($D63,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 5"},"FT038e","gSOX/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57,matrix_standardvalues_fuelsall,29,FALSE))","v":0.34499999999999997},0.34499999999999997]
["Feedstock 1 - Transport 6"]
[null,{"$f":"VLOOKUP($D65,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 6"},null,"FT001f","-",{"$f":"VLOOKUP(D65,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F65","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D66,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 6"},"FT002f","tkm/ha",null,{"$f":"'Conversion feedstock1'!G19*'Transport feedstock1'!G67/1000","v":0},"=BC014a*FT003f/1000"]
[null,null,{"$f":"VLOOKUP($D67,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 6"},"FT003f","km",{"$f":"VLOOKUP(D67,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F67=\"n.a.\",0,F67)","v":0}]
[null,null,{"$f":"VLOOKUP($D68,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 6"},"FT004f","-",{"$f":"VLOOKUP(D68,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F68","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D69,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 6"},"FT005f","MJfuel/tkm",{"$f":"IF(G65=\"n.a.\",0,VLOOKUP(G65,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D70,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 6"},"FT006f","MJfossil/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D71,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 6"},"FT007f","MJprim/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D72,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 6"},"FT008f","gCO2-eq/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D73,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 6"},"FT037f","gNOX/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D74,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 6"},"FT038f","gSOX/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 7"]
[null,{"$f":"VLOOKUP($D76,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 7"},null,"FT001g","-",{"$f":"VLOOKUP(D76,Parameters!$1:$2804,6,FALSE)","v":"Truck for liquids (Diesel)"},{"$f":"F76","v":"Truck for liquids (Diesel)"}]
[null,null,{"$f":"VLOOKUP($D77,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 7"},"FT002g","tkm/ha",null,{"$f":"'Conversion feedstock1'!G174*'Transport feedstock1'!G78/1000","v":135.14199870371556},"=BC015a*FT003g/1000"]
[null,null,{"$f":"VLOOKUP($D78,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 7"},"FT003g","km",{"$f":"VLOOKUP(D78,Parameters!$1:$2804,6,FALSE)","v":100},{"$f":"IF(F78=\"n.a.\",0,F78)","v":100}]
[null,null,{"$f":"VLOOKUP($D79,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 7"},"FT004g","-",{"$f":"VLOOKUP(D79,Parameters!$1:$2804,6,FALSE)","v":"Diesel"},{"$f":"F79","v":"Diesel"}]
[null,null,{"$f":"VLOOKUP($D80,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 7"},"FT005g","MJfuel/tkm",{"$f":"IF(G76=\"n.a.\",0,VLOOKUP(G76,matrix_standardvalues_transportmodes,15,FALSE))","v":1.008},1.008]
[null,null,{"$f":"VLOOKUP($D81,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 7"},"FT006g","MJfossil/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79, matrix_standardvalues_fuelsall,11,FALSE))","v":1.1599999999999999},1.1599999999999999]
[null,null,{"$f":"VLOOKUP($D82,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 7"},"FT007g","MJprim/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79, matrix_standardvalues_fuelsall,21,FALSE))","v":1.7399999999999998},1.7399999999999998]
[null,null,{"$f":"VLOOKUP($D83,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 7"},"FT008g","gCO2-eq/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79, matrix_standardvalues_fuelsall,9,FALSE))","v":87.6388888888889},87.6388888888889]
[null,null,{"$f":"VLOOKUP($D84,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 7"},"FT037g","gNOX/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79,matrix_standardvalues_fuelsall,27,FALSE))","v":0.88800000000000001},0.88800000000000001]
[null,null,{"$f":"VLOOKUP($D85,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 7"},"FT038g","gSOX/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79,matrix_standardvalues_fuelsall,29,FALSE))","v":0.34499999999999997},0.34499999999999997]
["Feedstock 1 - Transport 8"]
[null,{"$f":"VLOOKUP($D87,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 8"},null,"FT001h","-",{"$f":"VLOOKUP(D87,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F87","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D88,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 8"},"FT002h","tkm/ha",null,{"$f":"'Conversion feedstock1'!G174*'Transport feedstock1'!G89/1000","v":0},"=BC015a*FT003h/1000"]
[null,null,{"$f":"VLOOKUP($D89,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 8"},"FT003h","km",{"$f":"VLOOKUP(D89,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F89=\"n.a.\",0,F89)","v":0}]
[null,null,{"$f":"VLOOKUP($D90,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 8"},"FT004h","-",{"$f":"VLOOKUP(D90,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F90","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D91,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 8"},"FT005h","MJfuel/tkm",{"$f":"IF(G87=\"n.a.\",0,VLOOKUP(G87,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D92,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 8"},"FT006h","MJfossil/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D93,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 8"},"FT007h","MJprim/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D94,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 8"},"FT008h","gCO2-eq/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D95,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 8"},"FT037h","gNOX/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D96,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 8"},"FT038h","gSOX/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 9"]
[null,{"$f":"VLOOKUP($D98,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 9"},null,"FT001i","-",{"$f":"VLOOKUP(D98,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F98","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D99,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 9"},"FT002i","tkm/ha",null,{"$f":"'Conversion feedstock1'!G174*'Transport feedstock1'!G100/1000","v":0},"=BC015a*FT003i/1000"]
[null,null,{"$f":"VLOOKUP($D100,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 9"},"FT003i","km",{"$f":"VLOOKUP(D100,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F100=\"n.a.\",0,F100)","v":0}]
[null,null,{"$f":"VLOOKUP($D101,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 9"},"FT004i","-",{"$f":"VLOOKUP(D101,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F101","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D102,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 9"},"FT005i","MJfuel/tkm",{"$f":"IF(G98=\"n.a.\",0,VLOOKUP(G98,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D103,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 9"},"FT006i","MJfossil/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D104,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 9"},"FT007i","MJprim/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D105,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 9"},"FT008i","gCO2-eq/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D106,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 9"},"FT037i","gNOX/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D107,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 9"},"FT038i","gSOX/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[]
["ENERGY BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Energy use for transport feedstock 1"]
[null,{"$f":"VLOOKUP($D111,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport 1 (mode 1-2-3)"},null,"FT012a","MJfossil/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G113+G115+G117)/'Conversion feedstock1'!G21,(G113+G115+G117)/'Conversion feedstock1'!G176)","v":4.4348524663217689E-2},"=(FT009a+FT009b+FT009c)/BC015c"]
[null,{"$f":"VLOOKUP($D112,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport 1 (mode 1-2-3)"},null,"FT012b","MJprim/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G114+G116+G118)/'Conversion feedstock1'!G21,(G114+G116+G118)/'Conversion feedstock1'!G176)","v":6.6522786994826541E-2},"=(FT010a+FT010b+FT010c)/BC015c"]
[null,null,{"$f":"VLOOKUP($D113,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 1"},"FT009a","MJfossil/ha",null,{"$f":"G11*G14*G15","v":2217.5388571428571},"=FT002a*FT005a*FT006a"]
[null,null,{"$f":"VLOOKUP($D114,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 1"},"FT010a","MJprim/ha",null,{"$f":"G11*G14*G16","v":3326.3082857142858},"=FT002a*FT005a*FT007a"]
[null,null,{"$f":"VLOOKUP($D115,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 2"},"FT009b","MJfossil/ha",null,{"$f":"G22*G25*G26","v":0},"=FT002b*FT005b*FT006b"]
[null,null,{"$f":"VLOOKUP($D116,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 2"},"FT010b","MJprim/ha",null,{"$f":"G22*G25*G27","v":0},"=FT002b*FT005b*FT007b"]
[null,null,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 3"},"FT009c","MJfossil/ha",null,{"$f":"G33*G36*G37","v":0},"=FT002c*FT005c*FT006c"]
[null,null,{"$f":"VLOOKUP($D118,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 3"},"FT010c","MJprim/ha",null,{"$f":"G33*G36*G38","v":0},"=FT002c*FT005c*FT007c"]
[null,{"$f":"VLOOKUP($D119,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport 2 (mode 4-5-6)"},null,"FT013a","MJfossil/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G121+G123+G125)/'Conversion feedstock1'!G21,(G121+G123+G125)/'Conversion feedstock1'!G176)","v":0.1307783891036127},"=(FT009d+FT009e+FT009f)/BC015c"]
[null,{"$f":"VLOOKUP($D120,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport 2 (mode 4-5-6)"},null,"FT013b","MJprim/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G122+G124+G126)/'Conversion feedstock1'!G21,(G122+G124+G126)/'Conversion feedstock1'!G176)","v":0.19616758365541906},"=(FT010d+FT010e+FT010f)/BC015c"]
[null,null,{"$f":"VLOOKUP($D121,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 4"},"FT009d","MJfossil/ha",null,{"$f":"G44*G47*G48","v":740.99261129790364},"=FT002d*FT005d*FT006d"]
[null,null,{"$f":"VLOOKUP($D122,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 4"},"FT010d","MJprim/ha",null,{"$f":"G44*G47*G49","v":1111.4889169468554},"=FT002d*FT005d*FT007d"]
[null,null,{"$f":"VLOOKUP($D123,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 5"},"FT009e","MJfossil/ha",null,{"$f":"G55*G58*G59","v":5798.2589582664377},"=FT002e*FT005e*FT006e"]
[null,null,{"$f":"VLOOKUP($D124,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 5"},"FT010e","MJprim/ha",null,{"$f":"G55*G58*G60","v":8697.3884373996571},"=FT002e*FT005e*FT007e"]
[null,null,{"$f":"VLOOKUP($D125,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 6"},"FT009f","MJfossil/ha",null,{"$f":"G66*G69*G70","v":0},"=FT002f*FT005f*FT006f"]
[null,null,{"$f":"VLOOKUP($D126,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 6"},"FT010f","MJprim/ha",null,{"$f":"G66*G69*G71","v":0},"=FT002f*FT005f*FT007f"]
[null,{"$f":"VLOOKUP($D127,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport 3 (mode 7-8-9)"},null,"FT014a","MJfossil/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G129+G131+G133)/'Conversion feedstock1'!G21,(G129+G131+G133)/'Conversion feedstock1'!G176)","v":3.1602162162162164E-3},"=(FT009g+FT009h+FT009i)/BC015c"]
[null,{"$f":"VLOOKUP($D128,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport 3 (mode 7-8-9)"},null,"FT014b","MJprim/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G130+G132+G134)/'Conversion feedstock1'!G21,(G130+G132+G134)/'Conversion feedstock1'!G176)","v":4.7403243243243241E-3},"=(FT010g+FT010h+FT010i)/BC015c"]
[null,null,{"$f":"VLOOKUP($D129,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 7"},"FT009g","MJfossil/ha",null,{"$f":"G77*G80*G81","v":158.01883624428052},"=FT002g*FT005g*FT006g"]
[null,null,{"$f":"VLOOKUP($D130,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 7"},"FT010g","MJprim/ha",null,{"$f":"G77*G80*G82","v":237.02825436642075},"=FT002g*FT005g*FT007g"]
[null,null,{"$f":"VLOOKUP($D131,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 8"},"FT009h","MJfossil/ha",null,{"$f":"G88*G91*G92","v":0},"=FT002h*FT005h*FT006h"]
[null,null,{"$f":"VLOOKUP($D132,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 8"},"FT010h","MJprim/ha",null,{"$f":"G88*G91*G93","v":0},"=FT002h*FT005h*FT007h"]
[null,null,{"$f":"VLOOKUP($D133,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 9"},"FT009i","MJfossil/ha",null,{"$f":"G99*G102*G103","v":0},"=FT002i*FT005i*FT006i"]
[null,null,{"$f":"VLOOKUP($D134,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 9"},"FT010i","MJprim/ha",null,{"$f":"G99*G102*G104","v":0},"=FT002i*FT005i*FT007i"]
["Totally allocated energy use for transport"]
[null,{"$f":"VLOOKUP($D136,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 1"},null,"FT020a","MJfossil/MJendfuel_fs1",null,{"$f":"G111*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":4.2427297465073593E-2},"= FT012a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D137,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 1"},null,"FT020b","MJprim/MJendfuel_fs1",null,{"$f":"G112*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":6.364094619761039E-2},"= FT012b * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D138,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 1"},null,"FT021a","MJfossil/MJFU",null,{"$f":"G111*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":4.2427297465073593E-2},"= FT012a * BC050a / 100 * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D139,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 1"},null,"FT021b","MJprim/MJFU",null,{"$f":"G112*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":6.364094619761039E-2},"= FT012b * BC050a / 100 * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D140,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 2"},null,"FT022a","MJfossil/MJendfuel_fs1",null,{"$f":"G119*'Conversion feedstock1'!G256/100","v":0.1307783891036127},"= FT013a * BC050b / 100"]
[null,{"$f":"VLOOKUP($D141,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 2"},null,"FT022b","MJprim/MJendfuel_fs1",null,{"$f":"G120*'Conversion feedstock1'!G256/100","v":0.19616758365541906},"= FT013b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D142,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 2"},null,"FT023a","MJfossil/MJFU",null,{"$f":"G119*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":0.1307783891036127},"= FT013a * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D143,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 2"},null,"FT023b","MJprim/MJFU",null,{"$f":"G120*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":0.19616758365541906},"= FT013b * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D144,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 3"},null,"FT024a","MJfossil/MJendfuel_fs1",null,{"$f":"G127","v":3.1602162162162164E-3},"= FT014a"]
[null,{"$f":"VLOOKUP($D145,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 3"},null,"FT024b","MJprim/MJendfuel_fs1",null,{"$f":"G128","v":4.7403243243243241E-3},"= FT014b"]
[null,{"$f":"VLOOKUP($D146,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 3"},null,"FT025a","MJfossil/MJFU",null,{"$f":"G127*'Final conversion'!G68/100*'Final conversion'!G22","v":3.1602162162162164E-3},"= FT014a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D147,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 3"},null,"FT025b","MJprim/MJFU",null,{"$f":"G128*'Final conversion'!G68/100*'Final conversion'!G22","v":4.7403243243243241E-3},"= FT014b * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D148,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in total transport (1-3)"},null,"FT026a","MJfossil/MJendfuel_fs1",null,{"$f":"G136+G140+G144","v":0.1763659027849025},"= FT020a + FT022a + FT024a"]
[null,{"$f":"VLOOKUP($D149,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in total transport (1-3)"},null,"FT026b","MJprim/MJendfuel_fs1",null,{"$f":"G137+G141+G145","v":0.26454885417735374},"= FT020b + FT022b + FT024b"]
[null,{"$f":"VLOOKUP($D150,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in total transport (1-3)"},null,"FT027a","MJfossil/MJFU",null,{"$f":"G138+G142+G146","v":0.1763659027849025},"= FT021a + FT023a + FT025a"]
[null,{"$f":"VLOOKUP($D151,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in total transport (1-3)"},null,"FT027b","MJprim/MJFU",null,{"$f":"G139+G143+G147","v":0.26454885417735374},"= FT021b + FT023b + FT025b"]
[]
["GLOBAL WARMING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["GHG emissions from transport feedstock 1"]
[null,{"$f":"VLOOKUP($D155,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with transport 1 (mode 1-2-3)"},null,"FT015a","gCO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G156+G157+G158)/'Conversion feedstock1'!G21,(G156+G157+G158)/'Conversion feedstock1'!G176)","v":3.350565021849901},"=(FT011a+FT011b+FT011c)/BC015c"]
[null,null,{"$f":"VLOOKUP($D156,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 1"},"FT011a","gCO2-eq/ha",null,{"$f":"G11*G14*G17","v":167536.75992063497},"=FT002a*FT005a*FT008a"]
[null,null,{"$f":"VLOOKUP($D157,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 2"},"FT011b","gCO2-eq/ha",null,{"$f":"G22*G25*G28","v":0},"=FT002b*FT005b*FT008b"]
[null,null,{"$f":"VLOOKUP($D158,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 3"},"FT011c","gCO2-eq/ha",null,{"$f":"G33*G36*G39","v":0},"=FT002c*FT005c*FT008c"]
[null,{"$f":"VLOOKUP($D159,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with transport 2 (mode 4-5-6)"},null,"FT015b","gCO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G160+G161+G162)/'Conversion feedstock1'!G21,(G160+G161+G162)/'Conversion feedstock1'!G176)","v":10.413390327586322},"=(FT011d+FT011e+FT011f)/BC015c"]
[null,null,{"$f":"VLOOKUP($D160,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 4"},"FT011d","gCO2-eq/ha",null,{"$f":"G44*G47*G50","v":55982.559593986742},"=FT002d*FT005d*FT008d"]
[null,null,{"$f":"VLOOKUP($D161,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 5"},"FT011e","gCO2-eq/ha",null,{"$f":"G55*G58*G61","v":464713.40180223656},"=FT002e*FT005e*FT008e"]
[null,null,{"$f":"VLOOKUP($D162,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 6"},"FT011f","gCO2-eq/ha",null,{"$f":"G66*G69*G72","v":0},"=FT002f*FT005f*FT008f"]
[null,{"$f":"VLOOKUP($D163,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with transport 3 (mode 7-8-9)"},null,"FT015c","gCO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G164+G165+G166)/'Conversion feedstock1'!G21,(G164+G165+G166)/'Conversion feedstock1'!G176)","v":0.23875675675675681},"=(FT011g+FT011h+FT011i)/BC015c"]
[null,null,{"$f":"VLOOKUP($D164,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 7"},"FT011g","gCO2-eq/ha",null,{"$f":"G77*G80*G83","v":11938.444165486235},"=FT002g*FT005g*FT008g"]
[null,null,{"$f":"VLOOKUP($D165,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 8"},"FT011h","gCO2-eq/ha",null,{"$f":"G88*G91*G94","v":0},"=FT002h*FT005h*FT008h"]
[null,null,{"$f":"VLOOKUP($D166,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 9"},"FT011i","gCO2-eq/ha",null,{"$f":"G99*G102*G105","v":0},"=FT002i*FT005i*FT008i"]
["Totally allocated GHG emissions from transport"]
[null,{"$f":"VLOOKUP($D168,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 1"},null,"FT030a","gCO2_eq/MJendfuel_fs1",null,{"$f":"G155*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":3.2054148348253646},"= FT015a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D169,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 1"},null,"FT030b","gCO2_eq/MJFU",null,{"$f":"G155*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":3.2054148348253646},"= FT015a * BC050a / 100 * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D170,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 2"},null,"FT031a","gCO2_eq/MJendfuel_fs1",null,{"$f":"G159*'Conversion feedstock1'!G256/100","v":10.41339032758632},"= FT015b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D171,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 2"},null,"FT031b","gCO2_eq/MJFU",null,{"$f":"G159*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":10.41339032758632},"= FT015b * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D172,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 3"},null,"FT032a","gCO2_eq/MJendfuel_fs1",null,{"$f":"G163","v":0.23875675675675681},"= FT015c"]
[null,{"$f":"VLOOKUP($D173,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 3"},null,"FT032b","gCO2_eq/MJFU",null,{"$f":"G163*'Final conversion'!G68/100*'Final conversion'!G22","v":0.23875675675675681},"= FT015c * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D174,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from total transport (1-3)"},null,"FT033a","gCO2_eq/MJendfuel_fs1",null,{"$f":"G168+G170+G172","v":13.857561919168443},"= FT030a + FT031a + FT032a"]
[null,{"$f":"VLOOKUP($D175,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from total transport (1-3)"},null,"FT033b","gCO2_eq/MJFU",null,{"$f":"G169+G171+G173","v":13.857561919168443},"= FT030b + FT031b + FT032b"]
[]
["RESOURCE USE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["USE OF WATER"]
[null,"N.A."]
["USE OF LAND"]
[null,"N.A."]
[]
["ENVIRONMENTAL QUALITY",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["ACIDIFICATION POTENTIAL"]
["Acidification potential from transport feedstock 1"]
[null,{"$f":"VLOOKUP($D186,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with transport 1 (mode 1-2-3)"},null,"FT016a","gSO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G187+G188+G189)/'Conversion feedstock1'!G21,(G187+G188+G189)/'Conversion feedstock1'!G176)","v":3.6954555120229507E-2},"=(FT035a+FT035b+FT035c)/BC015c"]
[null,null,{"$f":"VLOOKUP($D187,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 1"},"FT035a","gSO2-eq/ha",null,{"$f":"G11*G14*G18*'Production feedstock1'!G274+G11*G14*G19*'Production feedstock1'!G275","v":1847.821602857143},"=FT002a*FT005a*FT037a*FP110b+FT002a*FT005a*FT038a*FP110c"]
[null,null,{"$f":"VLOOKUP($D188,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 2"},"FT035b","gSO2-eq/ha",null,{"$f":"G22*G25*G29*'Production feedstock1'!G274+G22*G25*G30*'Production feedstock1'!G275","v":0},"=FT002b*FT005b*FT037b*FP110b+FT002b*FT005b*FT038b*FP110c"]
[null,null,{"$f":"VLOOKUP($D189,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 3"},"FT035c","gSO2-eq/ha",null,{"$f":"G33*G36*G40*'Production feedstock1'!G274+G33*G36*G41*'Production feedstock1'!G275","v":0},"=FT002c*FT005c*FT037c*FP110b+FT002c*FT005c*FT038c*FP110c"]
[null,{"$f":"VLOOKUP($D190,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with transport 2 (mode 4-5-6)"},null,"FT016b","gSO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G191+G192+G193)/'Conversion feedstock1'!G21,(G191+G192+G193)/'Conversion feedstock1'!G176)","v":0.11536884766037943},"=(FT035d+FT035e+FT035f)/BC015c"]
[null,null,{"$f":"VLOOKUP($D191,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 4"},"FT035d","gSO2-eq/ha",null,{"$f":"G44*G47*G51*'Production feedstock1'!G274+G44*G47*G52*'Production feedstock1'!G275","v":617.45125696599439},"=FT002d*FT005d*FT037d*FP110b+FT002d*FT005d*FT038d*FP110c"]
[null,null,{"$f":"VLOOKUP($D192,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 5"},"FT035e","gSO2-eq/ha",null,{"$f":"G55*G58*G62*'Production feedstock1'!G274+G55*G58*G63*'Production feedstock1'!G275","v":5151.2841075922224},"=FT002e*FT005e*FT037e*FP110b+FT002e*FT005e*FT038e*FP110c"]
[null,null,{"$f":"VLOOKUP($D193,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 6"},"FT035f","gSO2-eq/ha",null,{"$f":"G66*G69*G73*'Production feedstock1'!G274+G66*G69*G74*'Production feedstock1'!G275","v":0},"=FT002f*FT005f*FT037f*FP110b+FT002f*FT005f*FT038f*FP110c"]
[null,{"$f":"VLOOKUP($D194,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with transport 3 (mode 7-8-9)"},null,"FT016c","gSO2_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G195+G196+G197)/'Conversion feedstock1'!G21,(G195+G196+G197)/'Conversion feedstock1'!G176)","v":2.633331891891892E-3},"=(FT035g+FT035h+FT035i)/BC015c"]
[null,null,{"$f":"VLOOKUP($D195,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 7"},"FT035g","gSO2-eq/ha",null,{"$f":"G77*G80*G84*'Production feedstock1'!G274+G77*G80*G85*'Production feedstock1'!G275","v":131.67328199458754},"=FT002g*FT005g*FT037g*FP110b+FT002g*FT005g*FT038g*FP110c"]
[null,null,{"$f":"VLOOKUP($D196,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 8"},"FT035h","gSO2-eq/ha",null,{"$f":"G88*G91*G95*'Production feedstock1'!G274+G88*G91*G96*'Production feedstock1'!G275","v":0},"=FT002h*FT005h*FT037h*FP110b+FT002h*FT005h*FT038h*FP110c"]
[null,null,{"$f":"VLOOKUP($D197,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 9"},"FT035i","gSO2-eq/ha",null,{"$f":"G99*G102*G106*'Production feedstock1'!G274+G99*G102*G107*'Production feedstock1'!G275","v":0},"=FT002i*FT005i*FT037i*FP110b+FT002i*FT005i*FT038i*FP110c"]
["Totally allocated acidification potential from transport"]
[null,{"$f":"VLOOKUP($D199,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 1"},null,"FT040a","gSO2_eq/MJendfuel_fs1",null,{"$f":"G186*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":3.5353642870465642E-2},"= FT016a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D200,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 1"},null,"FT040b","gSO2_eq/MJFU",null,{"$f":"G199*'Final conversion'!G68/100*'Final conversion'!G22","v":3.5353642870465642E-2},"= FT040a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D201,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 2"},null,"FT041a","gSO2_eq/MJendfuel_fs1",null,{"$f":"G190*'Conversion feedstock1'!G256/100","v":0.11536884766037943},"= FT016b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D202,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 2"},null,"FT041b","gSO2_eq/MJFU",null,{"$f":"G201*'Final conversion'!G68/100*'Final conversion'!G22","v":0.11536884766037943},"= FT041a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D203,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 3"},null,"FT042a","gSO2_eq/MJendfuel_fs1",null,{"$f":"G194","v":2.633331891891892E-3},"= FT016c"]
[null,{"$f":"VLOOKUP($D204,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 3"},null,"FT042b","gSO2_eq/MJFU",null,{"$f":"G203*'Final conversion'!G68/100*'Final conversion'!G22","v":2.633331891891892E-3},"= FT042a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D205,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from total transport (1-3)"},null,"FT043a","gSO2_eq/MJendfuel_fs1",null,{"$f":"G199+G201+G203","v":0.15335582242273696},"= FT040a + FT041a + FT042a"]
[null,{"$f":"VLOOKUP($D206,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from total transport (1-3)"},null,"FT043b","gSO2_eq/MJFU",null,{"$f":"G200+G202+G204","v":0.15335582242273696},"= FT040b + FT041b + FT042b"]
["EUTROPHICATION POTENTIAL"]
["Eutrophication potential from transport feedstock 1"]
[null,{"$f":"VLOOKUP($D209,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with transport 1 (mode 1-2-3)"},null,"FT017a","gPO4_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G210+G211+G212)/'Conversion feedstock1'!G21,(G210+G211+G212)/'Conversion feedstock1'!G176)","v":4.4134428337257343E-3},"=(FT036a+FT036b+FT036c)/BC015c"]
[null,null,{"$f":"VLOOKUP($D210,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 1"},"FT036a","gPO4-eq/ha",null,{"$f":"G11*G14*G18*'Production feedstock1'!G289","v":220.68334971428575},"=FT002a*FT005a*FT037a*FP120b"]
[null,null,{"$f":"VLOOKUP($D211,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 2"},"FT036b","gPO4-eq/ha",null,{"$f":"G22*G25*G29*'Production feedstock1'!G289","v":0},"=FT002b*FT005b*FT037b*FP120b"]
[null,null,{"$f":"VLOOKUP($D212,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 3"},"FT036c","gPO4-eq/ha",null,{"$f":"G33*G36*G40*'Production feedstock1'!G289","v":0},"=FT002c*FT005c*FT037c*FP120b"]
[null,{"$f":"VLOOKUP($D213,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with transport 2 (mode 4-5-6)"},null,"FT017b","gPO4_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G214+G215+G216)/'Conversion feedstock1'!G21,(G214+G215+G216)/'Conversion feedstock1'!G176)","v":1.3778377585261953E-2},"=(FT036d+FT036e+FT036f)/BC015c"]
[null,null,{"$f":"VLOOKUP($D214,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 4"},"FT036d","gPO4-eq/ha",null,{"$f":"G44*G47*G51*'Production feedstock1'!G289","v":73.741540558818954},"=FT002d*FT005d*FT037d*FP120b"]
[null,null,{"$f":"VLOOKUP($D215,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 5"},"FT036e","gPO4-eq/ha",null,{"$f":"G55*G58*G62*'Production feedstock1'!G289","v":615.21232917488749},"=FT002e*FT005e*FT037e*FP120b"]
[null,null,{"$f":"VLOOKUP($D216,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 6"},"FT036f","gPO4-eq/ha",null,{"$f":"G66*G69*G73*'Production feedstock1'!G289","v":0},"=FT002f*FT005f*FT037f*FP120b"]
[null,{"$f":"VLOOKUP($D217,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with transport 3 (mode 7-8-9)"},null,"FT017c","gPO4_eq/MJendfuel_fs1",null,{"$f":"IF('Conversion feedstock1'!G176=0,(G218+G219+G220)/'Conversion feedstock1'!G21,(G218+G219+G220)/'Conversion feedstock1'!G176)","v":3.1449600000000005E-4},"=(FT036g+FT036h+FT036i)/BC015c"]
[null,null,{"$f":"VLOOKUP($D218,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 7"},"FT036g","gPO4-eq/ha",null,{"$f":"G77*G80*G84*'Production feedstock1'!G289","v":15.72559866899978},"=FT002g*FT005g*FT037g*FP120b"]
[null,null,{"$f":"VLOOKUP($D219,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 8"},"FT036h","gPO4-eq/ha",null,{"$f":"G88*G91*G95*'Production feedstock1'!G289","v":0},"=FT002h*FT005h*FT037h*FP120b"]
[null,null,{"$f":"VLOOKUP($D220,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 9"},"FT036i","gPO4-eq/ha",null,{"$f":"G99*G102*G106*'Production feedstock1'!G289","v":0},"=FT002i*FT005i*FT037i*FP120b"]
["Totally allocated eutrophication potential from transport"]
[null,{"$f":"VLOOKUP($D222,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 1"},null,"FT044a","gPO4_eq/MJendfuel_fs1",null,{"$f":"G209*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":4.2222476029035319E-3},"= FT017a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D223,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 1"},null,"FT044b","gPO4_eq/MJFU",null,{"$f":"G222*'Final conversion'!G68/100*'Final conversion'!G22","v":4.2222476029035319E-3},"= FT044a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D224,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 2"},null,"FT045a","gPO4_eq/MJendfuel_fs1",null,{"$f":"G213*'Conversion feedstock1'!G256/100","v":1.3778377585261953E-2},"= FT017b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D225,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 2"},null,"FT045b","gPO4_eq/MJFU",null,{"$f":"G224*'Final conversion'!G68/100*'Final conversion'!G22","v":1.3778377585261953E-2},"= FT045a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D226,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 3"},null,"FT046a","gPO4_eq/MJendfuel_fs1",null,{"$f":"G217","v":3.1449600000000005E-4},"= FT017c"]
[null,{"$f":"VLOOKUP($D227,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 3"},null,"FT046b","gPO4_eq/MJFU",null,{"$f":"G226*'Final conversion'!G68/100*'Final conversion'!G22","v":3.144960000000001E-4},"= FT046a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D228,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from total transport (1-3)"},null,"FT047a","gPO4_eq/MJendfuel_fs1",null,{"$f":"G222+G224+G226","v":1.8315121188165487E-2},"= FT040a + FT041a + FT042a"]
[null,{"$f":"VLOOKUP($D229,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from total transport (1-3)"},null,"FT047b","gPO4_eq/MJFU",null,{"$f":"G223+G225+G227","v":1.8315121188165487E-2},"= FT040b + FT041b + FT042b"]
[]
["BIODIVERSITY & HIGH CARBON STOCK",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Land with high biodiversity value"]
[null,"N.A."]
["Land with high carbon stock"]
[null,"N.A."]
["Criterium RED"]
[null,"N.A."]

{"sheet":"Transport feedstock2","index":21,"n_rows":237,"n_cols":8,"rows_kept":237,"cut":false,"hidden":true,"merged":[]}
["Monitoring framework - Transport feedstock 2 (per year)"]
[]
[null,null,"From input"]
[null,null,"Standard value"]
[null,null,"Calculated from other fields"]
[null,null,"Determines value in other field"]
[]
["MASS BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Feedstock 1 - Transport 1"]
[null,{"$f":"VLOOKUP($D10,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 1"},null,"FT501a","-",{"$f":"VLOOKUP(D10,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F10","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D11,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 1"},"FT502a","tkm/ha",null,{"$f":"'Production feedstock2'!G12*'Transport feedstock2'!G12/1000","v":0},"=FP503a*FT503a/1000"]
[null,null,{"$f":"VLOOKUP($D12,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 1"},"FT503a","km",{"$f":"VLOOKUP(D12,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F12=\"n.a.\",0,F12)","v":0}]
[null,null,{"$f":"VLOOKUP($D13,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 1"},"FT504a","-",{"$f":"VLOOKUP(D13,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F13","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D14,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 1"},"FT505a","MJfuel/tkm",{"$f":"IF(G10=\"n.a.\",0,VLOOKUP(G10,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D15,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 1"},"FT506a","MJfossil/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D16,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 1"},"FT507a","MJprim/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D17,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 1"},"FT508a","gCO2-eq/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D18,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 1"},"FT537a","gNOX/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D19,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 1"},"FT538a","gSOX/MJfuel",{"$f":"IF(G13=\"n.a.\",0,VLOOKUP(G13,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 2"]
[null,{"$f":"VLOOKUP($D21,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 2"},null,"FT501b","-",{"$f":"VLOOKUP(D21,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F21","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D22,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 2"},"FT502b","tkm/ha",null,{"$f":"'Production feedstock2'!G12*'Transport feedstock2'!G23/1000","v":0},"=FP503a*FT503b/1000"]
[null,null,{"$f":"VLOOKUP($D23,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 2"},"FT503b","km",{"$f":"VLOOKUP(D23,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F23=\"n.a.\",0,F23)","v":0}]
[null,null,{"$f":"VLOOKUP($D24,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 2"},"FT504b","-",{"$f":"VLOOKUP(D24,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F24","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D25,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 2"},"FT505b","MJfuel/tkm",{"$f":"IF(G21=\"n.a.\",0,VLOOKUP(G21,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D26,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 2"},"FT506b","MJfossil/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D27,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 2"},"FT507b","MJprim/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D28,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 2"},"FT508b","gCO2-eq/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D29,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 2"},"FT537b","gNOX/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D30,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 2"},"FT538b","gSOX/MJfuel",{"$f":"IF(G24=\"n.a.\",0,VLOOKUP(G24,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 3"]
[null,{"$f":"VLOOKUP($D32,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 3"},null,"FT501c","-",{"$f":"VLOOKUP(D32,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F32","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D33,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 3"},"FT502c","tkm/ha",null,{"$f":"'Production feedstock2'!G12*'Transport feedstock2'!G34/1000","v":0},"=FP503a*FT503c/1000"]
[null,null,{"$f":"VLOOKUP($D34,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 3"},"FT503c","km",{"$f":"VLOOKUP(D34,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F34=\"n.a.\",0,F34)","v":0}]
[null,null,{"$f":"VLOOKUP($D35,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 3"},"FT504c","-",{"$f":"VLOOKUP(D35,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F35","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D36,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 3"},"FT505c","MJfuel/tkm",{"$f":"IF(G32=\"n.a.\",0,VLOOKUP(G32,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D37,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 3"},"FT506c","MJfossil/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D38,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 3"},"FT507c","MJprim/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D39,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 3"},"FT508c","gCO2-eq/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D40,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 3"},"FT537c","gNOX/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D41,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 3"},"FT538c","gSOX/MJfuel",{"$f":"IF(G35=\"n.a.\",0,VLOOKUP(G35,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 4"]
[null,{"$f":"VLOOKUP($D43,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 4"},null,"FT501d","-",{"$f":"VLOOKUP(D43,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F43","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D44,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 4"},"FT502d","tkm/ha",null,{"$f":"'Conversion feedstock2'!G19*'Transport feedstock2'!G45/1000","v":0},"=BC514a*FT503d/1000"]
[null,null,{"$f":"VLOOKUP($D45,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 4"},"FT503d","km",{"$f":"VLOOKUP(D45,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F45=\"n.a.\",0,F45)","v":0}]
[null,null,{"$f":"VLOOKUP($D46,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 4"},"FT504d","-",{"$f":"VLOOKUP(D46,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F46","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D47,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 4"},"FT505d","MJfuel/tkm",{"$f":"IF(G43=\"n.a.\",0,VLOOKUP(G43,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D48,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 4"},"FT506d","MJfossil/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D49,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 4"},"FT507d","MJprim/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D50,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 4"},"FT508d","gCO2-eq/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D51,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 4"},"FT537d","gNOX/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D52,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 4"},"FT538d","gSOX/MJfuel",{"$f":"IF(G46=\"n.a.\",0,VLOOKUP(G46,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 5"]
[null,{"$f":"VLOOKUP($D54,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 5"},null,"FT501e","-",{"$f":"VLOOKUP(D54,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F54","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D55,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 5"},"FT502e","tkm/ha",null,{"$f":"'Conversion feedstock2'!G19*'Transport feedstock2'!G56/1000","v":0},"=BC514a*FT503e/1000"]
[null,null,{"$f":"VLOOKUP($D56,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 5"},"FT503e","km",{"$f":"VLOOKUP(D56,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F56=\"n.a.\",0,F56)","v":0}]
[null,null,{"$f":"VLOOKUP($D57,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 5"},"FT504e","-",{"$f":"VLOOKUP(D57,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F57","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D58,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 5"},"FT505e","MJfuel/tkm",{"$f":"IF(G54=\"n.a.\",0,VLOOKUP(G54,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D59,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 5"},"FT506e","MJfossil/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D60,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 5"},"FT507e","MJprim/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D61,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 5"},"FT508e","gCO2-eq/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D62,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 5"},"FT537e","gNOX/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D63,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 5"},"FT538e","gSOX/MJfuel",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 6"]
[null,{"$f":"VLOOKUP($D65,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 6"},null,"FT501f","-",{"$f":"VLOOKUP(D65,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F65","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D66,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 6"},"FT502f","tkm/ha",null,{"$f":"'Conversion feedstock2'!G19*'Transport feedstock2'!G67/1000","v":0},"=BC514a*FT503f/1000"]
[null,null,{"$f":"VLOOKUP($D67,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 6"},"FT503f","km",{"$f":"VLOOKUP(D67,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F67=\"n.a.\",0,F67)","v":0}]
[null,null,{"$f":"VLOOKUP($D68,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 6"},"FT504f","-",{"$f":"VLOOKUP(D68,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F68","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D69,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 6"},"FT505f","MJfuel/tkm",{"$f":"IF(G65=\"n.a.\",0,VLOOKUP(G65,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D70,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 6"},"FT506f","MJfossil/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D71,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 6"},"FT507f","MJprim/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D72,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 6"},"FT508f","gCO2-eq/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D73,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 6"},"FT537f","gNOX/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D74,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 6"},"FT538f","gSOX/MJfuel",{"$f":"IF(G68=\"n.a.\",0,VLOOKUP(G68,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 7"]
[null,{"$f":"VLOOKUP($D76,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 7"},null,"FT501g","-",{"$f":"VLOOKUP(D76,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F76","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D77,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 7"},"FT502g","tkm/ha",null,{"$f":"'Conversion feedstock2'!G174*'Transport feedstock2'!G78/1000","v":0},"=BC515a*FT503g/1000"]
[null,null,{"$f":"VLOOKUP($D78,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 7"},"FT503g","km",{"$f":"VLOOKUP(D78,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F78=\"n.a.\",0,F78)","v":0}]
[null,null,{"$f":"VLOOKUP($D79,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 7"},"FT504g","-",{"$f":"VLOOKUP(D79,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F79","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D80,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 7"},"FT505g","MJfuel/tkm",{"$f":"IF(G76=\"n.a.\",0,VLOOKUP(G76,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D81,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 7"},"FT506g","MJfossil/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D82,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 7"},"FT507g","MJprim/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D83,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 7"},"FT508g","gCO2-eq/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D84,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 7"},"FT537g","gNOX/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D85,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 7"},"FT538g","gSOX/MJfuel",{"$f":"IF(G79=\"n.a.\",0,VLOOKUP(G79,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 8"]
[null,{"$f":"VLOOKUP($D87,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 8"},null,"FT501h","-",{"$f":"VLOOKUP(D87,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F87","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D88,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 8"},"FT502h","tkm/ha",null,{"$f":"'Conversion feedstock2'!G174*'Transport feedstock2'!G89/1000","v":0},"=BC515a*FT503h/1000"]
[null,null,{"$f":"VLOOKUP($D89,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 8"},"FT503h","km",{"$f":"VLOOKUP(D89,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F89=\"n.a.\",0,F89)","v":0}]
[null,null,{"$f":"VLOOKUP($D90,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 8"},"FT504h","-",{"$f":"VLOOKUP(D90,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F90","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D91,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 8"},"FT505h","MJfuel/tkm",{"$f":"IF(G87=\"n.a.\",0,VLOOKUP(G87,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D92,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 8"},"FT506h","MJfossil/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D93,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 8"},"FT507h","MJprim/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D94,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 8"},"FT508h","gCO2-eq/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D95,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 8"},"FT537h","gNOX/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D96,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 8"},"FT538h","gSOX/MJfuel",{"$f":"IF(G90=\"n.a.\",0,VLOOKUP(G90,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
["Feedstock 1 - Transport 9"]
[null,{"$f":"VLOOKUP($D98,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Transport mode 9"},null,"FT501i","-",{"$f":"VLOOKUP(D98,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F98","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D99,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of transport mode 9"},"FT502i","tkm/ha",null,{"$f":"'Conversion feedstock2'!G174*'Transport feedstock2'!G100/1000","v":0},"=BC515a*FT503i/1000"]
[null,null,{"$f":"VLOOKUP($D100,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Distance of transport mode 9"},"FT503i","km",{"$f":"VLOOKUP(D100,Parameters!$1:$2804,6,FALSE)","v":0},{"$f":"IF(F100=\"n.a.\",0,F100)","v":0}]
[null,null,{"$f":"VLOOKUP($D101,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel used for transport mode 9"},"FT504i","-",{"$f":"VLOOKUP(D101,Parameters!$1:$2804,6,FALSE)","v":"n.a."},{"$f":"F101","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D102,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel used per tkm - transport mode 9"},"FT505i","MJfuel/tkm",{"$f":"IF(G98=\"n.a.\",0,VLOOKUP(G98,matrix_standardvalues_transportmodes,15,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D103,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy related to fuel use - transport mode 9"},"FT506i","MJfossil/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101, matrix_standardvalues_fuelsall,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D104,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy related to fuel use -  transport mode 9"},"FT507i","MJprim/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D105,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel use - transport mode 9"},"FT508i","gCO2-eq/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D106,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel - transport mode 9"},"FT537i","gNOX/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101,matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D107,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel - transport mode 9"},"FT538i","gSOX/MJfuel",{"$f":"IF(G101=\"n.a.\",0,VLOOKUP(G101,matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[]
["ENERGY BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Energy use for transport feedstock 1"]
[null,{"$f":"VLOOKUP($D111,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport 1 (mode 1-2-3)"},null,"FT512a","MJfossil/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G113+G115+G117)/'Conversion feedstock2'!G176)","v":0},"=(FT509a+FT509b+FT509c)/BC515c"]
[null,{"$f":"VLOOKUP($D112,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport 1 (mode 1-2-3)"},null,"FT512b","MJprim/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G114+G116+G118)/'Conversion feedstock2'!G176)","v":0},"=(FT510a+FT510b+FT510c)/BC515c"]
[null,null,{"$f":"VLOOKUP($D113,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 1"},"FT509a","MJfossil/ha",null,{"$f":"G11*G14*G15","v":0},"=FT502a*FT505a*FT506a"]
[null,null,{"$f":"VLOOKUP($D114,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 1"},"FT510a","MJprim/ha",null,{"$f":"G11*G14*G16","v":0},"=FT502a*FT505a*FT507a"]
[null,null,{"$f":"VLOOKUP($D115,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 2"},"FT509b","MJfossil/ha",null,{"$f":"G22*G25*G26","v":0},"=FT502b*FT505b*FT506b"]
[null,null,{"$f":"VLOOKUP($D116,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 2"},"FT510b","MJprim/ha",null,{"$f":"G22*G25*G27","v":0},"=FT502b*FT505b*FT507b"]
[null,null,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 3"},"FT509c","MJfossil/ha",null,{"$f":"G33*G36*G37","v":0},"=FT502c*FT505c*FT506c"]
[null,null,{"$f":"VLOOKUP($D118,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 3"},"FT510c","MJprim/ha",null,{"$f":"G33*G36*G38","v":0},"=FT502c*FT505c*FT507c"]
[null,{"$f":"VLOOKUP($D119,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport 2 (mode 4-5-6)"},null,"FT513a","MJfossil/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G121+G123+G125)/'Conversion feedstock2'!G176)","v":0},"=(FT509d+FT509e+FT509f)/BC515c"]
[null,{"$f":"VLOOKUP($D120,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport 2 (mode 4-5-6)"},null,"FT513b","MJprim/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G122+G124+G126)/'Conversion feedstock2'!G176)","v":0},"=(FT510d+FT510e+FT510f)/BC515c"]
[null,null,{"$f":"VLOOKUP($D121,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 4"},"FT509d","MJfossil/ha",null,{"$f":"G44*G47*G48","v":0},"=FT502d*FT505d*FT506d"]
[null,null,{"$f":"VLOOKUP($D122,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 4"},"FT510d","MJprim/ha",null,{"$f":"G44*G47*G49","v":0},"=FT502d*FT505d*FT507d"]
[null,null,{"$f":"VLOOKUP($D123,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 5"},"FT509e","MJfossil/ha",null,{"$f":"G55*G58*G59","v":0},"=FT502e*FT505e*FT506e"]
[null,null,{"$f":"VLOOKUP($D124,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 5"},"FT510e","MJprim/ha",null,{"$f":"G55*G58*G60","v":0},"=FT502e*FT505e*FT507e"]
[null,null,{"$f":"VLOOKUP($D125,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 6"},"FT509f","MJfossil/ha",null,{"$f":"G66*G69*G70","v":0},"=FT502f*FT505f*FT506f"]
[null,null,{"$f":"VLOOKUP($D126,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 6"},"FT510f","MJprim/ha",null,{"$f":"G66*G69*G71","v":0},"=FT502f*FT505f*FT507f"]
[null,{"$f":"VLOOKUP($D127,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport 3 (mode 7-8-9)"},null,"FT514a","MJfossil/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G129+G131+G133)/'Conversion feedstock2'!G176)","v":0},"=(FT509g+FT509h+FT509i)/BC515c"]
[null,{"$f":"VLOOKUP($D128,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport 3 (mode 7-8-9)"},null,"FT514b","MJprim/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G130+G132+G134)/'Conversion feedstock2'!G176)","v":0},"=(FT510g+FT510h+FT510i)/BC515c"]
[null,null,{"$f":"VLOOKUP($D129,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 7"},"FT509g","MJfossil/ha",null,{"$f":"G77*G80*G81","v":0},"=FT502g*FT505g*FT506g"]
[null,null,{"$f":"VLOOKUP($D130,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 7"},"FT510g","MJprim/ha",null,{"$f":"G77*G80*G82","v":0},"=FT502g*FT505g*FT507g"]
[null,null,{"$f":"VLOOKUP($D131,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 8"},"FT509h","MJfossil/ha",null,{"$f":"G88*G91*G92","v":0},"=FT502h*FT505h*FT506h"]
[null,null,{"$f":"VLOOKUP($D132,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 8"},"FT510h","MJprim/ha",null,{"$f":"G88*G91*G93","v":0},"=FT502h*FT505h*FT507h"]
[null,null,{"$f":"VLOOKUP($D133,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for transport mode 9"},"FT509i","MJfossil/ha",null,{"$f":"G99*G102*G103","v":0},"=FT502i*FT505i*FT506i"]
[null,null,{"$f":"VLOOKUP($D134,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for transport mode 9"},"FT510i","MJprim/ha",null,{"$f":"G99*G102*G104","v":0},"=FT502i*FT505i*FT507i"]
["Totally allocated energy use for transport"]
[null,{"$f":"VLOOKUP($D136,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 1"},null,"FT520a","MJfossil/MJendfuel_fs1",null,{"$f":"G111*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FT512a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D137,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 1"},null,"FT520b","MJprim/MJendfuel_fs1",null,{"$f":"G112*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FT512b * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D138,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 1"},null,"FT521a","MJfossil/MJFU",null,{"$f":"G111*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT512a * BC050a / 100 * BC050b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D139,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 1"},null,"FT521b","MJprim/MJFU",null,{"$f":"G112*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT512b * BC050a / 100 * BC050b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D140,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 2"},null,"FT522a","MJfossil/MJendfuel_fs1",null,{"$f":"G119*'Conversion feedstock2'!G256/100","v":0},"= FT513a * BC050b / 100"]
[null,{"$f":"VLOOKUP($D141,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 2"},null,"FT522b","MJprim/MJendfuel_fs1",null,{"$f":"G120*'Conversion feedstock2'!G256/100","v":0},"= FT513b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D142,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 2"},null,"FT523a","MJfossil/MJFU",null,{"$f":"G119*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT513a * BC050b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D143,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 2"},null,"FT523b","MJprim/MJFU",null,{"$f":"G120*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT513b * BC050b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D144,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 3"},null,"FT524a","MJfossil/MJendfuel_fs1",null,{"$f":"G127","v":0},"= FT514a"]
[null,{"$f":"VLOOKUP($D145,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 3"},null,"FT524b","MJprim/MJendfuel_fs1",null,{"$f":"G128","v":0},"= FT514b"]
[null,{"$f":"VLOOKUP($D146,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in transport 3"},null,"FT525a","MJfossil/MJFU",null,{"$f":"G127*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT514a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D147,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in transport 3"},null,"FT525b","MJprim/MJFU",null,{"$f":"G128*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT514b * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D148,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in total transport (1-3)"},null,"FT526a","MJfossil/MJendfuel_fs1",null,{"$f":"G136+G140+G144","v":0},"= FT520a + FT522a + FT524a"]
[null,{"$f":"VLOOKUP($D149,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in total transport (1-3)"},null,"FT526b","MJprim/MJendfuel_fs1",null,{"$f":"G137+G141+G145","v":0},"= FT520b + FT522b + FT524b"]
[null,{"$f":"VLOOKUP($D150,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in total transport (1-3)"},null,"FT527a","MJfossil/MJFU",null,{"$f":"G138+G142+G146","v":0},"= FT521a + FT523a + FT525a"]
[null,{"$f":"VLOOKUP($D151,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in total transport (1-3)"},null,"FT527b","MJprim/MJFU",null,{"$f":"G139+G143+G147","v":0},"= FT521b + FT523b + FT525b"]
[]
["GLOBAL WARMING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["GHG emissions from transport feedstock 1"]
[null,{"$f":"VLOOKUP($D155,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with transport 1 (mode 1-2-3)"},null,"FT515a","gCO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G156+G157+G158)/'Conversion feedstock2'!G176)","v":0},"=(FT511a+FT511b+FT511c)/BC515c"]
[null,null,{"$f":"VLOOKUP($D156,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 1"},"FT511a","gCO2-eq/ha",null,{"$f":"G11*G14*G17","v":0},"=FT502a*FT505a*FT508a"]
[null,null,{"$f":"VLOOKUP($D157,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 2"},"FT511b","gCO2-eq/ha",null,{"$f":"G22*G25*G28","v":0},"=FT502b*FT505b*FT508b"]
[null,null,{"$f":"VLOOKUP($D158,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 3"},"FT511c","gCO2-eq/ha",null,{"$f":"G33*G36*G39","v":0},"=FT502c*FT505c*FT508c"]
[null,{"$f":"VLOOKUP($D159,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with transport 2 (mode 4-5-6)"},null,"FT515b","gCO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G160+G161+G162)/'Conversion feedstock2'!G176)","v":0},"=(FT511d+FT511e+FT511f)/BC515c"]
[null,null,{"$f":"VLOOKUP($D160,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 4"},"FT511d","gCO2-eq/ha",null,{"$f":"G44*G47*G50","v":0},"=FT502d*FT505d*FT508d"]
[null,null,{"$f":"VLOOKUP($D161,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 5"},"FT511e","gCO2-eq/ha",null,{"$f":"G55*G58*G61","v":0},"=FT502e*FT505e*FT508e"]
[null,null,{"$f":"VLOOKUP($D162,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 6"},"FT511f","gCO2-eq/ha",null,{"$f":"G66*G69*G72","v":0},"=FT502f*FT505f*FT508f"]
[null,{"$f":"VLOOKUP($D163,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with transport 3 (mode 7-8-9)"},null,"FT515c","gCO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G164+G165+G166)/'Conversion feedstock2'!G176)","v":0},"=(FT511g+FT511h+FT511i)/BC515c"]
[null,null,{"$f":"VLOOKUP($D164,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 7"},"FT511g","gCO2-eq/ha",null,{"$f":"G77*G80*G83","v":0},"=FT502g*FT505g*FT508g"]
[null,null,{"$f":"VLOOKUP($D165,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 8"},"FT511h","gCO2-eq/ha",null,{"$f":"G88*G91*G94","v":0},"=FT502h*FT505h*FT508h"]
[null,null,{"$f":"VLOOKUP($D166,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of fuel used in transport mode 9"},"FT511i","gCO2-eq/ha",null,{"$f":"G99*G102*G105","v":0},"=FT502i*FT505i*FT508i"]
["Totally allocated GHG emissions from transport"]
[null,{"$f":"VLOOKUP($D168,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 1"},null,"FT530a","gCO2_eq/MJendfuel_fs2",null,{"$f":"G155*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FT515a * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D169,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 1"},null,"FT530b","gCO2_eq/MJFU",null,{"$f":"G155*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT515a * BC550a / 100 * BC550b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D170,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 2"},null,"FT531a","gCO2_eq/MJendfuel_fs2",null,{"$f":"G159*'Conversion feedstock2'!G256/100","v":0},"= FT515b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D171,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 2"},null,"FT531b","gCO2_eq/MJFU",null,{"$f":"G159*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT515b * BC550b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D172,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 3"},null,"FT532a","gCO2_eq/MJendfuel_fs2",null,{"$f":"G163","v":0},"= FT515c"]
[null,{"$f":"VLOOKUP($D173,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from transport 3"},null,"FT532b","gCO2_eq/MJFU",null,{"$f":"G163*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT515c * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D174,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from total transport (1-3)"},null,"FT533a","gCO2_eq/MJendfuel_fs2",null,{"$f":"G168+G170+G172","v":0},"= FT530a + FT531a + FT532a"]
[null,{"$f":"VLOOKUP($D175,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from total transport (1-3)"},null,"FT533b","gCO2_eq/MJFU",null,{"$f":"G169+G171+G173","v":0},"= FT530b + FT531b + FT532b"]
[]
["RESOURCE USE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["USE OF WATER"]
[null,"N.A."]
["USE OF LAND"]
[null,"N.A."]
[]
["ENVIRONMENTAL QUALITY",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["ACIDIFICATION POTENTIAL"]
["Acidification potential from transport feedstock 1"]
[null,{"$f":"VLOOKUP($D186,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with transport 1 (mode 1-2-3)"},null,"FT516a","gSO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G187+G188+G189)/'Conversion feedstock2'!G176)","v":0},"=(FT535a+FT535b+FT535c)/BC515c"]
[null,null,{"$f":"VLOOKUP($D187,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 1"},"FT535a","gSO2-eq/ha",null,{"$f":"G11*G14*G18*'Production feedstock2'!G274+G11*G14*G19*'Production feedstock2'!G275","v":0},"=FT502a*FT505a*FT537a*FP610b+FT502a*FT505a*FT538a*FP610c"]
[null,null,{"$f":"VLOOKUP($D188,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 2"},"FT535b","gSO2-eq/ha",null,{"$f":"G22*G25*G29*'Production feedstock2'!G274+G22*G25*G30*'Production feedstock2'!G275","v":0},"=FT502b*FT505b*FT537b*FP610b+FT502b*FT505b*FT538b*FP610c"]
[null,null,{"$f":"VLOOKUP($D189,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 3"},"FT535c","gSO2-eq/ha",null,{"$f":"G33*G36*G40*'Production feedstock2'!G274+G33*G36*G41*'Production feedstock2'!G275","v":0},"=FT502c*FT505c*FT537c*FP610b+FT502c*FT505c*FT538c*FP610c"]
[null,{"$f":"VLOOKUP($D190,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with transport 2 (mode 4-5-6)"},null,"FT516b","gSO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G191+G192+G193)/'Conversion feedstock2'!G176)","v":0},"=(FT535d+FT535e+FT535f)/BC515c"]
[null,null,{"$f":"VLOOKUP($D191,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 4"},"FT535d","gSO2-eq/ha",null,{"$f":"G44*G47*G51*'Production feedstock2'!G274+G44*G47*G52*'Production feedstock2'!G275","v":0},"=FT502d*FT505d*FT537d*FP610b+FT502d*FT505d*FT538d*FP610c"]
[null,null,{"$f":"VLOOKUP($D192,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 5"},"FT535e","gSO2-eq/ha",null,{"$f":"G55*G58*G62*'Production feedstock2'!G274+G55*G58*G63*'Production feedstock2'!G275","v":0},"=FT502e*FT505e*FT537e*FP610b+FT502e*FT505e*FT538e*FP610c"]
[null,null,{"$f":"VLOOKUP($D193,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 6"},"FT535f","gSO2-eq/ha",null,{"$f":"G66*G69*G73*'Production feedstock2'!G274+G66*G69*G74*'Production feedstock2'!G275","v":0},"=FT502f*FT505f*FT537f*FP610b+FT502f*FT505f*FT538f*FP610c"]
[null,{"$f":"VLOOKUP($D194,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with transport 3 (mode 7-8-9)"},null,"FT516c","gSO2_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G195+G196+G197)/'Conversion feedstock2'!G176)","v":0},"=(FT535g+FT535h+FT535i)/BC515c"]
[null,null,{"$f":"VLOOKUP($D195,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 7"},"FT535g","gSO2-eq/ha",null,{"$f":"G77*G80*G84*'Production feedstock2'!G274+G77*G80*G85*'Production feedstock2'!G275","v":0},"=FT502g*FT505g*FT537g*FP610b+FT502g*FT505g*FT538g*FP610c"]
[null,null,{"$f":"VLOOKUP($D196,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 8"},"FT535h","gSO2-eq/ha",null,{"$f":"G88*G91*G95*'Production feedstock2'!G274+G88*G91*G96*'Production feedstock2'!G275","v":0},"=FT502h*FT505h*FT537h*FP610b+FT502h*FT505h*FT538h*FP610c"]
[null,null,{"$f":"VLOOKUP($D197,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel used in transport mode 9"},"FT535i","gSO2-eq/ha",null,{"$f":"G99*G102*G106*'Production feedstock2'!G274+G99*G102*G107*'Production feedstock2'!G275","v":0},"=FT502i*FT505i*FT537i*FP610b+FT502i*FT505i*FT538i*FP610c"]
["Totally allocated acidification potential from transport"]
[null,{"$f":"VLOOKUP($D199,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 1"},null,"FT540a","gSO2_eq/MJendfuel_fs2",null,{"$f":"G186*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FT516a * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D200,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 1"},null,"FT540b","gSO2_eq/MJFU",null,{"$f":"G199*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT540a * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D201,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 2"},null,"FT541a","gSO2_eq/MJendfuel_fs2",null,{"$f":"G190*'Conversion feedstock2'!G256/100","v":0},"= FT516b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D202,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 2"},null,"FT541b","gSO2_eq/MJFU",null,{"$f":"G201*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT541a * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D203,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 3"},null,"FT542a","gSO2_eq/MJendfuel_fs2",null,{"$f":"G194","v":0},"= FT516c"]
[null,{"$f":"VLOOKUP($D204,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from transport 3"},null,"FT542b","gSO2_eq/MJFU",null,{"$f":"G203*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT542a * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D205,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from total transport (1-3)"},null,"FT543a","gSO2_eq/MJendfuel_fs2",null,{"$f":"G199+G201+G203","v":0},"= FT540a + FT541a + FT542a"]
[null,{"$f":"VLOOKUP($D206,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from total transport (1-3)"},null,"FT543b","gSO2_eq/MJFU",null,{"$f":"G200+G202+G204","v":0},"= FT540b + FT541b + FT542b"]
["EUTROPHICATION POTENTIAL"]
["Eutrophication potential from transport feedstock 1"]
[null,{"$f":"VLOOKUP($D209,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with transport 1 (mode 1-2-3)"},null,"FT517a","gPO4_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G210+G211+G212)/'Conversion feedstock2'!G176)","v":0},"=(FT536a+FT536b+FT536c)/BC515c"]
[null,null,{"$f":"VLOOKUP($D210,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 1"},"FT536a","gPO4-eq/ha",null,{"$f":"G11*G14*G18*'Production feedstock2'!G289","v":0},"=FT502a*FT505a*FT537a*FP620b"]
[null,null,{"$f":"VLOOKUP($D211,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 2"},"FT536b","gPO4-eq/ha",null,{"$f":"G22*G25*G29*'Production feedstock2'!G289","v":0},"=FT502b*FT505b*FT537b*FP620b"]
[null,null,{"$f":"VLOOKUP($D212,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 3"},"FT536c","gPO4-eq/ha",null,{"$f":"G33*G36*G40*'Production feedstock2'!G289","v":0},"=FT502c*FT505c*FT537c*FP620b"]
[null,{"$f":"VLOOKUP($D213,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with transport 2 (mode 4-5-6)"},null,"FT517b","gPO4_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G214+G215+G216)/'Conversion feedstock2'!G176)","v":0},"=(FT536d+FT536e+FT536f)/BC515c"]
[null,null,{"$f":"VLOOKUP($D214,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 4"},"FT536d","gPO4-eq/ha",null,{"$f":"G44*G47*G51*'Production feedstock2'!G289","v":0},"=FT502d*FT505d*FT537d*FP620b"]
[null,null,{"$f":"VLOOKUP($D215,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 5"},"FT536e","gPO4-eq/ha",null,{"$f":"G55*G58*G62*'Production feedstock2'!G289","v":0},"=FT502e*FT505e*FT537e*FP620b"]
[null,null,{"$f":"VLOOKUP($D216,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 6"},"FT536f","gPO4-eq/ha",null,{"$f":"G66*G69*G73*'Production feedstock2'!G289","v":0},"=FT502f*FT505f*FT537f*FP620b"]
[null,{"$f":"VLOOKUP($D217,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with transport 3 (mode 7-8-9)"},null,"FT517c","gPO4_eq/MJendfuel_fs2",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,(G218+G219+G220)/'Conversion feedstock2'!G176)","v":0},"=(FT536g+FT536h+FT536i)/BC515c"]
[null,null,{"$f":"VLOOKUP($D218,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 7"},"FT536g","gPO4-eq/ha",null,{"$f":"G77*G80*G84*'Production feedstock2'!G289","v":0},"=FT502g*FT505g*FT537g*FP620b"]
[null,null,{"$f":"VLOOKUP($D219,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 8"},"FT536h","gPO4-eq/ha",null,{"$f":"G88*G91*G95*'Production feedstock2'!G289","v":0},"=FT502h*FT505h*FT537h*FP620b"]
[null,null,{"$f":"VLOOKUP($D220,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel used in transport mode 9"},"FT536i","gPO4-eq/ha",null,{"$f":"G99*G102*G106*'Production feedstock2'!G289","v":0},"=FT502i*FT505i*FT537i*FP620b"]
["Totally allocated eutrophication potential from transport"]
[null,{"$f":"VLOOKUP($D222,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 1"},null,"FT544a","gPO4_eq/MJendfuel_fs2",null,{"$f":"G209*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= FT517a * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D223,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 1"},null,"FT544b","gPO4_eq/MJFU",null,{"$f":"G222*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT544a * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D224,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 2"},null,"FT545a","gPO4_eq/MJendfuel_fs2",null,{"$f":"G213*'Conversion feedstock2'!G256/100","v":0},"= FT517b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D225,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 2"},null,"FT545b","gPO4_eq/MJFU",null,{"$f":"G224*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= FT545a * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D226,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 3"},null,"FT546a","gPO4_eq/MJendfuel_fs2",null,{"$f":"G217","v":0},"= FT517c"]
[null,{"$f":"VLOOKUP($D227,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from transport 3"},null,"FT546b","gPO4_eq/MJFU",null,{"$f":"G226*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= FT546a * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D228,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from total transport (1-3)"},null,"FT547a","gPO4_eq/MJendfuel_fs2",null,{"$f":"G222+G224+G226","v":0},"= FT544a + FT545a + FT546a"]
[null,{"$f":"VLOOKUP($D229,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from total transport (1-3)"},null,"FT547b","gPO4_eq/MJFU",null,{"$f":"G223+G225+G227","v":0},"= FT544b + FT545b + FT546b"]
[]
["BIODIVERSITY & HIGH CARBON STOCK",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Land with high biodiversity value"]
[null,"N.A."]
["Land with high carbon stock"]
[null,"N.A."]
["Criterium RED"]
[null,"N.A."]

{"sheet":"Conversion feedstock1","index":22,"n_rows":556,"n_cols":8,"rows_kept":556,"cut":false,"hidden":true,"merged":[]}
["Monitoring framework - Conversion feedstock 1 (per year)"]
[]
[null,null,"From input"]
[null,null,"Standard value"]
[null,null,"Calculated from other fields"]
[null,null,"Determines value in other field"]
[]
["MASS BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Feedstock 1 - Conversion process 1",null,null,"BC000a","-",{"$f":"VLOOKUP(D9,Parameters!$1:$2792,6,FALSE)","v":"Oil extraction"},{"$f":"F9","v":"Oil extraction"}]
[null,"Main input flow of process 1"]
[null,null,{"$f":"VLOOKUP($D11,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Pretreated feedstock"},"FP047","-",{"$f":"VLOOKUP(D11,Parameters!$1:$2792,6,FALSE)","v":"Fresh palm fruit bunches (FFB)"},{"$f":"F11","v":"Fresh palm fruit bunches (FFB)"}]
[null,null,{"$f":"VLOOKUP($D12,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content pretreated feedstock"},"FP048","%"]
[null,null,{"$f":"VLOOKUP($D13,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content pretreated feedstock (LHV)"},"FP049","MJ/kgdm",{"$f":"VLOOKUP(F11,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":24},{"$f":"F13","v":24}]
[null,"Main output flow of process 1"]
[null,null,{"$f":"VLOOKUP($D15,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of main output flow, process 1"},"BC001a","-",{"$f":"VLOOKUP(D15,Parameters!$1:$2792,6,FALSE)","v":"Crude palm oil"},{"$f":"F15","v":"Crude palm oil"}]
[null,null,{"$f":"VLOOKUP($D16,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of main output flow, process 1"},"BC012a","%",{"$f":"VLOOKUP(D16,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F16","v":0}]
[null,null,{"$f":"VLOOKUP($D17,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of main output flow, process 1 (LHV)"},"BC007a","MJ/kgdm",{"$f":"IF(G15=\"n.a.\",0,VLOOKUP(G15,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},{"$f":"F17","v":37}]
[null,{"$f":"VLOOKUP($D18,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate (output/input), process 1"},null,"BC008a","MJoutput /MJinput",{"$f":"VLOOKUP(D18,Parameters!$1:$2792,6,FALSE)","v":0.52999401737774465},{"$f":"F18","v":0.52999401737774465}]
[null,null,{"$f":"VLOOKUP($D19,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 1 per ha after conversion process 1"},"BC014a","kg/ha",null,{"$f":"G20*100/(100-G16)","v":4224.7799859623219},"= BC014b * 100 / (100-BC012a)"]
[null,null,{"$f":"VLOOKUP($D20,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (dry) of feedstock 1 per ha after conversion process 1"},"BC014b","kgdm/ha",null,{"$f":"IF(G17=0,0,G21/G17)","v":4224.7799859623219},"= BC014c / BC007a"]
[null,null,{"$f":"VLOOKUP($D21,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of feedstock 1 per ha after conversion process 1"},"BC014c","MJ/ha",null,{"$f":"'Production feedstock1'!G71*'Conversion feedstock1'!G18","v":156316.8594806059},"= FP055c * BC008a"]
[null,"Net electricity input process 1"]
[null,1,{"$f":"VLOOKUP($D23,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of electricity input 1, process 1"},"BC026a","MJe/MJoutput",{"$f":"VLOOKUP(D23,Parameters!$1:2792,6,FALSE)","v":0},{"$f":"IF(F23=\"n.a.\",0,F23)","v":0}]
[null,null,{"$f":"VLOOKUP($D24,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity flow 1, process 1"},"BC026a0","MWh/year",{"$f":"VLOOKUP(D24,Parameters!$1:2792,6,FALSE)","v":0},{"$f":"F24","v":0}]
[null,null,{"$f":"VLOOKUP($D25,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of electricity flow 1, process 1"},"BC027a","-",{"$f":"VLOOKUP(D25,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F25","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D26,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 1, process 1"},"BC028a","MJfossil/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D27,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production flow 1, process 1"},"BC029a","MJprim/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D28,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 1, process 1"},"BC042a","gCO2eq/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D29,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity flow 1, process 1"},"BC112a","gNOX/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D30,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity flow 1, process 1"},"BC113a","gSOX/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D31,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of electricity input 2, process 1"},"BC026a1","MJe/MJoutput",{"$f":"VLOOKUP(D31,Parameters!$1:2799,6,FALSE)","v":0},{"$f":"F31","v":0}]
[null,null,{"$f":"VLOOKUP($D32,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity flow 2, process 1"},"BC026a10","MWh/year",{"$f":"VLOOKUP(D32,Parameters!$1:2800,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D33,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of electricity flow 2, process 1"},"BC027a1","-",{"$f":"VLOOKUP(D33,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D34,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 2, process 1"},"BC028a1","MJfossil/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D35,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production flow 2, process 1"},"BC029a1","MJprim/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D36,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 2, process 1"},"BC042a1","gCO2eq/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D37,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity flow 2, process 1"},"BC112a1","gNOX/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D38,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity flow 2, process 1"},"BC113a1","gSOX/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,"Fuel / heat input"]
[null,1,{"$f":"VLOOKUP($D40,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 1, process 1"},"BC011a1","-",{"$f":"VLOOKUP(D40,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F40","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D41,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat input 1, process 1"},"BC031a1","MJf_h/MJoutput",{"$f":"VLOOKUP(D41,Parameters!$1:2792,6,FALSE)","v":0},{"$f":"IF(F41=\"n.a.\",0,F41)","v":0}]
[null,null,{"$f":"VLOOKUP($D42,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fuel/heat flow 1, process 1"},"BC031a10","MJ/year",{"$f":"VLOOKUP(D42,Parameters!$1:2809,6,FALSE)","v":0},{"$f":"F42","v":0}]
[null,null,{"$f":"VLOOKUP($D43,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, process 1"},"BC032a1","MJfossil/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F43","v":0}]
[null,null,{"$f":"VLOOKUP($D44,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, process 1"},"BC033a1","MJprim/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D45,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, process 1"},"BC043a1","gCO2_eq/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D46,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 1, process 1"},"BC115a","gNOX/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D47,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 1, process 1"},"BC116a","gSOX/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D48,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 2, process 1"},"BC011a2","-",{"$f":"VLOOKUP(D48,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D49,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat input 2, process 1"},"BC031a2","MJf_h/MJoutput",{"$f":"VLOOKUP(D49,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F49=\"n.a.\",0,F49)","v":0}]
[null,null,{"$f":"VLOOKUP($D50,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fuel/heat flow 2, process 1"},"BC031a20","MJ/year",{"$f":"VLOOKUP(D50,Parameters!$1:2817,6,FALSE)","v":0},{"$f":"F50","v":0}]
[null,null,{"$f":"VLOOKUP($D51,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, process 1"},"BC032a2","MJfossil/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F51","v":0}]
[null,null,{"$f":"VLOOKUP($D52,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, process 1"},"BC033a2","MJprim/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,21,FALSE))","v":0},{"$f":"F52","v":0}]
[null,null,{"$f":"VLOOKUP($D53,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, process 1"},"BC043a2","gCO2_eq/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,9,FALSE))","v":0},{"$f":"F53","v":0}]
[null,null,{"$f":"VLOOKUP($D54,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 2, process 1"},"BC117a","gNOX/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,27,FALSE))","v":0},{"$f":"F54","v":0}]
[null,null,{"$f":"VLOOKUP($D55,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 2, process 1"},"BC118a","gSOX/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,29,FALSE))","v":0},{"$f":"F55","v":0}]
[null,"Other material input flows"]
[null,null,{"$f":"VLOOKUP($D57,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of main input, process 1"},"BC009a0","-",{"$f":"VLOOKUP(D57,Parameters!$1:$2792,6,FALSE)","v":"Fresh palm fruit bunches (FFB)"},{"$f":"F57","v":"Fresh palm fruit bunches (FFB)"}]
[null,null,{"$f":"VLOOKUP($D58,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Main input, process 1"},"BC010a0","kg/year",{"$f":"VLOOKUP(D58,Parameters!$1:$2792,6,FALSE)","v":19000},19000]
[null,null,{"$f":"VLOOKUP($D59,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of main input, process 1"},"BC010a","kgdm/MJoutput",{"$f":"VLOOKUP(D59,Parameters!$1:2789,6,FALSE)","v":7.8617238875928711E-2},7.8617238875928711E-2]
[null,null,{"$f":"VLOOKUP($D60,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for main input, process 1"},"BC036a0","MJprim/kgdm",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues,20,FALSE))","v":0},0]
[null,1,{"$f":"VLOOKUP($D61,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 1, process 1"},"BC009a1","-",{"$f":"VLOOKUP(D61,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D62,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material input flow 1, process 1"},"BC010a01","kg/year",{"$f":"VLOOKUP(D62,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D63,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 1, process 1"},"BC010a1","kgdm/MJoutput",{"$f":"VLOOKUP(D63,Parameters!$1:2792,6,FALSE)","v":0},{"$f":"IF(F63=\"n.a.\",0,F63)","v":0}]
[null,null,{"$f":"VLOOKUP($D64,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 1, process 1"},"BC010a10","%",{"$f":"VLOOKUP(D64,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F64=\"n.a.\", 0, F64)","v":0}]
[null,null,{"$f":"VLOOKUP($D65,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 1, process 1"},"BC010a11","MJ/kgdm",{"$f":"VLOOKUP(D65,Parameters!$1:2781,6,FALSE)","v":0},{"$f":"F65","v":0}]
[null,null,{"$f":"VLOOKUP($D66,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 1, process 1"},"BC035a1","MJfossil/kgdm",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,10,FALSE))","v":0},{"$f":"F66","v":0}]
[null,null,{"$f":"VLOOKUP($D67,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 1, process 1"},"BC036a1","MJprim/kgdm",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D68,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, process 1"},"BC047a1","gCO2_eq/kgdm",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D69,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 1, process 1"},"BC120a","gNOX/kgdm",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D70,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 1, process 1"},"BC121a","gSOX/kgdm",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,28,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D71,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 2, process 1"},"BC009a2","-",{"$f":"VLOOKUP(D71,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,"Material input flow 2, process 1","BC010a02","kg/year",{"$f":"VLOOKUP(D72,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F72","v":0}]
[null,null,{"$f":"VLOOKUP($D73,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 2, process 1"},"BC010a2","kgdm/MJoutput",{"$f":"VLOOKUP(D73,Parameters!$1:2792,6,FALSE)","v":0},{"$f":"IF(F73=\"n.a.\",0,F73)","v":0}]
[null,null,{"$f":"VLOOKUP($D74,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 2, process 1"},"BC010a20","%",{"$f":"VLOOKUP(D74,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F74=\"n.a.\", 0, F74)","v":0}]
[null,null,{"$f":"VLOOKUP($D75,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 2, process 1"},"BC010a21","MJ/kgdm",{"$f":"VLOOKUP(D75,Parameters!$1:2791,6,FALSE)","v":0},{"$f":"F75","v":0}]
[null,null,{"$f":"VLOOKUP($D76,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 2, process 1"},"BC035a2","MJfossil/kgdm",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,10,FALSE))","v":0},{"$f":"F76","v":0}]
[null,null,{"$f":"VLOOKUP($D77,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 2, process 1"},"BC036a2","MJprim/kgdm",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D78,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, process 1"},"BC047a2","gCO2_eq/kgdm",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D79,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 2, process 1"},"BC122a","gNOX/kgdm",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D80,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 2, process 1"},"BC123a","gSOX/kgdm",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,28,FALSE))","v":0},0]
[null,3,{"$f":"VLOOKUP($D81,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 3, process 1"},"BC009a3","-",{"$f":"VLOOKUP(D81,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,"Material input flow 3, process 1","BC010a03","kg/year",{"$f":"VLOOKUP(D82,Parameters!$1:2799,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D83,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 3, process 1"},"BC010a3","kgdm/MJoutput",{"$f":"VLOOKUP(D83,Parameters!$1:2800,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D84,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 3, process 1"},"BC010a30","%",{"$f":"VLOOKUP(D84,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F84=\"n.a.\", 0, F84)","v":0}]
[null,null,{"$f":"VLOOKUP($D85,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 3, process 1"},"BC010a31","MJ/kgdm",{"$f":"VLOOKUP(D85,Parameters!$1:2801,6,FALSE)","v":0},{"$f":"F85","v":0}]
[null,null,{"$f":"VLOOKUP($D86,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 3, process 1"},"BC035a3","MJfossil/kgdm",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,10,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D87,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 3, process 1"},"BC036a3","MJprim/kgdm",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D88,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 3, process 1"},"BC047a3","gCO2_eq/kgdm",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D89,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 3, process 1"},"BC125a","gNOX/kgdm",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D90,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 3, process 1"},"BC126a","gSOX/kgdm",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,28,FALSE))","v":0},0]
[null,"Material output flow"]
[null,null,{"$f":"VLOOKUP($D92,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material output flow, process 1"},"BC009c","-",{"$f":"VLOOKUP(D92,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F92","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D93,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 1"},"BC010c","kgdm/MJoutput",{"$f":"VLOOKUP(D93,Parameters!$1:2807,6,FALSE)","v":2.6636946173917474E-3},{"$f":"IF(F93=\"n.a.\",0,F93)","v":2.6636946173917474E-3}]
[null,null,{"$f":"VLOOKUP($D94,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material output flow, process 1"},"BC010c0","kg/year",{"$f":"VLOOKUP(D94,Parameters!$1:2808,6,FALSE)","v":4311},{"$f":"F94","v":4311}]
[null,null,{"$f":"VLOOKUP($D95,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material output flow, process 1"},"BC035c","MJfossil/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,10,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D96,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material output flow, process 1"},"BC036c","MJprim/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D97,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material output flow, process 1"},"BC047c","gCO2_eq/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D98,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material output flow, process 1"},"BC120c","gNOX/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D99,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material output flow, process 1"},"BC121c","gSOX/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,28,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D100,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of output flow, process 1 (electricity)"},"BC009c1","-",{"$f":"VLOOKUP(D100,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F100","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D101,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 1 (Electricity)"},"BC010c1","MJe/MJoutput",{"$f":"VLOOKUP(D101,Parameters!$1:2814,6,FALSE)","v":0},{"$f":"IF(F101=\"n.a.\",0,F101)","v":0}]
[null,null,{"$f":"VLOOKUP($D102,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for  output flow, process 1 (electricity)"},"BC035c1","MJfossil/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,11,FALSE))","v":0},{"$f":"F102","v":0}]
[null,null,{"$f":"VLOOKUP($D103,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for  output flow, process 1 (electricity)"},"BC036c1","MJprim/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D104,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to  output flow, process 1 (electricity)"},"BC047c1","gCO2eq/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D105,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of output flow, process 1 (electricity)"},"BC120c1","gNOX/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D106,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of output flow, process 1 (electricity)"},"BC121c1","gSOX/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D107,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of output flow, process 1 (heat)"},"BC009c2","-",{"$f":"VLOOKUP(D107,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F107","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D108,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 1 (Heat)"},"BC010c2","MJf_h/MJoutput",{"$f":"VLOOKUP(D108,Parameters!$1:2815,6,FALSE)","v":0},{"$f":"IF(F108=\"n.a.\",0,F108)","v":0}]
[null,null,{"$f":"VLOOKUP($D109,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for  output flow, process 1 (heat)"},"BC035c2","MJfossil/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F109","v":0}]
[null,null,{"$f":"VLOOKUP($D110,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for  output flow, process 1 (heat)"},"BC036c2","MJprim/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D111,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to  output flow, process 1 (heat)"},"BC047c2","gCO2_eq/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D112,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of output flow, process 1 (heat)"},"BC120c2","gNOX/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D113,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of output flow, process 1 (heat)"},"BC121c2","gSOX/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[null,"By-products"]
[null,null,{"$f":"VLOOKUP($D115,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to energy crop, process 1"},"BC050a","%",null,{"$f":"100-G116","v":95.667889264109959},"= 1 - BC022a"]
[null,null,{"$f":"VLOOKUP($D116,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-products, process 1"},"BC022a","%",null,{"$f":"G124+G132+G140","v":4.3321107358900459},"= BC051a1 + BC051a2+BC051a3"]
[null,1,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 1, process 1"},"BC002a1","-",{"$f":"VLOOKUP(D117,Parameters!$1:2792,6,FALSE)","v":"Palm kernel meal"},{"$f":"F117","v":"Palm kernel meal"}]
[null,null,{"$f":"VLOOKUP($D118,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 1, process 1"},"BC002a10","%",{"$f":"VLOOKUP(D118,Parameters!$1:$2792,6,FALSE)","v":8.1999999999999993},{"$f":"IF(F118=\"n.a.\", 0, F118)","v":8.1999999999999993}]
[null,null,{"$f":"VLOOKUP($D119,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 1, process 1"},"BC002a11","kg/year",{"$f":"VLOOKUP(D119,Parameters!$1:2819,6,FALSE)","v":462.83},{"$f":"F119","v":462.83}]
[null,null,{"$f":"VLOOKUP($D120,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (kg)"},"BC003a1","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D121,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (MJ)"},"BC004a1","MJbyproduct /MJinput",{"$f":"VLOOKUP(D121,Parameters!$1:$2792,6,FALSE)","v":2.399961774322297E-2},{"$f":"IF(F121=\"n.a.\", 0, F121)","v":2.399961774322297E-2}]
[null,null,{"$f":"VLOOKUP($D122,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 1, process 1 (LHV)"},"BC005a1","MJ/kgdm",{"$f":"IF(G117=\"n.a.\",0,VLOOKUP(G117, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":17},{"$f":"F122","v":17}]
[null,null,{"$f":"VLOOKUP($D123,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 1, process 1"},"BC006a1","binary",{"$f":"IF(G117=\"n.a.\",0,VLOOKUP(G117,matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":1},{"$f":"IF(F123=\"n.a.\", 0, F123)","v":1}]
[null,null,{"$f":"VLOOKUP($D124,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 1, process 1"},"BC051a1","%",null,{"$f":"IF(G123=1,G121/(G121+G129+G137+G142+G146+G18)*100,0)","v":4.3321107358900459},"= BC004a1/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
[null,2,{"$f":"VLOOKUP($D125,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 2, process 1"},"BC002a2","-",{"$f":"VLOOKUP(D125,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F125","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D126,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 2, process 1"},"BC002a20","%",{"$f":"VLOOKUP(D126,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F126=\"n.a.\", 0, F126)","v":0}]
[null,null,{"$f":"VLOOKUP($D127,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 2, process 1"},"BC002a21","kg/year",{"$f":"VLOOKUP(D127,Parameters!$1:2828,6,FALSE)","v":0},{"$f":"F127","v":0}]
[null,null,{"$f":"VLOOKUP($D128,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (kg)"},"BC003a2","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D129,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (MJ)"},"BC004a2","MJbyproduct /MJinput",{"$f":"VLOOKUP(D129,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F129=\"n.a.\", 0, F129)","v":0}]
[null,null,{"$f":"VLOOKUP($D130,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 2, process 1 (LHV)"},"BC005a2","MJ/kgdm",{"$f":"IF(G125=\"n.a.\",0,VLOOKUP(G125, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F130","v":0}]
[null,null,{"$f":"VLOOKUP($D131,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 2, process 1"},"BC006a2","binary",{"$f":"IF(G125=\"n.a.\",0,VLOOKUP(G125, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F131=\"n.a.\", 0, F131)","v":0}]
[null,null,{"$f":"VLOOKUP($D132,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 2, process 1"},"BC051a2","%",null,{"$f":"IF(G131=1,G129/(G129+G121+G137+G142+G146+G18)*100,0)","v":0},"= BC004a2/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
[null,3,{"$f":"VLOOKUP($D133,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 3, process 1"},"BC002a3","-",{"$f":"VLOOKUP(D133,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F133","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D134,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 3, process 1"},"BC002a30","%",{"$f":"VLOOKUP(D134,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F134=\"n.a.\", 0, F134)","v":0}]
[null,null,{"$f":"VLOOKUP($D135,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 3, process 1"},"BC002a31","kg/year",{"$f":"VLOOKUP(D135,Parameters!$1:2837,6,FALSE)","v":0},{"$f":"F135","v":0}]
[null,null,{"$f":"VLOOKUP($D136,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (kg)"},"BC003a3","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D137,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (MJ)"},"BC004a3","MJbyproduct /MJinput",{"$f":"VLOOKUP(D137,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F137=\"n.a.\", 0, F137)","v":0}]
[null,null,{"$f":"VLOOKUP($D138,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 3, process 1 (LHV)"},"BC005a3","MJ/kgdm",{"$f":"IF(G133=\"n.a.\",0,VLOOKUP(G133, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F138","v":0}]
[null,null,{"$f":"VLOOKUP($D139,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 3, process 1"},"BC006a3","binary",{"$f":"IF(G133=\"n.a.\",0,VLOOKUP(G133, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F139=\"n.a.\", 0, F139)","v":0}]
[null,null,{"$f":"VLOOKUP($D140,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 3, process 1"},"BC051a3","%",null,{"$f":"IF(G139=1,G137/(G121+G137+G129+G142+G146+G18)*100,0)","v":0},"= BC004a3/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
[null,4,{"$f":"VLOOKUP($D141,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity by-product, process 1"},"BC002a41","MWh/year",{"$f":"VLOOKUP(D141,Parameters!$1:2843,6,FALSE)","v":0},{"$f":"F141","v":0}]
[null,null,{"$f":"VLOOKUP($D142,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of electricity by-product, process 1 (MJ)"},"BC004a4","MJbyproduct /MJinput",{"$f":"VLOOKUP(D142,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F142=\"n.a.\", 0, F142)","v":0}]
[null,null,{"$f":"VLOOKUP($D143,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of electricity by-product, process 1"},"BC006a4","binary",{"$f":"IF(G141=\"n.a.\",1,0)","v":0},{"$f":"IF(F143=\"n.a.\", 0, F143)","v":0}]
[null,null,{"$f":"VLOOKUP($D144,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to electricity by-product, process 1"},"BC051a4","%",null,{"$f":"IF(G143=1,G142/(G121+G137+G129+G142+G146+G18)*100,0)","v":0},"= BC004a4/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
[null,5,{"$f":"VLOOKUP($D145,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat by-product, process 1"},"BC002a51","MJ/year",{"$f":"VLOOKUP(D145,Parameters!$1:2844,6,FALSE)","v":0},{"$f":"F145","v":0}]
[null,null,{"$f":"VLOOKUP($D146,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of heat by-product, process 1 (MJ)"},"BC004a5","MJbyproduct /MJinput",{"$f":"VLOOKUP(D146,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F146=\"n.a.\", 0, F146)","v":0}]
[null,null,{"$f":"VLOOKUP($D147,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of heat by-product, process 1"},"BC006a5","binary",{"$f":"IF(G145=\"n.a.\",1,0)","v":0},{"$f":"IF(F147=\"n.a.\", 0, F147)","v":0}]
[null,null,{"$f":"VLOOKUP($D148,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to heat by-product, process 1"},"BC051a5","%",null,{"$f":"IF(G147=1,G146/(G121+G137+G129+G142+G146+G18)*100,0)","v":0},"= BC004a5/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
["Feedstock 1 - Treatment 2",null,null,"LC005","-",{"$f":"VLOOKUP(D149,Parameters!$1:$2792,6,FALSE)","v":"No treatment"},{"$f":"F149","v":"No treatment"}]
[null,{"$f":"VLOOKUP($D150,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat energy use for treatment 2 (storage)"},null,"BC060","MJh/MJinput",{"$f":"VLOOKUP(D150,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F150=\"n.a.\",0,F150)","v":0}]
[null,{"$f":"VLOOKUP($D151,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat source for treatment 2 (storage)"},null,"BC061","-",{"$f":"VLOOKUP(D151,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F151","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D152,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy use for heat production for treatment 2 (storage)"},"BC062a","MJfossil/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151,matrix_standardvalues_heat,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D153,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy use for heat production for treatment 2 (storage)"},"BC062b","MJprim/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151,matrix_standardvalues_heat,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D154,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to heat production for treatment 2 (storage)"},"BC062c","gCO2eq/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151,matrix_standardvalues_heat,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D155,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific NOx emissions related to heat production for treatment 2 (storage)"},"BC062d","gNOx/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151,matrix_standardvalues_heat,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D156,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific SOx emissions related to heat production for treatment 2 (storage)"},"BC062e","gSOx/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151,matrix_standardvalues_heat,11,FALSE))","v":0},0]
[null,{"$f":"VLOOKUP($D157,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity energy use for treatment 2 (storage)"},null,"BC065","MJe/MJinput",{"$f":"VLOOKUP(D157,Parameters!$1:$2792,6,FALSE)","v":8.4000000000000003E-4},{"$f":"IF(F157=\"n.a.\",0,F157)","v":8.4000000000000003E-4}]
[null,{"$f":"VLOOKUP($D158,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity source for treatment 2 (storage)"},null,"BC066","-",{"$f":"VLOOKUP(D158,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F158","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D159,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy use for electricity production for treatment 2 (storage)"},"BC067a","MJfossil/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D160,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy use for electricity production for treatment 2 (storage)"},"BC067b","MJprim/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D161,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for electricity production for treatment 2 (storage)"},"BC067c","gCO2eq/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D162,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific NOx emissions for electricity production for treatment 2 (storage)"},"BC067d","gNOx/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP(D163,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific SOx emissions for electricity production for treatment 2 (storage)"},"BC067e","gSOx/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
["Feedstock 1 - Conversion process 2",null,null,"BC000b","-",{"$f":"VLOOKUP(D164,Parameters!$1:2792,6,FALSE)","v":"Refining"},{"$f":"F164","v":"Refining"}]
[null,"Main input flow of process 2"]
[null,null,{"$f":"VLOOKUP($D166,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of main output flow, process 1"},"BC001a","-",{"$f":"VLOOKUP(D166,Parameters!$1:$2792,6,FALSE)","v":"Crude palm oil"},{"$f":"F166","v":"Crude palm oil"}]
[null,null,{"$f":"VLOOKUP($D167,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of main output flow, process 1"},"BC012a","%",{"$f":"VLOOKUP(D167,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F167","v":0}]
[null,null,{"$f":"VLOOKUP($D168,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of main output flow, process 1 (LHV)"},"BC007a","MJ/kgdm",{"$f":"IF(G166=\"n.a\",0,VLOOKUP(G166,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},{"$f":"F168","v":37}]
[null,"Main output flow of process 2"]
[null,null,{"$f":"VLOOKUP($D170,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of main output flow, process 2"},"BC001b","-",{"$f":"VLOOKUP(D170,Parameters!$1:2792,6,FALSE)","v":"Palm stearin"},{"$f":"F170","v":"Palm stearin"}]
[null,null,{"$f":"VLOOKUP($D171,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of main output flow, process 2"},"BC012b","%",{"$f":"VLOOKUP(D171,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F171","v":0}]
[null,null,{"$f":"VLOOKUP($D172,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of main output flow, process 2 (LHV)"},"BC007b","MJ/kgdm",{"$f":"IF(G170=\"n.a.\",0,VLOOKUP(G170,matrix_standardvalues,14,FALSE))","v":37},{"$f":"F172","v":37}]
[null,{"$f":"VLOOKUP($D173,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate (output/input), process 2"},null,"BC008b","MJoutput /MJinput",{"$f":"VLOOKUP(D173,Parameters!$1:$2792,6,FALSE)","v":0.31987937632906788},{"$f":"F173","v":0.31987937632906788}]
[null,null,{"$f":"VLOOKUP($D174,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 1 per ha after conversion process 2"},"BC015a","kg/ha",null,{"$f":"G175*100/(100-G171)","v":1351.4199870371556},"= BC015b * 100 / (100-BC012b)"]
[null,null,{"$f":"VLOOKUP($D175,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (dry) of feedstock 1 per ha after conversion process 2"},"BC015b","kgdm/ha",null,{"$f":"IF(G172=0,0,G176/G172)","v":1351.4199870371556},"= BC015c / BC007b"]
[null,null,{"$f":"VLOOKUP($D176,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of feedstock 1 per ha after conversion process 2"},"BC015c","MJ/ha",null,{"$f":"G21*G173","v":50002.539520374754},"= BC014c * BC008b"]
[null,"Net electricity input process 2"]
[null,1,{"$f":"VLOOKUP($D178,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of electricity input 1, process 2"},"BC026b","MJe/MJoutput",{"$f":"VLOOKUP(D178,Parameters!$1:2792,6,FALSE)","v":5.9972952198558455E-4},{"$f":"IF(F178=\"n.a.\",0,F178)","v":5.9972952198558455E-4}]
[null,null,{"$f":"VLOOKUP($D179,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity flow 1, process 2"},"BC026b0","MWh/year",{"$f":"VLOOKUP(D179,Parameters!$1:2792,6,FALSE)","v":8.5000000000000006E-3},{"$f":"F179","v":8.5000000000000006E-3}]
[null,null,{"$f":"VLOOKUP($D180,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of electricity flow 1, process 2"},"BC027b","-",{"$f":"VLOOKUP(D180,Parameters!$1:$2792,6,FALSE)","v":"Electricity EU mix LV"},{"$f":"F180","v":"Electricity EU mix LV"}]
[null,null,{"$f":"VLOOKUP($D181,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 1, process 2"},"BC028b","MJfossil/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,11,FALSE))","v":2.7275},2.7275]
[null,null,{"$f":"VLOOKUP($D182,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production flow 1, process 2"},"BC029b","MJprim/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,21,FALSE))","v":4.0912500000000005},4.0912500000000005]
[null,null,{"$f":"VLOOKUP($D183,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 1, process 2"},"BC042b","gCO2eq/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,9,FALSE))","v":129.18969444444446},129.18969444444446]
[null,null,{"$f":"VLOOKUP($D184,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity flow 1, process 2"},"BC112b","gNOX/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D185,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity flow 1, process 2"},"BC113b","gSOX/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D186,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of electricity input 2, process 2"},"BC026b1","MJe/MJoutput",{"$f":"VLOOKUP(D186,Parameters!$1:2799,6,FALSE)","v":0},{"$f":"F186","v":0}]
[null,null,{"$f":"VLOOKUP($D187,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity flow 2, process 2"},"BC026b10","MWh/year",{"$f":"VLOOKUP(D187,Parameters!$1:2800,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D188,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of electricity flow 2, process 2"},"BC027b1","-",{"$f":"VLOOKUP(D188,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D189,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 2, process 2"},"BC028b1","MJfossil/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D190,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production flow 2, process 2"},"BC029b1","MJprim/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D191,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 2, process 2"},"BC042b1","gCO2eq/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D192,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity flow 2, process 2"},"BC112b1","gNOX/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D193,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity flow 2, process 2"},"BC113b1","gSOX/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,"Fuel / heat input"]
[null,1,{"$f":"VLOOKUP($D195,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 1, process 2"},"BC011b1","-",{"$f":"VLOOKUP(D195,Parameters!$1:$2792,6,FALSE)","v":"Heat from NG boiler"},{"$f":"F195","v":"Heat from NG boiler"}]
[null,null,{"$f":"VLOOKUP($D196,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat input 1, process 2"},"BC031b1","MJf_h/MJoutput",{"$f":"VLOOKUP(D196,Parameters!$1:$2792,6,FALSE)","v":7.9963936264744601E-3},{"$f":"IF(F196=\"n.a.\",0,F196)","v":7.9963936264744601E-3}]
[null,null,{"$f":"VLOOKUP($D197,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fuel/heat flow 1, process 2"},"BC031b10","MJ/year",{"$f":"VLOOKUP(D197,Parameters!$1:2809,6,FALSE)","v":408},{"$f":"F197","v":408}]
[null,null,{"$f":"VLOOKUP($D198,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, process 2"},"BC032b1","MJfossil/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F198","v":0}]
[null,null,{"$f":"VLOOKUP($D199,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, process 2"},"BC033b1","MJprim/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D200,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, process 2"},"BC043b1","gCO2_eq/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,9,FALSE))","v":71.972777777777765},71.972777777777765]
[null,null,{"$f":"VLOOKUP($D201,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 1, process 2"},"BC115b","gNOX/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D202,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 1, process 2"},"BC116b","gSOX/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D203,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 2, process 2"},"BC011b2","-",{"$f":"VLOOKUP(D203,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D204,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat input 2, process 2"},"BC031b2","MJf_h/MJoutput",{"$f":"VLOOKUP(D204,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F204=\"n.a.\",0,F204)","v":0}]
[null,null,{"$f":"VLOOKUP($D205,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fuel/heat flow 2, process 2"},"BC031b20","MJ/year",{"$f":"VLOOKUP(D205,Parameters!$1:2817,6,FALSE)","v":0},{"$f":"F205","v":0}]
[null,null,{"$f":"VLOOKUP($D206,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, process 2"},"BC032b2","MJfossil/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F206","v":0}]
[null,null,{"$f":"VLOOKUP($D207,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, process 2"},"BC033b2","MJprim/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,21,FALSE))","v":0},{"$f":"F207","v":0}]
[null,null,{"$f":"VLOOKUP($D208,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, process 2"},"BC043b2","gCO2_eq/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,9,FALSE))","v":0},{"$f":"F208","v":0}]
[null,null,{"$f":"VLOOKUP($D209,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 2, process 2"},"BC117b","gNOX/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,27,FALSE))","v":0},{"$f":"F209","v":0}]
[null,null,{"$f":"VLOOKUP($D210,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 2, process 2"},"BC118b","gSOX/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,29,FALSE))","v":0},{"$f":"F210","v":0}]
[null,"Other material input flows"]
[null,1,{"$f":"VLOOKUP($D212,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 1, process 2"},"BC009b1","-",{"$f":"VLOOKUP(D212,Parameters!$1:2792,6,FALSE)","v":"Fuller's earth"},{"$f":"F212","v":"Fuller's earth"}]
[null,null,{"$f":"VLOOKUP($D213,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 1, process 2"},"BC010b1","kg/MJoutput",{"$f":"VLOOKUP(D213,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F213=\"n.a.\",0,F213)","v":0}]
[null,null,{"$f":"VLOOKUP($D214,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material input flow 1, process 2"},"BC010b10","kg/year",{"$f":"VLOOKUP(D214,Parameters!$1:2902,6,FALSE)","v":0},{"$f":"F214","v":0}]
[null,null,{"$f":"VLOOKUP($D215,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 1, process 2"},"BC010b11","%",{"$f":"VLOOKUP(D215,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F215=\"n.a.\", 0, F215)","v":0}]
[null,null,{"$f":"VLOOKUP($D216,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 1, process 2"},"BC010b12","MJ/kgdm",{"$f":"VLOOKUP(D216,Parameters!$1:2907,6,FALSE)","v":0},{"$f":"F216","v":0}]
[null,null,{"$f":"VLOOKUP($D217,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 1, process 2"},"BC035b1","MJfossil/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212,matrix_standardvalues,10,FALSE))","v":2.5405200000000003},{"$f":"F217","v":2.5405200000000003}]
[null,null,{"$f":"VLOOKUP($D218,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 1, process 2"},"BC036b1","MJprim/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212, matrix_standardvalues_conversioninputs,20,FALSE))","v":3.8107800000000003},3.8107800000000003]
[null,null,{"$f":"VLOOKUP($D219,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, process 2"},"BC047b1","gCO2_eq/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212,matrix_standardvalues,5,FALSE))","v":199.7227},199.7227]
[null,null,{"$f":"VLOOKUP($D220,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 1, process 2"},"BC120b","gNOX/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212,matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D221,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 1, process 2"},"BC121b","gSOX/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212,matrix_standardvalues,28,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D222,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 2, process 2"},"BC009b2","-",{"$f":"VLOOKUP(D222,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D223,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 2, process 2"},"BC010b2","kg/MJoutput",{"$f":"VLOOKUP(D223,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F223=\"n.a.\",0,F223)","v":0}]
[null,null,{"$f":"VLOOKUP($D224,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material input flow 2, process 2"},"BC010b20","kg/year",{"$f":"VLOOKUP(D224,Parameters!$1:2910,6,FALSE)","v":0},{"$f":"F224","v":0}]
[null,null,{"$f":"VLOOKUP($D225,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 2, process 2"},"BC010b21","%",{"$f":"VLOOKUP(D225,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F225=\"n.a.\", 0, F225)","v":0}]
[null,null,{"$f":"VLOOKUP($D226,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 2, process 2"},"BC010b22","MJ/kgdm",{"$f":"VLOOKUP(D226,Parameters!$1:2917,6,FALSE)","v":0},{"$f":"F226","v":0}]
[null,null,{"$f":"VLOOKUP($D227,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 2, process 2"},"BC035b2","MJfossil/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,10,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D228,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 2, process 2"},"BC036b2","MJprim/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D229,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, process 2"},"BC047b2","gCO2_eq/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D230,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 2, process 2"},"BC122b","gNOX/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D231,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 2, process 2"},"BC123b","gSOX/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,28,FALSE))","v":0},0]
[null,"Material output flow"]
[null,null,{"$f":"VLOOKUP($D233,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material output flow, process 2"},"BC009d","-",{"$f":"VLOOKUP(D233,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F233","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D234,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 2"},"BC010d","kgdm/MJoutput",{"$f":"VLOOKUP(D234,Parameters!$1:2899,6,FALSE)","v":0},{"$f":"IF(F234=\"n.a.\",0,F234)","v":0}]
[null,null,{"$f":"VLOOKUP($D235,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material output flow, process 2"},"BC010d0","kg/year",{"$f":"VLOOKUP(D235,Parameters!$1:2920,6,FALSE)","v":1379},{"$f":"F235","v":1379}]
[null,null,{"$f":"VLOOKUP($D236,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material output flow, process 2"},"BC035d","MJfossil/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,10,FALSE))","v":0},{"$f":"F236","v":0}]
[null,null,{"$f":"VLOOKUP($D237,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material output flow, process 2"},"BC036d","MJprim/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D238,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material output flow, process 2"},"BC047d","gCO2_eq/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D239,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material output flow, process 2"},"BC120d","gNOX/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D240,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material output flow, process 2"},"BC121d","gSOX/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,28,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D241,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of output flow, process 2 (electricity)"},"BC009d1","-",{"$f":"VLOOKUP(D241,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D242,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 2 (Electricity)"},"BC010d1","MJe/MJoutput",{"$f":"VLOOKUP(D242,Parameters!$1:2906,6,FALSE)","v":0},{"$f":"IF(F242=\"n.a.\",0,F242)","v":0}]
[null,null,{"$f":"VLOOKUP($D243,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for  output flow, process 2 (electricity)"},"BC035d1","MJfossil/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,11,FALSE))","v":0},{"$f":"F243","v":0}]
[null,null,{"$f":"VLOOKUP($D244,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for output flow, process 2 (electricity)"},"BC036d1","MJprim/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D245,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to  output flow, process 2 (electricity)"},"BC047d1","gCO2eq/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D246,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of output flow, process 2 (electricity)"},"BC120d1","gNOX/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D247,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of output flow, process 2 (electricity)"},"BC121d1","gSOX/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D248,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of output flow, process 2 (heat)"},"BC009d2","-",{"$f":"VLOOKUP(D248,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F248","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D249,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 2 (Heat)"},"BC010d2","MJf_h/MJoutput",{"$f":"VLOOKUP(D249,Parameters!$1:2907,6,FALSE)","v":0},{"$f":"IF(F249=\"n.a.\",0,F249)","v":0}]
[null,null,{"$f":"VLOOKUP($D250,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for  output flow, process 2 (heat)"},"BC035d2","MJfossil/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F250","v":0}]
[null,null,{"$f":"VLOOKUP($D251,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for output flow, process 2 (heat)"},"BC036d2","MJprim/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D252,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to  output flow, process 2 (heat)"},"BC047d2","gCO2_eq/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D253,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of output flow, process 2 (heat)"},"BC120d2","gNOX/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D254,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of output flow, process 2 (heat)"},"BC121d2","gSOX/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[null,"By-products"]
[null,null,{"$f":"VLOOKUP($D256,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to energy crop, process 2"},"BC050b","%",null,{"$f":"100-G257","v":100},"= 1 - BC022b"]
[null,null,{"$f":"VLOOKUP($D257,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-products, process 2"},"BC022b","%",null,{"$f":"G265+G273","v":0},"= BC051b1 + BC051b2"]
[null,1,{"$f":"VLOOKUP($D258,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 1, process 2"},"BC002b1","-",{"$f":"VLOOKUP(D258,Parameters!$1:$2792,6,FALSE)","v":"Palm olein"},{"$f":"F258","v":"Palm olein"}]
[null,null,{"$f":"VLOOKUP($D259,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 1, process 2"},"BC002b10","%",{"$f":"VLOOKUP(D259,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F259=\"n.a.\", 0, F259)","v":0}]
[null,null,{"$f":"VLOOKUP($D260,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 1, process 2"},"BC002b11","kg/year",{"$f":"VLOOKUP(D260,Parameters!$1:2930,6,FALSE)","v":0},{"$f":"F260","v":0}]
[null,null,{"$f":"VLOOKUP($D261,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (kg)"},"BC003b1","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D262,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (MJ)"},"BC004b1","MJbyproduct /MJinput",{"$f":"VLOOKUP(D262,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F262=\"n.a.\", 0, F262)","v":0}]
[null,null,{"$f":"VLOOKUP($D263,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 1, process 2 (LHV)"},"BC005b1","MJ/kgdm",{"$f":"IF(G258=\"n.a.\",0,VLOOKUP(G258, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":37},{"$f":"F263","v":37}]
[null,null,{"$f":"VLOOKUP($D264,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 1, process 2"},"BC006b1","binary",{"$f":"IF(G258=\"n.a.\",0,VLOOKUP(G258, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":1},{"$f":"IF(F264=\"n.a.\", 0, F264)","v":1}]
[null,null,{"$f":"VLOOKUP($D265,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 1, process 2"},"BC051b1","%",null,{"$f":"IF(G264=1,G262/(G262+G270+G275+G279+G173)*100,0)","v":0},"= BC004b1/(BC004b1+BC004b2+BC004b4+BC004b5+BC008b)*100"]
[null,2,{"$f":"VLOOKUP($D266,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 2, process 2"},"BC002b2","-",{"$f":"VLOOKUP(D266,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F266","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D267,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 2, process 2"},"BC002b20","%",{"$f":"VLOOKUP(D267,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F267=\"n.a.\", 0, F267)","v":0}]
[null,null,{"$f":"VLOOKUP($D268,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 2, process 2"},"BC002b21","kg/year",{"$f":"VLOOKUP(D268,Parameters!$1:2938,6,FALSE)","v":0},{"$f":"F268","v":0}]
[null,null,{"$f":"VLOOKUP($D269,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (kg)"},"BC003b2","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D270,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (MJ)"},"BC004b2","MJbyproduct /MJinput",{"$f":"VLOOKUP(D270,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F270=\"n.a.\", 0, F270)","v":0}]
[null,null,{"$f":"VLOOKUP($D271,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 2, process 2 (LHV)"},"BC005b2","MJ/kgdm",{"$f":"IF(G266=\"n.a.\",0,VLOOKUP(G266, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F271","v":0}]
[null,null,{"$f":"VLOOKUP($D272,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 2, process 2"},"BC006b2","binary",{"$f":"IF(G266=\"n.a.\",0,VLOOKUP(G266, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F272=\"n.a.\", 0, F272)","v":0}]
[null,null,{"$f":"VLOOKUP($D273,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 2, process 2"},"BC051b2","%",null,{"$f":"IF(G272=1,G270/(G270+G262+G275+G279+G173)*100,0)","v":0},"= BC004b2/(BC004b1+BC004b2+BC004b4+BC004b5+BC008b)*100"]
[null,4,{"$f":"VLOOKUP($D274,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity by-product, process 2"},"BC002b41","MWh/year",{"$f":"VLOOKUP(D274,Parameters!$1:2944,6,FALSE)","v":0},{"$f":"F274","v":0}]
[null,null,{"$f":"VLOOKUP($D275,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of electricity by-product, process 2 (MJ)"},"BC004b4","MJbyproduct /MJinput",{"$f":"VLOOKUP(D275,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F275=\"n.a.\", 0, F275)","v":0}]
[null,null,{"$f":"VLOOKUP($D276,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of electricity by-product, process 2"},"BC006b4","binary",{"$f":"IF(G274=\"n.a.\",1,0)","v":0},{"$f":"IF(F276=\"n.a.\", 0, F276)","v":0}]
[null,null,{"$f":"VLOOKUP($D277,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to electricity by-product, process 2"},"BC051b4","%",null,{"$f":"IF(G276=1,G275/(G270+G262+G275+G279+G173)*100,0)","v":0},"= BC004b4/(BC004b1+BC004b2+BC004b4+BC004b5+BC008b)*100"]
[null,5,{"$f":"VLOOKUP($D278,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat by-product, process 2"},"BC002b51","MJ/year",{"$f":"VLOOKUP(D278,Parameters!$1:2945,6,FALSE)","v":0},{"$f":"F278","v":0}]
[null,null,{"$f":"VLOOKUP($D279,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of heat by-product, process 2 (MJ)"},"BC004b5","MJbyproduct /MJinput",{"$f":"VLOOKUP(D279,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F279=\"n.a.\", 0, F279)","v":0}]
[null,null,{"$f":"VLOOKUP($D280,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of heat by-product, process 2"},"BC006b5","binary",{"$f":"IF(G275=\"n.a.\",1,0)","v":0},{"$f":"IF(F280=\"n.a.\", 0, F280)","v":0}]
[null,null,{"$f":"VLOOKUP($D281,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to heat by-product, process 2"},"BC051b5","%",null,{"$f":"IF(G280=1,G279/(G270+G262+G275+G279+G173)*100,0)","v":0},"= BC004b5/(BC004b1+BC004b2+BC004b4+BC004b5+BC008b)*100"]
["Feedstock 1 - Treatment 3",null,null,"LC008","-",{"$f":"VLOOKUP(D282,Parameters!$1:$2792,6,FALSE)","v":"No treatment"},{"$f":"F282","v":"No treatment"}]
[null,{"$f":"VLOOKUP($D283,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat energy use for treatment 3 (storage)"},null,"BC070","MJh/MJinput",{"$f":"VLOOKUP(D283,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F283=\"n.a.\",0,F283)","v":0}]
[null,{"$f":"VLOOKUP($D284,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat source for treatment 3 (storage)"},null,"BC071","-",{"$f":"VLOOKUP(D284,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F284","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D285,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy use for heat production for treatment 3 (storage)"},"BC072a","MJfossil/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D286,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy use for heat production for treatment 3 (storage)"},"BC072b","MJprim/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D287,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to heat production for treatment 3 (storage)"},"BC072c","gCO2eq/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D288,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific NOx emissions related to heat production for treatment 3 (storage)"},"BC072d","gNOX/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D289,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific SOx emissions related to heat production for treatment 3 (storage)"},"BC072e","gSOX/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,29,FALSE))","v":0},0]
[null,{"$f":"VLOOKUP($D290,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity energy use for treatment 3 (storage)"},null,"BC075","MJe/MJinput",{"$f":"VLOOKUP(D290,Parameters!$1:$2792,6,FALSE)","v":8.4000000000000003E-4},{"$f":"IF(F290=\"n.a.\",0,F290)","v":8.4000000000000003E-4}]
[null,{"$f":"VLOOKUP($D291,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity source for treatment 3 (storage)"},null,"BC076","-",{"$f":"VLOOKUP(D291,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F291","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D292,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy use for electricity production for treatment 3 (storage)"},"BC077a","MJfossil/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D293,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy use for electricity production for treatment 3 (storage)"},"BC077b","MJprim/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D294,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to electricity production for treatment 3 (storage)"},"BC077c","gCO2eq/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D295,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific NOx emissions related to electricity production for treatment 3 (storage)"},"BC077d","gNOX/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D296,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific SOx emissions related to electricity production for treatment 3 (storage)"},"BC077e","gSOX/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[]
["ENERGY BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D300,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use in process 1"},null,"BC020a","MJfossil/MJendfuel_fs1",null,{"$f":"IF(G173=0,(G302+G304+G306)/1,(G302+G304+G306)/G173)","v":0},"= (BC024a + BC030a + BC035a)/BC008b"]
[null,{"$f":"VLOOKUP($D301,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use in process 1"},null,"BC021a","MJprim/MJendfuel_fs1",null,{"$f":"IF(G173=0,(G303+G305+G307)/1,(G303+G305+G307)/G173)","v":0},"= (BC025a + BC034a + BC036a)/BC008b"]
[null,null,{"$f":"VLOOKUP($D302,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to electricity input, process 1"},"BC024a","MJfossil/MJoutput",null,{"$f":"G23*G26","v":0},"= BC026a * BC028a"]
[null,null,{"$f":"VLOOKUP($D303,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to electricity input, process 1"},"BC025a","MJprim/MJoutput",null,{"$f":"G23*G27","v":0},"= BC026a * BC029a"]
[null,null,{"$f":"VLOOKUP($D304,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, process 1"},"BC030a","MJfossil/MJoutput",null,{"$f":"G41*G43+G49*G51","v":0},"= BC031a1 * BC032a1 + BC031a2 * BC032a2"]
[null,null,{"$f":"VLOOKUP($D305,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to fuel/heat input flows, process 1"},"BC034a","MJprim/MJoutput",null,{"$f":"G41*G44+G49*G52","v":0},"= BC031a1 * BC033a1 + BC031a2 * BC033a2"]
[null,null,{"$f":"VLOOKUP($D306,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to material input flows, process 1"},"BC035a","MJfossil/MJoutput",null,{"$f":"G63*G66+G73*G76+G83*G86+G93*G95+G101*G102+G108*G109","v":0},"= BC010a1 * BC035a1 + BC010a2 * BC035a2 + BC010c * BC035c"]
[null,null,{"$f":"VLOOKUP($D307,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to material input flows, process 1"},"BC036a","MJprim/MJoutput",null,{"$f":"G63*G67+G58*G60+G73*G77+G83*G87+G93*G96+G101*G103+G108*G110","v":0},"= BC010a1 * BC036a1 + BC010a2 * BC036a3 + BC010c * BC036c"]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D309,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for treatment 2 (storage)"},null,"BC059a","MJfossil/MJendfuel_fs1",null,{"$f":"IF(G173=0,(G150*G152+G157*G159)/1,(G150*G152+G157*G159)/G173)","v":0},"= (BC060*BC062a+BC065*BC067a)/BC008b"]
[null,{"$f":"VLOOKUP($D310,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for treatment 2 (storage)"},null,"BC059b","MJprim/MJendfuel_fs1",null,{"$f":"IF(G173=0,(G150*G153+G157*G160)/1,(G150*G153+G157*G160)/G173)","v":0},"= (BC060*BC062b+BC065*BC067b)/BC008b"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D312,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use in process 2"},null,"BC020b","MJfossil/MJendfuel_fs1",null,{"$f":"G314+G316+G318","v":1.6357622712156819E-3},"= BC024b + BC030b + BC035b"]
[null,{"$f":"VLOOKUP($D313,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use in process 2"},null,"BC021b","MJprim/MJendfuel_fs1",null,{"$f":"G315+G317+G319","v":2.4536434068235229E-3},"= BC025b + BC034b + BC036b"]
[null,null,{"$f":"VLOOKUP($D314,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to electricity input, process 2"},"BC024b","MJfossil/MJoutput",null,{"$f":"G178*G181","v":1.6357622712156819E-3},"= BC026b * BC028b"]
[null,null,{"$f":"VLOOKUP($D315,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to electricity input, process 2"},"BC025b","MJprim/MJoutput",null,{"$f":"G178*G182","v":2.4536434068235229E-3},"= BC026b * BC029b"]
[null,null,{"$f":"VLOOKUP($D316,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, process 2"},"BC030b","MJfossil/MJoutput",null,{"$f":"G196*G198+G204*G206","v":0},"= BC031b1 * BC032b1 + BC031b2 * BC032b2"]
[null,null,{"$f":"VLOOKUP($D317,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to fuel/heat input flows, process 2"},"BC034b","MJprim/MJoutput",null,{"$f":"G196*G199+G204*G207","v":0},"= BC031b1 * BC033b1 + BC031b2 * BC033b2"]
[null,null,{"$f":"VLOOKUP($D318,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to material input flows, process 2"},"BC035b","MJfossil/MJoutput",null,{"$f":"G213*G217+G223*G227+G234*G236+G242*G243+G249*G250","v":0},"= BC010b1 * BC035b1 + BC010b2 * BC035b2 + BC010d * BC035d"]
[null,null,{"$f":"VLOOKUP($D319,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to material input flows, process 2"},"BC036b","MJprim/MJoutput",null,{"$f":"G213*G218+G223*G228+G234*G237+G242*G244+G249*G251","v":0},"= BC010b1 * BC036b1 + BC010b2 * BC036b3 + BC010d * BC036d"]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D321,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for treatment 3 (storage)"},null,"BC069a","MJfossil/MJendfuel_fs1",null,{"$f":"G283*G285+G290*G292","v":0},"= BC070*BC072a+BC075*BC077a"]
[null,{"$f":"VLOOKUP($D322,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for treatment 3 (storage)"},null,"BC069b","MJprim/MJendfuel_fs1",null,{"$f":"G283*G286+G290*G293","v":0},"= BC070*BC072b+BC075*BC077b"]
["Cumulated energy use after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D324,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated fossil energy use after conversion 1 (per MJ feedstock 1 fuel)"},null,"BC080a","MJfossil/MJendfuel_fs1",null,{"$f":"('Production feedstock1'!G100+'Production feedstock1'!G110+'Transport feedstock1'!G111+'Conversion feedstock1'!G300)*'Conversion feedstock1'!G115/100","v":4.2427297465073593E-2},"= (FP032a+FP039a+FT012a+BC020a)*BC050a/100"]
[null,{"$f":"VLOOKUP($D325,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated primary energy use after conversion 1 (per MJ feedstock 1 fuel)"},null,"BC080b","MJprim/MJendfuel_fs1",null,{"$f":"('Production feedstock1'!G101+'Production feedstock1'!G111+'Transport feedstock1'!G112+'Conversion feedstock1'!G301)*'Conversion feedstock1'!G115/100","v":0.35119170139699607},"= (FP032b+FP039b+FT012b+BC021a)*BC050a/100"]
["Cumulated energy use after allocation 3 (= energy use after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D327,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated fossil energy use after conversion 2 (per MJ feedstock 1 fuel)"},null,"BC081a","MJfossil/MJendfuel_fs1",null,{"$f":"(G324+G309+'Transport feedstock1'!G119+'Conversion feedstock1'!G312)*'Conversion feedstock1'!G256/100","v":0.17484144883990196},"= (BC080a+BC059a+FT013a+BC020b)*BC050b/100"]
[null,{"$f":"VLOOKUP($D328,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated primary energy use after conversion 2 (per MJ feedstock 1 fuel)"},null,"BC081b","MJprim/MJendfuel_fs1",null,{"$f":"(G325+G310+'Transport feedstock1'!G120+'Conversion feedstock1'!G313)*'Conversion feedstock1'!G256/100","v":0.54981292845923868},"= (BC080b+BC059b+FT013b+BC021b)*BC050b/100"]
["Total cumulated energy use feedstock 1 (= energy use after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D330,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use feedstock 1 (per MJ feedstock 1 fuel)"},null,"BC082a","MJfossil/MJendfuel_fs1",null,{"$f":"G327+G321+'Transport feedstock1'!G127","v":0.17800166505611817},"= BC081a+BC069a+FT014a"]
[null,{"$f":"VLOOKUP($D331,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use feedstock 1 (per MJ feedstock 1 fuel)"},null,"BC082b","MJprim/MJendfuel_fs1",null,{"$f":"G328+G322+'Transport feedstock1'!G128","v":0.55455325278356304},"= BC081b+BC069b+FT014b"]
[null,{"$f":"VLOOKUP($D332,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use feedstock 1 (per MJ functional unit)"},null,"BC083a","MJfossil/MJFU",null,{"$f":"G330*'Final conversion'!G68/100*'Final conversion'!G22","v":0.17800166505611817},"= BC082a * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D333,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use feedstock 1 (per MJ functional unit)"},null,"BC083b","MJprim/MJFU",null,{"$f":"G331*'Final conversion'!G68/100*'Final conversion'!G22","v":0.55455325278356304},"= BC082b * FC025c / 100 * FC033"]
["Totally allocated energy use for conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D335,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in process 1"},null,"BC090a","MJfossil/MJendfuel_fs1",null,{"$f":"G300*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":0},"= BC020a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D336,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in process 1"},null,"BC090b","MJprim/MJendfuel_fs1",null,{"$f":"G301*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100","v":0},"= BC021a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D337,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in process 1"},null,"BC091a","MJfossil/MJFU",null,{"$f":"G300*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= BC020a * BC050a / 100 * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D338,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in process 1"},null,"BC091b","MJprim/MJFU",null,{"$f":"G301*'Conversion feedstock1'!G115/100*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= BC021a * BC050a / 100 * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D339,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in process 2"},null,"BC092a","MJfossil/MJendfuel_fs1",null,{"$f":"G312*'Conversion feedstock1'!G256/100","v":1.6357622712156819E-3},"= BC020b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D340,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in process 2"},null,"BC092b","MJprim/MJendfuel_fs1",null,{"$f":"G313*'Conversion feedstock1'!G256/100","v":2.4536434068235229E-3},"= BC021b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D341,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in process 2"},null,"BC093a","MJfossil/MJFU",null,{"$f":"G312*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":1.6357622712156819E-3},"= BC020b * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D342,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in process 2"},null,"BC093b","MJprim/MJFU",null,{"$f":"G313*'Conversion feedstock1'!G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":2.4536434068235229E-3},"= BC021b * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D343,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for conversion (process 1 + 2)"},null,"BC094a","MJfossil/MJendfuel_fs1",null,{"$f":"G335+G339","v":1.6357622712156819E-3},"= BC090a + BC092a"]
[null,{"$f":"VLOOKUP($D344,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for conversion (process 1 + 2)"},null,"BC094b","MJprim/MJendfuel_fs1",null,{"$f":"G336+G340","v":2.4536434068235229E-3},"= BC090b + BC092b"]
[null,{"$f":"VLOOKUP($D345,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for conversion (process 1 + 2)"},null,"BC095a","MJfossil/MJFU",null,{"$f":"G337+G341","v":1.6357622712156819E-3},"= BC091a + BC093a"]
[null,{"$f":"VLOOKUP($D346,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for conversion (process 1 + 2)"},null,"BC095b","MJprim/MJFU",null,{"$f":"G338+G342","v":2.4536434068235229E-3},"= BC091b + BC093b"]
[]
["GLOBAL WARMING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D350,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to process 1"},null,"BC037a","gCO2_eq/MJendfuel_fs1",null,{"$f":"IF(G173=0,(G351+G352+G353)/1,(G351+G352+G353)/G173)","v":0},"= (BC041a + BC043a + BC047a)/BC008b"]
[null,null,{"$f":"VLOOKUP($D351,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to electricity input, process 1"},"BC041a","gCO2_eq/MJoutput",null,{"$f":"G23*G28+G31*G36","v":0},"= BC026a * BC042a"]
[null,null,{"$f":"VLOOKUP($D352,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to fuel/heat input flows, process 1"},"BC043a","gCO2_eq/MJoutput",null,{"$f":"G41*G45+G49*G53","v":0},"= BC031a1 * BC043a1 + BC031a2 * BC043a2"]
[null,null,{"$f":"VLOOKUP($D353,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to material input flows, process 1"},"BC047a","gCO2_eq/MJoutput",null,{"$f":"G63*G68+G73*G78+G83*G88+G93*G97+G101*G104+G108*G111","v":0},"= BC010a1 * BC047a1 + BC010a2 * BC047a2 + BC010c * BC047c"]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D355,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with treatment 2 (storage)"},null,"BC059c","gCO2_eq/MJendfuel_fs1",null,{"$f":"IF(G173=0,(G150*G154+G157*G161)/1,(G150*G154+G157*G161)/G173)","v":0},"= (BC060*BC062c+BC065*BC067c)/BC008b"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D357,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to process 2"},null,"BC037b","gCO2_eq/MJendfuel_fs1",null,{"$f":"G358+G359+G360","v":0.65300153519651516},"= BC041b + BC043b + BC047b"]
[null,null,{"$f":"VLOOKUP($D358,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to electricity input, process 2"},"BC041b","gCO2_eq/MJoutput",null,{"$f":"G178*G183","v":7.7478873694630399E-2},"= BC026b * BC042b"]
[null,null,{"$f":"VLOOKUP($D359,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to fuel/heat input flows, process 2"},"BC043b","gCO2_eq/MJoutput",null,{"$f":"G196*G200+G204*G208","v":0.5755226615018848},"= BC031b1 * BC043b1 + BC031b2 * BC043b2"]
[null,null,{"$f":"VLOOKUP($D360,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to material input flows, process 2"},"BC047b","gCO2_eq/MJoutput",null,{"$f":"G213*G219+G223*G229+G234*G238+G242*G245+G249*G252","v":0},"= BC010b1 * BC047b1 + BC010b2 * BC047b2 + BC010d * BC047d"]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D362,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with treatment 3 (storage)"},null,"BC069c","gCO2_eq/MJendfuel_fs1",null,{"$f":"G283*G287+G290*G294","v":0},"= BC070*BC072c+BC075*BC077c"]
["Cumulated GHG emissions after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D364,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated GHG emissions after conversion 1 (per MJ feedstock 1 fuel)"},null,"BC080c","gCO2_eq/MJendfuel_fs1",null,{"$f":"('Production feedstock1'!G234+'Production feedstock1'!G240+'Transport feedstock1'!G155+'Conversion feedstock1'!G350)*'Conversion feedstock1'!G115/100","v":47.891178160047083},"= (FP057+FP062b+FT015a+BC037a)*BC050a/100"]
["Cumulated GHG emissions after allocation 3 (= GHG emissions after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D366,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated GHG emissions after conversion 2 (per MJ feedstock 1 fuel)"},null,"BC081c","gCO2_eq/MJendfuel_fs1",null,{"$f":"(G364+G355+'Transport feedstock1'!G159+'Conversion feedstock1'!G357)*'Conversion feedstock1'!G256/100","v":58.95757002282992},"= (BC080c+BC059c+FT015b+BC037b)*BC050b/100"]
["Total cumulated GHG emissions feedstock 1 (= GHG emissions after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D368,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions feedstock 1 (per MJ feedstock 1 fuel)"},null,"BC082c","gCO2_eq/MJendfuel_fs1",null,{"$f":"G366+G362+'Transport feedstock1'!G163","v":59.196326779586677},"= BC081c+BC069c+FT015c"]
[null,{"$f":"VLOOKUP($D369,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions feedstock 1 (per MJ functional unit)"},null,"BC083c","gCO2_eq/MJFU",null,{"$f":"G368*'Final conversion'!G68/100*'Final conversion'!G22","v":59.196326779586677},"= BC082c * FC025c / 100 * FC033"]
["Totally allocated GHG emissions for conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D371,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions in process 1"},null,"BC090c","gCO2_eq/MJendfuel_fs1",null,{"$f":"G350*G115/100*G256/100","v":0},"= BC037a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D372,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions in process 1"},null,"BC091c","gCO2_eq/MJFU",null,{"$f":"G350*G115/100*G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= BC037a * BC050a / 100 * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D373,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions in process 2"},null,"BC092c","gCO2_eq/MJendfuel_fs1",null,{"$f":"G357*G256/100","v":0.65300153519651516},"= BC037b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D374,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions in process 2"},null,"BC093c","gCO2_eq/MJFU",null,{"$f":"G357*G256/100*'Final conversion'!G68/100*'Final conversion'!G22","v":0.65300153519651516},"= BC037b * BC050b / 100 * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D375,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from conversion (process 1 + 2)"},null,"BC094c","gCO2_eq/MJendfuel_fs1",null,{"$f":"G371+G373","v":0.65300153519651516},"= BC090c + BC092c"]
[null,{"$f":"VLOOKUP($D376,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from conversion (process 1 + 2)"},null,"BC095c","gCO2_eq/MJFU",null,{"$f":"G372+G374","v":0.65300153519651516},"= BC091c + BC093c"]
["Carbon debt & repayment time"]
[null,{"$f":"VLOOKUP($D378,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions feedstock 1 (per MJ feedstock 1 fuel) without LUC emissions"},null,"BC084","gCO2_eq/MJendfuel_fs1",null,{"$f":"(('Production feedstock1'!G245+'Production feedstock1'!G240+'Transport feedstock1'!G155+'Conversion feedstock1'!G350)*'Conversion feedstock1'!G115/100+G355+'Transport feedstock1'!G159+'Conversion feedstock1'!G357)*'Conversion feedstock1'!G256/100+G362+'Transport feedstock1'!G163","v":59.196326779586677},"= ((FP108 + FP062b + FT015a + BC037a) * BC050a / 100 + BC059c + FT015b + BC037b) * BC050b / 100 + BC069c + FT015c"]
[]
[null,"GHG emissions related to materials production, assemblage and recycling *",null,null,"gCO2-eq/conversion plant"]
[]
["RESOURCE USE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["USE OF WATER"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D385,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for conversion process 1"},null,"BC100a","m³/MJoutput",{"$f":"VLOOKUP(D385,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F385","v":0}]
[null,{"$f":"VLOOKUP($D386,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for conversion process 1"},null,"BC100b","m³/GJendfuel_fs1",null,{"$f":"IF(G173=0,G385/1*1000,G385/G173*1000)","v":0},"= BC100a / BC008b * 1000"]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D388,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},null,"BC101a","m³/MJinput",{"$f":"VLOOKUP(D388,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F388","v":0}]
[null,{"$f":"VLOOKUP($D389,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},null,"BC101b","m³/GJendfuel_fs1",null,{"$f":"IF(G173=0,G388/1*1000,G388/G173*1000)","v":0},"= BC101a / BC008b * 1000"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D391,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for conversion process 2"},null,"BC102a","m³/MJoutput",{"$f":"VLOOKUP(D391,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F391","v":0}]
[null,{"$f":"VLOOKUP($D392,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for conversion process 2"},null,"BC102b","m³/GJendfuel_fs1",null,{"$f":"G391*1000","v":0},"= BC102a * 1000"]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D394,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},null,"BC103a","m³/MJinput",{"$f":"VLOOKUP(D394,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F394","v":0}]
[null,{"$f":"VLOOKUP($D395,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},null,"BC103b","m³/GJendfuel_fs1",null,{"$f":"G394*1000","v":0},"= BC103a * 1000"]
["Cumulated water use after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D397,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated water use after conversion 1 (per GJ feedstock 1 fuel)"},null,"BC080d","m³/GJendfuel_fs1",null,{"$f":"('Production feedstock1'!G253+'Production feedstock1'!G259+'Conversion feedstock1'!G386)*'Conversion feedstock1'!G115/100","v":422.20878511090552},"= (FP101+FP103b+BC100b)*BC050a/100"]
["Cumulated GHG emissions after allocation 3 (= water use after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D399,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated water use after conversion 2 (per GJ feedstock 1 fuel)"},null,"BC081d","m³/GJendfuel_fs1",null,{"$f":"(G397+G389+G392)*'Conversion feedstock1'!G256/100","v":422.20878511090552},"= (BC080d+BC101b+BC102b)*BC050b/100"]
["Total cumulated GHG emissions feedstock 1 (= water use after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D401,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use feedstock 1 (per GJ feedstock 1 fuel)"},null,"BC082d","m³/GJendfuel_fs1",null,{"$f":"G399+G395","v":422.20878511090552},"= BC081d+BC103b"]
[null,{"$f":"VLOOKUP($D402,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use feedstock 1 (per GJ functional unit)"},null,"BC083d","m³/GJFU",null,{"$f":"G401*'Final conversion'!G68/100*'Final conversion'!G22","v":422.20878511090552},"= BC082d * FC025c / 100 * FC033"]
["Totally allocated GHG emissions for conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D404,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use in process 1"},null,"BC090d","m³/GJendfuel_fs1",null,{"$f":"G386*G115/100*G256/100","v":0},"= BC100b * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D405,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use in process 1"},null,"BC091d","m³/GJFU",null,{"$f":"G404*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= BC090d * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D406,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use in process 2"},null,"BC092d","m³/GJendfuel_fs1",null,{"$f":"G392*G256/100","v":0},"= BC102b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D407,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use in process 2"},null,"BC093d","m³/GJFU",null,{"$f":"G406*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= BC092d * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D408,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use for conversion (process 1 + 2)"},null,"BC094d","m³/GJendfuel_fs1",null,{"$f":"G404+G406","v":0},"= BC090d + BC092d"]
[null,{"$f":"VLOOKUP($D409,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use for conversion (process 1 + 2)"},null,"BC095d","m³/GJFU",null,{"$f":"G405+G407","v":0},"= BC091d + BC093d"]
["USE OF LAND"]
[null,"N.A."]
[]
["ENVIRONMENTAL QUALITY",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["ACIDIFICATION POTENTIAL"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D416,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process 1"},null,"BC110a","gSO2_eq/MJendfuel_fs1",null,{"$f":"IF(G173=0,(G417+G418+G419+G420)/1,(G417+G418+G419+G420)/G173)","v":0},"= (BC111a + BC114a + BC119a+BC124a)/BC008b"]
[null,null,{"$f":"VLOOKUP($D417,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to electricity input, process 1"},"BC111a","gSO2_eq/MJoutput",null,{"$f":"G23*G29*'Production feedstock1'!G274+G23*G30*'Production feedstock1'!G275","v":0},"= BC026a * BC112a * FP110b + BC026a * BC113a * FP110c"]
[null,null,{"$f":"VLOOKUP($D418,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel/heat input flows, process 1"},"BC114a","gSO2_eq/MJoutput",null,{"$f":"G41*G46*'Production feedstock1'!G274+G41*G47*'Production feedstock1'!G275+G49*G54*'Production feedstock1'!G274+G49*G55*'Production feedstock1'!G275","v":0},"= BC031a1 * BC115a * FP110b + BC031a1 * BC116a * FP110c + BC031a2 * BC117a * FP110b + BC031a2 * BC118a * FP110c"]
[null,null,{"$f":"VLOOKUP($D419,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to material input flows, process 1"},"BC119a","gSO2_eq/MJoutput",null,{"$f":"G63*G69*'Production feedstock1'!G274+G63*G70*'Production feedstock1'!G275+G73*G79*'Production feedstock1'!G274+G73*G80*'Production feedstock1'!G275+G83*G89*'Production feedstock1'!G274+G83*G90*'Production feedstock1'!G275+G93*G98*'Production feedstock1'!G274+G93*G99*'Production feedstock1'!G275+G101*G105*'Production feedstock1'!G274+G101*G106*'Production feedstock1'!G275+G108*G112*'Production feedstock1'!G274+G108*G113*'Production feedstock1'!G275","v":0},"= BC010a1 * BC120a * FP110b + BC010a1 * BC121a * FP110c + BC010a1 * BC122a * FP110b + BC010a1 * BC123a * FP110c + BC010c * BC120c * FP110b + BC010c * BC121c * FP110c"]
[null,null,{"$f":"VLOOKUP($D420,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process emissions, process 1"},"BC124a","gSO2_eq/MJoutput",null,{"$f":"G421*'Production feedstock1'!G274+G422*'Production feedstock1'!G275","v":0},"= BC016a * FP110b + BC016b * FP110c"]
[null,null,{"$f":"VLOOKUP($D421,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 1"},"BC016a","gNOX/MJoutput",{"$f":"VLOOKUP(D421,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F421","v":0}]
[null,null,{"$f":"VLOOKUP($D422,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 1"},"BC016b","gSOX/MJoutput",{"$f":"VLOOKUP(D422,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F422","v":0}]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D424,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to treatment 2 (storage)"},null,"BC059d","gSO2_eq/MJendfuel_fs1",null,null,"= (BC060*BC062d*FP110b+BC060*BC062e*FP110c+BC065*BC067d*FP110b+BC065*BC067e*FP110c)/BC008b"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D426,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process 2"},null,"BC110b","gSO2_eq/MJendfuel_fs1",null,{"$f":"G427+G428+G429+G430","v":0},"= BC111b + BC114b + BC119b+BC124b"]
[null,null,{"$f":"VLOOKUP($D427,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to electricity input, process 2"},"BC111b","gSO2_eq/MJoutput",null,{"$f":"G178*G184*'Production feedstock1'!G274+G178*G185*'Production feedstock1'!G275","v":0},"= BC026b * BC112b * FP110b + BC026b * BC113b * FP110c"]
[null,null,{"$f":"VLOOKUP($D428,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel/heat input flows, process 2"},"BC114b","gSO2_eq/MJoutput",null,{"$f":"G196*G201*'Production feedstock1'!G274+G196*G202*'Production feedstock1'!G275+G204*G209*'Production feedstock1'!G274+G204*G210*'Production feedstock1'!G275","v":0},"= BC031b1 * BC115b * FP110b + BC031b1 * BC116b * FP110c + BC031b2 * BC117b * FP110b + BC031b2 * BC118b * FP110c"]
[null,null,{"$f":"VLOOKUP($D429,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to material input flows, process 2"},"BC119b","gSO2_eq/MJoutput",null,{"$f":"G213*G220*'Production feedstock1'!G274+G213*G221*'Production feedstock1'!G275+G223*G230*'Production feedstock1'!G274+G223*G231*'Production feedstock1'!G275+G234*G239*'Production feedstock1'!G274+G234*G240*'Production feedstock1'!G275+G242*G246*'Production feedstock1'!G274+G242*G247*'Production feedstock1'!G275+G249*G253*'Production feedstock1'!G274+G249*G254*'Production feedstock1'!G275","v":0},"= BC010b1 * BC120b * FP110b + BC010b1 * BC121b * FP110c + BC010b1 * BC122b * FP110b + BC010b1 * BC123b * FP110c + BC010d * BC120d * FP110b + BC010d * BC121d * FP110c"]
[null,null,{"$f":"VLOOKUP($D430,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process emissions, process 2"},"BC124b","gSO2_eq/MJoutput",null,{"$f":"G431*'Production feedstock1'!G274+G432*'Production feedstock1'!G275","v":0},"= BC017a * FP110b + BC017b * FP110c"]
[null,null,{"$f":"VLOOKUP($D431,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 2"},"BC017a","gNOX/MJoutput",{"$f":"VLOOKUP(D431,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F431","v":0}]
[null,null,{"$f":"VLOOKUP($D432,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 2"},"BC017b","gSOX/MJoutput",{"$f":"VLOOKUP(D432,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F432","v":0}]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D434,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with treatment 3 (storage)"},null,"BC069d","gSO2_eq/MJendfuel_fs1",null,{"$f":"G283*G288*'Production feedstock1'!G274+G283*G289*'Production feedstock1'!G275+G290*G295*'Production feedstock1'!G274+G290*G296*'Production feedstock1'!G275","v":0},"= BC070*BC072d*FP110b+BC070*BC072e*FP110c+BC075*BC077d*FP110b+BC075*BC077e*FP110c"]
["Cumulated acidification potential after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D436,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated acidification potential after conversion 1 (per MJ feedstock 1 fuel)"},null,"BC080f","gSO2_eq/MJendfuel_fs1",null,{"$f":"('Production feedstock1'!G277+'Production feedstock1'!G283+'Transport feedstock1'!G186+'Conversion feedstock1'!G416)*'Conversion feedstock1'!G115/100","v":0.8198605978016702},"= (FP114+FP116b+FT016a+BC110a)*BC050a/100"]
["Cumulated acidification potential after allocation 3 (= AP after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D438,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated acidification potential after conversion 2 (per MJ feedstock 1 fuel)"},null,"BC081f","gSO2_eq/MJendfuel_fs1",null,{"$f":"(G436+G424+'Transport feedstock1'!G190+'Conversion feedstock1'!G426)*'Conversion feedstock1'!G256/100","v":0.93522944546204967},"= (BC080f+BC059d+FT016b+BC110b)*BC050b/100"]
["Total cumulated acidification potential feedstock 1 (= AP after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D440,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential feedstock 1 (per MJ feedstock 1 fuel)"},null,"BC082f","gSO2_eq/MJendfuel_fs1",null,{"$f":"G438+G434+'Transport feedstock1'!G194","v":0.93786277735394152},"= BC081f+BC069d+FT016c"]
[null,{"$f":"VLOOKUP($D441,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential feedstock 1 (per MJ functional unit)"},null,"BC083f","gSO2_eq/MJFU",null,{"$f":"G440*'Final conversion'!G68/100*'Final conversion'!G22","v":0.93786277735394152},"= BC082f * FC025c / 100 * FC033"]
["Totally allocated acidification potential from conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D443,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from process 1"},null,"BC090f","gSO2_eq/MJendfuel_fs1",null,{"$f":"G416*G115/100*G256/100","v":0},"= BC110a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D444,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from process 1"},null,"BC091f","gSO2_eq/MJFU",null,{"$f":"G443*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= BC090f * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D445,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from process 2"},null,"BC092f","gSO2_eq/MJendfuel_fs1",null,{"$f":"G426*G256/100","v":0},"= BC110b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D446,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from process 2"},null,"BC093f","gSO2_eq/MJFU",null,{"$f":"G445*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= BC092f * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D447,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from conversion (process 1 + 2)"},null,"BC094f","gSO2_eq/MJendfuel_fs1",null,{"$f":"G443+G445","v":0},"= BC090f + BC092f"]
[null,{"$f":"VLOOKUP($D448,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from conversion (process 1 + 2)"},null,"BC095f","gSO2_eq/MJFU",null,{"$f":"G444+G446","v":0},"= BC091f + BC093f"]
["EUTROPHICATION POTENTIAL"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D451,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process 1"},null,"BC130a","gPO4_eq/MJendfuel_fs1",null,{"$f":"IF(G173=0,(G452+G453+G454+G455)/1,(G452+G453+G454+G455)/G173)","v":1.3755185002841852},"= (BC131a + BC134a + BC139a+BC144a)/BC008b"]
[null,null,{"$f":"VLOOKUP($D452,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to electricity input, process 1"},"BC131a","gPO4_eq/MJoutput",null,{"$f":"G23*G29*'Production feedstock1'!G289","v":0},"= BC026a * BC112a * FP120b"]
[null,null,{"$f":"VLOOKUP($D453,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel/heat input flows, process 1"},"BC134a","gPO4_eq/MJoutput",null,{"$f":"G41*G46*'Production feedstock1'!G289+G49*G54*'Production feedstock1'!G289","v":0},"= BC031a1 * BC115a * FP120b + BC031a2 * BC117a * FP120b"]
[null,null,{"$f":"VLOOKUP($D454,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to material input flows, process 1"},"BC139a","gPO4_eq/MJoutput",null,{"$f":"G63*G69*'Production feedstock1'!G289+G73*G79*'Production feedstock1'!G289+G83*G89*'Production feedstock1'!G289+G93*G98*'Production feedstock1'!G289+G101*G105*'Production feedstock1'!G289+G108*G112*'Production feedstock1'!G289","v":0},"= BC010a1 * BC120a * FP120b + BC010a1 * BC122a * FP120b + BC010c * BC120c * FP120b"]
[null,null,{"$f":"VLOOKUP($D455,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process emissions, process 1"},"BC144a","gPO4_eq/MJoutput",null,{"$f":"G456*'Production feedstock1'!G289+G457*'Production feedstock1'!G290+G458*'Production feedstock1'!G293+G459*'Production feedstock1'!G294+G460*'Production feedstock1'!G297+G461*'Production feedstock1'!G298","v":0.43999999999999995},"= BC016a * FP120b + BC016c * FP120c + BC016d * FP120e + BC016e * FP120f + BC016f * FP120h + BC016g * FP120i"]
[null,null,{"$f":"VLOOKUP($D456,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 1"},"BC016a","gNOX/MJoutput",{"$f":"VLOOKUP(D456,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F456","v":0}]
[null,null,{"$f":"VLOOKUP($D457,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 1"},"BC016c","gNH3/MJoutput",{"$f":"VLOOKUP(D457,Parameters!$1:$2745,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D458,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 1"},"BC016d","gNO3/MJoutput",{"$f":"VLOOKUP(D458,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D459,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 1"},"BC016e","gNH4/MJoutput",{"$f":"VLOOKUP(D459,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D460,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 1"},"BC016f","gPO4/MJoutput",{"$f":"VLOOKUP(D460,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D461,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 1"},"BC016g","gCOD/MJoutput",{"$f":"VLOOKUP(D461,Parameters!$1:$2792,6,FALSE)","v":20},20]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D463,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to treatment 2 (storage)"},null,"BC059e","gPO4_eq/MJendfuel_fs1",null,null,"= (BC060*BC062d*FP120b+BC065*BC067d*FP120b)/BC008b"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D465,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process 2"},null,"BC130b","gPO4_eq/MJendfuel_fs1",null,{"$f":"G466+G467+G468+G469","v":0},"= BC111b + BC114b + BC119b+BC124b"]
[null,null,{"$f":"VLOOKUP($D466,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to electricity input, process 2"},"BC131b","gPO4_eq/MJoutput",null,{"$f":"G178*G184*'Production feedstock1'!G289","v":0},"= BC026b * BC112b * FP120b"]
[null,null,{"$f":"VLOOKUP($D467,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel/heat input flows, process 2"},"BC134b","gPO4_eq/MJoutput",null,{"$f":"G196*G201*'Production feedstock1'!G289+G204*G209*'Production feedstock1'!G289","v":0},"= BC031b1 * BC115b * FP120b + BC031b2 * BC117b * FP120b"]
[null,null,{"$f":"VLOOKUP($D468,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to material input flows, process 2"},"BC139b","gPO4_eq/MJoutput",null,{"$f":"G213*G220*'Production feedstock1'!G289+G223*G230*'Production feedstock1'!G289+G234*G239*'Production feedstock1'!G289+G242*G246*'Production feedstock1'!G289+G249*G253*'Production feedstock1'!G289","v":0},"= BC010b1 * BC120b * FP110b + BC010b1 * BC122b * FP110b + BC010d * BC120d * FP120b"]
[null,null,{"$f":"VLOOKUP($D469,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process emissions, process 2"},"BC144b","gPO4_eq/MJoutput",null,{"$f":"G470*'Production feedstock1'!G289+G471*'Production feedstock1'!G290+G472*'Production feedstock1'!G293+G473*'Production feedstock1'!G294+G474*'Production feedstock1'!G297+G475*'Production feedstock1'!G298","v":0},"= BC017a * FP120b + BC017c * FP120c + BC017d * FP120e + BC017e * FP120f + BC017f * FP120h + BC017g * FP120i"]
[null,null,{"$f":"VLOOKUP($D470,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 2"},"BC017a","gNOX/MJoutput",{"$f":"VLOOKUP(D470,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F470","v":0}]
[null,null,{"$f":"VLOOKUP($D471,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 2"},"BC017c","gNH3/MJoutput",{"$f":"VLOOKUP(D471,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D472,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 2"},"BC017d","gNO3/MJoutput",{"$f":"VLOOKUP(D472,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D473,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 2"},"BC017e","gNH4/MJoutput",{"$f":"VLOOKUP(D473,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D474,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 2"},"BC017f","gPO4/MJoutput",{"$f":"VLOOKUP(D474,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D475,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 2"},"BC017g","gCOD/MJoutput",{"$f":"VLOOKUP(D475,Parameters!$1:$2792,6,FALSE)","v":0},0]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D477,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with treatment 3 (storage)"},null,"BC069e","gPO4_eq/MJendfuel_fs1",null,{"$f":"G283*G288*'Production feedstock1'!G289+G290*G295*'Production feedstock1'!G289","v":0},"= BC070*BC072d*FP120b+BC075*BC077d*FP120b"]
["Cumulated eutrophication potential after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D479,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated eutrophication potential after conversion 1 (per MJ feedstock 1 fuel)"},null,"BC080g","gPO4_eq/MJendfuel_fs1",null,{"$f":"('Production feedstock1'!G300+'Production feedstock1'!G306+'Transport feedstock1'!G209+'Conversion feedstock1'!G451)*'Conversion feedstock1'!G115/100","v":3.3116164621061315},"= (FP124+FP126b+FT017a+BC130a)*BC050a/100"]
["Cumulated eutrophication potential after allocation 3 (= EP after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D481,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated eutrophication potential after conversion 2 (per MJ feedstock 1 fuel)"},null,"BC081g","gPO4_eq/MJendfuel_fs1",null,{"$f":"(G479+G463+'Transport feedstock1'!G213+'Conversion feedstock1'!G465)*'Conversion feedstock1'!G256/100","v":3.325394839691393},"= (BC080g+BC059e+FT017b+BC130b)*BC050b/100"]
["Total cumulated eutrophication potential feedstock 1 (= EP after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D483,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential feedstock 1 (per MJ feedstock 1 fuel)"},null,"BC082g","gPO4_eq/MJendfuel_fs1",null,{"$f":"G481+G477+'Transport feedstock1'!G217","v":3.3257093356913932},"= BC081g+BC069e+FT017c"]
[null,{"$f":"VLOOKUP($D484,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential feedstock 1 (per MJ functional unit)"},null,"BC083g","gPO4_eq/MJFU",null,{"$f":"G483*'Final conversion'!G68/100*'Final conversion'!G22","v":3.3257093356913932},"= BC082g * FC025c / 100 * FC033"]
["Totally allocated eutrophication potential from conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D486,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from process 1"},null,"BC090g","gPO4_eq/MJendfuel_fs1",null,{"$f":"G451*G115/100*G256/100","v":1.3159295156592201},"= BC130a * BC050a / 100 * BC050b / 100"]
[null,{"$f":"VLOOKUP($D487,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from process 1"},null,"BC091g","gPO4_eq/MJFU",null,{"$f":"G486*'Final conversion'!G68/100*'Final conversion'!G22","v":1.3159295156592201},"= BC090g * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D488,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from process 2"},null,"BC092g","gPO4_eq/MJendfuel_fs1",null,{"$f":"G465*G256/100","v":0},"= BC130b * BC050b / 100"]
[null,{"$f":"VLOOKUP($D489,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from process 2"},null,"BC093g","gPO4_eq/MJFU",null,{"$f":"G488*'Final conversion'!G68/100*'Final conversion'!G22","v":0},"= BC092g * FC025c / 100 * FC033"]
[null,{"$f":"VLOOKUP($D490,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from conversion (process 1 + 2)"},null,"BC094g","gPO4_eq/MJendfuel_fs1",null,{"$f":"G486+G488","v":1.3159295156592201},"= BC090f + BC092f"]
[null,{"$f":"VLOOKUP($D491,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from conversion (process 1 + 2)"},null,"BC095g","gPO4_eq/MJFU",null,{"$f":"G487+G489","v":1.3159295156592201},"= BC091f + BC093f"]
[]
["BIODIVERSITY & HIGH CARBON STOCK",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Land with high biodiversity value"]
[null,"N.A."]
["Land with high carbon stock"]
[null,"N.A."]
["Criterium RED"]
[null,"N.A."]
[]
["LOCAL WELL-BEING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Human and property rights, conversion process 1"]
[null,{"$f":"VLOOKUP($D503,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour, process 1"},null,"BC150a","-",{"$f":"VLOOKUP(D503,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F503=\"n.a.\",0,IF(F503=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D504,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour, process 1"},null,"BC150b","-",{"$f":"VLOOKUP(D504,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F504=\"n.a.\",0,IF(F504=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D505,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights, process 1"},null,"BC150c","-",{"$f":"VLOOKUP(D505,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D506,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination, process 1"},null,"BC150d","-",{"$f":"VLOOKUP(D506,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D507,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured, process 1"},null,"BC150e","-"]
[null,{"$f":"VLOOKUP($D508,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 1"},null,"BC150f","-",{"$f":"VLOOKUP(D508,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D509,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security, process 1"},null,"BC150g","-"]
["Labour rights and conditions, conversion process 1"]
[null,{"$f":"VLOOKUP($D511,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts, process 1"},null,"BC151a","-",{"$f":"VLOOKUP(D511,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F511=\"n.a.\",0,IF(F511=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D512,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights, process 1"},null,"BC151b","-",{"$f":"VLOOKUP(D512,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D513,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 1"},null,"BC151c","-",{"$f":"VLOOKUP(D513,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D514,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules, process 1"},null,"BC151d","-",{"$f":"VLOOKUP(D514,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D515,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy, process 1"},null,"BC151e","-",{"$f":"VLOOKUP(D515,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D516,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 1"},null,"BC151f","-",{"$f":"VLOOKUP(D516,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D517,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training, process 1"},null,"BC151g","-",{"$f":"VLOOKUP(D517,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
["Human and property rights, conversion process 2"]
[null,{"$f":"VLOOKUP($D519,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour, process 2"},null,"BC152a","-",{"$f":"VLOOKUP(D519,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F519=\"n.a.\",0,IF(F519=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D520,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour, process 2"},null,"BC152b","-",{"$f":"VLOOKUP(D520,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D521,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights, process 2"},null,"BC152c","-",{"$f":"VLOOKUP(D521,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D522,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination, process 2"},null,"BC152d","-",{"$f":"VLOOKUP(D522,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D523,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured, process 2"},null,"BC152e","-"]
[null,{"$f":"VLOOKUP($D524,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 2"},null,"BC152f","-",{"$f":"VLOOKUP(D524,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F524=\"n.a.\",0,IF(F524=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D525,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security, process 2"},null,"BC152g","-"]
["Labour rights and conditions, conversion process 2"]
[null,{"$f":"VLOOKUP($D527,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts, process 2"},null,"BC153a","-",{"$f":"VLOOKUP(D527,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},{"$f":"IF(F527=\"n.a.\",0,IF(F527=\"Fulfilled\",0,1))","v":1}]
[null,{"$f":"VLOOKUP($D528,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights, process 2"},null,"BC153b","-",{"$f":"VLOOKUP(D528,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D529,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 2"},null,"BC153c","-",{"$f":"VLOOKUP(D529,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D530,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules, process 2"},null,"BC153d","-",{"$f":"VLOOKUP(D530,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D531,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy, process 2"},null,"BC153e","-",{"$f":"VLOOKUP(D531,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D532,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 2"},null,"BC153f","-",{"$f":"VLOOKUP(D532,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
[null,{"$f":"VLOOKUP($D533,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training, process 2"},null,"BC153g","-",{"$f":"VLOOKUP(D533,Parameters!$1:$1958,6,FALSE)","v":"Not fulfilled"},1]
["Human and property rights, total conversion feedstock 1"]
[null,{"$f":"VLOOKUP($D535,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour, processing FS1"},null,"BC154a","-",null,{"$f":"G503+G519","v":2},"= BC150a + BC152a"]
[null,{"$f":"VLOOKUP($D536,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour, processing FS1"},null,"BC154b","-",null,{"$f":"G504+G520","v":2},"= BC150b + BC152b"]
[null,{"$f":"VLOOKUP($D537,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights, processing FS1"},null,"BC154c","-",null,2,"= BC150c + BC152c"]
[null,{"$f":"VLOOKUP($D538,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination, processing FS1"},null,"BC154d","-",null,2,"= BC150d + BC152d"]
[null,{"$f":"VLOOKUP($D539,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured, processing FS1"},null,"BC154e","-"]
[null,{"$f":"VLOOKUP($D540,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, processing FS1"},null,"BC154f","-",null,2,"= BC150f + BC152f"]
[null,{"$f":"VLOOKUP($D541,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security, processing FS1"},null,"BC154g","-"]
["Labour rights and conditions, total conversion feedstock 1"]
[null,{"$f":"VLOOKUP($D543,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts, processing FS1"},null,"BC155a","-",null,{"$f":"G511+G527","v":2},"= BC151a + BC153a"]
[null,{"$f":"VLOOKUP($D544,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights, processing FS1"},null,"BC155b","-",null,{"$f":"G512+G528","v":2},"= BC151b + BC153b"]
[null,{"$f":"VLOOKUP($D545,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, processing FS1"},null,"BC155c","-",null,2,"= BC151c + BC153c"]
[null,{"$f":"VLOOKUP($D546,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules, processing FS1"},null,"BC155d","-",null,2,"= BC151d + BC153d"]
[null,{"$f":"VLOOKUP($D547,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy, processing FS1"},null,"BC155e","-",null,2,"= BC151e + BC153e"]
[null,{"$f":"VLOOKUP($D548,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, processing FS1"},null,"BC155f","-",null,2,"= BC151f + BC153f"]
[null,{"$f":"VLOOKUP($D549,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training, processing FS1"},null,"BC155g","-",null,2,"= BC151g + BC153g"]
["Scores"]
[null,{"$f":"VLOOKUP($D551,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights, process 1_score"},null,"BC156","-",null,{"$f":"SUM(G503:G509)","v":5},"= FP150a + FP150b + FP150c + FP150d + FP150e + FP150f + FP150g"]
[null,{"$f":"VLOOKUP($D552,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions, process 1_score"},null,"BC157","-",null,{"$f":"SUM(G511:G517)","v":7},"= FP151a + FP151b + FP151c + FP151d + FP151e + FP151f + FP151g"]
[null,{"$f":"VLOOKUP($D553,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights, process 2_score"},null,"BC158","-",null,{"$f":"SUM(G519:G525)","v":5},"= FP152a + FP152b + FP152c + FP152d + FP152e + FP152f + FP152g"]
[null,{"$f":"VLOOKUP($D554,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions, process 2_score"},null,"BC159","-",null,{"$f":"SUM(G527:G533)","v":7},"= FP153a + FP153b + FP153c + FP153d + FP153e + FP153f + FP153g"]
[null,{"$f":"VLOOKUP($D555,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights, processing overall_score"},null,"BC160","-",null,{"$f":"G551+G553","v":10},"= BC156 + BC158"]
[null,{"$f":"VLOOKUP($D556,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions, processing overall_score"},null,"BC161","-",null,{"$f":"G552+G554","v":14},"= BC157 + BC159"]

{"sheet":"Conversion feedstock2","index":23,"n_rows":556,"n_cols":8,"rows_kept":556,"cut":false,"hidden":true,"merged":[]}
["Monitoring framework - Conversion feedstock 2 (per year)"]
[null,null,{"$f":"VLOOKUP($D2,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":{"$error":"#N/A"}}]
[null,null,"From input"]
[null,null,"Standard value"]
[null,null,"Calculated from other fields"]
[null,null,"Determines value in other field"]
[]
["MASS BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Feedstock 2 - Conversion process 1",null,null,"BC500a","-",{"$f":"VLOOKUP(D9,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F9","v":"n.a."}]
[null,"Main input flow of process 1"]
[null,null,{"$f":"VLOOKUP($D11,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Pretreated feedstock"},"FP547","-",{"$f":"VLOOKUP(D11,Parameters!$1:$2792,6,FALSE)","v":"No crop"},{"$f":"F11","v":"No crop"}]
[null,null,{"$f":"VLOOKUP($D12,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content pretreated feedstock"},"FP548","%"]
[null,null,{"$f":"VLOOKUP($D13,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content pretreated feedstock"},"FP549","MJ/kgdm",{"$f":"VLOOKUP(F11,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE)","v":0},{"$f":"F13","v":0}]
[null,"Main output flow of process 1"]
[null,null,{"$f":"VLOOKUP($D15,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of main output flow, process 1"},"BC501a","-",{"$f":"VLOOKUP(D15,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F15","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D16,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of main output flow, process 1"},"BC512a","%",{"$f":"VLOOKUP(D16,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F16","v":0}]
[null,null,{"$f":"VLOOKUP($D17,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of main output flow, process 1 (LHV)"},"BC507a","MJ/kgdm",{"$f":"IF(G15=\"n.a.\",0,VLOOKUP(F15,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F17","v":0}]
[null,{"$f":"VLOOKUP($D18,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate (output/input), process 1"},null,"BC508a","MJoutput /MJinput",{"$f":"VLOOKUP(D18,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F18","v":0}]
[null,null,{"$f":"VLOOKUP($D19,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 2 per ha after conversion process 1"},"BC514a","kg/ha",null,{"$f":"G20*100/(100-G16)","v":0},"= BC514b * 100 / (100-BC512a)"]
[null,null,{"$f":"VLOOKUP($D20,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (dry) of feedstock 2 per ha after conversion process 1"},"BC514b","kgdm/ha",null,{"$f":"IF(G17=0,0,G21/G17)","v":0},"= BC514c / BC507a"]
[null,null,{"$f":"VLOOKUP($D21,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of feedstock 2 per ha after conversion process 1"},"BC514c","MJ/ha",null,{"$f":"'Production feedstock2'!G71*'Conversion feedstock2'!G18","v":0},"= FP555c * BC508a"]
[null,"Net electricity input process 1"]
[null,1,{"$f":"VLOOKUP($D23,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of electricity input 1, process 1"},"BC526a","MJe/MJoutput",{"$f":"VLOOKUP(D23,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F23=\"n.a.\",0,F23)","v":0}]
[null,null,{"$f":"VLOOKUP($D24,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity flow 1, process 1"},"BC526a0","MWh/year",{"$f":"VLOOKUP(D24,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F24","v":0}]
[null,null,{"$f":"VLOOKUP($D25,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of electricity flow 1, process 1"},"BC527a","-",{"$f":"VLOOKUP(D25,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F25","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D26,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 1, process 1"},"BC528a","MJfossil/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D27,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production flow 1, process 1"},"BC529a","MJprim/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D28,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 1, process 1"},"BC542a","gCO2eq/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D29,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity flow 1, process 1"},"BC612a","gNOX/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D30,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity flow 1, process 1"},"BC613a","gSOX/MJe",{"$f":"IF(G25=\"n.a.\",0,VLOOKUP(G25, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D31,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of electricity input 2, process 1"},"BC526a1","MJe/MJoutput",{"$f":"VLOOKUP(D31,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F31","v":0}]
[null,null,{"$f":"VLOOKUP($D32,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity flow 2, process 1"},"BC526a10","MWh/year",{"$f":"VLOOKUP(D32,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D33,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of electricity flow 2, process 1"},"BC527a1","-",{"$f":"VLOOKUP(D33,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D34,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 2, process 1"},"BC528a1","MJfossil/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D35,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production flow 2, process 1"},"BC529a1","MJprim/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D36,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 2, process 1"},"BC542a1","gCO2eq/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D37,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity flow 2, process 1"},"BC612a1","gNOX/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D38,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity flow 2, process 1"},"BC613a1","gSOX/MJe",{"$f":"IF(G33=\"n.a.\",0,VLOOKUP(G33, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,"Fuel / heat input"]
[null,1,{"$f":"VLOOKUP($D40,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 1, process 1"},"BC511a1","-",{"$f":"VLOOKUP(D40,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F40","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D41,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat input 1, process 1"},"BC531a1","MJf_h/MJoutput",{"$f":"VLOOKUP(D41,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F41=\"n.a.\",0,F41)","v":0}]
[null,null,{"$f":"VLOOKUP($D42,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fuel/heat flow 1, process 1"},"BC531a10","MJ/year",{"$f":"VLOOKUP(D42,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F42","v":0}]
[null,null,{"$f":"VLOOKUP($D43,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, process 1"},"BC532a1","MJfossil/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F43","v":0}]
[null,null,{"$f":"VLOOKUP($D44,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, process 1"},"BC533a1","MJprim/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D45,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, process 1"},"BC543a1","gCO2_eq/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D46,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 1, process 1"},"BC615a","gNOX/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D47,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 1, process 1"},"BC616a","gSOX/MJf_h",{"$f":"IF(G40=\"n.a.\",0,VLOOKUP(G40, matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D48,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 2, process 1"},"BC511a2","-",{"$f":"VLOOKUP(D48,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D49,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat input 2, process 1"},"BC531a2","MJf_h/MJoutput",{"$f":"VLOOKUP(D49,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F49=\"n.a.\",0,F49)","v":0}]
[null,null,{"$f":"VLOOKUP($D50,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fuel/heat flow 2, process 1"},"BC531a20","MJ/year",{"$f":"VLOOKUP(D50,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F50","v":0}]
[null,null,{"$f":"VLOOKUP($D51,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, process 1"},"BC532a2","MJfossil/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F51","v":0}]
[null,null,{"$f":"VLOOKUP($D52,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, process 1"},"BC533a2","MJprim/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,21,FALSE))","v":0},{"$f":"F52","v":0}]
[null,null,{"$f":"VLOOKUP($D53,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, process 1"},"BC543a2","gCO2_eq/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,9,FALSE))","v":0},{"$f":"F53","v":0}]
[null,null,{"$f":"VLOOKUP($D54,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 2, process 1"},"BC617a","gNOX/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,27,FALSE))","v":0},{"$f":"F54","v":0}]
[null,null,{"$f":"VLOOKUP($D55,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 2, process 1"},"BC618a","gSOX/MJf_h",{"$f":"IF(G48=\"n.a.\",0,VLOOKUP(G48, matrix_standardvalues_fuelsall,29,FALSE))","v":0},{"$f":"F55","v":0}]
[null,"Other material input flows"]
[null,null,{"$f":"VLOOKUP($D57,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of main input,process 1"},"BC509a0","-",{"$f":"VLOOKUP(D57,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F57","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D58,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Main input, process 1"},"BC510a0","kg/year",{"$f":"VLOOKUP(D58,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D59,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of main input, process 1"},"BC510a","kgdm/MJoutput",{"$f":"VLOOKUP(D59,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D60,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for main input, process 1"},"BC536a0","MJprim/kg",{"$f":"IF(G57=\"n.a.\",0,VLOOKUP(G57, matrix_standardvalues,20,FALSE))","v":0},0]
[null,1,{"$f":"VLOOKUP($D61,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 1, process 1"},"BC509a1","-",{"$f":"VLOOKUP(D61,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D62,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material input flow 1, process 1"},"BC510a01","kg/year",{"$f":"VLOOKUP(D62,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D63,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 1, process 1"},"BC510a1","kgdm/MJoutput",{"$f":"VLOOKUP(D63,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F63=\"n.a.\",0,F63)","v":0}]
[null,null,{"$f":"VLOOKUP($D64,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 1, process 1"},"BC510a10","%",{"$f":"VLOOKUP(D64,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F64=\"n.a.\", 0, F64)","v":0}]
[null,null,{"$f":"VLOOKUP($D65,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 1, process 1"},"BC510a11","MJ/kgdm",{"$f":"VLOOKUP(D65,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F65","v":0}]
[null,null,{"$f":"VLOOKUP($D66,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 1, process 1"},"BC535a1","MJfossil/kg",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,10,FALSE))","v":0},{"$f":"F66","v":0}]
[null,null,{"$f":"VLOOKUP($D67,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 1, process 1"},"BC536a1","MJprim/kg",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D68,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, process 1"},"BC547a1","gCO2_eq/kg",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D69,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 1, process 1"},"BC620a","gNOX/kg",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D70,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 1, process 1"},"BC621a","gSOX/kg",{"$f":"IF(G61=\"n.a.\",0,VLOOKUP(G61, matrix_standardvalues,28,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D71,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 2, process 1"},"BC509a2","-",{"$f":"VLOOKUP(D71,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D72,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material input flow 2, process 1"},"BC510a02","kg/year",{"$f":"VLOOKUP(D72,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D73,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 2, process 1"},"BC510a2","kgdm/MJoutput",{"$f":"VLOOKUP(D73,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F73=\"n.a.\",0,F73)","v":0}]
[null,null,{"$f":"VLOOKUP($D74,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 2, process 1"},"BC510a20","%",{"$f":"VLOOKUP(D74,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F74=\"n.a.\", 0, F74)","v":0}]
[null,null,{"$f":"VLOOKUP($D75,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 2, process 1"},"BC510a21","MJ/kgdm",{"$f":"VLOOKUP(D75,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F75","v":0}]
[null,null,{"$f":"VLOOKUP($D76,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 2, process 1"},"BC535a2","MJfossil/kg",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,10,FALSE))","v":0},{"$f":"F76","v":0}]
[null,null,{"$f":"VLOOKUP($D77,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 2, process 1"},"BC536a2","MJprim/kg",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D78,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, process 1"},"BC547a2","gCO2_eq/kg",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D79,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 2, process 1"},"BC622a","gNOX/kg",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D80,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 2, process 1"},"BC623a","gSOX/kg",{"$f":"IF(G71=\"n.a.\",0,VLOOKUP(G71, matrix_standardvalues,28,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D81,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 3, process 1"},"BC509a3","-",{"$f":"VLOOKUP(D81,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D82,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material input flow 3, process 1"},"BC510a03","kg/year",{"$f":"VLOOKUP(D82,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D83,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 3, process 1"},"BC510a3","kgdm/MJoutput",{"$f":"VLOOKUP(D83,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D84,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 3, process 1"},"BC510a30","%",{"$f":"VLOOKUP(D84,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F84=\"n.a.\", 0, F84)","v":0}]
[null,null,{"$f":"VLOOKUP($D85,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 3, process 1"},"BC510a31","MJ/kgdm",{"$f":"VLOOKUP(D85,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F85","v":0}]
[null,null,{"$f":"VLOOKUP($D86,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 3, process 1"},"BC535a3","MJfossil/kg",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,10,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D87,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 3, process 1"},"BC536a3","MJprim/kg",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D88,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 3, process 1"},"BC547a3","gCO2_eq/kg",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D89,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 3, process 1"},"BC625a","gNOX/kg",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D90,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 2, process 1"},"BC626a","gSOX/kg",{"$f":"IF(G81=\"n.a.\",0,VLOOKUP(G81, matrix_standardvalues,28,FALSE))","v":0},0]
[null,"Material output flow"]
[null,null,{"$f":"VLOOKUP($D92,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material output flow, process 1"},"BC509c","-",{"$f":"VLOOKUP(D92,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F92","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D93,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 1"},"BC510c","kgdm/MJoutput",{"$f":"VLOOKUP(D93,Parameters!$1:2807,6,FALSE)","v":0},{"$f":"IF(F93=\"n.a.\",0,F93)","v":0}]
[null,null,{"$f":"VLOOKUP($D94,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material output flow, process 1"},"BC510c0","kg/year",{"$f":"VLOOKUP(D94,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F94","v":0}]
[null,null,{"$f":"VLOOKUP($D95,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material output flow, process 1"},"BC535c","MJfossil/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,10,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D96,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material output flow, process 1"},"BC536c","MJprim/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D97,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material output flow, process 1"},"BC547c","gCO2_eq/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D98,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material output flow, process 1"},"BC620c","gNOX/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D99,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material output flow, process 1"},"BC621c","gSOX/kgdm",{"$f":"IF(G92=\"n.a.\",0,VLOOKUP(G92, matrix_standardvalues,28,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D100,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of output flow, process 1 (electricity)"},"BC509c1","-",{"$f":"VLOOKUP(D100,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F100","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D101,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 1 (electricity)"},"BC510c1","MJe/MJoutput",{"$f":"VLOOKUP(D101,Parameters!$1:2814,6,FALSE)","v":0},{"$f":"IF(F101=\"n.a.\",0,F101)","v":0}]
[null,null,{"$f":"VLOOKUP($D102,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for output flow, process 1 (electricity)"},"BC535c1","MJfossil/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,11,FALSE))","v":0},{"$f":"F102","v":0}]
[null,null,{"$f":"VLOOKUP($D103,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for  output flow, process 1 (electricity)"},"BC536c1","MJprim/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D104,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to output flow, process 1 (electricity)"},"BC547c1","gCO2eq/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D105,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of output flow, process 1 (electricity)"},"BC620c1","gNOX/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D106,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of output flow, process 1 (electricity)"},"BC621c1","gSOX/MJe",{"$f":"IF(G100=\"n.a.\",0,VLOOKUP(G100, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D107,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of output flow, process 1 (heat)"},"BC509c2","-",{"$f":"VLOOKUP(D107,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F107","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D108,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 1 (heat)"},"BC510c2","MJf_h/MJoutput",{"$f":"VLOOKUP(D108,Parameters!$1:2815,6,FALSE)","v":0},{"$f":"IF(F108=\"n.a.\",0,F108)","v":0}]
[null,null,{"$f":"VLOOKUP($D109,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for output flow, process 1 (heat)"},"BC535c2","MJfossil/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F109","v":0}]
[null,null,{"$f":"VLOOKUP($D110,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for output flow, process 1 (heat)"},"BC536c2","MJprim/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,21,FALSE))","v":0},{"$f":"F110","v":0}]
[null,null,{"$f":"VLOOKUP($D111,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to output flow, process 1 (heat)"},"BC547c2","gCO2_eq/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,9,FALSE))","v":0},{"$f":"F111","v":0}]
[null,null,{"$f":"VLOOKUP($D112,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of output flow, process 1 (heat)"},"BC620c2","gNOX/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,27,FALSE))","v":0},{"$f":"F112","v":0}]
[null,null,{"$f":"VLOOKUP($D113,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of output flow, process 1 (heat)"},"BC621c2","gSOX/MJf_h",{"$f":"IF(G107=\"n.a.\",0,VLOOKUP(G107, matrix_standardvalues_fuelsall,29,FALSE))","v":0},{"$f":"F113","v":0}]
[null,"By-products"]
[null,null,{"$f":"VLOOKUP($D115,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to energy crop, process 1"},"BC550a","%",null,{"$f":"100-G116","v":100},"= 1 - BC022a"]
[null,null,{"$f":"VLOOKUP($D116,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-products, process 1"},"BC522a","%",null,{"$f":"G124+G132+G140","v":0},"= BC051a1 + BC051a2+BC051a3"]
[null,1,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 1, process 1"},"BC502a1","-",{"$f":"VLOOKUP(D117,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F117","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D118,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 1, process 1"},"BC502a10","%",{"$f":"VLOOKUP(D118,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F118=\"n.a.\", 0, F118)","v":0}]
[null,null,{"$f":"VLOOKUP($D119,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 1, process 1"},"BC502a11","kg/year",{"$f":"VLOOKUP(D119,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F119","v":0}]
[null,null,{"$f":"VLOOKUP($D120,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (kg)"},"BC503a1","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D121,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, process 1 (MJ)"},"BC504a1","MJbyproduct /MJinput",{"$f":"VLOOKUP(D121,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F121=\"n.a.\", 0, F121)","v":0}]
[null,null,{"$f":"VLOOKUP($D122,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 1, process 1 (LHV)"},"BC505a1","MJ/kgdm",{"$f":"IF(G117=\"n.a.\",0,VLOOKUP(G117, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F122","v":0}]
[null,null,{"$f":"VLOOKUP($D123,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 1, process 1"},"BC506a1","binary",{"$f":"IF(G117=\"n.a.\",0,VLOOKUP(G117, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F123=\"n.a.\", 0, F123)","v":0}]
[null,null,{"$f":"VLOOKUP($D124,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 1, process 1"},"BC551a1","%",null,{"$f":"IF(G123=1,G121/(G121+G129+G137+G142+G146+G18)*100,0)","v":0},"= BC004a1/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
[null,2,{"$f":"VLOOKUP($D125,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 2, process 1"},"BC502a2","-",{"$f":"VLOOKUP(D125,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F125","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D126,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 2, process 1"},"BC502a20","%",{"$f":"VLOOKUP(D126,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F126=\"n.a.\", 0, F126)","v":0}]
[null,null,{"$f":"VLOOKUP($D127,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 2, process 1"},"BC502a21","kg/year",{"$f":"VLOOKUP(D127,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F127","v":0}]
[null,null,{"$f":"VLOOKUP($D128,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (kg)"},"BC503a2","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D129,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, process 1 (MJ)"},"BC504a2","MJbyproduct /MJinput",{"$f":"VLOOKUP(D129,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F129=\"n.a.\", 0, F129)","v":0}]
[null,null,{"$f":"VLOOKUP($D130,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 2, process 1 (LHV)"},"BC505a2","MJ/kgdm",{"$f":"IF(G125=\"n.a.\",0,VLOOKUP(G125, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F130","v":0}]
[null,null,{"$f":"VLOOKUP($D131,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 2, process 1"},"BC506a2","binary",{"$f":"IF(G125=\"n.a.\",0,VLOOKUP(G125, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F131=\"n.a.\", 0, F131)","v":0}]
[null,null,{"$f":"VLOOKUP($D132,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 2, process 1"},"BC551a2","%",null,{"$f":"IF(G131=1,G129/(G129+G121+G137+G142+G146+G18)*100,0)","v":0},"= BC004a2/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
[null,3,{"$f":"VLOOKUP($D133,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 3, process 1"},"BC502a3","-",{"$f":"VLOOKUP(D133,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F133","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D134,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 3, process 1"},"BC502a30","%",{"$f":"VLOOKUP(D134,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F134=\"n.a.\", 0, F134)","v":0}]
[null,null,{"$f":"VLOOKUP($D135,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 3, process 1"},"BC502a31","kg/year",{"$f":"VLOOKUP(D135,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F135","v":0}]
[null,null,{"$f":"VLOOKUP($D136,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (kg)"},"BC503a3","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D137,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 3, process 1 (MJ)"},"BC504a3","MJbyproduct /MJinput",{"$f":"VLOOKUP(D137,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F137=\"n.a.\", 0, F137)","v":0}]
[null,null,{"$f":"VLOOKUP($D138,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 3, process 1 (LHV)"},"BC505a3","MJ/kgdm",{"$f":"IF(G133=\"n.a.\",0,VLOOKUP(G133, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F138","v":0}]
[null,null,{"$f":"VLOOKUP($D139,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 3, process 1"},"BC506a3","binary",{"$f":"IF(G133=\"n.a.\",0,VLOOKUP(G133, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F139=\"n.a.\", 0, F139)","v":0}]
[null,null,{"$f":"VLOOKUP($D140,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 3, process 1"},"BC551a3","%",null,{"$f":"IF(G139=1,G137/(G121+G137+G129+G142+G146+G18)*100,0)","v":0},"= BC004a3/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
[null,4,{"$f":"VLOOKUP($D141,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity by-product, process 1"},"BC502a41","MWh/year",{"$f":"VLOOKUP(D141,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F141=\"n.a.\", 0, F141)","v":0}]
[null,null,{"$f":"VLOOKUP($D142,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of electricity by-product, process 1 (MJ)"},"BC504a4","MJbyproduct /MJinput",{"$f":"VLOOKUP(D142,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F142=\"n.a.\", 0, F142)","v":0}]
[null,null,{"$f":"VLOOKUP($D143,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of electricity by-product, process 1"},"BC506a4","binary",{"$f":"IF(G141=\"n.a.\",1,0)","v":0},{"$f":"IF(F143=\"n.a.\", 0, F143)","v":0}]
[null,null,{"$f":"VLOOKUP($D144,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to electricity by-product, process 1"},"BC551a4","%",null,{"$f":"IF(G143=1,G142/(G121+G137+G129+G142+G146+G18)*100,0)","v":0},"= BC004a4/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
[null,5,{"$f":"VLOOKUP($D145,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat by-product, process 1"},"BC502a51","MJ/year",{"$f":"VLOOKUP(D145,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F145=\"n.a.\", 0, F145)","v":0}]
[null,null,{"$f":"VLOOKUP($D146,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of heat by-product, process 1 (MJ)"},"BC504a5","MJbyproduct /MJinput",{"$f":"VLOOKUP(D146,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F146=\"n.a.\", 0, F146)","v":0}]
[null,null,{"$f":"VLOOKUP($D147,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of heat by-product, process 1"},"BC506a5","binary",{"$f":"IF(G145=\"n.a.\",1,0)","v":0},{"$f":"IF(F147=\"n.a.\", 0, F147)","v":0}]
[null,null,{"$f":"VLOOKUP($D148,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to heat by-product, process 1"},"BC551a5","%",null,{"$f":"IF(G147=1,G146/(G121+G137+G129+G142+G146+G18)*100,0)","v":0},"= BC004a5/(BC004a1+BC004a2+BC004a3+BC004a4+BC004a5+BC008a)*100"]
["Feedstock 2 - Treatment 2",null,null,"LC505","-",{"$f":"VLOOKUP(D149,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F149","v":"n.a."}]
[null,{"$f":"VLOOKUP($D150,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat energy use for treatment 2 (storage)"},null,"BC560","MJh/MJinput",{"$f":"VLOOKUP(D150,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F150=\"n.a.\",0,F150)","v":0}]
[null,{"$f":"VLOOKUP($D151,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat source for treatment 2 (storage)"},null,"BC561","-",{"$f":"VLOOKUP(D151,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F151","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D152,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy use for heat production for treatment 2 (storage)"},"BC562a","MJfossil/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151, matrix_standardvalues_heat,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D153,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy use for heat production for treatment 2 (storage)"},"BC562b","MJprim/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151, matrix_standardvalues_heat,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D154,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to heat production for treatment 2 (storage)"},"BC562c","gCO2eq/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151, matrix_standardvalues_heat,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D155,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific NOx emissions related to heat production for treatment 2 (storage)"},"BC562d","gNOX/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151, matrix_standardvalues_heat,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D156,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific SOx emissions related to heat production for treatment 2 (storage)"},"BC562e","gSOX/MJh",{"$f":"IF(G151=\"n.a.\",0,VLOOKUP(G151, matrix_standardvalues_heat,29,FALSE))","v":0},0]
[null,{"$f":"VLOOKUP($D157,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity energy use for treatment 2 (storage)"},null,"BC565","MJe/MJinput",{"$f":"VLOOKUP(D157,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F157=\"n.a.\",0,F157)","v":0}]
[null,{"$f":"VLOOKUP($D158,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity source for treatment 2 (storage)"},null,"BC566","-",{"$f":"VLOOKUP(D158,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F158","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D159,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy use for electricity production for treatment 2 (storage)"},"BC567a","MJfossil/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D160,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy use for electricity production for treatment 2 (storage)"},"BC567b","MJprim/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D161,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for electricity production for treatment 2 (storage)"},"BC567c","gCO2eq/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D162,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific NOx emissions for electricity production for treatment 2 (storage)"},"BC567d","gNOX/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D163,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific SOx emissions for electricity production for treatment 2 (storage)"},"BC567e","gSOX/MJe",{"$f":"IF(G158=\"n.a.\",0,VLOOKUP(G158, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
["Feedstock 2 - Conversion process 2",null,null,"BC500b","-",{"$f":"VLOOKUP(D164,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,"Main input flow of process 2"]
[null,null,{"$f":"VLOOKUP($D166,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of main output flow, process 1"},"BC501a","-",{"$f":"VLOOKUP(D166,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F166","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D167,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of main output flow, process 1"},"BC512a","%",{"$f":"VLOOKUP(D167,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F167","v":0}]
[null,null,{"$f":"VLOOKUP($D168,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of main output flow, process 1 (LHV)"},"BC507a","MJ/kgdm",{"$f":"IF(G166=\"n.a.\",0,VLOOKUP(G166,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F168","v":0}]
[null,"Main output flow of process 2"]
[null,null,{"$f":"VLOOKUP($D170,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of main output flow, process 2"},"BC501b","-",{"$f":"VLOOKUP(D170,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F170","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D171,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of main output flow, process 2"},"BC512b","%",{"$f":"VLOOKUP(D171,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F171","v":0}]
[null,null,{"$f":"VLOOKUP($D172,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of main output flow, process 2 (LHV)"},"BC507b","MJ/kgdm",{"$f":"IF(G170=\"n.a.\",0,VLOOKUP(G170,matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F172","v":0}]
[null,{"$f":"VLOOKUP($D173,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate (output/input), process 2"},null,"BC508b","MJoutput /MJinput",{"$f":"VLOOKUP(D173,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F173","v":0}]
[null,null,{"$f":"VLOOKUP($D174,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (moist/wet) of feedstock 2 per ha after conversion process 2"},"BC515a","kg/ha",null,{"$f":"G175*100/(100-G171)","v":0},"= BC515b * 100 / (100-BC512b)"]
[null,null,{"$f":"VLOOKUP($D175,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (dry) of feedstock 2 per ha after conversion process 2"},"BC515b","kgdm/ha",null,{"$f":"IF(G172=0,0,G176/G172)","v":0},"= BC515c / BC507b"]
[null,null,{"$f":"VLOOKUP($D176,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Yield rate (energy) of feedstock 2 per ha after conversion process 2"},"BC515c","MJ/ha",null,{"$f":"G21*G173","v":0},"= BC514c * BC508b"]
[null,"Net electricity input process 2"]
[null,1,{"$f":"VLOOKUP($D178,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of electricity input 1, process 2"},"BC526b","MJe/MJoutput",{"$f":"VLOOKUP(D178,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F178=\"n.a.\",0,F178)","v":0}]
[null,null,{"$f":"VLOOKUP($D179,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity flow 1, process 2"},"BC526b0","MWh/year",{"$f":"VLOOKUP(D179,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F179","v":0}]
[null,null,{"$f":"VLOOKUP($D180,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of electricity flow 1, process 2"},"BC527b","-",{"$f":"VLOOKUP(D180,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F180","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D181,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 1, process 2"},"BC528b","MJfossil/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D182,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production flow 1, process 2"},"BC529b","MJprim/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D183,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 1, process 2"},"BC542b","gCO2eq/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D184,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity flow 1, process 2"},"BC612b","gNOX/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D185,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity flow 1, process 2"},"BC613b","gSOX/MJe",{"$f":"IF(G180=\"n.a.\",0,VLOOKUP(G180, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D186,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of electricity input 2, process 2"},"BC526b1","MJe/MJoutput",{"$f":"VLOOKUP(D186,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F186","v":0}]
[null,null,{"$f":"VLOOKUP($D187,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity flow 2, process 2"},"BC526b10","MWh/year",{"$f":"VLOOKUP(D187,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F187","v":0}]
[null,null,{"$f":"VLOOKUP($D188,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of electricity flow 2, process 2"},"BC527b1","-",{"$f":"VLOOKUP(D188,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D189,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production flow 2, process 2"},"BC528b1","MJfossil/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,11,FALSE))","v":0},{"$f":"F189","v":0}]
[null,null,{"$f":"VLOOKUP($D190,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production flow 2, process 2"},"BC529b1","MJprim/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,21,FALSE))","v":0},{"$f":"F190","v":0}]
[null,null,{"$f":"VLOOKUP($D191,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions for external electricity production flow 2, process 2"},"BC542b1","gCO2eq/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,9,FALSE))","v":0},{"$f":"F191","v":0}]
[null,null,{"$f":"VLOOKUP($D192,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity flow 2, process 2"},"BC612b1","gNOX/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,27,FALSE))","v":0},{"$f":"F192","v":0}]
[null,null,{"$f":"VLOOKUP($D193,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity flow 2, process 2"},"BC613b1","gSOX/MJe",{"$f":"IF(G188=\"n.a.\",0,VLOOKUP(G188, matrix_standardvalues_electricity,29,FALSE))","v":0},{"$f":"F193","v":0}]
[null,"Fuel / heat input"]
[null,1,{"$f":"VLOOKUP($D195,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 1, process 2"},"BC511b1","-",{"$f":"VLOOKUP(D195,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F195","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D196,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat input 1, process 2"},"BC531b1","MJf_h/MJoutput",{"$f":"VLOOKUP(D196,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F196=\"n.a.\",0,F196)","v":0}]
[null,null,{"$f":"VLOOKUP($D197,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fuel/heat flow 1, process 2"},"BC531b10","MJ/year",{"$f":"VLOOKUP(D197,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F197","v":0}]
[null,null,{"$f":"VLOOKUP($D198,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, process 2"},"BC532b1","MJfossil/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F198","v":0}]
[null,null,{"$f":"VLOOKUP($D199,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, process 2"},"BC533b1","MJprim/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D200,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, process 2"},"BC543b1","gCO2_eq/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D201,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 1, process 2"},"BC615b","gNOX/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D202,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 1, process 2"},"BC616b","gSOX/MJf_h",{"$f":"IF(G195=\"n.a.\",0,VLOOKUP(G195, matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D203,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 2, process 2"},"BC511b2","-",{"$f":"VLOOKUP(D203,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D204,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat input 2, process 2"},"BC531b2","MJf_h/MJoutput",{"$f":"VLOOKUP(D204,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F204=\"n.a.\",0,F204)","v":0}]
[null,null,{"$f":"VLOOKUP($D205,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fuel/heat flow 2, process 2"},"BC531b20","MJ/year",{"$f":"VLOOKUP(D205,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F205","v":0}]
[null,null,{"$f":"VLOOKUP($D206,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, process 2"},"BC532b2","MJfossil/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F206","v":0}]
[null,null,{"$f":"VLOOKUP($D207,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, process 2"},"BC533b2","MJprim/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,21,FALSE))","v":0},{"$f":"F207","v":0}]
[null,null,{"$f":"VLOOKUP($D208,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, process 2"},"BC543b2","gCO2_eq/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,9,FALSE))","v":0},{"$f":"F208","v":0}]
[null,null,{"$f":"VLOOKUP($D209,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 2, process 2"},"BC617b","gNOX/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,27,FALSE))","v":0},{"$f":"F209","v":0}]
[null,null,{"$f":"VLOOKUP($D210,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 2, process 2"},"BC618b","gSOX/MJf_h",{"$f":"IF(G203=\"n.a.\",0,VLOOKUP(G203, matrix_standardvalues_fuelsall,29,FALSE))","v":0},{"$f":"F210","v":0}]
[null,"Other material input flows"]
[null,1,{"$f":"VLOOKUP($D212,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 1, process 2"},"BC509b1","-",{"$f":"VLOOKUP(D212,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F212","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D213,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 1, process 2"},"BC510b1","kg/MJoutput",{"$f":"VLOOKUP(D213,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F213=\"n.a.\",0,F213)","v":0}]
[null,null,{"$f":"VLOOKUP($D214,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material input flow 1, process 2"},"BC510b10","kg/year",{"$f":"VLOOKUP(D214,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F214","v":0}]
[null,null,{"$f":"VLOOKUP($D215,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 1, process 2"},"BC510b11","%",{"$f":"VLOOKUP(D215,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F215=\"n.a.\", 0, F215)","v":0}]
[null,null,{"$f":"VLOOKUP($D216,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 1, process 2"},"BC510b12","MJ/kgdm",{"$f":"VLOOKUP(D216,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F216","v":0}]
[null,null,{"$f":"VLOOKUP($D217,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 1, process 2"},"BC535b1","MJfossil/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212, matrix_standardvalues_conversioninputs,10,FALSE))","v":0},{"$f":"F217","v":0}]
[null,null,{"$f":"VLOOKUP($D218,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 1, process 2"},"BC536b1","MJprim/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212, matrix_standardvalues_conversioninputs,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D219,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, process 2"},"BC547b1","gCO2_eq/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212, matrix_standardvalues_conversioninputs,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D220,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 1, process 2"},"BC620b","gNOX/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212, matrix_standardvalues_conversioninputs,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D221,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 1, process 2"},"BC621b","gSOX/kg",{"$f":"IF(G212=\"n.a.\",0,VLOOKUP(G212, matrix_standardvalues_conversioninputs,28,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D222,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 2, process 2"},"BC509b2","-",{"$f":"VLOOKUP(D222,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D223,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 2, process 2"},"BC510b2","kg/MJoutput",{"$f":"VLOOKUP(D223,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F223=\"n.a.\",0,F223)","v":0}]
[null,null,{"$f":"VLOOKUP($D224,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material input flow 2, process 2"},"BC510b20","kg/year",{"$f":"VLOOKUP(D224,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F224","v":0}]
[null,null,{"$f":"VLOOKUP($D225,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of material input flow 2, process 2"},"BC510b21","%",{"$f":"VLOOKUP(D225,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F225=\"n.a.\", 0, F225)","v":0}]
[null,null,{"$f":"VLOOKUP($D226,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of input flow 2, process 2"},"BC510b22","MJ/kgdm",{"$f":"VLOOKUP(D226,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F226","v":0}]
[null,null,{"$f":"VLOOKUP($D227,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 2, process 2"},"BC535b2","MJfossil/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,10,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D228,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 2, process 2"},"BC536b2","MJprim/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D229,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, process 2"},"BC547b2","gCO2_eq/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D230,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 2, process 2"},"BC622b","gNOX/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D231,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 2, process 2"},"BC623b","gSOX/kg",{"$f":"IF(G222=\"n.a.\",0,VLOOKUP(G222, matrix_standardvalues_conversioninputs,28,FALSE))","v":0},0]
[null,"Material output flow"]
[null,null,{"$f":"VLOOKUP($D233,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material output flow, process 2"},"BC509d","-",{"$f":"VLOOKUP(D233,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F233","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D234,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 2"},"BC510d","kgdm/MJoutput",{"$f":"VLOOKUP(D234,Parameters!$1:2899,6,FALSE)","v":0},{"$f":"IF(F234=\"n.a.\",0,F234)","v":0}]
[null,null,{"$f":"VLOOKUP($D235,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Material output flow, process 2"},"BC510d0","kg/year",{"$f":"VLOOKUP(D235,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F235","v":0}]
[null,null,{"$f":"VLOOKUP($D236,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material output flow, process 2"},"BC535d","MJfossil/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,10,FALSE))","v":0},{"$f":"F236","v":0}]
[null,null,{"$f":"VLOOKUP($D237,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material output flow, process 2"},"BC536d","MJprim/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D238,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material output flow, process 2"},"BC547d","gCO2_eq/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D239,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material output flow, process 2"},"BC620d","gNOX/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D240,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material output flow, process 2"},"BC621d","gSOX/kgdm",{"$f":"IF(G233=\"n.a.\",0,VLOOKUP(G233, matrix_standardvalues,28,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D241,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of output flow, process 2 (electricity)"},"BC509d1","-",{"$f":"VLOOKUP(D241,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D242,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 2 (electricity)"},"BC510d1","MJe/MJoutput",{"$f":"VLOOKUP(D242,Parameters!$1:2906,6,FALSE)","v":0},{"$f":"IF(F242=\"n.a.\",0,F242)","v":0}]
[null,null,{"$f":"VLOOKUP($D243,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for output flow, process 2 (electricity)"},"BC535d1","MJfossil/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,11,FALSE))","v":0},{"$f":"F243","v":0}]
[null,null,{"$f":"VLOOKUP($D244,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for output flow, process 2 (electricity)"},"BC536d1","MJprim/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D245,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to output flow, process 2 (electricity)"},"BC547d1","gCO2eq/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D246,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of output flow, process 2 (electricity)"},"BC620d1","gNOX/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D247,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of output flow, process 2 (electricity)"},"BC621d1","gSOX/MJe",{"$f":"IF(G241=\"n.a.\",0,VLOOKUP(G241, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D248,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of output flow, process 2 (heat)"},"BC509d2","-",{"$f":"VLOOKUP(D248,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F248","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D249,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material output flow, process 2 (heat)"},"BC510d2","MJf_h/MJoutput",{"$f":"VLOOKUP(D249,Parameters!$1:2907,6,FALSE)","v":0},{"$f":"IF(F249=\"n.a.\",0,F249)","v":0}]
[null,null,{"$f":"VLOOKUP($D250,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for output flow, process 2 (heat)"},"BC535d2","MJfossil/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G247, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F250","v":0}]
[null,null,{"$f":"VLOOKUP($D251,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for output flow, process 2 (heat)"},"BC536d2","MJprim/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,21,FALSE))","v":0},{"$f":"F251","v":0}]
[null,null,{"$f":"VLOOKUP($D252,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to output flow, process 2 (heat)"},"BC547d2","gCO2_eq/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,9,FALSE))","v":0},{"$f":"F252","v":0}]
[null,null,{"$f":"VLOOKUP($D253,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of output flow, process 2 (heat)"},"BC620d2","gNOX/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,27,FALSE))","v":0},{"$f":"F253","v":0}]
[null,null,{"$f":"VLOOKUP($D254,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of output flow, process 2 (heat)"},"BC621d2","gSOX/MJf_h",{"$f":"IF(G248=\"n.a.\",0,VLOOKUP(G248, matrix_standardvalues_fuelsall,29,FALSE))","v":0},{"$f":"F254","v":0}]
[null,"By-products"]
[null,null,{"$f":"VLOOKUP($D256,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to energy crop, process 2"},"BC550b","%",null,{"$f":"100-G257","v":100},"= 1 - BC022b"]
[null,null,{"$f":"VLOOKUP($D257,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-products, process 2"},"BC522b","%",null,{"$f":"G265+G273","v":0},"= BC051b1 + BC051b2"]
[null,1,{"$f":"VLOOKUP($D258,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 1, process 2"},"BC502b1","-",{"$f":"VLOOKUP(D258,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F258","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D259,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 1, process 2"},"BC502b10","%",{"$f":"VLOOKUP(D259,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F259=\"n.a.\", 0, F259)","v":0}]
[null,null,{"$f":"VLOOKUP($D260,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 1, process 2"},"BC502b11","kg/year",{"$f":"VLOOKUP(D260,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F260","v":0}]
[null,null,{"$f":"VLOOKUP($D261,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (kg)"},"BC503b1","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D262,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, process 2 (MJ)"},"BC504b1","MJbyproduct /MJinput",{"$f":"VLOOKUP(D262,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F262=\"n.a.\", 0, F262)","v":0}]
[null,null,{"$f":"VLOOKUP($D263,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 1, process 2 (LHV)"},"BC505b1","MJ/kgdm",{"$f":"IF(G258=\"n.a.\",0,VLOOKUP(G258, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F263","v":0}]
[null,null,{"$f":"VLOOKUP($D264,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 1, process 2"},"BC506b1","binary",{"$f":"IF(G258=\"n.a.\",0,VLOOKUP(G258, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F264=\"n.a.\", 0, F264)","v":0}]
[null,null,{"$f":"VLOOKUP($D265,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 1, process 2"},"BC551b1","%",null,{"$f":"IF(G264=1,G262/(G262+G270+G275+G279+G173)*100,0)","v":0},"= BC004b1/(BC004b1+BC004b2+BC004b4+BC004b5+BC008b)*100"]
[null,2,{"$f":"VLOOKUP($D266,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 2, process 2"},"BC502b2","-",{"$f":"VLOOKUP(D266,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F266","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D267,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 2, process 2"},"BC502b20","%",{"$f":"VLOOKUP(D267,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F267=\"n.a.\", 0, F267)","v":0}]
[null,null,{"$f":"VLOOKUP($D268,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"By-product flow 2, process 2"},"BC502b21","kg/year",{"$f":"VLOOKUP(D268,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F268","v":0}]
[null,null,{"$f":"VLOOKUP($D269,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (kg)"},"BC503b2","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D270,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, process 2 (MJ)"},"BC504b2","MJbyproduct /MJinput",{"$f":"VLOOKUP(D270,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F270=\"n.a.\", 0, F270)","v":0}]
[null,null,{"$f":"VLOOKUP($D271,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 2, process 2 (LHV)"},"BC505b2","MJ/kgdm",{"$f":"IF(G266=\"n.a.\",0,VLOOKUP(G266, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F271","v":0}]
[null,null,{"$f":"VLOOKUP($D272,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 2, process 2"},"BC506b2","binary",{"$f":"IF(G266=\"n.a.\",0,VLOOKUP(G266, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F272=\"n.a.\", 0, F272)","v":0}]
[null,null,{"$f":"VLOOKUP($D273,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 2, process 2"},"BC551b2","%",null,{"$f":"IF(G272=1,G270/(G270+G262+G275+G279+G173)*100,0)","v":0},"= BC004b2/(BC004b1+BC004b2+BC004b4+BC004b5+BC008b)*100"]
[null,4,{"$f":"VLOOKUP($D274,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity by-product, process 2"},"BC502b41","MWh/year",{"$f":"VLOOKUP(D274,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F274","v":0}]
[null,null,{"$f":"VLOOKUP($D275,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of electricity by-product, process 2 (MJ)"},"BC504b4","MJbyproduct /MJinput",{"$f":"VLOOKUP(D275,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F275=\"n.a.\", 0, F275)","v":0}]
[null,null,{"$f":"VLOOKUP($D276,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of electricity by-product, process 2"},"BC506b4","binary",{"$f":"IF(G274=\"n.a.\",1,0)","v":0},{"$f":"IF(F276=\"n.a.\", 0, F276)","v":0}]
[null,null,{"$f":"VLOOKUP($D277,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to electricity by-product, process 2"},"BC551b4","%",null,{"$f":"IF(G276=1,G275/(G270+G262+G275+G279+G173)*100,0)","v":0},"= BC004b4/(BC004b1+BC004b2+BC004b4+BC004b5+BC008b)*100"]
[null,5,{"$f":"VLOOKUP($D278,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat by-product, process 2"},"BC502b51","MJ/year",{"$f":"VLOOKUP(D278,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F278","v":0}]
[null,null,{"$f":"VLOOKUP($D279,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of heat by-product, process 2 (MJ)"},"BC504b5","MJbyproduct /MJinput",{"$f":"VLOOKUP(D279,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F279=\"n.a.\", 0, F279)","v":0}]
[null,null,{"$f":"VLOOKUP($D280,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of heat by-product, process 2"},"BC506b5","binary",{"$f":"IF(G278=\"n.a.\",1,0)","v":0},{"$f":"IF(F280=\"n.a.\", 0, F280)","v":0}]
[null,null,{"$f":"VLOOKUP($D281,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to heat by-product, process 2"},"BC551b5","%",null,{"$f":"IF(G280=1,G279/(G270+G262+G275+G279+G173)*100,0)","v":0},"= BC004b5/(BC004b1+BC004b2+BC004b4+BC004b5+BC008b)*100"]
["Feedstock 2 - Treatment 3",null,null,"LC508","-",{"$f":"VLOOKUP(D282,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F282","v":"n.a."}]
[null,{"$f":"VLOOKUP($D283,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat energy use for treatment 3 (storage)"},null,"BC570","MJh/MJinput",{"$f":"VLOOKUP(D283,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F283=\"n.a.\",0,F283)","v":0}]
[null,{"$f":"VLOOKUP($D284,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Heat source for treatment 3 (storage)"},null,"BC571","-",{"$f":"VLOOKUP(D284,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F284","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D285,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy use for heat production for treatment 3 (storage)"},"BC572a","MJfossil/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D286,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy use for heat production for treatment 3 (storage)"},"BC572b","MJprim/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D287,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to heat production for treatment 3 (storage)"},"BC572c","gCO2eq/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D288,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific NOx emissions related to heat production for treatment 3 (storage)"},"BC572d","gNOX/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D289,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific SOx emissions related to heat production for treatment 3 (storage)"},"BC572e","gSOX/MJh",{"$f":"IF(G284=\"n.a.\",0,VLOOKUP(G284, matrix_standardvalues_heat,29,FALSE))","v":0},0]
[null,{"$f":"VLOOKUP($D290,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity energy use for treatment 3 (storage)"},null,"BC575","MJe/MJinput",{"$f":"VLOOKUP(D290,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F290=\"n.a.\",0,F290)","v":0}]
[null,{"$f":"VLOOKUP($D291,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity source for treatment 3 (storage)"},null,"BC576","-",{"$f":"VLOOKUP(D291,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F291","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D292,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy use for electricity production for treatment 3 (storage)"},"BC577a","MJfossil/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D293,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy use for electricity production for treatment 3 (storage)"},"BC577b","MJprim/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D294,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to electricity production for treatment 3 (storage)"},"BC577c","gCO2eq/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D295,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific NOx emissions related to electricity production for treatment 3 (storage)"},"BC577d","gNOX/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D296,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific SOx emissions related to electricity production for treatment 3 (storage)"},"BC577e","gSOX/MJe",{"$f":"IF(G291=\"n.a.\",0,VLOOKUP(G291, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[]
["ENERGY BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D300,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use in process 1"},null,"BC520a","MJfossil/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G302+G304+G306)/G173)","v":0},"= (BC524a + BC530a + BC535a)/BC508b"]
[null,{"$f":"VLOOKUP($D301,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use in process 1"},null,"BC521a","MJprim/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G303+G305+G307)/G173)","v":0},"= (BC525a + BC534a + BC536a)/BC508b"]
[null,null,{"$f":"VLOOKUP($D302,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to electricity input, process 1"},"BC524a","MJfossil/MJoutput",null,{"$f":"G23*G26","v":0},"= BC526a * BC528a"]
[null,null,{"$f":"VLOOKUP($D303,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to electricity input, process 1"},"BC525a","MJprim/MJoutput",null,{"$f":"G23*G27","v":0},"= BC526a * BC529a"]
[null,null,{"$f":"VLOOKUP($D304,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, process 1"},"BC530a","MJfossil/MJoutput",null,{"$f":"G41*G43+G49*G51","v":0},"= BC531a1 * BC532a1 + BC531a2 * BC532a2"]
[null,null,{"$f":"VLOOKUP($D305,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to fuel/heat input flows, process 1"},"BC534a","MJprim/MJoutput",null,{"$f":"G41*G44+G49*G52","v":0},"= BC531a1 * BC533a1 + BC531a2 * BC533a2"]
[null,null,{"$f":"VLOOKUP($D306,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to material input flows, process 1"},"BC535a","MJfossil/MJoutput",null,{"$f":"G63*G66+G73*G76+G83*G86+G93*G95+G101*G102+G108*G109","v":0},"= BC510a1 * BC535a1 + BC510a2 * BC535a2 + BC510c * BC535c"]
[null,null,{"$f":"VLOOKUP($D307,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to material input flows, process 1"},"BC536a","MJprim/MJoutput",null,{"$f":"G63*G67+G73*G77+G83*G87+G93*G96+G101*G103+G108*G110","v":0},"= BC510a1 * BC536a1 + BC510a2 * BC536a3 + BC510c * BC536c"]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D309,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for treatment 2 (storage)"},null,"BC559a","MJfossil/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G150*G152+G157*G159)/G173)","v":0},"= (BC560*BC562a+BC565*BC567a)/BC508b"]
[null,{"$f":"VLOOKUP($D310,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for treatment 2 (storage)"},null,"BC559b","MJprim/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G150*G153+G157*G160)/G173)","v":0},"= (BC560*BC562b+BC565*BC567b)/BC508b"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D312,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use in process 2"},null,"BC520b","MJfossil/MJendfuel_fs2",null,{"$f":"G314+G316+G318","v":0},"= BC524b + BC530b + BC535b"]
[null,{"$f":"VLOOKUP($D313,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use in process 2"},null,"BC521b","MJprim/MJendfuel_fs2",null,{"$f":"G315+G317+G319","v":0},"= BC525b + BC534b + BC536b"]
[null,null,{"$f":"VLOOKUP($D314,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to electricity input, process 2"},"BC524b","MJfossil/MJoutput",null,{"$f":"G178*G181","v":0},"= BC526b * BC528b"]
[null,null,{"$f":"VLOOKUP($D315,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to electricity input, process 2"},"BC525b","MJprim/MJoutput",null,{"$f":"G178*G182","v":0},"= BC526b * BC529b"]
[null,null,{"$f":"VLOOKUP($D316,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, process 2"},"BC530b","MJfossil/MJoutput",null,{"$f":"G196*G198+G204*G206","v":0},"= BC531b1 * BC532b1 + BC531b2 * BC532b2"]
[null,null,{"$f":"VLOOKUP($D317,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to fuel/heat input flows, process 2"},"BC534b","MJprim/MJoutput",null,{"$f":"G196*G199+G204*G207","v":0},"= BC531b1 * BC533b1 + BC531b2 * BC533b2"]
[null,null,{"$f":"VLOOKUP($D318,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to material input flows, process 2"},"BC535b","MJfossil/MJoutput",null,{"$f":"G213*G217+G223*G227+G234*G236+G242*G243+G249*G250","v":0},"= BC510b1 * BC535b1 + BC510b2 * BC535b2 + BC510d * BC535d"]
[null,null,{"$f":"VLOOKUP($D319,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to material input flows, process 2"},"BC536b","MJprim/MJoutput",null,{"$f":"G213*G218+G223*G228+G234*G237+G242*G244+G249*G251","v":0},"= BC5105b1 * BC536b1 + BC510b2 * BC536b3 + BC510d * BC536d"]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D321,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use for treatment 3 (storage)"},null,"BC569a","MJfossil/MJendfuel_fs2",null,{"$f":"G283*G285+G290*G292","v":0},"= BC570*BC572a+BC575*BC577a"]
[null,{"$f":"VLOOKUP($D322,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use for treatment 3 (storage)"},null,"BC569b","MJprim/MJendfuel_fs2",null,{"$f":"G283*G286+G290*G293","v":0},"= BC570*BC572b+BC575*BC577b"]
["Cumulated energy use after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D324,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated fossil energy use after conversion 1 (per MJ feedstock 2 fuel)"},null,"BC580a","MJfossil/MJendfuel_fs2",null,{"$f":"('Production feedstock2'!G100+'Production feedstock2'!G110+'Transport feedstock2'!G111+'Conversion feedstock2'!G300)*'Conversion feedstock2'!G115/100","v":0},"= (FP532a+FP539a+FT512a+BC520a)*BC550a/100"]
[null,{"$f":"VLOOKUP($D325,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated primary energy use after conversion 1 (per MJ feedstock 2 fuel)"},null,"BC580b","MJprim/MJendfuel_fs2",null,{"$f":"('Production feedstock2'!G101+'Production feedstock2'!G111+'Transport feedstock2'!G112+'Conversion feedstock2'!G301)*'Conversion feedstock2'!G115/100","v":0},"= (FP532b+FP539b+FT512b+BC521a)*BC550a/100"]
["Cumulated energy use after allocation 3 (= energy use after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D327,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated fossil energy use after conversion 2 (per MJ feedstock 2 fuel)"},null,"BC581a","MJfossil/MJendfuel_fs2",null,{"$f":"(G324+G309+'Transport feedstock2'!G119+'Conversion feedstock2'!G312)*'Conversion feedstock2'!G256/100","v":0},"= (BC580a+BC559a+FT513a+BC520b)*BC550b/100"]
[null,{"$f":"VLOOKUP($D328,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated primary energy use after conversion 2 (per MJ feedstock 2 fuel)"},null,"BC581b","MJprim/MJendfuel_fs2",null,{"$f":"(G325+G310+'Transport feedstock2'!G120+'Conversion feedstock2'!G313)*'Conversion feedstock2'!G256/100","v":0},"= (BC580b+BC559b+FT513b+BC521b)*BC550b/100"]
["Total cumulated energy use feedstock 1 (= energy use after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D330,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use feedstock 2 (per MJ feedstock 2 fuel)"},null,"BC582a","MJfossil/MJendfuel_fs2",null,{"$f":"G327+G321+'Transport feedstock2'!G127","v":0},"= BC581a+BC569a+FT514a"]
[null,{"$f":"VLOOKUP($D331,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use feedstock 2 (per MJ feedstock 2 fuel)"},null,"BC582b","MJprim/MJendfuel_fs2",null,{"$f":"G328+G322+'Transport feedstock2'!G128","v":0},"= BC581b+BC569b+FT514b"]
[null,{"$f":"VLOOKUP($D332,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use feedstock 2 (per MJ functional unit)"},null,"BC583a","MJfossil/MJFU",null,{"$f":"G330*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC582a * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D333,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use feedstock 2 (per MJ functional unit)"},null,"BC583b","MJprim/MJFU",null,{"$f":"G331*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC582b * FC025c / 100 * FC034"]
["Totally allocated energy use for conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D335,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in process 1"},null,"BC590a","MJfossil/MJendfuel_fs2",null,{"$f":"G300*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= BC520a * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D336,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in process 1"},null,"BC590b","MJprim/MJendfuel_fs2",null,{"$f":"G301*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100","v":0},"= BC521a * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D337,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in process 1"},null,"BC591a","MJfossil/MJFU",null,{"$f":"G300*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC520a * BC550a / 100 * BC550b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D338,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in process 1"},null,"BC591b","MJprim/MJFU",null,{"$f":"G301*'Conversion feedstock2'!G115/100*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC521a * BC550a / 100 * BC550b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D339,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in process 2"},null,"BC592a","MJfossil/MJendfuel_fs2",null,{"$f":"G312*'Conversion feedstock2'!G256/100","v":0},"= BC520b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D340,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in process 2"},null,"BC592b","MJprim/MJendfuel_fs2",null,{"$f":"G313*'Conversion feedstock2'!G256/100","v":0},"= BC521b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D341,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement in process 2"},null,"BC593a","MJfossil/MJFU",null,{"$f":"G312*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC520b * BC550b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D342,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement in process 2"},null,"BC593b","MJprim/MJFU",null,{"$f":"G313*'Conversion feedstock2'!G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC521b * BC550b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D343,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for conversion (process 1 + 2)"},null,"BC594a","MJfossil/MJendfuel_fs2",null,{"$f":"G335+G339","v":0},"= BC590a + BC592a"]
[null,{"$f":"VLOOKUP($D344,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for conversion (process 1 + 2)"},null,"BC594b","MJprim/MJendfuel_fs2",null,{"$f":"G336+G340","v":0},"= BC590b + BC592b"]
[null,{"$f":"VLOOKUP($D345,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for conversion (process 1 + 2)"},null,"BC595a","MJfossil/MJFU",null,{"$f":"G337+G341","v":0},"= BC591a + BC593a"]
[null,{"$f":"VLOOKUP($D346,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for conversion (process 1 + 2)"},null,"BC595b","MJprim/MJFU",null,{"$f":"G338+G342","v":0},"= BC591b + BC593b"]
[]
["GLOBAL WARMING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D350,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to process 1"},null,"BC537a","gCO2_eq/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G351+G352+G353)/G173)","v":0},"= (BC541a + BC543a + BC547a)/BC508b"]
[null,null,{"$f":"VLOOKUP($D351,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to electricity input, process 1"},"BC541a","gCO2_eq/MJoutput",null,{"$f":"G23*G28","v":0},"= BC526a * BC542a"]
[null,null,{"$f":"VLOOKUP($D352,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to fuel/heat input flows, process 1"},"BC543a","gCO2_eq/MJoutput",null,{"$f":"G41*G45+G49*G53","v":0},"= BC531a1 * BC543a1 + BC531a2 * BC543a2"]
[null,null,{"$f":"VLOOKUP($D353,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to material input flows, process 1"},"BC547a","gCO2_eq/MJoutput",null,{"$f":"G63*G68+G73*G78+G83*G88+G93*G97+G101*G104+G108*G111","v":0},"= BC510a1 * BC547a1 + BC510a2 * BC547a2 + BC510c * BC547c"]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D355,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with treatment 2 (storage)"},null,"BC559c","gCO2_eq/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G150*G154+G157*G161)/G173)","v":0},"= (BC560*BC562c+BC565*BC567c)/BC508b"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D357,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to process 2"},null,"BC537b","gCO2_eq/MJendfuel_fs2",null,{"$f":"G358+G359+G360","v":0},"= BC541b + BC543b + BC547b"]
[null,null,{"$f":"VLOOKUP($D358,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to electricity input, process 2"},"BC541b","gCO2_eq/MJoutput",null,{"$f":"G178*G183","v":0},"= BC526b * BC542b"]
[null,null,{"$f":"VLOOKUP($D359,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to fuel/heat input flows, process 2"},"BC543b","gCO2_eq/MJoutput",null,{"$f":"G196*G200+G204*G208","v":0},"= BC531b1 * BC543b1 + BC531b2 * BC543b2"]
[null,null,{"$f":"VLOOKUP($D360,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to material input flows, process 2"},"BC547b","gCO2_eq/MJoutput",null,{"$f":"G213*G219+G223*G229+G234*G238+G242*G245+G249*G252","v":0},"= BC510b1 * BC547b1 + BC510b2 * BC547b2 + BC510d * BC547d"]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D362,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions associated with treatment 3 (storage)"},null,"BC569c","gCO2_eq/MJendfuel_fs2",null,{"$f":"G283*G287+G290*G294","v":0},"= BC570*BC572c+BC575*BC577c"]
["Cumulated GHG emissions after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D364,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated GHG emissions after conversion 1 (per MJ feedstock 2 fuel)"},null,"BC580c","gCO2_eq/MJendfuel_fs2",null,{"$f":"('Production feedstock2'!G234+'Production feedstock2'!G240+'Transport feedstock2'!G155+'Conversion feedstock2'!G350)*'Conversion feedstock2'!G115/100","v":0},"= (FP557+FP562b+FT515a+BC537a)*BC550a/100"]
["Cumulated GHG emissions after allocation 3 (= GHG emissions after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D366,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated GHG emissions after conversion 2 (per MJ feedstock 2 fuel)"},null,"BC581c","gCO2_eq/MJendfuel_fs2",null,{"$f":"(G364+G355+'Transport feedstock2'!G159+'Conversion feedstock2'!G357)*'Conversion feedstock2'!G256/100","v":0},"= (BC580c+BC559c+FT515b+BC537b)*BC550b/100"]
["Total cumulated GHG emissions feedstock 1 (= GHG emissions after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D368,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions feedstock 2 (per MJ feedstock 2 fuel)"},null,"BC582c","gCO2_eq/MJendfuel_fs2",null,{"$f":"G366+G362+'Transport feedstock2'!G163","v":0},"= BC581c+BC569c+FT515c"]
[null,{"$f":"VLOOKUP($D369,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions feedstock 2 (per MJ functional unit)"},null,"BC583c","gCO2_eq/MJFU",null,{"$f":"G368*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC582c * FC025c / 100 * FC034"]
["Totally allocated GHG emissions for conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D371,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions in process 1"},null,"BC590c","gCO2_eq/MJendfuel_fs2",null,{"$f":"G350*G115/100*G256/100","v":0},"= BC537a * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D372,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions in process 1"},null,"BC591c","gCO2_eq/MJFU",null,{"$f":"G350*G115/100*G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC537a * BC550a / 100 * BC550b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D373,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions in process 2"},null,"BC592c","gCO2_eq/MJendfuel_fs2",null,{"$f":"G357*G256/100","v":0},"= BC537b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D374,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions in process 2"},null,"BC593c","gCO2_eq/MJFU",null,{"$f":"G357*G256/100*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC537b * BC550b / 100 * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D375,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from conversion (process 1 + 2)"},null,"BC594c","gCO2_eq/MJendfuel_fs2",null,{"$f":"G371+G373","v":0},"= BC590c + BC592c"]
[null,{"$f":"VLOOKUP($D376,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from conversion (process 1 + 2)"},null,"BC595c","gCO2_eq/MJFU",null,{"$f":"G372+G374","v":0},"= BC591c + BC593c"]
["Carbon debt & repayment time"]
[null,{"$f":"VLOOKUP($D378,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions feedstock 2 (per MJ feedstock 2 fuel) without LUC emissions"},null,"BC584","gCO2_eq/MJendfuel_fs2",null,{"$f":"(('Production feedstock2'!G245+'Production feedstock2'!G240+'Transport feedstock2'!G155+'Conversion feedstock2'!G350)*'Conversion feedstock2'!G115/100+G355+'Transport feedstock2'!G159+'Conversion feedstock2'!G357)*'Conversion feedstock2'!G256/100+G362+'Transport feedstock2'!G163","v":0},"= ((FP608 + FP562b + FT515a + BC537a) * BC550a / 100 + BC559c + FT515b + BC537b) * BC550b / 100 + BC569c + FT515c"]
[]
[null,"GHG emissions related to materials production, assemblage and recycling *",null,null,"gCO2-eq/conversion plant"]
[]
["RESOURCE USE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["USE OF WATER"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D385,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for conversion process 1"},null,"BC600a","m³/MJoutput",{"$f":"VLOOKUP(D385,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F385","v":0}]
[null,{"$f":"VLOOKUP($D386,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for conversion process 1"},null,"BC600b","m³/GJendfuel_fs2",null,{"$f":"IF(G173=0,0,G385/G173*1000)","v":0},"= BC600a / BC508b * 1000"]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D388,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},null,"BC601a","m³/MJinput",{"$f":"VLOOKUP(D388,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F388","v":0}]
[null,{"$f":"VLOOKUP($D389,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 2 (drying and storage)"},null,"BC601b","m³/GJendfuel_fs2",null,{"$f":"IF(G173=0,0,G388/G173*1000)","v":0},"= BC601a / BC508b * 1000"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D391,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for conversion process 2"},null,"BC602a","m³/MJoutput",{"$f":"VLOOKUP(D391,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F391","v":0}]
[null,{"$f":"VLOOKUP($D392,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for conversion process 2"},null,"BC602b","m³/GJendfuel_fs2",null,{"$f":"G391*1000","v":0},"= BC602a * 1000"]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D394,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},null,"BC603a","m³/MJinput",{"$f":"VLOOKUP(D394,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F394","v":0}]
[null,{"$f":"VLOOKUP($D395,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for feedstock treatment 3 (drying and storage)"},null,"BC603b","m³/GJendfuel_fs2",null,{"$f":"G394*1000","v":0},"= BC603a * 1000"]
["Cumulated water use after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D397,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated water use after conversion 1 (per GJ feedstock 2 fuel)"},null,"BC580d","m³/GJendfuel_fs2",null,{"$f":"('Production feedstock2'!G253+'Production feedstock2'!G259+'Conversion feedstock2'!G386)*'Conversion feedstock2'!G115/100","v":0},"= (FP601+FP603b+BC600b)*BC550a/100"]
["Cumulated GHG emissions after allocation 3 (= water use after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D399,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated water use after conversion 2 (per GJ feedstock 2 fuel)"},null,"BC581d","m³/GJendfuel_fs2",null,{"$f":"(G397+G389+G392)*'Conversion feedstock2'!G256/100","v":0},"= (BC580d+BC601b+BC602b)*BC550b/100"]
["Total cumulated GHG emissions feedstock 1 (= water use after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D401,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use feedstock 2 (per GJ feedstock 2 fuel)"},null,"BC582d","m³/GJendfuel_fs2",null,{"$f":"G399+G395","v":0},"= BC581d+BC603b"]
[null,{"$f":"VLOOKUP($D402,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use feedstock 2 (per GJ functional unit)"},null,"BC583d","m³/GJFU",null,{"$f":"G401*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC582d * FC025c / 100 * FC034"]
["Totally allocated GHG emissions for conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D404,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use in process 1"},null,"BC590d","m³/GJendfuel_fs2",null,{"$f":"G386*G115/100*G256/100","v":0},"= BC600b * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D405,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use in process 1"},null,"BC591d","m³/GJFU",null,{"$f":"G404*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC590d * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D406,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use in process 2"},null,"BC592d","m³/GJendfuel_fs2",null,{"$f":"G392*G256/100","v":0},"= BC602b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D407,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use in process 2"},null,"BC593d","m³/GJFU",null,{"$f":"G406*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC592d * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D408,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use for conversion (process 1 + 2)"},null,"BC594d","m³/GJendfuel_fs2",null,{"$f":"G404+G406","v":0},"= BC590d + BC592d"]
[null,{"$f":"VLOOKUP($D409,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use for conversion (process 1 + 2)"},null,"BC595d","m³/GJFU",null,{"$f":"G405+G407","v":0},"= BC591d + BC593d"]
["USE OF LAND"]
[null,"N.A."]
[]
["ENVIRONMENTAL QUALITY",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["ACIDIFICATION POTENTIAL"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D416,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process 1"},null,"BC610a","gSO2_eq/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G417+G418+G419+G420)/G173)","v":0},"= (BC611a + BC614a + BC619a+BC624a)/BC508b"]
[null,null,{"$f":"VLOOKUP($D417,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to electricity input, process 1"},"BC611a","gSO2_eq/MJoutput",null,{"$f":"G23*G29*'Production feedstock2'!G278+G23*G30*'Production feedstock2'!G279","v":0},"= BC526a * BC612a * FP610b + BC526a * BC613a * FP610c"]
[null,null,{"$f":"VLOOKUP($D418,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel/heat input flows, process 1"},"BC614a","gSO2_eq/MJoutput",null,{"$f":"G41*G46*'Production feedstock2'!G278+G41*G47*'Production feedstock2'!G279+G49*G54*'Production feedstock2'!G278+G49*G55*'Production feedstock2'!G279","v":0},"= BC531a1 * BC615a * FP610b + BC531a1 * BC616a * FP610c + BC531a2 * BC617a * FP610b + BC531a2 * BC618a * FP610c"]
[null,null,{"$f":"VLOOKUP($D419,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to material input flows, process 1"},"BC619a","gSO2_eq/MJoutput",null,{"$f":"G63*G69*'Production feedstock2'!G274+G63*G70*'Production feedstock2'!G275+G73*G79*'Production feedstock2'!G274+G73*G80*'Production feedstock2'!G275+G83*G89*'Production feedstock2'!G274+G83*G90*'Production feedstock2'!G275+G93*G98*'Production feedstock2'!G274+G93*G99*'Production feedstock2'!G275+G101*G105*'Production feedstock2'!G274+G101*G106*'Production feedstock2'!G275+G108*G112*'Production feedstock2'!G274+G108*G113*'Production feedstock2'!G275","v":0},"= BC510a1 * BC620a * FP610b + BC510a1 * BC621a * FP610c + BC510a1 * BC622a * FP610b + BC510a1 * BC623a * FP610c + BC510c * BC620c * FP610b + BC510c * BC621c * FP610c"]
[null,null,{"$f":"VLOOKUP($D420,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process emissions, process 1"},"BC624a","gSO2_eq/MJoutput",null,{"$f":"G421*'Production feedstock2'!G278+G422*'Production feedstock2'!G279","v":0},"= BC516a * FP610b + BC516b * FP610c"]
[null,null,{"$f":"VLOOKUP($D421,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 1"},"BC516a","gNOX/MJoutput",{"$f":"VLOOKUP(D421,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F421","v":0}]
[null,null,{"$f":"VLOOKUP($D422,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 1"},"BC516b","gSOX/MJoutput",{"$f":"VLOOKUP(D422,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F422","v":0}]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D424,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to treatment 2 (storage)"},null,"BC559d","gSO2_eq/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G150*G155*'Production feedstock2'!G278+G150*G156*'Production feedstock2'!G279+G157*G162*'Production feedstock2'!G278+G157*G163*'Production feedstock2'!G279)/G173)","v":0},"= (BC560*BC562d*FP610b+BC560*BC562e*FP610c+BC565*BC567d*FP610b+BC565*BC567d*FP610c)/BC508b"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D426,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process 2"},null,"BC610b","gSO2_eq/MJendfuel_fs2",null,{"$f":"G427+G428+G429+G430","v":0},"= BC611b + BC614b + BC619b+BC624b"]
[null,null,{"$f":"VLOOKUP($D427,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to electricity input, process 2"},"BC611b","gSO2_eq/MJoutput",null,{"$f":"G178*G184*'Production feedstock2'!G278+G178*G185*'Production feedstock2'!G279","v":0},"= BC526b * BC612b * FP610b + BC526b * BC613b * FP610c"]
[null,null,{"$f":"VLOOKUP($D428,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel/heat input flows, process 2"},"BC614b","gSO2_eq/MJoutput",null,{"$f":"G196*G201*'Production feedstock2'!G278+G196*G202*'Production feedstock2'!G279+G204*G209*'Production feedstock2'!G278+G204*G210*'Production feedstock2'!G279","v":0},"= BC531b1 * BC615b * FP610b + BC531b1 * BC616b * FP610c + BC531b2 * BC617b * FP610b + BC531b2 * BC618b * FP610c"]
[null,null,{"$f":"VLOOKUP($D429,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to material input flows, process 2"},"BC619b","gSO2_eq/MJoutput",null,{"$f":"G213*G220*'Production feedstock2'!G274+G213*G221*'Production feedstock2'!G275+G223*G230*'Production feedstock2'!G274+G223*G231*'Production feedstock2'!G275+G234*G239*'Production feedstock2'!G274+G234*G240*'Production feedstock2'!G275+G242*G246*'Production feedstock2'!G274+G242*G247*'Production feedstock2'!G275+G249*G253*'Production feedstock2'!G274+G249*G254*'Production feedstock2'!G275","v":0},"= BC510b1 * BC620b * FP610b + BC510b1 * BC621b * FP610c + BC510b1 * BC622b * FP610b + BC510b1 * BC623b * FP610c + BC510d * BC620d * FP610b + BC510d * BC621d * FP610c"]
[null,null,{"$f":"VLOOKUP($D430,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process emissions, process 2"},"BC624b","gSO2_eq/MJoutput",null,{"$f":"G431*'Production feedstock2'!G278+G432*'Production feedstock2'!G279","v":0},"= BC517a * FP610b + BC517b * FP610c"]
[null,null,{"$f":"VLOOKUP($D431,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 2"},"BC517a","gNOX/MJoutput",{"$f":"VLOOKUP(D431,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F431","v":0}]
[null,null,{"$f":"VLOOKUP($D432,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOX emissions to air (not from material/energy input), conversion process 2"},"BC517b","gSOX/MJoutput",{"$f":"VLOOKUP(D432,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F432","v":0}]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D434,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential associated with treatment 3 (storage)"},null,"BC569d","gSO2_eq/MJendfuel_fs2",null,{"$f":"G283*G288*'Production feedstock2'!G278+G283*G289*'Production feedstock2'!G279+G290*G295*'Production feedstock2'!G278+G290*G296*'Production feedstock2'!G279","v":0},"= BC570*BC572d*FP610b+BC570*BC572e*FP610c+BC575*BC577d*FP610b+BC575*BC577e*FP610c"]
["Cumulated acidification potential after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D436,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated acidification potential after conversion 1 (per MJ feedstock 2 fuel)"},null,"BC580f","gSO2_eq/MJendfuel_fs2",null,{"$f":"('Production feedstock2'!G277+'Production feedstock2'!G283+'Transport feedstock2'!G186+'Conversion feedstock2'!G416)*'Conversion feedstock2'!G115/100","v":0},"= (FP614+FP616b+FT516a+BC610a)*BC550a/100"]
["Cumulated acidification potential after allocation 3 (= AP after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D438,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated acidification potential after conversion 2 (per MJ feedstock 2 fuel)"},null,"BC581f","gSO2_eq/MJendfuel_fs2",null,{"$f":"(G436+G424+'Transport feedstock2'!G190+'Conversion feedstock2'!G426)*'Conversion feedstock2'!G256/100","v":0},"= (BC580f+BC559d+FT516b+BC610b)*BC550b/100"]
["Total cumulated acidification potential feedstock 1 (= AP after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D440,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential feedstock 2 (per MJ feedstock 2 fuel)"},null,"BC582f","gSO2_eq/MJendfuel_fs2",null,{"$f":"G438+G434+'Transport feedstock2'!G194","v":0},"= BC581f+BC569d+FT516c"]
[null,{"$f":"VLOOKUP($D441,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential feedstock 2 (per MJ functional unit)"},null,"BC583f","gSO2_eq/MJFU",null,{"$f":"G440*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC582f * FC025c / 100 * FC034"]
["Totally allocated acidification potential from conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D443,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from process 1"},null,"BC590f","gSO2_eq/MJendfuel_fs2",null,{"$f":"G416*G115/100*G256/100","v":0},"= BC610a * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D444,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from process 1"},null,"BC591f","gSO2_eq/MJFU",null,{"$f":"G443*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC590f * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D445,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from process 2"},null,"BC592f","gSO2_eq/MJendfuel_fs2",null,{"$f":"G426*G256/100","v":0},"= BC610b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D446,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from process 2"},null,"BC593f","gSO2_eq/MJFU",null,{"$f":"G445*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC692f * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D447,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from conversion (process 1 + 2)"},null,"BC594f","gSO2_eq/MJendfuel_fs2",null,{"$f":"G443+G445","v":0},"= BC590f + BC592f"]
[null,{"$f":"VLOOKUP($D448,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from conversion (process 1 + 2)"},null,"BC595f","gSO2_eq/MJFU",null,{"$f":"G444+G446","v":0},"= BC591f + BC593f"]
["EUTROPHICATION POTENTIAL"]
["Conversion process 1"]
[null,{"$f":"VLOOKUP($D451,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process 1"},null,"BC630a","gPO4_eq/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G452+G453+G454+G455)/G173)","v":0},"= (BC631a + BC634a + BC639a+BC644a)/BC508b"]
[null,null,{"$f":"VLOOKUP($D452,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to electricity input, process 1"},"BC631a","gPO4_eq/MJoutput",null,{"$f":"G23*G29*'Production feedstock2'!G289","v":0},"= BC526a * BC612a * FP620b"]
[null,null,{"$f":"VLOOKUP($D453,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel/heat input flows, process 1"},"BC634a","gPO4_eq/MJoutput",null,{"$f":"G41*G46*'Production feedstock2'!G289+G49*G54*'Production feedstock2'!G289","v":0},"= BC531a1 * BC615a * FP620b + BC531a2 * BC617a * FP620b"]
[null,null,{"$f":"VLOOKUP($D454,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to material input flows, process 1"},"BC639a","gPO4_eq/MJoutput",null,{"$f":"G63*G69*'Production feedstock2'!G289+G73*G79*'Production feedstock2'!G289+G83*G89*'Production feedstock2'!G289+G93*G98*'Production feedstock2'!G289+G101*G105*'Production feedstock2'!G289+G108*G112*'Production feedstock2'!G289","v":0},"= BC510a1 * BC620a * FP620b + BC510a1 * BC622a * FP620b + BC510c * BC620c * FP620b"]
[null,null,{"$f":"VLOOKUP($D455,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process emissions, process 1"},"BC644a","gPO4_eq/MJoutput",null,{"$f":"G456*'Production feedstock2'!G289+G457*'Production feedstock2'!G290+G458*'Production feedstock2'!G293+G459*'Production feedstock2'!G294+G460*'Production feedstock2'!G297+G461*'Production feedstock2'!G298","v":0},"= BC516a * FP620b + BC516c * FP620c + BC516d * FP620e + BC516e * FP620f + BC516f * FP620h + BC516g * FP620i"]
[null,null,{"$f":"VLOOKUP($D456,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 1"},"BC516a","gNOX/MJoutput",{"$f":"VLOOKUP(D456,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F456","v":0}]
[null,null,{"$f":"VLOOKUP($D457,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 1"},"BC516c","gNH3/MJoutput",{"$f":"VLOOKUP(D457,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D458,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 1"},"BC516d","gNO3/MJoutput",{"$f":"VLOOKUP(D458,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D459,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 1"},"BC516e","gNH4/MJoutput",{"$f":"VLOOKUP(D459,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D460,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 1"},"BC516f","gPO4/MJoutput",{"$f":"VLOOKUP(D460,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D461,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 1"},"BC516g","gCOD/MJoutput",{"$f":"VLOOKUP(D461,Parameters!$1:$2792,6,FALSE)","v":0},0]
["Feedstock treatment 2"]
[null,{"$f":"VLOOKUP($D463,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to treatment 2 (storage)"},null,"BC559e","gPO4_eq/MJendfuel_fs2",null,{"$f":"IF(G173=0,0,(G150*G155*'Production feedstock2'!G289+G157*G162*'Production feedstock2'!G289)/G173)","v":0},"= (BC560*BC562d*FP620b+BC565*BC567d*FP620b)/BC508b"]
["Conversion process 2"]
[null,{"$f":"VLOOKUP($D465,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process 2"},null,"BC630b","gPO4_eq/MJendfuel_fs2",null,{"$f":"G466+G467+G468+G469","v":0},"= BC611b + BC614b + BC619b+BC624b"]
[null,null,{"$f":"VLOOKUP($D466,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to electricity input, process 2"},"BC631b","gPO4_eq/MJoutput",null,{"$f":"G178*G184*'Production feedstock2'!G289","v":0},"= BC526b * BC612b * FP620b"]
[null,null,{"$f":"VLOOKUP($D467,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel/heat input flows, process 2"},"BC634b","gPO4_eq/MJoutput",null,{"$f":"G196*G201*'Production feedstock2'!G289+G204*G209*'Production feedstock2'!G289","v":0},"= BC531b1 * BC615b * FP620b + BC531b2 * BC617b * FP620b"]
[null,null,{"$f":"VLOOKUP($D468,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to material input flows, process 2"},"BC639b","gPO4_eq/MJoutput",null,{"$f":"G213*G220*'Production feedstock2'!G289+G223*G230*'Production feedstock2'!G289+G234*G239*'Production feedstock2'!G289+G242*G246*'Production feedstock2'!G289+G249*G253*'Production feedstock2'!G289","v":0},"= BC510b1 * BC620b * FP610b + BC510b1 * BC622b * FP610b + BC510d * BC620d * FP620b"]
[null,null,{"$f":"VLOOKUP($D469,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process emissions, process 2"},"BC644b","gPO4_eq/MJoutput",null,{"$f":"G470*'Production feedstock2'!G289+G471*'Production feedstock2'!G290+G472*'Production feedstock2'!G293+G473*'Production feedstock2'!G294+G474*'Production feedstock2'!G297+G475*'Production feedstock2'!G298","v":0},"= BC517a * FP620b + BC517c * FP620c + BC517d * FP620e + BC517e * FP620f + BC517f * FP620h + BC517g * FP620i"]
[null,null,{"$f":"VLOOKUP($D470,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), conversion process 2"},"BC517a","gNOX/MJoutput",{"$f":"VLOOKUP(D470,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F470","v":0}]
[null,null,{"$f":"VLOOKUP($D471,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), conversion process 2"},"BC517c","gNH3/MJoutput",{"$f":"VLOOKUP(D471,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D472,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), conversion process 2"},"BC517d","gNO3/MJoutput",{"$f":"VLOOKUP(D472,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D473,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), conversion process 2"},"BC517e","gNH4/MJoutput",{"$f":"VLOOKUP(D473,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D474,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), conversion process 2"},"BC517f","gPO4/MJoutput",{"$f":"VLOOKUP(D474,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D475,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"COD emissions to water (not from material/energy input), conversion process 2"},"BC517g","gCOD/MJoutput",{"$f":"VLOOKUP(D475,Parameters!$1:$2792,6,FALSE)","v":0},0]
["Feedstock treatment 3"]
[null,{"$f":"VLOOKUP($D477,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential associated with treatment 3 (storage)"},null,"BC569e","gPO4_eq/MJendfuel_fs2",null,{"$f":"G283*G288*'Production feedstock2'!G289+G290*G295*'Production feedstock2'!G289","v":0},"= BC570*BC572d*FP620b+BC575*BC577d*FP620b"]
["Cumulated eutrophication potential after allocation 2 (= production + t&t 1 + conversion 1)"]
[null,{"$f":"VLOOKUP($D479,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated eutrophication potential after conversion 1 (per MJ feedstock 2 fuel)"},null,"BC580g","gPO4_eq/MJendfuel_fs2",null,{"$f":"('Production feedstock2'!G300+'Production feedstock2'!G306+'Transport feedstock2'!G209+'Conversion feedstock2'!G451)*'Conversion feedstock2'!G115/100","v":0},"= (FP624+FP626b+FT517a+BC630a)*BC550a/100"]
["Cumulated acidification potential after allocation 3 (= EP after allocation 2 + t&t 2 + conversion 2)"]
[null,{"$f":"VLOOKUP($D481,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocated eutrophication potential after conversion 2 (per MJ feedstock 2 fuel)"},null,"BC581g","gPO4_eq/MJendfuel_fs2",null,{"$f":"(G479+G463+'Transport feedstock2'!G213+'Conversion feedstock2'!G465)*'Conversion feedstock2'!G256/100","v":0},"= (BC580g+BC559e+FT517b+BC630b)*BC550b/100"]
["Total cumulated acidification potential feedstock 1 (= EP after allocation 3 + t&t 3)"]
[null,{"$f":"VLOOKUP($D483,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential feedstock 2 (per MJ feedstock 2 fuel)"},null,"BC582g","gPO4_eq/MJendfuel_fs2",null,{"$f":"G481+G477+'Transport feedstock2'!G217","v":0},"= BC581g+BC569e+FT517c"]
[null,{"$f":"VLOOKUP($D484,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential feedstock 2 (per MJ functional unit)"},null,"BC583g","gPO4_eq/MJFU",null,{"$f":"G483*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC582g * FC025c / 100 * FC034"]
["Totally allocated eutrophication potential from conversion (1, 2, 1+2)"]
[null,{"$f":"VLOOKUP($D486,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from process 1"},null,"BC590g","gPO4_eq/MJendfuel_fs2",null,{"$f":"G451*G115/100*G256/100","v":0},"= BC630a * BC550a / 100 * BC550b / 100"]
[null,{"$f":"VLOOKUP($D487,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from process 1"},null,"BC591g","gPO4_eq/MJFU",null,{"$f":"G486*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC590g * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D488,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from process 2"},null,"BC592g","gPO4_eq/MJendfuel_fs2",null,{"$f":"G465*G256/100","v":0},"= BC630b * BC550b / 100"]
[null,{"$f":"VLOOKUP($D489,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from process 2"},null,"BC593g","gPO4_eq/MJFU",null,{"$f":"G488*'Final conversion'!G68/100*'Final conversion'!G23","v":0},"= BC592g * FC025c / 100 * FC034"]
[null,{"$f":"VLOOKUP($D490,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from conversion (process 1 + 2)"},null,"BC594g","gPO4_eq/MJendfuel_fs2",null,{"$f":"G486+G488","v":0},"= BC590f + BC592f"]
[null,{"$f":"VLOOKUP($D491,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from conversion (process 1 + 2)"},null,"BC595g","gPO4_eq/MJFU",null,{"$f":"G487+G489","v":0},"= BC591f + BC593f"]
[]
["BIODIVERSITY & HIGH CARBON STOCK",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Land with high biodiversity value"]
[null,"N.A."]
["Land with high carbon stock"]
[null,"N.A."]
["Criterium RED"]
[null,"N.A."]
[]
["LOCAL WELL-BEING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Human and property rights, conversion process 1"]
[null,{"$f":"VLOOKUP($D503,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour, process 1"},null,"BC650a","-",{"$f":"VLOOKUP(D503,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F503=\"n.a.\",0,IF(F503=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D504,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour, process 1"},null,"BC650b","-",{"$f":"VLOOKUP(D504,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F504=\"n.a.\",0,IF(F504=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D505,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights, process 1"},null,"BC650c","-",{"$f":"VLOOKUP(D505,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D506,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination, process 1"},null,"BC650d","-",{"$f":"VLOOKUP(D506,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D507,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured, process 1"},null,"BC650e","-",{"$f":"VLOOKUP(D507,Parameters!$1:$1958,6,FALSE)","v":0}]
[null,{"$f":"VLOOKUP($D508,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 1"},null,"BC650f","-",{"$f":"VLOOKUP(D508,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D509,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security, process 1"},null,"BC650g","-",{"$f":"VLOOKUP(D509,Parameters!$1:$1958,6,FALSE)","v":0}]
["Labour rights and conditions, conversion process 1"]
[null,{"$f":"VLOOKUP($D511,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts, process 1"},null,"BC651a","-",{"$f":"VLOOKUP(D511,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F511=\"n.a.\",0,IF(F511=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D512,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights, process 1"},null,"BC651b","-",{"$f":"VLOOKUP(D512,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D513,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 1"},null,"BC651c","-",{"$f":"VLOOKUP(D513,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D514,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules, process 1"},null,"BC651d","-",{"$f":"VLOOKUP(D514,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D515,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy, process 1"},null,"BC651e","-",{"$f":"VLOOKUP(D515,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D516,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 1"},null,"BC651f","-",{"$f":"VLOOKUP(D516,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D517,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training, process 1"},null,"BC651g","-",{"$f":"VLOOKUP(D517,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
["Human and property rights, conversion process 2"]
[null,{"$f":"VLOOKUP($D519,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour, process 2"},null,"BC652a","-",{"$f":"VLOOKUP(D519,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F519=\"n.a.\",0,IF(F519=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D520,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour, process 2"},null,"BC652b","-",{"$f":"VLOOKUP(D520,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D521,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights, process 2"},null,"BC652c","-",{"$f":"VLOOKUP(D521,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D522,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination, process 2"},null,"BC652d","-",{"$f":"VLOOKUP(D522,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D523,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured, process 2"},null,"BC652e","-",{"$f":"VLOOKUP(D523,Parameters!$1:$1958,6,FALSE)","v":0}]
[null,{"$f":"VLOOKUP($D524,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, process 2"},null,"BC652f","-",{"$f":"VLOOKUP(D524,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F524=\"n.a.\",0,IF(F524=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D525,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security, process 2"},null,"BC652g","-",{"$f":"VLOOKUP(D525,Parameters!$1:$1958,6,FALSE)","v":0}]
["Labour rights and conditions, conversion process 2"]
[null,{"$f":"VLOOKUP($D527,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts, process 2"},null,"BC653a","-",{"$f":"VLOOKUP(D527,Parameters!$1:$1958,6,FALSE)","v":"n.a."},{"$f":"IF(F527=\"n.a.\",0,IF(F527=\"Fulfilled\",0,1))","v":0}]
[null,{"$f":"VLOOKUP($D528,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights, process 2"},null,"BC653b","-",{"$f":"VLOOKUP(D528,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D529,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, process 2"},null,"BC653c","-",{"$f":"VLOOKUP(D529,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D530,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules, process 2"},null,"BC653d","-",{"$f":"VLOOKUP(D530,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D531,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy, process 2"},null,"BC653e","-",{"$f":"VLOOKUP(D531,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D532,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, process 2"},null,"BC653f","-",{"$f":"VLOOKUP(D532,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
[null,{"$f":"VLOOKUP($D533,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training, process 2"},null,"BC653g","-",{"$f":"VLOOKUP(D533,Parameters!$1:$1958,6,FALSE)","v":"n.a."},0]
["Human and property rights, total conversion feedstock 1"]
[null,{"$f":"VLOOKUP($D535,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour, processing FS2"},null,"BC654a","-",null,{"$f":"G503+G519","v":0},"= BC650a + BC652a"]
[null,{"$f":"VLOOKUP($D536,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour, processing FS2"},null,"BC654b","-",null,{"$f":"G504+G520","v":0},"= BC650b + BC652b"]
[null,{"$f":"VLOOKUP($D537,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights, processing FS2"},null,"BC654c","-",null,0,"= BC650c + BC652c"]
[null,{"$f":"VLOOKUP($D538,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination, processing FS2"},null,"BC654d","-",null,0,"= BC650d + BC652d"]
[null,{"$f":"VLOOKUP($D539,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured, processing FS2"},null,"BC654e","-"]
[null,{"$f":"VLOOKUP($D540,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, processing FS2"},null,"BC654f","-",null,0,"= BC650f + BC652f"]
[null,{"$f":"VLOOKUP($D541,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security, processing FS2"},null,"BC654g","-"]
["Labour rights and conditions, total conversion feedstock 1"]
[null,{"$f":"VLOOKUP($D543,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts, processing FS2"},null,"BC655a","-",null,{"$f":"G511+G527","v":0},"= BC651a + BC653a"]
[null,{"$f":"VLOOKUP($D544,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights, processing FS2"},null,"BC655b","-",null,{"$f":"G512+G528","v":0},"= BC651b + BC653b"]
[null,{"$f":"VLOOKUP($D545,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, processing FS2"},null,"BC655c","-",null,0,"= BC651c + BC653c"]
[null,{"$f":"VLOOKUP($D546,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules, processing FS2"},null,"BC655d","-",null,0,"= BC651d + BC653d"]
[null,{"$f":"VLOOKUP($D547,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy, processing FS2"},null,"BC655e","-",null,0,"= BC651e + BC653e"]
[null,{"$f":"VLOOKUP($D548,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, processing FS2"},null,"BC655f","-",null,0,"= BC651f + BC653f"]
[null,{"$f":"VLOOKUP($D549,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training, processing FS2"},null,"BC655g","-",null,0,"= BC651g + BC653g"]
["Scores"]
[null,{"$f":"VLOOKUP($D551,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights, process 1_score"},null,"BC656","-",null,{"$f":"SUM(G503:G509)","v":0},"= FP650a + FP650b + FP650c + FP650d + FP650e + FP650f + FP650g"]
[null,{"$f":"VLOOKUP($D552,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions, process 1_score"},null,"BC657","-",null,{"$f":"SUM(G511:G517)","v":0},"= FP651a + FP651b + FP651c + FP651d + FP651e + FP651f + FP651g"]
[null,{"$f":"VLOOKUP($D553,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights, process 2_score"},null,"BC658","-",null,{"$f":"SUM(G519:G525)","v":0},"= FP652a + FP652b + FP652c + FP652d + FP652e + FP652f + FP652g"]
[null,{"$f":"VLOOKUP($D554,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions, process 2_score"},null,"BC659","-",null,{"$f":"SUM(G527:G533)","v":0},"= FP653a + FP653b + FP653c + FP653d + FP653e + FP653f + FP653g"]
[null,{"$f":"VLOOKUP($D555,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights, processing overall_score"},null,"BC660","-",null,{"$f":"G551+G553","v":0},"= BC656 + BC658"]
[null,{"$f":"VLOOKUP($D556,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions, processing overall_score"},null,"BC661","-",null,{"$f":"G552+G554","v":0},"= BC657 + BC659"]

{"sheet":"Final conversion","index":24,"n_rows":314,"n_cols":8,"rows_kept":314,"cut":false,"hidden":true,"merged":[]}
["Monitoring framework - Final conversion (Electricity and/or heat production) (per year)"]
[]
[null,null,"From input"]
[null,null,"Standard value"]
[null,null,"Calculated from other fields"]
[null,null,"Determines value in other field"]
[]
["MASS BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
[{"$f":"VLOOKUP($D9,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Final conversion process"},null,null,"FC000","-",{"$f":"VLOOKUP(D9,Parameters!$1:$2792,6,FALSE)","v":"No final conversion"},{"$f":"F9","v":"No final conversion"}]
[null,{"$f":"VLOOKUP($D10,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of input flow, feedstock 1"},null,"FC001a","-",{"$f":"VLOOKUP(D10,Parameters!$1:$2792,6,FALSE)","v":"Liquid biomethane (LBM)"},"Liquid biomethane (LBM)"]
[null,null,{"$f":"VLOOKUP($D11,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Share of input flow 1 (caloric)"},"FC002a","%",{"$f":"VLOOKUP(D11,Parameters!$1:$2792,6,FALSE)","v":100},100]
[null,{"$f":"VLOOKUP($D12,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of input flow, feedstock 2"},null,"FC001b","-",{"$f":"VLOOKUP(D12,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D13,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Share of input flow 2 (caloric)"},"FC002b","%",{"$f":"VLOOKUP(D13,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,{"$f":"VLOOKUP($D14,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Net electrical efficiency, final conversion"},null,"FC003a","%",{"$f":"VLOOKUP(D14,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F14","v":0}]
[null,{"$f":"VLOOKUP($D15,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Net thermal efficiency, final conversion"},null,"FC003b","%",{"$f":"VLOOKUP(D15,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,{"$f":"VLOOKUP($D16,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Net conversion efficiency, final conversion - other than electricity or heat"},null,"FC003c","%",{"$f":"VLOOKUP(D16,Parameters!$1:$2792,6,FALSE)","v":100},100]
[null,{"$f":"VLOOKUP($D17,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Gross electrical efficiency, final conversion"},null,"FC037a","%",{"$f":"VLOOKUP(D17,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F17","v":0}]
[null,{"$f":"VLOOKUP($D18,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Gross thermal efficiency, final conversion"},null,"FC037b","%",{"$f":"VLOOKUP(D18,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,{"$f":"VLOOKUP($D19,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Functional unit"},null,"FC030","-",{"$f":"VLOOKUP(D19,Parameters!$1:$2792,6,FALSE)","v":"MJ diesel"},"MJ diesel"]
[null,{"$f":"VLOOKUP($D20,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Output heat per MJ functional unit"},null,"FC031","MJh/MJFU",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,IF(G19=\"MJ heat\",1,1*G15/G14)))))","v":0}]
[null,{"$f":"VLOOKUP($D21,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Output electricity per MJ functional unit"},null,"FC032","MJe/MJFU",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,IF(G19=\"MJ electricity\",1,1*G14/G15)))))","v":0}]
[null,{"$f":"VLOOKUP($D22,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input feedstock 1 per MJ functional unit"},null,"FC033","MJ/MJFU",null,{"$f":"IF(G19=\"MJ gas\",G11/G16,IF(G19=\"MJ diesel\",G11/G16,IF(G19=\"MJ gasoline\",G11/G16,IF(G19=\"MJ heavy fuel oil\",G11/G16,IF(G19=\"MJ heat\",G11/G15,G11/G14)))))","v":1}]
[null,{"$f":"VLOOKUP($D23,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Input feedstock 2 per MJ functional unit"},null,"FC034","MJ/MJFU",null,{"$f":"IF(G19=\"MJ gas\",G13/G16,IF(G19=\"MJ diesel\",G13/G16,IF(G19=\"MJ gasoline\",G13/G16,IF(G19=\"MJ heavy fuel oil\",G13/G16,IF(G19=\"MJ heat\",G13/G15,G13/G14)))))","v":0}]
[null,{"$f":"VLOOKUP($D24,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Temperature of useful heat"},null,"FC038","°C",{"$f":"VLOOKUP(D24,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"IF(F24=\"n.a.\",0,F24)","v":0}]
[null,{"$f":"VLOOKUP($D25,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carnot efficiency of electricity"},null,"FC039a","-",null,1]
[null,{"$f":"VLOOKUP($D26,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Carnot efficiency of heat"},null,"FC039b","-",null,{"$f":"IF(G24<150,0.3546,G24/(G24+273))","v":0.35460000000000003}]
[null,"Electricity input"]
[null,null,{"$f":"VLOOKUP($D28,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Net amount of electricity input, final conversion"},"FC013","MJe/MJinput",{"$f":"VLOOKUP(D28,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F28=\"n.a.\",0,F28)","v":0}]
[null,null,{"$f":"VLOOKUP($D29,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Electricity source, final conversion"},"FC014","-",{"$f":"VLOOKUP(D29,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F29","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D30,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy used for external electricity production, final conversion"},"FC015e","MJfossil/MJe",{"$f":"IF(G29=\"n.a.\",0,VLOOKUP(G29, matrix_standardvalues_electricity,11,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D31,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy used for external electricity production, final conversion"},"FC016e","MJprim/MJe",{"$f":"IF(G29=\"n.a.\",0,VLOOKUP(G29, matrix_standardvalues_electricity,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D32,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to external electricity production, final conversion"},"FC017e","gCO2eq/MJe",{"$f":"IF(G29=\"n.a.\",0,VLOOKUP(G29, matrix_standardvalues_electricity,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D33,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of electricity, final conversion"},"FC035e","gNOX/MJe",{"$f":"IF(G29=\"n.a.\",0,VLOOKUP(G29, matrix_standardvalues_electricity,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D34,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of electricity, final conversion"},"FC036e","gSOX/MJe",{"$f":"IF(G29=\"n.a.\",0,VLOOKUP(G29, matrix_standardvalues_electricity,29,FALSE))","v":0},0]
[null,"Fuel / heat input"]
[null,1,{"$f":"VLOOKUP($D36,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 1, final conversion"},"FC011a","-",{"$f":"VLOOKUP(D36,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F36","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D37,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat flow 1, final conversion"},"FC012a","MJf_h/MJinput",{"$f":"VLOOKUP(D37,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F37=\"n.a.\",0,F37)","v":0}]
[null,null,{"$f":"VLOOKUP($D38,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 1, final conversion"},"FC015c","MJfossil/MJf_h",{"$f":"IF(G36=\"n.a.\",0,VLOOKUP(G36, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F38","v":0}]
[null,null,{"$f":"VLOOKUP($D39,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 1, final conversion"},"FC016c","MJprim/MJf_h",{"$f":"IF(G36=\"n.a.\",0,VLOOKUP(G36, matrix_standardvalues_fuelsall,21,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D40,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 1, final conversion"},"FC017c","gCO2_eq/MJf_h",{"$f":"IF(G36=\"n.a.\",0,VLOOKUP(G36, matrix_standardvalues_fuelsall,9,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D41,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 1, final conversion"},"FC035c","gNOX/MJf_h",{"$f":"IF(G36=\"n.a.\",0,VLOOKUP(G36, matrix_standardvalues_fuelsall,27,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D42,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 1, final conversion"},"FC036c","gSOX/MJf_h",{"$f":"IF(G36=\"n.a.\",0,VLOOKUP(G36, matrix_standardvalues_fuelsall,29,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D43,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of fuel/heat flow 2, final conversion"},"FC011b","-",{"$f":"VLOOKUP(D43,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D44,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of fuel/heat flow 2, final conversion"},"FC012b","MJf_h/MJinput",{"$f":"VLOOKUP(D44,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F44=\"n.a.\",0,F44)","v":0}]
[null,null,{"$f":"VLOOKUP($D45,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for fuel/heat flow 2, final conversion"},"FC015d","MJfossil/MJf_h",{"$f":"IF(G43=\"n.a.\",0,VLOOKUP(G43, matrix_standardvalues_fuelsall,11,FALSE))","v":0},{"$f":"F45","v":0}]
[null,null,{"$f":"VLOOKUP($D46,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for fuel/heat flow 2, final conversion"},"FC016d","MJprim/MJf_h",{"$f":"IF(G43=\"n.a.\",0,VLOOKUP(G43, matrix_standardvalues_fuelsall,21,FALSE))","v":0},{"$f":"F46","v":0}]
[null,null,{"$f":"VLOOKUP($D47,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to fuel/heat flow 2, final conversion"},"FC017d","gCO2_eq/MJf_h",{"$f":"IF(G43=\"n.a.\",0,VLOOKUP(G43, matrix_standardvalues_fuelsall,9,FALSE))","v":0},{"$f":"F47","v":0}]
[null,null,{"$f":"VLOOKUP($D48,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of fuel/heat flow 2, final conversion"},"FC035d","gNOX/MJf_h",{"$f":"IF(G43=\"n.a.\",0,VLOOKUP(G43, matrix_standardvalues_fuelsall,27,FALSE))","v":0},{"$f":"F48","v":0}]
[null,null,{"$f":"VLOOKUP($D49,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of fuel/heat flow 2, final conversion"},"FC036d","gSOX/MJf_h",{"$f":"IF(G43=\"n.a.\",0,VLOOKUP(G43, matrix_standardvalues_fuelsall,29,FALSE))","v":0},{"$f":"F49","v":0}]
[null,"Other material input flows"]
[null,1,{"$f":"VLOOKUP($D51,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 1, final conversion"},"FC009a","-",{"$f":"VLOOKUP(D51,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F51","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D52,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 1, final conversion"},"FC010a","kg/MJinput",{"$f":"VLOOKUP(D52,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F52=\"n.a.\",0,F52)","v":0}]
[null,null,{"$f":"VLOOKUP($D53,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 1, final conversion"},"FC015a","MJfossil/kg",{"$f":"IF(G51=\"n.a.\",0,VLOOKUP(G51, matrix_standardvalues_conversioninputs,10,FALSE))","v":0},{"$f":"F53","v":0}]
[null,null,{"$f":"VLOOKUP($D54,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 1, final conversion"},"FC016a","MJprim/kg",{"$f":"IF(G51=\"n.a.\",0,VLOOKUP(G51, matrix_standardvalues_conversioninputs,20,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D55,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 1, final conversion"},"FC017a","gCO2_eq/kg",{"$f":"IF(G51=\"n.a.\",0,VLOOKUP(G51, matrix_standardvalues_conversioninputs,5,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D56,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 1, final conversion"},"FC035a","gNOX/kg",{"$f":"IF(G51=\"n.a.\",0,VLOOKUP(G51, matrix_standardvalues_conversioninputs,26,FALSE))","v":0},0]
[null,null,{"$f":"VLOOKUP($D57,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 1, final conversion"},"FC036a","gSOX/kg",{"$f":"IF(G51=\"n.a.\",0,VLOOKUP(G51, matrix_standardvalues_conversioninputs,28,FALSE))","v":0},0]
[null,2,{"$f":"VLOOKUP($D58,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of material input flow 2, final conversion"},"FC009b","-",{"$f":"VLOOKUP(D58,Parameters!$1:$2792,6,FALSE)","v":"n.a."},"n.a."]
[null,null,{"$f":"VLOOKUP($D59,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Amount of material input flow 2, final conversion"},"FC010b","kg/MJinput",{"$f":"VLOOKUP(D59,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F59=\"n.a.\",0,F59)","v":0}]
[null,null,{"$f":"VLOOKUP($D60,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific fossil energy for material input flow 2, final conversion"},"FC015b","MJfossil/kg",{"$f":"IF(G58=\"n.a.\",0,VLOOKUP(G58, matrix_standardvalues_conversioninputs,10,FALSE))","v":0},{"$f":"F60","v":0}]
[null,null,{"$f":"VLOOKUP($D61,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific primary energy for material input flow 2, final conversion"},"FC016b","MJprim/kg",{"$f":"IF(G58=\"n.a.\",0,VLOOKUP(G58, matrix_standardvalues_conversioninputs,20,FALSE))","v":0},{"$f":"F61","v":0}]
[null,null,{"$f":"VLOOKUP($D62,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Specific GHG emissions related to material input flow 2, final conversion"},"FC017b","gCO2_eq/kg",{"$f":"IF(G58=\"n.a.\",0,VLOOKUP(G58, matrix_standardvalues_conversioninputs,5,FALSE))","v":0},{"$f":"F62","v":0}]
[null,null,{"$f":"VLOOKUP($D63,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOx emissions factor of material input flow 2, final conversion"},"FC035b","gNOX/kg",{"$f":"IF(G58=\"n.a.\",0,VLOOKUP(G58, matrix_standardvalues_conversioninputs,26,FALSE))","v":0},{"$f":"F63","v":0}]
[null,null,{"$f":"VLOOKUP($D64,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOx emissions factor of material input flow 2, final conversion"},"FC036b","gSOX/kg",{"$f":"IF(G58=\"n.a.\",0,VLOOKUP(G58, matrix_standardvalues_conversioninputs,28,FALSE))","v":0},{"$f":"F64","v":0}]
[null,"By-products"]
[null,null,{"$f":"VLOOKUP($D66,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to heat, final conversion"},"FC025a","%",null,{"$f":"G68*IF(G14=0,1,G26*G15/(G25*G14+G26*G15))","v":100},"=FC025c (only heat) or =FC025c*0.3546*FC003b/(FC003a+0.3546*FC003b) (CHP, carnot efficiency)"]
[null,null,{"$f":"VLOOKUP($D67,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to electricity, final conversion"},"FC025b","%",null,{"$f":"G68*IF(G15=0,1,G25*G14/(G25*G14+G26*G15))","v":100},"=FC025c (only power) or =FC025c*FC003a/(FC003a+0.3546*FC003b) (CHP, carnot efficiency)"]
[null,null,{"$f":"VLOOKUP($D68,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to energy products, final conversion"},"FC025c","%",null,{"$f":"100-G69","v":100},"= 100-FC026"]
[null,null,{"$f":"VLOOKUP($D69,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-products, final conversion"},"FC026","%",null,{"$f":"G76+G83","v":0},"= FC027a + FC027b"]
[null,1,{"$f":"VLOOKUP($D70,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 1, final conversion"},"FC004a","-",{"$f":"VLOOKUP(D70,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F70","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D71,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, final conversion (kg)"},"FC005a","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D72,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 1, final conversion (MJ)"},"FC006a","MJbyproduct /MJinput",{"$f":"VLOOKUP(D72,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F72=\"n.a.\", 0, F72)","v":0}]
[null,null,{"$f":"VLOOKUP($D73,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 1, final conversion (LHV)"},"FC007a","MJ/kg",{"$f":"IF(G70=\"n.a.\",0,VLOOKUP(G70, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F73","v":0}]
[null,null,{"$f":"VLOOKUP($D74,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 1, final conversion"},"FC024a","%"]
[null,null,{"$f":"VLOOKUP($D75,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 1, final conversion"},"FC008a","binary",{"$f":"IF(G70=\"n.a.\",0,VLOOKUP(G70, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F75=\"n.a.\", 0, F75)","v":0}]
[null,null,{"$f":"VLOOKUP($D76,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 1, final conversion"},"FC027a","%",null,{"$f":"IF(G75=1,G72/(G72+G79+G14/100+G15/100)*100,0)","v":0},"= FC006a / (FC006a + FC006b + FC003a / 100 + FC003b / 100) * 100"]
[null,2,{"$f":"VLOOKUP($D77,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Type of by-product 2, final conversion"},"FC004b","-",{"$f":"VLOOKUP(D77,Parameters!$1:$2792,6,FALSE)","v":"n.a."},{"$f":"F77","v":"n.a."}]
[null,null,{"$f":"VLOOKUP($D78,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, final conversion (kg)"},"FC005b","kgbyproduct /kginput"]
[null,null,{"$f":"VLOOKUP($D79,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Extraction rate of by-product 2, final conversion (MJ)"},"FC006b","MJbyproduct /MJinput",{"$f":"VLOOKUP(D79,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"IF(F79=\"n.a.\", 0, F79)","v":0}]
[null,null,{"$f":"VLOOKUP($D80,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Energy content of by-product 2, final conversion (LHV)"},"FC007b","MJ/kg",{"$f":"IF(G77=\"n.a.\",0,VLOOKUP(G77, matrix_standardvalues_fuelsfeedstockcoproductssolids,14,FALSE))","v":0},{"$f":"F80","v":0}]
[null,null,{"$f":"VLOOKUP($D81,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Moisture content of by-product 2, final conversion"},"FC024b","%"]
[null,null,{"$f":"VLOOKUP($D82,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Valorisation of by-product 2, final conversion"},"FC008b","binary",{"$f":"IF(G77=\"n.a.\",0,VLOOKUP(G77, matrix_standardvalues_fuelsfeedstockcoproductssolids,18,FALSE))","v":0},{"$f":"IF(F82=\"n.a.\", 0, F82)","v":0}]
[null,null,{"$f":"VLOOKUP($D83,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Allocation to by-product 2, final conversion"},"FC027b","%",null,{"$f":"IF(G82=1,G79/(G72+G79+G14/100+G15/100)*100,0)","v":0},"= FC006b / (FC006a + FC006b + FC003a / 100 + FC003b / 100) * 100"]
[]
["ENERGY BALANCE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Final conversion process"]
[null,{"$f":"VLOOKUP($D87,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use in final conversion process"},null,"FC019","MJfossil/MJinput",null,{"$f":"G89+G91+G93","v":0},"= FC018a + FC018b + FC018c"]
[null,{"$f":"VLOOKUP($D88,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use in final conversion process"},null,"FC021","MJprim/MJinput",null,{"$f":"G90+G92+G94","v":0},"= FC020a + FC020b + FC020c"]
[null,null,{"$f":"VLOOKUP($D89,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to electricity input, final conversion"},"FC018a","MJfossil/MJinput",null,{"$f":"G28*G30","v":0},"= FC013 * FC015e"]
[null,null,{"$f":"VLOOKUP($D90,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to electricity input, final conversion"},"FC020a","MJprim/MJinput",null,{"$f":"G28*G31","v":0},"= FC013 * FC016e"]
[null,null,{"$f":"VLOOKUP($D91,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to fuel/heat input flows, final conversion"},"FC018b","MJfossil/MJinput",null,{"$f":"G37*G38+G44*G45","v":0},"= FC012a * FC015c + FC012b * FC015d"]
[null,null,{"$f":"VLOOKUP($D92,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to fuel/heat flows, final conversion"},"FC020b","MJprim/MJinput",null,{"$f":"G37*G39+G44*G46","v":0},"= FC012a * FC016c + FC012b * FC016d"]
[null,null,{"$f":"VLOOKUP($D93,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy use related to material input flows, final conversion"},"FC018c","MJfossil/MJinput",null,{"$f":"G52*G53+G59*G60","v":0},"= FC010a * FC015a + FC010b * FC015b"]
[null,null,{"$f":"VLOOKUP($D94,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy use related to material input flows, final conversion"},"FC020c","MJprim/MJinput",null,{"$f":"G52*G54+G59*G61","v":0},"= FC010a * FC016a + FC010b * FC016b"]
["Totally allocated energy use for final conversion"]
[null,{"$f":"VLOOKUP($D96,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated fossil energy requirement for final conversion"},null,"FC045a","MJfossil/MJFU",null,{"$f":"G87*(G22+G23)*G68/100","v":0},"= FC019 * (FC033 + FC034) * FC025c / 100"]
[null,{"$f":"VLOOKUP($D97,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated primary energy requirement for final conversion"},null,"FC045b","MJprim/MJFU",null,{"$f":"G88*(G22+G23)*G68/100","v":0},"= FC021 * (FC033 + FC034) * FC025c / 100"]
["Total cumulated energy use (before allocation 4)"]
[null,{"$f":"VLOOKUP($D99,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use before allocation 4"},null,"FC040a","MJfossil/MJinput",null,{"$f":"'Conversion feedstock1'!G330*'Final conversion'!G11/100+'Conversion feedstock2'!G330*'Final conversion'!G13/100+'Final conversion'!G87","v":0.17800166505611817},"= BC082a * FC002a / 100 + BC582a * FC002b / 100 + FC019"]
[null,{"$f":"VLOOKUP($D100,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use before allocation 4"},null,"FC040b","MJprim/MJinput",null,{"$f":"'Conversion feedstock1'!G331*'Final conversion'!G11/100+'Conversion feedstock2'!G331*'Final conversion'!G13/100+'Final conversion'!G87","v":0.55455325278356304},"= BC082b * FC002a / 100 + BC582b * FC002b / 100 + FC021"]
["Total cumulated energy use (after allocation 4)"]
[null,{"$f":"VLOOKUP($D102,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use allocated to heat production"},null,"FC041a","MJfossil/MJh",null,{"$f":"IF(F15=0,0,G99/G15*G66)","v":0},"= FC040a / FC003b * FC025a"]
[null,{"$f":"VLOOKUP($D103,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use allocated to heat production"},null,"FC041b","MJprim/MJh",null,{"$f":"IF(F15=0,0,G100/G15*G66)","v":0},"= FC040b / FC003b * FC025a"]
[null,{"$f":"VLOOKUP($D104,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use allocated to heat production"},null,"FC042a","MJfossil/MJFU",null,{"$f":"G102*G20","v":0},"= FC041a * FC031"]
[null,{"$f":"VLOOKUP($D105,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use allocated to heat production"},null,"FC042b","MJprim/MJFU",null,{"$f":"G103*G20","v":0},"= FC041b * FC031"]
[null,{"$f":"VLOOKUP($D106,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use allocated to electricity production"},null,"FC043a","MJfossil/MJe",null,{"$f":"IF(F14=0,0,G99/G14*G67)","v":0},"= FC040a / FC003a * FC025b"]
[null,{"$f":"VLOOKUP($D107,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use allocated to electricity production"},null,"FC043b","MJprim/MJe",null,{"$f":"IF(F14=0,0,G100/G14*G67)","v":0},"= FC040b / FC003a * FC025b"]
[null,{"$f":"VLOOKUP($D108,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use allocated to electricity production"},null,"FC044a","MJfossil/MJFU",null,{"$f":"G106*G21","v":0},"= FC043a * FC032"]
[null,{"$f":"VLOOKUP($D109,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use allocated to electricity production"},null,"FC044b","MJprim/MJFU",null,{"$f":"G107*G21","v":0},"= FC043b * FC032"]
[null,{"$f":"VLOOKUP($D110,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total fossil energy use allocated to energy production"},null,"FC046a","MJfossil/MJFU",null,{"$f":"G99*(G22+G23)*G68/100","v":0.17800166505611817},"= FC040a * (FC033 + FC034) * FC025c / 100"]
[null,{"$f":"VLOOKUP($D111,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total primary energy use allocated to energy production"},null,"FC046b","MJprim/MJFU",null,{"$f":"G100*(G22+G23)*G68/100","v":0.55455325278356304},"= FC040b * (FC033 + FC034) * FC025c / 100"]
[null,null,"Allocation check fossil (result has to be same as FC046a) (not in case of biogas)",null,null,null,{"$f":"G104+G108","v":0},"= FC042a + FC044a"]
[null,null,"Allocation check prim (result has to be same as FC046b) (not in case of biogas)",null,null,null,{"$f":"G105+G109","v":0},"= FC042b + FC044b"]
["Comparison to fossil reference system"]
[null,{"$f":"VLOOKUP($D115,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy requirement of reference system for heat"},null,"FC047a","MJfossil/MJh",{"$f":"'Standard Values'!K115","v":1.43},{"$f":"F115","v":1.43}]
[null,{"$f":"VLOOKUP($D116,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy requirement of reference system for heat"},null,"FC047b","MJprim/MJh",{"$f":"'Standard Values'!U115","v":2.145},{"$f":"F116","v":2.145}]
[null,{"$f":"VLOOKUP($D117,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy requirement of reference system for electricity"},null,"FC048a","MJfossil/MJe",{"$f":"'Standard Values'!K105","v":2.7275},{"$f":"F117","v":2.7275}]
[null,{"$f":"VLOOKUP($D118,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy requirement of reference system for electricity"},null,"FC048b","MJprim/MJe",{"$f":"'Standard Values'!U105","v":4.0912500000000005},{"$f":"F118","v":4.0912500000000005}]
[null,{"$f":"VLOOKUP($D119,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy requirement of reference system for biogas"},null,"FC110a","MJfossil/MJbiogas",{"$f":"'Standard Values'!K27","v":1.1281000000000001},{"$f":"F119","v":1.1281000000000001}]
[null,{"$f":"VLOOKUP($D120,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy requirement of reference system for biogas"},null,"FC110b","MJprim/MJbiogas",{"$f":"'Standard Values'!U27","v":1.6921500000000003},1.6921500000000003]
[null,{"$f":"VLOOKUP($D121,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy requirement of reference system for diesel"},null,"FC111a","MJfossil/MJdiesel",{"$f":"'Standard Values'!K32","v":1.1599999999999999},{"$f":"F121","v":1.1599999999999999}]
[null,{"$f":"VLOOKUP($D122,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy requirement of reference system for diesel"},null,"FC111b","MJprim/MJdiesel",{"$f":"'Standard Values'!U32","v":1.7399999999999998},1.7399999999999998]
[null,{"$f":"VLOOKUP($D123,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy requirement of reference system for gasoline"},null,"FC112a","MJfossil/MJgasoline",{"$f":"'Standard Values'!K33","v":1.1399999999999999},1.1399999999999999]
[null,{"$f":"VLOOKUP($D124,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy requirement of reference system for gasoline"},null,"FC112b","MJprim/MJgasoline",{"$f":"'Standard Values'!U33","v":1.71},1.71]
[null,{"$f":"VLOOKUP($D125,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy requirement of reference system for heavy fuel oil"},null,"FC113a","MJfossil/MJhfo",{"$f":"'Standard Values'!K34","v":1.0880000000000001},1.0880000000000001]
[null,{"$f":"VLOOKUP($D126,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy requirement of reference system for heavy fuel oil"},null,"FC113b","MJprim/MJhfo",{"$f":"'Standard Values'!U34","v":1.6320000000000001},1.6320000000000001]
[null,{"$f":"VLOOKUP($D127,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy requirement of total reference system"},null,"FC051a","MJfossil/MJFU",null,{"$f":"IF(G19=\"MJ gas\",G119,IF(G19=\"MJ diesel\",G121,IF(G19=\"MJ gasoline\",G123,IF(G19=\"MJ heavy fuel oil\",G125,G115*G20+G117*G21))))","v":1.1599999999999999},"= FC047a * FC031 + FC048a * FC032"]
[null,{"$f":"VLOOKUP($D128,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy requirement of total reference system"},null,"FC051b","MJprim/MJFU",null,{"$f":"IF(G19=\"MJ gas\",G120,IF(G19=\"MJ diesel\",G122,IF(G19=\"MJ gasoline\",G124,IF(G19=\"MJ heavy fuel oil\",G126,G116*G20+G118*G21))))","v":1.7399999999999998},"= FC047b * FC031 + FC048b * FC032"]
[null,{"$f":"VLOOKUP($D129,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy reduction of heat production"},null,"FC049a","%",null,{"$f":"IF(F15=0,0,(G115-G102)/G115*100)","v":0},"= (FC047a - FC041a) / FC047a * 100"]
[null,{"$f":"VLOOKUP($D130,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy reduction of heat production"},null,"FC049b","%",null,{"$f":"IF(F15=0,0,(G116-G103)/G116*100)","v":0},"= (FC047b - FC041b) / FC047b * 100"]
[null,{"$f":"VLOOKUP($D131,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy reduction of electricity production"},null,"FC050a","%",null,{"$f":"IF(F14=0,0,(G117-G106)/G117*100)","v":0},"= (FC048a - FC043a) / FC048a * 100"]
[null,{"$f":"VLOOKUP($D132,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy reduction of electricity production"},null,"FC050b","%",null,{"$f":"IF(F14=0,0,(G118-G107)/G118*100)","v":0},"= (FC048b - FC043b) / FC048b * 100"]
[null,{"$f":"VLOOKUP($D133,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fossil energy reduction of total energy production"},null,"FC052a","%",null,{"$f":"IF(G127=0,0,(G127-G110)/G127*100)","v":84.655028874472578},"= (FC051a - FC046a) / FC051a * 100"]
[null,{"$f":"VLOOKUP($D134,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Primary energy reduction of total energy production"},null,"FC052b","%",null,{"$f":"IF(G128=0,0,(G128-G111)/G128*100)","v":68.129123403243497},"= (FC051b - FC046b) / FC051b * 100"]
[]
["GLOBAL WARMING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["GHG balance of final conversion process"]
[null,{"$f":"VLOOKUP($D138,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to final conversion"},null,"FC023","gCO2_eq/MJinput",null,{"$f":"G139+G140+G141","v":0},"= FC022a + FC022b + FC022c"]
[null,null,{"$f":"VLOOKUP($D139,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to electricity use, final conversion"},"FC022a","gCO2_eq/MJinput",null,{"$f":"G28*G32","v":0},"= FC013 * FC017e"]
[null,null,{"$f":"VLOOKUP($D140,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to fuel/heat flows, final conversion"},"FC022b","gCO2_eq/MJinput",null,{"$f":"G37*G40+G44*G47","v":0},"= FC012a * FC017c + FC012b * FC017d"]
[null,null,{"$f":"VLOOKUP($D141,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions related to material input flows, final conversion"},"FC022c","gCO2_eq/MJinput",null,{"$f":"G52*G55+G59*G62","v":0},"= FC010a * FC035a + FC010b * FC035b"]
["Totally allocated GHG emissions from final conversion"]
[null,{"$f":"VLOOKUP($D143,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated GHG emissions from final conversion"},null,"FC045c","gCO2_eq/MJFU",null,{"$f":"G138*(G22+G23)*G68/100","v":0},"= FC023 * (FC033 + FC034) * FC025c / 100"]
["Total cumulated GHG emissions (before allocation 4)"]
[null,{"$f":"VLOOKUP($D145,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions before allocation 4"},null,"FC040c","gCO2_eq/MJinput",null,{"$f":"'Conversion feedstock1'!G368*G11/100+'Conversion feedstock2'!G368*G13/100+G138","v":59.196326779586677},"= BC082c * FC002a / 100 + BC582c * FC002b / 100 + FC023"]
["Total cumulated GHG emissions (after allocation 4)"]
[null,{"$f":"VLOOKUP($D147,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions allocated to heat production"},null,"FC041c","gCO2_eq/MJh",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G145/G15*G66))))","v":0},"= FC040c / FC003b * FC025a"]
[null,{"$f":"VLOOKUP($D148,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions allocated to heat production"},null,"FC042c","gCO2_eq/MJFU",null,{"$f":"G147*G20","v":0},"= FC041c * FC031"]
[null,{"$f":"VLOOKUP($D149,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions allocated to electricity production"},null,"FC043c","gCO2_eq/MJe",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G145/G14*G67))))","v":0},"= FC040c / FC003a * FC025b"]
[null,{"$f":"VLOOKUP($D150,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions allocated to electricity production"},null,"FC044c","gCO2_eq/MJFU",null,{"$f":"G149*G21","v":0},"= FC043c * FC032"]
[null,{"$f":"VLOOKUP($D151,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions allocated to energy production"},null,"FC046c","gCO2_eq/MJFU",null,{"$f":"IF(F19=\"MJ gas\",G145*G68/100,IF(F19=\"MJ diesel\",G145*G68/100,G145*(G22+G23)*G68/100))","v":59.196326779586677},"= FC040c * (FC033 + FC034) * FC025c / 100"]
["Comparison to fossil reference system"]
[null,{"$f":"VLOOKUP($D153,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of reference system for heat"},null,"FC047c","gCO2_eq/MJh",{"$f":"'Standard Values'!I123","v":85.18},{"$f":"F153","v":85.18}]
[null,{"$f":"VLOOKUP($D154,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of reference system for electricity"},null,"FC048c","gCO2_eq/MJe",{"$f":"'Standard Values'!I109","v":129.19},129.19]
[null,{"$f":"VLOOKUP($D155,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of reference system for biogas"},null,"FC110c","gCO2_eq/MJbiogas",{"$f":"'Standard Values'!I27","v":67.586972222222229},67.586972222222229]
[null,{"$f":"VLOOKUP($D156,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of reference system for diesel"},null,"FC111c","gCO2_eq/MJdiesel",{"$f":"'Standard Values'!I32","v":87.6388888888889},87.6388888888889]
[null,{"$f":"VLOOKUP($D157,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of reference system for gasoline"},null,"FC112c","gCO2_eq/MJgasoline",{"$f":"'Standard Values'!I33","v":86},86]
[null,{"$f":"VLOOKUP($D158,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of reference system for heavy fuel oil"},null,"FC113c","gCO2_eq/MJhfo",{"$f":"'Standard Values'!I34","v":84.977777777777803},84.977777777777803]
[null,{"$f":"VLOOKUP($D159,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emissions of total reference system"},null,"FC051c","gCO2_eq/MJFU",null,{"$f":"IF(G19=\"MJ gas\",G155,IF(G19=\"MJ diesel\",G156,IF(G19=\"MJ gasoline\",G157,IF(G19=\"MJ heavy fuel oil\",G158,G153*G20+G154*G21))))","v":87.6388888888889},"= FC047c * FC031 + FC048c * FC032"]
[null,{"$f":"VLOOKUP($D160,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emission reduction of heat production"},null,"FC049c","%",null,{"$f":"IF(F15=0,0,(G153-G147)/G153*100)","v":0},"= (FC047c - FC041c) / FC047c * 100"]
[null,{"$f":"VLOOKUP($D161,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emission reduction of electricity production"},null,"FC050c","%",null,{"$f":"IF(F14=0,0,(G154-G149)/G154*100)","v":0},"= (FC048c - FC043c) / FC048c * 100"]
[null,{"$f":"VLOOKUP($D162,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emission reduction of total energy production"},null,"FC052c","%",null,{"$f":"IF(G159=0,0,(G159-G151)/G159*100)","v":32.454270552611092},"= (FC051c - FC046c) / FC051c * 100"]
[null,{"$f":"VLOOKUP($D163,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Compliance with RED requirements on GHG savings"},null,"FC029","-",null,{"$f":"IF(G162>35,\"yes\",\"no\")","v":"no"},"= if FC052c >35 then yes otherwise no (only for biofuels for transport and from 2014 onwards 60)"]
["Carbon debt & repayment time"]
[null,{"$f":"VLOOKUP($D165,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total GHG emissions allocated to energy production without LUC emissions"},null,"FC053","gCO2_eq/MJFU",null,{"$f":"('Conversion feedstock1'!G378*G11/100+'Conversion feedstock2'!G378*G13/100+G138)*(G22+G23)*G68/100","v":59.196326779586677},"= (BC084 * FC002a / 100 + BC584 * FC002b / 100 + FC023) * (FC033 + FC034) * FC025c / 100"]
[null,{"$f":"VLOOKUP($D166,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"GHG emission reduction of total energy production without LUC emissions"},null,"FC054","gCO2_eq/MJFU",null,{"$f":"G159-G165","v":28.442562109302223},"= FC051c - FC053"]
[null,{"$f":"VLOOKUP($D167,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total carbon debt due to land use change"},null,"FC055","gCO2_eq/MJFU",null,{"$f":"G168+G169","v":0},"= FC033 / BC015c * FP107c + FC034 / BC515c * FP607c"]
[null,{"$f":"VLOOKUP($D168,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total carbon debt due to land use change_FS1"},null,"FC057a","gCO2_eq/MJFU",null,{"$f":"IF('Conversion feedstock1'!G176=0,0,G22/'Conversion feedstock1'!G176*'Production feedstock1'!G244)","v":0},"= FC033 / BC015c * FP107c"]
[null,{"$f":"VLOOKUP($D169,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total carbon debt due to land use change_FS2"},null,"FC057b","gCO2_eq/MJFU",null,{"$f":"IF('Conversion feedstock2'!G176=0,0,G23/'Conversion feedstock2'!G176*'Production feedstock2'!G244)","v":0},"= FC034 / BC515c * FP607c"]
[null,{"$f":"VLOOKUP($D170,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Repayment time"},null,"FC056","years",null,{"$f":"IF(G166>0,G167/G166,IF(G166=0,IF(G167=0,0,\"no repayment possible\"),\"no repayment possible\"))","v":0},"= FC055 / FC054"]
[]
[null,"GHG emissions related to materials production, assemblage and recycling *",null,null,"gCO2-eq/conversion plant"]
[]
["RESOURCE USE",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["USE OF WATER"]
["Water use for final conversion process"]
[null,{"$f":"VLOOKUP($D177,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for final conversion process"},null,"FC058a","m³/MJinput",{"$f":"VLOOKUP(D177,Parameters!$1:$1958,6,FALSE)","v":0},{"$f":"F177","v":0}]
[null,{"$f":"VLOOKUP($D178,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use for final conversion process"},null,"FC058b","m³/GJinput",null,{"$f":"G177*1000","v":0},"= FC058a * 1000"]
["Totally allocated water use for final conversion"]
[null,{"$f":"VLOOKUP($D180,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated water use from final conversion"},null,"FC045d","m³/GJFU",null,{"$f":"G177*(G22+G23)*G68*10","v":0},"= FC058a * (FC033 + FC034) * FC025c / 100 * 1000"]
["Total cumulated water use (before allocation 4)"]
[null,{"$f":"VLOOKUP($D182,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use before allocation 4"},null,"FC040d","m³/GJinput",null,{"$f":"'Conversion feedstock1'!G401*G11/100+'Conversion feedstock2'!G401*G13/100+G178","v":422.20878511090552},"= BC082d * FC002a / 100 + BC582d * FC002b / 100 + FC055b"]
["Total cumulated water use (after allocation 4)"]
[null,{"$f":"VLOOKUP($D184,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use allocated to heat production"},null,"FC041d","m³/GJh",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G182/G15*G66))))","v":0},"= FC040d / FC003b * FC025a"]
[null,{"$f":"VLOOKUP($D185,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use allocated to heat production"},null,"FC042d","m³/GJFU",null,{"$f":"G184*G20","v":0},"= FC041d * FC031"]
[null,{"$f":"VLOOKUP($D186,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use allocated to electricity production"},null,"FC043d","m³/GJe",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G182/G14*G67))))","v":0},"= FC040d / FC003a * FC025b"]
[null,{"$f":"VLOOKUP($D187,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use allocated to electricity production"},null,"FC044d","m³/GJFU",null,{"$f":"G186*G21","v":0},"= FC043d * FC032"]
[null,{"$f":"VLOOKUP($D188,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total water use allocated to energy production"},null,"FC046d","m³/GJFU",null,{"$f":"G182*(G22+G23)*G68/100","v":422.20878511090552},"= FC040d * (FC033 + FC034) * FC025c / 100"]
["Comparison to fossil reference system"]
[null,{"$f":"VLOOKUP($D190,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use of reference system for heat"},null,"FC047d","m³/GJh",{"$f":"'Standard Values'!V123","v":0.76},{"$f":"F190","v":0.76}]
[null,{"$f":"VLOOKUP($D191,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use of reference system for electricity"},null,"FC048d","m³/GJe",{"$f":"'Standard Values'!V109","v":0.61},0.61]
[null,{"$f":"VLOOKUP($D192,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use of reference system for biogas"},null,"FC110d","m³/GJbiogas",{"$f":"'Standard Values'!V27","v":0},0]
[null,{"$f":"VLOOKUP($D193,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use of reference system for diesel"},null,"FC111d","m³/GJdiesel",{"$f":"'Standard Values'!V32","v":0},0]
[null,{"$f":"VLOOKUP($D194,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use of reference system for gasoline"},null,"FC112d","m³/GJgasoline",{"$f":"'Standard Values'!V33","v":0},0]
[null,{"$f":"VLOOKUP($D195,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use of reference system for heavy fuel oil"},null,"FC113d","m³/GJhfo",{"$f":"'Standard Values'!V34","v":0},0]
[null,{"$f":"VLOOKUP($D196,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use of total reference system"},null,"FC051d","m³/GJFU",null,{"$f":"IF(G19=\"MJ gas\",G192,IF(G19=\"MJ diesel\",G193,IF(G19=\"MJ gasoline\",G194,IF(G19=\"MJ heavy fuel oil\",G195,G190*G20+G191*G21))))","v":0},"= FC047d * FC031 + FC048d * FC032"]
[null,{"$f":"VLOOKUP($D197,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use reduction of heat production"},null,"FC049d","%",null,{"$f":"IF(F15=0,0,(G190-G184)/G190*100)","v":0},"= (FC047d - FC041d) / FC047d * 100"]
[null,{"$f":"VLOOKUP($D198,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use reduction of electricity production"},null,"FC050d","%",null,{"$f":"IF(F14=0,0,(G191-G186)/G191*100)","v":0},"= (FC048d - FC043d) / FC048d * 100"]
[null,{"$f":"VLOOKUP($D199,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Water use reduction of total energy production"},null,"FC052d","%",null,{"$f":"IF(G196=0,0,(G196-G188)/G196*100)","v":0},"= (FC051d - FC046d) / FC051d * 100"]
["USE OF LAND"]
["Total land use before allocation 4"]
[null,{"$f":"VLOOKUP($D202,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total land use before allocation 4"},null,"FC040e","ha/GJinput",null,{"$f":"'Production feedstock1'!G264*G11/100+'Production feedstock2'!G264*G13/100","v":1.9132606099961733E-2},"= FP106a * FC002a / 100 + FP606a * FC002b / 100"]
["Total land use after allocation 4"]
[null,{"$f":"VLOOKUP($D204,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total land use allocated to heat production"},null,"FC041e","ha/GJh",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G202/G15*G66))))","v":0},"= FC040e / FC003b * FC025a"]
[null,{"$f":"VLOOKUP($D205,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total land use allocated to heat production"},null,"FC042e","ha/GJFU",null,{"$f":"G204*G20","v":0},"= FC041e * FC031"]
[null,{"$f":"VLOOKUP($D206,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total land use allocated to electricity production"},null,"FC043e","ha/GJe",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G202/G14*G67))))","v":0},"= FC040e / FC003a * FC025b"]
[null,{"$f":"VLOOKUP($D207,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total land use allocated to electricity production"},null,"FC044e","ha/GJFU",null,{"$f":"G206*G21","v":0},"= FC043e * FC032"]
[null,{"$f":"VLOOKUP($D208,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total land use allocated to energy production"},null,"FC046e","ha/GJFU",null,{"$f":"G202*(G22+G23)*G68/100","v":1.9132606099961733E-2},"= FC040e * (FC033 + FC034) * FC025c / 100"]
["Comparison to fossil reference system"]
[null,{"$f":"VLOOKUP($D210,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use of reference system for heat"},null,"FC047e","ha/GJh",{"$f":"'Standard Values'!W123","v":0},{"$f":"F210","v":0}]
[null,{"$f":"VLOOKUP($D211,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use of reference system for electricity"},null,"FC048e","ha/GJe",{"$f":"'Standard Values'!W109","v":0},0]
[null,{"$f":"VLOOKUP($D212,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use of reference system for biogas"},null,"FC110e","ha/GJbiogas",{"$f":"'Standard Values'!W27","v":0},0]
[null,{"$f":"VLOOKUP($D213,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use of reference system for diesel"},null,"FC111e","ha/GJdiesel",{"$f":"'Standard Values'!W32","v":0},0]
[null,{"$f":"VLOOKUP($D214,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use of reference system for gasoline"},null,"FC112e","ha/GJgasoline",{"$f":"'Standard Values'!W33","v":0},0]
[null,{"$f":"VLOOKUP($D215,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use of reference system for heavy fuel oil"},null,"FC113e","ha/GJhfo",{"$f":"'Standard Values'!W34","v":0},0]
[null,{"$f":"VLOOKUP($D216,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use of total reference system"},null,"FC051e","ha/GJFU",null,{"$f":"IF(G19=\"MJ gas\",G212,IF(G19=\"MJ diesel\",G213,IF(G19=\"MJ gasoline\",G214,IF(G19=\"MJ heavy fuel oil\",G215,G210*G20+G211*G21))))","v":0},"= FC047e * FC031 + FC048e * FC032"]
[null,{"$f":"VLOOKUP($D217,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use reduction of heat production"},null,"FC049e","%",null,{"$f":"IF(F15=0,0,(G210-G204)/G210*100)","v":0}]
[null,{"$f":"VLOOKUP($D218,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use reduction of electricity production"},null,"FC050e","%",null,{"$f":"IF(F14=0,0,(G211-G206)/G211*100)","v":0}]
[null,{"$f":"VLOOKUP($D219,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land use reduction of total energy production"},null,"FC052e","%",null,{"$f":"IF(G216=0,0,(G216-G208)/G216*100)","v":0}]
[]
["ENVIRONMENTAL QUALITY",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["ACIDIFICATION POTENTIAL"]
["Final conversion process"]
[null,{"$f":"VLOOKUP($D224,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to final conversion process "},null,"FC060","gSO2_eq/MJinput",null,{"$f":"G225+G226+G227+G228","v":0},"= FC061 + FC062 + FC063 + FC064"]
[null,null,{"$f":"VLOOKUP($D225,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to electricity input, final conversion"},"FC061","gSO2_eq/MJinput",null,{"$f":"G28*G33*'Production feedstock1'!G274+G28*G34*'Production feedstock1'!G275","v":0},"= FC013 * FC035e * FP110b + FC013 * FC036e * FP110c"]
[null,null,{"$f":"VLOOKUP($D226,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to fuel/heat input flows, final conversion"},"FC062","gSO2_eq/MJinput",null,{"$f":"G37*G41*'Production feedstock1'!G274+G37*G42*'Production feedstock1'!G275+G44*G48*'Production feedstock1'!G274+G44*G49*'Production feedstock1'!G275","v":0},"= FC012a * FC035c * FP110b + FC012a * FC036c * FP110c + FC012b * FC035d * FP110b + FC012b * FC036d * FP110c"]
[null,null,{"$f":"VLOOKUP($D227,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to material input flows, final conversion"},"FC063","gSO2_eq/MJinput",null,{"$f":"G52*G56*'Production feedstock1'!G274+G52*G57*'Production feedstock1'!G275+G59*G63*'Production feedstock1'!G274+G59*G64*'Production feedstock1'!G275","v":0},"= FC010a * FC035a * FP110b + FC010a * FC036a * FP110c + FC010b * FC035b * FP110b + FC010b * FC036b * FP110c"]
[null,null,{"$f":"VLOOKUP($D228,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential related to process emissions, final conversion"},"FC064","gSO2_eq/MJinput",null,{"$f":"G229*'Production feedstock1'!G274+G230*'Production feedstock1'!G275","v":0},"= FC028a * FP110b + FC028b * FP110c"]
[null,null,{"$f":"VLOOKUP($D229,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), final conversion"},"FC028a","gNOX/MJoutput",{"$f":"VLOOKUP(D229,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F229","v":0}]
[null,null,{"$f":"VLOOKUP($D230,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"SOX emissions to air (not from material/energy input), final conversion"},"FC028b","gSOX/MJoutput",{"$f":"VLOOKUP(D230,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F230","v":0}]
["Totally allocated acidification potential from final conversion"]
[null,{"$f":"VLOOKUP($D232,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated acidification potential from final conversion"},null,"FC045f","gSO2_eq/MJFU",null,{"$f":"G224*(G22+G23)*G68/100","v":0},"= FC060 * (FC033 + FC034) * FC025c / 100"]
["Total cumulated acidification potential (before allocation 4)"]
[null,{"$f":"VLOOKUP($D234,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential before allocation 4"},null,"FC040f","gSO2_eq/MJinput",null,{"$f":"'Conversion feedstock1'!G440*G11/100+'Conversion feedstock2'!G440*G13/100+G224","v":0.93786277735394152},"= BC082f * FC002a / 100 + BC582f * FC002b / 100 + FC060"]
["Total cumulated acidification potential (after allocation 4)"]
[null,{"$f":"VLOOKUP($D236,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential allocated to heat production"},null,"FC041f","gSO2_eq/MJh",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G234/G15*G66))))","v":0},"= FC040f / FC003b * FC025a"]
[null,{"$f":"VLOOKUP($D237,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential allocated to heat production"},null,"FC042f","gSO2_eq/MJFU",null,{"$f":"G236*G20","v":0},"= FC041f * FC031"]
[null,{"$f":"VLOOKUP($D238,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential allocated to electricity production"},null,"FC043f","gSO2_eq/MJe",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G234/G14*G67))))","v":0},"= FC040f / FC003a * FC025b"]
[null,{"$f":"VLOOKUP($D239,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential allocated to electricity production"},null,"FC044f","gSO2_eq/MJFU",null,{"$f":"G238*G21","v":0},"= FC043f * FC032"]
[null,{"$f":"VLOOKUP($D240,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total acidification potential allocated to energy production"},null,"FC046f","gSO2_eq/MJFU",null,{"$f":"G234*(G22+G23)*G68/100","v":0.93786277735394152},"= FC040f * (FC033 + FC034) * FC025c / 100"]
["Comparison to fossil reference system"]
[null,{"$f":"VLOOKUP($D242,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of reference system for heat"},null,"FC047f","gSO2_eq/MJh",{"$f":"'Standard Values'!X123","v":1.53},{"$f":"F242","v":1.53}]
[null,{"$f":"VLOOKUP($D243,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of reference system for electricity"},null,"FC048f","gSO2_eq/MJe",{"$f":"'Standard Values'!X109","v":2.46},2.46]
[null,{"$f":"VLOOKUP($D244,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of reference system for biogas"},null,"FC110f","gSO2_eq/MJbiogas",{"$f":"'Standard Values'!X27","v":0},0]
[null,{"$f":"VLOOKUP($D245,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of reference system for diesel"},null,"FC111f","gSO2_eq/MJdiesel",{"$f":"'Standard Values'!X32","v":0},0]
[null,{"$f":"VLOOKUP($D246,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of reference system for gasoline"},null,"FC112f","gSO2_eq/MJgasoline",{"$f":"'Standard Values'!X33","v":0},0]
[null,{"$f":"VLOOKUP($D247,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of reference system for heavy fuel oil"},null,"FC113f","gSO2_eq/MJhfo",{"$f":"'Standard Values'!X34","v":0},0]
[null,{"$f":"VLOOKUP($D248,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential of total reference system"},null,"FC051f","gSO2_eq/MJFU",null,{"$f":"IF(G19=\"MJ gas\",G244,IF(G19=\"MJ diesel\",G245,IF(G19=\"MJ gasoline\",G246,IF(G19=\"MJ heavy fuel oil\",G247,G242*G20+G243*G21))))","v":0},"= FC047f * FC031 + FC048f * FC032"]
[null,{"$f":"VLOOKUP($D249,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential reduction of heat production"},null,"FC049f","%",null,{"$f":"IF(F15=0,0,(G242-G236)/G242*100)","v":0},"= (FC047f - FC041f) / FC047f * 100"]
[null,{"$f":"VLOOKUP($D250,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential reduction of electricity production"},null,"FC050f","%",null,{"$f":"IF(F14=0,0,(G243-G238)/G243*100)","v":0},"= (FC048f - FC043f) / FC048f * 100"]
[null,{"$f":"VLOOKUP($D251,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Acidification potential reduction of total energy production"},null,"FC052f","%",null,{"$f":"IF(G248=0,0,(G248-G240)/G248*100)","v":0},"= (FC051f - FC046f) / FC051f * 100"]
["EUTROPHICATION POTENTIAL"]
["Final conversion process"]
[null,{"$f":"VLOOKUP($D254,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to final conversion process "},null,"FC070","gSO2_eq/MJinput",null,{"$f":"G255+G256+G257+G258","v":0},"= FC061 + FC062 + FC063 + FC064"]
[null,null,{"$f":"VLOOKUP($D255,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to electricity input, final conversion"},"FC071","gSO2_eq/MJinput",null,{"$f":"G28*G33*'Production feedstock1'!G289","v":0},"= FC013 * FC035e * FP120b"]
[null,null,{"$f":"VLOOKUP($D256,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to fuel/heat input flows, final conversion"},"FC072","gSO2_eq/MJinput",null,{"$f":"G37*G41*'Production feedstock1'!G289+G44*G48*'Production feedstock1'!G289","v":0},"= FC012a * FC035c * FP120b + FC012b * FC035d * FP120b"]
[null,null,{"$f":"VLOOKUP($D257,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to material input flows, final conversion"},"FC073","gSO2_eq/MJinput",null,{"$f":"G52*G56*'Production feedstock1'!G289+G59*G63*'Production feedstock1'!G289","v":0},"= FC010a * FC035a * FP120b + FC010b * FC035b * FP120b"]
[null,null,{"$f":"VLOOKUP($D258,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential related to process emissions, final conversion"},"FC074","gSO2_eq/MJinput",null,{"$f":"G259*'Production feedstock1'!G289+G260*'Production feedstock1'!G290+G261*'Production feedstock1'!G293+G262*'Production feedstock1'!G294+G263*'Production feedstock1'!G297+G264*'Production feedstock1'!G298","v":0},"= FC028a * FP120b + FC028c * FP120c + FC028d * FP120e + FC028e * FP120f + FC028f * FP120h + FC028g * FP120i"]
[null,null,{"$f":"VLOOKUP($D259,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NOX emissions to air (not from material/energy input), final conversion"},"FC028a","gNOX/MJoutput",{"$f":"VLOOKUP(D259,Parameters!$1:$2792,6,FALSE)","v":0},{"$f":"F259","v":0}]
[null,null,{"$f":"VLOOKUP($D260,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH3 emissions to air (not from material/energy input), final conversion"},"FC028c","gNH3/MJoutput",{"$f":"VLOOKUP(D260,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D261,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NO3- emissions to water (not from material/energy input), final conversion"},"FC028d","gNO3/MJoutput",{"$f":"VLOOKUP(D261,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D262,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"NH4+ emissions to water (not from material/energy input), final conversion"},"FC028e","gNH4/MJoutput",{"$f":"VLOOKUP(D262,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D263,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"PO43- emissions to water (not from material/energy input), final conversion"},"FC028f","gPO4/MJoutput",{"$f":"VLOOKUP(D263,Parameters!$1:$2792,6,FALSE)","v":0},0]
[null,null,{"$f":"VLOOKUP($D264,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"COD emissions to water (not from material/energy input), final conversion"},"FC028g","gCOD/MJoutput",{"$f":"VLOOKUP(D264,Parameters!$1:$2792,6,FALSE)","v":0},0]
["Totally allocated eutrophication potential from final conversion"]
[null,{"$f":"VLOOKUP($D266,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Totally allocated eutrophication potential from final conversion"},null,"FC045g","gSO2_eq/MJFU",null,{"$f":"G254*(G22+G23)*G68/100","v":0},"= FC070 * (FC033 + FC034) * FC025c / 100"]
["Total cumulated eutrophication potential (before allocation 4)"]
[null,{"$f":"VLOOKUP($D268,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential before allocation 4"},null,"FC040g","gSO2_eq/MJinput",null,{"$f":"'Conversion feedstock1'!G483*G11/100+'Conversion feedstock2'!G483*G13/100+G254","v":3.3257093356913932},"= BC082g * FC002a / 100 + BC582g * FC002b / 100 + FC070"]
["Total cumulated eutrophication potential (after allocation 4)"]
[null,{"$f":"VLOOKUP($D270,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential allocated to heat production"},null,"FC041g","gSO2_eq/MJh",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G268/G15*G66))))","v":0},"= FC040g / FC003b * FC025a"]
[null,{"$f":"VLOOKUP($D271,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential allocated to heat production"},null,"FC042g","gSO2_eq/MJFU",null,{"$f":"G270*G20","v":0},"= FC041g * FC031"]
[null,{"$f":"VLOOKUP($D272,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential allocated to electricity production"},null,"FC043g","gSO2_eq/MJe",null,{"$f":"IF(G19=\"MJ gas\",0,IF(G19=\"MJ diesel\",0,IF(G19=\"MJ gasoline\",0,IF(G19=\"MJ heavy fuel oil\",0,G268/G14*G67))))","v":0},"= FC040g / FC003a * FC025b"]
[null,{"$f":"VLOOKUP($D273,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential allocated to electricity production"},null,"FC044g","gSO2_eq/MJFU",null,{"$f":"G272*G21","v":0},"= FC043g * FC032"]
[null,{"$f":"VLOOKUP($D274,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Total eutrophication potential allocated to energy production"},null,"FC046g","gSO2_eq/MJFU",null,{"$f":"IF(functionalunit=\"0\",G268*(G22+G23)*G68/100,G268*G68/100)","v":3.3257093356913932},"= FC040g * (FC033 + FC034) * FC025c / 100"]
["Comparison to fossil reference system"]
[null,{"$f":"VLOOKUP($D276,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of reference system for heat"},null,"FC047g","gSO2_eq/MJh",{"$f":"'Standard Values'!Y123","v":0.4},{"$f":"F276","v":0.4}]
[null,{"$f":"VLOOKUP($D277,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of reference system for electricity"},null,"FC048g","gSO2_eq/MJe",{"$f":"'Standard Values'!Y109","v":0.6},0.6]
[null,{"$f":"VLOOKUP($D278,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of reference system for biogas"},null,"FC110g","gSO2_eq/MJbiogas",{"$f":"'Standard Values'!Y27","v":0},0]
[null,{"$f":"VLOOKUP($D279,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of reference system for diesel"},null,"FC111g","gSO2_eq/MJdiesel",{"$f":"'Standard Values'!Y32","v":0},0]
[null,{"$f":"VLOOKUP($D280,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of reference system for gasoline"},null,"FC112g","gSO2_eq/MJgasoline",{"$f":"'Standard Values'!Y33","v":0},0]
[null,{"$f":"VLOOKUP($D281,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of reference system for heavy fuel oil"},null,"FC113g","gSO2_eq/MJhfo",{"$f":"'Standard Values'!Y34","v":0},0]
[null,{"$f":"VLOOKUP($D282,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential of total reference system"},null,"FC051g","gSO2_eq/MJFU",null,{"$f":"IF(G19=\"MJ gas\",G278,IF(G19=\"MJ diesel\",G279,IF(G19=\"MJ gasoline\",G280,IF(G19=\"MJ heavy fuel oil\",G281,G276*G20+G277*G21))))","v":0},"= FC047g * FC031 + FC048g * FC032"]
[null,{"$f":"VLOOKUP($D283,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential reduction of heat production"},null,"FC049g","%",null,{"$f":"IF(F15=0,0,(G276-G270)/G276*100)","v":0},"= (FC047f - FC041f) / FC047f * 100"]
[null,{"$f":"VLOOKUP($D284,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential reduction of electricity production"},null,"FC050g","%",null,{"$f":"IF(F14=0,0,(G277-G272)/G277*100)","v":0},"= (FC048f - FC043f) / FC048f * 100"]
[null,{"$f":"VLOOKUP($D285,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Eutrophication potential reduction of total energy production"},null,"FC052g","%",null,{"$f":"IF(G282=0,0,(G282-G274)/G282*100)","v":0},"= (FC051f - FC046f) / FC051f * 100"]
[]
["BIODIVERSITY & HIGH CARBON STOCK",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Land with high biodiversity value"]
[null,"N.A."]
["Land with high carbon stock"]
[null,"N.A."]
["Criterium RED"]
[null,"N.A."]
[]
["LOCAL WELL-BEING",null,null,"ID-number","Unit","Input/Database","Calculated","Formula"]
["Human and property rights, final conversion"]
[null,{"$f":"VLOOKUP($D297,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No forced labour, final conversion"},null,"FC080a","-",{"$f":"VLOOKUP(D297,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},{"$f":"IF(F297=\"Fulfilled\",0,1)","v":0}]
[null,{"$f":"VLOOKUP($D298,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No child labour, final conversion"},null,"FC080b","-",{"$f":"VLOOKUP(D298,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},{"$f":"IF(F298=\"Fulfilled\",0,1)","v":0}]
[null,{"$f":"VLOOKUP($D299,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Good social practices regarding human rights, final conversion"},null,"FC080c","-",{"$f":"VLOOKUP(D299,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},0]
[null,{"$f":"VLOOKUP($D300,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"No discrimination, final conversion"},null,"FC080d","-",{"$f":"VLOOKUP(D300,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},0]
[null,{"$f":"VLOOKUP($D301,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Land is used legitimately / land rights have been secured, final conversion"},null,"FC080e","-"]
[null,{"$f":"VLOOKUP($D302,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Open and transparent communication with local communities and stakeholders, final conversion"},null,"FC080f","-",{"$f":"VLOOKUP(D302,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},0]
[null,{"$f":"VLOOKUP($D303,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Food security, final conversion"},null,"FC080g","-"]
["Labour rights and conditions, final conversion"]
[null,{"$f":"VLOOKUP($D305,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair legal contracts, final conversion"},null,"FC081a","-",{"$f":"VLOOKUP(D305,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},{"$f":"IF(F305=\"Fulfilled\",0,1)","v":0}]
[null,{"$f":"VLOOKUP($D306,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Workers rights, final conversion"},null,"FC081b","-",{"$f":"VLOOKUP(D306,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},{"$f":"IF(F306=\"Fulfilled\",0,1)","v":0}]
[null,{"$f":"VLOOKUP($D307,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Freedom to join labour organizations or organize themselves, final conversion"},null,"FC081c","-",{"$f":"VLOOKUP(D307,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},0]
[null,{"$f":"VLOOKUP($D308,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Fair wages and compensation rules, final conversion"},null,"FC081d","-",{"$f":"VLOOKUP(D308,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},0]
[null,{"$f":"VLOOKUP($D309,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health, safety and hygiene policy, final conversion"},null,"FC081e","-",{"$f":"VLOOKUP(D309,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},0]
[null,{"$f":"VLOOKUP($D310,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Risk assessment for safe and healthy working conditions, final conversion"},null,"FC081f","-",{"$f":"VLOOKUP(D310,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},0]
[null,{"$f":"VLOOKUP($D311,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Health and safety training, final conversion"},null,"FC081g","-",{"$f":"VLOOKUP(D311,Parameters!$1:$1958,6,FALSE)","v":"Fulfilled"},0]
["Scores"]
[null,{"$f":"VLOOKUP($D313,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Human and property rights, final conversion_score"},null,"FC082","-",null,{"$f":"SUM(G297:G303)","v":0},"= FP080a + FP080b + FP080c + FP080d + FP080e + FP080f + FP080g"]
[null,{"$f":"VLOOKUP($D314,'ID-numbers'!$A$3:$C$3320,2,FALSE)","v":"Labour rights and conditions, final conversion_score"},null,"FC083","-",null,{"$f":"SUM(G305:G311)","v":0},"= FP081a + FP081b + FP081c + FP081d + FP081e + FP081f + FP081g"]

{"sheet":"Graph results","index":25,"n_rows":78,"n_cols":8,"rows_kept":78,"cut":false,"hidden":true,"merged":[]}
["Monitoring framework - Graph results"]
[]
["MASS BALANCE"]
[null,"Bioenergy system","Fossil reference system"]
["Fossil energy requirement",{"$f":"IF(VLOOKUP(\"FC046a\",Parameters!$1:$5288,7,FALSE)<1,VLOOKUP(\"FC046a\",Parameters!$1:$5288,7,FALSE),1)","v":0.17800166505611817},{"$f":"IF(VLOOKUP(\"FC051a\",Parameters!$1:$5288,7,FALSE)<1,VLOOKUP(\"FC051a\",Parameters!$1:$5288,7,FALSE),1)","v":1}]
["Greenhouse gas balance",{"$f":"IF(VLOOKUP(\"FC046c\",Parameters!$1:$5288,7,FALSE)/VLOOKUP(\"FC051c\",Parameters!$1:$5288,7,FALSE)<1,VLOOKUP(\"FC046c\",Parameters!$1:$5288,7,FALSE)/VLOOKUP(\"FC051c\",Parameters!$1:$5288,7,FALSE),1)","v":0.67545729447388914},1]
["Use of water",{"$f":"IF(VLOOKUP(\"FC046d\",Parameters!$1:$5288,7,FALSE)/500<1,VLOOKUP(\"FC046d\",Parameters!$1:$5288,7,FALSE)/500,1)","v":0.84441757022181108},{"$f":"IF(VLOOKUP(\"FC051d\",Parameters!$1:$5288,7,FALSE)/300<1,VLOOKUP(\"FC051d\",Parameters!$1:$5288,7,FALSE)/300,1)","v":0}]
["Use of land",{"$f":"IF(VLOOKUP(\"FC046e\",Parameters!$1:$5288,7,FALSE)/0.1<1,VLOOKUP(\"FC046e\",Parameters!$1:$5288,7,FALSE)/0.1,1)","v":0.19132606099961733},0]
["Acidification",{"$f":"IF(VLOOKUP(\"FC046f\",Parameters!$1:$5288,7,FALSE)/10<1,VLOOKUP(\"FC046f\",Parameters!$1:$5288,7,FALSE)/10,1)","v":9.378627773539415E-2},{"$f":"IF(VLOOKUP(\"FC051f\",Parameters!$1:$5288,7,FALSE)/10<1,VLOOKUP(\"FC051f\",Parameters!$1:$5288,7,FALSE)/10,1)","v":0}]
["Eutrophication",{"$f":"IF(VLOOKUP(\"FC046g\",Parameters!$1:$5288,7,FALSE)/20<1,VLOOKUP(\"FC046g\",Parameters!$1:$5288,7,FALSE)/20,1)","v":0.16628546678456965},{"$f":"IF(VLOOKUP(\"FC051g\",Parameters!$1:$5288,7,FALSE)/20<1,VLOOKUP(\"FC051g\",Parameters!$1:$5288,7,FALSE)/20,1)","v":0}]
["ENERGY BALANCE"]
["Fossil energy requirement","MJfossil/MJFU","Formula","Feedstock 1","Feedstock 2","Formula","Uncertainty","Std"]
["Cultivation",{"$f":"'Production feedstock1'!G105+'Production feedstock2'!G105","v":0},"= FP025a + FP525a",{"$f":"'Production feedstock1'!G103","v":0},{"$f":"'Production feedstock2'!G103","v":0},"= FP024a","Feedstock 1",{"$f":"MonteCarlo!N9","v":0}]
["Processing",{"$f":"VLOOKUP(\"FC046a\",Parameters!$1:$5288,7,FALSE)-'Graph results'!B13-'Graph results'!B15","v":1.6357622712156739E-3},"= FC046a - Cultivation - Transport",{"$f":"'Conversion feedstock1'!G330-'Graph results'!D13-'Graph results'!D15","v":1.6357622712156739E-3},{"$f":"'Conversion feedstock2'!G330-'Graph results'!E13-'Graph results'!E15","v":0},"= BC082a - FP024a - FT026a","Feedstock 2",{"$f":"MonteCarlo!O9","v":0}]
["Transport ",{"$f":"'Transport feedstock1'!G150+'Transport feedstock2'!G150","v":0.1763659027849025},"= FT027a + FT527a",{"$f":"'Transport feedstock1'!G148","v":0.1763659027849025},{"$f":"'Transport feedstock2'!G148","v":0},"= FT026a","Total",{"$f":"MonteCarlo!P9","v":0}]
["Fossil Reference",{"$f":"'Final conversion'!G127","v":1.1599999999999999},"= FC051a",null,null,null,"Fossil reference",{"$f":"B16*0.15","v":0.17399999999999999}]
["Primary energy requirement","MJprim/MJFU","Formula","Feedstock 1","Feedstock 2","Formula"]
["Cultivation",{"$f":"'Production feedstock1'!G106+'Production feedstock2'!G106","v":0.28755075519938561},"= FP025b + FP525b",{"$f":"'Production feedstock1'!G104","v":0.28755075519938561},{"$f":"'Production feedstock2'!G104","v":0},"= FP024b","Feedstock 1",{"$f":"MonteCarlo!Q9","v":0}]
["Processing",{"$f":"'Final conversion'!G111-'Graph results'!B18-'Graph results'!B20","v":2.4536434068236912E-3},"= FC046b - Cultivation - Transport",{"$f":"'Conversion feedstock1'!G331-'Graph results'!D18-'Graph results'!D20","v":2.4536434068236912E-3},{"$f":"'Conversion feedstock2'!G331-'Graph results'!E18-'Graph results'!E20","v":0},"= BC082b - FP024b - FT026b","Feedstock 2",{"$f":"MonteCarlo!R9","v":0}]
["Transport ",{"$f":"'Transport feedstock1'!G151+'Transport feedstock2'!G151","v":0.26454885417735374},"= FT027b + FT527b",{"$f":"'Transport feedstock1'!G149","v":0.26454885417735374},{"$f":"'Transport feedstock2'!G149","v":0},"= FT026b","Total",{"$f":"MonteCarlo!S$9","v":0}]
["Fossil Reference",{"$f":"'Final conversion'!G128","v":1.7399999999999998},"= FC051b",null,null,null,"Fossil reference",{"$f":"B21*0.15","v":0.26099999999999995}]
["GLOBAL WARMING"]
["GHG balance","gCO2_eq/MJFU","Formula","Feedstock 1","Feedstock 2","Formula"]
["Cultivation",{"$f":"'Production feedstock1'!G237+'Production feedstock2'!G237","v":44.685763325221714},"= FP061b + FP561b",{"$f":"'Production feedstock1'!G236","v":44.685763325221714},{"$f":"'Production feedstock2'!G236","v":0},"= FP061a","Feedstock 1",{"$f":"MonteCarlo!T9","v":0}]
["Processing",{"$f":"'Final conversion'!G151-'Graph results'!B24-'Graph results'!B26","v":0.65300153519651971},"= FC046c - Cultivation - Transport",{"$f":"'Conversion feedstock1'!G368-'Graph results'!D24-'Graph results'!D26","v":0.65300153519651971},{"$f":"'Conversion feedstock2'!G368-'Graph results'!E24-'Graph results'!E26","v":0},"= BC082c - FP061a - FT033a","Feedstock 2",{"$f":"MonteCarlo!U9","v":0}]
["Transport ",{"$f":"'Transport feedstock1'!G175+'Transport feedstock2'!G175","v":13.857561919168443},"= FT033b + FT533b",{"$f":"'Transport feedstock1'!G174","v":13.857561919168443},{"$f":"'Transport feedstock2'!G174","v":0},"= FT033a","Total",{"$f":"MonteCarlo!V9","v":0}]
["Fossil Reference",{"$f":"'Final conversion'!G159","v":87.6388888888889},"= FC051c",null,null,null,"Fossil reference",{"$f":"B27*0.15","v":13.145833333333334}]
["Carbon debt & repayment time","tCO2_eq/ha","Formula","Feedstock 1","Feedstock 2","Formula"]
["Carbon stock emissions per ha",{"$f":"VLOOKUP(\"FC055\",Parameters!$1:$5288,7,FALSE)","v":0},"= FC055",{"$f":"IF('Production feedstock1'!G242<0,0,'Production feedstock1'!G242/1000000)","v":0},{"$f":"IF('Production feedstock2'!G242<0,0,'Production feedstock2'!G242/1000000)","v":0},"= FP107a (if <0 than no debt)","Feedstock 1",{"$f":"MonteCarlo!W9","v":0}]
[null,null,null,null,null,null,"Feedstock 2",{"$f":"MonteCarlo!X9","v":0}]
[null,null,null,null,null,null,"Total",{"$f":"MonteCarlo!Y9","v":0}]
["RESOURCE USE"]
["Use of water","m³/GJFU","Formula","Feedstock 1","Feedstock 2","Formula"]
["Cultivation",{"$f":"VLOOKUP(\"FP102b\",Parameters!$1:$5288,7,FALSE)+VLOOKUP(\"FP602b\",Parameters!$1:$5288,7,FALSE)","v":422.20878511090552},"= FP102b + FP602b",{"$f":"VLOOKUP(\"FP102a\",Parameters!$1:$5288,7,FALSE)","v":422.20878511090552},{"$f":"VLOOKUP(\"FP602a\",Parameters!$1:$5288,7,FALSE)","v":0},"= FP102a","Feedstock 1",{"$f":"MonteCarlo!Z9","v":0}]
["Processing",{"$f":"VLOOKUP(\"FC046d\",Parameters!$1:$5288,7,FALSE)-B34-B36","v":0},"= FC046d - Cultivation - Transport",{"$f":"VLOOKUP(\"BC082d\",Parameters!$1:$5288,7,FALSE)-D34-D36","v":0},{"$f":"VLOOKUP(\"BC582d\",Parameters!$1:$5288,7,FALSE)-E34-E36","v":0},"= BC082d - FP102a","Feedstock 2",{"$f":"MonteCarlo!AA9","v":0}]
["Transport ",0,"/",0,0,"/","Total",{"$f":"MonteCarlo!AB9","v":0}]
["Fossil Reference",{"$f":"VLOOKUP(\"FC051d\",Parameters!$1:$5288,7,FALSE)","v":0},"= FC051d",null,null,null,"Fossil reference",{"$f":"B37*0.15","v":0}]
["Use of land","ha/GJFU","Formula","Feedstock 1","Feedstock 2","Formula"]
["Cultivation",{"$f":"VLOOKUP(\"FC046e\",Parameters!$1:$5288,7,FALSE)","v":1.9132606099961733E-2},"= FC046e",{"$f":"VLOOKUP(\"FP106a\",Parameters!$1:$5288,7,FALSE)","v":1.9132606099961733E-2},{"$f":"VLOOKUP(\"FP606a\",Parameters!$1:$5288,7,FALSE)","v":0},"= FP106a","Feedstock 1",{"$f":"MonteCarlo!AC9","v":0}]
["Processing",0,"/",0,0,"/","Feedstock 2",{"$f":"MonteCarlo!AD9","v":0}]
["Transport ",0,"/",0,0,"/","Total",{"$f":"MonteCarlo!AE9","v":0}]
["Fossil Reference",{"$f":"VLOOKUP(\"FC051e\",Parameters!$1:$5288,7,FALSE)","v":0},"= FC051e",null,null,null,"Fossil reference",{"$f":"B42*0.15","v":0}]
["ENVIRONMENTAL QUALITY"]
["Acidification potential","gSO2_eq/MJFU","Formula","Feedstock 1","Feedstock 2","Formula"]
["Cultivation",{"$f":"VLOOKUP(\"FP115b\",Parameters!$1:$5288,7,FALSE)+VLOOKUP(\"FP615b\",Parameters!$1:$5288,7,FALSE)","v":0.78450695493120459},"= FP115b + FP615b",{"$f":"VLOOKUP(\"FP115a\",Parameters!$1:$5288,7,FALSE)","v":0.78450695493120459},{"$f":"VLOOKUP(\"FP615a\",Parameters!$1:$5288,7,FALSE)","v":0},"= FP115a","Feedstock 1",{"$f":"MonteCarlo!AF9","v":0}]
["Processing",{"$f":"VLOOKUP(\"FC046f\",Parameters!$1:$5288,7,FALSE)-B45-B47","v":0},"= FC046f - Cultivation - Transport",{"$f":"VLOOKUP(\"BC082f\",Parameters!$1:$5288,7,FALSE)-D45-D47","v":0},{"$f":"VLOOKUP(\"BC582f\",Parameters!$1:$5288,7,FALSE)-E45-E47","v":0},"= BC082f - Cultivation - Transport","Feedstock 2",{"$f":"MonteCarlo!AG9","v":0}]
["Transport ",{"$f":"VLOOKUP(\"FT043b\",Parameters!$1:$5288,7,FALSE)+VLOOKUP(\"FT543b\",Parameters!$1:$5288,7,FALSE)","v":0.15335582242273696},"= FT043b + FT543b",{"$f":"VLOOKUP(\"FT043a\",Parameters!$1:$5288,7,FALSE)","v":0.15335582242273696},{"$f":"VLOOKUP(\"FT543a\",Parameters!$1:$5288,7,FALSE)","v":0},"= FT043a","Total",{"$f":"MonteCarlo!AH9","v":0}]
["Fossil Reference",{"$f":"VLOOKUP(\"FC051f\",Parameters!$1:$5288,7,FALSE)","v":0},"= FC051f",null,null,null,"Fossil reference",{"$f":"B48*0.15","v":0}]
["Eutrophication potential","gPO4_eq/MJFU","Formula","Feedstock 1","Feedstock 2","Formula"]
["Cultivation",{"$f":"VLOOKUP(\"FP125b\",Parameters!$1:$5288,7,FALSE)+VLOOKUP(\"FP625b\",Parameters!$1:$5288,7,FALSE)","v":1.9914646988440075},"= FP125b + FP625b",{"$f":"VLOOKUP(\"FP125a\",Parameters!$1:$5288,7,FALSE)","v":1.9914646988440075},{"$f":"VLOOKUP(\"FP625a\",Parameters!$1:$5288,7,FALSE)","v":0},"= FP125a","Feedstock 1",{"$f":"MonteCarlo!AI9","v":0}]
["Processing",{"$f":"VLOOKUP(\"FC046g\",Parameters!$1:$5288,7,FALSE)-B50-B52","v":1.3159295156592201},"= FC046g - Cultivation - Transport",{"$f":"VLOOKUP(\"BC082g\",Parameters!$1:$5288,7,FALSE)-D50-D52","v":1.3159295156592201},{"$f":"VLOOKUP(\"BC582g\",Parameters!$1:$5288,7,FALSE)-E50-E52","v":0},"= BC082g - Cultivation - Transport","Feedstock 2",{"$f":"MonteCarlo!AJ9","v":0}]
["Transport ",{"$f":"VLOOKUP(\"FT047b\",Parameters!$1:$5288,7,FALSE)+VLOOKUP(\"FT547b\",Parameters!$1:$5288,7,FALSE)","v":1.8315121188165487E-2},"= FT047b + FT547b+5",{"$f":"VLOOKUP(\"FT047a\",Parameters!$1:$5288,7,FALSE)","v":1.8315121188165487E-2},{"$f":"VLOOKUP(\"FT547a\",Parameters!$1:$5288,7,FALSE)","v":0},"= FT047a","Total",{"$f":"MonteCarlo!AK9","v":0}]
["Fossil Reference",{"$f":"VLOOKUP(\"FC051g\",Parameters!$1:$5288,7,FALSE)","v":0},"= FC051g",null,null,null,"Fossil reference",{"$f":"B53*0.15","v":0}]
["BIODIVERSITY & HIGH CARBON STOCK"]
["Biodiversity & high carbon stock ",null,"Feedstock 1",null,"Feedstock 2"]
["Undisturbed forest","green",{"$f":"IF(VLOOKUP(\"FP161\",Parameters!$1:$5067,6,FALSE)=0,1,0)","v":0},"green",{"$f":"IF(VLOOKUP(\"FP661\",Parameters!$1:$5296,6,FALSE)=0,1,0)","v":1}]
[null,"red",{"$f":"IF(VLOOKUP(\"FP161\",Parameters!$1:$5067,6,FALSE)=0,0,1)","v":1},"red",{"$f":"IF(VLOOKUP(\"FP661\",Parameters!$1:$5296,6,FALSE)=0,0,1)","v":0}]
["Nature protection area","green",{"$f":"IF(VLOOKUP(\"FP162\",Parameters!$1:$5067,6,FALSE)=0,1,0)","v":0},"green",{"$f":"IF(VLOOKUP(\"FP662\",Parameters!$1:$5296,6,FALSE)=0,1,0)","v":1}]
[null,"red",{"$f":"IF(VLOOKUP(\"FP162\",Parameters!$1:$5067,6,FALSE)=0,0,1)","v":1},"red",{"$f":"IF(VLOOKUP(\"FP662\",Parameters!$1:$5296,6,FALSE)=0,0,1)","v":0}]
["Highly biodiverse grassland","green",{"$f":"IF(VLOOKUP(\"FP163\",Parameters!$1:$5067,6,FALSE)=0,1,0)","v":1},"green",{"$f":"IF(VLOOKUP(\"FP663\",Parameters!$1:$5296,6,FALSE)=0,1,0)","v":1}]
[null,"red",{"$f":"IF(VLOOKUP(\"FP163\",Parameters!$1:$5067,6,FALSE)=0,0,1)","v":0},"red",{"$f":"IF(VLOOKUP(\"FP663\",Parameters!$1:$5296,6,FALSE)=0,0,1)","v":0}]
["Wetlands","green",{"$f":"IF(VLOOKUP(\"FP164\",Parameters!$1:$5067,6,FALSE)=0,1,0)","v":1},"green",{"$f":"IF(VLOOKUP(\"FP664\",Parameters!$1:$5296,6,FALSE)=0,1,0)","v":1}]
[null,"red",{"$f":"IF(VLOOKUP(\"FP164\",Parameters!$1:$5067,6,FALSE)=0,0,1)","v":0},"red",{"$f":"IF(VLOOKUP(\"FP664\",Parameters!$1:$5296,6,FALSE)=0,0,1)","v":0}]
["Continuously forested areas","green",{"$f":"IF(VLOOKUP(\"FP165\",Parameters!$1:$5067,6,FALSE)=0,1,0)","v":0},"green",{"$f":"IF(VLOOKUP(\"FP665\",Parameters!$1:$5296,6,FALSE)=0,1,0)","v":1}]
[null,"red",{"$f":"IF(VLOOKUP(\"FP165\",Parameters!$1:$5067,6,FALSE)=0,0,1)","v":1},"red",{"$f":"IF(VLOOKUP(\"FP665\",Parameters!$1:$5296,6,FALSE)=0,0,1)","v":0}]
["Peatland","green",{"$f":"IF(VLOOKUP(\"FP166\",Parameters!$1:$5067,6,FALSE)=0,1,0)","v":1},"green",{"$f":"IF(VLOOKUP(\"FP666\",Parameters!$1:$5296,6,FALSE)=0,1,0)","v":1}]
[null,"red",{"$f":"IF(VLOOKUP(\"FP166\",Parameters!$1:$5067,6,FALSE)=0,0,1)","v":0},"red",{"$f":"IF(VLOOKUP(\"FP666\",Parameters!$1:$5296,6,FALSE)=0,0,1)","v":0}]
["LOCAL WELL-BEING"]
["Human and property rights","Final conversion",null,"Feedstock 1","Feedstock 2"]
["Cultivation",null,null,{"$f":"IF(VLOOKUP(\"FP172\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"FP172\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"FP172\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"FP172\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":95},{"$f":"IF(VLOOKUP(\"FP672\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"FP672\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"FP672\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"FP672\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":5},"=FP172 or FP672 (if 0 then 10, 1 then 40, 2 then 60, 3 then 80, 4 or more then 90)"]
["Processing",{"$f":"IF(VLOOKUP(\"FC082\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"FC082\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"FC082\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"FC082\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":5},null,{"$f":"IF(VLOOKUP(\"BC160\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"BC160\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"BC160\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"BC160\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":95},{"$f":"IF(VLOOKUP(\"BC660\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"BC660\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"BC660\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"BC660\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":5},"=BC160 or BC660 (if 0 then 10, 1 then 40, 2 then 60, 3 then 80, 4 or more then 90)"]
[]
["Fossil Reference"]
["Labour rights and conditions","Final conversion",null,"Feedstock 1","Feedstock 2"]
["Cultivation",null,null,{"$f":"IF(VLOOKUP(\"FP173\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"FP173\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"FP173\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"FP173\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":95},{"$f":"IF(VLOOKUP(\"FP673\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"FP673\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"FP673\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"FP673\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":5},"=FP173 or FP673 (if 0 then 10, 1 then 40, 2 then 60, 3 then 80, 4 or more then 90)"]
["Processing",{"$f":"IF(VLOOKUP(\"FC083\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"FC083\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"FC083\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"FC083\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":5},null,{"$f":"IF(VLOOKUP(\"BC161\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"BC161\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"BC161\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"BC161\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":95},{"$f":"IF(VLOOKUP(\"BC661\",Parameters!$1:$5296,7,FALSE)=0,5,IF(VLOOKUP(\"BC661\",Parameters!$1:$5296,7,FALSE)=1,40,IF(VLOOKUP(\"BC661\",Parameters!$1:$5296,7,FALSE)=2,60,IF(VLOOKUP(\"BC661\",Parameters!$1:$5296,7,FALSE)=3,80,95))))","v":5},"=BC161 or BC661 (if 0 then 10, 1 then 40, 2 then 60, 3 then 80, 4 or more then 90)"]
[]
["Fossil Reference"]

{"sheet":"MonteCarlo","index":26,"n_rows":209,"n_cols":37,"rows_kept":209,"cut":false,"hidden":true,"merged":[]}
["Monte Carlo Simulation"]
[]
["Inputs"]
[null,"Iterations",200]
[null,"Screen update interval",{"$f":"Iterations/10","v":20}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"FER fs1","FER fs2","FER total","PER fs1","PER fs2","PER total","GHG fs1","GHG fs2","GHG total","CD fs1","CD fs2","CD total","WATER fs1","WATER fs2","WATER total","LAND fs1","LAND fs2","LAND total","AP fs1","AP fs2","AP total","EP fs1","EP fs2","EP total"]
["Results preprocessing",null,null,null,null,null,null,null,null,null,null,null,null,"BC082a","BC582a","FC046a","BC082b","BC582b","FC046b","BC082c","BC582c","FC046c","FP107a","FP607a","FC055","BC082d","BC582d","FC046d","FP106a","FP606a","FC046e","BC082f","BC582f","FC046f","BC082g","BC582g","FC046g"]
[null,null,null,null,null,null,null,null,null,null,null,null,"MEAN",{"$f":"AVERAGE(N10:N209)","v":0},{"$f":"AVERAGE(O10:O209)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"Output Fossil","Mean","Std",null,null,null,null,null,null,null,null,"STD",{"$f":"STDEV(N10:N209)","v":0},{"$f":"STDEV(O10:O209)","v":0},0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37568396262810788,{"$f":"AVERAGE($B$10:B10)","v":0.37568396262810788},null,null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37910436251934754,{"$f":"AVERAGE($B$10:B11)","v":0.37739416257372771},{"$f":"STDEV($B$10:B11)","v":2.4185879574652905E-3},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.43458746019323824,{"$f":"AVERAGE($B$10:B12)","v":0.39645859511356457},{"$f":"STDEV($B$10:B12)","v":3.3064823423874012E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.4112340331113476,{"$f":"AVERAGE($B$10:B13)","v":0.4001524546130103},{"$f":"STDEV($B$10:B13)","v":2.7989880743604961E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41588133027477847,{"$f":"AVERAGE($B$10:B14)","v":0.40329822974536389},{"$f":"STDEV($B$10:B14)","v":2.5239940054358163E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32992957912085769,{"$f":"AVERAGE($B$10:B15)","v":0.39107012130794622},{"$f":"STDEV($B$10:B15)","v":3.7507378939370742E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34867249224775043,{"$f":"AVERAGE($B$10:B16)","v":0.38501331715648973},{"$f":"STDEV($B$10:B16)","v":3.7803840608969019E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3621643816263862,{"$f":"AVERAGE($B$10:B17)","v":0.38215720021522681},{"$f":"STDEV($B$10:B17)","v":3.5919745488542099E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33374362645284561,{"$f":"AVERAGE($B$10:B18)","v":0.37677791424162893},{"$f":"STDEV($B$10:B18)","v":3.7274388790940083E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.30540279875527709,{"$f":"AVERAGE($B$10:B19)","v":0.3696404026929937},{"$f":"STDEV($B$10:B19)","v":4.1766556101910254E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36825199547540521,{"$f":"AVERAGE($B$10:B20)","v":0.36951418385503115},{"$f":"STDEV($B$10:B20)","v":3.9625445497788257E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.43474637331758686,{"$f":"AVERAGE($B$10:B21)","v":0.37495019964357751},{"$f":"STDEV($B$10:B21)","v":4.2214166772456561E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.31951369675157543,{"$f":"AVERAGE($B$10:B22)","v":0.3706858532672696},{"$f":"STDEV($B$10:B22)","v":4.324272582555834E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36167947912707726,{"$f":"AVERAGE($B$10:B23)","v":0.37004254082868443},{"$f":"STDEV($B$10:B23)","v":4.1615937132615258E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.30345771230417717,{"$f":"AVERAGE($B$10:B24)","v":0.36560355226038399},{"$f":"STDEV($B$10:B24)","v":4.3631976316140048E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32783303890443255,{"$f":"AVERAGE($B$10:B25)","v":0.36324289517563702},{"$f":"STDEV($B$10:B25)","v":4.3197175409783711E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36449936827496127,{"$f":"AVERAGE($B$10:B26)","v":0.36331680535795019},{"$f":"STDEV($B$10:B26)","v":4.1826595388914874E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.42542394312456211,{"$f":"AVERAGE($B$10:B27)","v":0.36676720190053974},{"$f":"STDEV($B$10:B27)","v":4.3137555370880987E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3778205647468611,{"$f":"AVERAGE($B$10:B28)","v":0.3673489578398198},{"$f":"STDEV($B$10:B28)","v":4.1998792368959176E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35932932143381663,{"$f":"AVERAGE($B$10:B29)","v":0.36694797601951962},{"$f":"STDEV($B$10:B29)","v":4.0917936440095046E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36531534379474595,{"$f":"AVERAGE($B$10:B30)","v":0.36687023162786375},{"$f":"STDEV($B$10:B30)","v":3.9883462417259666E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34306818901882608,{"$f":"AVERAGE($B$10:B31)","v":0.36578832060018018},{"$f":"STDEV($B$10:B31)","v":3.9251689091810336E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41312080689582797,{"$f":"AVERAGE($B$10:B32)","v":0.36784625478694744},{"$f":"STDEV($B$10:B32)","v":3.9598871738402465E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.44633004667389187,{"$f":"AVERAGE($B$10:B33)","v":0.37111641278223678},{"$f":"STDEV($B$10:B33)","v":4.1911192514863242E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36235624585110293,{"$f":"AVERAGE($B$10:B34)","v":0.37076600610499144},{"$f":"STDEV($B$10:B34)","v":4.1066143921568141E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39149780490073588,{"$f":"AVERAGE($B$10:B35)","v":0.37156338298175079},{"$f":"STDEV($B$10:B35)","v":4.0441341551645527E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36990749738292888,{"$f":"AVERAGE($B$10:B36)","v":0.37150205388549817},{"$f":"STDEV($B$10:B36)","v":3.9657278440295991E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.29798940608708369,{"$f":"AVERAGE($B$10:B37)","v":0.36887660217841189},{"$f":"STDEV($B$10:B37)","v":4.1321368584255454E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3229639542946966,{"$f":"AVERAGE($B$10:B38)","v":0.36729340742380101},{"$f":"STDEV($B$10:B38)","v":4.1462797919875533E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41378053352280408,{"$f":"AVERAGE($B$10:B39)","v":0.36884297829376778},{"$f":"STDEV($B$10:B39)","v":4.1616309350259159E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39995291536355071,{"$f":"AVERAGE($B$10:B40)","v":0.36984652465085754},{"$f":"STDEV($B$10:B40)","v":4.1296572430258402E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37083077044864399,{"$f":"AVERAGE($B$10:B41)","v":0.36987728233203837},{"$f":"STDEV($B$10:B41)","v":4.0625411283794273E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39769000314167013,{"$f":"AVERAGE($B$10:B42)","v":0.37072009205354239},{"$f":"STDEV($B$10:B42)","v":4.0277650404975954E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36180727125401208,{"$f":"AVERAGE($B$10:B43)","v":0.37045795026532091},{"$f":"STDEV($B$10:B43)","v":3.9692131065229126E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.49685054112485216,{"$f":"AVERAGE($B$10:B44)","v":0.37406916714702176},{"$f":"STDEV($B$10:B44)","v":4.4559613020691204E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41122739921299972,{"$f":"AVERAGE($B$10:B45)","v":0.37510134025996561},{"$f":"STDEV($B$10:B45)","v":4.4352932036767892E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36756757072403995,{"$f":"AVERAGE($B$10:B46)","v":0.37489772486710271},{"$f":"STDEV($B$10:B46)","v":4.3750115555724202E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40421001199589213,{"$f":"AVERAGE($B$10:B47)","v":0.3756691008441761},{"$f":"STDEV($B$10:B47)","v":4.3416030600119337E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39356599737048481,{"$f":"AVERAGE($B$10:B48)","v":0.37612799562690202},{"$f":"STDEV($B$10:B48)","v":4.2936703565413459E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32957863899823503,{"$f":"AVERAGE($B$10:B49)","v":0.37496426171118535},{"$f":"STDEV($B$10:B49)","v":4.3016982643387477E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41230817431707206,{"$f":"AVERAGE($B$10:B50)","v":0.37587508884791426},{"$f":"STDEV($B$10:B50)","v":4.2874387748876669E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32212506407277702,{"$f":"AVERAGE($B$10:B51)","v":0.37459532635326814},{"$f":"STDEV($B$10:B51)","v":4.315282058191567E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36634642593925582,{"$f":"AVERAGE($B$10:B52)","v":0.37440349145991902},{"$f":"STDEV($B$10:B52)","v":4.2654555058015062E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40194566393246611,{"$f":"AVERAGE($B$10:B53)","v":0.37502944992520421},{"$f":"STDEV($B$10:B53)","v":4.2359643977790143E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40266603650794791,{"$f":"AVERAGE($B$10:B54)","v":0.37564359629370964},{"$f":"STDEV($B$10:B54)","v":4.2077688927052083E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3446799603951573,{"$f":"AVERAGE($B$10:B55)","v":0.37497047377417586},{"$f":"STDEV($B$10:B55)","v":4.1857246357082017E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40644578499849504,{"$f":"AVERAGE($B$10:B56)","v":0.37564016124703375},{"$f":"STDEV($B$10:B56)","v":4.1653572544188139E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32406881214317079,{"$f":"AVERAGE($B$10:B57)","v":0.37456575814070331},{"$f":"STDEV($B$10:B57)","v":4.1874971068300758E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.31488690597838992,{"$f":"AVERAGE($B$10:B58)","v":0.37334782238228875},{"$f":"STDEV($B$10:B58)","v":4.2304452307051328E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.46324363940167002,{"$f":"AVERAGE($B$10:B59)","v":0.37514573872267643},{"$f":"STDEV($B$10:B59)","v":4.3758062496564526E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33781229888953168,{"$f":"AVERAGE($B$10:B60)","v":0.37441371049065397},{"$f":"STDEV($B$10:B60)","v":4.3632577333233065E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35812772625613087,{"$f":"AVERAGE($B$10:B61)","v":0.3741005184861439},{"$f":"STDEV($B$10:B61)","v":4.3261680476336072E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39464241805645583,{"$f":"AVERAGE($B$10:B62)","v":0.37448810149690454},{"$f":"STDEV($B$10:B62)","v":4.2936498465789126E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38918843524880664,{"$f":"AVERAGE($B$10:B63)","v":0.37476032989971747},{"$f":"STDEV($B$10:B63)","v":4.2576530161222252E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3134049796632567,{"$f":"AVERAGE($B$10:B64)","v":0.37364477807723639},{"$f":"STDEV($B$10:B64)","v":4.2984140641258578E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.2851936612401017,{"$f":"AVERAGE($B$10:B65)","v":0.37206529384800185},{"$f":"STDEV($B$10:B65)","v":4.4201245487528094E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32033605763486955,{"$f":"AVERAGE($B$10:B66)","v":0.37115776338812229},{"$f":"STDEV($B$10:B66)","v":4.4337428494312624E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38584694277583409,{"$f":"AVERAGE($B$10:B67)","v":0.37141102510170354},{"$f":"STDEV($B$10:B67)","v":4.3989088649402701E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37116721247186474,{"$f":"AVERAGE($B$10:B68)","v":0.37140689268424865},{"$f":"STDEV($B$10:B68)","v":4.360823512245901E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3371875776286547,{"$f":"AVERAGE($B$10:B69)","v":0.37083657076665538},{"$f":"STDEV($B$10:B69)","v":4.3462194634862582E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41455709156476545,{"$f":"AVERAGE($B$10:B70)","v":0.37155330061580477},{"$f":"STDEV($B$10:B70)","v":4.3460504584204994E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3961325545312071,{"$f":"AVERAGE($B$10:B71)","v":0.37194974019508542},{"$f":"STDEV($B$10:B71)","v":4.3215685346262897E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.4014890204626137,{"$f":"AVERAGE($B$10:B72)","v":0.3724186176596494},{"$f":"STDEV($B$10:B72)","v":4.3027006116688728E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3258786880501377,{"$f":"AVERAGE($B$10:B73)","v":0.37169143125950077},{"$f":"STDEV($B$10:B73)","v":4.3078769432552337E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33922954329586752,{"$f":"AVERAGE($B$10:B74)","v":0.37119201759852183},{"$f":"STDEV($B$10:B74)","v":4.2930125992838034E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38371748964967733,{"$f":"AVERAGE($B$10:B75)","v":0.37138179747808475},{"$f":"STDEV($B$10:B75)","v":4.2626506073862737E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.29681886622214604,{"$f":"AVERAGE($B$10:B76)","v":0.37026891790710059},{"$f":"STDEV($B$10:B76)","v":4.3272023199746379E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.30857909558002389,{"$f":"AVERAGE($B$10:B77)","v":0.36936171463758477},{"$f":"STDEV($B$10:B77)","v":4.3594562927624779E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37989209456776313,{"$f":"AVERAGE($B$10:B78)","v":0.36951432883947144},{"$f":"STDEV($B$10:B78)","v":4.3291392678829796E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37003104792953129,{"$f":"AVERAGE($B$10:B79)","v":0.36952171054075794},{"$f":"STDEV($B$10:B79)","v":4.2976586384170727E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.50161886118727816,{"$f":"AVERAGE($B$10:B80)","v":0.37138223378930052},{"$f":"STDEV($B$10:B80)","v":4.545735659751822E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35946264787716831,{"$f":"AVERAGE($B$10:B81)","v":0.37121668398496532},{"$f":"STDEV($B$10:B81)","v":4.5157953156245455E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39068502900234053,{"$f":"AVERAGE($B$10:B82)","v":0.37148337364273765},{"$f":"STDEV($B$10:B82)","v":4.4901113032637829E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39370444986315128,{"$f":"AVERAGE($B$10:B83)","v":0.371783658456527},{"$f":"STDEV($B$10:B83)","v":4.4667266076655714E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34650371971682198,{"$f":"AVERAGE($B$10:B84)","v":0.37144659260666424},{"$f":"STDEV($B$10:B84)","v":4.4460364126046363E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41287613915361748,{"$f":"AVERAGE($B$10:B85)","v":0.37199171821912413},{"$f":"STDEV($B$10:B85)","v":4.441792392093951E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33448646268766635,{"$f":"AVERAGE($B$10:B86)","v":0.37150463697845587},{"$f":"STDEV($B$10:B86)","v":4.4331255086676909E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.43023346475533619,{"$f":"AVERAGE($B$10:B87)","v":0.37225757066790305},{"$f":"STDEV($B$10:B87)","v":4.4541623579368438E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41696839608108649,{"$f":"AVERAGE($B$10:B88)","v":0.37282353048325978},{"$f":"STDEV($B$10:B88)","v":4.4540155200509808E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40156491543160722,{"$f":"AVERAGE($B$10:B89)","v":0.37318279779511415},{"$f":"STDEV($B$10:B89)","v":4.4373861125112317E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34745158576246005,{"$f":"AVERAGE($B$10:B90)","v":0.37286512851076037},{"$f":"STDEV($B$10:B90)","v":4.4188240205662511E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.42064315951574183,{"$f":"AVERAGE($B$10:B91)","v":0.37344778742545526},{"$f":"STDEV($B$10:B91)","v":4.4230449785842015E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39016935910065809,{"$f":"AVERAGE($B$10:B92)","v":0.37364925214443362},{"$f":"STDEV($B$10:B92)","v":4.3998224728798364E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38520973545901149,{"$f":"AVERAGE($B$10:B93)","v":0.3737868769457976},{"$f":"STDEV($B$10:B93)","v":4.3750558504756815E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36258205869061866,{"$f":"AVERAGE($B$10:B94)","v":0.37365505555456024},{"$f":"STDEV($B$10:B94)","v":4.3506337056758541E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32887104145987778,{"$f":"AVERAGE($B$10:B95)","v":0.37313431120462209},{"$f":"STDEV($B$10:B95)","v":4.3518434427967413E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41149143548859191,{"$f":"AVERAGE($B$10:B96)","v":0.37357519769064473},{"$f":"STDEV($B$10:B96)","v":4.3459679164609223E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36095492311239086,{"$f":"AVERAGE($B$10:B97)","v":0.37343178547952821},{"$f":"STDEV($B$10:B97)","v":4.3230127419674969E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41826180155190246,{"$f":"AVERAGE($B$10:B98)","v":0.37393549352528516},{"$f":"STDEV($B$10:B98)","v":4.324567370059592E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34969439598336655,{"$f":"AVERAGE($B$10:B99)","v":0.37366614799704168},{"$f":"STDEV($B$10:B99)","v":4.3077884969263271E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3594932426166067,{"$f":"AVERAGE($B$10:B100)","v":0.37351040178406986},{"$f":"STDEV($B$10:B100)","v":4.2863651436906153E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38759230380404247,{"$f":"AVERAGE($B$10:B101)","v":0.37366346593646088},{"$f":"STDEV($B$10:B101)","v":4.265276099117777E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37347396399935606,{"$f":"AVERAGE($B$10:B102)","v":0.37366142828122323},{"$f":"STDEV($B$10:B102)","v":4.2420323697640899E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41422102140822958,{"$f":"AVERAGE($B$10:B103)","v":0.37409291331448924},{"$f":"STDEV($B$10:B103)","v":4.2398531002346786E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37672018201630564,{"$f":"AVERAGE($B$10:B104)","v":0.37412056877450839},{"$f":"STDEV($B$10:B104)","v":4.2173265326495409E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3909686799262248,{"$f":"AVERAGE($B$10:B105)","v":0.37429606993233877},{"$f":"STDEV($B$10:B105)","v":4.1985940875798239E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.42660955438537129,{"$f":"AVERAGE($B$10:B106)","v":0.37483538420505047},{"$f":"STDEV($B$10:B106)","v":4.2103087056907448E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.4284657501475192,{"$f":"AVERAGE($B$10:B107)","v":0.37538263283711643},{"$f":"STDEV($B$10:B107)","v":4.2234395180807321E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39208482648558013,{"$f":"AVERAGE($B$10:B108)","v":0.37555134186386857},{"$f":"STDEV($B$10:B108)","v":4.2051878392590329E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.43431915810776611,{"$f":"AVERAGE($B$10:B109)","v":0.37613902002630761},{"$f":"STDEV($B$10:B109)","v":4.2249672325027125E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35152599450476374,{"$f":"AVERAGE($B$10:B110)","v":0.37589532670431208},{"$f":"STDEV($B$10:B110)","v":4.2109173506614542E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39700274252349826,{"$f":"AVERAGE($B$10:B111)","v":0.37610226215351977},{"$f":"STDEV($B$10:B111)","v":4.1952283652660995E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35231904714167783,{"$f":"AVERAGE($B$10:B112)","v":0.37587135715340481},{"$f":"STDEV($B$10:B112)","v":4.181185146324802E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36945084306396497,{"$f":"AVERAGE($B$10:B113)","v":0.37580962144100638},{"$f":"STDEV($B$10:B113)","v":4.1613149148325722E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35217548002621801,{"$f":"AVERAGE($B$10:B114)","v":0.37558453437991313},{"$f":"STDEV($B$10:B114)","v":4.1476781462550127E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33228258283235534,{"$f":"AVERAGE($B$10:B115)","v":0.3751760254030494},{"$f":"STDEV($B$10:B115)","v":4.1492512626127964E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3134559435233098,{"$f":"AVERAGE($B$10:B116)","v":0.37459920220791165},{"$f":"STDEV($B$10:B116)","v":4.1725153080368053E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38293895867785449,{"$f":"AVERAGE($B$10:B117)","v":0.3746764221752259},{"$f":"STDEV($B$10:B117)","v":4.153747074245031E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40517926149291156,{"$f":"AVERAGE($B$10:B118)","v":0.37495626473777349},{"$f":"STDEV($B$10:B118)","v":4.1447821404511885E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40494744646426789,{"$f":"AVERAGE($B$10:B119)","v":0.37522891184437801},{"$f":"STDEV($B$10:B119)","v":4.1356234798794973E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35780274348316288,{"$f":"AVERAGE($B$10:B120)","v":0.37507191933661932},{"$f":"STDEV($B$10:B120)","v":4.1201036466418414E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.46611549319532664,{"$f":"AVERAGE($B$10:B121)","v":0.37588480838892918},{"$f":"STDEV($B$10:B121)","v":4.1907525681018451E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35790224570969653,{"$f":"AVERAGE($B$10:B122)","v":0.37572567066610407},{"$f":"STDEV($B$10:B122)","v":4.1754301481010794E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34892337133060991,{"$f":"AVERAGE($B$10:B123)","v":0.37549056277719622},{"$f":"STDEV($B$10:B123)","v":4.164486299211026E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39456506659734436,{"$f":"AVERAGE($B$10:B124)","v":0.37565642802780619},{"$f":"STDEV($B$10:B124)","v":4.1499943377577959E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33739119822104569,{"$f":"AVERAGE($B$10:B125)","v":0.37532655535705828},{"$f":"STDEV($B$10:B125)","v":4.1471579519055571E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35602882993405882,{"$f":"AVERAGE($B$10:B126)","v":0.37516161753293009},{"$f":"STDEV($B$10:B126)","v":4.1330959077543826E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41623337872424587,{"$f":"AVERAGE($B$10:B127)","v":0.37550968330573786},{"$f":"STDEV($B$10:B127)","v":4.132727236086596E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36630092420047256,{"$f":"AVERAGE($B$10:B128)","v":0.37543229877544154},{"$f":"STDEV($B$10:B128)","v":4.116044168046943E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38788670335481001,{"$f":"AVERAGE($B$10:B129)","v":0.37553608548026957},{"$f":"STDEV($B$10:B129)","v":4.1002899138421478E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39901982765428828,{"$f":"AVERAGE($B$10:B130)","v":0.37573016599410441},{"$f":"STDEV($B$10:B130)","v":4.0887469474426896E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35880602676783807,{"$f":"AVERAGE($B$10:B131)","v":0.37559144354143009},{"$f":"STDEV($B$10:B131)","v":4.0746981628629469E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38877699483149236,{"$f":"AVERAGE($B$10:B132)","v":0.37569864314541435},{"$f":"STDEV($B$10:B132)","v":4.0597054646661773E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36392951342599461,{"$f":"AVERAGE($B$10:B133)","v":0.37560373080896742},{"$f":"STDEV($B$10:B133)","v":4.0445500678224458E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.4281910675274252,{"$f":"AVERAGE($B$10:B134)","v":0.37602442950271509},{"$f":"STDEV($B$10:B134)","v":4.0555760414608316E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34671642064946551,{"$f":"AVERAGE($B$10:B135)","v":0.37579182625784802},{"$f":"STDEV($B$10:B135)","v":4.0477508361367223E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32333483137994007,{"$f":"AVERAGE($B$10:B136)","v":0.37537877905408495},{"$f":"STDEV($B$10:B136)","v":4.0584387342296184E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34562855087802363,{"$f":"AVERAGE($B$10:B137)","v":0.37514635539645946},{"$f":"STDEV($B$10:B137)","v":4.0509726246245957E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.43116503532255579,{"$f":"AVERAGE($B$10:B138)","v":0.37558060872921989},{"$f":"STDEV($B$10:B138)","v":4.0651489643631467E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3238583361891883,{"$f":"AVERAGE($B$10:B139)","v":0.37518274509429661},{"$f":"STDEV($B$10:B139)","v":4.0746921429995364E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40121128940362927,{"$f":"AVERAGE($B$10:B140)","v":0.37538143627223042},{"$f":"STDEV($B$10:B140)","v":4.0653556061091806E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33290579239297274,{"$f":"AVERAGE($B$10:B141)","v":0.37505965109132694},{"$f":"STDEV($B$10:B141)","v":4.0666491536918203E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38506175786567098,{"$f":"AVERAGE($B$10:B142)","v":0.37513485490166038},{"$f":"STDEV($B$10:B142)","v":4.0521441470441157E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34698385318182418,{"$f":"AVERAGE($B$10:B143)","v":0.3749247727992735},{"$f":"STDEV($B$10:B143)","v":4.0442001334074197E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33305659274509547,{"$f":"AVERAGE($B$10:B144)","v":0.37461463813220552},{"$f":"STDEV($B$10:B144)","v":4.0451632947720119E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36041321578345253,{"$f":"AVERAGE($B$10:B145)","v":0.37451021590905292},{"$f":"STDEV($B$10:B145)","v":4.0319927518949708E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38862028705826274,{"$f":"AVERAGE($B$10:B146)","v":0.37461320912912016},{"$f":"STDEV($B$10:B146)","v":4.018950292869683E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36469795883176476,{"$f":"AVERAGE($B$10:B147)","v":0.37454135948928419},{"$f":"STDEV($B$10:B147)","v":4.0051451907895559E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.27655390182122647,{"$f":"AVERAGE($B$10:B148)","v":0.37383641375066506},{"$f":"STDEV($B$10:B148)","v":4.0762367342646912E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36938573415247661,{"$f":"AVERAGE($B$10:B149)","v":0.37380462318210655},{"$f":"STDEV($B$10:B149)","v":4.0617217232967427E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36538550108913348,{"$f":"AVERAGE($B$10:B150)","v":0.37374491309634084},{"$f":"STDEV($B$10:B150)","v":4.0478105861561683E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35499955322536858,{"$f":"AVERAGE($B$10:B151)","v":0.37361290351978466},{"$f":"STDEV($B$10:B151)","v":4.0364975121006598E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32609789915089643,{"$f":"AVERAGE($B$10:B152)","v":0.37328063076196027},{"$f":"STDEV($B$10:B152)","v":4.0418374467098117E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34832542025805679,{"$f":"AVERAGE($B$10:B153)","v":0.37310733068901647},{"$f":"STDEV($B$10:B153)","v":4.0330455532911362E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35851573825182403,{"$f":"AVERAGE($B$10:B154)","v":0.37300669901703587},{"$f":"STDEV($B$10:B154)","v":4.0208438964704364E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34616510802630174,{"$f":"AVERAGE($B$10:B155)","v":0.37282285250340069},{"$f":"STDEV($B$10:B155)","v":4.013107914948931E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36997241631183331,{"$f":"AVERAGE($B$10:B156)","v":0.37280346178100904},{"$f":"STDEV($B$10:B156)","v":3.9994098811389565E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35634270436346055,{"$f":"AVERAGE($B$10:B157)","v":0.37269224044710669},{"$f":"STDEV($B$10:B157)","v":3.9880792177250081E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35770348734185431,{"$f":"AVERAGE($B$10:B158)","v":0.37259164478868217},{"$f":"STDEV($B$10:B158)","v":3.9764794957422279E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37295342823763283,{"$f":"AVERAGE($B$10:B159)","v":0.37259405667834189},{"$f":"STDEV($B$10:B159)","v":3.9631142411694041E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41769421285100583,{"$f":"AVERAGE($B$10:B160)","v":0.37289273320928668},{"$f":"STDEV($B$10:B160)","v":3.9668967183274235E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35451792029027251,{"$f":"AVERAGE($B$10:B161)","v":0.37277184628218785},{"$f":"STDEV($B$10:B161)","v":3.9565475625585184E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34199807907486263,{"$f":"AVERAGE($B$10:B162)","v":0.37257071054880664},{"$f":"STDEV($B$10:B162)","v":3.951351293904589E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35128772390747465,{"$f":"AVERAGE($B$10:B163)","v":0.37243250933684996},{"$f":"STDEV($B$10:B163)","v":3.9421496019952061E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41882201870981656,{"$f":"AVERAGE($B$10:B164)","v":0.37273179649409488},{"$f":"STDEV($B$10:B164)","v":3.9469568921314362E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.31885137230667415,{"$f":"AVERAGE($B$10:B165)","v":0.37238640915956017},{"$f":"STDEV($B$10:B165)","v":3.9577845595167679E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34783744798828242,{"$f":"AVERAGE($B$10:B166)","v":0.37223004634955204},{"$f":"STDEV($B$10:B166)","v":3.9499409404303756E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34742050434818933,{"$f":"AVERAGE($B$10:B167)","v":0.37207302393182184},{"$f":"STDEV($B$10:B167)","v":3.9422853735415854E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3634391282431193,{"$f":"AVERAGE($B$10:B168)","v":0.37201872270107533},{"$f":"STDEV($B$10:B168)","v":3.9303864482646868E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37832007102237131,{"$f":"AVERAGE($B$10:B169)","v":0.37205810612808343},{"$f":"STDEV($B$10:B169)","v":3.9183239374970313E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41843766571948104,{"$f":"AVERAGE($B$10:B170)","v":0.37234617792678776},{"$f":"STDEV($B$10:B170)","v":3.9231251598965719E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38348299297370958,{"$f":"AVERAGE($B$10:B171)","v":0.37241492369868234},{"$f":"STDEV($B$10:B171)","v":3.9119012499115535E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39706759444873901,{"$f":"AVERAGE($B$10:B172)","v":0.37256616707751705},{"$f":"STDEV($B$10:B172)","v":3.9045862949770416E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.30306357019092212,{"$f":"AVERAGE($B$10:B173)","v":0.37214237075503781},{"$f":"STDEV($B$10:B173)","v":3.9302431356342545E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34127505767613853,{"$f":"AVERAGE($B$10:B174)","v":0.37195529613031719},{"$f":"STDEV($B$10:B174)","v":3.9256041755010608E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40760412811676028,{"$f":"AVERAGE($B$10:B175)","v":0.37217004813023552},{"$f":"STDEV($B$10:B175)","v":3.9234587485772986E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32163412689314486,{"$f":"AVERAGE($B$10:B176)","v":0.37186743782342663},{"$f":"STDEV($B$10:B176)","v":3.9311224044008913E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35470597237026658,{"$f":"AVERAGE($B$10:B177)","v":0.37176528624334831},{"$f":"STDEV($B$10:B177)","v":3.9215707058382031E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35710146824420841,{"$f":"AVERAGE($B$10:B178)","v":0.37167851808950725},{"$f":"STDEV($B$10:B178)","v":3.9115087043353328E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38967201198553914,{"$f":"AVERAGE($B$10:B179)","v":0.37178436217124861},{"$f":"STDEV($B$10:B179)","v":3.902359983110186E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38829420674437193,{"$f":"AVERAGE($B$10:B180)","v":0.37188091096992182},{"$f":"STDEV($B$10:B180)","v":3.8929133809786756E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37751405938329813,{"$f":"AVERAGE($B$10:B181)","v":0.37191366183279029},{"$f":"STDEV($B$10:B181)","v":3.8817515484246508E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.43698185075949225,{"$f":"AVERAGE($B$10:B182)","v":0.37228977853178857},{"$f":"STDEV($B$10:B182)","v":3.9019383369559742E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.36781053837977112,{"$f":"AVERAGE($B$10:B183)","v":0.37226403577229422},{"$f":"STDEV($B$10:B183)","v":3.8907928980269742E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41872261043450637,{"$f":"AVERAGE($B$10:B184)","v":0.37252951334179257},{"$f":"STDEV($B$10:B184)","v":3.8954595264281903E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35852676916885967,{"$f":"AVERAGE($B$10:B185)","v":0.37244995229535544},{"$f":"STDEV($B$10:B185)","v":3.8857474987070408E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38250283913721089,{"$f":"AVERAGE($B$10:B186)","v":0.37250674826621344},{"$f":"STDEV($B$10:B186)","v":3.8754294335747834E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.43273699830442586,{"$f":"AVERAGE($B$10:B187)","v":0.37284512045743928},{"$f":"STDEV($B$10:B187)","v":3.8907457984274606E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40640412348292626,{"$f":"AVERAGE($B$10:B188)","v":0.37303260092126889},{"$f":"STDEV($B$10:B188)","v":3.8879011104160907E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35573373689045146,{"$f":"AVERAGE($B$10:B189)","v":0.37293649612109769},{"$f":"STDEV($B$10:B189)","v":3.8791692941201002E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.37116637092931076,{"$f":"AVERAGE($B$10:B190)","v":0.37292671642390551},{"$f":"STDEV($B$10:B190)","v":3.8684011915250033E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38205350361264867,{"$f":"AVERAGE($B$10:B191)","v":0.37297686360626126},{"$f":"STDEV($B$10:B191)","v":3.8582933605615669E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33972776499686702,{"$f":"AVERAGE($B$10:B192)","v":0.37279517454282196},{"$f":"STDEV($B$10:B192)","v":3.8555212453659865E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.32237318311900204,{"$f":"AVERAGE($B$10:B193)","v":0.37252114198073594},{"$f":"STDEV($B$10:B193)","v":3.8628987819236273E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.31419738633142114,{"$f":"AVERAGE($B$10:B194)","v":0.37220587843668557},{"$f":"STDEV($B$10:B194)","v":3.8761788894527492E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.35427845962654836,{"$f":"AVERAGE($B$10:B195)","v":0.37210949446458802},{"$f":"STDEV($B$10:B195)","v":3.8679228285244636E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.47148721499643587,{"$f":"AVERAGE($B$10:B196)","v":0.37264092612518612},{"$f":"STDEV($B$10:B196)","v":3.9253684061632627E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.41982111010146123,{"$f":"AVERAGE($B$10:B197)","v":0.37289188455059186},{"$f":"STDEV($B$10:B197)","v":3.9299518169590833E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.42326636438772214,{"$f":"AVERAGE($B$10:B198)","v":0.37315841618994178},{"$f":"STDEV($B$10:B198)","v":3.93657636806252E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40072010989305484,{"$f":"AVERAGE($B$10:B199)","v":0.37330347773574768},{"$f":"STDEV($B$10:B199)","v":3.9312367202541498E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.39572755947768795,{"$f":"AVERAGE($B$10:B200)","v":0.37342088130507722},{"$f":"STDEV($B$10:B200)","v":3.9242335183378413E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.42642601485475107,{"$f":"AVERAGE($B$10:B201)","v":0.37369694970898176},{"$f":"STDEV($B$10:B201)","v":3.9325962046757701E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.40730284680400969,{"$f":"AVERAGE($B$10:B202)","v":0.37387107352812704},{"$f":"STDEV($B$10:B202)","v":3.9297939228126647E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33759349331829208,{"$f":"AVERAGE($B$10:B203)","v":0.37368407569199386},{"$f":"STDEV($B$10:B203)","v":3.9282440822232111E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.28863439224192072,{"$f":"AVERAGE($B$10:B204)","v":0.37324792346917296},{"$f":"STDEV($B$10:B204)","v":3.9651615217698069E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.34274740449972474,{"$f":"AVERAGE($B$10:B205)","v":0.37309230857647169},{"$f":"STDEV($B$10:B205)","v":3.9609772794399215E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.33525865443555358,{"$f":"AVERAGE($B$10:B206)","v":0.37290025957068018},{"$f":"STDEV($B$10:B206)","v":3.9600445081673478E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.3466655424194508,{"$f":"AVERAGE($B$10:B207)","v":0.37276776099920927},{"$f":"STDEV($B$10:B207)","v":3.9543784988656086E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.38834965917499387,{"$f":"AVERAGE($B$10:B208)","v":0.37284606199506748},{"$f":"STDEV($B$10:B208)","v":3.9459263543785192E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,0.29584965965891002,{"$f":"AVERAGE($B$10:B209)","v":0.37246107998338673},{"$f":"STDEV($B$10:B209)","v":3.9734763374658984E-2},null,null,null,null,null,null,null,null,null,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0]

{"sheet":"ID-numbers","index":27,"n_rows":2175,"n_cols":5,"rows_kept":2175,"cut":false,"hidden":true,"merged":[[28,0,28,1],[9,0,9,1]]}
["ID-number","Description","Unit",null,"Remarks"]
["Data Source"]
["DS001","CO2-tool solid-biogas Agentschap NL"]
["DS002","CO2-tool biofuels-bioliquids SenterNovem"]
["DS003","Biofuel Cities"]
["DS004","EUCAR-CONCAWE-JRC"]
["DS005","STORG"]
["DS006","Own calculations"]
[" "]
["Lyfe cycle process descriptions"]
["LC001","FT_Process description transport 1 (mode 1-2-3)"]
["LC002","FT_Process description treatment 1"]
["LC003","BC_Process description conversion process 1"]
["LC004","FT_Process description transport 2 (mode 4-5-6)"]
["LC005","FT_Process description treatment 2"]
["LC006","BC_Process description conversion process 2"]
["LC007","FT_Process description transport 3 (mode 7-8-9)"]
["LC008","FT_Process description treatment 3"]
["LC501","FT_Process description transport 1 (mode 1-2-3)"]
["LC502","FT_Process description treatment 1"]
["LC503","BC_Process description conversion process 1"]
["LC504","FT_Process description transport 2 (mode 4-5-6)"]
["LC505","FT_Process description treatment 2"]
["LC506","BC_Process description conversion process 2"]
["LC507","FT_Process description transport 3 (mode 7-8-9)"]
["LC508","FT_Process description treatment 3"]
["LC010","FC_Process description final conversion"]
["LC009","BC_Process description composting"]
["Feedstock Production 1"]
["FP001","Feedstock type 1",{"$f":"VLOOKUP(A30,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP002","Origin of the feedstock",{"$f":"VLOOKUP(A31,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP003a","Yield rate (moist/wet) of feedstock 1 per ha",{"$f":"VLOOKUP(A32,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP003b","Yield rate (dry) of feedstock 1 per ha",{"$f":"VLOOKUP(A33,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgdm/ha"}]
["FP003c","Yield rate (energy) of feedstock 1 per ha",{"$f":"VLOOKUP(A34,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP005","Number of harvests per year",{"$f":"VLOOKUP(A35,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"1/yr"}]
["FP006","Rotation system",{"$f":"VLOOKUP(A36,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP009","Moisture content of the harvested crop",{"$f":"VLOOKUP(A37,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP010","Energy content of the dry energy crop (LHV)",{"$f":"VLOOKUP(A38,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgdm"}]
["FP016a","Type of by-product 1",{"$f":"VLOOKUP(A39,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP016b","Type of by-product 2",{"$f":"VLOOKUP(A40,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP017a","Yield rate (moist/wet) of by-product 1 per ha",{"$f":"VLOOKUP(A41,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP017b","Yield rate (moist/wet) of by-product 2 per ha",{"$f":"VLOOKUP(A42,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP018a","Yield rate (energy) of by-product 1 per ha",{"$f":"VLOOKUP(A43,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP018b","Yield rate (energy) of by-product 2 per ha",{"$f":"VLOOKUP(A44,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP019a","Moisture content of by-product 1",{"$f":"VLOOKUP(A45,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP019b","Moisture content of by-product 2",{"$f":"VLOOKUP(A46,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP020a","Energy content of the dry by-product 1 (LHV)",{"$f":"VLOOKUP(A47,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgdm"}]
["FP020b","Energy content of the dry by-product 2 (LHV)",{"$f":"VLOOKUP(A48,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgdm"}]
["FP021a","Valorisation of by-product 1",{"$f":"VLOOKUP(A49,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP021b","Valorisation of by-product 2",{"$f":"VLOOKUP(A50,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP022","Use of seeds",{"$f":"VLOOKUP(A51,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP023a","Use of N fertiliser (synthetic)",{"$f":"VLOOKUP(A52,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP023b","Use of P2O5 fertiliser",{"$f":"VLOOKUP(A53,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP023c","Use of K2O fertiliser",{"$f":"VLOOKUP(A54,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP023d","Use of CaO fertiliser",{"$f":"VLOOKUP(A55,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP023e","Use of pesticides",{"$f":"VLOOKUP(A56,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP024a","Totally allocated fossil energy requirement for feedstock production",{"$f":"VLOOKUP(A57,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FP024b","Totally allocated primary energy requirement for feedstock production",{"$f":"VLOOKUP(A58,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FP025a","Totally allocated fossil energy requirement for feedstock production",{"$f":"VLOOKUP(A59,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJfossil/MJFU"}]
["FP025b","Totally allocated primary energy requirement for feedstock production",{"$f":"VLOOKUP(A60,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJprim/MJFU"}]
["FP028a","Fossil energy used for feedstock production",{"$f":"VLOOKUP(A61,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgdm"}]
["FP028b","Fossil energy used for feedstock production",{"$f":"VLOOKUP(A62,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP029a","Primary energy used for feedstock production",{"$f":"VLOOKUP(A63,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgdm"}]
["FP029b","Primary energy used for feedstock production",{"$f":"VLOOKUP(A64,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP030","Allocation to energy crop",{"$f":"VLOOKUP(A65,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP031","Allocation to by-products",{"$f":"VLOOKUP(A66,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP031a","Allocation to by-product 1",{"$f":"VLOOKUP(A67,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP031b","Allocation to by-product 2",{"$f":"VLOOKUP(A68,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP032a","Allocated fossil energy requirement for feedstock production",{"$f":"VLOOKUP(A69,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FP032b","Allocated primary energy requirement for feedstock production",{"$f":"VLOOKUP(A70,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FP034","Type of fuel used for agricultural machinery",{"$f":"VLOOKUP(A71,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP035a","Fossil energy use related to agrifuel use",{"$f":"VLOOKUP(A72,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP035b","Primary energy use related to agrifuel use",{"$f":"VLOOKUP(A73,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP036","Fossil energy coefficient of fuel used in agricultural machinery",{"$f":"VLOOKUP(A74,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgfuel"}]
["FP037","Amount of fuel used in agricultural machinery",{"$f":"VLOOKUP(A75,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP038a","Fossil energy used for heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A76,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJfossil/kgfm"}]
["FP038b","Primary energy used for heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A77,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJprim/kgfm"}]
["FP039a","Fossil energy used for heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A78,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FP039b","Primary energy used for heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A79,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FP040","Heat energy use for drying and storage of the crop",{"$f":"VLOOKUP(A80,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJheat/kgfm"}]
["FP041","Heat source",{"$f":"VLOOKUP(A81,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP042a","Fossil energy coefficient of heat production for crop drying and storage",{"$f":"VLOOKUP(A82,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/MJheat"}]
["FP042b","Primary energy coefficient of heat production for crop drying and storage",{"$f":"VLOOKUP(A83,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/MJheat"}]
["FP042c","GHG coefficient of heat production for crop drying and storage",{"$f":"VLOOKUP(A84,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/MJheat"}]
["FP042d","NOx emissions factor of heat production for crop drying and storage",{"$f":"VLOOKUP(A85,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gNOX/MJheat"}]
["FP042e","SOx emissions factor of heat production for crop drying and storage",{"$f":"VLOOKUP(A86,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSOX/MJheat"}]
["FP043","Electricity energy use for drying and storage of the crop",{"$f":"VLOOKUP(A87,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJe/kgfm"}]
["FP044","Electricity source",{"$f":"VLOOKUP(A88,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP045a","Fossil energy coefficient of electricity for crop drying and storage",{"$f":"VLOOKUP(A89,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/MJe"}]
["FP045b","Primary energy coefficient of electricity for crop drying and storage",{"$f":"VLOOKUP(A90,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/MJe"}]
["FP045c","GHG coefficient of electricity for crop drying and storage",{"$f":"VLOOKUP(A91,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/MJe"}]
["FP045d","NOx emissions factor of electricity for crop drying and storage",{"$f":"VLOOKUP(A92,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gNOX/MJe"}]
["FP045e","SOx emissions factor of electricity for crop drying and storage",{"$f":"VLOOKUP(A93,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSOX/MJe"}]
["FP046a","Fossil energy use of seeds, fertilisers and pesticides",{"$f":"VLOOKUP(A94,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP046b","Primary energy use of seeds, fertilisers and pesticides",{"$f":"VLOOKUP(A95,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP047","Pretreated feedstock",{"$f":"VLOOKUP(A96,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP048","Moisture content pretreated feedstock",{"$f":"VLOOKUP(A97,'Conversion feedstock1'!D$10:E$683,2,FALSE)","v":"%"}]
["FP049","Energy content pretreated feedstock (LHV)",{"$f":"VLOOKUP(A98,'Conversion feedstock1'!D$10:E$683,2,FALSE)","v":"MJ/kgdm"}]
["FP050a","Fossil energy coefficient of N fertiliser",{"$f":"VLOOKUP(A99,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgfertiliser"}]
["FP050b","Fossil energy coefficient of P fertiliser",{"$f":"VLOOKUP(A100,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgfertiliser"}]
["FP050c","Fossil energy coefficient of K fertiliser",{"$f":"VLOOKUP(A101,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgfertiliser"}]
["FP050d","Fossil energy coefficient of Ca fertiliser",{"$f":"VLOOKUP(A102,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgfertiliser"}]
["FP050e","Fossil energy coefficient of pesticides",{"$f":"VLOOKUP(A103,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgpesticides"}]
["FP050f","Fossil energy coefficient of seeds",{"$f":"VLOOKUP(A104,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/kgseeds"}]
["FP051","Yield rate (moist/wet) of pretreated feedstock 1 per ha",{"$f":"VLOOKUP(A105,'Production feedstock1'!D$10:E$631,2,FALSE)","v":{"$error":"#N/A"}}]
["FP052","Yield rate (dry) of pretreated feedstock 1 per ha",{"$f":"VLOOKUP(A106,'Production feedstock1'!D$10:E$631,2,FALSE)","v":{"$error":"#N/A"}}]
["FP053","Yield rate (energy) of pretreated feedstock 1 per ha",{"$f":"VLOOKUP(A107,'Production feedstock1'!D$10:E$631,2,FALSE)","v":{"$error":"#N/A"}}]
["FP054","Yield loss through treatment and transport of feedstock 1",{"$f":"VLOOKUP(A108,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP055a","Yield rate (moist/wet) of pretreated feedstock 1 before conversion",{"$f":"VLOOKUP(A109,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP055b","Yield rate (dry) of pretreated feedstock 1 before conversion",{"$f":"VLOOKUP(A110,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgdm/ha"}]
["FP055c","Yield rate (energy) of pretreated feedstock 1 before conversion",{"$f":"VLOOKUP(A111,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"MJ/ha"}]
["FP056a","GHG emissions associated with inputs for feedstock production",{"$f":"VLOOKUP(A112,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/kgdm"}]
["FP056b","GHG emissions associated with inputs for feedstock production",{"$f":"VLOOKUP(A113,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha"}]
["FP057","Allocated GHG emissions from feedstock production",{"$f":"VLOOKUP(A114,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FP058","GHG emissions associated with fuel used in agricultural machinery",{"$f":"VLOOKUP(A115,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha"}]
["FP059","Specific GHG emissions of the fuel used in agricultural machinery",{"$f":"VLOOKUP(A116,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/kgfuel"}]
["FP061a","Totally allocated GHG emissions from feedstock production",{"$f":"VLOOKUP(A117,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FP061b","Totally allocated GHG emissions from feedstock production",{"$f":"VLOOKUP(A118,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FP062a","GHG emissions associated with heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A119,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/kgfm"}]
["FP062b","GHG emissions associated with heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A120,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FP064","GHG emissions associated with production of seeds, fertilisers and pesticides",{"$f":"VLOOKUP(A121,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha"}]
["FP067a","N: specific GHG emissions",{"$f":"VLOOKUP(A122,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/kgfertiliser"}]
["FP067b","P2O5: specific GHG emissions",{"$f":"VLOOKUP(A123,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/kgfertiliser"}]
["FP067c","K2O: specific GHG emissions",{"$f":"VLOOKUP(A124,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/kgfertiliser"}]
["FP067d","CaO: specific GHG emissions",{"$f":"VLOOKUP(A125,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/kgfertiliser"}]
["FP067e","Pesticides: specific GHG emissions",{"$f":"VLOOKUP(A126,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/kgpesticides"}]
["FP067f","Seeds: specific GHG emissions",{"$f":"VLOOKUP(A127,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/kgseeds"}]
["FP068a","GHG emissions associated with land use change (carbon stock changes) per MJ",{"$f":"VLOOKUP(A128,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/MJendfuel_fs1 (over 20yr)"}]
["FP068b","GHG emissions associated with land use change (carbon stock changes) per ha",{"$f":"VLOOKUP(A129,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha (over 20yr)"}]
["FP069a","Actual land use",{"$f":"VLOOKUP(A130,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP069b","Previous land use (January 1st, 2008)",{"$f":"VLOOKUP(A131,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP069c","Actual land use_specific for carbon stock veg",{"$f":"VLOOKUP(A132,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP069d","Previous land use (January 1st, 2008)_specific for carbon stock veg",{"$f":"VLOOKUP(A133,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP070a","Climate region",{"$f":"VLOOKUP(A134,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP070b","Soil type",{"$f":"VLOOKUP(A135,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP070c","Climate region_specific for carbon stock_actual land use",{"$f":"VLOOKUP(A136,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP070d","Climate region_specific for carbon stock_previous land use",{"$f":"VLOOKUP(A137,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP071","Carbon stock actual land use",{"$f":"VLOOKUP(A138,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP072","Carbon stock previous land use",{"$f":"VLOOKUP(A139,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP073a","Soil organic carbon actual land use",{"$f":"VLOOKUP(A140,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP073b","Soil organic carbon previous land use",{"$f":"VLOOKUP(A141,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP074","Standard soil organic carbon_feedstock 1",{"$f":"VLOOKUP(A142,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP075a","Land use factor actual land use",{"$f":"VLOOKUP(A143,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP075b","Land use factor previous land use",{"$f":"VLOOKUP(A144,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP076a","Management factor actual land use",{"$f":"VLOOKUP(A145,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP076b","Management factor previous land use",{"$f":"VLOOKUP(A146,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP077a","Input factor actual land use",{"$f":"VLOOKUP(A147,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP077b","Input factor previous land use",{"$f":"VLOOKUP(A148,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP078a","Above and below vegetation carbon stock actual land use",{"$f":"VLOOKUP(A149,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP078b","Above and below vegetation carbon stock previous land use",{"$f":"VLOOKUP(A150,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP079a","Above and below vegetation carbon stock in living biomass actual land use",{"$f":"VLOOKUP(A151,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP079b","Above and below vegetation carbon stock in living biomass previous land use",{"$f":"VLOOKUP(A152,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP080a","Above ground vegetation carbon stock in living biomass actual land use",{"$f":"VLOOKUP(A153,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP080b","Above ground vegetation carbon stock in living biomass previous land use",{"$f":"VLOOKUP(A154,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP081a","Weight of above ground living biomass actual land use",{"$f":"VLOOKUP(A155,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP081b","Weight of above ground living biomass previous land use",{"$f":"VLOOKUP(A156,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP082aa","Carbon fraction of dry matter in living biomass actual land use",{"$f":"VLOOKUP(A157,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP082ab","Carbon fraction of dry matter in living biomass previous land use",{"$f":"VLOOKUP(A158,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP082ba","Carbon fraction of dry matter in dead wood actual land use",{"$f":"VLOOKUP(A159,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP082bb","Carbon fraction of dry matter in dead wood previous land use",{"$f":"VLOOKUP(A160,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP082ca","Carbon fraction of dry matter in litter actual land use",{"$f":"VLOOKUP(A161,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP082cb","Carbon fraction of dry matter in litter previous land use",{"$f":"VLOOKUP(A162,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP083a","Ratio of below ground carbon stock to above ground carbon stock in living biomass actual land use",{"$f":"VLOOKUP(A163,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP083b","Ratio of below ground carbon stock to above ground carbon stock in living biomass previous land use",{"$f":"VLOOKUP(A164,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP084a","Below ground vegetation carbon stock in living biomass actual land use",{"$f":"VLOOKUP(A165,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP084b","Below ground vegetation carbon stock in living biomass previous land use",{"$f":"VLOOKUP(A166,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP085a","Weight of below ground living biomass actual land use",{"$f":"VLOOKUP(A167,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP085b","Weight of below ground living biomass previous land use",{"$f":"VLOOKUP(A168,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP086a","Above and below vegetation carbon stock in dead organic matter actual land use",{"$f":"VLOOKUP(A169,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP086b","Above and below vegetation carbon stock in dead organic matter previous land use",{"$f":"VLOOKUP(A170,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP087a","Carbon stock in dead wood pool actual land use",{"$f":"VLOOKUP(A171,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP087b","Carbon stock in dead wood pool previous land use",{"$f":"VLOOKUP(A172,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP088a","Weight of dead wood pool actual land use",{"$f":"VLOOKUP(A173,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP088b","Weight of dead wood pool previous land use",{"$f":"VLOOKUP(A174,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP089a","Carbon stock in litter actual land use",{"$f":"VLOOKUP(A175,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP089b","Carbon stock in litter previous land use",{"$f":"VLOOKUP(A176,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP090a","Weight of litter actual land use",{"$f":"VLOOKUP(A177,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP090b","Weight of litter previous land use",{"$f":"VLOOKUP(A178,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP091a","Peatland",{"$f":"VLOOKUP(A179,'Production feedstock1'!D$10:E$631,2,FALSE)","v":{"$error":"#N/A"}}]
["FP091b","Emission factor soil organic carbon_peatland",{"$f":"VLOOKUP(A180,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP092a","Previously degraded land",{"$f":"VLOOKUP(A181,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP092b","Bonus restored degraded land",{"$f":"VLOOKUP(A182,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/MJ (per year)"}]
["FP093a","Land management actual land use",{"$f":"VLOOKUP(A183,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP093b","Land management previous land use",{"$f":"VLOOKUP(A184,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP094a","Input actual land use",{"$f":"VLOOKUP(A185,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP094b","Input previous land use",{"$f":"VLOOKUP(A186,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP095a","Domain actual land use",{"$f":"VLOOKUP(A187,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP095b","Domain previous land use",{"$f":"VLOOKUP(A188,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP096a","Ecological zone actual land use",{"$f":"VLOOKUP(A189,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP096b","Ecological zone previous land use",{"$f":"VLOOKUP(A190,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP097a","Continent actual land use",{"$f":"VLOOKUP(A191,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP097b","Continent previous land use",{"$f":"VLOOKUP(A192,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP098a","Type actual land use",{"$f":"VLOOKUP(A193,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP098b","Type previous land use",{"$f":"VLOOKUP(A194,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP099","GHG emissions associated with indirect land use change (soil carbon release)",{"$f":"VLOOKUP(A195,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha (spread over 20yr)"}]
["FP100","Water use for feedstock production",{"$f":"VLOOKUP(A196,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"m³/ha"}]
["FP101","Allocated water use for feedstock production",{"$f":"VLOOKUP(A197,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["FP102a","Totally allocated water use for feedstock production",{"$f":"VLOOKUP(A198,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["FP102b","Totally allocated water use for feedstock production",{"$f":"VLOOKUP(A199,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"m³/GJFU"}]
["FP103a","Water use for feedstock treatment 1 (drying and storage)",{"$f":"VLOOKUP(A200,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"m³/kgfm"}]
["FP103b","Water use for feedstock treatment 1 (drying and storage)",{"$f":"VLOOKUP(A201,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["FP104a","Country freshwater availability",{"$f":"VLOOKUP(A202,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"m³/capita.yr"}]
["FP104b","Country freshwater level",{"$f":"VLOOKUP(A203,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP105","Allocated land use for feedstock production",{"$f":"VLOOKUP(A204,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"ha/GJendfuel_fs1"}]
["FP106a","Totally allocated land use for feedstock production",{"$f":"VLOOKUP(A205,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"ha/GJendfuel_fs1"}]
["FP106b","Totally allocated land use for feedstock production",{"$f":"VLOOKUP(A206,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"ha/GJFU"}]
["FP107a","Carbon debt due to land use change",{"$f":"VLOOKUP(A207,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha"}]
["FP107b","Allocated carbon debt",{"$f":"VLOOKUP(A208,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha"}]
["FP107c","Totally allocated carbon debt",{"$f":"VLOOKUP(A209,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha"}]
["FP108","Allocated GHG emissions from feedstock production without LUC emissions",{"$f":"VLOOKUP(A210,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FP109","Input of N-fixing crop residue to the soil",{"$f":"VLOOKUP(A211,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kg/ha"}]
["FP110a","Acidification potential of NH3",{"$f":"VLOOKUP(A212,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2_eq/gNH3"}]
["FP110b","Acidification potential of NOx",{"$f":"VLOOKUP(A213,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2_eq/gNOx"}]
["FP110c","Acidification potential of SOx",{"$f":"VLOOKUP(A214,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2_eq/gSOx"}]
["FP111a","Agrifuel NOx emissions factor",{"$f":"VLOOKUP(A215,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gNOX/kgfuel"}]
["FP111b","Agrifuel SOx emissions factor",{"$f":"VLOOKUP(A216,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSOX/kgfuel"}]
["FP112","Acidification potential from feedstock production",{"$f":"VLOOKUP(A217,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2_eq/ha"}]
["FP113","NH3 volatilization from fertiliser use",{"$f":"VLOOKUP(A218,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gNH3/ha"}]
["FP114","Allocated acidification potential from feedstock production",{"$f":"VLOOKUP(A219,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FP115a","Totally allocated acidification potential from feedstock production",{"$f":"VLOOKUP(A220,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FP115b","Totally allocated acidification potential from feedstock production",{"$f":"VLOOKUP(A221,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FP116a","Acidification potential associated with heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A222,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2-eq/kgfm"}]
["FP116b","Acidification potential associated with heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A223,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FP120a","Eutrophication potential of N to air",{"$f":"VLOOKUP(A224,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gN"}]
["FP120b","Eutrophication potential of NOx to air",{"$f":"VLOOKUP(A225,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gNOx"}]
["FP120c","Eutrophication potential of NH3 to air",{"$f":"VLOOKUP(A226,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gNH3"}]
["FP120d","Eutrophication potential of N to water",{"$f":"VLOOKUP(A227,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gN"}]
["FP120e","Eutrophication potential of NO3- to water",{"$f":"VLOOKUP(A228,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gNO3"}]
["FP120f","Eutrophication potential of NH4+ to water",{"$f":"VLOOKUP(A229,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gNH4+"}]
["FP120g","Eutrophication potential of P to water",{"$f":"VLOOKUP(A230,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gP"}]
["FP120h","Eutrophication potential of PO43-",{"$f":"VLOOKUP(A231,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gPO4"}]
["FP120i","Eutrophication potential of COD",{"$f":"VLOOKUP(A232,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/gCOD"}]
["FP122","Eutrophication potential of feedstock production",{"$f":"VLOOKUP(A233,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/ha"}]
["FP123a","N volatilization from fertiliser use (including NOx and NH3)",{"$f":"VLOOKUP(A234,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gN/ha"}]
["FP123d","N leaching from fertiliser use (including NO3- and NH4+)",{"$f":"VLOOKUP(A235,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gN/ha"}]
["FP123g","P leaching from fertiliser use (total P to water)",{"$f":"VLOOKUP(A236,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gP/ha"}]
["FP124","Allocated eutrophication potential from feedstock production",{"$f":"VLOOKUP(A237,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FP125a","Totally allocated eutrophication potential from feedstock production",{"$f":"VLOOKUP(A238,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FP125b","Totally allocated eutrophication potential from feedstock production",{"$f":"VLOOKUP(A239,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/MJFU"}]
["FP126a","Eutrophication potential associated with heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A240,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4-eq/kgfm"}]
["FP126b","Eutrophication potential associated with heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A241,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FP130a","Total (direct + indirect) N2O emissions from managed soils",{"$f":"VLOOKUP(A242,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gN20/ha"}]
["FP130b","Total (direct + indirect) N2O emissions from managed soils",{"$f":"VLOOKUP(A243,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"gCO2-eq/ha"}]
["FP131","Soil water saturation (yes=1,no=0)",{"$f":"VLOOKUP(A244,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP132","Field renewal (annual crops = 1)",{"$f":"VLOOKUP(A245,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"years"}]
["FP133","Amount of crop residue returned to the field (only for palm)",{"$f":"VLOOKUP(A246,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgdm/kgfm"}]
["FP134","Organic soil (yes=1,no=0)",{"$f":"VLOOKUP(A247,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP135","Nutrient level (only for ORGANIC soils + temperate/boreal climate + forest (native and managed))",{"$f":"VLOOKUP(A248,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP137a","Emission factor for direct N2O emissions from N inputs",{"$f":"VLOOKUP(A249,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/kgN_input"}]
["FP137b","Emission factor for direct N2O emissions from drained/managed organic soils",{"$f":"VLOOKUP(A250,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/ha"}]
["FP137c","Emission factor for direct N2O emissions from urine and dung N deposited by grazing animals",{"$f":"VLOOKUP(A251,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/kgN_input"}]
["FP137d","Emission factor for indirect N2O emissions from atmospheric deposition of N",{"$f":"VLOOKUP(A252,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/kgN_volatilised"}]
["FP137e","Emission factor for indirect N2O emissions from leaching and runoff",{"$f":"VLOOKUP(A253,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/kgN_leached+runoff"}]
["FP138a","Direct N2O_N emissions from managed soils",{"$f":"VLOOKUP(A254,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/ha"}]
["FP138b","Direct N2O emissions from managed soils",{"$f":"VLOOKUP(A255,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20/ha"}]
["FP139","Direct N2O_N emissions from N inputs to managed mineral soils",{"$f":"VLOOKUP(A256,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/ha"}]
["FP140","Total amount of organic N fertiliser applied to soil (other than by grazing animals)",{"$f":"VLOOKUP(A257,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/ha"}]
["FP141a","Amount of animal manure N applied to soil (other than by grazing animals)",{"$f":"VLOOKUP(A258,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/ha"}]
["FP141b","Amount of total sewage N applied to soil",{"$f":"VLOOKUP(A259,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/ha"}]
["FP141c","Amount of total compost N applied to soil",{"$f":"VLOOKUP(A260,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/ha"}]
["FP141d","Amount of N of other organic amendments applied to soil (used as fertiliser)",{"$f":"VLOOKUP(A261,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/ha"}]
["FP142","Total amount of N in crop residues (including N-fixing crops and renewal) returned to soil",{"$f":"VLOOKUP(A262,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/ha"}]
["FP143a","Ratio of above-ground residues to harvested yield_calculated",{"$f":"VLOOKUP(A263,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgdm/kgdm"}]
["FP143b","Ratio of above-ground residues to harvested yield_final",{"$f":"VLOOKUP(A264,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgdm/kgdm"}]
["FP144","Above-ground residue (dry) (=AGDM(T))",{"$f":"VLOOKUP(A265,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"t/ha"}]
["FP145a","Slope to calculate above-ground residue",{"$f":"VLOOKUP(A266,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP145b","Intercept to calculate above-ground residue",{"$f":"VLOOKUP(A267,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP146a","Ratio of below-ground residues to harvested yield_calculated",{"$f":"VLOOKUP(A268,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgdm/kgdm"}]
["FP146b","Ratio of below-ground residues to harvested yield_final",{"$f":"VLOOKUP(A269,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgdm/kgdm"}]
["FP147","Ratio of below-ground residues to above-ground biomass",{"$f":"VLOOKUP(A270,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgdm/kgdm"}]
["FP148a","N content of above-ground residues",{"$f":"VLOOKUP(A271,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/kgdm"}]
["FP148b","N content of below-ground residues",{"$f":"VLOOKUP(A272,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/kgdm"}]
["FP149","Fraction of above-ground residues removed",{"$f":"VLOOKUP(A273,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"%"}]
["FP150","Total amount of N mineralised in mineral soil due to carbon loss through land use change",{"$f":"VLOOKUP(A274,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN/ha"}]
["FP151","Average annual loss of soil carbon",{"$f":"VLOOKUP(A275,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"tC/ha"}]
["FP152","C:N ratio of the soil organic matter",{"$f":"VLOOKUP(A276,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP153","Previous land use is cropland (yes=1,no=0)",{"$f":"VLOOKUP(A277,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP154","Direct N2O_N emissions from managed organic soils",{"$f":"VLOOKUP(A278,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/ha"}]
["FP155a","Indirect N2O_N emissions from managed soils",{"$f":"VLOOKUP(A279,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/ha"}]
["FP155b","Indirect N2O emissions from managed soils",{"$f":"VLOOKUP(A280,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20/ha"}]
["FP156","Indirect N2O_N emissions from atmospheric deposition of N volatilized from managed soils",{"$f":"VLOOKUP(A281,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/ha"}]
["FP157","Fraction of synthetic fertiliser N that volatilises as NH3 and NOx",{"$f":"VLOOKUP(A282,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN_volatilised/kgN_applied"}]
["FP158","Fraction of organic fertiliser N that volatilises as NH3 and NOx",{"$f":"VLOOKUP(A283,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN_volatilised/kgN_applied"}]
["FP159","Indirect N2O_N emissions from N leaching/runoff from managed soils",{"$f":"VLOOKUP(A284,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN20_N/ha"}]
["FP160","Fraction of all N added to managed soils that is lost through leaching and runoff",{"$f":"VLOOKUP(A285,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"kgN_leached/kgN_applied"}]
["FP161","Land status in or after January 2008 = undisturbed forest (yes=1,no=0)",{"$f":"VLOOKUP(A286,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP162","Land status in or after January 2008 = nature protection area",{"$f":"VLOOKUP(A287,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP163","Land status in or after January 2008 = highly biodiverse grassland",{"$f":"VLOOKUP(A288,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP164","Land status in January 2008 and not longer now = wetland",{"$f":"VLOOKUP(A289,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP165","Land status in January 2008 and not longer now = continuously forested area",{"$f":"VLOOKUP(A290,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP166","Land status in January 2008 and not longer now = peatland",{"$f":"VLOOKUP(A291,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP167","The requirements of the RED concerning biodiversity & high carbon stocks are met",{"$f":"VLOOKUP(A292,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"binary"}]
["FP170a","No forced labour",{"$f":"VLOOKUP(A293,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP170b","No child labour ",{"$f":"VLOOKUP(A294,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP170c","Good social practices regarding human rights",{"$f":"VLOOKUP(A295,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP170d","No discrimination",{"$f":"VLOOKUP(A296,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP170e","Land is used legitimately / land rights have been secured",{"$f":"VLOOKUP(A297,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP170f","Open and transparent communication with local communities and stakeholders",{"$f":"VLOOKUP(A298,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP170g","Food security",{"$f":"VLOOKUP(A299,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP171a","Fair legal contracts",{"$f":"VLOOKUP(A300,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP171b","Workers rights",{"$f":"VLOOKUP(A301,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP171c","Freedom to join labour organizations or organize themselves",{"$f":"VLOOKUP(A302,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP171d","Fair wages and compensation rules",{"$f":"VLOOKUP(A303,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP171e","Health, safety and hygiene policy",{"$f":"VLOOKUP(A304,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP171f","Risk assessment for safe and healthy working conditions",{"$f":"VLOOKUP(A305,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP171g","Health and safety training",{"$f":"VLOOKUP(A306,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP172","Human and property rights_score",{"$f":"VLOOKUP(A307,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
["FP173","Labour rights and conditions_score",{"$f":"VLOOKUP(A308,'Production feedstock1'!D$10:E$631,2,FALSE)","v":"-"}]
[]
["Feedstock Production 2"]
["FP501","Feedstock type 2",{"$f":"VLOOKUP(A311,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP502","Origin of the feedstock",{"$f":"VLOOKUP(A312,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP503a","Yield rate (moist/wet) of feedstock 2 per ha",{"$f":"VLOOKUP(A313,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP503b","Yield rate (dry) of feedstock 2 per ha",{"$f":"VLOOKUP(A314,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgdm/ha"}]
["FP503c","Yield rate (energy) of feedstock 2 per ha",{"$f":"VLOOKUP(A315,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP505","Number of harvests per year",{"$f":"VLOOKUP(A316,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"1/yr"}]
["FP506","Rotation system",{"$f":"VLOOKUP(A317,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP509","Moisture content of the harvested crop",{"$f":"VLOOKUP(A318,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP510","Energy content of the dry energy crop (LHV)",{"$f":"VLOOKUP(A319,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kgdm"}]
["FP516a","Type of by-product 1",{"$f":"VLOOKUP(A320,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP516b","Type of by-product 2",{"$f":"VLOOKUP(A321,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP517a","Yield rate (moist/wet) of by-product 1 per ha",{"$f":"VLOOKUP(A322,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP517b","Yield rate (moist/wet) of by-product 2 per ha",{"$f":"VLOOKUP(A323,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP518a","Yield rate (energy) of by-product 1 per ha",{"$f":"VLOOKUP(A324,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP518b","Yield rate (energy) of by-product 2 per ha",{"$f":"VLOOKUP(A325,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP519a","Moisture content of by-product 1",{"$f":"VLOOKUP(A326,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP519b","Moisture content of by-product 2",{"$f":"VLOOKUP(A327,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP520a","Energy content of the dry by-product 1 (LHV)",{"$f":"VLOOKUP(A328,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kgdm"}]
["FP520b","Energy content of the dry by-product 2 (LHV)",{"$f":"VLOOKUP(A329,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kgdm"}]
["FP521a","Valorisation of by-product 1",{"$f":"VLOOKUP(A330,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP521b","Valorisation of by-product 2",{"$f":"VLOOKUP(A331,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP522","Use of seeds",{"$f":"VLOOKUP(A332,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP523a","Use of N-fertiliser (synthetic)",{"$f":"VLOOKUP(A333,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP523b","Use of P2O5-fertiliser",{"$f":"VLOOKUP(A334,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP523c","Use of K2O-fertiliser",{"$f":"VLOOKUP(A335,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP523d","Use of CaO-fertiliser",{"$f":"VLOOKUP(A336,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP523e","Use of pesticides",{"$f":"VLOOKUP(A337,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP524a","Totally allocated fossil energy requirement for feedstock production",{"$f":"VLOOKUP(A338,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["FP524b","Totally allocated primary energy requirement for feedstock production",{"$f":"VLOOKUP(A339,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["FP525a","Totally allocated fossil energy requirement for feedstock production",{"$f":"VLOOKUP(A340,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJfossil/MJFU"}]
["FP525b","Totally allocated primary energy requirement for feedstock production",{"$f":"VLOOKUP(A341,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJprim/MJFU"}]
["FP528a","Fossil energy used for feedstock production",{"$f":"VLOOKUP(A342,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kgdm"}]
["FP528b","Fossil energy used for feedstock production",{"$f":"VLOOKUP(A343,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP529a","Primary energy used for feedstock production",{"$f":"VLOOKUP(A344,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kgdm"}]
["FP529b","Primary energy used for feedstock production",{"$f":"VLOOKUP(A345,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP530","Allocation to energy crop",{"$f":"VLOOKUP(A346,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP531","Allocation to by-products",{"$f":"VLOOKUP(A347,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP531a","Allocation to by-product 1",{"$f":"VLOOKUP(A348,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP531b","Allocation to by-product 2",{"$f":"VLOOKUP(A349,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP532a","Allocated fossil energy requirement for feedstock production",{"$f":"VLOOKUP(A350,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["FP532b","Allocated primary energy requirement for feedstock production",{"$f":"VLOOKUP(A351,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["FP534","Type of fuel used for agricultural machinery",{"$f":"VLOOKUP(A352,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP535a","Fossil energy use related to agrifuel use",{"$f":"VLOOKUP(A353,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP535b","Primary energy use related to agrifuel use",{"$f":"VLOOKUP(A354,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP536","Fossil energy coefficient of fuel used in agricultural machinery",{"$f":"VLOOKUP(A355,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kgfuel"}]
["FP537","Amount of fuel used in agricultural machinery",{"$f":"VLOOKUP(A356,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP538a","Fossil energy used for heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A357,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJfossil/kgfm"}]
["FP538b","Primary energy used for heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A358,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJprim/kgfm"}]
["FP539a","Fossil energy used for heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A359,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["FP539b","Primary energy used for heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A360,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["FP540","Heat energy use for drying and storage of the crop",{"$f":"VLOOKUP(A361,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJheat/kgfm"}]
["FP541","Heat source",{"$f":"VLOOKUP(A362,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP542a","Fossil energy coefficient of heat production for crop drying and storage",{"$f":"VLOOKUP(A363,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/MJheat"}]
["FP542b","Primary energy coefficient of heat production for crop drying and storage",{"$f":"VLOOKUP(A364,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/MJheat"}]
["FP542c","GHG coefficient of heat production for crop drying and storage",{"$f":"VLOOKUP(A365,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/MJheat"}]
["FP542d","NOx emissions factor of heat production for crop drying and storage",{"$f":"VLOOKUP(A366,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gNOX/MJheat"}]
["FP542e","SOx emissions factor of heat production for crop drying and storage",{"$f":"VLOOKUP(A367,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSOX/MJheat"}]
["FP543","Electricity energy use for drying and storage of the crop",{"$f":"VLOOKUP(A368,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJe/kgfm"}]
["FP544","Electricity source",{"$f":"VLOOKUP(A369,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP545a","Fossil energy coefficient of electricity for crop drying and storage",{"$f":"VLOOKUP(A370,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/MJe"}]
["FP545b","Primary energy coefficient of electricity for crop drying and storage",{"$f":"VLOOKUP(A371,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/MJe"}]
["FP545c","GHG coefficient of electricity for crop drying and storage",{"$f":"VLOOKUP(A372,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/MJe"}]
["FP545d","NOx emissions factor of electricity for crop drying and storage",{"$f":"VLOOKUP(A373,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gNOX/MJe"}]
["FP545e","SOx emissions factor of electricity for crop drying and storage",{"$f":"VLOOKUP(A374,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSOX/MJe"}]
["FP546a","Fossil energy use of seeds, fertilisers and pesticides",{"$f":"VLOOKUP(A375,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP546b","Primary energy use of seeds, fertilisers and pesticides",{"$f":"VLOOKUP(A376,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP547","Pretreated feedstock",{"$f":"VLOOKUP(A377,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP548","Moisture content pretreated feedstock",{"$f":"VLOOKUP(A378,'Conversion feedstock2'!D$10:E$694,2,FALSE)","v":"%"}]
["FP549","Energy content pretreated feedstock",{"$f":"VLOOKUP(A379,'Conversion feedstock2'!D$10:E$694,2,FALSE)","v":"MJ/kgdm"}]
["FP550a","Fossil energy coefficient of N fertiliser",{"$f":"VLOOKUP(A380,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kg"}]
["FP550b","Fossil energy coefficient of P fertiliser",{"$f":"VLOOKUP(A381,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kg"}]
["FP550c","Fossil energy coefficient of K fertiliser",{"$f":"VLOOKUP(A382,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kg"}]
["FP550d","Fossil energy coefficient of Ca fertiliser",{"$f":"VLOOKUP(A383,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kg"}]
["FP550e","Fossil energy coefficient of pesticides",{"$f":"VLOOKUP(A384,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kg"}]
["FP550f","Fossil energy coefficient of seeds",{"$f":"VLOOKUP(A385,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/kg"}]
["FP551","Yield rate (moist/wet) of pretreated feedstock 2 per ha",{"$f":"VLOOKUP(A386,'Production feedstock2'!D$10:E$642,2,FALSE)","v":{"$error":"#N/A"}}]
["FP552","Yield rate (dry) of pretreated feedstock 2 per ha",{"$f":"VLOOKUP(A387,'Production feedstock2'!D$10:E$642,2,FALSE)","v":{"$error":"#N/A"}}]
["FP553","Yield rate (energy) of pretreated feedstock 2 per ha",{"$f":"VLOOKUP(A388,'Production feedstock2'!D$10:E$642,2,FALSE)","v":{"$error":"#N/A"}}]
["FP554","Yield loss through treatment and transport of feedstock 2",{"$f":"VLOOKUP(A389,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP555a","Yield rate (moist/wet) of pretreated feedstock 2 before conversion",{"$f":"VLOOKUP(A390,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP555b","Yield rate (dry) of pretreated feedstock 2 before conversion",{"$f":"VLOOKUP(A391,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgdm/ha"}]
["FP555c","Yield rate (energy) of pretreated feedstock 2 before conversion",{"$f":"VLOOKUP(A392,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"MJ/ha"}]
["FP556a","GHG emissions associated with inputs for feedstock production",{"$f":"VLOOKUP(A393,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/kgdm"}]
["FP556b","GHG emissions associated with inputs for feedstock production",{"$f":"VLOOKUP(A394,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha"}]
["FP557","Allocated GHG emissions from feedstock production",{"$f":"VLOOKUP(A395,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FP558","GHG emissions associated with fuel used in agricultural machinery",{"$f":"VLOOKUP(A396,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha"}]
["FP559","Specific GHG emissions of the fuel used in agricultural machinery",{"$f":"VLOOKUP(A397,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/kgfuel"}]
["FP561a","Totally allocated GHG emissions from feedstock production",{"$f":"VLOOKUP(A398,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FP561b","Totally allocated GHG emissions from feedstock production",{"$f":"VLOOKUP(A399,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FP562a","GHG emissions associated with heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A400,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/kgfm"}]
["FP562b","GHG emissions associated with heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A401,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FP564","GHG emissions associated with production of seeds, fertilisers and pesticides",{"$f":"VLOOKUP(A402,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha"}]
["FP567a","N: specific GHG emissions",{"$f":"VLOOKUP(A403,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/kgfertiliser"}]
["FP567b","P2O5: specific GHG emissions",{"$f":"VLOOKUP(A404,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/kgfertiliser"}]
["FP567c","K2O: specific GHG emissions",{"$f":"VLOOKUP(A405,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/kgfertiliser"}]
["FP567d","CaO: specific GHG emissions",{"$f":"VLOOKUP(A406,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/kgfertiliser"}]
["FP567e","Pesticides: specific GHG emissions",{"$f":"VLOOKUP(A407,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/kgpesticides"}]
["FP567f","Seeds: specific GHG emissions",{"$f":"VLOOKUP(A408,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/kgseeds"}]
["FP568a","GHG emissions associated with land use change (carbon stock changes) per MJ",{"$f":"VLOOKUP(A409,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/MJendfuel_fs2 (over 20yr)"}]
["FP568b","GHG emissions associated with land use change (carbon stock changes) per ha",{"$f":"VLOOKUP(A410,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha (over 20yr)"}]
["FP569a","Actual land use",{"$f":"VLOOKUP(A411,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP569b","Previous land use (January 1st, 2008)",{"$f":"VLOOKUP(A412,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP569c","Actual land use_specific for carbon stock veg",{"$f":"VLOOKUP(A413,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP569d","Previous land use (January 1st, 2008)_specific for carbon stock veg",{"$f":"VLOOKUP(A414,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP570a","Climate region",{"$f":"VLOOKUP(A415,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP570b","Soil type",{"$f":"VLOOKUP(A416,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP570c","Climate region_specific for carbon stock_actual land use",{"$f":"VLOOKUP(A417,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP570d","Climate region_specific for carbon stock_previous land use",{"$f":"VLOOKUP(A418,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP571","Carbon stock actual land use",{"$f":"VLOOKUP(A419,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP572","Carbon stock previous land use",{"$f":"VLOOKUP(A420,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP573a","Soil organic carbon actual land use",{"$f":"VLOOKUP(A421,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP573b","Soil organic carbon previous land use",{"$f":"VLOOKUP(A422,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP574","Standard soil organic carbon_feedstock 2",{"$f":"VLOOKUP(A423,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP575a","Land use factor actual land use",{"$f":"VLOOKUP(A424,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP575b","Land use factor previous land use",{"$f":"VLOOKUP(A425,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP576a","Management factor actual land use",{"$f":"VLOOKUP(A426,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP576b","Management factor previous land use",{"$f":"VLOOKUP(A427,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP577a","Input factor actual land use",{"$f":"VLOOKUP(A428,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP577b","Input factor previous land use",{"$f":"VLOOKUP(A429,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP578a","Above and below vegetation carbon stock actual land use",{"$f":"VLOOKUP(A430,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP578b","Above and below vegetation carbon stock previous land use",{"$f":"VLOOKUP(A431,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP579a","Above and below vegetation carbon stock in living biomass actual land use",{"$f":"VLOOKUP(A432,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP579b","Above and below vegetation carbon stock in living biomass previous land use",{"$f":"VLOOKUP(A433,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP580a","Above ground vegetation carbon stock in living biomass actual land use",{"$f":"VLOOKUP(A434,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP580b","Above ground vegetation carbon stock in living biomass previous land use",{"$f":"VLOOKUP(A435,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP581a","Weight of above ground living biomass actual land use",{"$f":"VLOOKUP(A436,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP581b","Weight of above ground living biomass previous land use",{"$f":"VLOOKUP(A437,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP582aa","Carbon fraction of dry matter in living biomass actual land use",{"$f":"VLOOKUP(A438,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP582ab","Carbon fraction of dry matter in living biomass previous land use",{"$f":"VLOOKUP(A439,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP582ba","Carbon fraction of dry matter in dead wood actual land use",{"$f":"VLOOKUP(A440,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP582bb","Carbon fraction of dry matter in dead wood previous land use",{"$f":"VLOOKUP(A441,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP582ca","Carbon fraction of dry matter in litter actual land use",{"$f":"VLOOKUP(A442,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP582cb","Carbon fraction of dry matter in litter previous land use",{"$f":"VLOOKUP(A443,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP583a","Ratio of below ground carbon stock to above ground carbon stock in living biomass actual land use",{"$f":"VLOOKUP(A444,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP583b","Ratio of below ground carbon stock to above ground carbon stock in living biomass previous land use",{"$f":"VLOOKUP(A445,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP584a","Below ground vegetation carbon stock in living biomass actual land use",{"$f":"VLOOKUP(A446,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP584b","Below ground vegetation carbon stock in living biomass previous land use",{"$f":"VLOOKUP(A447,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP585a","Weight of below ground living biomass actual land use",{"$f":"VLOOKUP(A448,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP585b","Weight of below ground living biomass previous land use",{"$f":"VLOOKUP(A449,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP586a","Above and below vegetation carbon stock in dead organic matter actual land use",{"$f":"VLOOKUP(A450,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP586b","Above and below vegetation carbon stock in dead organic matter previous land use",{"$f":"VLOOKUP(A451,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP587a","Carbon stock in dead wood pool actual land use",{"$f":"VLOOKUP(A452,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP587b","Carbon stock in dead wood pool previous land use",{"$f":"VLOOKUP(A453,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP588a","Weight of dead wood pool actual land use",{"$f":"VLOOKUP(A454,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP588b","Weight of dead wood pool previous land use",{"$f":"VLOOKUP(A455,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP589a","Carbon stock in litter actual land use",{"$f":"VLOOKUP(A456,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP589b","Carbon stock in litter previous land use",{"$f":"VLOOKUP(A457,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP590a","Weight of litter actual land use",{"$f":"VLOOKUP(A458,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP590b","Weight of litter previous land use",{"$f":"VLOOKUP(A459,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP591a","Peatland",{"$f":"VLOOKUP(A460,'Production feedstock2'!D$10:E$642,2,FALSE)","v":{"$error":"#N/A"}}]
["FP591b","Emission factor soil organic carbon_peatland",{"$f":"VLOOKUP(A461,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP592a","Previously degraded land",{"$f":"VLOOKUP(A462,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP592b","Bonus restored degraded land",{"$f":"VLOOKUP(A463,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/MJ (per year)"}]
["FP593a","Land management actual land use",{"$f":"VLOOKUP(A464,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP593b","Land management previous land use",{"$f":"VLOOKUP(A465,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP594a","Input actual land use",{"$f":"VLOOKUP(A466,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP594b","Input previous land use",{"$f":"VLOOKUP(A467,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP595a","Domain actual land use",{"$f":"VLOOKUP(A468,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP595b","Domain previous land use",{"$f":"VLOOKUP(A469,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP596a","Ecological zone actual land use",{"$f":"VLOOKUP(A470,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP596b","Ecological zone previous land use",{"$f":"VLOOKUP(A471,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP597a","Continent actual land use",{"$f":"VLOOKUP(A472,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP597b","Continent previous land use",{"$f":"VLOOKUP(A473,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP598a","Type actual land use",{"$f":"VLOOKUP(A474,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP598b","Type previous land use",{"$f":"VLOOKUP(A475,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP599","GHG emissions associated with indirect land use change (soil carbon release)",{"$f":"VLOOKUP(A476,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha (spread over 20yr)"}]
["FP600","Water use for feedstock production",{"$f":"VLOOKUP(A477,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"m³/ha"}]
["FP601","Allocated water use for feedstock production",{"$f":"VLOOKUP(A478,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["FP602a","Totally allocated water use for feedstock production",{"$f":"VLOOKUP(A479,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["FP602b","Totally allocated water use for feedstock production",{"$f":"VLOOKUP(A480,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"m³/GJFU"}]
["FP603a","Water use for feedstock treatment 1 (drying and storage)",{"$f":"VLOOKUP(A481,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"m³/kgfm"}]
["FP603b","Water use for feedstock treatment 1 (drying and storage)",{"$f":"VLOOKUP(A482,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["FP604a","Country freshwater availability",{"$f":"VLOOKUP(A483,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"m³/capita.yr"}]
["FP604b","Country freshwater level",{"$f":"VLOOKUP(A484,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP605","Allocated land use for feedstock production",{"$f":"VLOOKUP(A485,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"ha/GJendfuel_fs1"}]
["FP606a","Totally allocated land use for feedstock production",{"$f":"VLOOKUP(A486,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"ha/GJendfuel_fs1"}]
["FP606b","Totally allocated land use for feedstock production",{"$f":"VLOOKUP(A487,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"ha/GJFU"}]
["FP607a","Carbon debt due to land use change",{"$f":"VLOOKUP(A488,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha"}]
["FP607b","Allocated carbon debt",{"$f":"VLOOKUP(A489,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha"}]
["FP607c","Totally allocated carbon debt",{"$f":"VLOOKUP(A490,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha"}]
["FP608","Allocated GHG emissions from feedstock production without LUC emissions",{"$f":"VLOOKUP(A491,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FP609","Input of N-fixing crop residue to the soil",{"$f":"VLOOKUP(A492,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kg/ha"}]
["FP610a","Acidification potential of NH3",{"$f":"VLOOKUP(A493,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2_eq/gNH3"}]
["FP610b","Acidification potential of NOx",{"$f":"VLOOKUP(A494,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2_eq/gNOx"}]
["FP610c","Acidification potential of SOx",{"$f":"VLOOKUP(A495,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2_eq/gSOx"}]
["FP611a","Agrifuel NOx emissions factor",{"$f":"VLOOKUP(A496,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gNOX/kgfuel"}]
["FP611b","Agrifuel SOx emissions factor",{"$f":"VLOOKUP(A497,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSOX/kgfuel"}]
["FP612","Acidification potential from feedstock production",{"$f":"VLOOKUP(A498,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2_eq/ha"}]
["FP613","NH3 volatilization from fertiliser use",{"$f":"VLOOKUP(A499,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gNH3/ha"}]
["FP614","Allocated acidification potential from feedstock production",{"$f":"VLOOKUP(A500,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FP615a","Totally allocated acidification potential from feedstock production",{"$f":"VLOOKUP(A501,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FP615b","Totally allocated acidification potential from feedstock production",{"$f":"VLOOKUP(A502,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FP616a","Acidification potential associated with heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A503,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2-eq/kgfm"}]
["FP616b","Acidification potential associated with heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A504,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FP620a","Eutrophication potential of N to air",{"$f":"VLOOKUP(A505,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gN"}]
["FP620b","Eutrophication potential of NOx to air",{"$f":"VLOOKUP(A506,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gNOx"}]
["FP620c","Eutrophication potential of NH3 to air",{"$f":"VLOOKUP(A507,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gNH3"}]
["FP620d","Eutrophication potential of N to water",{"$f":"VLOOKUP(A508,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gN"}]
["FP620e","Eutrophication potential of NO3- to water",{"$f":"VLOOKUP(A509,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gNO3"}]
["FP620f","Eutrophication potential of NH4+ to water",{"$f":"VLOOKUP(A510,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gNH4+"}]
["FP620g","Eutrophication potential of P to water",{"$f":"VLOOKUP(A511,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gP"}]
["FP620h","Eutrophication potential of PO43-",{"$f":"VLOOKUP(A512,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gPO4"}]
["FP620i","Eutrophication potential of COD",{"$f":"VLOOKUP(A513,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/gCOD"}]
["FP622","Eutrophication potential of feedstock production",{"$f":"VLOOKUP(A514,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/ha"}]
["FP623a","N volatilization from fertiliser use (including NOx and NH3)",{"$f":"VLOOKUP(A515,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gN/ha"}]
["FP623d","N leaching from fertiliser use (including NO3- and NH4+)",{"$f":"VLOOKUP(A516,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gN/ha"}]
["FP623g","P leaching from fertiliser use (total P to water)",{"$f":"VLOOKUP(A517,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gP/ha"}]
["FP624","Allocated eutrophication potential from feedstock production",{"$f":"VLOOKUP(A518,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FP625a","Totally allocated eutrophication potential from feedstock production",{"$f":"VLOOKUP(A519,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FP625b","Totally allocated eutrophication potential from feedstock production",{"$f":"VLOOKUP(A520,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/MJFU"}]
["FP626a","Eutrophication potential associated with heat and electricity for drying and storage per kg",{"$f":"VLOOKUP(A521,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4-eq/kgfm"}]
["FP626b","Eutrophication potential associated with heat and electricity for drying and storage per MJ endfuel",{"$f":"VLOOKUP(A522,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FP630a","Total (direct + indirect) N2O emissions from managed soils",{"$f":"VLOOKUP(A523,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gN20/ha"}]
["FP630b","Total (direct + indirect) N2O emissions from managed soils",{"$f":"VLOOKUP(A524,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"gCO2-eq/ha"}]
["FP631","Soil water saturation (yes=1,no=0)",{"$f":"VLOOKUP(A525,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP632","Field renewal (annual crops = 1)",{"$f":"VLOOKUP(A526,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"years"}]
["FP633","Amount of crop residue returned to the field (only for palm)",{"$f":"VLOOKUP(A527,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgdm/kgfm"}]
["FP634","Organic soil (yes=1,no=0)",{"$f":"VLOOKUP(A528,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP635","Nutrient level (only for ORGANIC soils + temperate/boreal climate + forest (native and managed))",{"$f":"VLOOKUP(A529,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP637a","Emission factor for direct N2O emissions from N inputs",{"$f":"VLOOKUP(A530,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/kgN_input"}]
["FP637b","Emission factor for direct N2O emissions from drained/managed organic soils",{"$f":"VLOOKUP(A531,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/ha"}]
["FP637c","Emission factor for direct N2O emissions from urine and dung N deposited by grazing animals",{"$f":"VLOOKUP(A532,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/kgN_input"}]
["FP637d","Emission factor for indirect N2O emissions from atmospheric deposition of N",{"$f":"VLOOKUP(A533,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/kgN_volatilised"}]
["FP637e","Emission factor for indirect N2O emissions from leaching and runoff",{"$f":"VLOOKUP(A534,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/kgN_leached+runoff"}]
["FP638a","Direct N2O_N emissions from managed soils",{"$f":"VLOOKUP(A535,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/ha"}]
["FP638b","Direct N2O emissions from managed soils",{"$f":"VLOOKUP(A536,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20/ha"}]
["FP639","Direct N2O_N emissions from N inputs to managed mineral soils",{"$f":"VLOOKUP(A537,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/ha"}]
["FP640","Total amount of organic N fertiliser applied to soil (other than by grazing animals)",{"$f":"VLOOKUP(A538,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/ha"}]
["FP641a","Amount of animal manure N applied to soil (other than by grazing animals)",{"$f":"VLOOKUP(A539,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/ha"}]
["FP641b","Amount of total sewage N applied to soil",{"$f":"VLOOKUP(A540,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/ha"}]
["FP641c","Amount of total compost N applied to soil",{"$f":"VLOOKUP(A541,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/ha"}]
["FP641d","Amount of N of other organic amendments applied to soil (used as fertiliser)",{"$f":"VLOOKUP(A542,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/ha"}]
["FP642","Total amount of N in crop residues (including N-fixing crops and renewal) returned to soil",{"$f":"VLOOKUP(A543,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/ha"}]
["FP643a","Ratio of above-ground residues to harvested yield_calculated",{"$f":"VLOOKUP(A544,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgdm/kgdm"}]
["FP643b","Ratio of above-ground residues to harvested yield_final",{"$f":"VLOOKUP(A545,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgdm/kgdm"}]
["FP644","Above-ground residue (dry) (=AGDM(T))",{"$f":"VLOOKUP(A546,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"t/ha"}]
["FP645a","Slope to calculate above-ground residue",{"$f":"VLOOKUP(A547,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP645b","Intercept to calculate above-ground residue",{"$f":"VLOOKUP(A548,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP646a","Ratio of below-ground residues to harvested yield_calculated",{"$f":"VLOOKUP(A549,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgdm/kgdm"}]
["FP646b","Ratio of below-ground residues to harvested yield_final",{"$f":"VLOOKUP(A550,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgdm/kgdm"}]
["FP647","Ratio of below-ground residues to above-ground biomass",{"$f":"VLOOKUP(A551,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgdm/kgdm"}]
["FP648a","N content of above-ground residues",{"$f":"VLOOKUP(A552,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/kgdm"}]
["FP648b","N content of below-ground residues",{"$f":"VLOOKUP(A553,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/kgdm"}]
["FP649","Fraction of above-ground residues removed",{"$f":"VLOOKUP(A554,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"%"}]
["FP650","Total amount of N mineralised in mineral soil due to carbon loss through land use change",{"$f":"VLOOKUP(A555,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN/ha"}]
["FP651","Average annual loss of soil carbon",{"$f":"VLOOKUP(A556,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"tC/ha"}]
["FP652","C:N ratio of the soil organic matter",{"$f":"VLOOKUP(A557,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP653","Previous land use is cropland (yes=1,no=0)",{"$f":"VLOOKUP(A558,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP654","Direct N2O_N emissions from managed organic soils",{"$f":"VLOOKUP(A559,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/ha"}]
["FP655a","Indirect N2O_N emissions from managed soils",{"$f":"VLOOKUP(A560,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/ha"}]
["FP655b","Indirect N2O emissions from managed soils",{"$f":"VLOOKUP(A561,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20/ha"}]
["FP656","Indirect N2O_N emissions from atmospheric deposition of N volatilized from managed soils",{"$f":"VLOOKUP(A562,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/ha"}]
["FP657","Fraction of synthetic fertiliser N that volatilises as NH3 and NOx",{"$f":"VLOOKUP(A563,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN_volatilised/kgN_applied"}]
["FP658","Fraction of organic fertiliser N that volatilises as NH3 and NOx",{"$f":"VLOOKUP(A564,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN_volatilised/kgN_applied"}]
["FP659","Indirect N2O_N emissions from N leaching/runoff from managed soils",{"$f":"VLOOKUP(A565,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN20_N/ha"}]
["FP660","Fraction of all N added to managed soils that is lost through leaching and runoff",{"$f":"VLOOKUP(A566,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"kgN_leached/kgN_applied"}]
["FP661","Land status in or after January 2008 = undisturbed forest (yes=1,no=0)",{"$f":"VLOOKUP(A567,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP662","Land status in or after January 2008 = nature protection area",{"$f":"VLOOKUP(A568,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP663","Land status in or after January 2008 = highly biodiverse grassland",{"$f":"VLOOKUP(A569,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP664","Land status in January 2008 and not longer now = wetland",{"$f":"VLOOKUP(A570,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP665","Land status in January 2008 and not longer now = continuously forested area",{"$f":"VLOOKUP(A571,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP666","Land status in January 2008 and not longer now = peatland",{"$f":"VLOOKUP(A572,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP667","The requirements of the RED concerning biodiversity & high carbon stocks are met",{"$f":"VLOOKUP(A573,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"binary"}]
["FP670a","No forced labour",{"$f":"VLOOKUP(A574,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP670b","No child labour ",{"$f":"VLOOKUP(A575,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP670c","Good social practices regarding human rights",{"$f":"VLOOKUP(A576,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP670d","No discrimination",{"$f":"VLOOKUP(A577,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP670e","Land is used legitimately / land rights have been secured",{"$f":"VLOOKUP(A578,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP670f","Open and transparent communication with local communities and stakeholders",{"$f":"VLOOKUP(A579,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP670g","Food security",{"$f":"VLOOKUP(A580,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP671a","Fair legal contracts",{"$f":"VLOOKUP(A581,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP671b","Workers rights",{"$f":"VLOOKUP(A582,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP671c","Freedom to join labour organizations or organize themselves",{"$f":"VLOOKUP(A583,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP671d","Fair wages and compensation rules",{"$f":"VLOOKUP(A584,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP671e","Health, safety and hygiene policy",{"$f":"VLOOKUP(A585,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP671f","Risk assessment for safe and healthy working conditions",{"$f":"VLOOKUP(A586,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP671g","Health and safety training",{"$f":"VLOOKUP(A587,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP672","Human and property rights_score",{"$f":"VLOOKUP(A588,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
["FP673","Labour rights and conditions_score",{"$f":"VLOOKUP(A589,'Production feedstock2'!D$10:E$642,2,FALSE)","v":"-"}]
[]
["Transport Feedstock 1"]
["FT001a","Transport mode 1",{"$f":"VLOOKUP(A592,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT001b","Transport mode 2",{"$f":"VLOOKUP(A593,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT001c","Transport mode 3",{"$f":"VLOOKUP(A594,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT001d","Transport mode 4",{"$f":"VLOOKUP(A595,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT001e","Transport mode 5",{"$f":"VLOOKUP(A596,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT001f","Transport mode 6",{"$f":"VLOOKUP(A597,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT001g","Transport mode 7",{"$f":"VLOOKUP(A598,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT001h","Transport mode 8",{"$f":"VLOOKUP(A599,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT001i","Transport mode 9",{"$f":"VLOOKUP(A600,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT002a","Amount of transport mode 1",{"$f":"VLOOKUP(A601,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT002b","Amount of transport mode 2",{"$f":"VLOOKUP(A602,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT002c","Amount of transport mode 3",{"$f":"VLOOKUP(A603,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT002d","Amount of transport mode 4",{"$f":"VLOOKUP(A604,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT002e","Amount of transport mode 5",{"$f":"VLOOKUP(A605,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT002f","Amount of transport mode 6",{"$f":"VLOOKUP(A606,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT002g","Amount of transport mode 7",{"$f":"VLOOKUP(A607,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT002h","Amount of transport mode 8",{"$f":"VLOOKUP(A608,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT002i","Amount of transport mode 9",{"$f":"VLOOKUP(A609,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"tkm/ha"}]
["FT003a","Distance of transport mode 1",{"$f":"VLOOKUP(A610,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT003b","Distance of transport mode 2",{"$f":"VLOOKUP(A611,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT003c","Distance of transport mode 3",{"$f":"VLOOKUP(A612,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT003d","Distance of transport mode 4",{"$f":"VLOOKUP(A613,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT003e","Distance of transport mode 5",{"$f":"VLOOKUP(A614,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT003f","Distance of transport mode 6",{"$f":"VLOOKUP(A615,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT003g","Distance of transport mode 7",{"$f":"VLOOKUP(A616,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT003h","Distance of transport mode 8",{"$f":"VLOOKUP(A617,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT003i","Distance of transport mode 9",{"$f":"VLOOKUP(A618,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"km"}]
["FT004a","Type of fuel used for transport mode 1",{"$f":"VLOOKUP(A619,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT004b","Type of fuel used for transport mode 2",{"$f":"VLOOKUP(A620,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT004c","Type of fuel used for transport mode 3",{"$f":"VLOOKUP(A621,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT004d","Type of fuel used for transport mode 4",{"$f":"VLOOKUP(A622,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT004e","Type of fuel used for transport mode 5",{"$f":"VLOOKUP(A623,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT004f","Type of fuel used for transport mode 6",{"$f":"VLOOKUP(A624,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT004g","Type of fuel used for transport mode 7",{"$f":"VLOOKUP(A625,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT004h","Type of fuel used for transport mode 8",{"$f":"VLOOKUP(A626,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT004i","Type of fuel used for transport mode 9",{"$f":"VLOOKUP(A627,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"-"}]
["FT005a","Amount of fuel used per tkm - transport mode 1",{"$f":"VLOOKUP(A628,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT005b","Amount of fuel used per tkm - transport mode 2",{"$f":"VLOOKUP(A629,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT005c","Amount of fuel used per tkm - transport mode 3",{"$f":"VLOOKUP(A630,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT005d","Amount of fuel used per tkm - transport mode 4",{"$f":"VLOOKUP(A631,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT005e","Amount of fuel used per tkm - transport mode 5",{"$f":"VLOOKUP(A632,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT005f","Amount of fuel used per tkm - transport mode 6",{"$f":"VLOOKUP(A633,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT005g","Amount of fuel used per tkm - transport mode 7",{"$f":"VLOOKUP(A634,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT005h","Amount of fuel used per tkm - transport mode 8",{"$f":"VLOOKUP(A635,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT005i","Amount of fuel used per tkm - transport mode 9",{"$f":"VLOOKUP(A636,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfuel/tkm"}]
["FT006a","Specific fossil energy related to fuel use - transport mode 1",{"$f":"VLOOKUP(A637,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT006b","Specific fossil energy related to fuel use - transport mode 2",{"$f":"VLOOKUP(A638,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT006c","Specific fossil energy related to fuel use - transport mode 3",{"$f":"VLOOKUP(A639,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT006d","Specific fossil energy related to fuel use - transport mode 4",{"$f":"VLOOKUP(A640,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT006e","Specific fossil energy related to fuel use - transport mode 5",{"$f":"VLOOKUP(A641,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT006f","Specific fossil energy related to fuel use - transport mode 6",{"$f":"VLOOKUP(A642,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT006g","Specific fossil energy related to fuel use - transport mode 7",{"$f":"VLOOKUP(A643,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT006h","Specific fossil energy related to fuel use - transport mode 8",{"$f":"VLOOKUP(A644,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT006i","Specific fossil energy related to fuel use - transport mode 9",{"$f":"VLOOKUP(A645,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT007a","Specific primary energy related to fuel use -  transport mode 1",{"$f":"VLOOKUP(A646,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT007b","Specific primary energy related to fuel use -  transport mode 2",{"$f":"VLOOKUP(A647,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT007c","Specific primary energy related to fuel use -  transport mode 3",{"$f":"VLOOKUP(A648,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT007d","Specific primary energy related to fuel use -  transport mode 4",{"$f":"VLOOKUP(A649,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT007e","Specific primary energy related to fuel use -  transport mode 5",{"$f":"VLOOKUP(A650,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT007f","Specific primary energy related to fuel use -  transport mode 6",{"$f":"VLOOKUP(A651,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT007g","Specific primary energy related to fuel use -  transport mode 7",{"$f":"VLOOKUP(A652,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT007h","Specific primary energy related to fuel use -  transport mode 8",{"$f":"VLOOKUP(A653,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT007i","Specific primary energy related to fuel use -  transport mode 9",{"$f":"VLOOKUP(A654,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJfuel"}]
["FT008a","Specific GHG emissions related to fuel use - transport mode 1",{"$f":"VLOOKUP(A655,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT008b","Specific GHG emissions related to fuel use - transport mode 2",{"$f":"VLOOKUP(A656,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT008c","Specific GHG emissions related to fuel use - transport mode 3",{"$f":"VLOOKUP(A657,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT008d","Specific GHG emissions related to fuel use - transport mode 4",{"$f":"VLOOKUP(A658,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT008e","Specific GHG emissions related to fuel use - transport mode 5",{"$f":"VLOOKUP(A659,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT008f","Specific GHG emissions related to fuel use - transport mode 6",{"$f":"VLOOKUP(A660,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT008g","Specific GHG emissions related to fuel use - transport mode 7",{"$f":"VLOOKUP(A661,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT008h","Specific GHG emissions related to fuel use - transport mode 8",{"$f":"VLOOKUP(A662,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT008i","Specific GHG emissions related to fuel use - transport mode 9",{"$f":"VLOOKUP(A663,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT009a","Fossil energy use for transport mode 1",{"$f":"VLOOKUP(A664,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT009b","Fossil energy use for transport mode 2",{"$f":"VLOOKUP(A665,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT009c","Fossil energy use for transport mode 3",{"$f":"VLOOKUP(A666,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT009d","Fossil energy use for transport mode 4",{"$f":"VLOOKUP(A667,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT009e","Fossil energy use for transport mode 5",{"$f":"VLOOKUP(A668,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT009f","Fossil energy use for transport mode 6",{"$f":"VLOOKUP(A669,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT009g","Fossil energy use for transport mode 7",{"$f":"VLOOKUP(A670,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT009h","Fossil energy use for transport mode 8",{"$f":"VLOOKUP(A671,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT009i","Fossil energy use for transport mode 9",{"$f":"VLOOKUP(A672,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/ha"}]
["FT010a","Primary energy use for transport mode 1",{"$f":"VLOOKUP(A673,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT010b","Primary energy use for transport mode 2",{"$f":"VLOOKUP(A674,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT010c","Primary energy use for transport mode 3",{"$f":"VLOOKUP(A675,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT010d","Primary energy use for transport mode 4",{"$f":"VLOOKUP(A676,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT010e","Primary energy use for transport mode 5",{"$f":"VLOOKUP(A677,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT010f","Primary energy use for transport mode 6",{"$f":"VLOOKUP(A678,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT010g","Primary energy use for transport mode 7",{"$f":"VLOOKUP(A679,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT010h","Primary energy use for transport mode 8",{"$f":"VLOOKUP(A680,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT010i","Primary energy use for transport mode 9",{"$f":"VLOOKUP(A681,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/ha"}]
["FT011a","GHG emissions of fuel used in transport mode 1",{"$f":"VLOOKUP(A682,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT011b","GHG emissions of fuel used in transport mode 2",{"$f":"VLOOKUP(A683,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT011c","GHG emissions of fuel used in transport mode 3",{"$f":"VLOOKUP(A684,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT011d","GHG emissions of fuel used in transport mode 4",{"$f":"VLOOKUP(A685,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT011e","GHG emissions of fuel used in transport mode 5",{"$f":"VLOOKUP(A686,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT011f","GHG emissions of fuel used in transport mode 6",{"$f":"VLOOKUP(A687,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT011g","GHG emissions of fuel used in transport mode 7",{"$f":"VLOOKUP(A688,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT011h","GHG emissions of fuel used in transport mode 8",{"$f":"VLOOKUP(A689,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT011i","GHG emissions of fuel used in transport mode 9",{"$f":"VLOOKUP(A690,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2-eq/ha"}]
["FT012a","Fossil energy use for transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A691,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT012b","Primary energy use for transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A692,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT013a","Fossil energy use for transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A693,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT013b","Primary energy use for transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A694,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT014a","Fossil energy use for transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A695,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT014b","Primary energy use for transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A696,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT015a","GHG emissions associated with transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A697,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FT015b","GHG emissions associated with transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A698,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FT015c","GHG emissions associated with transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A699,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FT016a","Acidification potential associated with transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A700,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FT016b","Acidification potential associated with transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A701,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FT016c","Acidification potential associated with transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A702,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FT017a","Eutrophication potential associated with transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A703,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FT017b","Eutrophication potential associated with transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A704,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FT017c","Eutrophication potential associated with transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A705,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FT020a","Totally allocated fossil energy requirement in transport 1",{"$f":"VLOOKUP(A706,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT020b","Totally allocated primary energy requirement in transport 1",{"$f":"VLOOKUP(A707,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT021a","Totally allocated fossil energy requirement in transport 1",{"$f":"VLOOKUP(A708,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJFU"}]
["FT021b","Totally allocated primary energy requirement in transport 1",{"$f":"VLOOKUP(A709,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJFU"}]
["FT022a","Totally allocated fossil energy requirement in transport 2",{"$f":"VLOOKUP(A710,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT022b","Totally allocated primary energy requirement in transport 2",{"$f":"VLOOKUP(A711,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT023a","Totally allocated fossil energy requirement in transport 2",{"$f":"VLOOKUP(A712,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJFU"}]
["FT023b","Totally allocated primary energy requirement in transport 2",{"$f":"VLOOKUP(A713,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJFU"}]
["FT024a","Totally allocated fossil energy requirement in transport 3",{"$f":"VLOOKUP(A714,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT024b","Totally allocated primary energy requirement in transport 3",{"$f":"VLOOKUP(A715,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT025a","Totally allocated fossil energy requirement in transport 3",{"$f":"VLOOKUP(A716,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJFU"}]
["FT025b","Totally allocated primary energy requirement in transport 3",{"$f":"VLOOKUP(A717,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJFU"}]
["FT026a","Totally allocated fossil energy requirement in total transport (1-3)",{"$f":"VLOOKUP(A718,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT026b","Totally allocated primary energy requirement in total transport (1-3)",{"$f":"VLOOKUP(A719,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT027a","Totally allocated fossil energy requirement in total transport (1-3)",{"$f":"VLOOKUP(A720,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJfossil/MJFU"}]
["FT027b","Totally allocated primary energy requirement in total transport (1-3)",{"$f":"VLOOKUP(A721,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"MJprim/MJFU"}]
["FT030a","Totally allocated GHG emissions from transport 1",{"$f":"VLOOKUP(A722,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FT030b","Totally allocated GHG emissions from transport 1",{"$f":"VLOOKUP(A723,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FT031a","Totally allocated GHG emissions from transport 2",{"$f":"VLOOKUP(A724,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FT031b","Totally allocated GHG emissions from transport 2",{"$f":"VLOOKUP(A725,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FT032a","Totally allocated GHG emissions from transport 3",{"$f":"VLOOKUP(A726,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FT032b","Totally allocated GHG emissions from transport 3",{"$f":"VLOOKUP(A727,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FT033a","Totally allocated GHG emissions from total transport (1-3)",{"$f":"VLOOKUP(A728,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["FT033b","Totally allocated GHG emissions from total transport (1-3)",{"$f":"VLOOKUP(A729,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FT035a","Acidification potential related to fuel used in transport mode 1",{"$f":"VLOOKUP(A730,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT035b","Acidification potential related to fuel used in transport mode 2",{"$f":"VLOOKUP(A731,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT035c","Acidification potential related to fuel used in transport mode 3",{"$f":"VLOOKUP(A732,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT035d","Acidification potential related to fuel used in transport mode 4",{"$f":"VLOOKUP(A733,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT035e","Acidification potential related to fuel used in transport mode 5",{"$f":"VLOOKUP(A734,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT035f","Acidification potential related to fuel used in transport mode 6",{"$f":"VLOOKUP(A735,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT035g","Acidification potential related to fuel used in transport mode 7",{"$f":"VLOOKUP(A736,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT035h","Acidification potential related to fuel used in transport mode 8",{"$f":"VLOOKUP(A737,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT035i","Acidification potential related to fuel used in transport mode 9",{"$f":"VLOOKUP(A738,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2-eq/ha"}]
["FT036a","Eutrophication potential related to fuel used in transport mode 1",{"$f":"VLOOKUP(A739,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT036b","Eutrophication potential related to fuel used in transport mode 2",{"$f":"VLOOKUP(A740,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT036c","Eutrophication potential related to fuel used in transport mode 3",{"$f":"VLOOKUP(A741,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT036d","Eutrophication potential related to fuel used in transport mode 4",{"$f":"VLOOKUP(A742,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT036e","Eutrophication potential related to fuel used in transport mode 5",{"$f":"VLOOKUP(A743,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT036f","Eutrophication potential related to fuel used in transport mode 6",{"$f":"VLOOKUP(A744,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT036g","Eutrophication potential related to fuel used in transport mode 7",{"$f":"VLOOKUP(A745,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT036h","Eutrophication potential related to fuel used in transport mode 8",{"$f":"VLOOKUP(A746,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT036i","Eutrophication potential related to fuel used in transport mode 9",{"$f":"VLOOKUP(A747,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4-eq/ha"}]
["FT037a","NOx emissions factor of fuel - transport mode 1",{"$f":"VLOOKUP(A748,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT037b","NOx emissions factor of fuel - transport mode 2",{"$f":"VLOOKUP(A749,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT037c","NOx emissions factor of fuel - transport mode 3",{"$f":"VLOOKUP(A750,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT037d","NOx emissions factor of fuel - transport mode 4",{"$f":"VLOOKUP(A751,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT037e","NOx emissions factor of fuel - transport mode 5",{"$f":"VLOOKUP(A752,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT037f","NOx emissions factor of fuel - transport mode 6",{"$f":"VLOOKUP(A753,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT037g","NOx emissions factor of fuel - transport mode 7",{"$f":"VLOOKUP(A754,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT037h","NOx emissions factor of fuel - transport mode 8",{"$f":"VLOOKUP(A755,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT037i","NOx emissions factor of fuel - transport mode 9",{"$f":"VLOOKUP(A756,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gNOX/MJfuel"}]
["FT038a","SOx emissions factor of fuel - transport mode 1",{"$f":"VLOOKUP(A757,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT038b","SOx emissions factor of fuel - transport mode 2",{"$f":"VLOOKUP(A758,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT038c","SOx emissions factor of fuel - transport mode 3",{"$f":"VLOOKUP(A759,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT038d","SOx emissions factor of fuel - transport mode 4",{"$f":"VLOOKUP(A760,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT038e","SOx emissions factor of fuel - transport mode 5",{"$f":"VLOOKUP(A761,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT038f","SOx emissions factor of fuel - transport mode 6",{"$f":"VLOOKUP(A762,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT038g","SOx emissions factor of fuel - transport mode 7",{"$f":"VLOOKUP(A763,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT038h","SOx emissions factor of fuel - transport mode 8",{"$f":"VLOOKUP(A764,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT038i","SOx emissions factor of fuel - transport mode 9",{"$f":"VLOOKUP(A765,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSOX/MJfuel"}]
["FT040a","Totally allocated acidification potential from transport 1",{"$f":"VLOOKUP(A766,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FT040b","Totally allocated acidification potential from transport 1",{"$f":"VLOOKUP(A767,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FT041a","Totally allocated acidification potential from transport 2",{"$f":"VLOOKUP(A768,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FT041b","Totally allocated acidification potential from transport 2",{"$f":"VLOOKUP(A769,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FT042a","Totally allocated acidification potential from transport 3",{"$f":"VLOOKUP(A770,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FT042b","Totally allocated acidification potential from transport 3",{"$f":"VLOOKUP(A771,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FT043a","Totally allocated acidification potential from total transport (1-3)",{"$f":"VLOOKUP(A772,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["FT043b","Totally allocated acidification potential from total transport (1-3)",{"$f":"VLOOKUP(A773,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FT044a","Totally allocated eutrophication potential from transport 1",{"$f":"VLOOKUP(A774,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FT044b","Totally allocated eutrophication potential from transport 1",{"$f":"VLOOKUP(A775,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJFU"}]
["FT045a","Totally allocated eutrophication potential from transport 2",{"$f":"VLOOKUP(A776,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FT045b","Totally allocated eutrophication potential from transport 2",{"$f":"VLOOKUP(A777,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJFU"}]
["FT046a","Totally allocated eutrophication potential from transport 3",{"$f":"VLOOKUP(A778,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FT046b","Totally allocated eutrophication potential from transport 3",{"$f":"VLOOKUP(A779,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJFU"}]
["FT047a","Totally allocated eutrophication potential from total transport (1-3)",{"$f":"VLOOKUP(A780,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["FT047b","Totally allocated eutrophication potential from total transport (1-3)",{"$f":"VLOOKUP(A781,'Transport feedstock1'!D$10:E$615,2,FALSE)","v":"gPO4_eq/MJFU"}]
[]
["Transport Feedstock 2"]
["FT501a","Transport mode 1",{"$f":"VLOOKUP(A784,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT501b","Transport mode 2",{"$f":"VLOOKUP(A785,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT501c","Transport mode 3",{"$f":"VLOOKUP(A786,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT501d","Transport mode 4",{"$f":"VLOOKUP(A787,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT501e","Transport mode 5",{"$f":"VLOOKUP(A788,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT501f","Transport mode 6",{"$f":"VLOOKUP(A789,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT501g","Transport mode 7",{"$f":"VLOOKUP(A790,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT501h","Transport mode 8",{"$f":"VLOOKUP(A791,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT501i","Transport mode 9",{"$f":"VLOOKUP(A792,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT502a","Amount of transport mode 1",{"$f":"VLOOKUP(A793,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT502b","Amount of transport mode 2",{"$f":"VLOOKUP(A794,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT502c","Amount of transport mode 3",{"$f":"VLOOKUP(A795,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT502d","Amount of transport mode 4",{"$f":"VLOOKUP(A796,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT502e","Amount of transport mode 5",{"$f":"VLOOKUP(A797,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT502f","Amount of transport mode 6",{"$f":"VLOOKUP(A798,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT502g","Amount of transport mode 7",{"$f":"VLOOKUP(A799,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT502h","Amount of transport mode 8",{"$f":"VLOOKUP(A800,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT502i","Amount of transport mode 9",{"$f":"VLOOKUP(A801,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"tkm/ha"}]
["FT503a","Distance of transport mode 1",{"$f":"VLOOKUP(A802,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT503b","Distance of transport mode 2",{"$f":"VLOOKUP(A803,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT503c","Distance of transport mode 3",{"$f":"VLOOKUP(A804,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT503d","Distance of transport mode 4",{"$f":"VLOOKUP(A805,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT503e","Distance of transport mode 5",{"$f":"VLOOKUP(A806,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT503f","Distance of transport mode 6",{"$f":"VLOOKUP(A807,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT503g","Distance of transport mode 7",{"$f":"VLOOKUP(A808,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT503h","Distance of transport mode 8",{"$f":"VLOOKUP(A809,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT503i","Distance of transport mode 9",{"$f":"VLOOKUP(A810,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"km"}]
["FT504a","Type of fuel used for transport mode 1",{"$f":"VLOOKUP(A811,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT504b","Type of fuel used for transport mode 2",{"$f":"VLOOKUP(A812,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT504c","Type of fuel used for transport mode 3",{"$f":"VLOOKUP(A813,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT504d","Type of fuel used for transport mode 4",{"$f":"VLOOKUP(A814,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT504e","Type of fuel used for transport mode 5",{"$f":"VLOOKUP(A815,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT504f","Type of fuel used for transport mode 6",{"$f":"VLOOKUP(A816,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT504g","Type of fuel used for transport mode 7",{"$f":"VLOOKUP(A817,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT504h","Type of fuel used for transport mode 8",{"$f":"VLOOKUP(A818,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT504i","Type of fuel used for transport mode 9",{"$f":"VLOOKUP(A819,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"-"}]
["FT505a","Amount of fuel used per tkm - transport mode 1",{"$f":"VLOOKUP(A820,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT505b","Amount of fuel used per tkm - transport mode 2",{"$f":"VLOOKUP(A821,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT505c","Amount of fuel used per tkm - transport mode 3",{"$f":"VLOOKUP(A822,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT505d","Amount of fuel used per tkm - transport mode 4",{"$f":"VLOOKUP(A823,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT505e","Amount of fuel used per tkm - transport mode 5",{"$f":"VLOOKUP(A824,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT505f","Amount of fuel used per tkm - transport mode 6",{"$f":"VLOOKUP(A825,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT505g","Amount of fuel used per tkm - transport mode 7",{"$f":"VLOOKUP(A826,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT505h","Amount of fuel used per tkm - transport mode 8",{"$f":"VLOOKUP(A827,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT505i","Amount of fuel used per tkm - transport mode 9",{"$f":"VLOOKUP(A828,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfuel/tkm"}]
["FT506a","Specific fossil energy related to fuel use - transport mode 1",{"$f":"VLOOKUP(A829,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT506b","Specific fossil energy related to fuel use - transport mode 2",{"$f":"VLOOKUP(A830,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT506c","Specific fossil energy related to fuel use - transport mode 3",{"$f":"VLOOKUP(A831,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT506d","Specific fossil energy related to fuel use - transport mode 4",{"$f":"VLOOKUP(A832,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT506e","Specific fossil energy related to fuel use - transport mode 5",{"$f":"VLOOKUP(A833,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT506f","Specific fossil energy related to fuel use - transport mode 6",{"$f":"VLOOKUP(A834,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT506g","Specific fossil energy related to fuel use - transport mode 7",{"$f":"VLOOKUP(A835,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT506h","Specific fossil energy related to fuel use - transport mode 8",{"$f":"VLOOKUP(A836,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT506i","Specific fossil energy related to fuel use - transport mode 9",{"$f":"VLOOKUP(A837,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJfuel"}]
["FT507a","Specific primary energy related to fuel use -  transport mode 1",{"$f":"VLOOKUP(A838,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT507b","Specific primary energy related to fuel use -  transport mode 2",{"$f":"VLOOKUP(A839,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT507c","Specific primary energy related to fuel use -  transport mode 3",{"$f":"VLOOKUP(A840,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT507d","Specific primary energy related to fuel use -  transport mode 4",{"$f":"VLOOKUP(A841,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT507e","Specific primary energy related to fuel use -  transport mode 5",{"$f":"VLOOKUP(A842,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT507f","Specific primary energy related to fuel use -  transport mode 6",{"$f":"VLOOKUP(A843,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT507g","Specific primary energy related to fuel use -  transport mode 7",{"$f":"VLOOKUP(A844,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT507h","Specific primary energy related to fuel use -  transport mode 8",{"$f":"VLOOKUP(A845,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT507i","Specific primary energy related to fuel use -  transport mode 9",{"$f":"VLOOKUP(A846,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJfuel"}]
["FT508a","Specific GHG emissions related to fuel use - transport mode 1",{"$f":"VLOOKUP(A847,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT508b","Specific GHG emissions related to fuel use - transport mode 2",{"$f":"VLOOKUP(A848,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT508c","Specific GHG emissions related to fuel use - transport mode 3",{"$f":"VLOOKUP(A849,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT508d","Specific GHG emissions related to fuel use - transport mode 4",{"$f":"VLOOKUP(A850,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT508e","Specific GHG emissions related to fuel use - transport mode 5",{"$f":"VLOOKUP(A851,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT508f","Specific GHG emissions related to fuel use - transport mode 6",{"$f":"VLOOKUP(A852,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT508g","Specific GHG emissions related to fuel use - transport mode 7",{"$f":"VLOOKUP(A853,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT508h","Specific GHG emissions related to fuel use - transport mode 8",{"$f":"VLOOKUP(A854,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT508i","Specific GHG emissions related to fuel use - transport mode 9",{"$f":"VLOOKUP(A855,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/MJfuel"}]
["FT509a","Fossil energy use for transport mode 1",{"$f":"VLOOKUP(A856,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT509b","Fossil energy use for transport mode 2",{"$f":"VLOOKUP(A857,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT509c","Fossil energy use for transport mode 3",{"$f":"VLOOKUP(A858,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT509d","Fossil energy use for transport mode 4",{"$f":"VLOOKUP(A859,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT509e","Fossil energy use for transport mode 5",{"$f":"VLOOKUP(A860,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT509f","Fossil energy use for transport mode 6",{"$f":"VLOOKUP(A861,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT509g","Fossil energy use for transport mode 7",{"$f":"VLOOKUP(A862,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT509h","Fossil energy use for transport mode 8",{"$f":"VLOOKUP(A863,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT509i","Fossil energy use for transport mode 9",{"$f":"VLOOKUP(A864,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/ha"}]
["FT510a","Primary energy use for transport mode 1",{"$f":"VLOOKUP(A865,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT510b","Primary energy use for transport mode 2",{"$f":"VLOOKUP(A866,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT510c","Primary energy use for transport mode 3",{"$f":"VLOOKUP(A867,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT510d","Primary energy use for transport mode 4",{"$f":"VLOOKUP(A868,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT510e","Primary energy use for transport mode 5",{"$f":"VLOOKUP(A869,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT510f","Primary energy use for transport mode 6",{"$f":"VLOOKUP(A870,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT510g","Primary energy use for transport mode 7",{"$f":"VLOOKUP(A871,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT510h","Primary energy use for transport mode 8",{"$f":"VLOOKUP(A872,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT510i","Primary energy use for transport mode 9",{"$f":"VLOOKUP(A873,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/ha"}]
["FT511a","GHG emissions of fuel used in transport mode 1",{"$f":"VLOOKUP(A874,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT511b","GHG emissions of fuel used in transport mode 2",{"$f":"VLOOKUP(A875,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT511c","GHG emissions of fuel used in transport mode 3",{"$f":"VLOOKUP(A876,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT511d","GHG emissions of fuel used in transport mode 4",{"$f":"VLOOKUP(A877,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT511e","GHG emissions of fuel used in transport mode 5",{"$f":"VLOOKUP(A878,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT511f","GHG emissions of fuel used in transport mode 6",{"$f":"VLOOKUP(A879,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT511g","GHG emissions of fuel used in transport mode 7",{"$f":"VLOOKUP(A880,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT511h","GHG emissions of fuel used in transport mode 8",{"$f":"VLOOKUP(A881,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT511i","GHG emissions of fuel used in transport mode 9",{"$f":"VLOOKUP(A882,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2-eq/ha"}]
["FT512a","Fossil energy use for transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A883,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["FT512b","Primary energy use for transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A884,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["FT513a","Fossil energy use for transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A885,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["FT513b","Primary energy use for transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A886,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["FT514a","Fossil energy use for transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A887,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["FT514b","Primary energy use for transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A888,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["FT515a","GHG emissions associated with transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A889,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FT515b","GHG emissions associated with transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A890,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FT515c","GHG emissions associated with transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A891,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FT516a","Acidification potential associated with transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A892,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FT516b","Acidification potential associated with transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A893,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FT516c","Acidification potential associated with transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A894,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FT517a","Eutrophication potential associated with transport 1 (mode 1-2-3)",{"$f":"VLOOKUP(A895,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FT517b","Eutrophication potential associated with transport 2 (mode 4-5-6)",{"$f":"VLOOKUP(A896,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FT517c","Eutrophication potential associated with transport 3 (mode 7-8-9)",{"$f":"VLOOKUP(A897,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FT520a","Totally allocated fossil energy requirement in transport 1",{"$f":"VLOOKUP(A898,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT520b","Totally allocated primary energy requirement in transport 1",{"$f":"VLOOKUP(A899,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT521a","Totally allocated fossil energy requirement in transport 1",{"$f":"VLOOKUP(A900,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJFU"}]
["FT521b","Totally allocated primary energy requirement in transport 1",{"$f":"VLOOKUP(A901,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJFU"}]
["FT522a","Totally allocated fossil energy requirement in transport 2",{"$f":"VLOOKUP(A902,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT522b","Totally allocated primary energy requirement in transport 2",{"$f":"VLOOKUP(A903,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT523a","Totally allocated fossil energy requirement in transport 2",{"$f":"VLOOKUP(A904,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJFU"}]
["FT523b","Totally allocated primary energy requirement in transport 2",{"$f":"VLOOKUP(A905,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJFU"}]
["FT524a","Totally allocated fossil energy requirement in transport 3",{"$f":"VLOOKUP(A906,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT524b","Totally allocated primary energy requirement in transport 3",{"$f":"VLOOKUP(A907,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT525a","Totally allocated fossil energy requirement in transport 3",{"$f":"VLOOKUP(A908,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJFU"}]
["FT525b","Totally allocated primary energy requirement in transport 3",{"$f":"VLOOKUP(A909,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJFU"}]
["FT526a","Totally allocated fossil energy requirement in total transport (1-3)",{"$f":"VLOOKUP(A910,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["FT526b","Totally allocated primary energy requirement in total transport (1-3)",{"$f":"VLOOKUP(A911,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["FT527a","Totally allocated fossil energy requirement in total transport (1-3)",{"$f":"VLOOKUP(A912,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJfossil/MJFU"}]
["FT527b","Totally allocated primary energy requirement in total transport (1-3)",{"$f":"VLOOKUP(A913,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"MJprim/MJFU"}]
["FT530a","Totally allocated GHG emissions from transport 1",{"$f":"VLOOKUP(A914,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FT530b","Totally allocated GHG emissions from transport 1",{"$f":"VLOOKUP(A915,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FT531a","Totally allocated GHG emissions from transport 2",{"$f":"VLOOKUP(A916,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FT531b","Totally allocated GHG emissions from transport 2",{"$f":"VLOOKUP(A917,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FT532a","Totally allocated GHG emissions from transport 3",{"$f":"VLOOKUP(A918,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FT532b","Totally allocated GHG emissions from transport 3",{"$f":"VLOOKUP(A919,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FT533a","Totally allocated GHG emissions from total transport (1-3)",{"$f":"VLOOKUP(A920,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["FT533b","Totally allocated GHG emissions from total transport (1-3)",{"$f":"VLOOKUP(A921,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FT535a","Acidification potential related to fuel used in transport mode 1",{"$f":"VLOOKUP(A922,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT535b","Acidification potential related to fuel used in transport mode 2",{"$f":"VLOOKUP(A923,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT535c","Acidification potential related to fuel used in transport mode 3",{"$f":"VLOOKUP(A924,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT535d","Acidification potential related to fuel used in transport mode 4",{"$f":"VLOOKUP(A925,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT535e","Acidification potential related to fuel used in transport mode 5",{"$f":"VLOOKUP(A926,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT535f","Acidification potential related to fuel used in transport mode 6",{"$f":"VLOOKUP(A927,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT535g","Acidification potential related to fuel used in transport mode 7",{"$f":"VLOOKUP(A928,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT535h","Acidification potential related to fuel used in transport mode 8",{"$f":"VLOOKUP(A929,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT535i","Acidification potential related to fuel used in transport mode 9",{"$f":"VLOOKUP(A930,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2-eq/ha"}]
["FT536a","Eutrophication potential related to fuel used in transport mode 1",{"$f":"VLOOKUP(A931,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT536b","Eutrophication potential related to fuel used in transport mode 2",{"$f":"VLOOKUP(A932,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT536c","Eutrophication potential related to fuel used in transport mode 3",{"$f":"VLOOKUP(A933,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT536d","Eutrophication potential related to fuel used in transport mode 4",{"$f":"VLOOKUP(A934,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT536e","Eutrophication potential related to fuel used in transport mode 5",{"$f":"VLOOKUP(A935,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT536f","Eutrophication potential related to fuel used in transport mode 6",{"$f":"VLOOKUP(A936,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT536g","Eutrophication potential related to fuel used in transport mode 7",{"$f":"VLOOKUP(A937,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT536h","Eutrophication potential related to fuel used in transport mode 8",{"$f":"VLOOKUP(A938,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT536i","Eutrophication potential related to fuel used in transport mode 9",{"$f":"VLOOKUP(A939,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4-eq/ha"}]
["FT537a","NOx emissions factor of fuel - transport mode 1",{"$f":"VLOOKUP(A940,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT537b","NOx emissions factor of fuel - transport mode 2",{"$f":"VLOOKUP(A941,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT537c","NOx emissions factor of fuel - transport mode 3",{"$f":"VLOOKUP(A942,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT537d","NOx emissions factor of fuel - transport mode 4",{"$f":"VLOOKUP(A943,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT537e","NOx emissions factor of fuel - transport mode 5",{"$f":"VLOOKUP(A944,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT537f","NOx emissions factor of fuel - transport mode 6",{"$f":"VLOOKUP(A945,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT537g","NOx emissions factor of fuel - transport mode 7",{"$f":"VLOOKUP(A946,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT537h","NOx emissions factor of fuel - transport mode 8",{"$f":"VLOOKUP(A947,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT537i","NOx emissions factor of fuel - transport mode 9",{"$f":"VLOOKUP(A948,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gNOX/MJfuel"}]
["FT538a","SOx emissions factor of fuel - transport mode 1",{"$f":"VLOOKUP(A949,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT538b","SOx emissions factor of fuel - transport mode 2",{"$f":"VLOOKUP(A950,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT538c","SOx emissions factor of fuel - transport mode 3",{"$f":"VLOOKUP(A951,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT538d","SOx emissions factor of fuel - transport mode 4",{"$f":"VLOOKUP(A952,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT538e","SOx emissions factor of fuel - transport mode 5",{"$f":"VLOOKUP(A953,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT538f","SOx emissions factor of fuel - transport mode 6",{"$f":"VLOOKUP(A954,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT538g","SOx emissions factor of fuel - transport mode 7",{"$f":"VLOOKUP(A955,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT538h","SOx emissions factor of fuel - transport mode 8",{"$f":"VLOOKUP(A956,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT538i","SOx emissions factor of fuel - transport mode 9",{"$f":"VLOOKUP(A957,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSOX/MJfuel"}]
["FT540a","Totally allocated acidification potential from transport 1",{"$f":"VLOOKUP(A958,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FT540b","Totally allocated acidification potential from transport 1",{"$f":"VLOOKUP(A959,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FT541a","Totally allocated acidification potential from transport 2",{"$f":"VLOOKUP(A960,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FT541b","Totally allocated acidification potential from transport 2",{"$f":"VLOOKUP(A961,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FT542a","Totally allocated acidification potential from transport 3",{"$f":"VLOOKUP(A962,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FT542b","Totally allocated acidification potential from transport 3",{"$f":"VLOOKUP(A963,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FT543a","Totally allocated acidification potential from total transport (1-3)",{"$f":"VLOOKUP(A964,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["FT543b","Totally allocated acidification potential from total transport (1-3)",{"$f":"VLOOKUP(A965,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FT544a","Totally allocated eutrophication potential from transport 1",{"$f":"VLOOKUP(A966,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FT544b","Totally allocated eutrophication potential from transport 1",{"$f":"VLOOKUP(A967,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJFU"}]
["FT545a","Totally allocated eutrophication potential from transport 2",{"$f":"VLOOKUP(A968,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FT545b","Totally allocated eutrophication potential from transport 2",{"$f":"VLOOKUP(A969,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJFU"}]
["FT546a","Totally allocated eutrophication potential from transport 3",{"$f":"VLOOKUP(A970,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FT546b","Totally allocated eutrophication potential from transport 3",{"$f":"VLOOKUP(A971,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJFU"}]
["FT547a","Totally allocated eutrophication potential from total transport (1-3)",{"$f":"VLOOKUP(A972,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["FT547b","Totally allocated eutrophication potential from total transport (1-3)",{"$f":"VLOOKUP(A973,'Transport feedstock2'!D$10:E$663,2,FALSE)","v":"gPO4_eq/MJFU"}]
[]
["Biomass conversion feedstock 1"]
["BC000a","Process 1 description ",{"$f":"VLOOKUP(A976,'Conversion feedstock1'!D$9:E$785,2,FALSE)","v":"-"}]
["BC000b","Process 2 description ",{"$f":"VLOOKUP(A977,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC001a","Type of main output flow, process 1",{"$f":"VLOOKUP(A978,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC001b","Type of main output flow, process 2",{"$f":"VLOOKUP(A979,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC002a1","Type of by-product 1, process 1",{"$f":"VLOOKUP(A980,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC002a10","Moisture content of by-product 1, process 1",{"$f":"VLOOKUP(A981,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC002a11","By-product flow 1, process 1",{"$f":"VLOOKUP(A982,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC002a2","Type of by-product 2, process 1",{"$f":"VLOOKUP(A983,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC002a20","Moisture content of by-product 2, process 1",{"$f":"VLOOKUP(A984,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC002a21","By-product flow 2, process 1",{"$f":"VLOOKUP(A985,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC002a3","Type of by-product 3, process 1",{"$f":"VLOOKUP(A986,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC002a30","Moisture content of by-product 3, process 1",{"$f":"VLOOKUP(A987,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC002a31","By-product flow 3, process 1",{"$f":"VLOOKUP(A988,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC002a41","Electricity by-product, process 1",{"$f":"VLOOKUP(A989,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MWh/year"}]
["BC002a51","Heat by-product, process 1",{"$f":"VLOOKUP(A990,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/year"}]
["BC002b1","Type of by-product 1, process 2",{"$f":"VLOOKUP(A991,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC002b10","Moisture content of by-product 1, process 2",{"$f":"VLOOKUP(A992,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC002b11","By-product flow 1, process 2",{"$f":"VLOOKUP(A993,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC002b2","Type of by-product 2, process 2",{"$f":"VLOOKUP(A994,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC002b20","Moisture content of by-product 2, process 2",{"$f":"VLOOKUP(A995,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC002b21","By-product flow 2, process 2",{"$f":"VLOOKUP(A996,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC002b41","Electricity by-product, process 2",{"$f":"VLOOKUP(A997,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MWh/year"}]
["BC002b51","Heat by-product, process 2",{"$f":"VLOOKUP(A998,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/year"}]
["BC003a1","Extraction rate of by-product 1, process 1 (kg)",{"$f":"VLOOKUP(A999,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC003a2","Extraction rate of by-product 2, process 1 (kg)",{"$f":"VLOOKUP(A1000,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC003a3","Extraction rate of by-product 3, process 1 (kg)",{"$f":"VLOOKUP(A1001,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC003b1","Extraction rate of by-product 1, process 2 (kg)",{"$f":"VLOOKUP(A1002,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC003b2","Extraction rate of by-product 2, process 2 (kg)",{"$f":"VLOOKUP(A1003,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC004a1","Extraction rate of by-product 1, process 1 (MJ)",{"$f":"VLOOKUP(A1004,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC004a2","Extraction rate of by-product 2, process 1 (MJ)",{"$f":"VLOOKUP(A1005,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC004a3","Extraction rate of by-product 3, process 1 (MJ)",{"$f":"VLOOKUP(A1006,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC004a4","Extraction rate of electricity by-product, process 1 (MJ)",{"$f":"VLOOKUP(A1007,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC004a5","Extraction rate of heat by-product, process 1 (MJ)",{"$f":"VLOOKUP(A1008,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC004b1","Extraction rate of by-product 1, process 2 (MJ)",{"$f":"VLOOKUP(A1009,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC004b2","Extraction rate of by-product 2, process 2 (MJ)",{"$f":"VLOOKUP(A1010,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC004b4","Extraction rate of electricity by-product, process 2 (MJ)",{"$f":"VLOOKUP(A1011,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC004b5","Extraction rate of heat by-product, process 2 (MJ)",{"$f":"VLOOKUP(A1012,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC005a1","Energy content of by-product 1, process 1 (LHV)",{"$f":"VLOOKUP(A1013,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC005a2","Energy content of by-product 2, process 1 (LHV)",{"$f":"VLOOKUP(A1014,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC005a3","Energy content of by-product 3, process 1 (LHV)",{"$f":"VLOOKUP(A1015,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC005b1","Energy content of by-product 1, process 2 (LHV)",{"$f":"VLOOKUP(A1016,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC005b2","Energy content of by-product 2, process 2 (LHV)",{"$f":"VLOOKUP(A1017,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC006a1","Valorisation of by-product 1, process 1",{"$f":"VLOOKUP(A1018,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC006a2","Valorisation of by-product 2, process 1",{"$f":"VLOOKUP(A1019,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC006a3","Valorisation of by-product 3, process 1",{"$f":"VLOOKUP(A1020,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC006a4","Valorisation of electricity by-product, process 1",{"$f":"VLOOKUP(A1021,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC006a5","Valorisation of heat by-product, process 1",{"$f":"VLOOKUP(A1022,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC006b1","Valorisation of by-product 1, process 2",{"$f":"VLOOKUP(A1023,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC006b2","Valorisation of by-product 2, process 2",{"$f":"VLOOKUP(A1024,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC006b4","Valorisation of electricity by-product, process 2",{"$f":"VLOOKUP(A1025,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC006b5","Valorisation of heat by-product, process 2",{"$f":"VLOOKUP(A1026,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"binary"}]
["BC007a","Energy content of main output flow, process 1 (LHV)",{"$f":"VLOOKUP(A1027,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC007b","Energy content of main output flow, process 2 (LHV)",{"$f":"VLOOKUP(A1028,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC008a","Extraction rate (output/input), process 1",{"$f":"VLOOKUP(A1029,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJoutput /MJinput"}]
["BC008b","Extraction rate (output/input), process 2",{"$f":"VLOOKUP(A1030,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJoutput /MJinput"}]
["BC009a0","Type of main input, process 1",{"$f":"VLOOKUP(A1031,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009a1","Type of material input flow 1, process 1",{"$f":"VLOOKUP(A1032,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009a2","Type of material input flow 2, process 1",{"$f":"VLOOKUP(A1033,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009a3","Type of material input flow 3, process 1",{"$f":"VLOOKUP(A1034,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009b1","Type of material input flow 1, process 2",{"$f":"VLOOKUP(A1035,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009b2","Type of material input flow 2, process 2",{"$f":"VLOOKUP(A1036,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009c","Type of material output flow, process 1",{"$f":"VLOOKUP(A1037,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009c1","Type of output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1038,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009c2","Type of output flow, process 1 (heat)",{"$f":"VLOOKUP(A1039,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009d","Type of material output flow, process 2",{"$f":"VLOOKUP(A1040,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009d1","Type of output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1041,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC009d2","Type of output flow, process 2 (heat)",{"$f":"VLOOKUP(A1042,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC010a0","Main input, process 1",{"$f":"VLOOKUP(A1043,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC010a01","Material input flow 1, process 1",{"$f":"VLOOKUP(A1044,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC010a","Amount of main input, process 1",{"$f":"VLOOKUP(A1045,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgdm/MJoutput"}]
["BC010a1","Amount of material input flow 1, process 1",{"$f":"VLOOKUP(A1046,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgdm/MJoutput"}]
["BC010a10","Moisture content of material input flow 1, process 1",{"$f":"VLOOKUP(A1047,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC010a11","Energy content of input flow 1, process 1",{"$f":"VLOOKUP(A1048,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC010a02","Material input flow 2, process 1",{"$f":"VLOOKUP(A1049,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC010a2","Amount of material input flow 2, process 1",{"$f":"VLOOKUP(A1050,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgdm/MJoutput"}]
["BC010a20","Moisture content of material input flow 2, process 1",{"$f":"VLOOKUP(A1051,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC010a21","Energy content of input flow 2, process 1",{"$f":"VLOOKUP(A1052,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC010a03","Material input flow 3, process 1",{"$f":"VLOOKUP(A1053,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC010a3","Amount of material input flow 3, process 1",{"$f":"VLOOKUP(A1054,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgdm/MJoutput"}]
["BC010a30","Moisture content of material input flow 3, process 1",{"$f":"VLOOKUP(A1055,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC010a31","Energy content of input flow 3, process 1",{"$f":"VLOOKUP(A1056,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC010b1","Amount of material input flow 1, process 2",{"$f":"VLOOKUP(A1057,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/MJoutput"}]
["BC010b10","Material input flow 1, process 2",{"$f":"VLOOKUP(A1058,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC010b11","Moisture content of material input flow 1, process 2",{"$f":"VLOOKUP(A1059,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC010b12","Energy content of input flow 1, process 2",{"$f":"VLOOKUP(A1060,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC010b2","Amount of material input flow 2, process 2",{"$f":"VLOOKUP(A1061,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/MJoutput"}]
["BC010b20","Material input flow 2, process 2",{"$f":"VLOOKUP(A1062,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC010b21","Moisture content of material input flow 2, process 2",{"$f":"VLOOKUP(A1063,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC010b22","Energy content of input flow 2, process 2",{"$f":"VLOOKUP(A1064,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/kgdm"}]
["BC010c","Amount of material output flow, process 1",{"$f":"VLOOKUP(A1065,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgdm/MJoutput"}]
["BC010c0","Material output flow, process 1",{"$f":"VLOOKUP(A1066,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC010c1","Amount of material output flow, process 1 (Electricity)",{"$f":"VLOOKUP(A1067,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJe/MJoutput"}]
["BC010c2","Amount of material output flow, process 1 (Heat)",{"$f":"VLOOKUP(A1068,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC010d","Amount of material output flow, process 2",{"$f":"VLOOKUP(A1069,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgdm/MJoutput"}]
["BC010d0","Material output flow, process 2",{"$f":"VLOOKUP(A1070,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/year"}]
["BC010d1","Amount of material output flow, process 2 (Electricity)",{"$f":"VLOOKUP(A1071,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJe/MJoutput"}]
["BC010d2","Amount of material output flow, process 2 (Heat)",{"$f":"VLOOKUP(A1072,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC011a1","Type of fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1073,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC011a2","Type of fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1074,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC011b1","Type of fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1075,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC011b2","Type of fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1076,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC012a","Moisture content of main output flow, process 1",{"$f":"VLOOKUP(A1077,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC012b","Moisture content of main output flow, process 2",{"$f":"VLOOKUP(A1078,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC014a","Yield rate (moist/wet) of feedstock 1 per ha after conversion process 1",{"$f":"VLOOKUP(A1079,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/ha"}]
["BC014b","Yield rate (dry) of feedstock 1 per ha after conversion process 1",{"$f":"VLOOKUP(A1080,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgdm/ha"}]
["BC014c","Yield rate (energy) of feedstock 1 per ha after conversion process 1",{"$f":"VLOOKUP(A1081,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/ha"}]
["BC015a","Yield rate (moist/wet) of feedstock 1 per ha after conversion process 2",{"$f":"VLOOKUP(A1082,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kg/ha"}]
["BC015b","Yield rate (dry) of feedstock 1 per ha after conversion process 2",{"$f":"VLOOKUP(A1083,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"kgdm/ha"}]
["BC015c","Yield rate (energy) of feedstock 1 per ha after conversion process 2",{"$f":"VLOOKUP(A1084,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/ha"}]
["BC016a","NOX emissions to air (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1085,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJoutput"}]
["BC016b","SOX emissions to air (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1086,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJoutput"}]
["BC016c","NH3 emissions to air (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1087,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNH3/MJoutput"}]
["BC016d","NO3- emissions to water (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1088,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNO3/MJoutput"}]
["BC016e","NH4+ emissions to water (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1089,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNH4/MJoutput"}]
["BC016f","PO43- emissions to water (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1090,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4/MJoutput"}]
["BC016g","COD emissions to water (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1091,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCOD/MJoutput"}]
["BC017a","NOX emissions to air (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1092,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJoutput"}]
["BC017b","SOX emissions to air (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1093,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJoutput"}]
["BC017c","NH3 emissions to air (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1094,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNH3/MJoutput"}]
["BC017d","NO3- emissions to water (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1095,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNO3/MJoutput"}]
["BC017e","NH4+ emissions to water (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1096,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNH4/MJoutput"}]
["BC017f","PO43- emissions to water (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1097,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4/MJoutput"}]
["BC017g","COD emissions to water (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1098,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCOD/MJoutput"}]
["BC019a","Total allocated fossil energy use for processing (process 1+2)",{"$f":"VLOOKUP(A1099,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":{"$error":"#N/A"}}]
["BC019b","Total allocated primary energy use for processing (process 1+2)",{"$f":"VLOOKUP(A1100,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":{"$error":"#N/A"}}]
["BC020a","Fossil energy use in process 1",{"$f":"VLOOKUP(A1101,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC020b","Fossil energy use in process 2",{"$f":"VLOOKUP(A1102,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC021a","Primary energy use in process 1",{"$f":"VLOOKUP(A1103,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC021b","Primary energy use in process 2",{"$f":"VLOOKUP(A1104,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC022a","Allocation to by-products, process 1",{"$f":"VLOOKUP(A1105,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC022b","Allocation to by-products, process 2",{"$f":"VLOOKUP(A1106,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC024a","Fossil energy use related to electricity input, process 1",{"$f":"VLOOKUP(A1107,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC024b","Fossil energy use related to electricity input, process 2",{"$f":"VLOOKUP(A1108,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC025a","Primary energy use related to electricity input, process 1",{"$f":"VLOOKUP(A1109,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJoutput"}]
["BC025b","Primary energy use related to electricity input, process 2",{"$f":"VLOOKUP(A1110,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJoutput"}]
["BC026a","Amount of electricity input 1, process 1",{"$f":"VLOOKUP(A1111,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJe/MJoutput"}]
["BC026a0","Electricity flow 1, process 1",{"$f":"VLOOKUP(A1112,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MWh/year"}]
["BC026a1","Amount of electricity input 2, process 1",{"$f":"VLOOKUP(A1113,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJe/MJoutput"}]
["BC026a10","Electricity flow 2, process 1",{"$f":"VLOOKUP(A1114,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MWh/year"}]
["BC026b","Amount of electricity input 1, process 2",{"$f":"VLOOKUP(A1115,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJe/MJoutput"}]
["BC026b0","Electricity flow 1, process 2",{"$f":"VLOOKUP(A1116,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MWh/year"}]
["BC026b1","Amount of electricity input 2, process 2",{"$f":"VLOOKUP(A1117,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJe/MJoutput"}]
["BC026b10","Electricity flow 2, process 2",{"$f":"VLOOKUP(A1118,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MWh/year"}]
["BC027a","Type of electricity flow 1, process 1",{"$f":"VLOOKUP(A1119,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC027a1","Type of electricity flow 2, process 1",{"$f":"VLOOKUP(A1120,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC027b","Type of electricity flow 1, process 2",{"$f":"VLOOKUP(A1121,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC027b1","Type of electricity flow 2, process 2",{"$f":"VLOOKUP(A1122,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC028a","Specific fossil energy used for external electricity production flow 1, process 1",{"$f":"VLOOKUP(A1123,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJe"}]
["BC028a1","Specific fossil energy used for external electricity production flow 2, process 1",{"$f":"VLOOKUP(A1124,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJe"}]
["BC028b","Specific fossil energy used for external electricity production flow 1, process 2",{"$f":"VLOOKUP(A1125,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJe"}]
["BC028b1","Specific fossil energy used for external electricity production flow 2, process 2",{"$f":"VLOOKUP(A1126,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJe"}]
["BC029a","Specific primary energy used for external electricity production flow 1, process 1",{"$f":"VLOOKUP(A1127,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJe"}]
["BC029a1","Specific primary energy used for external electricity production flow 2, process 1",{"$f":"VLOOKUP(A1128,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJe"}]
["BC029b","Specific primary energy used for external electricity production flow 1, process 2",{"$f":"VLOOKUP(A1129,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJe"}]
["BC029b1","Specific primary energy used for external electricity production flow 2, process 2",{"$f":"VLOOKUP(A1130,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJe"}]
["BC030a","Fossil energy use related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1131,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC030b","Fossil energy use related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1132,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC031a1","Amount of fuel/heat input 1, process 1",{"$f":"VLOOKUP(A1133,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC031a10","Fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1134,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/year"}]
["BC031a2","Amount of fuel/heat input 2, process 1",{"$f":"VLOOKUP(A1135,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC031a20","Fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1136,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/year"}]
["BC031b1","Amount of fuel/heat input 1, process 2",{"$f":"VLOOKUP(A1137,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC031b10","Fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1138,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/year"}]
["BC031b2","Amount of fuel/heat input 2, process 2",{"$f":"VLOOKUP(A1139,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC031b20","Fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1140,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJ/year"}]
["BC032a1","Specific fossil energy for fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1141,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC032a2","Specific fossil energy for fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1142,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC032b1","Specific fossil energy for fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1143,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC032b2","Specific fossil energy for fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1144,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC033a1","Specific primary energy for fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1145,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJf_h"}]
["BC033a2","Specific primary energy for fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1146,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJf_h"}]
["BC033b1","Specific primary energy for fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1147,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJf_h"}]
["BC033b2","Specific primary energy for fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1148,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJf_h"}]
["BC034a","Primary energy use related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1149,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJoutput"}]
["BC034b","Primary energy use related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1150,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJoutput"}]
["BC035a","Fossil energy use related to material input flows, process 1",{"$f":"VLOOKUP(A1151,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC035a1","Specific fossil energy for material input flow 1, process 1",{"$f":"VLOOKUP(A1152,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/kgdm"}]
["BC035a2","Specific fossil energy for material input flow 2, process 1",{"$f":"VLOOKUP(A1153,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/kgdm"}]
["BC035a3","Specific fossil energy for material input flow 3, process 1",{"$f":"VLOOKUP(A1154,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/kgdm"}]
["BC035b","Fossil energy use related to material input flows, process 2",{"$f":"VLOOKUP(A1155,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC035b1","Specific fossil energy for material input flow 1, process 2",{"$f":"VLOOKUP(A1156,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/kg"}]
["BC035b2","Specific fossil energy for material input flow 2, process 2",{"$f":"VLOOKUP(A1157,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/kg"}]
["BC035c","Specific fossil energy for material output flow, process 1",{"$f":"VLOOKUP(A1158,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/kgdm"}]
["BC035c1","Specific fossil energy for  output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1159,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJe"}]
["BC035c2","Specific fossil energy for  output flow, process 1 (heat)",{"$f":"VLOOKUP(A1160,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC035d","Specific fossil energy for material output flow, process 2",{"$f":"VLOOKUP(A1161,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/kgdm"}]
["BC035d1","Specific fossil energy for  output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1162,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJe"}]
["BC035d2","Specific fossil energy for  output flow, process 2 (heat)",{"$f":"VLOOKUP(A1163,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC036a","Primary energy use related to material input flows, process 1",{"$f":"VLOOKUP(A1164,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJoutput"}]
["BC036a0","Specific primary energy for main input, process 1",{"$f":"VLOOKUP(A1165,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/kgdm"}]
["BC036a1","Specific primary energy for material input flow 1, process 1",{"$f":"VLOOKUP(A1166,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/kgdm"}]
["BC036a2","Specific primary energy for material input flow 2, process 1",{"$f":"VLOOKUP(A1167,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/kgdm"}]
["BC036a3","Specific primary energy for material input flow 3, process 1",{"$f":"VLOOKUP(A1168,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/kgdm"}]
["BC036b","Primary energy use related to material input flows, process 2",{"$f":"VLOOKUP(A1169,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJoutput"}]
["BC036b1","Specific primary energy for material input flow 1, process 2",{"$f":"VLOOKUP(A1170,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/kg"}]
["BC036b2","Specific primary energy for material input flow 2, process 2",{"$f":"VLOOKUP(A1171,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/kg"}]
["BC036c","Specific primary energy for material output flow, process 1",{"$f":"VLOOKUP(A1172,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/kgdm"}]
["BC036c1","Specific primary energy for  output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1173,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJe"}]
["BC036c2","Specific primary energy for  output flow, process 1 (heat)",{"$f":"VLOOKUP(A1174,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJf_h"}]
["BC036d","Specific primary energy for material output flow, process 2",{"$f":"VLOOKUP(A1175,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/kgdm"}]
["BC036d1","Specific primary energy for output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1176,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJe"}]
["BC036d2","Specific primary energy for output flow, process 2 (heat)",{"$f":"VLOOKUP(A1177,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJf_h"}]
["BC037a","GHG emissions related to process 1",{"$f":"VLOOKUP(A1178,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC037b","GHG emissions related to process 2",{"$f":"VLOOKUP(A1179,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC041a","GHG emissions related to electricity input, process 1",{"$f":"VLOOKUP(A1180,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC041b","GHG emissions related to electricity input, process 2",{"$f":"VLOOKUP(A1181,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC042a","Specific GHG emissions for external electricity production flow 1, process 1",{"$f":"VLOOKUP(A1182,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJe"}]
["BC042a1","Specific GHG emissions for external electricity production flow 2, process 1",{"$f":"VLOOKUP(A1183,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJe"}]
["BC042b","Specific GHG emissions for external electricity production flow 1, process 2",{"$f":"VLOOKUP(A1184,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJe"}]
["BC042b1","Specific GHG emissions for external electricity production flow 2, process 2",{"$f":"VLOOKUP(A1185,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJe"}]
["BC043a","GHG emissions related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1186,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC043a1","Specific GHG emissions related to fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1187,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC043a2","Specific GHG emissions related to fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1188,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC043b","GHG emissions related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1189,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC043b1","Specific GHG emissions related to fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1190,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC043b2","Specific GHG emissions related to fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1191,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC047a","GHG emissions related to material input flows, process 1",{"$f":"VLOOKUP(A1192,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC047a1","Specific GHG emissions related to material input flow 1, process 1",{"$f":"VLOOKUP(A1193,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/kgdm"}]
["BC047a2","Specific GHG emissions related to material input flow 2, process 1",{"$f":"VLOOKUP(A1194,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/kgdm"}]
["BC047a3","Specific GHG emissions related to material input flow 3, process 1",{"$f":"VLOOKUP(A1195,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/kgdm"}]
["BC047b","GHG emissions related to material input flows, process 2",{"$f":"VLOOKUP(A1196,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC047b1","Specific GHG emissions related to material input flow 1, process 2",{"$f":"VLOOKUP(A1197,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/kg"}]
["BC047b2","Specific GHG emissions related to material input flow 2, process 2",{"$f":"VLOOKUP(A1198,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/kg"}]
["BC047c","Specific GHG emissions related to material output flow, process 1",{"$f":"VLOOKUP(A1199,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/kgdm"}]
["BC047c1","Specific GHG emissions related to  output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1200,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJe"}]
["BC047c2","Specific GHG emissions related to  output flow, process 1 (heat)",{"$f":"VLOOKUP(A1201,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC047d","Specific GHG emissions related to material output flow, process 2",{"$f":"VLOOKUP(A1202,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/kgdm"}]
["BC047d1","Specific GHG emissions related to  output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1203,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJe"}]
["BC047d2","Specific GHG emissions related to  output flow, process 2 (heat)",{"$f":"VLOOKUP(A1204,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC050a","Allocation to energy crop, process 1",{"$f":"VLOOKUP(A1205,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC050b","Allocation to energy crop, process 2",{"$f":"VLOOKUP(A1206,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051a1","Allocation to by-product 1, process 1",{"$f":"VLOOKUP(A1207,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051a2","Allocation to by-product 2, process 1",{"$f":"VLOOKUP(A1208,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051a3","Allocation to by-product 3, process 1",{"$f":"VLOOKUP(A1209,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051a4","Allocation to electricity by-product, process 1",{"$f":"VLOOKUP(A1210,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051a5","Allocation to heat by-product, process 1",{"$f":"VLOOKUP(A1211,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051b1","Allocation to by-product 1, process 2",{"$f":"VLOOKUP(A1212,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051b2","Allocation to by-product 2, process 2",{"$f":"VLOOKUP(A1213,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051b4","Allocation to electricity by-product, process 2",{"$f":"VLOOKUP(A1214,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC051b5","Allocation to heat by-product, process 2",{"$f":"VLOOKUP(A1215,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"%"}]
["BC059a","Fossil energy use for treatment 2 (storage)",{"$f":"VLOOKUP(A1216,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC059b","Primary energy use for treatment 2 (storage)",{"$f":"VLOOKUP(A1217,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC059c","GHG emissions associated with treatment 2 (storage)",{"$f":"VLOOKUP(A1218,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC059d","Acidification potential related to treatment 2 (storage)",{"$f":"VLOOKUP(A1219,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC059e","Eutrophication potential related to treatment 2 (storage)",{"$f":"VLOOKUP(A1220,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC060","Heat energy use for treatment 2 (storage)",{"$f":"VLOOKUP(A1221,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJh/MJinput"}]
["BC061","Heat source for treatment 2 (storage)",{"$f":"VLOOKUP(A1222,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC062a","Specific fossil energy use for heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1223,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJh"}]
["BC062b","Specific primary energy use for heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1224,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJh"}]
["BC062c","Specific GHG emissions related to heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1225,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJh"}]
["BC062d","Specific NOx emissions related to heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1226,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOx/MJh"}]
["BC062e","Specific SOx emissions related to heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1227,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOx/MJh"}]
["BC065","Electricity energy use for treatment 2 (storage)",{"$f":"VLOOKUP(A1228,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJe/MJinput"}]
["BC066","Electricity source for treatment 2 (storage)",{"$f":"VLOOKUP(A1229,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC067a","Specific fossil energy use for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1230,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJe"}]
["BC067b","Specific primary energy use for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1231,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJe"}]
["BC067c","Specific GHG emissions for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1232,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJe"}]
["BC067d","Specific NOx emissions for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1233,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOx/MJe"}]
["BC067e","Specific SOx emissions for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1234,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOx/MJe"}]
["BC069a","Fossil energy use for treatment 3 (storage)",{"$f":"VLOOKUP(A1235,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC069b","Primary energy use for treatment 3 (storage)",{"$f":"VLOOKUP(A1236,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC069c","GHG emissions associated with treatment 3 (storage)",{"$f":"VLOOKUP(A1237,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC069d","Acidification potential associated with treatment 3 (storage)",{"$f":"VLOOKUP(A1238,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC069e","Eutrophication potential associated with treatment 3 (storage)",{"$f":"VLOOKUP(A1239,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC070","Heat energy use for treatment 3 (storage)",{"$f":"VLOOKUP(A1240,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJh/MJinput"}]
["BC071","Heat source for treatment 3 (storage)",{"$f":"VLOOKUP(A1241,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC072a","Specific fossil energy use for heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1242,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJh"}]
["BC072b","Specific primary energy use for heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1243,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJh"}]
["BC072c","Specific GHG emissions related to heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1244,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJh"}]
["BC072d","Specific NOx emissions related to heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1245,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJh"}]
["BC072e","Specific SOx emissions related to heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1246,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJh"}]
["BC075","Electricity energy use for treatment 3 (storage)",{"$f":"VLOOKUP(A1247,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJe/MJinput"}]
["BC076","Electricity source for treatment 3 (storage)",{"$f":"VLOOKUP(A1248,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC077a","Specific fossil energy use for electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1249,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJe"}]
["BC077b","Specific primary energy use for electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1250,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJe"}]
["BC077c","Specific GHG emissions related to electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1251,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2eq/MJe"}]
["BC077d","Specific NOx emissions related to electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1252,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJe"}]
["BC077e","Specific SOx emissions related to electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1253,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJe"}]
["BC080a","Allocated fossil energy use after conversion 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1254,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC080b","Allocated primary energy use after conversion 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1255,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC080c","Allocated GHG emissions after conversion 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1256,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC080d","Allocated water use after conversion 1 (per GJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1257,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC080f","Allocated acidification potential after conversion 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1258,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC080g","Allocated eutrophication potential after conversion 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1259,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC081a","Allocated fossil energy use after conversion 2 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1260,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC081b","Allocated primary energy use after conversion 2 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1261,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC081c","Allocated GHG emissions after conversion 2 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1262,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC081d","Allocated water use after conversion 2 (per GJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1263,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC081f","Allocated acidification potential after conversion 2 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1264,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC081g","Allocated eutrophication potential after conversion 2 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1265,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC082a","Total fossil energy use feedstock 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1266,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC082b","Total primary energy use feedstock 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1267,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC082c","Total GHG emissions feedstock 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1268,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC082d","Total water use feedstock 1 (per GJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1269,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC082f","Total acidification potential feedstock 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1270,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC082g","Total eutrophication potential feedstock 1 (per MJ feedstock 1 fuel)",{"$f":"VLOOKUP(A1271,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC083a","Total fossil energy use feedstock 1 (per MJ functional unit)",{"$f":"VLOOKUP(A1272,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJFU"}]
["BC083b","Total primary energy use feedstock 1 (per MJ functional unit)",{"$f":"VLOOKUP(A1273,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJFU"}]
["BC083c","Total GHG emissions feedstock 1 (per MJ functional unit)",{"$f":"VLOOKUP(A1274,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJFU"}]
["BC083d","Total water use feedstock 1 (per GJ functional unit)",{"$f":"VLOOKUP(A1275,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJFU"}]
["BC083f","Total acidification potential feedstock 1 (per MJ functional unit)",{"$f":"VLOOKUP(A1276,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJFU"}]
["BC083g","Total eutrophication potential feedstock 1 (per MJ functional unit)",{"$f":"VLOOKUP(A1277,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJFU"}]
["BC084","Total GHG emissions feedstock 1 (per MJ feedstock 1 fuel) without LUC emissions",{"$f":"VLOOKUP(A1278,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC090a","Totally allocated fossil energy requirement in process 1",{"$f":"VLOOKUP(A1279,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC090b","Totally allocated primary energy requirement in process 1",{"$f":"VLOOKUP(A1280,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC090c","Totally allocated GHG emissions in process 1",{"$f":"VLOOKUP(A1281,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC090d","Totally allocated water use in process 1",{"$f":"VLOOKUP(A1282,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC090f","Totally allocated acidification potential from process 1",{"$f":"VLOOKUP(A1283,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC090g","Totally allocated eutrophication potential from process 1",{"$f":"VLOOKUP(A1284,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC091a","Totally allocated fossil energy requirement in process 1",{"$f":"VLOOKUP(A1285,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJFU"}]
["BC091b","Totally allocated primary energy requirement in process 1",{"$f":"VLOOKUP(A1286,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJFU"}]
["BC091c","Totally allocated GHG emissions in process 1",{"$f":"VLOOKUP(A1287,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJFU"}]
["BC091d","Totally allocated water use in process 1",{"$f":"VLOOKUP(A1288,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJFU"}]
["BC091f","Totally allocated acidification potential from process 1",{"$f":"VLOOKUP(A1289,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJFU"}]
["BC091g","Totally allocated eutrophication potential from process 1",{"$f":"VLOOKUP(A1290,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJFU"}]
["BC092a","Totally allocated fossil energy requirement in process 2",{"$f":"VLOOKUP(A1291,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC092b","Totally allocated primary energy requirement in process 2",{"$f":"VLOOKUP(A1292,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC092c","Totally allocated GHG emissions in process 2",{"$f":"VLOOKUP(A1293,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC092d","Totally allocated water use in process 2",{"$f":"VLOOKUP(A1294,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC092f","Totally allocated acidification potential from process 2",{"$f":"VLOOKUP(A1295,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC092g","Totally allocated eutrophication potential from process 2",{"$f":"VLOOKUP(A1296,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC093a","Totally allocated fossil energy requirement in process 2",{"$f":"VLOOKUP(A1297,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJFU"}]
["BC093b","Totally allocated primary energy requirement in process 2",{"$f":"VLOOKUP(A1298,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJFU"}]
["BC093c","Totally allocated GHG emissions in process 2",{"$f":"VLOOKUP(A1299,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJFU"}]
["BC093d","Totally allocated water use in process 2",{"$f":"VLOOKUP(A1300,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJFU"}]
["BC093f","Totally allocated acidification potential from process 2",{"$f":"VLOOKUP(A1301,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJFU"}]
["BC093g","Totally allocated eutrophication potential from process 2",{"$f":"VLOOKUP(A1302,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJFU"}]
["BC094a","Totally allocated fossil energy requirement for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1303,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJendfuel_fs1"}]
["BC094b","Totally allocated primary energy requirement for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1304,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJendfuel_fs1"}]
["BC094c","Totally allocated GHG emissions from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1305,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJendfuel_fs1"}]
["BC094d","Totally allocated water use for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1306,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC094f","Totally allocated acidification potential from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1307,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC094g","Totally allocated eutrophication potential from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1308,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC095a","Totally allocated fossil energy requirement for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1309,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJfossil/MJFU"}]
["BC095b","Totally allocated primary energy requirement for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1310,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"MJprim/MJFU"}]
["BC095c","Totally allocated GHG emissions from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1311,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gCO2_eq/MJFU"}]
["BC095d","Totally allocated water use for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1312,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJFU"}]
["BC095f","Totally allocated acidification potential from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1313,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJFU"}]
["BC095g","Totally allocated eutrophication potential from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1314,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJFU"}]
["BC100a","Water use for conversion process 1",{"$f":"VLOOKUP(A1315,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/MJoutput"}]
["BC100b","Water use for conversion process 1",{"$f":"VLOOKUP(A1316,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC101a","Water use for feedstock treatment 2 (drying and storage)",{"$f":"VLOOKUP(A1317,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/MJinput"}]
["BC101b","Water use for feedstock treatment 2 (drying and storage)",{"$f":"VLOOKUP(A1318,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC102a","Water use for conversion process 2",{"$f":"VLOOKUP(A1319,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/MJoutput"}]
["BC102b","Water use for conversion process 2",{"$f":"VLOOKUP(A1320,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC103a","Water use for feedstock treatment 3 (drying and storage)",{"$f":"VLOOKUP(A1321,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/MJinput"}]
["BC103b","Water use for feedstock treatment 3 (drying and storage)",{"$f":"VLOOKUP(A1322,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"m³/GJendfuel_fs1"}]
["BC110a","Acidification potential related to process 1",{"$f":"VLOOKUP(A1323,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC110b","Acidification potential related to process 2",{"$f":"VLOOKUP(A1324,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJendfuel_fs1"}]
["BC111a","Acidification potential related to electricity input, process 1",{"$f":"VLOOKUP(A1325,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC111b","Acidification potential related to electricity input, process 2",{"$f":"VLOOKUP(A1326,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC112a","NOx emissions factor of electricity flow 1, process 1",{"$f":"VLOOKUP(A1327,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJe"}]
["BC112a1","NOx emissions factor of electricity flow 2, process 1",{"$f":"VLOOKUP(A1328,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJe"}]
["BC112b","NOx emissions factor of electricity flow 1, process 2",{"$f":"VLOOKUP(A1329,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJe"}]
["BC112b1","NOx emissions factor of electricity flow 2, process 2",{"$f":"VLOOKUP(A1330,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJe"}]
["BC113a","SOx emissions factor of electricity flow 1, process 1",{"$f":"VLOOKUP(A1331,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJe"}]
["BC113a1","SOx emissions factor of electricity flow 2, process 1",{"$f":"VLOOKUP(A1332,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJe"}]
["BC113b","SOx emissions factor of electricity flow 1, process 2",{"$f":"VLOOKUP(A1333,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJe"}]
["BC113b1","SOx emissions factor of electricity flow 2, process 2",{"$f":"VLOOKUP(A1334,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJe"}]
["BC114a","Acidification potential related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1335,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC114b","Acidification potential related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1336,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC115a","NOx emissions factor of fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1337,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJf_h"}]
["BC115b","NOx emissions factor of fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1338,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJf_h"}]
["BC116a","SOx emissions factor of fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1339,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJf_h"}]
["BC116b","SOx emissions factor of fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1340,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJf_h"}]
["BC117a","NOx emissions factor of fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1341,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJf_h"}]
["BC117b","NOx emissions factor of fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1342,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJf_h"}]
["BC118a","SOx emissions factor of fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1343,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJf_h"}]
["BC118b","SOx emissions factor of fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1344,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJf_h"}]
["BC119a","Acidification potential related to material input flows, process 1",{"$f":"VLOOKUP(A1345,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC119b","Acidification potential related to material input flows, process 2",{"$f":"VLOOKUP(A1346,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC120a","NOx emissions factor of material input flow 1, process 1",{"$f":"VLOOKUP(A1347,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/kgdm"}]
["BC120b","NOx emissions factor of material input flow 1, process 2",{"$f":"VLOOKUP(A1348,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/kg"}]
["BC120c","NOx emissions factor of material output flow, process 1",{"$f":"VLOOKUP(A1349,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/kgdm"}]
["BC120c1","NOx emissions factor of output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1350,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJe"}]
["BC120c2","NOx emissions factor of output flow, process 1 (heat)",{"$f":"VLOOKUP(A1351,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJf_h"}]
["BC120d","NOx emissions factor of material output flow, process 2",{"$f":"VLOOKUP(A1352,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/kgdm"}]
["BC120d1","NOx emissions factor of output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1353,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJe"}]
["BC120d2","NOx emissions factor of output flow, process 2 (heat)",{"$f":"VLOOKUP(A1354,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/MJf_h"}]
["BC121a","SOx emissions factor of material input flow 1, process 1",{"$f":"VLOOKUP(A1355,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/kgdm"}]
["BC121b","SOx emissions factor of material input flow 1, process 2",{"$f":"VLOOKUP(A1356,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/kg"}]
["BC121c","SOx emissions factor of material output flow, process 1",{"$f":"VLOOKUP(A1357,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/kgdm"}]
["BC121c1","SOx emissions factor of output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1358,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJe"}]
["BC121c2","SOx emissions factor of output flow, process 1 (heat)",{"$f":"VLOOKUP(A1359,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJf_h"}]
["BC121d","SOx emissions factor of material output flow, process 2",{"$f":"VLOOKUP(A1360,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/kgdm"}]
["BC121d1","SOx emissions factor of output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1361,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJe"}]
["BC121d2","SOx emissions factor of output flow, process 2 (heat)",{"$f":"VLOOKUP(A1362,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/MJf_h"}]
["BC122a","NOx emissions factor of material input flow 2, process 1",{"$f":"VLOOKUP(A1363,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/kgdm"}]
["BC122b","NOx emissions factor of material input flow 2, process 2",{"$f":"VLOOKUP(A1364,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/kg"}]
["BC123a","SOx emissions factor of material input flow 2, process 1",{"$f":"VLOOKUP(A1365,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/kgdm"}]
["BC123b","SOx emissions factor of material input flow 2, process 2",{"$f":"VLOOKUP(A1366,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/kg"}]
["BC124a","Acidification potential related to process emissions, process 1",{"$f":"VLOOKUP(A1367,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC124b","Acidification potential related to process emissions, process 2",{"$f":"VLOOKUP(A1368,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC125a","NOx emissions factor of material input flow 3, process 1",{"$f":"VLOOKUP(A1369,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gNOX/kgdm"}]
["BC126a","SOx emissions factor of material input flow 3, process 1",{"$f":"VLOOKUP(A1370,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gSOX/kgdm"}]
["BC130a","Eutrophication potential related to process 1",{"$f":"VLOOKUP(A1371,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC130b","Eutrophication potential related to process 2",{"$f":"VLOOKUP(A1372,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJendfuel_fs1"}]
["BC131a","Eutrophication potential related to electricity input, process 1",{"$f":"VLOOKUP(A1373,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC131b","Eutrophication potential related to electricity input, process 2",{"$f":"VLOOKUP(A1374,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC134a","Eutrophication potential related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1375,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC134b","Eutrophication potential related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1376,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC139a","Eutrophication potential related to material input flows, process 1",{"$f":"VLOOKUP(A1377,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC139b","Eutrophication potential related to material input flows, process 2",{"$f":"VLOOKUP(A1378,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC144a","Eutrophication potential related to process emissions, process 1",{"$f":"VLOOKUP(A1379,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC144b","Eutrophication potential related to process emissions, process 2",{"$f":"VLOOKUP(A1380,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC150a","No forced labour, process 1",{"$f":"VLOOKUP(A1381,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC150b","No child labour, process 1",{"$f":"VLOOKUP(A1382,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC150c","Good social practices regarding human rights, process 1",{"$f":"VLOOKUP(A1383,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC150d","No discrimination, process 1",{"$f":"VLOOKUP(A1384,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC150e","Land is used legitimately / land rights have been secured, process 1",{"$f":"VLOOKUP(A1385,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC150f","Open and transparent communication with local communities and stakeholders, process 1",{"$f":"VLOOKUP(A1386,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC150g","Food security, process 1",{"$f":"VLOOKUP(A1387,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC151a","Fair legal contracts, process 1",{"$f":"VLOOKUP(A1388,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC151b","Workers rights, process 1",{"$f":"VLOOKUP(A1389,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC151c","Freedom to join labour organizations or organize themselves, process 1",{"$f":"VLOOKUP(A1390,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC151d","Fair wages and compensation rules, process 1",{"$f":"VLOOKUP(A1391,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC151e","Health, safety and hygiene policy, process 1",{"$f":"VLOOKUP(A1392,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC151f","Risk assessment for safe and healthy working conditions, process 1",{"$f":"VLOOKUP(A1393,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC151g","Health and safety training, process 1",{"$f":"VLOOKUP(A1394,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC152a","No forced labour, process 2",{"$f":"VLOOKUP(A1395,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC152b","No child labour, process 2",{"$f":"VLOOKUP(A1396,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC152c","Good social practices regarding human rights, process 2",{"$f":"VLOOKUP(A1397,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC152d","No discrimination, process 2",{"$f":"VLOOKUP(A1398,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC152e","Land is used legitimately / land rights have been secured, process 2",{"$f":"VLOOKUP(A1399,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC152f","Open and transparent communication with local communities and stakeholders, process 2",{"$f":"VLOOKUP(A1400,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC152g","Food security, process 2",{"$f":"VLOOKUP(A1401,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC153a","Fair legal contracts, process 2",{"$f":"VLOOKUP(A1402,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC153b","Workers rights, process 2",{"$f":"VLOOKUP(A1403,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC153c","Freedom to join labour organizations or organize themselves, process 2",{"$f":"VLOOKUP(A1404,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC153d","Fair wages and compensation rules, process 2",{"$f":"VLOOKUP(A1405,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC153e","Health, safety and hygiene policy, process 2",{"$f":"VLOOKUP(A1406,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC153f","Risk assessment for safe and healthy working conditions, process 2",{"$f":"VLOOKUP(A1407,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC153g","Health and safety training, process 2",{"$f":"VLOOKUP(A1408,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC154a","No forced labour, processing FS1",{"$f":"VLOOKUP(A1409,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC154b","No child labour, processing FS1",{"$f":"VLOOKUP(A1410,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC154c","Good social practices regarding human rights, processing FS1",{"$f":"VLOOKUP(A1411,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC154d","No discrimination, processing FS1",{"$f":"VLOOKUP(A1412,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC154e","Land is used legitimately / land rights have been secured, processing FS1",{"$f":"VLOOKUP(A1413,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC154f","Open and transparent communication with local communities and stakeholders, processing FS1",{"$f":"VLOOKUP(A1414,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC154g","Food security, processing FS1",{"$f":"VLOOKUP(A1415,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC155a","Fair legal contracts, processing FS1",{"$f":"VLOOKUP(A1416,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC155b","Workers rights, processing FS1",{"$f":"VLOOKUP(A1417,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC155c","Freedom to join labour organizations or organize themselves, processing FS1",{"$f":"VLOOKUP(A1418,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC155d","Fair wages and compensation rules, processing FS1",{"$f":"VLOOKUP(A1419,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC155e","Health, safety and hygiene policy, processing FS1",{"$f":"VLOOKUP(A1420,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC155f","Risk assessment for safe and healthy working conditions, processing FS1",{"$f":"VLOOKUP(A1421,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC155g","Health and safety training, processing FS1",{"$f":"VLOOKUP(A1422,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC156","Human and property rights, process 1_score",{"$f":"VLOOKUP(A1423,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC157","Labour rights and conditions, process 1_score",{"$f":"VLOOKUP(A1424,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC158","Human and property rights, process 2_score",{"$f":"VLOOKUP(A1425,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC159","Labour rights and conditions, process 2_score",{"$f":"VLOOKUP(A1426,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC160","Human and property rights, processing overall_score",{"$f":"VLOOKUP(A1427,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["BC161","Labour rights and conditions, processing overall_score",{"$f":"VLOOKUP(A1428,'Conversion feedstock1'!D$10:E$785,2,FALSE)","v":"-"}]
["Biomass conversion feedstock 2"]
["BC500a","Process 1 description ",{"$f":"VLOOKUP(A1430,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC500b","Process 2 description ",{"$f":"VLOOKUP(A1431,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC501a","Type of main output flow, process 1",{"$f":"VLOOKUP(A1432,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC501b","Type of main output flow, process 2",{"$f":"VLOOKUP(A1433,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC502a1","Type of by-product 1, process 1",{"$f":"VLOOKUP(A1434,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC502a10","Moisture content of by-product 1, process 1",{"$f":"VLOOKUP(A1435,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC502a11","By-product flow 1, process 1",{"$f":"VLOOKUP(A1436,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC502a2","Type of by-product 2, process 1",{"$f":"VLOOKUP(A1437,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC502a20","Moisture content of by-product 2, process 1",{"$f":"VLOOKUP(A1438,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC502a21","By-product flow 2, process 1",{"$f":"VLOOKUP(A1439,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC502a3","Type of by-product 3, process 1",{"$f":"VLOOKUP(A1440,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC502a30","Moisture content of by-product 3, process 1",{"$f":"VLOOKUP(A1441,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC502a31","By-product flow 3, process 1",{"$f":"VLOOKUP(A1442,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC502a41","Electricity by-product, process 1",{"$f":"VLOOKUP(A1443,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MWh/year"}]
["BC502a51","Heat by-product, process 1",{"$f":"VLOOKUP(A1444,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/year"}]
["BC502b1","Type of by-product 1, process 2",{"$f":"VLOOKUP(A1445,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC502b10","Moisture content of by-product 1, process 2",{"$f":"VLOOKUP(A1446,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC502b11","By-product flow 1, process 2",{"$f":"VLOOKUP(A1447,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC502b2","Type of by-product 2, process 2",{"$f":"VLOOKUP(A1448,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC502b20","Moisture content of by-product 2, process 2",{"$f":"VLOOKUP(A1449,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC502b21","By-product flow 2, process 2",{"$f":"VLOOKUP(A1450,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC502b41","Electricity by-product, process 2",{"$f":"VLOOKUP(A1451,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MWh/year"}]
["BC502b51","Heat by-product, process 2",{"$f":"VLOOKUP(A1452,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/year"}]
["BC503a1","Extraction rate of by-product 1, process 1 (kg)",{"$f":"VLOOKUP(A1453,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC503a2","Extraction rate of by-product 2, process 1 (kg)",{"$f":"VLOOKUP(A1454,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC503a3","Extraction rate of by-product 3, process 1 (kg)",{"$f":"VLOOKUP(A1455,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC503b1","Extraction rate of by-product 1, process 2 (kg)",{"$f":"VLOOKUP(A1456,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC503b2","Extraction rate of by-product 2, process 2 (kg)",{"$f":"VLOOKUP(A1457,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgbyproduct /kginput"}]
["BC504a1","Extraction rate of by-product 1, process 1 (MJ)",{"$f":"VLOOKUP(A1458,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC504a2","Extraction rate of by-product 2, process 1 (MJ)",{"$f":"VLOOKUP(A1459,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC504a3","Extraction rate of by-product 3, process 1 (MJ)",{"$f":"VLOOKUP(A1460,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC504a4","Extraction rate of electricity by-product, process 1 (MJ)",{"$f":"VLOOKUP(A1461,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC504a5","Extraction rate of heat by-product, process 1 (MJ)",{"$f":"VLOOKUP(A1462,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC504b1","Extraction rate of by-product 1, process 2 (MJ)",{"$f":"VLOOKUP(A1463,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC504b2","Extraction rate of by-product 2, process 2 (MJ)",{"$f":"VLOOKUP(A1464,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC504b4","Extraction rate of electricity by-product, process 2 (MJ)",{"$f":"VLOOKUP(A1465,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC504b5","Extraction rate of heat by-product, process 2 (MJ)",{"$f":"VLOOKUP(A1466,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJbyproduct /MJinput"}]
["BC505a1","Energy content of by-product 1, process 1 (LHV)",{"$f":"VLOOKUP(A1467,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC505a2","Energy content of by-product 2, process 1 (LHV)",{"$f":"VLOOKUP(A1468,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC505a3","Energy content of by-product 3, process 1 (LHV)",{"$f":"VLOOKUP(A1469,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC505b1","Energy content of by-product 1, process 2 (LHV)",{"$f":"VLOOKUP(A1470,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC505b2","Energy content of by-product 2, process 2 (LHV)",{"$f":"VLOOKUP(A1471,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC506a1","Valorisation of by-product 1, process 1",{"$f":"VLOOKUP(A1472,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC506a2","Valorisation of by-product 2, process 1",{"$f":"VLOOKUP(A1473,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC506a3","Valorisation of by-product 3, process 1",{"$f":"VLOOKUP(A1474,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC506a4","Valorisation of electricity by-product, process 1",{"$f":"VLOOKUP(A1475,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC506a5","Valorisation of heat by-product, process 1",{"$f":"VLOOKUP(A1476,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC506b1","Valorisation of by-product 1, process 2",{"$f":"VLOOKUP(A1477,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC506b2","Valorisation of by-product 2, process 2",{"$f":"VLOOKUP(A1478,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC506b4","Valorisation of electricity by-product, process 2",{"$f":"VLOOKUP(A1479,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC506b5","Valorisation of heat by-product, process 2",{"$f":"VLOOKUP(A1480,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"binary"}]
["BC507a","Energy content of main output flow, process 1 (LHV)",{"$f":"VLOOKUP(A1481,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC507b","Energy content of main output flow, process 2 (LHV)",{"$f":"VLOOKUP(A1482,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC508a","Extraction rate (output/input), process 1",{"$f":"VLOOKUP(A1483,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJoutput /MJinput"}]
["BC508b","Extraction rate (output/input), process 2",{"$f":"VLOOKUP(A1484,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJoutput /MJinput"}]
["BC509a0","Type of main input,process 1",{"$f":"VLOOKUP(A1485,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509a1","Type of material input flow 1, process 1",{"$f":"VLOOKUP(A1486,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509a2","Type of material input flow 2, process 1",{"$f":"VLOOKUP(A1487,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509a3","Type of material input flow 3, process 1",{"$f":"VLOOKUP(A1488,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509b1","Type of material input flow 1, process 2",{"$f":"VLOOKUP(A1489,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509b2","Type of material input flow 2, process 2",{"$f":"VLOOKUP(A1490,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509c","Type of material output flow, process 1",{"$f":"VLOOKUP(A1491,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509c1","Type of output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1492,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509c2","Type of output flow, process 1 (heat)",{"$f":"VLOOKUP(A1493,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509d","Type of material output flow, process 2",{"$f":"VLOOKUP(A1494,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509d1","Type of output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1495,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC509d2","Type of output flow, process 2 (heat)",{"$f":"VLOOKUP(A1496,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC510a0","Main input, process 1",{"$f":"VLOOKUP(A1497,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC510a","Amount of main input, process 1",{"$f":"VLOOKUP(A1498,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgdm/MJoutput"}]
["BC510a01","Material input flow 1, process 1",{"$f":"VLOOKUP(A1499,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC510a1","Amount of material input flow 1, process 1",{"$f":"VLOOKUP(A1500,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgdm/MJoutput"}]
["BC510a10","Moisture content of material input flow 1, process 1",{"$f":"VLOOKUP(A1501,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC510a11","Energy content of input flow 1, process 1",{"$f":"VLOOKUP(A1502,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC510a02","Material input flow 2, process 1",{"$f":"VLOOKUP(A1503,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC510a2","Amount of material input flow 2, process 1",{"$f":"VLOOKUP(A1504,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgdm/MJoutput"}]
["BC510a20","Moisture content of material input flow 2, process 1",{"$f":"VLOOKUP(A1505,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC510a21","Energy content of input flow 2, process 1",{"$f":"VLOOKUP(A1506,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC510a03","Material input flow 3, process 1",{"$f":"VLOOKUP(A1507,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC510a3","Amount of material input flow 3, process 1",{"$f":"VLOOKUP(A1508,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgdm/MJoutput"}]
["BC510a30","Moisture content of material input flow 3, process 1",{"$f":"VLOOKUP(A1509,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC510a31","Energy content of input flow 3, process 1",{"$f":"VLOOKUP(A1510,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/kgdm"}]
["BC510b1","Amount of material input flow 1, process 2",{"$f":"VLOOKUP(A1511,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/MJoutput"}]
["BC510b10","Material input flow 1, process 2",{"$f":"VLOOKUP(A1512,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC510b11","Moisture content of material input flow 1, process 2",{"$f":"VLOOKUP(A1513,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC510b12","Energy content of input flow 1, process 2"]
["BC510b2","Amount of material input flow 2, process 2",{"$f":"VLOOKUP(A1515,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/MJoutput"}]
["BC510b20","Material input flow 2, process 2",{"$f":"VLOOKUP(A1516,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC510b21","Moisture content of material input flow 2, process 2",{"$f":"VLOOKUP(A1517,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC510b22","Energy content of input flow 2, process 2"]
["BC510c","Amount of material output flow, process 1",{"$f":"VLOOKUP(A1519,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgdm/MJoutput"}]
["BC510c0","Material output flow, process 1",{"$f":"VLOOKUP(A1520,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC510c1","Amount of material output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1521,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJe/MJoutput"}]
["BC510c2","Amount of material output flow, process 1 (heat)",{"$f":"VLOOKUP(A1522,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC510d","Amount of material output flow, process 2",{"$f":"VLOOKUP(A1523,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgdm/MJoutput"}]
["BC510d0","Material output flow, process 2",{"$f":"VLOOKUP(A1524,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/year"}]
["BC510d1","Amount of material output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1525,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJe/MJoutput"}]
["BC510d2","Amount of material output flow, process 2 (heat)",{"$f":"VLOOKUP(A1526,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC511a1","Type of fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1527,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC511a2","Type of fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1528,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC511b1","Type of fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1529,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC511b2","Type of fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1530,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC512a","Moisture content of main output flow, process 1",{"$f":"VLOOKUP(A1531,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC512b","Moisture content of main output flow, process 2",{"$f":"VLOOKUP(A1532,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC514a","Yield rate (moist/wet) of feedstock 2 per ha after conversion process 1",{"$f":"VLOOKUP(A1533,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/ha"}]
["BC514b","Yield rate (dry) of feedstock 2 per ha after conversion process 1",{"$f":"VLOOKUP(A1534,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgdm/ha"}]
["BC514c","Yield rate (energy) of feedstock 2 per ha after conversion process 1",{"$f":"VLOOKUP(A1535,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/ha"}]
["BC515a","Yield rate (moist/wet) of feedstock 2 per ha after conversion process 2",{"$f":"VLOOKUP(A1536,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kg/ha"}]
["BC515b","Yield rate (dry) of feedstock 2 per ha after conversion process 2",{"$f":"VLOOKUP(A1537,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"kgdm/ha"}]
["BC515c","Yield rate (energy) of feedstock 2 per ha after conversion process 2",{"$f":"VLOOKUP(A1538,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/ha"}]
["BC516a","NOX emissions to air (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1539,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJoutput"}]
["BC516b","SOX emissions to air (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1540,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJoutput"}]
["BC516c","NH3 emissions to air (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1541,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNH3/MJoutput"}]
["BC516d","NO3- emissions to water (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1542,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNO3/MJoutput"}]
["BC516e","NH4+ emissions to water (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1543,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNH4/MJoutput"}]
["BC516f","PO43- emissions to water (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1544,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4/MJoutput"}]
["BC516g","COD emissions to water (not from material/energy input), conversion process 1",{"$f":"VLOOKUP(A1545,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCOD/MJoutput"}]
["BC517a","NOX emissions to air (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1546,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJoutput"}]
["BC517b","SOX emissions to air (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1547,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJoutput"}]
["BC517c","NH3 emissions to air (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1548,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNH3/MJoutput"}]
["BC517d","NO3- emissions to water (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1549,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNO3/MJoutput"}]
["BC517e","NH4+ emissions to water (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1550,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNH4/MJoutput"}]
["BC517f","PO43- emissions to water (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1551,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4/MJoutput"}]
["BC517g","COD emissions to water (not from material/energy input), conversion process 2",{"$f":"VLOOKUP(A1552,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCOD/MJoutput"}]
["BC519a","Total allocated fossil energy use for processing (process 1+2)",{"$f":"VLOOKUP(A1553,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":{"$error":"#N/A"}}]
["BC519b","Total allocated primary energy use for processing (process 1+2)",{"$f":"VLOOKUP(A1554,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":{"$error":"#N/A"}}]
["BC520a","Fossil energy use in process 1",{"$f":"VLOOKUP(A1555,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC520b","Fossil energy use in process 2",{"$f":"VLOOKUP(A1556,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC521a","Primary energy use in process 1",{"$f":"VLOOKUP(A1557,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC521b","Primary energy use in process 2",{"$f":"VLOOKUP(A1558,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC522a","Allocation to by-products, process 1",{"$f":"VLOOKUP(A1559,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC522b","Allocation to by-products, process 2",{"$f":"VLOOKUP(A1560,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC524a","Fossil energy use related to electricity input, process 1",{"$f":"VLOOKUP(A1561,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC524b","Fossil energy use related to electricity input, process 2",{"$f":"VLOOKUP(A1562,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC525a","Primary energy use related to electricity input, process 1",{"$f":"VLOOKUP(A1563,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJoutput"}]
["BC525b","Primary energy use related to electricity input, process 2",{"$f":"VLOOKUP(A1564,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJoutput"}]
["BC526a","Amount of electricity input 1, process 1",{"$f":"VLOOKUP(A1565,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJe/MJoutput"}]
["BC526a0","Electricity flow 1, process 1",{"$f":"VLOOKUP(A1566,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MWh/year"}]
["BC526a1","Amount of electricity input 2, process 1",{"$f":"VLOOKUP(A1567,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJe/MJoutput"}]
["BC526a10","Electricity flow 2, process 1",{"$f":"VLOOKUP(A1568,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MWh/year"}]
["BC526b","Amount of electricity input 1, process 2",{"$f":"VLOOKUP(A1569,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJe/MJoutput"}]
["BC526b0","Electricity flow 1, process 2",{"$f":"VLOOKUP(A1570,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MWh/year"}]
["BC526b1","Amount of electricity input 2, process 2",{"$f":"VLOOKUP(A1571,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJe/MJoutput"}]
["BC526b10","Electricity flow 2, process 2",{"$f":"VLOOKUP(A1572,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MWh/year"}]
["BC527a","Type of electricity flow 1, process 1",{"$f":"VLOOKUP(A1573,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC527a1","Type of electricity flow 2, process 1",{"$f":"VLOOKUP(A1574,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC527b","Type of electricity flow 1, process 2",{"$f":"VLOOKUP(A1575,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC527b1","Type of electricity flow 2, process 2",{"$f":"VLOOKUP(A1576,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC528a","Specific fossil energy used for external electricity production flow 1, process 1",{"$f":"VLOOKUP(A1577,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJe"}]
["BC528a1","Specific fossil energy used for external electricity production flow 2, process 1",{"$f":"VLOOKUP(A1578,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJe"}]
["BC528b","Specific fossil energy used for external electricity production flow 1, process 2",{"$f":"VLOOKUP(A1579,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJe"}]
["BC528b1","Specific fossil energy used for external electricity production flow 2, process 2",{"$f":"VLOOKUP(A1580,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJe"}]
["BC529a","Specific primary energy used for external electricity production flow 1, process 1",{"$f":"VLOOKUP(A1581,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJe"}]
["BC529a1","Specific primary energy used for external electricity production flow 2, process 1",{"$f":"VLOOKUP(A1582,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJe"}]
["BC529b","Specific primary energy used for external electricity production flow 1, process 2",{"$f":"VLOOKUP(A1583,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJe"}]
["BC529b1","Specific primary energy used for external electricity production flow 2, process 2",{"$f":"VLOOKUP(A1584,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJe"}]
["BC530a","Fossil energy use related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1585,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC530b","Fossil energy use related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1586,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC531a1","Amount of fuel/heat input 1, process 1",{"$f":"VLOOKUP(A1587,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC531a10","Fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1588,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/year"}]
["BC531a2","Amount of fuel/heat input 2, process 1",{"$f":"VLOOKUP(A1589,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC531a20","Fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1590,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/year"}]
["BC531b1","Amount of fuel/heat input 1, process 2",{"$f":"VLOOKUP(A1591,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC531b10","Fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1592,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/year"}]
["BC531b2","Amount of fuel/heat input 2, process 2",{"$f":"VLOOKUP(A1593,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJf_h/MJoutput"}]
["BC531b20","Fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1594,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJ/year"}]
["BC532a1","Specific fossil energy for fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1595,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC532a2","Specific fossil energy for fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1596,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC532b1","Specific fossil energy for fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1597,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC532b2","Specific fossil energy for fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1598,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC533a1","Specific primary energy for fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1599,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJf_h"}]
["BC533a2","Specific primary energy for fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1600,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJf_h"}]
["BC533b1","Specific primary energy for fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1601,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJf_h"}]
["BC533b2","Specific primary energy for fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1602,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJf_h"}]
["BC534a","Primary energy use related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1603,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJoutput"}]
["BC534b","Primary energy use related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1604,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJoutput"}]
["BC535a","Fossil energy use related to material input flows, process 1",{"$f":"VLOOKUP(A1605,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC535a1","Specific fossil energy for material input flow 1, process 1",{"$f":"VLOOKUP(A1606,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/kg"}]
["BC535a2","Specific fossil energy for material input flow 2, process 1",{"$f":"VLOOKUP(A1607,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/kg"}]
["BC535a3","Specific fossil energy for material input flow 3, process 1",{"$f":"VLOOKUP(A1608,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/kg"}]
["BC535b","Fossil energy use related to material input flows, process 2",{"$f":"VLOOKUP(A1609,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJoutput"}]
["BC535b1","Specific fossil energy for material input flow 1, process 2",{"$f":"VLOOKUP(A1610,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/kg"}]
["BC535b2","Specific fossil energy for material input flow 2, process 2",{"$f":"VLOOKUP(A1611,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/kg"}]
["BC535c","Specific fossil energy for material output flow, process 1",{"$f":"VLOOKUP(A1612,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/kgdm"}]
["BC535c1","Specific fossil energy for output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1613,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJe"}]
["BC535c2","Specific fossil energy for output flow, process 1 (heat)",{"$f":"VLOOKUP(A1614,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC535d","Specific fossil energy for material output flow, process 2",{"$f":"VLOOKUP(A1615,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/kgdm"}]
["BC535d1","Specific fossil energy for output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1616,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJe"}]
["BC535d2","Specific fossil energy for output flow, process 2 (heat)",{"$f":"VLOOKUP(A1617,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJf_h"}]
["BC536a","Primary energy use related to material input flows, process 1",{"$f":"VLOOKUP(A1618,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJoutput"}]
["BC536a0","Specific primary energy for main input, process 1",{"$f":"VLOOKUP(A1619,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/kg"}]
["BC536a1","Specific primary energy for material input flow 1, process 1",{"$f":"VLOOKUP(A1620,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/kg"}]
["BC536a2","Specific primary energy for material input flow 2, process 1",{"$f":"VLOOKUP(A1621,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/kg"}]
["BC536a3","Specific primary energy for material input flow 3, process 1",{"$f":"VLOOKUP(A1622,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/kg"}]
["BC536b","Primary energy use related to material input flows, process 2",{"$f":"VLOOKUP(A1623,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJoutput"}]
["BC536b1","Specific primary energy for material input flow 1, process 2",{"$f":"VLOOKUP(A1624,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/kg"}]
["BC536b2","Specific primary energy for material input flow 2, process 2",{"$f":"VLOOKUP(A1625,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/kg"}]
["BC536c","Specific primary energy for material output flow, process 1",{"$f":"VLOOKUP(A1626,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/kgdm"}]
["BC536c1","Specific primary energy for  output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1627,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJe"}]
["BC536c2","Specific primary energy for output flow, process 1 (heat)",{"$f":"VLOOKUP(A1628,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJf_h"}]
["BC536d","Specific primary energy for material output flow, process 2",{"$f":"VLOOKUP(A1629,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/kgdm"}]
["BC536d1","Specific primary energy for output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1630,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJe"}]
["BC536d2","Specific primary energy for output flow, process 2 (heat)",{"$f":"VLOOKUP(A1631,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJf_h"}]
["BC537a","GHG emissions related to process 1",{"$f":"VLOOKUP(A1632,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC537b","GHG emissions related to process 2",{"$f":"VLOOKUP(A1633,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC541a","GHG emissions related to electricity input, process 1",{"$f":"VLOOKUP(A1634,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC541b","GHG emissions related to electricity input, process 2",{"$f":"VLOOKUP(A1635,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC542a","Specific GHG emissions for external electricity production flow 1, process 1",{"$f":"VLOOKUP(A1636,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJe"}]
["BC542a1","Specific GHG emissions for external electricity production flow 2, process 1",{"$f":"VLOOKUP(A1637,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJe"}]
["BC542b","Specific GHG emissions for external electricity production flow 1, process 2",{"$f":"VLOOKUP(A1638,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJe"}]
["BC542b1","Specific GHG emissions for external electricity production flow 2, process 2",{"$f":"VLOOKUP(A1639,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJe"}]
["BC543a","GHG emissions related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1640,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC543a1","Specific GHG emissions related to fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1641,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC543a2","Specific GHG emissions related to fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1642,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC543b","GHG emissions related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1643,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC543b1","Specific GHG emissions related to fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1644,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC543b2","Specific GHG emissions related to fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1645,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC547a","GHG emissions related to material input flows, process 1",{"$f":"VLOOKUP(A1646,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC547a1","Specific GHG emissions related to material input flow 1, process 1",{"$f":"VLOOKUP(A1647,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/kg"}]
["BC547a2","Specific GHG emissions related to material input flow 2, process 1",{"$f":"VLOOKUP(A1648,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/kg"}]
["BC547a3","Specific GHG emissions related to material input flow 3, process 1",{"$f":"VLOOKUP(A1649,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/kg"}]
["BC547b","GHG emissions related to material input flows, process 2",{"$f":"VLOOKUP(A1650,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJoutput"}]
["BC547b1","Specific GHG emissions related to material input flow 1, process 2",{"$f":"VLOOKUP(A1651,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/kg"}]
["BC547b2","Specific GHG emissions related to material input flow 2, process 2",{"$f":"VLOOKUP(A1652,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/kg"}]
["BC547c","Specific GHG emissions related to material output flow, process 1",{"$f":"VLOOKUP(A1653,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/kgdm"}]
["BC547c1","Specific GHG emissions related to output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1654,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJe"}]
["BC547c2","Specific GHG emissions related to output flow, process 1 (heat)",{"$f":"VLOOKUP(A1655,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC547d","Specific GHG emissions related to material output flow, process 2",{"$f":"VLOOKUP(A1656,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/kgdm"}]
["BC547d1","Specific GHG emissions related to output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1657,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJe"}]
["BC547d2","Specific GHG emissions related to output flow, process 2 (heat)",{"$f":"VLOOKUP(A1658,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["BC550a","Allocation to energy crop, process 1",{"$f":"VLOOKUP(A1659,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC550b","Allocation to energy crop, process 2",{"$f":"VLOOKUP(A1660,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551a1","Allocation to by-product 1, process 1",{"$f":"VLOOKUP(A1661,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551a2","Allocation to by-product 2, process 1",{"$f":"VLOOKUP(A1662,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551a3","Allocation to by-product 3, process 1",{"$f":"VLOOKUP(A1663,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551a4","Allocation to electricity by-product, process 1",{"$f":"VLOOKUP(A1664,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551a5","Allocation to heat by-product, process 1",{"$f":"VLOOKUP(A1665,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551b1","Allocation to by-product 1, process 2",{"$f":"VLOOKUP(A1666,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551b2","Allocation to by-product 2, process 2",{"$f":"VLOOKUP(A1667,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551b4","Allocation to electricity by-product, process 2",{"$f":"VLOOKUP(A1668,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC551b5","Allocation to heat by-product, process 2",{"$f":"VLOOKUP(A1669,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"%"}]
["BC559a","Fossil energy use for treatment 2 (storage)",{"$f":"VLOOKUP(A1670,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC559b","Primary energy use for treatment 2 (storage)",{"$f":"VLOOKUP(A1671,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC559c","GHG emissions associated with treatment 2 (storage)",{"$f":"VLOOKUP(A1672,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC559d","Acidification potential related to treatment 2 (storage)",{"$f":"VLOOKUP(A1673,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC559e","Eutrophication potential related to treatment 2 (storage)",{"$f":"VLOOKUP(A1674,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC560","Heat energy use for treatment 2 (storage)",{"$f":"VLOOKUP(A1675,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJh/MJinput"}]
["BC561","Heat source for treatment 2 (storage)",{"$f":"VLOOKUP(A1676,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC562a","Specific fossil energy use for heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1677,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJh"}]
["BC562b","Specific primary energy use for heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1678,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJh"}]
["BC562c","Specific GHG emissions related to heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1679,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJh"}]
["BC562d","Specific NOx emissions related to heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1680,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJh"}]
["BC562e","Specific SOx emissions related to heat production for treatment 2 (storage)",{"$f":"VLOOKUP(A1681,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJh"}]
["BC565","Electricity energy use for treatment 2 (storage)",{"$f":"VLOOKUP(A1682,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJe/MJinput"}]
["BC566","Electricity source for treatment 2 (storage)",{"$f":"VLOOKUP(A1683,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC567a","Specific fossil energy use for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1684,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJe"}]
["BC567b","Specific primary energy use for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1685,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJe"}]
["BC567c","Specific GHG emissions for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1686,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJe"}]
["BC567d","Specific NOx emissions for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1687,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJe"}]
["BC567e","Specific SOx emissions for electricity production for treatment 2 (storage)",{"$f":"VLOOKUP(A1688,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJe"}]
["BC569a","Fossil energy use for treatment 3 (storage)",{"$f":"VLOOKUP(A1689,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC569b","Primary energy use for treatment 3 (storage)",{"$f":"VLOOKUP(A1690,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC569c","GHG emissions associated with treatment 3 (storage)",{"$f":"VLOOKUP(A1691,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC569d","Acidification potential associated with treatment 3 (storage)",{"$f":"VLOOKUP(A1692,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC569e","Eutrophication potential associated with treatment 3 (storage)",{"$f":"VLOOKUP(A1693,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC570","Heat energy use for treatment 3 (storage)",{"$f":"VLOOKUP(A1694,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJh/MJinput"}]
["BC571","Heat source for treatment 3 (storage)",{"$f":"VLOOKUP(A1695,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC572a","Specific fossil energy use for heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1696,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJh"}]
["BC572b","Specific primary energy use for heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1697,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJh"}]
["BC572c","Specific GHG emissions related to heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1698,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJh"}]
["BC572d","Specific NOx emissions related to heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1699,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJh"}]
["BC572e","Specific SOx emissions related to heat production for treatment 3 (storage)",{"$f":"VLOOKUP(A1700,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJh"}]
["BC575","Electricity energy use for treatment 3 (storage)",{"$f":"VLOOKUP(A1701,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJe/MJinput"}]
["BC576","Electricity source for treatment 3 (storage)",{"$f":"VLOOKUP(A1702,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC577a","Specific fossil energy use for electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1703,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJe"}]
["BC577b","Specific primary energy use for electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1704,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJe"}]
["BC577c","Specific GHG emissions related to electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1705,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2eq/MJe"}]
["BC577d","Specific NOx emissions related to electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1706,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJe"}]
["BC577e","Specific SOx emissions related to electricity production for treatment 3 (storage)",{"$f":"VLOOKUP(A1707,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJe"}]
["BC580a","Allocated fossil energy use after conversion 1 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1708,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC580b","Allocated primary energy use after conversion 1 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1709,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC580c","Allocated GHG emissions after conversion 1 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1710,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC580d","Allocated water use after conversion 1 (per GJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1711,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC580f","Allocated acidification potential after conversion 1 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1712,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC580g","Allocated eutrophication potential after conversion 1 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1713,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC581a","Allocated fossil energy use after conversion 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1714,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC581b","Allocated primary energy use after conversion 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1715,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC581c","Allocated GHG emissions after conversion 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1716,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC581d","Allocated water use after conversion 2 (per GJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1717,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC581f","Allocated acidification potential after conversion 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1718,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC581g","Allocated eutrophication potential after conversion 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1719,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC582a","Total fossil energy use feedstock 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1720,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC582b","Total primary energy use feedstock 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1721,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC582c","Total GHG emissions feedstock 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1722,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC582d","Total water use feedstock 2 (per GJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1723,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC582f","Total acidification potential feedstock 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1724,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC582g","Total eutrophication potential feedstock 2 (per MJ feedstock 2 fuel)",{"$f":"VLOOKUP(A1725,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC583a","Total fossil energy use feedstock 2 (per MJ functional unit)",{"$f":"VLOOKUP(A1726,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJFU"}]
["BC583b","Total primary energy use feedstock 2 (per MJ functional unit)",{"$f":"VLOOKUP(A1727,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJFU"}]
["BC583c","Total GHG emissions feedstock 2 (per MJ functional unit)",{"$f":"VLOOKUP(A1728,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJFU"}]
["BC583d","Total water use feedstock 2 (per GJ functional unit)",{"$f":"VLOOKUP(A1729,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJFU"}]
["BC583f","Total acidification potential feedstock 2 (per MJ functional unit)",{"$f":"VLOOKUP(A1730,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJFU"}]
["BC583g","Total eutrophication potential feedstock 2 (per MJ functional unit)",{"$f":"VLOOKUP(A1731,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJFU"}]
["BC584","Total GHG emissions feedstock 2 (per MJ feedstock 2 fuel) without LUC emissions",{"$f":"VLOOKUP(A1732,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC590a","Totally allocated fossil energy requirement in process 1",{"$f":"VLOOKUP(A1733,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC590b","Totally allocated primary energy requirement in process 1",{"$f":"VLOOKUP(A1734,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC590c","Totally allocated GHG emissions in process 1",{"$f":"VLOOKUP(A1735,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC590d","Totally allocated water use in process 1",{"$f":"VLOOKUP(A1736,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC590f","Totally allocated acidification potential from process 1",{"$f":"VLOOKUP(A1737,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC590g","Totally allocated eutrophication potential from process 1",{"$f":"VLOOKUP(A1738,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC591a","Totally allocated fossil energy requirement in process 1",{"$f":"VLOOKUP(A1739,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJFU"}]
["BC591b","Totally allocated primary energy requirement in process 1",{"$f":"VLOOKUP(A1740,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJFU"}]
["BC591c","Totally allocated GHG emissions in process 1",{"$f":"VLOOKUP(A1741,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJFU"}]
["BC591d","Totally allocated water use in process 1",{"$f":"VLOOKUP(A1742,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJFU"}]
["BC591f","Totally allocated acidification potential from process 1",{"$f":"VLOOKUP(A1743,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJFU"}]
["BC591g","Totally allocated eutrophication potential from process 1",{"$f":"VLOOKUP(A1744,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJFU"}]
["BC592a","Totally allocated fossil energy requirement in process 2",{"$f":"VLOOKUP(A1745,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC592b","Totally allocated primary energy requirement in process 2",{"$f":"VLOOKUP(A1746,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC592c","Totally allocated GHG emissions in process 2",{"$f":"VLOOKUP(A1747,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC592d","Totally allocated water use in process 2",{"$f":"VLOOKUP(A1748,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC592f","Totally allocated acidification potential from process 2",{"$f":"VLOOKUP(A1749,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC592g","Totally allocated eutrophication potential from process 2",{"$f":"VLOOKUP(A1750,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC593a","Totally allocated fossil energy requirement in process 2",{"$f":"VLOOKUP(A1751,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJFU"}]
["BC593b","Totally allocated primary energy requirement in process 2",{"$f":"VLOOKUP(A1752,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJFU"}]
["BC593c","Totally allocated GHG emissions in process 2",{"$f":"VLOOKUP(A1753,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJFU"}]
["BC593d","Totally allocated water use in process 2",{"$f":"VLOOKUP(A1754,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJFU"}]
["BC593f","Totally allocated acidification potential from process 2",{"$f":"VLOOKUP(A1755,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJFU"}]
["BC593g","Totally allocated eutrophication potential from process 2",{"$f":"VLOOKUP(A1756,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJFU"}]
["BC594a","Totally allocated fossil energy requirement for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1757,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJendfuel_fs2"}]
["BC594b","Totally allocated primary energy requirement for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1758,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJendfuel_fs2"}]
["BC594c","Totally allocated GHG emissions from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1759,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJendfuel_fs2"}]
["BC594d","Totally allocated water use for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1760,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC594f","Totally allocated acidification potential from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1761,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC594g","Totally allocated eutrophication potential from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1762,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC595a","Totally allocated fossil energy requirement for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1763,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJfossil/MJFU"}]
["BC595b","Totally allocated primary energy requirement for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1764,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"MJprim/MJFU"}]
["BC595c","Totally allocated GHG emissions from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1765,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gCO2_eq/MJFU"}]
["BC595d","Totally allocated water use for conversion (process 1 + 2)",{"$f":"VLOOKUP(A1766,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJFU"}]
["BC595f","Totally allocated acidification potential from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1767,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJFU"}]
["BC595g","Totally allocated eutrophication potential from conversion (process 1 + 2)",{"$f":"VLOOKUP(A1768,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJFU"}]
["BC600a","Water use for conversion process 1",{"$f":"VLOOKUP(A1769,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/MJoutput"}]
["BC600b","Water use for conversion process 1",{"$f":"VLOOKUP(A1770,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC601a","Water use for feedstock treatment 2 (drying and storage)",{"$f":"VLOOKUP(A1771,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/MJinput"}]
["BC601b","Water use for feedstock treatment 2 (drying and storage)",{"$f":"VLOOKUP(A1772,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC602a","Water use for conversion process 2",{"$f":"VLOOKUP(A1773,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/MJoutput"}]
["BC602b","Water use for conversion process 2",{"$f":"VLOOKUP(A1774,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC603a","Water use for feedstock treatment 3 (drying and storage)",{"$f":"VLOOKUP(A1775,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/MJinput"}]
["BC603b","Water use for feedstock treatment 3 (drying and storage)",{"$f":"VLOOKUP(A1776,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"m³/GJendfuel_fs2"}]
["BC610a","Acidification potential related to process 1",{"$f":"VLOOKUP(A1777,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC610b","Acidification potential related to process 2",{"$f":"VLOOKUP(A1778,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJendfuel_fs2"}]
["BC611a","Acidification potential related to electricity input, process 1",{"$f":"VLOOKUP(A1779,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC611b","Acidification potential related to electricity input, process 2",{"$f":"VLOOKUP(A1780,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC612a","NOx emissions factor of electricity flow 1, process 1",{"$f":"VLOOKUP(A1781,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJe"}]
["BC612a1","NOx emissions factor of electricity flow 2, process 1",{"$f":"VLOOKUP(A1782,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJe"}]
["BC612b","NOx emissions factor of electricity flow 1, process 2",{"$f":"VLOOKUP(A1783,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJe"}]
["BC612b1","NOx emissions factor of electricity flow 2, process 2",{"$f":"VLOOKUP(A1784,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJe"}]
["BC613a","SOx emissions factor of electricity flow 1, process 1",{"$f":"VLOOKUP(A1785,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJe"}]
["BC613a1","SOx emissions factor of electricity flow 2, process 1",{"$f":"VLOOKUP(A1786,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJe"}]
["BC613b","SOx emissions factor of electricity flow 1, process 2",{"$f":"VLOOKUP(A1787,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJe"}]
["BC613b1","SOx emissions factor of electricity flow 2, process 2",{"$f":"VLOOKUP(A1788,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJe"}]
["BC614a","Acidification potential related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1789,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC614b","Acidification potential related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1790,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC615a","NOx emissions factor of fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1791,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJf_h"}]
["BC615b","NOx emissions factor of fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1792,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJf_h"}]
["BC616a","SOx emissions factor of fuel/heat flow 1, process 1",{"$f":"VLOOKUP(A1793,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJf_h"}]
["BC616b","SOx emissions factor of fuel/heat flow 1, process 2",{"$f":"VLOOKUP(A1794,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJf_h"}]
["BC617a","NOx emissions factor of fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1795,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJf_h"}]
["BC617b","NOx emissions factor of fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1796,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJf_h"}]
["BC618a","SOx emissions factor of fuel/heat flow 2, process 1",{"$f":"VLOOKUP(A1797,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJf_h"}]
["BC618b","SOx emissions factor of fuel/heat flow 2, process 2",{"$f":"VLOOKUP(A1798,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJf_h"}]
["BC619a","Acidification potential related to material input flows, process 1",{"$f":"VLOOKUP(A1799,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC619b","Acidification potential related to material input flows, process 2",{"$f":"VLOOKUP(A1800,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC620a","NOx emissions factor of material input flow 1, process 1",{"$f":"VLOOKUP(A1801,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/kg"}]
["BC620b","NOx emissions factor of material input flow 1, process 2",{"$f":"VLOOKUP(A1802,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/kg"}]
["BC620c","NOx emissions factor of material output flow, process 1",{"$f":"VLOOKUP(A1803,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/kgdm"}]
["BC620c1","NOx emissions factor of output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1804,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJe"}]
["BC620c2","NOx emissions factor of output flow, process 1 (heat)",{"$f":"VLOOKUP(A1805,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJf_h"}]
["BC620d","NOx emissions factor of material output flow, process 2",{"$f":"VLOOKUP(A1806,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/kgdm"}]
["BC620d1","NOx emissions factor of output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1807,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJe"}]
["BC620d2","NOx emissions factor of output flow, process 2 (heat)",{"$f":"VLOOKUP(A1808,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/MJf_h"}]
["BC621a","SOx emissions factor of material input flow 1, process 1",{"$f":"VLOOKUP(A1809,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/kg"}]
["BC621b","SOx emissions factor of material input flow 1, process 2",{"$f":"VLOOKUP(A1810,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/kg"}]
["BC621c","SOx emissions factor of material output flow, process 1",{"$f":"VLOOKUP(A1811,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/kgdm"}]
["BC621c1","SOx emissions factor of output flow, process 1 (electricity)",{"$f":"VLOOKUP(A1812,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJe"}]
["BC621c2","SOx emissions factor of output flow, process 1 (heat)",{"$f":"VLOOKUP(A1813,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJf_h"}]
["BC621d","SOx emissions factor of material output flow, process 2",{"$f":"VLOOKUP(A1814,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/kgdm"}]
["BC621d1","SOx emissions factor of output flow, process 2 (electricity)",{"$f":"VLOOKUP(A1815,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJe"}]
["BC621d2","SOx emissions factor of output flow, process 2 (heat)",{"$f":"VLOOKUP(A1816,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/MJf_h"}]
["BC622a","NOx emissions factor of material input flow 2, process 1",{"$f":"VLOOKUP(A1817,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/kg"}]
["BC622b","NOx emissions factor of material input flow 2, process 2",{"$f":"VLOOKUP(A1818,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/kg"}]
["BC623a","SOx emissions factor of material input flow 2, process 1",{"$f":"VLOOKUP(A1819,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/kg"}]
["BC623b","SOx emissions factor of material input flow 2, process 2",{"$f":"VLOOKUP(A1820,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/kg"}]
["BC624a","Acidification potential related to process emissions, process 1",{"$f":"VLOOKUP(A1821,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC624b","Acidification potential related to process emissions, process 2",{"$f":"VLOOKUP(A1822,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSO2_eq/MJoutput"}]
["BC625a","NOx emissions factor of material input flow 3, process 1",{"$f":"VLOOKUP(A1823,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gNOX/kg"}]
["BC626a","SOx emissions factor of material input flow 2, process 1",{"$f":"VLOOKUP(A1824,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gSOX/kg"}]
["BC630a","Eutrophication potential related to process 1",{"$f":"VLOOKUP(A1825,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC630b","Eutrophication potential related to process 2",{"$f":"VLOOKUP(A1826,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJendfuel_fs2"}]
["BC631a","Eutrophication potential related to electricity input, process 1",{"$f":"VLOOKUP(A1827,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC631b","Eutrophication potential related to electricity input, process 2",{"$f":"VLOOKUP(A1828,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC634a","Eutrophication potential related to fuel/heat input flows, process 1",{"$f":"VLOOKUP(A1829,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC634b","Eutrophication potential related to fuel/heat input flows, process 2",{"$f":"VLOOKUP(A1830,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC639a","Eutrophication potential related to material input flows, process 1",{"$f":"VLOOKUP(A1831,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC639b","Eutrophication potential related to material input flows, process 2",{"$f":"VLOOKUP(A1832,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC644a","Eutrophication potential related to process emissions, process 1",{"$f":"VLOOKUP(A1833,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC644b","Eutrophication potential related to process emissions, process 2",{"$f":"VLOOKUP(A1834,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"gPO4_eq/MJoutput"}]
["BC650a","No forced labour, process 1",{"$f":"VLOOKUP(A1835,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC650b","No child labour, process 1",{"$f":"VLOOKUP(A1836,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC650c","Good social practices regarding human rights, process 1",{"$f":"VLOOKUP(A1837,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC650d","No discrimination, process 1",{"$f":"VLOOKUP(A1838,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC650e","Land is used legitimately / land rights have been secured, process 1",{"$f":"VLOOKUP(A1839,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC650f","Open and transparent communication with local communities and stakeholders, process 1",{"$f":"VLOOKUP(A1840,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC650g","Food security, process 1",{"$f":"VLOOKUP(A1841,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC651a","Fair legal contracts, process 1",{"$f":"VLOOKUP(A1842,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC651b","Workers rights, process 1",{"$f":"VLOOKUP(A1843,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC651c","Freedom to join labour organizations or organize themselves, process 1",{"$f":"VLOOKUP(A1844,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC651d","Fair wages and compensation rules, process 1",{"$f":"VLOOKUP(A1845,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC651e","Health, safety and hygiene policy, process 1",{"$f":"VLOOKUP(A1846,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC651f","Risk assessment for safe and healthy working conditions, process 1",{"$f":"VLOOKUP(A1847,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC651g","Health and safety training, process 1",{"$f":"VLOOKUP(A1848,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC652a","No forced labour, process 2",{"$f":"VLOOKUP(A1849,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC652b","No child labour, process 2",{"$f":"VLOOKUP(A1850,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC652c","Good social practices regarding human rights, process 2",{"$f":"VLOOKUP(A1851,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC652d","No discrimination, process 2",{"$f":"VLOOKUP(A1852,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC652e","Land is used legitimately / land rights have been secured, process 2",{"$f":"VLOOKUP(A1853,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC652f","Open and transparent communication with local communities and stakeholders, process 2",{"$f":"VLOOKUP(A1854,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC652g","Food security, process 2",{"$f":"VLOOKUP(A1855,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC653a","Fair legal contracts, process 2",{"$f":"VLOOKUP(A1856,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC653b","Workers rights, process 2",{"$f":"VLOOKUP(A1857,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC653c","Freedom to join labour organizations or organize themselves, process 2",{"$f":"VLOOKUP(A1858,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC653d","Fair wages and compensation rules, process 2",{"$f":"VLOOKUP(A1859,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC653e","Health, safety and hygiene policy, process 2",{"$f":"VLOOKUP(A1860,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC653f","Risk assessment for safe and healthy working conditions, process 2",{"$f":"VLOOKUP(A1861,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC653g","Health and safety training, process 2",{"$f":"VLOOKUP(A1862,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC654a","No forced labour, processing FS2",{"$f":"VLOOKUP(A1863,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC654b","No child labour, processing FS2",{"$f":"VLOOKUP(A1864,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC654c","Good social practices regarding human rights, processing FS2",{"$f":"VLOOKUP(A1865,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC654d","No discrimination, processing FS2",{"$f":"VLOOKUP(A1866,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC654e","Land is used legitimately / land rights have been secured, processing FS2",{"$f":"VLOOKUP(A1867,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC654f","Open and transparent communication with local communities and stakeholders, processing FS2",{"$f":"VLOOKUP(A1868,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC654g","Food security, processing FS2",{"$f":"VLOOKUP(A1869,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC655a","Fair legal contracts, processing FS2",{"$f":"VLOOKUP(A1870,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC655b","Workers rights, processing FS2",{"$f":"VLOOKUP(A1871,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC655c","Freedom to join labour organizations or organize themselves, processing FS2",{"$f":"VLOOKUP(A1872,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC655d","Fair wages and compensation rules, processing FS2",{"$f":"VLOOKUP(A1873,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC655e","Health, safety and hygiene policy, processing FS2",{"$f":"VLOOKUP(A1874,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC655f","Risk assessment for safe and healthy working conditions, processing FS2",{"$f":"VLOOKUP(A1875,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC655g","Health and safety training, processing FS2",{"$f":"VLOOKUP(A1876,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC656","Human and property rights, process 1_score",{"$f":"VLOOKUP(A1877,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC657","Labour rights and conditions, process 1_score",{"$f":"VLOOKUP(A1878,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC658","Human and property rights, process 2_score",{"$f":"VLOOKUP(A1879,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC659","Labour rights and conditions, process 2_score",{"$f":"VLOOKUP(A1880,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC660","Human and property rights, processing overall_score",{"$f":"VLOOKUP(A1881,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
["BC661","Labour rights and conditions, processing overall_score",{"$f":"VLOOKUP(A1882,'Conversion feedstock2'!D$9:E$766,2,FALSE)","v":"-"}]
[]
["Final Conversion (Electricity & Heat)"]
["FC000","Final conversion process",{"$f":"VLOOKUP(A1885,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC001a","Type of input flow, feedstock 1",{"$f":"VLOOKUP(A1886,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC001b","Type of input flow, feedstock 2",{"$f":"VLOOKUP(A1887,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC002a","Share of input flow 1 (caloric)",{"$f":"VLOOKUP(A1888,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC002b","Share of input flow 2 (caloric)",{"$f":"VLOOKUP(A1889,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC003a","Net electrical efficiency, final conversion",{"$f":"VLOOKUP(A1890,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC003b","Net thermal efficiency, final conversion",{"$f":"VLOOKUP(A1891,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC003c","Net conversion efficiency, final conversion - other than electricity or heat",{"$f":"VLOOKUP(A1892,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC004a","Type of by-product 1, final conversion",{"$f":"VLOOKUP(A1893,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC004b","Type of by-product 2, final conversion",{"$f":"VLOOKUP(A1894,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC005a","Extraction rate of by-product 1, final conversion (kg)",{"$f":"VLOOKUP(A1895,'Final conversion'!D$7:F$1091,2,FALSE)","v":"kgbyproduct /kginput"}]
["FC005b","Extraction rate of by-product 2, final conversion (kg)",{"$f":"VLOOKUP(A1896,'Final conversion'!D$7:F$1091,2,FALSE)","v":"kgbyproduct /kginput"}]
["FC006a","Extraction rate of by-product 1, final conversion (MJ)",{"$f":"VLOOKUP(A1897,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJbyproduct /MJinput"}]
["FC006b","Extraction rate of by-product 2, final conversion (MJ)",{"$f":"VLOOKUP(A1898,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJbyproduct /MJinput"}]
["FC007a","Energy content of by-product 1, final conversion (LHV)",{"$f":"VLOOKUP(A1899,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJ/kg"}]
["FC007b","Energy content of by-product 2, final conversion (LHV)",{"$f":"VLOOKUP(A1900,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJ/kg"}]
["FC008a","Valorisation of by-product 1, final conversion",{"$f":"VLOOKUP(A1901,'Final conversion'!D$7:F$1091,2,FALSE)","v":"binary"}]
["FC008b","Valorisation of by-product 2, final conversion",{"$f":"VLOOKUP(A1902,'Final conversion'!D$7:F$1091,2,FALSE)","v":"binary"}]
["FC009a","Type of material input flow 1, final conversion",{"$f":"VLOOKUP(A1903,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC009b","Type of material input flow 2, final conversion",{"$f":"VLOOKUP(A1904,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC010a","Amount of material input flow 1, final conversion",{"$f":"VLOOKUP(A1905,'Final conversion'!D$7:F$1091,2,FALSE)","v":"kg/MJinput"}]
["FC010b","Amount of material input flow 2, final conversion",{"$f":"VLOOKUP(A1906,'Final conversion'!D$7:F$1091,2,FALSE)","v":"kg/MJinput"}]
["FC011a","Type of fuel/heat flow 1, final conversion",{"$f":"VLOOKUP(A1907,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC011b","Type of fuel/heat flow 2, final conversion",{"$f":"VLOOKUP(A1908,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC012a","Amount of fuel/heat flow 1, final conversion",{"$f":"VLOOKUP(A1909,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJf_h/MJinput"}]
["FC012b","Amount of fuel/heat flow 2, final conversion",{"$f":"VLOOKUP(A1910,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJf_h/MJinput"}]
["FC013","Net amount of electricity input, final conversion",{"$f":"VLOOKUP(A1911,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJe/MJinput"}]
["FC014","Electricity source, final conversion",{"$f":"VLOOKUP(A1912,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC015a","Specific fossil energy for material input flow 1, final conversion",{"$f":"VLOOKUP(A1913,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/kg"}]
["FC015b","Specific fossil energy for material input flow 2, final conversion",{"$f":"VLOOKUP(A1914,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/kg"}]
["FC015c","Specific fossil energy for fuel/heat flow 1, final conversion",{"$f":"VLOOKUP(A1915,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJf_h"}]
["FC015d","Specific fossil energy for fuel/heat flow 2, final conversion",{"$f":"VLOOKUP(A1916,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJf_h"}]
["FC015e","Specific fossil energy used for external electricity production, final conversion",{"$f":"VLOOKUP(A1917,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJe"}]
["FC016a","Specific primary energy for material input flow 1, final conversion",{"$f":"VLOOKUP(A1918,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/kg"}]
["FC016b","Specific primary energy for material input flow 2, final conversion",{"$f":"VLOOKUP(A1919,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/kg"}]
["FC016c","Specific primary energy for fuel/heat flow 1, final conversion",{"$f":"VLOOKUP(A1920,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJf_h"}]
["FC016d","Specific primary energy for fuel/heat flow 2, final conversion",{"$f":"VLOOKUP(A1921,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJf_h"}]
["FC016e","Specific primary energy used for external electricity production, final conversion",{"$f":"VLOOKUP(A1922,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJe"}]
["FC017a","Specific GHG emissions related to material input flow 1, final conversion",{"$f":"VLOOKUP(A1923,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/kg"}]
["FC017b","Specific GHG emissions related to material input flow 2, final conversion",{"$f":"VLOOKUP(A1924,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/kg"}]
["FC017c","Specific GHG emissions related to fuel/heat flow 1, final conversion",{"$f":"VLOOKUP(A1925,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["FC017d","Specific GHG emissions related to fuel/heat flow 2, final conversion",{"$f":"VLOOKUP(A1926,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJf_h"}]
["FC017e","Specific GHG emissions related to external electricity production, final conversion",{"$f":"VLOOKUP(A1927,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2eq/MJe"}]
["FC018a","Fossil energy use related to electricity input, final conversion",{"$f":"VLOOKUP(A1928,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJinput"}]
["FC018b","Fossil energy use related to fuel/heat input flows, final conversion",{"$f":"VLOOKUP(A1929,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJinput"}]
["FC018c","Fossil energy use related to material input flows, final conversion",{"$f":"VLOOKUP(A1930,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJinput"}]
["FC019","Fossil energy use in final conversion process",{"$f":"VLOOKUP(A1931,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJinput"}]
["FC020a","Primary energy use related to electricity input, final conversion",{"$f":"VLOOKUP(A1932,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJinput"}]
["FC020b","Primary energy use related to fuel/heat flows, final conversion",{"$f":"VLOOKUP(A1933,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJinput"}]
["FC020c","Primary energy use related to material input flows, final conversion",{"$f":"VLOOKUP(A1934,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJinput"}]
["FC021","Primary energy use in final conversion process",{"$f":"VLOOKUP(A1935,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJinput"}]
["FC022a","GHG emissions related to electricity use, final conversion",{"$f":"VLOOKUP(A1936,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJinput"}]
["FC022b","GHG emissions related to fuel/heat flows, final conversion",{"$f":"VLOOKUP(A1937,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJinput"}]
["FC022c","GHG emissions related to material input flows, final conversion",{"$f":"VLOOKUP(A1938,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJinput"}]
["FC023","GHG emissions related to final conversion",{"$f":"VLOOKUP(A1939,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJinput"}]
["FC024a","Moisture content of by-product 1, final conversion",{"$f":"VLOOKUP(A1940,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC024b","Moisture content of by-product 2, final conversion",{"$f":"VLOOKUP(A1941,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC025a","Allocation to heat, final conversion",{"$f":"VLOOKUP(A1942,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC025b","Allocation to electricity, final conversion",{"$f":"VLOOKUP(A1943,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC025c","Allocation to energy products, final conversion",{"$f":"VLOOKUP(A1944,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC026","Allocation to by-products, final conversion",{"$f":"VLOOKUP(A1945,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC027a","Allocation to by-product 1, final conversion",{"$f":"VLOOKUP(A1946,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC027b","Allocation to by-product 2, final conversion",{"$f":"VLOOKUP(A1947,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC028a","NOX emissions to air (not from material/energy input), final conversion",{"$f":"VLOOKUP(A1948,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNOX/MJoutput"}]
["FC028b","SOX emissions to air (not from material/energy input), final conversion",{"$f":"VLOOKUP(A1949,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSOX/MJoutput"}]
["FC028c","NH3 emissions to air (not from material/energy input), final conversion",{"$f":"VLOOKUP(A1950,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNH3/MJoutput"}]
["FC028d","NO3- emissions to water (not from material/energy input), final conversion",{"$f":"VLOOKUP(A1951,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNO3/MJoutput"}]
["FC028e","NH4+ emissions to water (not from material/energy input), final conversion",{"$f":"VLOOKUP(A1952,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNH4/MJoutput"}]
["FC028f","PO43- emissions to water (not from material/energy input), final conversion",{"$f":"VLOOKUP(A1953,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gPO4/MJoutput"}]
["FC028g","COD emissions to water (not from material/energy input), final conversion",{"$f":"VLOOKUP(A1954,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCOD/MJoutput"}]
["FC029","Compliance with RED requirements on GHG savings",{"$f":"VLOOKUP(A1955,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC030","Functional unit",{"$f":"VLOOKUP(A1956,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC031","Output heat per MJ functional unit",{"$f":"VLOOKUP(A1957,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJh/MJFU"}]
["FC032","Output electricity per MJ functional unit",{"$f":"VLOOKUP(A1958,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJe/MJFU"}]
["FC033","Input feedstock 1 per MJ functional unit",{"$f":"VLOOKUP(A1959,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJ/MJFU"}]
["FC034","Input feedstock 2 per MJ functional unit",{"$f":"VLOOKUP(A1960,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJ/MJFU"}]
["FC035a","NOx emissions factor of material input flow 1, final conversion",{"$f":"VLOOKUP(A1961,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNOX/kg"}]
["FC035b","NOx emissions factor of material input flow 2, final conversion",{"$f":"VLOOKUP(A1962,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNOX/kg"}]
["FC035c","NOx emissions factor of fuel/heat flow 1, final conversion",{"$f":"VLOOKUP(A1963,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNOX/MJf_h"}]
["FC035d","NOx emissions factor of fuel/heat flow 2, final conversion",{"$f":"VLOOKUP(A1964,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNOX/MJf_h"}]
["FC035e","NOx emissions factor of electricity, final conversion",{"$f":"VLOOKUP(A1965,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gNOX/MJe"}]
["FC036a","SOx emissions factor of material input flow 1, final conversion",{"$f":"VLOOKUP(A1966,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSOX/kg"}]
["FC036b","SOx emissions factor of material input flow 2, final conversion",{"$f":"VLOOKUP(A1967,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSOX/kg"}]
["FC036c","SOx emissions factor of fuel/heat flow 1, final conversion",{"$f":"VLOOKUP(A1968,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSOX/MJf_h"}]
["FC036d","SOx emissions factor of fuel/heat flow 2, final conversion",{"$f":"VLOOKUP(A1969,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSOX/MJf_h"}]
["FC036e","SOx emissions factor of electricity, final conversion",{"$f":"VLOOKUP(A1970,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSOX/MJe"}]
["FC037a","Gross electrical efficiency, final conversion",{"$f":"VLOOKUP(A1971,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC037b","Gross thermal efficiency, final conversion",{"$f":"VLOOKUP(A1972,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC038","Temperature of useful heat",{"$f":"VLOOKUP(A1973,'Final conversion'!D$7:F$1091,2,FALSE)","v":"°C"}]
["FC039a","Carnot efficiency of electricity"]
["FC039b","Carnot efficiency of heat"]
["FC040a","Total fossil energy use before allocation 4",{"$f":"VLOOKUP(A1976,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJinput"}]
["FC040b","Total primary energy use before allocation 4",{"$f":"VLOOKUP(A1977,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJinput"}]
["FC040c","Total GHG emissions before allocation 4",{"$f":"VLOOKUP(A1978,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJinput"}]
["FC040d","Total water use before allocation 4",{"$f":"VLOOKUP(A1979,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJinput"}]
["FC040e","Total land use before allocation 4",{"$f":"VLOOKUP(A1980,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJinput"}]
["FC040f","Total acidification potential before allocation 4",{"$f":"VLOOKUP(A1981,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC040g","Total eutrophication potential before allocation 4",{"$f":"VLOOKUP(A1982,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC041a","Total fossil energy use allocated to heat production",{"$f":"VLOOKUP(A1983,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJh"}]
["FC041b","Total primary energy use allocated to heat production",{"$f":"VLOOKUP(A1984,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJh"}]
["FC041c","Total GHG emissions allocated to heat production",{"$f":"VLOOKUP(A1985,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJh"}]
["FC041d","Total water use allocated to heat production",{"$f":"VLOOKUP(A1986,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJh"}]
["FC041e","Total land use allocated to heat production",{"$f":"VLOOKUP(A1987,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJh"}]
["FC041f","Total acidification potential allocated to heat production",{"$f":"VLOOKUP(A1988,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJh"}]
["FC041g","Total eutrophication potential allocated to heat production",{"$f":"VLOOKUP(A1989,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJh"}]
["FC042a","Total fossil energy use allocated to heat production",{"$f":"VLOOKUP(A1990,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJFU"}]
["FC042b","Total primary energy use allocated to heat production",{"$f":"VLOOKUP(A1991,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJFU"}]
["FC042c","Total GHG emissions allocated to heat production",{"$f":"VLOOKUP(A1992,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC042d","Total water use allocated to heat production",{"$f":"VLOOKUP(A1993,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJFU"}]
["FC042e","Total land use allocated to heat production",{"$f":"VLOOKUP(A1994,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJFU"}]
["FC042f","Total acidification potential allocated to heat production",{"$f":"VLOOKUP(A1995,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC042g","Total eutrophication potential allocated to heat production",{"$f":"VLOOKUP(A1996,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC043a","Total fossil energy use allocated to electricity production",{"$f":"VLOOKUP(A1997,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJe"}]
["FC043b","Total primary energy use allocated to electricity production",{"$f":"VLOOKUP(A1998,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJe"}]
["FC043c","Total GHG emissions allocated to electricity production",{"$f":"VLOOKUP(A1999,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJe"}]
["FC043d","Total water use allocated to electricity production",{"$f":"VLOOKUP(A2000,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJe"}]
["FC043e","Total land use allocated to electricity production",{"$f":"VLOOKUP(A2001,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJe"}]
["FC043f","Total acidification potential allocated to electricity production",{"$f":"VLOOKUP(A2002,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJe"}]
["FC043g","Total eutrophication potential allocated to electricity production",{"$f":"VLOOKUP(A2003,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJe"}]
["FC044a","Total fossil energy use allocated to electricity production",{"$f":"VLOOKUP(A2004,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJFU"}]
["FC044b","Total primary energy use allocated to electricity production",{"$f":"VLOOKUP(A2005,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJFU"}]
["FC044c","Total GHG emissions allocated to electricity production",{"$f":"VLOOKUP(A2006,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC044d","Total water use allocated to electricity production",{"$f":"VLOOKUP(A2007,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJFU"}]
["FC044e","Total land use allocated to electricity production",{"$f":"VLOOKUP(A2008,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJFU"}]
["FC044f","Total acidification potential allocated to electricity production",{"$f":"VLOOKUP(A2009,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC044g","Total eutrophication potential allocated to electricity production",{"$f":"VLOOKUP(A2010,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC045a","Totally allocated fossil energy requirement for final conversion",{"$f":"VLOOKUP(A2011,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJFU"}]
["FC045b","Totally allocated primary energy requirement for final conversion",{"$f":"VLOOKUP(A2012,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJFU"}]
["FC045c","Totally allocated GHG emissions from final conversion",{"$f":"VLOOKUP(A2013,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC045d","Totally allocated water use from final conversion",{"$f":"VLOOKUP(A2014,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJFU"}]
["FC045f","Totally allocated acidification potential from final conversion",{"$f":"VLOOKUP(A2015,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC045g","Totally allocated eutrophication potential from final conversion",{"$f":"VLOOKUP(A2016,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC046a","Total fossil energy use allocated to energy production",{"$f":"VLOOKUP(A2017,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJFU"}]
["FC046b","Total primary energy use allocated to energy production",{"$f":"VLOOKUP(A2018,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJFU"}]
["FC046c","Total GHG emissions allocated to energy production",{"$f":"VLOOKUP(A2019,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC046d","Total water use allocated to energy production",{"$f":"VLOOKUP(A2020,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJFU"}]
["FC046e","Total land use allocated to energy production",{"$f":"VLOOKUP(A2021,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJFU"}]
["FC046f","Total acidification potential allocated to energy production",{"$f":"VLOOKUP(A2022,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC046g","Total eutrophication potential allocated to energy production",{"$f":"VLOOKUP(A2023,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC047a","Fossil energy requirement of reference system for heat",{"$f":"VLOOKUP(A2024,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJh"}]
["FC047b","Primary energy requirement of reference system for heat",{"$f":"VLOOKUP(A2025,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJh"}]
["FC047c","GHG emissions of reference system for heat",{"$f":"VLOOKUP(A2026,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJh"}]
["FC047d","Water use of reference system for heat",{"$f":"VLOOKUP(A2027,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJh"}]
["FC047e","Land use of reference system for heat",{"$f":"VLOOKUP(A2028,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJh"}]
["FC047f","Acidification potential of reference system for heat",{"$f":"VLOOKUP(A2029,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJh"}]
["FC047g","Eutrophication potential of reference system for heat",{"$f":"VLOOKUP(A2030,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJh"}]
["FC048a","Fossil energy requirement of reference system for electricity",{"$f":"VLOOKUP(A2031,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJe"}]
["FC048b","Primary energy requirement of reference system for electricity",{"$f":"VLOOKUP(A2032,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJe"}]
["FC048c","GHG emissions of reference system for electricity",{"$f":"VLOOKUP(A2033,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJe"}]
["FC048d","Water use of reference system for electricity",{"$f":"VLOOKUP(A2034,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJe"}]
["FC048e","Land use of reference system for electricity",{"$f":"VLOOKUP(A2035,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJe"}]
["FC048f","Acidification potential of reference system for electricity",{"$f":"VLOOKUP(A2036,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJe"}]
["FC048g","Eutrophication potential of reference system for electricity",{"$f":"VLOOKUP(A2037,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJe"}]
["FC049a","Fossil energy reduction of heat production",{"$f":"VLOOKUP(A2038,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC049b","Primary energy reduction of heat production",{"$f":"VLOOKUP(A2039,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC049c","GHG emission reduction of heat production",{"$f":"VLOOKUP(A2040,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC049d","Water use reduction of heat production",{"$f":"VLOOKUP(A2041,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC049e","Land use reduction of heat production",{"$f":"VLOOKUP(A2042,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC049f","Acidification potential reduction of heat production",{"$f":"VLOOKUP(A2043,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC049g","Eutrophication potential reduction of heat production",{"$f":"VLOOKUP(A2044,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC050a","Fossil energy reduction of electricity production",{"$f":"VLOOKUP(A2045,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC050b","Primary energy reduction of electricity production",{"$f":"VLOOKUP(A2046,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC050c","GHG emission reduction of electricity production",{"$f":"VLOOKUP(A2047,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC050d","Water use reduction of electricity production",{"$f":"VLOOKUP(A2048,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC050e","Land use reduction of electricity production",{"$f":"VLOOKUP(A2049,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC050f","Acidification potential reduction of electricity production",{"$f":"VLOOKUP(A2050,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC050g","Eutrophication potential reduction of electricity production",{"$f":"VLOOKUP(A2051,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC051a","Fossil energy requirement of total reference system",{"$f":"VLOOKUP(A2052,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJFU"}]
["FC051b","Primary energy requirement of total reference system",{"$f":"VLOOKUP(A2053,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJFU"}]
["FC051c","GHG emissions of total reference system",{"$f":"VLOOKUP(A2054,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC051d","Water use of total reference system",{"$f":"VLOOKUP(A2055,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJFU"}]
["FC051e","Land use of total reference system",{"$f":"VLOOKUP(A2056,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJFU"}]
["FC051f","Acidification potential of total reference system",{"$f":"VLOOKUP(A2057,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC051g","Eutrophication potential of total reference system",{"$f":"VLOOKUP(A2058,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJFU"}]
["FC052a","Fossil energy reduction of total energy production",{"$f":"VLOOKUP(A2059,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC052b","Primary energy reduction of total energy production",{"$f":"VLOOKUP(A2060,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC052c","GHG emission reduction of total energy production",{"$f":"VLOOKUP(A2061,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC052d","Water use reduction of total energy production",{"$f":"VLOOKUP(A2062,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC052e","Land use reduction of total energy production",{"$f":"VLOOKUP(A2063,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC052f","Acidification potential reduction of total energy production",{"$f":"VLOOKUP(A2064,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC052g","Eutrophication potential reduction of total energy production",{"$f":"VLOOKUP(A2065,'Final conversion'!D$7:F$1091,2,FALSE)","v":"%"}]
["FC053","Total GHG emissions allocated to energy production without LUC emissions",{"$f":"VLOOKUP(A2066,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC054","GHG emission reduction of total energy production without LUC emissions",{"$f":"VLOOKUP(A2067,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC055","Total carbon debt due to land use change",{"$f":"VLOOKUP(A2068,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC056","Repayment time",{"$f":"VLOOKUP(A2069,'Final conversion'!D$7:F$1091,2,FALSE)","v":"years"}]
["FC057a","Total carbon debt due to land use change_FS1",{"$f":"VLOOKUP(A2070,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC057b","Total carbon debt due to land use change_FS2",{"$f":"VLOOKUP(A2071,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJFU"}]
["FC058a","Water use for final conversion process",{"$f":"VLOOKUP(A2072,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/MJinput"}]
["FC058b","Water use for final conversion process",{"$f":"VLOOKUP(A2073,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJinput"}]
["FC060","Acidification potential related to final conversion process ",{"$f":"VLOOKUP(A2074,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC061","Acidification potential related to electricity input, final conversion",{"$f":"VLOOKUP(A2075,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC062","Acidification potential related to fuel/heat input flows, final conversion",{"$f":"VLOOKUP(A2076,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC063","Acidification potential related to material input flows, final conversion",{"$f":"VLOOKUP(A2077,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC064","Acidification potential related to process emissions, final conversion",{"$f":"VLOOKUP(A2078,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC070","Eutrophication potential related to final conversion process ",{"$f":"VLOOKUP(A2079,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC071","Eutrophication potential related to electricity input, final conversion",{"$f":"VLOOKUP(A2080,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC072","Eutrophication potential related to fuel/heat input flows, final conversion",{"$f":"VLOOKUP(A2081,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC073","Eutrophication potential related to material input flows, final conversion",{"$f":"VLOOKUP(A2082,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC074","Eutrophication potential related to process emissions, final conversion",{"$f":"VLOOKUP(A2083,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJinput"}]
["FC080a","No forced labour, final conversion",{"$f":"VLOOKUP(A2084,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC080b","No child labour, final conversion",{"$f":"VLOOKUP(A2085,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC080c","Good social practices regarding human rights, final conversion",{"$f":"VLOOKUP(A2086,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC080d","No discrimination, final conversion",{"$f":"VLOOKUP(A2087,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC080e","Land is used legitimately / land rights have been secured, final conversion",{"$f":"VLOOKUP(A2088,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC080f","Open and transparent communication with local communities and stakeholders, final conversion",{"$f":"VLOOKUP(A2089,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC080g","Food security, final conversion",{"$f":"VLOOKUP(A2090,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC081a","Fair legal contracts, final conversion",{"$f":"VLOOKUP(A2091,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC081b","Workers rights, final conversion",{"$f":"VLOOKUP(A2092,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC081c","Freedom to join labour organizations or organize themselves, final conversion",{"$f":"VLOOKUP(A2093,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC081d","Fair wages and compensation rules, final conversion",{"$f":"VLOOKUP(A2094,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC081e","Health, safety and hygiene policy, final conversion",{"$f":"VLOOKUP(A2095,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC081f","Risk assessment for safe and healthy working conditions, final conversion",{"$f":"VLOOKUP(A2096,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC081g","Health and safety training, final conversion",{"$f":"VLOOKUP(A2097,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC082","Human and property rights, final conversion_score",{"$f":"VLOOKUP(A2098,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC083","Labour rights and conditions, final conversion_score",{"$f":"VLOOKUP(A2099,'Final conversion'!D$7:F$1091,2,FALSE)","v":"-"}]
["FC100a","Mean of BC082a"]
["FC100b","Mean of BC082b"]
["FC100c","Mean of BC082c"]
["FC100d","Mean of BC082d"]
["FC100e","Mean of FP106a"]
["FC100f","Mean of BC082f"]
["FC100g","Mean of BC082g"]
["FC100h","Mean of FP107a"]
["FC101a","Mean of BC582a"]
["FC101b","Mean of BC582b"]
["FC101c","Mean of BC582c"]
["FC101d","Mean of BC582d"]
["FC101e","Mean of FP606a"]
["FC101f","Mean of BC582f"]
["FC101g","Mean of BC582g"]
["FC101h","Mean of FP607a"]
["FC102a","Mean of FC046a"]
["FC102b","Mean of FC046b"]
["FC102c","Mean of FC046c"]
["FC102d","Mean of FC046d"]
["FC102e","Mean of FC046e"]
["FC102f","Mean of FC046f"]
["FC102g","Mean of FC046g"]
["FC102h","Mean of FC055"]
["FC103a","Standard deviation of BC082a"]
["FC103b","Standard deviation of BC082b"]
["FC103c","Standard deviation of BC082c"]
["FC103d","Standard deviation of BC082d"]
["FC103e","Standard deviation of FP106a"]
["FC103f","Standard deviation of BC082f"]
["FC103g","Standard deviation of BC082g"]
["FC103h","Standard deviation of FP107a"]
["FC104a","Standard deviation of BC582a"]
["FC104b","Standard deviation of BC582b"]
["FC104c","Standard deviation of BC582c"]
["FC104d","Standard deviation of BC582d"]
["FC104e","Standard deviation of FP606a"]
["FC104f","Standard deviation of BC582f"]
["FC104g","Standard deviation of BC582g"]
["FC104h","Standard deviation of FP607a"]
["FC105a","Standard deviation of FC046a"]
["FC105b","Standard deviation of FC046b"]
["FC105c","Standard deviation of FC046c"]
["FC105d","Standard deviation of FC046d"]
["FC105e","Standard deviation of FC046e"]
["FC105f","Standard deviation of FC046f"]
["FC105g","Standard deviation of FC046g"]
["FC105h","Standard deviation of FC055"]
["FC110a","Fossil energy requirement of reference system for biogas",{"$f":"VLOOKUP(A2148,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJbiogas"}]
["FC110b","Primary energy requirement of reference system for biogas",{"$f":"VLOOKUP(A2149,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJbiogas"}]
["FC110c","GHG emissions of reference system for biogas",{"$f":"VLOOKUP(A2150,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJbiogas"}]
["FC110d","Water use of reference system for biogas",{"$f":"VLOOKUP(A2151,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJbiogas"}]
["FC110e","Land use of reference system for biogas",{"$f":"VLOOKUP(A2152,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJbiogas"}]
["FC110f","Acidification potential of reference system for biogas",{"$f":"VLOOKUP(A2153,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJbiogas"}]
["FC110g","Eutrophication potential of reference system for biogas",{"$f":"VLOOKUP(A2154,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJbiogas"}]
["FC111a","Fossil energy requirement of reference system for diesel",{"$f":"VLOOKUP(A2155,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJdiesel"}]
["FC111b","Primary energy requirement of reference system for diesel",{"$f":"VLOOKUP(A2156,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJdiesel"}]
["FC111c","GHG emissions of reference system for diesel",{"$f":"VLOOKUP(A2157,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJdiesel"}]
["FC111d","Water use of reference system for diesel",{"$f":"VLOOKUP(A2158,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJdiesel"}]
["FC111e","Land use of reference system for diesel",{"$f":"VLOOKUP(A2159,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJdiesel"}]
["FC111f","Acidification potential of reference system for diesel",{"$f":"VLOOKUP(A2160,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJdiesel"}]
["FC111g","Eutrophication potential of reference system for diesel",{"$f":"VLOOKUP(A2161,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJdiesel"}]
["FC112a","Fossil energy requirement of reference system for gasoline",{"$f":"VLOOKUP(A2162,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJgasoline"}]
["FC112b","Primary energy requirement of reference system for gasoline",{"$f":"VLOOKUP(A2163,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJgasoline"}]
["FC112c","GHG emissions of reference system for gasoline",{"$f":"VLOOKUP(A2164,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJgasoline"}]
["FC112d","Water use of reference system for gasoline",{"$f":"VLOOKUP(A2165,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJgasoline"}]
["FC112e","Land use of reference system for gasoline",{"$f":"VLOOKUP(A2166,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJgasoline"}]
["FC112f","Acidification potential of reference system for gasoline",{"$f":"VLOOKUP(A2167,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJgasoline"}]
["FC112g","Eutrophication potential of reference system for gasoline",{"$f":"VLOOKUP(A2168,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJgasoline"}]
["FC113a","Fossil energy requirement of reference system for heavy fuel oil",{"$f":"VLOOKUP(A2169,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJfossil/MJhfo"}]
["FC113b","Primary energy requirement of reference system for heavy fuel oil",{"$f":"VLOOKUP(A2170,'Final conversion'!D$7:F$1091,2,FALSE)","v":"MJprim/MJhfo"}]
["FC113c","GHG emissions of reference system for heavy fuel oil",{"$f":"VLOOKUP(A2171,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gCO2_eq/MJhfo"}]
["FC113d","Water use of reference system for heavy fuel oil",{"$f":"VLOOKUP(A2172,'Final conversion'!D$7:F$1091,2,FALSE)","v":"m³/GJhfo"}]
["FC113e","Land use of reference system for heavy fuel oil",{"$f":"VLOOKUP(A2173,'Final conversion'!D$7:F$1091,2,FALSE)","v":"ha/GJhfo"}]
["FC113f","Acidification potential of reference system for heavy fuel oil",{"$f":"VLOOKUP(A2174,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJhfo"}]
["FC113g","Eutrophication potential of reference system for heavy fuel oil",{"$f":"VLOOKUP(A2175,'Final conversion'!D$7:F$1091,2,FALSE)","v":"gSO2_eq/MJhfo"}]